{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["测量数据"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"测量数据","index":0,"n_rows":31,"n_cols":20,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
["序号","时间","场站","风机","叶片1角度偏差","叶片2角度偏差","叶片3角度偏差","相对偏差","叶片1净空值","叶片2净空值","叶片3净空值","净空值平均","叶片1扭转变形","叶片2扭转变形","叶片3扭转变形","扭转变形平均","塔筒晃动幅值","塔筒晃动主频","叶片采集频率","塔筒采集频率"]
[1]
[2]
[3]
[4]
[5]
[6]
[7]
[8]
[9]
[10]
[11]
[12]
[13]
[14]
[15]
[16]
[17]
[18]
[19]
[20]
[21]
[22]
[23]
[24]
[25]
[26]
[27]
[28]
[29]
[30]