{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":3582,"n_cols":11,"rows_kept":3582,"cut":false,"hidden":false,"merged":[]}
["顺序号","遥测ID号","场站","场站标准化编号","风机号","遥测别名","标准化中文","标准化英文","遥测ID","历史采样表名","历史采样域名"]
[0,"c_阳曲一期Ⅲ-030 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅲ-030 机舱中轴线与风向夹角","yc_hs_0498","cur_24"]
[1,"c_阳曲一期Ⅲ-030 风向","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅲ-030 风向","yc_hs_0498","cur_25"]
[2,"c_阳曲一期Ⅲ-030 舱外温度","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅲ-030 舱外温度","yc_hs_0498","cur_26"]
[3,"c_阳曲一期Ⅲ-030 扭揽角度","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅲ-030 扭揽角度","yc_hs_0498","cur_27"]
[4,"c_阳曲一期Ⅲ-030 1#桨叶片角度","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅲ-030 1#桨叶片角度","yc_hs_0498","cur_28"]
[5,"c_阳曲一期Ⅲ-030 2#桨叶片角度","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅲ-030 2#桨叶片角度","yc_hs_0498","cur_29"]
[6,"c_阳曲一期Ⅲ-030 3#桨叶片角度","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅲ-030 3#桨叶片角度","yc_hs_0498","cur_30"]
[7,"c_阳曲一期Ⅲ-030 发电机转速","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅲ-030 发电机转速","yc_hs_0498","cur_31"]
[8,"c_阳曲一期Ⅲ-030 发电机有功功率","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅲ-030 发电机有功功率","yc_hs_0498","cur_32"]
[9,"c_阳曲一期Ⅲ-030 发电机 绕组温度1","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅲ-030 发电机 绕组温度1","yc_hs_0498","cur_85"]
[10,"c_阳曲一期Ⅲ-030 发电机 绕组温度2","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅲ-030 发电机 绕组温度2","yc_hs_0498","cur_86"]
[11,"c_阳曲一期Ⅲ-030 发电机 绕组温度3","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅲ-030 发电机 绕组温度3","yc_hs_0498","cur_87"]
[12,"c_阳曲一期Ⅲ-030 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅲ-030 机舱侧向振动(已滤波)","yc_hs_0498","cur_92"]
[13,"c_阳曲一期Ⅲ-030 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅲ-030 机舱轴向振动(已滤波)","yc_hs_0498","cur_93"]
[14,"c_阳曲一期Ⅲ-030 舱内温度","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅲ-030 舱内温度","yc_hs_0498","cur_100"]
[15,"c_阳曲一期Ⅱ-019 舱内温度","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅱ-019 舱内温度","yc_hs_0499","cur_08"]
[16,"c_阳曲一期Ⅰ-006 风速","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅰ-006 风速","yc_hs_0499","cur_15"]
[17,"c_阳曲一期Ⅰ-006 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅰ-006 机舱中轴线与风向夹角","yc_hs_0499","cur_16"]
[18,"c_阳曲一期Ⅰ-006 风向","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅰ-006 风向","yc_hs_0499","cur_17"]
[19,"c_阳曲一期Ⅰ-006 舱外温度","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅰ-006 舱外温度","yc_hs_0499","cur_18"]
[20,"c_阳曲一期Ⅰ-006 扭揽角度","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅰ-006 扭揽角度","yc_hs_0499","cur_19"]
[21,"c_阳曲一期Ⅰ-006 1#桨叶片角度","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅰ-006 1#桨叶片角度","yc_hs_0499","cur_20"]
[22,"c_阳曲一期Ⅰ-006 2#桨叶片角度","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅰ-006 2#桨叶片角度","yc_hs_0499","cur_62"]
[23,"c_阳曲一期Ⅰ-006 3#桨叶片角度","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅰ-006 3#桨叶片角度","yc_hs_0499","cur_63"]
[24,"c_阳曲一期Ⅰ-006 发电机转速","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅰ-006 发电机转速","yc_hs_0499","cur_64"]
[25,"c_阳曲一期Ⅰ-006 发电机有功功率","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅰ-006 发电机有功功率","yc_hs_0499","cur_65"]
[26,"c_阳曲一期Ⅰ-006 发电机 绕组温度1","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅰ-006 发电机 绕组温度1","yc_hs_0499","cur_77"]
[27,"c_阳曲一期Ⅰ-006 发电机 绕组温度2","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅰ-006 发电机 绕组温度2","yc_hs_0499","cur_78"]
[28,"c_阳曲一期Ⅰ-006 发电机 绕组温度3","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅰ-006 发电机 绕组温度3","yc_hs_0499","cur_79"]
[29,"c_阳曲一期Ⅰ-006 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅰ-006 机舱侧向振动(已滤波)","yc_hs_0499","cur_84"]
[30,"c_阳曲一期Ⅰ-006 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅰ-006 机舱轴向振动(已滤波)","yc_hs_0499","cur_85"]
[31,"c_阳曲一期Ⅰ-006 舱内温度","阳曲风电场","WOF35100072",6,"YNJS.T1_L1.WTG006.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅰ-006 舱内温度","yc_hs_0499","cur_92"]
[32,"c_阳曲一期Ⅲ-034 风速","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅲ-034 风速","yc_hs_0499","cur_99"]
[33,"c_阳曲一期Ⅲ-034 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅲ-034 机舱中轴线与风向夹角","yc_hs_0499","cur_100"]
[34,"c_阳曲一期Ⅲ-034 风向","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅲ-034 风向","yc_hs_0500","cur_01"]
[35,"c_阳曲一期Ⅲ-034 舱外温度","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅲ-034 舱外温度","yc_hs_0500","cur_02"]
[36,"c_阳曲一期Ⅲ-034 扭揽角度","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅲ-034 扭揽角度","yc_hs_0500","cur_45"]
[37,"c_阳曲一期Ⅲ-034 1#桨叶片角度","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅲ-034 1#桨叶片角度","yc_hs_0500","cur_46"]
[38,"c_阳曲一期Ⅲ-034 2#桨叶片角度","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅲ-034 2#桨叶片角度","yc_hs_0500","cur_47"]
[39,"c_阳曲一期Ⅲ-034 3#桨叶片角度","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅲ-034 3#桨叶片角度","yc_hs_0500","cur_48"]
[40,"c_阳曲一期Ⅲ-034 发电机转速","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅲ-034 发电机转速","yc_hs_0500","cur_49"]
[41,"c_阳曲一期Ⅲ-034 发电机有功功率","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅲ-034 发电机有功功率","yc_hs_0500","cur_50"]
[42,"c_阳曲一期Ⅲ-034 发电机 绕组温度1","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅲ-034 发电机 绕组温度1","yc_hs_0500","cur_62"]
[43,"c_阳曲一期Ⅲ-034 发电机 绕组温度2","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅲ-034 发电机 绕组温度2","yc_hs_0500","cur_63"]
[44,"c_阳曲一期Ⅲ-034 发电机 绕组温度3","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅲ-034 发电机 绕组温度3","yc_hs_0500","cur_64"]
[45,"c_阳曲一期Ⅲ-034 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅲ-034 机舱侧向振动(已滤波)","yc_hs_0500","cur_69"]
[46,"c_阳曲一期Ⅲ-034 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅲ-034 机舱轴向振动(已滤波)","yc_hs_0500","cur_70"]
[47,"c_阳曲一期Ⅳ-043 舱内温度","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-043 舱内温度","yc_hs_0501","cur_15"]
[48,"c_阳曲一期Ⅳ-044 风速","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-044 风速","yc_hs_0501","cur_22"]
[49,"c_阳曲一期Ⅳ-044 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-044 机舱中轴线与风向夹角","yc_hs_0501","cur_23"]
[50,"c_阳曲一期Ⅳ-044 风向","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-044 风向","yc_hs_0501","cur_24"]
[51,"c_阳曲一期Ⅳ-044 舱外温度","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-044 舱外温度","yc_hs_0501","cur_25"]
[52,"c_阳曲一期Ⅳ-044 扭揽角度","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-044 扭揽角度","yc_hs_0501","cur_26"]
[53,"c_阳曲一期Ⅳ-044 1#桨叶片角度","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-044 1#桨叶片角度","yc_hs_0501","cur_27"]
[54,"c_阳曲一期Ⅳ-044 2#桨叶片角度","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-044 2#桨叶片角度","yc_hs_0501","cur_28"]
[55,"c_阳曲一期Ⅳ-044 3#桨叶片角度","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-044 3#桨叶片角度","yc_hs_0501","cur_70"]
[56,"c_阳曲一期Ⅳ-044 发电机转速","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-044 发电机转速","yc_hs_0501","cur_71"]
[57,"c_阳曲一期Ⅳ-044 发电机有功功率","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-044 发电机有功功率","yc_hs_0501","cur_72"]
[58,"c_阳曲一期Ⅳ-044 发电机 绕组温度1","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-044 发电机 绕组温度1","yc_hs_0501","cur_84"]
[59,"c_阳曲一期Ⅳ-044 发电机 绕组温度2","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-044 发电机 绕组温度2","yc_hs_0501","cur_85"]
[60,"c_阳曲一期Ⅳ-044 发电机 绕组温度3","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-044 发电机 绕组温度3","yc_hs_0501","cur_86"]
[61,"c_阳曲一期Ⅳ-044 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-044 机舱侧向振动(已滤波)","yc_hs_0501","cur_91"]
[62,"c_阳曲一期Ⅳ-044 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-044 机舱轴向振动(已滤波)","yc_hs_0501","cur_92"]
[63,"c_阳曲一期Ⅱ-020 风速","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅱ-020 风速","yc_hs_0501","cur_99"]
[64,"c_阳曲一期Ⅱ-020 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅱ-020 机舱中轴线与风向夹角","yc_hs_0501","cur_100"]
[65,"c_阳曲一期Ⅱ-020 风向","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅱ-020 风向","yc_hs_0502","cur_01"]
[66,"c_阳曲一期Ⅱ-020 舱外温度","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅱ-020 舱外温度","yc_hs_0502","cur_02"]
[67,"c_阳曲一期Ⅱ-020 扭揽角度","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅱ-020 扭揽角度","yc_hs_0502","cur_03"]
[68,"c_阳曲一期Ⅱ-020 1#桨叶片角度","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅱ-020 1#桨叶片角度","yc_hs_0502","cur_04"]
[69,"c_阳曲一期Ⅱ-020 2#桨叶片角度","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅱ-020 2#桨叶片角度","yc_hs_0502","cur_05"]
[70,"c_阳曲一期Ⅱ-020 3#桨叶片角度","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅱ-020 3#桨叶片角度","yc_hs_0502","cur_06"]
[71,"c_阳曲一期Ⅱ-020 发电机转速","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅱ-020 发电机转速","yc_hs_0502","cur_85"]
[72,"c_阳曲一期Ⅱ-020 发电机有功功率","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅱ-020 发电机有功功率","yc_hs_0502","cur_86"]
[73,"c_阳曲一期Ⅱ-020 发电机 绕组温度1","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅱ-020 发电机 绕组温度1","yc_hs_0502","cur_98"]
[74,"c_阳曲一期Ⅱ-020 发电机 绕组温度2","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅱ-020 发电机 绕组温度2","yc_hs_0502","cur_99"]
[75,"c_阳曲一期Ⅱ-020 发电机 绕组温度3","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅱ-020 发电机 绕组温度3","yc_hs_0502","cur_100"]
[76,"c_阳曲一期Ⅱ-020 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅱ-020 机舱侧向振动(已滤波)","yc_hs_0503","cur_05"]
[77,"c_阳曲一期Ⅱ-020 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅱ-020 机舱轴向振动(已滤波)","yc_hs_0503","cur_06"]
[78,"c_阳曲一期Ⅰ-003 风速","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅰ-003 风速","yc_hs_0503","cur_15"]
[79,"c_阳曲一期Ⅰ-003 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅰ-003 机舱中轴线与风向夹角","yc_hs_0503","cur_16"]
[80,"c_阳曲一期Ⅰ-003 风向","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅰ-003 风向","yc_hs_0503","cur_17"]
[81,"c_阳曲一期Ⅰ-003 舱外温度","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅰ-003 舱外温度","yc_hs_0503","cur_18"]
[82,"c_阳曲一期Ⅰ-003 扭揽角度","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅰ-003 扭揽角度","yc_hs_0503","cur_19"]
[83,"c_阳曲一期Ⅰ-003 1#桨叶片角度","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅰ-003 1#桨叶片角度","yc_hs_0503","cur_20"]
[84,"c_阳曲一期Ⅰ-003 2#桨叶片角度","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅰ-003 2#桨叶片角度","yc_hs_0503","cur_21"]
[85,"c_阳曲一期Ⅰ-003 3#桨叶片角度","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅰ-003 3#桨叶片角度","yc_hs_0503","cur_22"]
[86,"c_阳曲一期Ⅰ-003 发电机转速","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅰ-003 发电机转速","yc_hs_0503","cur_23"]
[87,"c_阳曲一期Ⅰ-003 发电机有功功率","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅰ-003 发电机有功功率","yc_hs_0503","cur_24"]
[88,"c_阳曲一期Ⅰ-003 发电机 绕组温度1","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅰ-003 发电机 绕组温度1","yc_hs_0504","cur_14"]
[89,"c_阳曲一期Ⅰ-003 发电机 绕组温度2","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅰ-003 发电机 绕组温度2","yc_hs_0504","cur_15"]
[90,"c_阳曲一期Ⅰ-003 发电机 绕组温度3","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅰ-003 发电机 绕组温度3","yc_hs_0504","cur_16"]
[91,"c_阳曲一期Ⅰ-003 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅰ-003 机舱侧向振动(已滤波)","yc_hs_0504","cur_21"]
[92,"c_阳曲一期Ⅰ-003 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅰ-003 机舱轴向振动(已滤波)","yc_hs_0504","cur_22"]
[93,"c_阳曲一期Ⅰ-003 舱内温度","阳曲风电场","WOF35100072",3,"YNJS.T1_L1.WTG003.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅰ-003 舱内温度","yc_hs_0504","cur_29"]
[94,"c_阳曲一期Ⅱ-020 舱内温度","阳曲风电场","WOF35100072",20,"YNJS.T1_L2.WTG020.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅱ-020 舱内温度","yc_hs_0504","cur_32"]
[95,"c_阳曲一期Ⅲ-034 舱内温度","阳曲风电场","WOF35100072",34,"YNJS.T1_L3.WTG034.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅲ-034 舱内温度","yc_hs_0504","cur_39"]
[96,"c_阳曲一期Ⅲ-035 风速","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅲ-035 风速","yc_hs_0505","cur_26"]
[97,"c_阳曲一期Ⅲ-035 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅲ-035 机舱中轴线与风向夹角","yc_hs_0505","cur_27"]
[98,"c_阳曲一期Ⅲ-035 风向","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅲ-035 风向","yc_hs_0505","cur_28"]
[99,"c_阳曲一期Ⅲ-035 舱外温度","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅲ-035 舱外温度","yc_hs_0505","cur_29"]
[100,"c_阳曲一期Ⅲ-035 扭揽角度","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅲ-035 扭揽角度","yc_hs_0505","cur_30"]
[101,"c_阳曲一期Ⅲ-035 1#桨叶片角度","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅲ-035 1#桨叶片角度","yc_hs_0505","cur_31"]
[102,"c_阳曲一期Ⅲ-035 2#桨叶片角度","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅲ-035 2#桨叶片角度","yc_hs_0505","cur_32"]
[103,"c_阳曲一期Ⅲ-035 3#桨叶片角度","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅲ-035 3#桨叶片角度","yc_hs_0505","cur_33"]
[104,"c_阳曲一期Ⅲ-035 发电机转速","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅲ-035 发电机转速","yc_hs_0505","cur_34"]
[105,"c_阳曲一期Ⅲ-035 发电机有功功率","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅲ-035 发电机有功功率","yc_hs_0505","cur_35"]
[106,"c_阳曲一期Ⅲ-035 发电机 绕组温度1","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅲ-035 发电机 绕组温度1","yc_hs_0505","cur_47"]
[107,"c_阳曲一期Ⅲ-035 发电机 绕组温度2","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅲ-035 发电机 绕组温度2","yc_hs_0505","cur_48"]
[108,"c_阳曲一期Ⅲ-035 发电机 绕组温度3","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅲ-035 发电机 绕组温度3","yc_hs_0505","cur_49"]
[109,"c_阳曲一期Ⅱ-016 风速","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅱ-016 风速","yc_hs_0505","cur_57"]
[110,"c_阳曲一期Ⅱ-016 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅱ-016 机舱中轴线与风向夹角","yc_hs_0505","cur_58"]
[111,"c_阳曲一期Ⅱ-016 风向","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅱ-016 风向","yc_hs_0505","cur_59"]
[112,"c_阳曲一期Ⅱ-016 舱外温度","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅱ-016 舱外温度","yc_hs_0505","cur_60"]
[113,"c_阳曲一期Ⅱ-016 扭揽角度","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅱ-016 扭揽角度","yc_hs_0505","cur_61"]
[114,"c_阳曲一期Ⅱ-016 1#桨叶片角度","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅱ-016 1#桨叶片角度","yc_hs_0505","cur_62"]
[115,"c_阳曲一期Ⅱ-016 2#桨叶片角度","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅱ-016 2#桨叶片角度","yc_hs_0505","cur_63"]
[116,"c_阳曲一期Ⅱ-016 3#桨叶片角度","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅱ-016 3#桨叶片角度","yc_hs_0505","cur_64"]
[117,"c_阳曲一期Ⅱ-016 发电机转速","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅱ-016 发电机转速","yc_hs_0505","cur_65"]
[118,"c_阳曲一期Ⅱ-016 发电机有功功率","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅱ-016 发电机有功功率","yc_hs_0505","cur_66"]
[119,"c_阳曲一期Ⅱ-016 发电机 绕组温度1","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅱ-016 发电机 绕组温度1","yc_hs_0506","cur_56"]
[120,"c_阳曲一期Ⅱ-016 发电机 绕组温度2","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅱ-016 发电机 绕组温度2","yc_hs_0506","cur_57"]
[121,"c_阳曲一期Ⅱ-016 发电机 绕组温度3","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅱ-016 发电机 绕组温度3","yc_hs_0506","cur_58"]
[122,"c_阳曲一期Ⅱ-016 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅱ-016 机舱侧向振动(已滤波)","yc_hs_0506","cur_63"]
[123,"c_阳曲一期Ⅱ-016 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅱ-016 机舱轴向振动(已滤波)","yc_hs_0506","cur_64"]
[124,"c_阳曲一期Ⅳ-046 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-046 机舱侧向振动(已滤波)","yc_hs_0506","cur_74"]
[125,"c_阳曲一期Ⅳ-046 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-046 机舱轴向振动(已滤波)","yc_hs_0506","cur_75"]
[126,"c_阳曲一期Ⅰ-007 风速","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅰ-007 风速","yc_hs_0506","cur_83"]
[127,"c_阳曲一期Ⅰ-007 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅰ-007 机舱中轴线与风向夹角","yc_hs_0506","cur_84"]
[128,"c_阳曲一期Ⅰ-007 风向","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅰ-007 风向","yc_hs_0506","cur_85"]
[129,"c_阳曲一期Ⅰ-007 舱外温度","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅰ-007 舱外温度","yc_hs_0506","cur_86"]
[130,"c_阳曲一期Ⅰ-007 扭揽角度","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅰ-007 扭揽角度","yc_hs_0507","cur_28"]
[131,"c_阳曲一期Ⅰ-007 1#桨叶片角度","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅰ-007 1#桨叶片角度","yc_hs_0507","cur_29"]
[132,"c_阳曲一期Ⅰ-007 2#桨叶片角度","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅰ-007 2#桨叶片角度","yc_hs_0507","cur_30"]
[133,"c_阳曲一期Ⅰ-007 3#桨叶片角度","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅰ-007 3#桨叶片角度","yc_hs_0507","cur_31"]
[134,"c_阳曲一期Ⅰ-007 发电机转速","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅰ-007 发电机转速","yc_hs_0507","cur_32"]
[135,"c_阳曲一期Ⅰ-007 发电机有功功率","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅰ-007 发电机有功功率","yc_hs_0507","cur_33"]
[136,"c_阳曲一期Ⅰ-007 发电机 绕组温度1","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅰ-007 发电机 绕组温度1","yc_hs_0507","cur_45"]
[137,"c_阳曲一期Ⅰ-007 发电机 绕组温度2","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅰ-007 发电机 绕组温度2","yc_hs_0507","cur_46"]
[138,"c_阳曲一期Ⅰ-007 发电机 绕组温度3","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅰ-007 发电机 绕组温度3","yc_hs_0507","cur_47"]
[139,"c_阳曲一期Ⅰ-007 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅰ-007 机舱侧向振动(已滤波)","yc_hs_0507","cur_52"]
[140,"c_阳曲一期Ⅱ-016 舱内温度","阳曲风电场","WOF35100072",16,"YNJS.T1_L2.WTG016.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅱ-016 舱内温度","yc_hs_0507","cur_53"]
[141,"c_阳曲一期Ⅲ-031 风速","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅲ-031 风速","yc_hs_0507","cur_60"]
[142,"c_阳曲一期Ⅲ-031 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅲ-031 机舱中轴线与风向夹角","yc_hs_0507","cur_61"]
[143,"c_阳曲一期Ⅲ-031 风向","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅲ-031 风向","yc_hs_0507","cur_62"]
[144,"c_阳曲一期Ⅲ-031 舱外温度","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅲ-031 舱外温度","yc_hs_0507","cur_63"]
[145,"c_阳曲一期Ⅲ-031 扭揽角度","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅲ-031 扭揽角度","yc_hs_0507","cur_64"]
[146,"c_阳曲一期Ⅲ-031 1#桨叶片角度","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅲ-031 1#桨叶片角度","yc_hs_0507","cur_65"]
[147,"c_阳曲一期Ⅲ-031 2#桨叶片角度","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅲ-031 2#桨叶片角度","yc_hs_0507","cur_66"]
[148,"c_阳曲一期Ⅲ-031 3#桨叶片角度","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅲ-031 3#桨叶片角度","yc_hs_0507","cur_67"]
[149,"c_阳曲一期Ⅲ-031 发电机转速","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅲ-031 发电机转速","yc_hs_0507","cur_68"]
[150,"c_阳曲一期Ⅲ-031 发电机有功功率","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅲ-031 发电机有功功率","yc_hs_0507","cur_69"]
[151,"c_阳曲一期Ⅲ-031 发电机 绕组温度1","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅲ-031 发电机 绕组温度1","yc_hs_0508","cur_43"]
[152,"c_阳曲一期Ⅲ-031 发电机 绕组温度2","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅲ-031 发电机 绕组温度2","yc_hs_0508","cur_44"]
[153,"c_阳曲一期Ⅲ-031 发电机 绕组温度3","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅲ-031 发电机 绕组温度3","yc_hs_0508","cur_45"]
[154,"c_阳曲一期Ⅲ-031 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅲ-031 机舱侧向振动(已滤波)","yc_hs_0508","cur_50"]
[155,"c_阳曲一期Ⅲ-031 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅲ-031 机舱轴向振动(已滤波)","yc_hs_0508","cur_51"]
[156,"c_阳曲一期Ⅳ-037 发电机 绕组温度1","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-037 发电机 绕组温度1","yc_hs_0508","cur_66"]
[157,"c_阳曲一期Ⅳ-037 发电机 绕组温度2","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-037 发电机 绕组温度2","yc_hs_0508","cur_67"]
[158,"c_阳曲一期Ⅳ-037 发电机 绕组温度3","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-037 发电机 绕组温度3","yc_hs_0508","cur_68"]
[159,"c_阳曲一期Ⅳ-037 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-037 机舱侧向振动(已滤波)","yc_hs_0509","cur_51"]
[160,"c_阳曲一期Ⅳ-037 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-037 机舱轴向振动(已滤波)","yc_hs_0509","cur_52"]
[161,"c_阳曲一期Ⅲ-031 舱内温度","阳曲风电场","WOF35100072",31,"YNJS.T1_L3.WTG031.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅲ-031 舱内温度","yc_hs_0509","cur_75"]
[162,"c_阳曲一期Ⅳ-044 舱内温度","阳曲风电场","WOF35100072",44,"YNJS.T1_L4.WTG044.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-044 舱内温度","yc_hs_0509","cur_82"]
[163,"c_阳曲一期Ⅳ-045 风速","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-045 风速","yc_hs_0509","cur_89"]
[164,"c_阳曲一期Ⅳ-045 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-045 机舱中轴线与风向夹角","yc_hs_0510","cur_35"]
[165,"c_阳曲一期Ⅳ-045 风向","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-045 风向","yc_hs_0510","cur_36"]
[166,"c_阳曲一期Ⅳ-045 舱外温度","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-045 舱外温度","yc_hs_0510","cur_37"]
[167,"c_阳曲一期Ⅳ-045 扭揽角度","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-045 扭揽角度","yc_hs_0510","cur_38"]
[168,"c_阳曲一期Ⅳ-045 1#桨叶片角度","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-045 1#桨叶片角度","yc_hs_0510","cur_39"]
[169,"c_阳曲一期Ⅳ-045 2#桨叶片角度","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-045 2#桨叶片角度","yc_hs_0510","cur_40"]
[170,"c_阳曲一期Ⅳ-045 3#桨叶片角度","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-045 3#桨叶片角度","yc_hs_0510","cur_41"]
[171,"c_阳曲一期Ⅳ-045 发电机转速","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-045 发电机转速","yc_hs_0510","cur_42"]
[172,"c_阳曲一期Ⅳ-045 发电机有功功率","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-045 发电机有功功率","yc_hs_0510","cur_43"]
[173,"c_阳曲一期Ⅳ-045 发电机 绕组温度1","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-045 发电机 绕组温度1","yc_hs_0510","cur_55"]
[174,"c_阳曲一期Ⅳ-045 发电机 绕组温度2","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-045 发电机 绕组温度2","yc_hs_0510","cur_56"]
[175,"c_阳曲一期Ⅳ-045 发电机 绕组温度3","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-045 发电机 绕组温度3","yc_hs_0510","cur_57"]
[176,"c_阳曲一期Ⅱ-021 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅱ-021 机舱侧向振动(已滤波)","yc_hs_0510","cur_59"]
[177,"c_阳曲一期Ⅱ-021 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅱ-021 机舱轴向振动(已滤波)","yc_hs_0510","cur_60"]
[178,"c_阳曲一期Ⅱ-021 舱内温度","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅱ-021 舱内温度","yc_hs_0510","cur_67"]
[179,"c_阳曲一期Ⅲ-035 舱内温度","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅲ-035 舱内温度","yc_hs_0510","cur_74"]
[180,"c_阳曲一期Ⅲ-036 风速","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅲ-036 风速","yc_hs_0497","cur_06"]
[181,"c_阳曲一期Ⅲ-036 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅲ-036 机舱中轴线与风向夹角","yc_hs_0497","cur_07"]
[182,"c_阳曲一期Ⅲ-036 风向","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅲ-036 风向","yc_hs_0497","cur_08"]
[183,"c_阳曲一期Ⅲ-036 舱外温度","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅲ-036 舱外温度","yc_hs_0497","cur_09"]
[184,"c_阳曲一期Ⅲ-036 扭揽角度","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅲ-036 扭揽角度","yc_hs_0497","cur_10"]
[185,"c_阳曲一期Ⅲ-036 1#桨叶片角度","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅲ-036 1#桨叶片角度","yc_hs_0497","cur_11"]
[186,"c_阳曲一期Ⅲ-036 2#桨叶片角度","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅲ-036 2#桨叶片角度","yc_hs_0497","cur_12"]
[187,"c_阳曲一期Ⅲ-036 3#桨叶片角度","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅲ-036 3#桨叶片角度","yc_hs_0497","cur_13"]
[188,"c_阳曲一期Ⅲ-036 发电机转速","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅲ-036 发电机转速","yc_hs_0497","cur_14"]
[189,"c_阳曲一期Ⅲ-036 发电机有功功率","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅲ-036 发电机有功功率","yc_hs_0497","cur_15"]
[190,"c_阳曲一期Ⅳ-045 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-045 机舱侧向振动(已滤波)","yc_hs_0497","cur_28"]
[191,"c_阳曲一期Ⅳ-045 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-045 机舱轴向振动(已滤波)","yc_hs_0497","cur_29"]
[192,"c_阳曲一期Ⅰ-004 风速","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅰ-004 风速","yc_hs_0497","cur_36"]
[193,"c_阳曲一期Ⅰ-004 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅰ-004 机舱中轴线与风向夹角","yc_hs_0497","cur_37"]
[194,"c_阳曲一期Ⅰ-004 风向","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅰ-004 风向","yc_hs_0497","cur_38"]
[195,"c_阳曲一期Ⅰ-004 舱外温度","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅰ-004 舱外温度","yc_hs_0497","cur_39"]
[196,"c_阳曲一期Ⅰ-004 扭揽角度","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅰ-004 扭揽角度","yc_hs_0497","cur_40"]
[197,"c_阳曲一期Ⅰ-004 1#桨叶片角度","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅰ-004 1#桨叶片角度","yc_hs_0497","cur_41"]
[198,"c_阳曲一期Ⅰ-004 2#桨叶片角度","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅰ-004 2#桨叶片角度","yc_hs_0499","cur_21"]
[199,"c_阳曲一期Ⅰ-004 3#桨叶片角度","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅰ-004 3#桨叶片角度","yc_hs_0499","cur_22"]
[200,"c_阳曲一期Ⅰ-004 发电机转速","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅰ-004 发电机转速","yc_hs_0499","cur_23"]
[201,"c_阳曲一期Ⅰ-004 发电机有功功率","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅰ-004 发电机有功功率","yc_hs_0499","cur_24"]
[202,"c_阳曲一期Ⅰ-004 发电机 绕组温度1","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅰ-004 发电机 绕组温度1","yc_hs_0499","cur_36"]
[203,"c_阳曲一期Ⅰ-004 发电机 绕组温度2","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅰ-004 发电机 绕组温度2","yc_hs_0499","cur_37"]
[204,"c_阳曲一期Ⅰ-004 发电机 绕组温度3","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅰ-004 发电机 绕组温度3","yc_hs_0499","cur_38"]
[205,"c_阳曲一期Ⅰ-004 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅰ-004 机舱侧向振动(已滤波)","yc_hs_0499","cur_43"]
[206,"c_阳曲一期Ⅰ-004 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅰ-004 机舱轴向振动(已滤波)","yc_hs_0499","cur_44"]
[207,"c_阳曲一期Ⅳ-049 发电机 绕组温度1","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-049 发电机 绕组温度1","yc_hs_0499","cur_48"]
[208,"c_阳曲一期Ⅳ-049 发电机 绕组温度2","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-049 发电机 绕组温度2","yc_hs_0499","cur_49"]
[209,"c_阳曲一期Ⅳ-049 发电机 绕组温度3","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-049 发电机 绕组温度3","yc_hs_0499","cur_50"]
[210,"c_阳曲一期Ⅳ-049 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-049 机舱侧向振动(已滤波)","yc_hs_0499","cur_55"]
[211,"c_阳曲一期Ⅳ-049 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-049 机舱轴向振动(已滤波)","yc_hs_0499","cur_56"]
[212,"c_阳曲一期Ⅰ-008 风速","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅰ-008 风速","yc_hs_0500","cur_05"]
[213,"c_阳曲一期Ⅰ-008 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅰ-008 机舱中轴线与风向夹角","yc_hs_0500","cur_06"]
[214,"c_阳曲一期Ⅰ-008 风向","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅰ-008 风向","yc_hs_0500","cur_07"]
[215,"c_阳曲一期Ⅰ-008 舱外温度","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅰ-008 舱外温度","yc_hs_0500","cur_08"]
[216,"c_阳曲一期Ⅰ-008 扭揽角度","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅰ-008 扭揽角度","yc_hs_0500","cur_09"]
[217,"c_阳曲一期Ⅰ-008 1#桨叶片角度","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅰ-008 1#桨叶片角度","yc_hs_0500","cur_10"]
[218,"c_阳曲一期Ⅰ-008 2#桨叶片角度","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅰ-008 2#桨叶片角度","yc_hs_0500","cur_11"]
[219,"c_阳曲一期Ⅰ-008 3#桨叶片角度","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅰ-008 3#桨叶片角度","yc_hs_0500","cur_12"]
[220,"c_阳曲一期Ⅰ-008 发电机转速","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅰ-008 发电机转速","yc_hs_0500","cur_13"]
[221,"c_阳曲一期Ⅰ-008 发电机有功功率","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅰ-008 发电机有功功率","yc_hs_0500","cur_14"]
[222,"c_阳曲一期Ⅰ-004 舱内温度","阳曲风电场","WOF35100072",4,"YNJS.T1_L1.WTG004.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅰ-004 舱内温度","yc_hs_0500","cur_33"]
[223,"c_阳曲一期Ⅱ-017 风速","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅱ-017 风速","yc_hs_0500","cur_40"]
[224,"c_阳曲一期Ⅱ-017 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅱ-017 机舱中轴线与风向夹角","yc_hs_0500","cur_41"]
[225,"c_阳曲一期Ⅱ-017 风向","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅱ-017 风向","yc_hs_0500","cur_42"]
[226,"c_阳曲一期Ⅱ-017 舱外温度","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅱ-017 舱外温度","yc_hs_0500","cur_43"]
[227,"c_阳曲一期Ⅱ-017 扭揽角度","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅱ-017 扭揽角度","yc_hs_0500","cur_44"]
[228,"c_阳曲一期Ⅱ-017 1#桨叶片角度","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅱ-017 1#桨叶片角度","yc_hs_0500","cur_75"]
[229,"c_阳曲一期Ⅱ-017 2#桨叶片角度","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅱ-017 2#桨叶片角度","yc_hs_0500","cur_76"]
[230,"c_阳曲一期Ⅱ-017 3#桨叶片角度","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅱ-017 3#桨叶片角度","yc_hs_0500","cur_77"]
[231,"c_阳曲一期Ⅱ-017 发电机转速","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅱ-017 发电机转速","yc_hs_0500","cur_78"]
[232,"c_阳曲一期Ⅱ-017 发电机有功功率","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅱ-017 发电机有功功率","yc_hs_0500","cur_79"]
[233,"c_阳曲一期Ⅱ-017 发电机 绕组温度1","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅱ-017 发电机 绕组温度1","yc_hs_0500","cur_91"]
[234,"c_阳曲一期Ⅱ-017 发电机 绕组温度2","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅱ-017 发电机 绕组温度2","yc_hs_0500","cur_92"]
[235,"c_阳曲一期Ⅱ-017 发电机 绕组温度3","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅱ-017 发电机 绕组温度3","yc_hs_0500","cur_93"]
[236,"c_阳曲一期Ⅰ-009 风速","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅰ-009 风速","yc_hs_0501","cur_36"]
[237,"c_阳曲一期Ⅰ-009 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅰ-009 机舱中轴线与风向夹角","yc_hs_0501","cur_37"]
[238,"c_阳曲一期Ⅰ-009 风向","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅰ-009 风向","yc_hs_0501","cur_38"]
[239,"c_阳曲一期Ⅰ-009 舱外温度","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅰ-009 舱外温度","yc_hs_0501","cur_39"]
[240,"c_阳曲一期Ⅰ-009 扭揽角度","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅰ-009 扭揽角度","yc_hs_0501","cur_40"]
[241,"c_阳曲一期Ⅰ-009 1#桨叶片角度","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅰ-009 1#桨叶片角度","yc_hs_0501","cur_41"]
[242,"c_阳曲一期Ⅰ-009 2#桨叶片角度","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅰ-009 2#桨叶片角度","yc_hs_0501","cur_42"]
[243,"c_阳曲一期Ⅰ-009 3#桨叶片角度","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅰ-009 3#桨叶片角度","yc_hs_0501","cur_43"]
[244,"c_阳曲一期Ⅰ-009 发电机转速","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅰ-009 发电机转速","yc_hs_0501","cur_44"]
[245,"c_阳曲一期Ⅰ-009 发电机有功功率","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅰ-009 发电机有功功率","yc_hs_0501","cur_45"]
[246,"c_阳曲一期Ⅱ-017 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅱ-017 机舱侧向振动(已滤波)","yc_hs_0501","cur_52"]
[247,"c_阳曲一期Ⅱ-017 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅱ-017 机舱轴向振动(已滤波)","yc_hs_0501","cur_53"]
[248,"c_阳曲一期Ⅱ-017 舱内温度","阳曲风电场","WOF35100072",17,"YNJS.T1_L2.WTG017.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅱ-017 舱内温度","yc_hs_0501","cur_60"]
[249,"c_阳曲一期Ⅲ-032 风速","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅲ-032 风速","yc_hs_0501","cur_67"]
[250,"c_阳曲一期Ⅲ-032 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅲ-032 机舱中轴线与风向夹角","yc_hs_0501","cur_68"]
[251,"c_阳曲一期Ⅲ-032 风向","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅲ-032 风向","yc_hs_0501","cur_69"]
[252,"c_阳曲一期Ⅲ-032 舱外温度","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅲ-032 舱外温度","yc_hs_0502","cur_07"]
[253,"c_阳曲一期Ⅲ-032 扭揽角度","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅲ-032 扭揽角度","yc_hs_0502","cur_08"]
[254,"c_阳曲一期Ⅲ-032 1#桨叶片角度","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅲ-032 1#桨叶片角度","yc_hs_0502","cur_09"]
[255,"c_阳曲一期Ⅲ-032 2#桨叶片角度","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅲ-032 2#桨叶片角度","yc_hs_0502","cur_10"]
[256,"c_阳曲一期Ⅲ-032 3#桨叶片角度","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅲ-032 3#桨叶片角度","yc_hs_0502","cur_11"]
[257,"c_阳曲一期Ⅲ-032 发电机转速","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅲ-032 发电机转速","yc_hs_0502","cur_12"]
[258,"c_阳曲一期Ⅲ-032 发电机有功功率","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅲ-032 发电机有功功率","yc_hs_0502","cur_13"]
[259,"c_阳曲一期Ⅲ-032 发电机 绕组温度1","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅲ-032 发电机 绕组温度1","yc_hs_0502","cur_25"]
[260,"c_阳曲一期Ⅲ-032 发电机 绕组温度2","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅲ-032 发电机 绕组温度2","yc_hs_0502","cur_26"]
[261,"c_阳曲一期Ⅲ-032 发电机 绕组温度3","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅲ-032 发电机 绕组温度3","yc_hs_0502","cur_27"]
[262,"c_阳曲一期Ⅲ-036 发电机 绕组温度1","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅲ-036 发电机 绕组温度1","yc_hs_0502","cur_32"]
[263,"c_阳曲一期Ⅲ-036 发电机 绕组温度2","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅲ-036 发电机 绕组温度2","yc_hs_0502","cur_33"]
[264,"c_阳曲一期Ⅲ-036 发电机 绕组温度3","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅲ-036 发电机 绕组温度3","yc_hs_0502","cur_34"]
[265,"c_阳曲一期Ⅲ-036 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅲ-036 机舱侧向振动(已滤波)","yc_hs_0502","cur_39"]
[266,"c_阳曲一期Ⅲ-036 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅲ-036 机舱轴向振动(已滤波)","yc_hs_0502","cur_40"]
[267,"c_阳曲一期Ⅳ-048 舱内温度","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-048 舱内温度","yc_hs_0502","cur_46"]
[268,"c_阳曲一期Ⅳ-049 风速","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-049 风速","yc_hs_0503","cur_32"]
[269,"c_阳曲一期Ⅳ-049 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-049 机舱中轴线与风向夹角","yc_hs_0503","cur_33"]
[270,"c_阳曲一期Ⅳ-049 风向","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-049 风向","yc_hs_0503","cur_34"]
[271,"c_阳曲一期Ⅳ-049 舱外温度","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-049 舱外温度","yc_hs_0503","cur_35"]
[272,"c_阳曲一期Ⅳ-049 扭揽角度","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-049 扭揽角度","yc_hs_0503","cur_36"]
[273,"c_阳曲一期Ⅳ-049 1#桨叶片角度","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-049 1#桨叶片角度","yc_hs_0503","cur_37"]
[274,"c_阳曲一期Ⅳ-049 2#桨叶片角度","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-049 2#桨叶片角度","yc_hs_0503","cur_38"]
[275,"c_阳曲一期Ⅳ-049 3#桨叶片角度","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-049 3#桨叶片角度","yc_hs_0503","cur_39"]
[276,"c_阳曲一期Ⅳ-049 发电机转速","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-049 发电机转速","yc_hs_0503","cur_40"]
[277,"c_阳曲一期Ⅳ-049 发电机有功功率","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-049 发电机有功功率","yc_hs_0503","cur_41"]
[278,"c_阳曲一期Ⅲ-032 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅲ-032 机舱侧向振动(已滤波)","yc_hs_0503","cur_52"]
[279,"c_阳曲一期Ⅲ-032 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅲ-032 机舱轴向振动(已滤波)","yc_hs_0503","cur_53"]
[280,"c_阳曲一期Ⅲ-032 舱内温度","阳曲风电场","WOF35100072",32,"YNJS.T1_L3.WTG032.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅲ-032 舱内温度","yc_hs_0503","cur_60"]
[281,"c_阳曲一期Ⅳ-050 舱内温度","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-050 舱内温度","yc_hs_0503","cur_67"]
[282,"c_阳曲一期Ⅰ-008 发电机 绕组温度1","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅰ-008 发电机 绕组温度1","yc_hs_0504","cur_66"]
[283,"c_阳曲一期Ⅰ-008 发电机 绕组温度2","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅰ-008 发电机 绕组温度2","yc_hs_0504","cur_67"]
[284,"c_阳曲一期Ⅰ-008 发电机 绕组温度3","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅰ-008 发电机 绕组温度3","yc_hs_0504","cur_68"]
[285,"c_阳曲一期Ⅰ-008 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅰ-008 机舱侧向振动(已滤波)","yc_hs_0504","cur_73"]
[286,"c_阳曲一期Ⅰ-008 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅰ-008 机舱轴向振动(已滤波)","yc_hs_0504","cur_74"]
[287,"c_阳曲一期Ⅰ-008 舱内温度","阳曲风电场","WOF35100072",8,"YNJS.T1_L1.WTG008.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅰ-008 舱内温度","yc_hs_0504","cur_81"]
[288,"c_阳曲一期Ⅱ-022 风速","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅱ-022 风速","yc_hs_0505","cur_70"]
[289,"c_阳曲一期Ⅱ-022 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅱ-022 机舱中轴线与风向夹角","yc_hs_0505","cur_71"]
[290,"c_阳曲一期Ⅱ-022 风向","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅱ-022 风向","yc_hs_0505","cur_72"]
[291,"c_阳曲一期Ⅱ-022 舱外温度","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅱ-022 舱外温度","yc_hs_0505","cur_73"]
[292,"c_阳曲一期Ⅱ-022 扭揽角度","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅱ-022 扭揽角度","yc_hs_0505","cur_74"]
[293,"c_阳曲一期Ⅱ-022 1#桨叶片角度","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅱ-022 1#桨叶片角度","yc_hs_0505","cur_75"]
[294,"c_阳曲一期Ⅱ-022 2#桨叶片角度","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅱ-022 2#桨叶片角度","yc_hs_0505","cur_76"]
[295,"c_阳曲一期Ⅱ-022 3#桨叶片角度","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅱ-022 3#桨叶片角度","yc_hs_0505","cur_77"]
[296,"c_阳曲一期Ⅱ-022 发电机转速","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅱ-022 发电机转速","yc_hs_0505","cur_78"]
[297,"c_阳曲一期Ⅱ-022 发电机有功功率","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅱ-022 发电机有功功率","yc_hs_0505","cur_79"]
[298,"c_阳曲一期Ⅲ-029 风速","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅲ-029 风速","yc_hs_0505","cur_93"]
[299,"c_阳曲一期Ⅲ-029 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅲ-029 机舱中轴线与风向夹角","yc_hs_0505","cur_94"]
[300,"c_阳曲一期Ⅲ-029 风向","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅲ-029 风向","yc_hs_0505","cur_95"]
[301,"c_阳曲一期Ⅲ-029 舱外温度","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅲ-029 舱外温度","yc_hs_0505","cur_96"]
[302,"c_阳曲一期Ⅲ-029 扭揽角度","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅲ-029 扭揽角度","yc_hs_0505","cur_97"]
[303,"c_阳曲一期Ⅲ-029 1#桨叶片角度","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅲ-029 1#桨叶片角度","yc_hs_0505","cur_98"]
[304,"c_阳曲一期Ⅲ-029 2#桨叶片角度","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅲ-029 2#桨叶片角度","yc_hs_0505","cur_99"]
[305,"c_阳曲一期Ⅲ-029 3#桨叶片角度","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅲ-029 3#桨叶片角度","yc_hs_0505","cur_100"]
[306,"c_阳曲一期Ⅲ-029 发电机转速","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅲ-029 发电机转速","yc_hs_0506","cur_01"]
[307,"c_阳曲一期Ⅰ-005 风速","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅰ-005 风速","yc_hs_0506","cur_96"]
[308,"c_阳曲一期Ⅰ-005 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅰ-005 机舱中轴线与风向夹角","yc_hs_0506","cur_97"]
[309,"c_阳曲一期Ⅰ-005 风向","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅰ-005 风向","yc_hs_0506","cur_98"]
[310,"c_阳曲一期Ⅰ-005 舱外温度","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅰ-005 舱外温度","yc_hs_0506","cur_99"]
[311,"c_阳曲一期Ⅰ-005 扭揽角度","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅰ-005 扭揽角度","yc_hs_0506","cur_100"]
[312,"c_阳曲一期Ⅰ-005 1#桨叶片角度","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅰ-005 1#桨叶片角度","yc_hs_0507","cur_01"]
[313,"c_阳曲一期Ⅰ-005 2#桨叶片角度","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅰ-005 2#桨叶片角度","yc_hs_0507","cur_02"]
[314,"c_阳曲一期Ⅰ-005 3#桨叶片角度","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅰ-005 3#桨叶片角度","yc_hs_0507","cur_03"]
[315,"c_阳曲一期Ⅰ-005 发电机转速","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅰ-005 发电机转速","yc_hs_0507","cur_04"]
[316,"c_阳曲一期Ⅰ-005 发电机有功功率","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅰ-005 发电机有功功率","yc_hs_0507","cur_05"]
[317,"c_阳曲一期Ⅰ-005 发电机 绕组温度1","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅰ-005 发电机 绕组温度1","yc_hs_0507","cur_17"]
[318,"c_阳曲一期Ⅰ-005 发电机 绕组温度2","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅰ-005 发电机 绕组温度2","yc_hs_0507","cur_18"]
[319,"c_阳曲一期Ⅰ-009 发电机 绕组温度1","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅰ-009 发电机 绕组温度1","yc_hs_0507","cur_24"]
[320,"c_阳曲一期Ⅰ-009 发电机 绕组温度2","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅰ-009 发电机 绕组温度2","yc_hs_0507","cur_25"]
[321,"c_阳曲一期Ⅰ-009 发电机 绕组温度3","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅰ-009 发电机 绕组温度3","yc_hs_0507","cur_26"]
[322,"c_阳曲一期Ⅰ-009 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅰ-009 机舱侧向振动(已滤波)","yc_hs_0507","cur_73"]
[323,"c_阳曲一期Ⅰ-009 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅰ-009 机舱轴向振动(已滤波)","yc_hs_0507","cur_74"]
[324,"c_阳曲一期Ⅰ-009 舱内温度","阳曲风电场","WOF35100072",9,"YNJS.T1_L1.WTG009.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅰ-009 舱内温度","yc_hs_0507","cur_81"]
[325,"c_阳曲一期Ⅱ-023 风速","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅱ-023 风速","yc_hs_0507","cur_88"]
[326,"c_阳曲一期Ⅱ-023 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅱ-023 机舱中轴线与风向夹角","yc_hs_0507","cur_89"]
[327,"c_阳曲一期Ⅱ-023 风向","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅱ-023 风向","yc_hs_0507","cur_90"]
[328,"c_阳曲一期Ⅱ-023 舱外温度","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅱ-023 舱外温度","yc_hs_0507","cur_91"]
[329,"c_阳曲一期Ⅱ-023 扭揽角度","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅱ-023 扭揽角度","yc_hs_0507","cur_92"]
[330,"c_阳曲一期Ⅱ-023 1#桨叶片角度","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅱ-023 1#桨叶片角度","yc_hs_0507","cur_93"]
[331,"c_阳曲一期Ⅱ-023 2#桨叶片角度","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅱ-023 2#桨叶片角度","yc_hs_0507","cur_94"]
[332,"c_阳曲一期Ⅱ-023 3#桨叶片角度","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅱ-023 3#桨叶片角度","yc_hs_0507","cur_95"]
[333,"c_阳曲一期Ⅱ-023 发电机转速","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅱ-023 发电机转速","yc_hs_0507","cur_96"]
[334,"c_阳曲一期Ⅱ-023 发电机有功功率","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅱ-023 发电机有功功率","yc_hs_0507","cur_97"]
[335,"c_阳曲一期Ⅲ-029 发电机有功功率","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅲ-029 发电机有功功率","yc_hs_0508","cur_02"]
[336,"c_阳曲一期Ⅲ-029 发电机 绕组温度1","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅲ-029 发电机 绕组温度1","yc_hs_0508","cur_76"]
[337,"c_阳曲一期Ⅲ-029 发电机 绕组温度2","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅲ-029 发电机 绕组温度2","yc_hs_0508","cur_77"]
[338,"c_阳曲一期Ⅲ-029 发电机 绕组温度3","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅲ-029 发电机 绕组温度3","yc_hs_0508","cur_78"]
[339,"c_阳曲一期Ⅲ-029 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅲ-029 机舱侧向振动(已滤波)","yc_hs_0508","cur_83"]
[340,"c_阳曲一期Ⅲ-029 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅲ-029 机舱轴向振动(已滤波)","yc_hs_0508","cur_84"]
[341,"c_阳曲一期Ⅲ-029 舱内温度","阳曲风电场","WOF35100072",29,"YNJS.T1_L3.WTG029.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅲ-029 舱内温度","yc_hs_0508","cur_91"]
[342,"c_阳曲一期Ⅳ-042 舱内温度","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-042 舱内温度","yc_hs_0508","cur_98"]
[343,"c_阳曲一期Ⅰ-005 发电机 绕组温度3","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅰ-005 发电机 绕组温度3","yc_hs_0509","cur_05"]
[344,"c_阳曲一期Ⅰ-005 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅰ-005 机舱侧向振动(已滤波)","yc_hs_0509","cur_10"]
[345,"c_阳曲一期Ⅰ-005 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅰ-005 机舱轴向振动(已滤波)","yc_hs_0509","cur_11"]
[346,"c_阳曲一期Ⅰ-005 舱内温度","阳曲风电场","WOF35100072",5,"YNJS.T1_L1.WTG005.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅰ-005 舱内温度","yc_hs_0509","cur_94"]
[347,"c_阳曲一期Ⅱ-018 风速","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅱ-018 风速","yc_hs_0510","cur_01"]
[348,"c_阳曲一期Ⅱ-018 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅱ-018 机舱中轴线与风向夹角","yc_hs_0510","cur_02"]
[349,"c_阳曲一期Ⅱ-018 风向","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅱ-018 风向","yc_hs_0510","cur_03"]
[350,"c_阳曲一期Ⅱ-018 舱外温度","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅱ-018 舱外温度","yc_hs_0510","cur_04"]
[351,"c_阳曲一期Ⅱ-018 扭揽角度","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅱ-018 扭揽角度","yc_hs_0510","cur_05"]
[352,"c_阳曲一期Ⅱ-018 1#桨叶片角度","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅱ-018 1#桨叶片角度","yc_hs_0510","cur_06"]
[353,"c_阳曲一期Ⅱ-018 2#桨叶片角度","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅱ-018 2#桨叶片角度","yc_hs_0510","cur_07"]
[354,"c_阳曲一期Ⅱ-018 3#桨叶片角度","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅱ-018 3#桨叶片角度","yc_hs_0510","cur_08"]
[355,"c_阳曲一期Ⅱ-018 发电机转速","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅱ-018 发电机转速","yc_hs_0510","cur_09"]
[356,"c_阳曲一期Ⅱ-018 发电机有功功率","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅱ-018 发电机有功功率","yc_hs_0510","cur_10"]
[357,"c_阳曲一期Ⅲ-035 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅲ-035 机舱侧向振动(已滤波)","yc_hs_0510","cur_24"]
[358,"c_阳曲一期Ⅲ-035 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",35,"YNJS.T1_L3.WTG035.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅲ-035 机舱轴向振动(已滤波)","yc_hs_0510","cur_25"]
[359,"c_阳曲一期Ⅳ-045 舱内温度","阳曲风电场","WOF35100072",45,"YNJS.T1_L4.WTG045.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-045 舱内温度","yc_hs_0510","cur_76"]
[360,"c_阳曲一期Ⅳ-046 风速","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-046 风速","yc_hs_0510","cur_83"]
[361,"c_阳曲一期Ⅳ-046 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-046 机舱中轴线与风向夹角","yc_hs_0510","cur_84"]
[362,"c_阳曲一期Ⅳ-046 风向","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-046 风向","yc_hs_0510","cur_85"]
[363,"c_阳曲一期Ⅳ-046 舱外温度","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-046 舱外温度","yc_hs_0510","cur_86"]
[364,"c_阳曲一期Ⅳ-046 扭揽角度","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-046 扭揽角度","yc_hs_0510","cur_87"]
[365,"c_阳曲一期Ⅳ-046 1#桨叶片角度","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-046 1#桨叶片角度","yc_hs_0510","cur_88"]
[366,"c_阳曲一期Ⅳ-046 2#桨叶片角度","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-046 2#桨叶片角度","yc_hs_0510","cur_89"]
[367,"c_阳曲一期Ⅳ-046 3#桨叶片角度","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-046 3#桨叶片角度","yc_hs_0510","cur_90"]
[368,"c_阳曲一期Ⅳ-046 发电机转速","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-046 发电机转速","yc_hs_0510","cur_91"]
[369,"c_阳曲一期Ⅳ-046 发电机有功功率","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-046 发电机有功功率","yc_hs_0510","cur_92"]
[370,"c_阳曲一期Ⅳ-046 发电机 绕组温度1","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-046 发电机 绕组温度1","yc_hs_0511","cur_04"]
[371,"c_阳曲一期Ⅳ-046 发电机 绕组温度2","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-046 发电机 绕组温度2","yc_hs_0511","cur_05"]
[372,"c_阳曲一期Ⅳ-046 发电机 绕组温度3","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-046 发电机 绕组温度3","yc_hs_0511","cur_06"]
[373,"c_阳曲一期Ⅳ-043 风速","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-043 风速","yc_hs_0511","cur_08"]
[374,"c_阳曲一期Ⅳ-043 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-043 机舱中轴线与风向夹角","yc_hs_0511","cur_09"]
[375,"c_阳曲一期Ⅳ-043 风向","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-043 风向","yc_hs_0511","cur_10"]
[376,"c_阳曲一期Ⅳ-043 舱外温度","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-043 舱外温度","yc_hs_0511","cur_11"]
[377,"c_阳曲一期Ⅳ-043 扭揽角度","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-043 扭揽角度","yc_hs_0511","cur_12"]
[378,"c_阳曲一期Ⅳ-043 1#桨叶片角度","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-043 1#桨叶片角度","yc_hs_0511","cur_13"]
[379,"c_阳曲一期Ⅳ-043 2#桨叶片角度","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-043 2#桨叶片角度","yc_hs_0511","cur_14"]
[380,"c_阳曲一期Ⅳ-043 3#桨叶片角度","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-043 3#桨叶片角度","yc_hs_0511","cur_15"]
[381,"c_阳曲一期Ⅳ-043 发电机转速","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-043 发电机转速","yc_hs_0511","cur_16"]
[382,"c_阳曲一期Ⅳ-043 发电机有功功率","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-043 发电机有功功率","yc_hs_0497","cur_42"]
[383,"c_阳曲一期Ⅳ-043 发电机 绕组温度1","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-043 发电机 绕组温度1","yc_hs_0497","cur_54"]
[384,"c_阳曲一期Ⅳ-043 发电机 绕组温度2","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-043 发电机 绕组温度2","yc_hs_0497","cur_55"]
[385,"c_阳曲一期Ⅳ-043 发电机 绕组温度3","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-043 发电机 绕组温度3","yc_hs_0497","cur_56"]
[386,"c_阳曲一期Ⅳ-043 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-043 机舱侧向振动(已滤波)","yc_hs_0497","cur_61"]
[387,"c_阳曲一期Ⅳ-043 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",43,"YNJS.T1_L4.WTG043.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-043 机舱轴向振动(已滤波)","yc_hs_0497","cur_62"]
[388,"c_阳曲一期Ⅰ-002 风速","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅰ-002 风速","yc_hs_0497","cur_69"]
[389,"c_阳曲一期Ⅰ-002 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅰ-002 机舱中轴线与风向夹角","yc_hs_0497","cur_70"]
[390,"c_阳曲一期Ⅰ-002 风向","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅰ-002 风向","yc_hs_0497","cur_71"]
[391,"c_阳曲一期Ⅰ-002 舱外温度","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅰ-002 舱外温度","yc_hs_0497","cur_72"]
[392,"c_阳曲一期Ⅰ-002 扭揽角度","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅰ-002 扭揽角度","yc_hs_0497","cur_73"]
[393,"c_阳曲一期Ⅱ-018 发电机 绕组温度1","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅱ-018 发电机 绕组温度1","yc_hs_0497","cur_74"]
[394,"c_阳曲一期Ⅱ-018 发电机 绕组温度2","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅱ-018 发电机 绕组温度2","yc_hs_0497","cur_75"]
[395,"c_阳曲一期Ⅱ-018 发电机 绕组温度3","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅱ-018 发电机 绕组温度3","yc_hs_0497","cur_76"]
[396,"c_阳曲一期Ⅱ-018 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅱ-018 机舱侧向振动(已滤波)","yc_hs_0497","cur_81"]
[397,"c_阳曲一期Ⅱ-018 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅱ-018 机舱轴向振动(已滤波)","yc_hs_0497","cur_82"]
[398,"c_阳曲一期Ⅱ-018 舱内温度","阳曲风电场","WOF35100072",18,"YNJS.T1_L2.WTG018.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅱ-018 舱内温度","yc_hs_0497","cur_89"]
[399,"c_阳曲一期Ⅲ-033 风速","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅲ-033 风速","yc_hs_0497","cur_96"]
[400,"c_阳曲一期Ⅲ-033 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅲ-033 机舱中轴线与风向夹角","yc_hs_0497","cur_97"]
[401,"c_阳曲一期Ⅲ-033 风向","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅲ-033 风向","yc_hs_0497","cur_98"]
[402,"c_阳曲一期Ⅲ-033 舱外温度","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅲ-033 舱外温度","yc_hs_0497","cur_99"]
[403,"c_阳曲一期Ⅲ-033 扭揽角度","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅲ-033 扭揽角度","yc_hs_0497","cur_100"]
[404,"c_阳曲一期Ⅲ-033 1#桨叶片角度","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅲ-033 1#桨叶片角度","yc_hs_0498","cur_01"]
[405,"c_阳曲一期Ⅲ-033 2#桨叶片角度","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅲ-033 2#桨叶片角度","yc_hs_0498","cur_02"]
[406,"c_阳曲一期Ⅲ-033 3#桨叶片角度","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅲ-033 3#桨叶片角度","yc_hs_0498","cur_03"]
[407,"c_阳曲一期Ⅲ-033 发电机转速","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅲ-033 发电机转速","yc_hs_0498","cur_04"]
[408,"c_阳曲一期Ⅲ-033 发电机有功功率","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅲ-033 发电机有功功率","yc_hs_0498","cur_05"]
[409,"c_阳曲一期Ⅱ-022 发电机 绕组温度1","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅱ-022 发电机 绕组温度1","yc_hs_0498","cur_16"]
[410,"c_阳曲一期Ⅱ-022 发电机 绕组温度2","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅱ-022 发电机 绕组温度2","yc_hs_0498","cur_17"]
[411,"c_阳曲一期Ⅱ-022 发电机 绕组温度3","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅱ-022 发电机 绕组温度3","yc_hs_0498","cur_18"]
[412,"c_阳曲一期Ⅱ-022 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅱ-022 机舱侧向振动(已滤波)","yc_hs_0498","cur_23"]
[413,"c_阳曲一期Ⅱ-022 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅱ-022 机舱轴向振动(已滤波)","yc_hs_0498","cur_39"]
[414,"c_阳曲一期Ⅱ-022 舱内温度","阳曲风电场","WOF35100072",22,"YNJS.T1_L2.WTG022.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅱ-022 舱内温度","yc_hs_0498","cur_46"]
[415,"c_阳曲一期Ⅲ-036 舱内温度","阳曲风电场","WOF35100072",36,"YNJS.T1_L3.WTG036.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅲ-036 舱内温度","yc_hs_0498","cur_53"]
[416,"c_阳曲一期Ⅳ-037 风速","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-037 风速","yc_hs_0498","cur_60"]
[417,"c_阳曲一期Ⅳ-037 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-037 机舱中轴线与风向夹角","yc_hs_0498","cur_61"]
[418,"c_阳曲一期Ⅳ-037 风向","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-037 风向","yc_hs_0498","cur_62"]
[419,"c_阳曲一期Ⅳ-037 舱外温度","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-037 舱外温度","yc_hs_0498","cur_63"]
[420,"c_阳曲一期Ⅳ-037 扭揽角度","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-037 扭揽角度","yc_hs_0498","cur_64"]
[421,"c_阳曲一期Ⅳ-037 1#桨叶片角度","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-037 1#桨叶片角度","yc_hs_0498","cur_65"]
[422,"c_阳曲一期Ⅳ-037 2#桨叶片角度","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-037 2#桨叶片角度","yc_hs_0498","cur_66"]
[423,"c_阳曲一期Ⅳ-037 3#桨叶片角度","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-037 3#桨叶片角度","yc_hs_0498","cur_67"]
[424,"c_阳曲一期Ⅳ-037 发电机转速","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-037 发电机转速","yc_hs_0498","cur_68"]
[425,"c_阳曲一期Ⅳ-037 发电机有功功率","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-037 发电机有功功率","yc_hs_0498","cur_69"]
[426,"c_阳曲一期Ⅰ-002 1#桨叶片角度","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅰ-002 1#桨叶片角度","yc_hs_0498","cur_71"]
[427,"c_阳曲一期Ⅰ-002 2#桨叶片角度","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅰ-002 2#桨叶片角度","yc_hs_0498","cur_72"]
[428,"c_阳曲一期Ⅰ-002 3#桨叶片角度","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅰ-002 3#桨叶片角度","yc_hs_0498","cur_73"]
[429,"c_阳曲一期Ⅰ-002 发电机转速","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅰ-002 发电机转速","yc_hs_0498","cur_74"]
[430,"c_阳曲一期Ⅰ-002 发电机有功功率","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅰ-002 发电机有功功率","yc_hs_0498","cur_75"]
[431,"c_阳曲一期Ⅰ-002 发电机 绕组温度1","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅰ-002 发电机 绕组温度1","yc_hs_0504","cur_92"]
[432,"c_阳曲一期Ⅰ-002 发电机 绕组温度2","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅰ-002 发电机 绕组温度2","yc_hs_0504","cur_93"]
[433,"c_阳曲一期Ⅰ-002 发电机 绕组温度3","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅰ-002 发电机 绕组温度3","yc_hs_0504","cur_94"]
[434,"c_阳曲一期Ⅰ-002 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅰ-002 机舱侧向振动(已滤波)","yc_hs_0504","cur_99"]
[435,"c_阳曲一期Ⅰ-002 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅰ-002 机舱轴向振动(已滤波)","yc_hs_0504","cur_100"]
[436,"c_阳曲一期Ⅰ-002 舱内温度","阳曲风电场","WOF35100072",2,"YNJS.T1_L1.WTG002.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅰ-002 舱内温度","yc_hs_0505","cur_07"]
[437,"c_阳曲一期Ⅱ-015 风速","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅱ-015 风速","yc_hs_0505","cur_14"]
[438,"c_阳曲一期Ⅱ-015 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅱ-015 机舱中轴线与风向夹角","yc_hs_0505","cur_15"]
[439,"c_阳曲一期Ⅱ-015 风向","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅱ-015 风向","yc_hs_0505","cur_16"]
[440,"c_阳曲一期Ⅲ-033 发电机 绕组温度1","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅲ-033 发电机 绕组温度1","yc_hs_0505","cur_19"]
[441,"c_阳曲一期Ⅲ-033 发电机 绕组温度2","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅲ-033 发电机 绕组温度2","yc_hs_0505","cur_20"]
[442,"c_阳曲一期Ⅲ-033 发电机 绕组温度3","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅲ-033 发电机 绕组温度3","yc_hs_0505","cur_21"]
[443,"c_阳曲一期Ⅲ-033 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅲ-033 机舱侧向振动(已滤波)","yc_hs_0508","cur_13"]
[444,"c_阳曲一期Ⅲ-033 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅲ-033 机舱轴向振动(已滤波)","yc_hs_0508","cur_11"]
[445,"c_阳曲一期Ⅲ-033 舱内温度","阳曲风电场","WOF35100072",33,"YNJS.T1_L3.WTG033.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅲ-033 舱内温度","yc_hs_0508","cur_19"]
[446,"c_阳曲一期Ⅰ-007 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅰ-007 机舱轴向振动(已滤波)","yc_hs_0508","cur_23"]
[447,"c_阳曲一期Ⅰ-007 舱内温度","阳曲风电场","WOF35100072",7,"YNJS.T1_L1.WTG007.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅰ-007 舱内温度","yc_hs_0508","cur_30"]
[448,"c_阳曲一期Ⅱ-021 风速","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅱ-021 风速","yc_hs_0502","cur_53"]
[449,"c_阳曲一期Ⅱ-021 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅱ-021 机舱中轴线与风向夹角","yc_hs_0502","cur_54"]
[450,"c_阳曲一期Ⅱ-021 风向","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅱ-021 风向","yc_hs_0502","cur_55"]
[451,"c_阳曲一期Ⅱ-021 舱外温度","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅱ-021 舱外温度","yc_hs_0502","cur_56"]
[452,"c_阳曲一期Ⅱ-021 扭揽角度","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅱ-021 扭揽角度","yc_hs_0502","cur_57"]
[453,"c_阳曲一期Ⅱ-021 1#桨叶片角度","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅱ-021 1#桨叶片角度","yc_hs_0502","cur_58"]
[454,"c_阳曲一期Ⅱ-021 2#桨叶片角度","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅱ-021 2#桨叶片角度","yc_hs_0502","cur_59"]
[455,"c_阳曲一期Ⅱ-021 3#桨叶片角度","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅱ-021 3#桨叶片角度","yc_hs_0502","cur_60"]
[456,"c_阳曲一期Ⅱ-021 发电机转速","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅱ-021 发电机转速","yc_hs_0502","cur_61"]
[457,"c_阳曲一期Ⅱ-021 发电机有功功率","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅱ-021 发电机有功功率","yc_hs_0502","cur_62"]
[458,"c_阳曲一期Ⅱ-021 发电机 绕组温度1","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅱ-021 发电机 绕组温度1","yc_hs_0502","cur_74"]
[459,"c_阳曲一期Ⅱ-021 发电机 绕组温度2","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅱ-021 发电机 绕组温度2","yc_hs_0502","cur_75"]
[460,"c_阳曲一期Ⅱ-021 发电机 绕组温度3","阳曲风电场","WOF35100072",21,"YNJS.T1_L2.WTG021.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅱ-021 发电机 绕组温度3","yc_hs_0502","cur_76"]
[461,"c_阳曲一期Ⅱ-015 舱外温度","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅱ-015 舱外温度","yc_hs_0502","cur_81"]
[462,"c_阳曲一期Ⅱ-015 扭揽角度","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅱ-015 扭揽角度","yc_hs_0502","cur_82"]
[463,"c_阳曲一期Ⅱ-015 1#桨叶片角度","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅱ-015 1#桨叶片角度","yc_hs_0502","cur_83"]
[464,"c_阳曲一期Ⅱ-015 2#桨叶片角度","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅱ-015 2#桨叶片角度","yc_hs_0502","cur_84"]
[465,"c_阳曲一期Ⅱ-015 3#桨叶片角度","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅱ-015 3#桨叶片角度","yc_hs_0503","cur_68"]
[466,"c_阳曲一期Ⅱ-015 发电机转速","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅱ-015 发电机转速","yc_hs_0503","cur_69"]
[467,"c_阳曲一期Ⅱ-015 发电机有功功率","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅱ-015 发电机有功功率","yc_hs_0503","cur_70"]
[468,"c_阳曲一期Ⅱ-015 发电机 绕组温度1","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅱ-015 发电机 绕组温度1","yc_hs_0503","cur_82"]
[469,"c_阳曲一期Ⅱ-015 发电机 绕组温度2","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅱ-015 发电机 绕组温度2","yc_hs_0503","cur_83"]
[470,"c_阳曲一期Ⅱ-015 发电机 绕组温度3","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅱ-015 发电机 绕组温度3","yc_hs_0503","cur_84"]
[471,"c_阳曲一期Ⅱ-015 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅱ-015 机舱侧向振动(已滤波)","yc_hs_0503","cur_89"]
[472,"c_阳曲一期Ⅱ-015 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅱ-015 机舱轴向振动(已滤波)","yc_hs_0503","cur_90"]
[473,"c_阳曲一期Ⅱ-015 舱内温度","阳曲风电场","WOF35100072",15,"YNJS.T1_L2.WTG015.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅱ-015 舱内温度","yc_hs_0503","cur_97"]
[474,"c_阳曲一期Ⅲ-030 风速","阳曲风电场","WOF35100072",30,"YNJS.T1_L3.WTG030.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅲ-030 风速","yc_hs_0504","cur_04"]
[475,"c_阳曲一期Ⅱ-019 风速","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅱ-019 风速","yc_hs_0506","cur_12"]
[476,"c_阳曲一期Ⅱ-019 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅱ-019 机舱中轴线与风向夹角","yc_hs_0506","cur_13"]
[477,"c_阳曲一期Ⅱ-019 风向","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅱ-019 风向","yc_hs_0506","cur_14"]
[478,"c_阳曲一期Ⅱ-019 舱外温度","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅱ-019 舱外温度","yc_hs_0506","cur_15"]
[479,"c_阳曲一期Ⅱ-019 扭揽角度","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅱ-019 扭揽角度","yc_hs_0506","cur_16"]
[480,"c_阳曲一期Ⅱ-019 1#桨叶片角度","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅱ-019 1#桨叶片角度","yc_hs_0506","cur_17"]
[481,"c_阳曲一期Ⅱ-019 2#桨叶片角度","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅱ-019 2#桨叶片角度","yc_hs_0506","cur_18"]
[482,"c_阳曲一期Ⅱ-019 3#桨叶片角度","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅱ-019 3#桨叶片角度","yc_hs_0506","cur_19"]
[483,"c_阳曲一期Ⅱ-019 发电机转速","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅱ-019 发电机转速","yc_hs_0506","cur_20"]
[484,"c_阳曲一期Ⅱ-019 发电机有功功率","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅱ-019 发电机有功功率","yc_hs_0506","cur_21"]
[485,"c_阳曲一期Ⅱ-019 发电机 绕组温度1","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅱ-019 发电机 绕组温度1","yc_hs_0506","cur_33"]
[486,"c_阳曲一期Ⅱ-019 发电机 绕组温度2","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅱ-019 发电机 绕组温度2","yc_hs_0506","cur_34"]
[487,"c_阳曲一期Ⅱ-019 发电机 绕组温度3","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅱ-019 发电机 绕组温度3","yc_hs_0506","cur_35"]
[488,"c_阳曲一期Ⅱ-019 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅱ-019 机舱侧向振动(已滤波)","yc_hs_0506","cur_40"]
[489,"c_阳曲一期Ⅱ-019 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",19,"YNJS.T1_L2.WTG019.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅱ-019 机舱轴向振动(已滤波)","yc_hs_0506","cur_41"]
[493,"c_阳曲一期Ⅳ-048 发电机 绕组温度3","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-048 发电机 绕组温度3","yc_hs_0510","cur_31"]
[494,"c_阳曲一期Ⅳ-048 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-048 机舱侧向振动(已滤波)","yc_hs_0509","cur_15"]
[495,"c_阳曲一期Ⅳ-048 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-048 机舱轴向振动(已滤波)","yc_hs_0509","cur_16"]
[496,"c_阳曲一期Ⅰ-013 风速","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅰ-013 风速","yc_hs_0509","cur_24"]
[497,"c_阳曲一期Ⅰ-013 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅰ-013 机舱中轴线与风向夹角","yc_hs_0509","cur_25"]
[498,"c_阳曲一期Ⅰ-013 风向","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅰ-013 风向","yc_hs_0509","cur_26"]
[499,"c_阳曲一期Ⅰ-013 舱外温度","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅰ-013 舱外温度","yc_hs_0509","cur_27"]
[500,"c_阳曲一期Ⅰ-013 扭揽角度","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅰ-013 扭揽角度","yc_hs_0509","cur_28"]
[501,"c_阳曲一期Ⅰ-013 1#桨叶片角度","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅰ-013 1#桨叶片角度","yc_hs_0509","cur_29"]
[502,"c_阳曲一期Ⅰ-013 2#桨叶片角度","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅰ-013 2#桨叶片角度","yc_hs_0509","cur_30"]
[503,"c_阳曲一期Ⅰ-013 3#桨叶片角度","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅰ-013 3#桨叶片角度","yc_hs_0509","cur_31"]
[504,"c_阳曲一期Ⅰ-013 发电机转速","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅰ-013 发电机转速","yc_hs_0509","cur_32"]
[505,"c_阳曲一期Ⅰ-013 发电机有功功率","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅰ-013 发电机有功功率","yc_hs_0509","cur_33"]
[506,"c_阳曲一期Ⅰ-013 发电机 绕组温度1","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅰ-013 发电机 绕组温度1","yc_hs_0509","cur_45"]
[507,"c_阳曲一期Ⅰ-013 发电机 绕组温度2","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅰ-013 发电机 绕组温度2","yc_hs_0509","cur_46"]
[508,"c_阳曲一期Ⅰ-013 发电机 绕组温度3","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅰ-013 发电机 绕组温度3","yc_hs_0509","cur_47"]
[513,"c_阳曲一期Ⅱ-023 发电机 绕组温度1","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅱ-023 发电机 绕组温度1","yc_hs_0513","cur_23"]
[514,"c_阳曲一期Ⅱ-023 发电机 绕组温度2","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅱ-023 发电机 绕组温度2","yc_hs_0513","cur_24"]
[515,"c_阳曲一期Ⅱ-023 发电机 绕组温度3","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅱ-023 发电机 绕组温度3","yc_hs_0513","cur_25"]
[516,"c_阳曲一期Ⅱ-023 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅱ-023 机舱侧向振动(已滤波)","yc_hs_0513","cur_30"]
[517,"c_阳曲一期Ⅱ-023 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅱ-023 机舱轴向振动(已滤波)","yc_hs_0513","cur_31"]
[518,"c_阳曲一期Ⅱ-023 舱内温度","阳曲风电场","WOF35100072",23,"YNJS.T1_L2.WTG023.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅱ-023 舱内温度","yc_hs_0513","cur_38"]
[519,"c_阳曲一期Ⅳ-037 舱内温度","阳曲风电场","WOF35100072",37,"YNJS.T1_L4.WTG037.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-037 舱内温度","yc_hs_0513","cur_45"]
[520,"c_阳曲一期Ⅳ-038 风速","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-038 风速","yc_hs_0513","cur_52"]
[521,"c_阳曲一期Ⅳ-038 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-038 机舱中轴线与风向夹角","yc_hs_0513","cur_53"]
[522,"c_阳曲一期Ⅳ-038 风向","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-038 风向","yc_hs_0513","cur_54"]
[523,"c_阳曲一期Ⅳ-038 舱外温度","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-038 舱外温度","yc_hs_0513","cur_55"]
[524,"c_阳曲一期Ⅳ-038 扭揽角度","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-038 扭揽角度","yc_hs_0513","cur_56"]
[525,"c_阳曲一期Ⅰ-013 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅰ-013 机舱侧向振动(已滤波)","yc_hs_0513","cur_58"]
[526,"c_阳曲一期Ⅰ-013 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅰ-013 机舱轴向振动(已滤波)","yc_hs_0513","cur_59"]
[527,"c_阳曲一期Ⅰ-013 舱内温度","阳曲风电场","WOF35100072",13,"YNJS.T1_L1.WTG013.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅰ-013 舱内温度","yc_hs_0514","cur_02"]
[528,"c_阳曲一期Ⅲ-027 风速","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅲ-027 风速","yc_hs_0514","cur_09"]
[529,"c_阳曲一期Ⅲ-027 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅲ-027 机舱中轴线与风向夹角","yc_hs_0514","cur_10"]
[530,"c_阳曲一期Ⅲ-027 风向","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅲ-027 风向","yc_hs_0514","cur_11"]
[531,"c_阳曲一期Ⅲ-027 舱外温度","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅲ-027 舱外温度","yc_hs_0514","cur_12"]
[532,"c_阳曲一期Ⅲ-027 扭揽角度","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅲ-027 扭揽角度","yc_hs_0514","cur_13"]
[533,"c_阳曲一期Ⅲ-027 1#桨叶片角度","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅲ-027 1#桨叶片角度","yc_hs_0514","cur_14"]
[534,"c_阳曲一期Ⅲ-027 2#桨叶片角度","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅲ-027 2#桨叶片角度","yc_hs_0514","cur_15"]
[535,"c_阳曲一期Ⅲ-027 3#桨叶片角度","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅲ-027 3#桨叶片角度","yc_hs_0514","cur_16"]
[536,"c_阳曲一期Ⅲ-027 发电机转速","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅲ-027 发电机转速","yc_hs_0514","cur_17"]
[537,"c_阳曲一期Ⅲ-027 发电机有功功率","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅲ-027 发电机有功功率","yc_hs_0514","cur_18"]
[538,"c_阳曲一期Ⅲ-027 发电机 绕组温度1","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅲ-027 发电机 绕组温度1","yc_hs_0514","cur_30"]
[539,"c_阳曲一期Ⅲ-027 发电机 绕组温度2","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅲ-027 发电机 绕组温度2","yc_hs_0514","cur_31"]
[540,"c_阳曲一期Ⅲ-027 发电机 绕组温度3","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅲ-027 发电机 绕组温度3","yc_hs_0514","cur_32"]
[547,"c_阳曲一期Ⅳ-038 1#桨叶片角度","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-038 1#桨叶片角度","yc_hs_0514","cur_53"]
[548,"c_阳曲一期Ⅳ-038 2#桨叶片角度","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-038 2#桨叶片角度","yc_hs_0514","cur_54"]
[549,"c_阳曲一期Ⅳ-038 3#桨叶片角度","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-038 3#桨叶片角度","yc_hs_0514","cur_55"]
[550,"c_阳曲一期Ⅳ-038 发电机转速","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-038 发电机转速","yc_hs_0514","cur_56"]
[551,"c_阳曲一期Ⅳ-038 发电机有功功率","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-038 发电机有功功率","yc_hs_0515","cur_20"]
[552,"c_阳曲一期Ⅳ-038 发电机 绕组温度1","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-038 发电机 绕组温度1","yc_hs_0515","cur_32"]
[553,"c_阳曲一期Ⅳ-038 发电机 绕组温度2","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-038 发电机 绕组温度2","yc_hs_0515","cur_33"]
[554,"c_阳曲一期Ⅳ-038 发电机 绕组温度3","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-038 发电机 绕组温度3","yc_hs_0515","cur_34"]
[555,"c_阳曲一期Ⅳ-038 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-038 机舱侧向振动(已滤波)","yc_hs_0515","cur_39"]
[556,"c_阳曲一期Ⅳ-038 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-038 机舱轴向振动(已滤波)","yc_hs_0515","cur_40"]
[557,"c_阳曲一期Ⅳ-046 舱内温度","阳曲风电场","WOF35100072",46,"YNJS.T1_L4.WTG046.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-046 舱内温度","yc_hs_0515","cur_46"]
[558,"c_阳曲一期Ⅳ-047 风速","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-047 风速","yc_hs_0515","cur_53"]
[559,"c_阳曲一期Ⅳ-047 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-047 机舱中轴线与风向夹角","yc_hs_0515","cur_54"]
[560,"c_阳曲一期Ⅳ-047 风向","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-047 风向","yc_hs_0515","cur_55"]
[561,"c_阳曲一期Ⅳ-047 舱外温度","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-047 舱外温度","yc_hs_0515","cur_56"]
[562,"c_阳曲一期Ⅲ-027 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅲ-027 机舱侧向振动(已滤波)","yc_hs_0515","cur_60"]
[563,"c_阳曲一期Ⅲ-027 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅲ-027 机舱轴向振动(已滤波)","yc_hs_0515","cur_61"]
[564,"c_阳曲一期Ⅲ-027 舱内温度","阳曲风电场","WOF35100072",27,"YNJS.T1_L3.WTG027.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅲ-027 舱内温度","yc_hs_0515","cur_68"]
[565,"c_阳曲一期Ⅳ-041 舱内温度","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-041 舱内温度","yc_hs_0515","cur_75"]
[566,"c_阳曲一期Ⅳ-042 风速","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-042 风速","yc_hs_0515","cur_82"]
[567,"c_阳曲一期Ⅳ-042 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-042 机舱中轴线与风向夹角","yc_hs_0515","cur_83"]
[568,"c_阳曲一期Ⅳ-042 风向","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-042 风向","yc_hs_0515","cur_84"]
[569,"c_阳曲一期Ⅳ-042 舱外温度","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-042 舱外温度","yc_hs_0515","cur_85"]
[570,"c_阳曲一期Ⅳ-042 扭揽角度","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-042 扭揽角度","yc_hs_0515","cur_86"]
[571,"c_阳曲一期Ⅳ-042 1#桨叶片角度","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-042 1#桨叶片角度","yc_hs_0515","cur_87"]
[572,"c_阳曲一期Ⅳ-042 2#桨叶片角度","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-042 2#桨叶片角度","yc_hs_0515","cur_88"]
[573,"c_阳曲一期Ⅳ-042 3#桨叶片角度","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-042 3#桨叶片角度","yc_hs_0515","cur_89"]
[574,"c_阳曲一期Ⅳ-042 发电机转速","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-042 发电机转速","yc_hs_0515","cur_90"]
[575,"c_阳曲一期Ⅳ-042 发电机有功功率","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-042 发电机有功功率","yc_hs_0515","cur_91"]
[578,"c_阳曲一期Ⅳ-047 扭揽角度","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-047 扭揽角度","yc_hs_0516","cur_59"]
[579,"c_阳曲一期Ⅳ-047 1#桨叶片角度","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-047 1#桨叶片角度","yc_hs_0516","cur_60"]
[580,"c_阳曲一期Ⅳ-047 2#桨叶片角度","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-047 2#桨叶片角度","yc_hs_0516","cur_61"]
[581,"c_阳曲一期Ⅳ-047 3#桨叶片角度","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-047 3#桨叶片角度","yc_hs_0516","cur_62"]
[582,"c_阳曲一期Ⅳ-047 发电机转速","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-047 发电机转速","yc_hs_0517","cur_39"]
[583,"c_阳曲一期Ⅳ-047 发电机有功功率","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-047 发电机有功功率","yc_hs_0517","cur_40"]
[584,"c_阳曲一期Ⅳ-047 发电机 绕组温度1","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-047 发电机 绕组温度1","yc_hs_0517","cur_52"]
[585,"c_阳曲一期Ⅳ-047 发电机 绕组温度2","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-047 发电机 绕组温度2","yc_hs_0517","cur_53"]
[586,"c_阳曲一期Ⅳ-047 发电机 绕组温度3","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-047 发电机 绕组温度3","yc_hs_0517","cur_54"]
[587,"c_阳曲一期Ⅳ-047 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-047 机舱侧向振动(已滤波)","yc_hs_0517","cur_59"]
[588,"c_阳曲一期Ⅳ-047 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-047 机舱轴向振动(已滤波)","yc_hs_0517","cur_60"]
[589,"c_阳曲一期Ⅰ-010 风速","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅰ-010 风速","yc_hs_0517","cur_68"]
[590,"c_阳曲一期Ⅰ-010 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅰ-010 机舱中轴线与风向夹角","yc_hs_0517","cur_69"]
[591,"c_阳曲一期Ⅰ-010 风向","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅰ-010 风向","yc_hs_0517","cur_70"]
[592,"c_阳曲一期Ⅰ-010 舱外温度","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅰ-010 舱外温度","yc_hs_0517","cur_71"]
[593,"c_阳曲一期Ⅰ-010 扭揽角度","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅰ-010 扭揽角度","yc_hs_0517","cur_72"]
[594,"c_阳曲一期Ⅰ-010 1#桨叶片角度","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅰ-010 1#桨叶片角度","yc_hs_0517","cur_73"]
[595,"c_阳曲一期Ⅰ-010 2#桨叶片角度","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅰ-010 2#桨叶片角度","yc_hs_0517","cur_74"]
[596,"c_阳曲一期Ⅰ-010 3#桨叶片角度","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅰ-010 3#桨叶片角度","yc_hs_0517","cur_75"]
[597,"c_阳曲一期Ⅳ-042 发电机 绕组温度1","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-042 发电机 绕组温度1","yc_hs_0518","cur_08"]
[598,"c_阳曲一期Ⅳ-042 发电机 绕组温度2","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-042 发电机 绕组温度2","yc_hs_0518","cur_09"]
[599,"c_阳曲一期Ⅳ-042 发电机 绕组温度3","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-042 发电机 绕组温度3","yc_hs_0518","cur_10"]
[600,"c_阳曲一期Ⅳ-042 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-042 机舱侧向振动(已滤波)","yc_hs_0518","cur_15"]
[601,"c_阳曲一期Ⅳ-042 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",42,"YNJS.T1_L4.WTG042.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-042 机舱轴向振动(已滤波)","yc_hs_0518","cur_16"]
[602,"c_阳曲一期Ⅰ-001 风速","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅰ-001 风速","yc_hs_0518","cur_23"]
[603,"c_阳曲一期Ⅰ-001 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅰ-001 机舱中轴线与风向夹角","yc_hs_0518","cur_24"]
[604,"c_阳曲一期Ⅰ-001 风向","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅰ-001 风向","yc_hs_0518","cur_25"]
[605,"c_阳曲一期Ⅰ-001 舱外温度","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅰ-001 舱外温度","yc_hs_0518","cur_26"]
[606,"c_阳曲一期Ⅰ-001 扭揽角度","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅰ-001 扭揽角度","yc_hs_0518","cur_27"]
[607,"c_阳曲一期Ⅰ-001 1#桨叶片角度","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅰ-001 1#桨叶片角度","yc_hs_0518","cur_28"]
[608,"c_阳曲一期Ⅰ-001 2#桨叶片角度","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅰ-001 2#桨叶片角度","yc_hs_0518","cur_29"]
[609,"c_阳曲一期Ⅰ-001 3#桨叶片角度","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅰ-001 3#桨叶片角度","yc_hs_0518","cur_30"]
[610,"c_阳曲一期Ⅰ-001 发电机转速","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅰ-001 发电机转速","yc_hs_0518","cur_31"]
[611,"c_阳曲一期Ⅰ-001 发电机有功功率","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅰ-001 发电机有功功率","yc_hs_0518","cur_32"]
[619,"c_阳曲一期Ⅰ-010 发电机转速","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅰ-010 发电机转速","yc_hs_0519","cur_06"]
[620,"c_阳曲一期Ⅰ-010 发电机有功功率","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅰ-010 发电机有功功率","yc_hs_0519","cur_07"]
[621,"c_阳曲一期Ⅰ-010 发电机 绕组温度1","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅰ-010 发电机 绕组温度1","yc_hs_0511","cur_63"]
[622,"c_阳曲一期Ⅰ-010 发电机 绕组温度2","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅰ-010 发电机 绕组温度2","yc_hs_0511","cur_64"]
[623,"c_阳曲一期Ⅰ-010 发电机 绕组温度3","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅰ-010 发电机 绕组温度3","yc_hs_0511","cur_65"]
[624,"c_阳曲一期Ⅰ-010 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅰ-010 机舱侧向振动(已滤波)","yc_hs_0511","cur_70"]
[625,"c_阳曲一期Ⅰ-010 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅰ-010 机舱轴向振动(已滤波)","yc_hs_0511","cur_71"]
[626,"c_阳曲一期Ⅰ-010 舱内温度","阳曲风电场","WOF35100072",10,"YNJS.T1_L1.WTG010.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅰ-010 舱内温度","yc_hs_0511","cur_78"]
[627,"c_阳曲一期Ⅱ-024 风速","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅱ-024 风速","yc_hs_0511","cur_85"]
[628,"c_阳曲一期Ⅱ-024 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅱ-024 机舱中轴线与风向夹角","yc_hs_0511","cur_86"]
[629,"c_阳曲一期Ⅱ-024 风向","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅱ-024 风向","yc_hs_0511","cur_87"]
[630,"c_阳曲一期Ⅱ-024 舱外温度","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅱ-024 舱外温度","yc_hs_0511","cur_88"]
[631,"c_阳曲一期Ⅱ-024 扭揽角度","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅱ-024 扭揽角度","yc_hs_0511","cur_89"]
[632,"c_阳曲一期Ⅱ-024 1#桨叶片角度","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅱ-024 1#桨叶片角度","yc_hs_0511","cur_90"]
[633,"c_阳曲一期Ⅰ-001 发电机 绕组温度1","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅰ-001 发电机 绕组温度1","yc_hs_0511","cur_91"]
[634,"c_阳曲一期Ⅰ-001 发电机 绕组温度2","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅰ-001 发电机 绕组温度2","yc_hs_0511","cur_92"]
[635,"c_阳曲一期Ⅰ-001 发电机 绕组温度3","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅰ-001 发电机 绕组温度3","yc_hs_0511","cur_93"]
[636,"c_阳曲一期Ⅰ-001 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅰ-001 机舱侧向振动(已滤波)","yc_hs_0511","cur_98"]
[637,"c_阳曲一期Ⅰ-001 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅰ-001 机舱轴向振动(已滤波)","yc_hs_0511","cur_99"]
[638,"c_阳曲一期Ⅰ-001 舱内温度","阳曲风电场","WOF35100072",1,"YNJS.T1_L1.WTG001.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅰ-001 舱内温度","yc_hs_0512","cur_06"]
[639,"c_阳曲一期Ⅱ-014 风速","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅱ-014 风速","yc_hs_0512","cur_13"]
[640,"c_阳曲一期Ⅱ-014 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅱ-014 机舱中轴线与风向夹角","yc_hs_0512","cur_14"]
[641,"c_阳曲一期Ⅱ-014 风向","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅱ-014 风向","yc_hs_0512","cur_15"]
[642,"c_阳曲一期Ⅱ-014 舱外温度","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅱ-014 舱外温度","yc_hs_0512","cur_16"]
[643,"c_阳曲一期Ⅱ-014 扭揽角度","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅱ-014 扭揽角度","yc_hs_0512","cur_17"]
[644,"c_阳曲一期Ⅱ-014 1#桨叶片角度","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅱ-014 1#桨叶片角度","yc_hs_0512","cur_18"]
[645,"c_阳曲一期Ⅱ-014 2#桨叶片角度","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅱ-014 2#桨叶片角度","yc_hs_0512","cur_19"]
[646,"c_阳曲一期Ⅱ-014 3#桨叶片角度","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅱ-014 3#桨叶片角度","yc_hs_0512","cur_20"]
[647,"c_阳曲一期Ⅱ-014 发电机转速","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅱ-014 发电机转速","yc_hs_0512","cur_21"]
[648,"c_阳曲一期Ⅱ-014 发电机有功功率","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅱ-014 发电机有功功率","yc_hs_0512","cur_22"]
[650,"c_阳曲一期Ⅱ-024 2#桨叶片角度","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅱ-024 2#桨叶片角度","yc_hs_0512","cur_86"]
[651,"c_阳曲一期Ⅱ-024 3#桨叶片角度","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅱ-024 3#桨叶片角度","yc_hs_0512","cur_87"]
[652,"c_阳曲一期Ⅱ-024 发电机转速","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅱ-024 发电机转速","yc_hs_0512","cur_88"]
[653,"c_阳曲一期Ⅱ-024 发电机有功功率","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅱ-024 发电机有功功率","yc_hs_0512","cur_89"]
[654,"c_阳曲一期Ⅱ-024 发电机 绕组温度1","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅱ-024 发电机 绕组温度1","yc_hs_0513","cur_71"]
[655,"c_阳曲一期Ⅱ-024 发电机 绕组温度2","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅱ-024 发电机 绕组温度2","yc_hs_0513","cur_72"]
[656,"c_阳曲一期Ⅱ-024 发电机 绕组温度3","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅱ-024 发电机 绕组温度3","yc_hs_0513","cur_73"]
[657,"c_阳曲一期Ⅱ-024 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅱ-024 机舱侧向振动(已滤波)","yc_hs_0513","cur_78"]
[658,"c_阳曲一期Ⅱ-024 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅱ-024 机舱轴向振动(已滤波)","yc_hs_0513","cur_79"]
[659,"c_阳曲一期Ⅱ-024 舱内温度","阳曲风电场","WOF35100072",24,"YNJS.T1_L2.WTG024.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅱ-024 舱内温度","yc_hs_0513","cur_86"]
[660,"c_阳曲一期Ⅳ-038 舱内温度","阳曲风电场","WOF35100072",38,"YNJS.T1_L4.WTG038.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-038 舱内温度","yc_hs_0513","cur_93"]
[666,"c_阳曲一期Ⅳ-039 风速","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-039 风速","yc_hs_0514","cur_37"]
[667,"c_阳曲一期Ⅳ-039 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-039 机舱中轴线与风向夹角","yc_hs_0514","cur_38"]
[668,"c_阳曲一期Ⅳ-039 风向","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-039 风向","yc_hs_0514","cur_39"]
[669,"c_阳曲一期Ⅳ-039 舱外温度","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-039 舱外温度","yc_hs_0514","cur_57"]
[670,"c_阳曲一期Ⅳ-039 扭揽角度","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-039 扭揽角度","yc_hs_0514","cur_58"]
[671,"c_阳曲一期Ⅳ-039 1#桨叶片角度","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-039 1#桨叶片角度","yc_hs_0514","cur_59"]
[672,"c_阳曲一期Ⅳ-039 2#桨叶片角度","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-039 2#桨叶片角度","yc_hs_0514","cur_60"]
[673,"c_阳曲一期Ⅳ-039 3#桨叶片角度","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-039 3#桨叶片角度","yc_hs_0514","cur_61"]
[674,"c_阳曲一期Ⅳ-039 发电机转速","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-039 发电机转速","yc_hs_0514","cur_62"]
[675,"c_阳曲一期Ⅳ-039 发电机有功功率","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-039 发电机有功功率","yc_hs_0514","cur_63"]
[676,"c_阳曲一期Ⅳ-039 发电机 绕组温度1","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-039 发电机 绕组温度1","yc_hs_0514","cur_75"]
[677,"c_阳曲一期Ⅳ-039 发电机 绕组温度2","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-039 发电机 绕组温度2","yc_hs_0514","cur_76"]
[678,"c_阳曲一期Ⅳ-039 发电机 绕组温度3","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-039 发电机 绕组温度3","yc_hs_0514","cur_77"]
[679,"c_阳曲一期Ⅳ-039 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-039 机舱侧向振动(已滤波)","yc_hs_0514","cur_82"]
[680,"c_阳曲一期Ⅳ-039 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-039 机舱轴向振动(已滤波)","yc_hs_0514","cur_83"]
[681,"c_阳曲一期Ⅳ-049 舱内温度","阳曲风电场","WOF35100072",49,"YNJS.T1_L4.WTG049.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-049 舱内温度","yc_hs_0514","cur_89"]
[684,"c_阳曲一期Ⅳ-050 风速","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-050 风速","yc_hs_0516","cur_02"]
[685,"c_阳曲一期Ⅳ-050 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-050 机舱中轴线与风向夹角","yc_hs_0516","cur_03"]
[686,"c_阳曲一期Ⅳ-050 风向","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-050 风向","yc_hs_0516","cur_04"]
[687,"c_阳曲一期Ⅳ-050 舱外温度","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-050 舱外温度","yc_hs_0516","cur_05"]
[688,"c_阳曲一期Ⅳ-050 扭揽角度","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-050 扭揽角度","yc_hs_0516","cur_06"]
[689,"c_阳曲一期Ⅳ-050 1#桨叶片角度","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-050 1#桨叶片角度","yc_hs_0516","cur_07"]
[690,"c_阳曲一期Ⅳ-050 2#桨叶片角度","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-050 2#桨叶片角度","yc_hs_0516","cur_08"]
[691,"c_阳曲一期Ⅳ-050 3#桨叶片角度","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-050 3#桨叶片角度","yc_hs_0516","cur_09"]
[692,"c_阳曲一期Ⅳ-050 发电机转速","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-050 发电机转速","yc_hs_0516","cur_10"]
[693,"c_阳曲一期Ⅳ-050 发电机有功功率","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-050 发电机有功功率","yc_hs_0516","cur_11"]
[694,"c_阳曲一期Ⅳ-050 发电机 绕组温度1","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-050 发电机 绕组温度1","yc_hs_0516","cur_23"]
[695,"c_阳曲一期Ⅳ-050 发电机 绕组温度2","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-050 发电机 绕组温度2","yc_hs_0516","cur_24"]
[696,"c_阳曲一期Ⅳ-050 发电机 绕组温度3","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-050 发电机 绕组温度3","yc_hs_0516","cur_25"]
[697,"c_阳曲一期Ⅳ-050 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-050 机舱侧向振动(已滤波)","yc_hs_0516","cur_30"]
[698,"c_阳曲一期Ⅳ-050 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",50,"YNJS.T1_L4.WTG050.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-050 机舱轴向振动(已滤波)","yc_hs_0516","cur_31"]
[699,"c_阳曲一期Ⅱ-014 发电机 绕组温度1","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅱ-014 发电机 绕组温度1","yc_hs_0516","cur_41"]
[700,"c_阳曲一期Ⅱ-014 发电机 绕组温度2","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅱ-014 发电机 绕组温度2","yc_hs_0516","cur_42"]
[701,"c_阳曲一期Ⅱ-014 发电机 绕组温度3","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅱ-014 发电机 绕组温度3","yc_hs_0516","cur_43"]
[702,"c_阳曲一期Ⅱ-014 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅱ-014 机舱侧向振动(已滤波)","yc_hs_0516","cur_66"]
[703,"c_阳曲一期Ⅱ-014 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅱ-014 机舱轴向振动(已滤波)","yc_hs_0516","cur_67"]
[704,"c_阳曲一期Ⅱ-014 舱内温度","阳曲风电场","WOF35100072",14,"YNJS.T1_L2.WTG014.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅱ-014 舱内温度","yc_hs_0516","cur_74"]
[705,"c_阳曲一期Ⅲ-028 风速","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅲ-028 风速","yc_hs_0516","cur_81"]
[706,"c_阳曲一期Ⅲ-028 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅲ-028 机舱中轴线与风向夹角","yc_hs_0516","cur_82"]
[707,"c_阳曲一期Ⅲ-028 风向","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅲ-028 风向","yc_hs_0516","cur_83"]
[708,"c_阳曲一期Ⅲ-028 舱外温度","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅲ-028 舱外温度","yc_hs_0516","cur_84"]
[709,"c_阳曲一期Ⅲ-028 扭揽角度","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅲ-028 扭揽角度","yc_hs_0516","cur_85"]
[710,"c_阳曲一期Ⅲ-028 1#桨叶片角度","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅲ-028 1#桨叶片角度","yc_hs_0516","cur_86"]
[711,"c_阳曲一期Ⅲ-028 2#桨叶片角度","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅲ-028 2#桨叶片角度","yc_hs_0516","cur_87"]
[712,"c_阳曲一期Ⅲ-028 3#桨叶片角度","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅲ-028 3#桨叶片角度","yc_hs_0516","cur_88"]
[713,"c_阳曲一期Ⅲ-028 发电机转速","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅲ-028 发电机转速","yc_hs_0516","cur_89"]
[714,"c_阳曲一期Ⅲ-028 发电机有功功率","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅲ-028 发电机有功功率","yc_hs_0516","cur_90"]
[720,"c_阳曲一期Ⅰ-011 风速","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅰ-011 风速","yc_hs_0518","cur_44"]
[721,"c_阳曲一期Ⅰ-011 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅰ-011 机舱中轴线与风向夹角","yc_hs_0518","cur_45"]
[722,"c_阳曲一期Ⅰ-011 风向","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅰ-011 风向","yc_hs_0518","cur_46"]
[723,"c_阳曲一期Ⅰ-011 舱外温度","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅰ-011 舱外温度","yc_hs_0518","cur_47"]
[724,"c_阳曲一期Ⅰ-011 扭揽角度","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅰ-011 扭揽角度","yc_hs_0518","cur_48"]
[725,"c_阳曲一期Ⅰ-011 1#桨叶片角度","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅰ-011 1#桨叶片角度","yc_hs_0518","cur_49"]
[726,"c_阳曲一期Ⅰ-011 2#桨叶片角度","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅰ-011 2#桨叶片角度","yc_hs_0518","cur_50"]
[727,"c_阳曲一期Ⅰ-011 3#桨叶片角度","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅰ-011 3#桨叶片角度","yc_hs_0518","cur_51"]
[728,"c_阳曲一期Ⅰ-011 发电机转速","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅰ-011 发电机转速","yc_hs_0518","cur_52"]
[729,"c_阳曲一期Ⅰ-011 发电机有功功率","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅰ-011 发电机有功功率","yc_hs_0518","cur_53"]
[730,"c_阳曲一期Ⅰ-011 发电机 绕组温度1","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅰ-011 发电机 绕组温度1","yc_hs_0518","cur_65"]
[731,"c_阳曲一期Ⅰ-011 发电机 绕组温度2","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅰ-011 发电机 绕组温度2","yc_hs_0518","cur_66"]
[732,"c_阳曲一期Ⅰ-011 发电机 绕组温度3","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅰ-011 发电机 绕组温度3","yc_hs_0518","cur_67"]
[733,"c_阳曲一期Ⅰ-011 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅰ-011 机舱侧向振动(已滤波)","yc_hs_0518","cur_72"]
[734,"c_阳曲一期Ⅰ-011 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅰ-011 机舱轴向振动(已滤波)","yc_hs_0518","cur_73"]
[735,"c_阳曲一期Ⅰ-011 舱内温度","阳曲风电场","WOF35100072",11,"YNJS.T1_L1.WTG011.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅰ-011 舱内温度","yc_hs_0518","cur_80"]
[736,"c_阳曲一期Ⅲ-028 发电机 绕组温度1","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅲ-028 发电机 绕组温度1","yc_hs_0518","cur_89"]
[737,"c_阳曲一期Ⅲ-028 发电机 绕组温度2","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅲ-028 发电机 绕组温度2","yc_hs_0518","cur_90"]
[738,"c_阳曲一期Ⅲ-028 发电机 绕组温度3","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅲ-028 发电机 绕组温度3","yc_hs_0519","cur_10"]
[739,"c_阳曲一期Ⅲ-028 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅲ-028 机舱侧向振动(已滤波)","yc_hs_0519","cur_15"]
[740,"c_阳曲一期Ⅲ-028 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅲ-028 机舱轴向振动(已滤波)","yc_hs_0519","cur_16"]
[741,"c_阳曲一期Ⅲ-028 舱内温度","阳曲风电场","WOF35100072",28,"YNJS.T1_L3.WTG028.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅲ-028 舱内温度","yc_hs_0519","cur_23"]
[750,"c_阳曲一期Ⅱ-025 风速","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅱ-025 风速","yc_hs_0512","cur_34"]
[751,"c_阳曲一期Ⅱ-025 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅱ-025 机舱中轴线与风向夹角","yc_hs_0512","cur_35"]
[752,"c_阳曲一期Ⅱ-025 风向","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅱ-025 风向","yc_hs_0512","cur_36"]
[753,"c_阳曲一期Ⅱ-025 舱外温度","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅱ-025 舱外温度","yc_hs_0512","cur_37"]
[754,"c_阳曲一期Ⅱ-025 扭揽角度","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅱ-025 扭揽角度","yc_hs_0512","cur_38"]
[755,"c_阳曲一期Ⅱ-025 1#桨叶片角度","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅱ-025 1#桨叶片角度","yc_hs_0512","cur_39"]
[756,"c_阳曲一期Ⅱ-025 2#桨叶片角度","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅱ-025 2#桨叶片角度","yc_hs_0512","cur_40"]
[757,"c_阳曲一期Ⅱ-025 3#桨叶片角度","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅱ-025 3#桨叶片角度","yc_hs_0512","cur_41"]
[758,"c_阳曲一期Ⅱ-025 发电机转速","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅱ-025 发电机转速","yc_hs_0512","cur_42"]
[759,"c_阳曲一期Ⅱ-025 发电机有功功率","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅱ-025 发电机有功功率","yc_hs_0512","cur_43"]
[760,"c_阳曲一期Ⅱ-025 发电机 绕组温度1","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅱ-025 发电机 绕组温度1","yc_hs_0512","cur_55"]
[761,"c_阳曲一期Ⅱ-025 发电机 绕组温度2","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅱ-025 发电机 绕组温度2","yc_hs_0512","cur_56"]
[762,"c_阳曲一期Ⅱ-025 发电机 绕组温度3","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅱ-025 发电机 绕组温度3","yc_hs_0512","cur_57"]
[763,"c_阳曲一期Ⅱ-025 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅱ-025 机舱侧向振动(已滤波)","yc_hs_0512","cur_62"]
[764,"c_阳曲一期Ⅱ-025 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅱ-025 机舱轴向振动(已滤波)","yc_hs_0512","cur_63"]
[765,"c_阳曲一期Ⅱ-025 舱内温度","阳曲风电场","WOF35100072",25,"YNJS.T1_L2.WTG025.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅱ-025 舱内温度","yc_hs_0512","cur_70"]
[768,"c_阳曲一期Ⅳ-039 舱内温度","阳曲风电场","WOF35100072",39,"YNJS.T1_L4.WTG039.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-039 舱内温度","yc_hs_0517","cur_02"]
[769,"c_阳曲一期Ⅳ-040 风速","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-040 风速","yc_hs_0517","cur_09"]
[770,"c_阳曲一期Ⅳ-040 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-040 机舱中轴线与风向夹角","yc_hs_0517","cur_10"]
[771,"c_阳曲一期Ⅳ-040 风向","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-040 风向","yc_hs_0517","cur_11"]
[772,"c_阳曲一期Ⅳ-040 舱外温度","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-040 舱外温度","yc_hs_0517","cur_80"]
[773,"c_阳曲一期Ⅳ-040 扭揽角度","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-040 扭揽角度","yc_hs_0517","cur_81"]
[774,"c_阳曲一期Ⅳ-040 1#桨叶片角度","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-040 1#桨叶片角度","yc_hs_0517","cur_82"]
[775,"c_阳曲一期Ⅳ-040 2#桨叶片角度","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-040 2#桨叶片角度","yc_hs_0517","cur_83"]
[776,"c_阳曲一期Ⅳ-040 3#桨叶片角度","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-040 3#桨叶片角度","yc_hs_0517","cur_84"]
[777,"c_阳曲一期Ⅳ-040 发电机转速","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-040 发电机转速","yc_hs_0517","cur_85"]
[778,"c_阳曲一期Ⅳ-040 发电机有功功率","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-040 发电机有功功率","yc_hs_0517","cur_86"]
[779,"c_阳曲一期Ⅳ-040 发电机 绕组温度1","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-040 发电机 绕组温度1","yc_hs_0517","cur_98"]
[780,"c_阳曲一期Ⅳ-040 发电机 绕组温度2","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-040 发电机 绕组温度2","yc_hs_0517","cur_99"]
[781,"c_阳曲一期Ⅳ-040 发电机 绕组温度3","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-040 发电机 绕组温度3","yc_hs_0517","cur_100"]
[782,"c_阳曲一期Ⅳ-040 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-040 机舱侧向振动(已滤波)","yc_hs_0518","cur_05"]
[783,"c_阳曲一期Ⅳ-040 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-040 机舱轴向振动(已滤波)","yc_hs_0518","cur_06"]
[796,"c_阳曲一期Ⅰ-012 风速","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅰ-012 风速","yc_hs_0512","cur_76"]
[797,"c_阳曲一期Ⅰ-012 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅰ-012 机舱中轴线与风向夹角","yc_hs_0512","cur_77"]
[798,"c_阳曲一期Ⅰ-012 风向","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅰ-012 风向","yc_hs_0512","cur_78"]
[799,"c_阳曲一期Ⅰ-012 舱外温度","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅰ-012 舱外温度","yc_hs_0512","cur_79"]
[800,"c_阳曲一期Ⅰ-012 扭揽角度","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅰ-012 扭揽角度","yc_hs_0512","cur_80"]
[801,"c_阳曲一期Ⅰ-012 1#桨叶片角度","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅰ-012 1#桨叶片角度","yc_hs_0512","cur_81"]
[802,"c_阳曲一期Ⅰ-012 2#桨叶片角度","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅰ-012 2#桨叶片角度","yc_hs_0512","cur_91"]
[803,"c_阳曲一期Ⅰ-012 3#桨叶片角度","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅰ-012 3#桨叶片角度","yc_hs_0512","cur_92"]
[804,"c_阳曲一期Ⅰ-012 发电机转速","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅰ-012 发电机转速","yc_hs_0512","cur_93"]
[805,"c_阳曲一期Ⅰ-012 发电机有功功率","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅰ-012 发电机有功功率","yc_hs_0512","cur_94"]
[806,"c_阳曲一期Ⅰ-012 发电机 绕组温度1","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅰ-012 发电机 绕组温度1","yc_hs_0513","cur_06"]
[807,"c_阳曲一期Ⅰ-012 发电机 绕组温度2","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅰ-012 发电机 绕组温度2","yc_hs_0513","cur_07"]
[808,"c_阳曲一期Ⅰ-012 发电机 绕组温度3","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅰ-012 发电机 绕组温度3","yc_hs_0513","cur_08"]
[809,"c_阳曲一期Ⅰ-012 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅰ-012 机舱侧向振动(已滤波)","yc_hs_0513","cur_13"]
[810,"c_阳曲一期Ⅰ-012 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅰ-012 机舱轴向振动(已滤波)","yc_hs_0513","cur_14"]
[821,"c_阳曲一期Ⅰ-012 舱内温度","阳曲风电场","WOF35100072",12,"YNJS.T1_L1.WTG012.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅰ-012 舱内温度","yc_hs_0514","cur_41"]
[822,"c_阳曲一期Ⅱ-026 风速","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅱ-026 风速","yc_hs_0514","cur_48"]
[823,"c_阳曲一期Ⅱ-026 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅱ-026 机舱中轴线与风向夹角","yc_hs_0514","cur_49"]
[824,"c_阳曲一期Ⅱ-026 风向","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅱ-026 风向","yc_hs_0514","cur_50"]
[825,"c_阳曲一期Ⅱ-026 舱外温度","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅱ-026 舱外温度","yc_hs_0514","cur_51"]
[826,"c_阳曲一期Ⅱ-026 扭揽角度","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅱ-026 扭揽角度","yc_hs_0514","cur_52"]
[827,"c_阳曲一期Ⅱ-026 1#桨叶片角度","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅱ-026 1#桨叶片角度","yc_hs_0514","cur_92"]
[828,"c_阳曲一期Ⅱ-026 2#桨叶片角度","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅱ-026 2#桨叶片角度","yc_hs_0514","cur_93"]
[829,"c_阳曲一期Ⅱ-026 3#桨叶片角度","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅱ-026 3#桨叶片角度","yc_hs_0514","cur_94"]
[830,"c_阳曲一期Ⅱ-026 发电机转速","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅱ-026 发电机转速","yc_hs_0514","cur_95"]
[831,"c_阳曲一期Ⅱ-026 发电机有功功率","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅱ-026 发电机有功功率","yc_hs_0514","cur_96"]
[832,"c_阳曲一期Ⅱ-026 发电机 绕组温度1","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅱ-026 发电机 绕组温度1","yc_hs_0515","cur_08"]
[833,"c_阳曲一期Ⅱ-026 发电机 绕组温度2","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅱ-026 发电机 绕组温度2","yc_hs_0515","cur_09"]
[834,"c_阳曲一期Ⅱ-026 发电机 绕组温度3","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅱ-026 发电机 绕组温度3","yc_hs_0515","cur_10"]
[835,"c_阳曲一期Ⅱ-026 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅱ-026 机舱侧向振动(已滤波)","yc_hs_0515","cur_15"]
[836,"c_阳曲一期Ⅱ-026 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅱ-026 机舱轴向振动(已滤波)","yc_hs_0515","cur_16"]
[838,"c_阳曲一期Ⅱ-026 舱内温度","阳曲风电场","WOF35100072",26,"YNJS.T1_L2.WTG026.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅱ-026 舱内温度","yc_hs_0516","cur_48"]
[839,"c_阳曲一期Ⅳ-040 舱内温度","阳曲风电场","WOF35100072",40,"YNJS.T1_L4.WTG040.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-040 舱内温度","yc_hs_0516","cur_55"]
[840,"c_阳曲一期Ⅳ-041 风速","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-041 风速","yc_hs_0517","cur_15"]
[841,"c_阳曲一期Ⅳ-041 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-041 机舱中轴线与风向夹角","yc_hs_0517","cur_16"]
[842,"c_阳曲一期Ⅳ-041 风向","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-041 风向","yc_hs_0517","cur_17"]
[843,"c_阳曲一期Ⅳ-041 舱外温度","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-041 舱外温度","yc_hs_0517","cur_18"]
[844,"c_阳曲一期Ⅳ-041 扭揽角度","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-041 扭揽角度","yc_hs_0517","cur_19"]
[845,"c_阳曲一期Ⅳ-041 1#桨叶片角度","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-041 1#桨叶片角度","yc_hs_0517","cur_20"]
[846,"c_阳曲一期Ⅳ-041 2#桨叶片角度","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-041 2#桨叶片角度","yc_hs_0517","cur_21"]
[847,"c_阳曲一期Ⅳ-041 3#桨叶片角度","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-041 3#桨叶片角度","yc_hs_0517","cur_22"]
[848,"c_阳曲一期Ⅳ-041 发电机转速","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-041 发电机转速","yc_hs_0517","cur_23"]
[849,"c_阳曲一期Ⅳ-041 发电机有功功率","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-041 发电机有功功率","yc_hs_0517","cur_24"]
[850,"c_阳曲一期Ⅳ-041 发电机 绕组温度1","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-041 发电机 绕组温度1","yc_hs_0517","cur_36"]
[851,"c_阳曲一期Ⅳ-041 发电机 绕组温度2","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-041 发电机 绕组温度2","yc_hs_0517","cur_37"]
[852,"c_阳曲一期Ⅳ-041 发电机 绕组温度3","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","c_阳曲一期Ⅳ-041 发电机 绕组温度3","yc_hs_0517","cur_38"]
[863,"c_阳曲一期Ⅳ-041 机舱侧向振动(已滤波)","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","c_阳曲一期Ⅳ-041 机舱侧向振动(已滤波)","yc_hs_0518","cur_95"]
[864,"c_阳曲一期Ⅳ-041 机舱轴向振动(已滤波)","阳曲风电场","WOF35100072",41,"YNJS.T1_L4.WTG041.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","c_阳曲一期Ⅳ-041 机舱轴向振动(已滤波)","yc_hs_0518","cur_96"]
[865,"c_阳曲一期Ⅳ-047 舱内温度","阳曲风电场","WOF35100072",47,"YNJS.T1_L4.WTG047.WNAC.TemNacelle","机舱内温度","cabin_temperature","c_阳曲一期Ⅳ-047 舱内温度","yc_hs_0519","cur_02"]
[866,"c_阳曲一期Ⅳ-048 风速","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WNAC.WindSpeed","风速","wind_velocity","c_阳曲一期Ⅳ-048 风速","yc_hs_0511","cur_31"]
[867,"c_阳曲一期Ⅳ-048 机舱中轴线与风向夹角","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WNAC.WindVaneDirection","对风角度","yaw_error1","c_阳曲一期Ⅳ-048 机舱中轴线与风向夹角","yc_hs_0511","cur_32"]
[868,"c_阳曲一期Ⅳ-048 风向","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WNAC.WindDirection","绝对风向","true_wind_direction","c_阳曲一期Ⅳ-048 风向","yc_hs_0511","cur_33"]
[869,"c_阳曲一期Ⅳ-048 舱外温度","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WNAC.TemOut","环境温度","outside_cabin_temperature","c_阳曲一期Ⅳ-048 舱外温度","yc_hs_0511","cur_34"]
[870,"c_阳曲一期Ⅳ-048 扭揽角度","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","c_阳曲一期Ⅳ-048 扭揽角度","yc_hs_0511","cur_35"]
[871,"c_阳曲一期Ⅳ-048 1#桨叶片角度","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","c_阳曲一期Ⅳ-048 1#桨叶片角度","yc_hs_0511","cur_36"]
[872,"c_阳曲一期Ⅳ-048 2#桨叶片角度","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","c_阳曲一期Ⅳ-048 2#桨叶片角度","yc_hs_0511","cur_37"]
[873,"c_阳曲一期Ⅳ-048 3#桨叶片角度","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","c_阳曲一期Ⅳ-048 3#桨叶片角度","yc_hs_0511","cur_38"]
[874,"c_阳曲一期Ⅳ-048 发电机转速","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WGEN.GenSpd","发电机转速","generator_speed","c_阳曲一期Ⅳ-048 发电机转速","yc_hs_0511","cur_39"]
[875,"c_阳曲一期Ⅳ-048 发电机有功功率","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WGEN.GenActivePW","有功功率","active_power","c_阳曲一期Ⅳ-048 发电机有功功率","yc_hs_0511","cur_40"]
[876,"c_阳曲一期Ⅳ-048 发电机 绕组温度1","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","c_阳曲一期Ⅳ-048 发电机 绕组温度1","yc_hs_0511","cur_52"]
[877,"c_阳曲一期Ⅳ-048 发电机 绕组温度2","阳曲风电场","WOF35100072",48,"YNJS.T1_L4.WTG048.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","c_阳曲一期Ⅳ-048 发电机 绕组温度2","yc_hs_0511","cur_53"]
[950,"g_西潘一期I-001 风速","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期I-001 风速","yc_hs_0017","cur_02"]
[951,"g_西潘一期I-001 机舱与风向夹角","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期I-001 机舱与风向夹角","yc_hs_0017","cur_03"]
[952,"g_西潘一期I-001 风向","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期I-001 风向","yc_hs_0017","cur_04"]
[953,"g_西潘一期I-001 舱外温度","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期I-001 舱外温度","yc_hs_0017","cur_05"]
[954,"g_西潘一期I-001 偏航角度(扭缆角度）","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期I-001 偏航角度(扭缆角度）","yc_hs_0017","cur_06"]
[955,"g_西潘一期I-001 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期I-001 1#桨叶片角度(桨距角)","yc_hs_0017","cur_07"]
[956,"g_西潘一期I-001 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期I-001 2#桨叶片角度(桨距角)","yc_hs_0017","cur_08"]
[957,"g_西潘一期I-001 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期I-001 3#桨叶片角度(桨距角)","yc_hs_0017","cur_09"]
[958,"g_西潘一期I-001 发电机测速模块测量转速","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期I-001 发电机测速模块测量转速","yc_hs_0017","cur_10"]
[959,"g_西潘一期I-001 发电机有功功率","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WGEN.GenActivePW","有功功率","active_power","g_西潘一期I-001 发电机有功功率","yc_hs_0017","cur_12"]
[960,"g_西潘一期I-001 发电机绕组温度1","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期I-001 发电机绕组温度1","yc_hs_0017","cur_24"]
[961,"g_西潘一期I-001 发电机绕组温度2","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期I-001 发电机绕组温度2","yc_hs_0017","cur_25"]
[962,"g_西潘一期I-001 发电机绕组温度3","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期I-001 发电机绕组温度3","yc_hs_0017","cur_26"]
[963,"g_西潘一期I-001 舱内温度","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期I-001 舱内温度","yc_hs_0017","cur_39"]
[964,"g_西潘一期I-001 发电机转速","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期I-001 发电机转速","yc_hs_0017","cur_67"]
[965,"g_西潘一期I-001 发电机前轴承温度1","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期I-001 发电机前轴承温度1","yc_hs_0017","cur_80"]
[966,"g_西潘一期I-001 发电机后轴承温度1","西潘风电场","WOF35300077",1,"YQXP.T1_L1.WTG001.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期I-001 发电机后轴承温度1","yc_hs_0017","cur_82"]
[967,"g_西潘一期I-002 风速","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期I-002 风速","yc_hs_0019","cur_02"]
[968,"g_西潘一期I-002 机舱与风向夹角","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期I-002 机舱与风向夹角","yc_hs_0019","cur_03"]
[969,"g_西潘一期I-002 风向","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期I-002 风向","yc_hs_0019","cur_04"]
[970,"g_西潘一期I-002 舱外温度","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期I-002 舱外温度","yc_hs_0019","cur_05"]
[971,"g_西潘一期I-002 偏航角度(扭缆角度）","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期I-002 偏航角度(扭缆角度）","yc_hs_0019","cur_06"]
[972,"g_西潘一期I-002 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期I-002 1#桨叶片角度(桨距角)","yc_hs_0019","cur_07"]
[973,"g_西潘一期I-002 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期I-002 2#桨叶片角度(桨距角)","yc_hs_0019","cur_08"]
[974,"g_西潘一期I-002 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期I-002 3#桨叶片角度(桨距角)","yc_hs_0019","cur_09"]
[975,"g_西潘一期I-002 发电机测速模块测量转速","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期I-002 发电机测速模块测量转速","yc_hs_0019","cur_10"]
[976,"g_西潘一期I-002 发电机有功功率","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WGEN.GenActivePW","有功功率","active_power","g_西潘一期I-002 发电机有功功率","yc_hs_0019","cur_12"]
[977,"g_西潘一期I-002 发电机绕组温度1","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期I-002 发电机绕组温度1","yc_hs_0019","cur_24"]
[978,"g_西潘一期I-002 发电机绕组温度2","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期I-002 发电机绕组温度2","yc_hs_0019","cur_25"]
[979,"g_西潘一期I-002 发电机绕组温度3","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期I-002 发电机绕组温度3","yc_hs_0019","cur_26"]
[980,"g_西潘一期I-002 舱内温度","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期I-002 舱内温度","yc_hs_0019","cur_39"]
[981,"g_西潘一期I-002 发电机转速","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期I-002 发电机转速","yc_hs_0019","cur_67"]
[982,"g_西潘一期I-002 发电机前轴承温度1","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期I-002 发电机前轴承温度1","yc_hs_0019","cur_80"]
[983,"g_西潘一期I-002 发电机后轴承温度1","西潘风电场","WOF35300077",2,"YQXP.T1_L1.WTG002.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期I-002 发电机后轴承温度1","yc_hs_0019","cur_82"]
[984,"g_西潘一期I-003 风速","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期I-003 风速","yc_hs_0020","cur_02"]
[985,"g_西潘一期I-003 机舱与风向夹角","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期I-003 机舱与风向夹角","yc_hs_0020","cur_03"]
[986,"g_西潘一期I-003 风向","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期I-003 风向","yc_hs_0020","cur_04"]
[987,"g_西潘一期I-003 舱外温度","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期I-003 舱外温度","yc_hs_0020","cur_05"]
[988,"g_西潘一期I-003 偏航角度(扭缆角度）","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期I-003 偏航角度(扭缆角度）","yc_hs_0020","cur_06"]
[989,"g_西潘一期I-003 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期I-003 1#桨叶片角度(桨距角)","yc_hs_0020","cur_07"]
[990,"g_西潘一期I-003 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期I-003 2#桨叶片角度(桨距角)","yc_hs_0020","cur_08"]
[991,"g_西潘一期I-003 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期I-003 3#桨叶片角度(桨距角)","yc_hs_0020","cur_09"]
[992,"g_西潘一期I-003 发电机测速模块测量转速","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期I-003 发电机测速模块测量转速","yc_hs_0020","cur_10"]
[993,"g_西潘一期I-003 发电机有功功率","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WGEN.GenActivePW","有功功率","active_power","g_西潘一期I-003 发电机有功功率","yc_hs_0020","cur_12"]
[994,"g_西潘一期I-003 发电机绕组温度1","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期I-003 发电机绕组温度1","yc_hs_0020","cur_24"]
[995,"g_西潘一期I-003 发电机绕组温度2","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期I-003 发电机绕组温度2","yc_hs_0020","cur_25"]
[996,"g_西潘一期I-003 发电机绕组温度3","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期I-003 发电机绕组温度3","yc_hs_0020","cur_26"]
[997,"g_西潘一期I-003 舱内温度","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期I-003 舱内温度","yc_hs_0020","cur_39"]
[998,"g_西潘一期I-003 发电机转速","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期I-003 发电机转速","yc_hs_0020","cur_67"]
[999,"g_西潘一期I-003 发电机前轴承温度1","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期I-003 发电机前轴承温度1","yc_hs_0020","cur_80"]
[1000,"g_西潘一期I-003 发电机后轴承温度1","西潘风电场","WOF35300077",3,"YQXP.T1_L1.WTG003.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期I-003 发电机后轴承温度1","yc_hs_0020","cur_82"]
[1001,"g_西潘一期I-004 风速","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期I-004 风速","yc_hs_0021","cur_02"]
[1002,"g_西潘一期I-004 机舱与风向夹角","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期I-004 机舱与风向夹角","yc_hs_0021","cur_03"]
[1003,"g_西潘一期I-004 风向","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期I-004 风向","yc_hs_0021","cur_04"]
[1004,"g_西潘一期I-004 舱外温度","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期I-004 舱外温度","yc_hs_0021","cur_05"]
[1005,"g_西潘一期I-004 偏航角度(扭缆角度）","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期I-004 偏航角度(扭缆角度）","yc_hs_0021","cur_06"]
[1006,"g_西潘一期I-004 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期I-004 1#桨叶片角度(桨距角)","yc_hs_0021","cur_07"]
[1007,"g_西潘一期I-004 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期I-004 2#桨叶片角度(桨距角)","yc_hs_0021","cur_08"]
[1008,"g_西潘一期I-004 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期I-004 3#桨叶片角度(桨距角)","yc_hs_0021","cur_09"]
[1009,"g_西潘一期I-004 发电机测速模块测量转速","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期I-004 发电机测速模块测量转速","yc_hs_0021","cur_10"]
[1010,"g_西潘一期I-004 发电机有功功率","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WGEN.GenActivePW","有功功率","active_power","g_西潘一期I-004 发电机有功功率","yc_hs_0021","cur_12"]
[1011,"g_西潘一期I-004 发电机绕组温度1","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期I-004 发电机绕组温度1","yc_hs_0021","cur_24"]
[1012,"g_西潘一期I-004 发电机绕组温度2","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期I-004 发电机绕组温度2","yc_hs_0021","cur_25"]
[1013,"g_西潘一期I-004 发电机绕组温度3","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期I-004 发电机绕组温度3","yc_hs_0021","cur_26"]
[1014,"g_西潘一期I-004 舱内温度","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期I-004 舱内温度","yc_hs_0021","cur_39"]
[1015,"g_西潘一期I-004 发电机转速","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期I-004 发电机转速","yc_hs_0021","cur_67"]
[1016,"g_西潘一期I-004 发电机前轴承温度1","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期I-004 发电机前轴承温度1","yc_hs_0021","cur_80"]
[1017,"g_西潘一期I-004 发电机后轴承温度1","西潘风电场","WOF35300077",4,"YQXP.T1_L1.WTG004.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期I-004 发电机后轴承温度1","yc_hs_0021","cur_82"]
[1018,"g_西潘一期I-005 风速","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期I-005 风速","yc_hs_0022","cur_02"]
[1019,"g_西潘一期I-005 机舱与风向夹角","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期I-005 机舱与风向夹角","yc_hs_0022","cur_03"]
[1020,"g_西潘一期I-005 风向","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期I-005 风向","yc_hs_0022","cur_04"]
[1021,"g_西潘一期I-005 舱外温度","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期I-005 舱外温度","yc_hs_0022","cur_05"]
[1022,"g_西潘一期I-005 偏航角度(扭缆角度）","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期I-005 偏航角度(扭缆角度）","yc_hs_0022","cur_06"]
[1023,"g_西潘一期I-005 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期I-005 1#桨叶片角度(桨距角)","yc_hs_0022","cur_07"]
[1024,"g_西潘一期I-005 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期I-005 2#桨叶片角度(桨距角)","yc_hs_0022","cur_08"]
[1025,"g_西潘一期I-005 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期I-005 3#桨叶片角度(桨距角)","yc_hs_0022","cur_09"]
[1026,"g_西潘一期I-005 发电机测速模块测量转速","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期I-005 发电机测速模块测量转速","yc_hs_0022","cur_10"]
[1027,"g_西潘一期I-005 发电机有功功率","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WGEN.GenActivePW","有功功率","active_power","g_西潘一期I-005 发电机有功功率","yc_hs_0022","cur_12"]
[1028,"g_西潘一期I-005 发电机绕组温度1","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期I-005 发电机绕组温度1","yc_hs_0022","cur_24"]
[1029,"g_西潘一期I-005 发电机绕组温度2","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期I-005 发电机绕组温度2","yc_hs_0022","cur_25"]
[1030,"g_西潘一期I-005 发电机绕组温度3","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期I-005 发电机绕组温度3","yc_hs_0022","cur_26"]
[1031,"g_西潘一期I-005 舱内温度","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期I-005 舱内温度","yc_hs_0022","cur_39"]
[1032,"g_西潘一期I-005 发电机转速","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期I-005 发电机转速","yc_hs_0022","cur_67"]
[1033,"g_西潘一期I-005 发电机前轴承温度1","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期I-005 发电机前轴承温度1","yc_hs_0022","cur_80"]
[1034,"g_西潘一期I-005 发电机后轴承温度1","西潘风电场","WOF35300077",5,"YQXP.T1_L1.WTG005.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期I-005 发电机后轴承温度1","yc_hs_0022","cur_82"]
[1035,"g_西潘一期I-006 风速","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期I-006 风速","yc_hs_0023","cur_02"]
[1036,"g_西潘一期I-006 机舱与风向夹角","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期I-006 机舱与风向夹角","yc_hs_0023","cur_03"]
[1037,"g_西潘一期I-006 风向","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期I-006 风向","yc_hs_0023","cur_04"]
[1038,"g_西潘一期I-006 舱外温度","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期I-006 舱外温度","yc_hs_0023","cur_05"]
[1039,"g_西潘一期I-006 偏航角度(扭缆角度）","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期I-006 偏航角度(扭缆角度）","yc_hs_0023","cur_06"]
[1040,"g_西潘一期I-006 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期I-006 1#桨叶片角度(桨距角)","yc_hs_0023","cur_07"]
[1041,"g_西潘一期I-006 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期I-006 2#桨叶片角度(桨距角)","yc_hs_0023","cur_08"]
[1042,"g_西潘一期I-006 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期I-006 3#桨叶片角度(桨距角)","yc_hs_0023","cur_09"]
[1043,"g_西潘一期I-006 发电机测速模块测量转速","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期I-006 发电机测速模块测量转速","yc_hs_0023","cur_10"]
[1044,"g_西潘一期I-006 发电机有功功率","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WGEN.GenActivePW","有功功率","active_power","g_西潘一期I-006 发电机有功功率","yc_hs_0023","cur_12"]
[1045,"g_西潘一期I-006 发电机绕组温度1","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期I-006 发电机绕组温度1","yc_hs_0023","cur_24"]
[1046,"g_西潘一期I-006 发电机绕组温度2","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期I-006 发电机绕组温度2","yc_hs_0023","cur_25"]
[1047,"g_西潘一期I-006 发电机绕组温度3","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期I-006 发电机绕组温度3","yc_hs_0023","cur_26"]
[1048,"g_西潘一期I-006 舱内温度","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期I-006 舱内温度","yc_hs_0023","cur_39"]
[1049,"g_西潘一期I-006 发电机转速","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期I-006 发电机转速","yc_hs_0023","cur_67"]
[1050,"g_西潘一期I-006 发电机前轴承温度1","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期I-006 发电机前轴承温度1","yc_hs_0023","cur_80"]
[1051,"g_西潘一期I-006 发电机后轴承温度1","西潘风电场","WOF35300077",6,"YQXP.T1_L1.WTG006.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期I-006 发电机后轴承温度1","yc_hs_0023","cur_82"]
[1052,"g_西潘一期I-007 风速","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期I-007 风速","yc_hs_0024","cur_02"]
[1053,"g_西潘一期I-007 机舱与风向夹角","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期I-007 机舱与风向夹角","yc_hs_0024","cur_03"]
[1054,"g_西潘一期I-007 风向","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期I-007 风向","yc_hs_0024","cur_04"]
[1055,"g_西潘一期I-007 舱外温度","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期I-007 舱外温度","yc_hs_0024","cur_05"]
[1056,"g_西潘一期I-007 偏航角度(扭缆角度）","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期I-007 偏航角度(扭缆角度）","yc_hs_0024","cur_06"]
[1057,"g_西潘一期I-007 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期I-007 1#桨叶片角度(桨距角)","yc_hs_0024","cur_07"]
[1058,"g_西潘一期I-007 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期I-007 2#桨叶片角度(桨距角)","yc_hs_0024","cur_08"]
[1059,"g_西潘一期I-007 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期I-007 3#桨叶片角度(桨距角)","yc_hs_0024","cur_09"]
[1060,"g_西潘一期I-007 发电机测速模块测量转速","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期I-007 发电机测速模块测量转速","yc_hs_0024","cur_10"]
[1061,"g_西潘一期I-007 发电机有功功率","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WGEN.GenActivePW","有功功率","active_power","g_西潘一期I-007 发电机有功功率","yc_hs_0024","cur_12"]
[1062,"g_西潘一期I-007 发电机绕组温度1","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期I-007 发电机绕组温度1","yc_hs_0024","cur_24"]
[1063,"g_西潘一期I-007 发电机绕组温度2","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期I-007 发电机绕组温度2","yc_hs_0024","cur_25"]
[1064,"g_西潘一期I-007 发电机绕组温度3","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期I-007 发电机绕组温度3","yc_hs_0024","cur_26"]
[1065,"g_西潘一期I-007 舱内温度","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期I-007 舱内温度","yc_hs_0024","cur_39"]
[1066,"g_西潘一期I-007 发电机转速","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期I-007 发电机转速","yc_hs_0024","cur_67"]
[1067,"g_西潘一期I-007 发电机前轴承温度1","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期I-007 发电机前轴承温度1","yc_hs_0024","cur_80"]
[1068,"g_西潘一期I-007 发电机后轴承温度1","西潘风电场","WOF35300077",7,"YQXP.T1_L1.WTG007.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期I-007 发电机后轴承温度1","yc_hs_0024","cur_82"]
[1069,"g_西潘一期I-008 风速","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期I-008 风速","yc_hs_0025","cur_02"]
[1070,"g_西潘一期I-008 机舱与风向夹角","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期I-008 机舱与风向夹角","yc_hs_0025","cur_03"]
[1071,"g_西潘一期I-008 风向","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期I-008 风向","yc_hs_0025","cur_04"]
[1072,"g_西潘一期I-008 舱外温度","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期I-008 舱外温度","yc_hs_0025","cur_05"]
[1073,"g_西潘一期I-008 偏航角度(扭缆角度）","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期I-008 偏航角度(扭缆角度）","yc_hs_0025","cur_06"]
[1074,"g_西潘一期I-008 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期I-008 1#桨叶片角度(桨距角)","yc_hs_0025","cur_07"]
[1075,"g_西潘一期I-008 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期I-008 2#桨叶片角度(桨距角)","yc_hs_0025","cur_08"]
[1076,"g_西潘一期I-008 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期I-008 3#桨叶片角度(桨距角)","yc_hs_0025","cur_09"]
[1077,"g_西潘一期I-008 发电机测速模块测量转速","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期I-008 发电机测速模块测量转速","yc_hs_0025","cur_10"]
[1078,"g_西潘一期I-008 发电机有功功率","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WGEN.GenActivePW","有功功率","active_power","g_西潘一期I-008 发电机有功功率","yc_hs_0025","cur_12"]
[1079,"g_西潘一期I-008 发电机绕组温度1","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期I-008 发电机绕组温度1","yc_hs_0025","cur_24"]
[1080,"g_西潘一期I-008 发电机绕组温度2","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期I-008 发电机绕组温度2","yc_hs_0025","cur_25"]
[1081,"g_西潘一期I-008 发电机绕组温度3","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期I-008 发电机绕组温度3","yc_hs_0025","cur_26"]
[1082,"g_西潘一期I-008 舱内温度","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期I-008 舱内温度","yc_hs_0025","cur_39"]
[1083,"g_西潘一期I-008 发电机转速","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期I-008 发电机转速","yc_hs_0025","cur_67"]
[1084,"g_西潘一期I-008 发电机前轴承温度1","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期I-008 发电机前轴承温度1","yc_hs_0025","cur_80"]
[1085,"g_西潘一期I-008 发电机后轴承温度1","西潘风电场","WOF35300077",8,"YQXP.T1_L1.WTG008.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期I-008 发电机后轴承温度1","yc_hs_0025","cur_82"]
[1086,"g_西潘一期I-009 风速","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期I-009 风速","yc_hs_0026","cur_02"]
[1087,"g_西潘一期I-009 机舱与风向夹角","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期I-009 机舱与风向夹角","yc_hs_0026","cur_03"]
[1088,"g_西潘一期I-009 风向","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期I-009 风向","yc_hs_0026","cur_04"]
[1089,"g_西潘一期I-009 舱外温度","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期I-009 舱外温度","yc_hs_0026","cur_05"]
[1090,"g_西潘一期I-009 偏航角度(扭缆角度）","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期I-009 偏航角度(扭缆角度）","yc_hs_0026","cur_06"]
[1091,"g_西潘一期I-009 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期I-009 1#桨叶片角度(桨距角)","yc_hs_0026","cur_07"]
[1092,"g_西潘一期I-009 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期I-009 2#桨叶片角度(桨距角)","yc_hs_0026","cur_08"]
[1093,"g_西潘一期I-009 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期I-009 3#桨叶片角度(桨距角)","yc_hs_0026","cur_09"]
[1094,"g_西潘一期I-009 发电机测速模块测量转速","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期I-009 发电机测速模块测量转速","yc_hs_0026","cur_10"]
[1095,"g_西潘一期I-009 发电机有功功率","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WGEN.GenActivePW","有功功率","active_power","g_西潘一期I-009 发电机有功功率","yc_hs_0026","cur_12"]
[1096,"g_西潘一期I-009 发电机绕组温度1","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期I-009 发电机绕组温度1","yc_hs_0026","cur_24"]
[1097,"g_西潘一期I-009 发电机绕组温度2","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期I-009 发电机绕组温度2","yc_hs_0026","cur_25"]
[1098,"g_西潘一期I-009 发电机绕组温度3","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期I-009 发电机绕组温度3","yc_hs_0026","cur_26"]
[1099,"g_西潘一期I-009 舱内温度","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期I-009 舱内温度","yc_hs_0026","cur_39"]
[1100,"g_西潘一期I-009 发电机转速","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期I-009 发电机转速","yc_hs_0026","cur_67"]
[1101,"g_西潘一期I-009 发电机前轴承温度1","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期I-009 发电机前轴承温度1","yc_hs_0026","cur_80"]
[1102,"g_西潘一期I-009 发电机后轴承温度1","西潘风电场","WOF35300077",9,"YQXP.T1_L1.WTG009.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期I-009 发电机后轴承温度1","yc_hs_0026","cur_82"]
[1103,"g_西潘一期I-010 风速","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期I-010 风速","yc_hs_0027","cur_02"]
[1104,"g_西潘一期I-010 机舱与风向夹角","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期I-010 机舱与风向夹角","yc_hs_0027","cur_03"]
[1105,"g_西潘一期I-010 风向","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期I-010 风向","yc_hs_0027","cur_04"]
[1106,"g_西潘一期I-010 舱外温度","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期I-010 舱外温度","yc_hs_0027","cur_05"]
[1107,"g_西潘一期I-010 偏航角度(扭缆角度）","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期I-010 偏航角度(扭缆角度）","yc_hs_0027","cur_06"]
[1108,"g_西潘一期I-010 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期I-010 1#桨叶片角度(桨距角)","yc_hs_0027","cur_07"]
[1109,"g_西潘一期I-010 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期I-010 2#桨叶片角度(桨距角)","yc_hs_0027","cur_08"]
[1110,"g_西潘一期I-010 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期I-010 3#桨叶片角度(桨距角)","yc_hs_0027","cur_09"]
[1111,"g_西潘一期I-010 发电机测速模块测量转速","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期I-010 发电机测速模块测量转速","yc_hs_0027","cur_10"]
[1112,"g_西潘一期I-010 发电机有功功率","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WGEN.GenActivePW","有功功率","active_power","g_西潘一期I-010 发电机有功功率","yc_hs_0027","cur_12"]
[1113,"g_西潘一期I-010 发电机绕组温度1","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期I-010 发电机绕组温度1","yc_hs_0027","cur_24"]
[1114,"g_西潘一期I-010 发电机绕组温度2","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期I-010 发电机绕组温度2","yc_hs_0027","cur_25"]
[1115,"g_西潘一期I-010 发电机绕组温度3","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期I-010 发电机绕组温度3","yc_hs_0027","cur_26"]
[1116,"g_西潘一期I-010 舱内温度","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期I-010 舱内温度","yc_hs_0027","cur_39"]
[1117,"g_西潘一期I-010 发电机转速","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期I-010 发电机转速","yc_hs_0027","cur_67"]
[1118,"g_西潘一期I-010 发电机前轴承温度1","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期I-010 发电机前轴承温度1","yc_hs_0027","cur_80"]
[1119,"g_西潘一期I-010 发电机后轴承温度1","西潘风电场","WOF35300077",10,"YQXP.T1_L1.WTG010.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期I-010 发电机后轴承温度1","yc_hs_0027","cur_82"]
[1120,"g_西潘一期I-011 风速","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期I-011 风速","yc_hs_0028","cur_02"]
[1121,"g_西潘一期I-011 机舱与风向夹角","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期I-011 机舱与风向夹角","yc_hs_0028","cur_03"]
[1122,"g_西潘一期I-011 风向","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期I-011 风向","yc_hs_0028","cur_04"]
[1123,"g_西潘一期I-011 舱外温度","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期I-011 舱外温度","yc_hs_0028","cur_05"]
[1124,"g_西潘一期I-011 偏航角度(扭缆角度）","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期I-011 偏航角度(扭缆角度）","yc_hs_0028","cur_06"]
[1125,"g_西潘一期I-011 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期I-011 1#桨叶片角度(桨距角)","yc_hs_0028","cur_07"]
[1126,"g_西潘一期I-011 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期I-011 2#桨叶片角度(桨距角)","yc_hs_0028","cur_08"]
[1127,"g_西潘一期I-011 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期I-011 3#桨叶片角度(桨距角)","yc_hs_0028","cur_09"]
[1128,"g_西潘一期I-011 发电机测速模块测量转速","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期I-011 发电机测速模块测量转速","yc_hs_0028","cur_10"]
[1129,"g_西潘一期I-011 发电机有功功率","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WGEN.GenActivePW","有功功率","active_power","g_西潘一期I-011 发电机有功功率","yc_hs_0028","cur_12"]
[1130,"g_西潘一期I-011 发电机绕组温度1","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期I-011 发电机绕组温度1","yc_hs_0028","cur_24"]
[1131,"g_西潘一期I-011 发电机绕组温度2","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期I-011 发电机绕组温度2","yc_hs_0028","cur_25"]
[1132,"g_西潘一期I-011 发电机绕组温度3","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期I-011 发电机绕组温度3","yc_hs_0028","cur_26"]
[1133,"g_西潘一期I-011 舱内温度","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期I-011 舱内温度","yc_hs_0028","cur_39"]
[1134,"g_西潘一期I-011 发电机转速","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期I-011 发电机转速","yc_hs_0028","cur_67"]
[1135,"g_西潘一期I-011 发电机前轴承温度1","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期I-011 发电机前轴承温度1","yc_hs_0028","cur_80"]
[1136,"g_西潘一期I-011 发电机后轴承温度1","西潘风电场","WOF35300077",11,"YQXP.T1_L1.WTG011.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期I-011 发电机后轴承温度1","yc_hs_0028","cur_82"]
[1137,"g_西潘一期I-012 风速","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期I-012 风速","yc_hs_0029","cur_02"]
[1138,"g_西潘一期I-012 机舱与风向夹角","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期I-012 机舱与风向夹角","yc_hs_0029","cur_03"]
[1139,"g_西潘一期I-012 风向","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期I-012 风向","yc_hs_0029","cur_04"]
[1140,"g_西潘一期I-012 舱外温度","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期I-012 舱外温度","yc_hs_0029","cur_05"]
[1141,"g_西潘一期I-012 偏航角度(扭缆角度）","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期I-012 偏航角度(扭缆角度）","yc_hs_0029","cur_06"]
[1142,"g_西潘一期I-012 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期I-012 1#桨叶片角度(桨距角)","yc_hs_0029","cur_07"]
[1143,"g_西潘一期I-012 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期I-012 2#桨叶片角度(桨距角)","yc_hs_0029","cur_08"]
[1144,"g_西潘一期I-012 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期I-012 3#桨叶片角度(桨距角)","yc_hs_0029","cur_09"]
[1145,"g_西潘一期I-012 发电机测速模块测量转速","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期I-012 发电机测速模块测量转速","yc_hs_0029","cur_10"]
[1146,"g_西潘一期I-012 发电机有功功率","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WGEN.GenActivePW","有功功率","active_power","g_西潘一期I-012 发电机有功功率","yc_hs_0029","cur_12"]
[1147,"g_西潘一期I-012 发电机绕组温度1","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期I-012 发电机绕组温度1","yc_hs_0029","cur_24"]
[1148,"g_西潘一期I-012 发电机绕组温度2","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期I-012 发电机绕组温度2","yc_hs_0029","cur_25"]
[1149,"g_西潘一期I-012 发电机绕组温度3","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期I-012 发电机绕组温度3","yc_hs_0029","cur_26"]
[1150,"g_西潘一期I-012 舱内温度","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期I-012 舱内温度","yc_hs_0029","cur_39"]
[1151,"g_西潘一期I-012 发电机转速","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期I-012 发电机转速","yc_hs_0029","cur_67"]
[1152,"g_西潘一期I-012 发电机前轴承温度1","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期I-012 发电机前轴承温度1","yc_hs_0029","cur_80"]
[1153,"g_西潘一期I-012 发电机后轴承温度1","西潘风电场","WOF35300077",12,"YQXP.T1_L1.WTG012.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期I-012 发电机后轴承温度1","yc_hs_0029","cur_82"]
[1154,"g_西潘一期I-013 风速","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期I-013 风速","yc_hs_0030","cur_02"]
[1155,"g_西潘一期I-013 机舱与风向夹角","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期I-013 机舱与风向夹角","yc_hs_0030","cur_03"]
[1156,"g_西潘一期I-013 风向","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期I-013 风向","yc_hs_0030","cur_04"]
[1157,"g_西潘一期I-013 舱外温度","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期I-013 舱外温度","yc_hs_0030","cur_05"]
[1158,"g_西潘一期I-013 偏航角度(扭缆角度）","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期I-013 偏航角度(扭缆角度）","yc_hs_0030","cur_06"]
[1159,"g_西潘一期I-013 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期I-013 1#桨叶片角度(桨距角)","yc_hs_0030","cur_07"]
[1160,"g_西潘一期I-013 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期I-013 2#桨叶片角度(桨距角)","yc_hs_0030","cur_08"]
[1161,"g_西潘一期I-013 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期I-013 3#桨叶片角度(桨距角)","yc_hs_0030","cur_09"]
[1162,"g_西潘一期I-013 发电机测速模块测量转速","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期I-013 发电机测速模块测量转速","yc_hs_0030","cur_10"]
[1163,"g_西潘一期I-013 发电机有功功率","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WGEN.GenActivePW","有功功率","active_power","g_西潘一期I-013 发电机有功功率","yc_hs_0030","cur_12"]
[1164,"g_西潘一期I-013 发电机绕组温度1","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期I-013 发电机绕组温度1","yc_hs_0030","cur_24"]
[1165,"g_西潘一期I-013 发电机绕组温度2","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期I-013 发电机绕组温度2","yc_hs_0030","cur_25"]
[1166,"g_西潘一期I-013 发电机绕组温度3","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期I-013 发电机绕组温度3","yc_hs_0030","cur_26"]
[1167,"g_西潘一期I-013 舱内温度","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期I-013 舱内温度","yc_hs_0030","cur_39"]
[1168,"g_西潘一期I-013 发电机转速","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期I-013 发电机转速","yc_hs_0030","cur_67"]
[1169,"g_西潘一期I-013 发电机前轴承温度1","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期I-013 发电机前轴承温度1","yc_hs_0030","cur_80"]
[1170,"g_西潘一期I-013 发电机后轴承温度1","西潘风电场","WOF35300077",13,"YQXP.T1_L2.WTG013.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期I-013 发电机后轴承温度1","yc_hs_0030","cur_82"]
[1171,"g_西潘一期Ⅱ-014 风速","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期Ⅱ-014 风速","yc_hs_0031","cur_02"]
[1172,"g_西潘一期Ⅱ-014 机舱与风向夹角","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期Ⅱ-014 机舱与风向夹角","yc_hs_0031","cur_03"]
[1173,"g_西潘一期Ⅱ-014 风向","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期Ⅱ-014 风向","yc_hs_0031","cur_04"]
[1174,"g_西潘一期Ⅱ-014 舱外温度","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期Ⅱ-014 舱外温度","yc_hs_0031","cur_05"]
[1175,"g_西潘一期Ⅱ-014 偏航角度(扭缆角度）","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期Ⅱ-014 偏航角度(扭缆角度）","yc_hs_0031","cur_06"]
[1176,"g_西潘一期Ⅱ-014 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期Ⅱ-014 1#桨叶片角度(桨距角)","yc_hs_0031","cur_07"]
[1177,"g_西潘一期Ⅱ-014 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期Ⅱ-014 2#桨叶片角度(桨距角)","yc_hs_0031","cur_08"]
[1178,"g_西潘一期Ⅱ-014 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期Ⅱ-014 3#桨叶片角度(桨距角)","yc_hs_0031","cur_09"]
[1179,"g_西潘一期Ⅱ-014 发电机测速模块测量转速","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期Ⅱ-014 发电机测速模块测量转速","yc_hs_0031","cur_10"]
[1180,"g_西潘一期Ⅱ-014 发电机有功功率","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WGEN.GenActivePW","有功功率","active_power","g_西潘一期Ⅱ-014 发电机有功功率","yc_hs_0031","cur_12"]
[1181,"g_西潘一期Ⅱ-014 发电机绕组温度1","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期Ⅱ-014 发电机绕组温度1","yc_hs_0031","cur_24"]
[1182,"g_西潘一期Ⅱ-014 发电机绕组温度2","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期Ⅱ-014 发电机绕组温度2","yc_hs_0031","cur_25"]
[1183,"g_西潘一期Ⅱ-014 发电机绕组温度3","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期Ⅱ-014 发电机绕组温度3","yc_hs_0031","cur_26"]
[1184,"g_西潘一期Ⅱ-014 舱内温度","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期Ⅱ-014 舱内温度","yc_hs_0031","cur_39"]
[1185,"g_西潘一期Ⅱ-014 发电机转速","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期Ⅱ-014 发电机转速","yc_hs_0031","cur_67"]
[1186,"g_西潘一期Ⅱ-014 发电机前轴承温度1","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期Ⅱ-014 发电机前轴承温度1","yc_hs_0031","cur_80"]
[1187,"g_西潘一期Ⅱ-014 发电机后轴承温度1","西潘风电场","WOF35300077",14,"YQXP.T1_L2.WTG014.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期Ⅱ-014 发电机后轴承温度1","yc_hs_0031","cur_82"]
[1188,"g_西潘一期Ⅱ-015 风速","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期Ⅱ-015 风速","yc_hs_0032","cur_02"]
[1189,"g_西潘一期Ⅱ-015 机舱与风向夹角","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期Ⅱ-015 机舱与风向夹角","yc_hs_0032","cur_03"]
[1190,"g_西潘一期Ⅱ-015 风向","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期Ⅱ-015 风向","yc_hs_0032","cur_04"]
[1191,"g_西潘一期Ⅱ-015 舱外温度","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期Ⅱ-015 舱外温度","yc_hs_0032","cur_05"]
[1192,"g_西潘一期Ⅱ-015 偏航角度(扭缆角度）","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期Ⅱ-015 偏航角度(扭缆角度）","yc_hs_0032","cur_06"]
[1193,"g_西潘一期Ⅱ-015 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期Ⅱ-015 1#桨叶片角度(桨距角)","yc_hs_0032","cur_07"]
[1194,"g_西潘一期Ⅱ-015 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期Ⅱ-015 2#桨叶片角度(桨距角)","yc_hs_0032","cur_08"]
[1195,"g_西潘一期Ⅱ-015 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期Ⅱ-015 3#桨叶片角度(桨距角)","yc_hs_0032","cur_09"]
[1196,"g_西潘一期Ⅱ-015 发电机测速模块测量转速","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期Ⅱ-015 发电机测速模块测量转速","yc_hs_0032","cur_10"]
[1197,"g_西潘一期Ⅱ-015 发电机有功功率","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WGEN.GenActivePW","有功功率","active_power","g_西潘一期Ⅱ-015 发电机有功功率","yc_hs_0032","cur_12"]
[1198,"g_西潘一期Ⅱ-015 发电机绕组温度1","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期Ⅱ-015 发电机绕组温度1","yc_hs_0032","cur_24"]
[1199,"g_西潘一期Ⅱ-015 发电机绕组温度2","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期Ⅱ-015 发电机绕组温度2","yc_hs_0032","cur_25"]
[1200,"g_西潘一期Ⅱ-015 发电机绕组温度3","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期Ⅱ-015 发电机绕组温度3","yc_hs_0032","cur_26"]
[1201,"g_西潘一期Ⅱ-015 舱内温度","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期Ⅱ-015 舱内温度","yc_hs_0032","cur_39"]
[1202,"g_西潘一期Ⅱ-015 发电机转速","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期Ⅱ-015 发电机转速","yc_hs_0032","cur_67"]
[1203,"g_西潘一期Ⅱ-015 发电机前轴承温度1","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期Ⅱ-015 发电机前轴承温度1","yc_hs_0032","cur_80"]
[1204,"g_西潘一期Ⅱ-015 发电机后轴承温度1","西潘风电场","WOF35300077",15,"YQXP.T1_L2.WTG015.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期Ⅱ-015 发电机后轴承温度1","yc_hs_0032","cur_82"]
[1205,"g_西潘一期Ⅱ-016 风速","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期Ⅱ-016 风速","yc_hs_0033","cur_02"]
[1206,"g_西潘一期Ⅱ-016 机舱与风向夹角","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期Ⅱ-016 机舱与风向夹角","yc_hs_0033","cur_03"]
[1207,"g_西潘一期Ⅱ-016 风向","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期Ⅱ-016 风向","yc_hs_0033","cur_04"]
[1208,"g_西潘一期Ⅱ-016 舱外温度","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期Ⅱ-016 舱外温度","yc_hs_0033","cur_05"]
[1209,"g_西潘一期Ⅱ-016 偏航角度(扭缆角度）","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期Ⅱ-016 偏航角度(扭缆角度）","yc_hs_0033","cur_06"]
[1210,"g_西潘一期Ⅱ-016 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期Ⅱ-016 1#桨叶片角度(桨距角)","yc_hs_0033","cur_07"]
[1211,"g_西潘一期Ⅱ-016 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期Ⅱ-016 2#桨叶片角度(桨距角)","yc_hs_0033","cur_08"]
[1212,"g_西潘一期Ⅱ-016 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期Ⅱ-016 3#桨叶片角度(桨距角)","yc_hs_0033","cur_09"]
[1213,"g_西潘一期Ⅱ-016 发电机测速模块测量转速","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期Ⅱ-016 发电机测速模块测量转速","yc_hs_0033","cur_10"]
[1214,"g_西潘一期Ⅱ-016 发电机有功功率","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WGEN.GenActivePW","有功功率","active_power","g_西潘一期Ⅱ-016 发电机有功功率","yc_hs_0033","cur_12"]
[1215,"g_西潘一期Ⅱ-016 发电机绕组温度1","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期Ⅱ-016 发电机绕组温度1","yc_hs_0033","cur_24"]
[1216,"g_西潘一期Ⅱ-016 发电机绕组温度2","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期Ⅱ-016 发电机绕组温度2","yc_hs_0033","cur_25"]
[1217,"g_西潘一期Ⅱ-016 发电机绕组温度3","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期Ⅱ-016 发电机绕组温度3","yc_hs_0033","cur_26"]
[1218,"g_西潘一期Ⅱ-016 舱内温度","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期Ⅱ-016 舱内温度","yc_hs_0033","cur_39"]
[1219,"g_西潘一期Ⅱ-016 发电机转速","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期Ⅱ-016 发电机转速","yc_hs_0033","cur_67"]
[1220,"g_西潘一期Ⅱ-016 发电机前轴承温度1","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期Ⅱ-016 发电机前轴承温度1","yc_hs_0033","cur_80"]
[1221,"g_西潘一期Ⅱ-016 发电机后轴承温度1","西潘风电场","WOF35300077",16,"YQXP.T1_L2.WTG016.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期Ⅱ-016 发电机后轴承温度1","yc_hs_0033","cur_82"]
[1222,"g_西潘一期Ⅱ-017 风速","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期Ⅱ-017 风速","yc_hs_0036","cur_02"]
[1223,"g_西潘一期Ⅱ-017 机舱与风向夹角","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期Ⅱ-017 机舱与风向夹角","yc_hs_0036","cur_03"]
[1224,"g_西潘一期Ⅱ-017 风向","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期Ⅱ-017 风向","yc_hs_0036","cur_04"]
[1225,"g_西潘一期Ⅱ-017 舱外温度","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期Ⅱ-017 舱外温度","yc_hs_0036","cur_05"]
[1226,"g_西潘一期Ⅱ-017 偏航角度(扭缆角度）","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期Ⅱ-017 偏航角度(扭缆角度）","yc_hs_0036","cur_06"]
[1227,"g_西潘一期Ⅱ-017 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期Ⅱ-017 1#桨叶片角度(桨距角)","yc_hs_0036","cur_07"]
[1228,"g_西潘一期Ⅱ-017 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期Ⅱ-017 2#桨叶片角度(桨距角)","yc_hs_0036","cur_08"]
[1229,"g_西潘一期Ⅱ-017 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期Ⅱ-017 3#桨叶片角度(桨距角)","yc_hs_0036","cur_09"]
[1230,"g_西潘一期Ⅱ-017 发电机测速模块测量转速","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期Ⅱ-017 发电机测速模块测量转速","yc_hs_0036","cur_10"]
[1231,"g_西潘一期Ⅱ-017 发电机有功功率","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WGEN.GenActivePW","有功功率","active_power","g_西潘一期Ⅱ-017 发电机有功功率","yc_hs_0036","cur_12"]
[1232,"g_西潘一期Ⅱ-017 发电机绕组温度1","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期Ⅱ-017 发电机绕组温度1","yc_hs_0036","cur_24"]
[1233,"g_西潘一期Ⅱ-017 发电机绕组温度2","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期Ⅱ-017 发电机绕组温度2","yc_hs_0036","cur_25"]
[1234,"g_西潘一期Ⅱ-017 发电机绕组温度3","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期Ⅱ-017 发电机绕组温度3","yc_hs_0036","cur_26"]
[1235,"g_西潘一期Ⅱ-017 舱内温度","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期Ⅱ-017 舱内温度","yc_hs_0036","cur_39"]
[1236,"g_西潘一期Ⅱ-017 发电机转速","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期Ⅱ-017 发电机转速","yc_hs_0036","cur_67"]
[1237,"g_西潘一期Ⅱ-017 发电机前轴承温度1","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期Ⅱ-017 发电机前轴承温度1","yc_hs_0036","cur_80"]
[1238,"g_西潘一期Ⅱ-017 发电机后轴承温度1","西潘风电场","WOF35300077",17,"YQXP.T1_L2.WTG017.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期Ⅱ-017 发电机后轴承温度1","yc_hs_0036","cur_82"]
[1239,"g_西潘一期Ⅱ-018 风速","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期Ⅱ-018 风速","yc_hs_0039","cur_02"]
[1240,"g_西潘一期Ⅱ-018 机舱与风向夹角","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期Ⅱ-018 机舱与风向夹角","yc_hs_0039","cur_03"]
[1241,"g_西潘一期Ⅱ-018 风向","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期Ⅱ-018 风向","yc_hs_0039","cur_04"]
[1242,"g_西潘一期Ⅱ-018 舱外温度","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期Ⅱ-018 舱外温度","yc_hs_0039","cur_05"]
[1243,"g_西潘一期Ⅱ-018 偏航角度(扭缆角度）","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期Ⅱ-018 偏航角度(扭缆角度）","yc_hs_0039","cur_06"]
[1244,"g_西潘一期Ⅱ-018 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期Ⅱ-018 1#桨叶片角度(桨距角)","yc_hs_0039","cur_07"]
[1245,"g_西潘一期Ⅱ-018 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期Ⅱ-018 2#桨叶片角度(桨距角)","yc_hs_0039","cur_08"]
[1246,"g_西潘一期Ⅱ-018 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期Ⅱ-018 3#桨叶片角度(桨距角)","yc_hs_0039","cur_09"]
[1247,"g_西潘一期Ⅱ-018 发电机测速模块测量转速","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期Ⅱ-018 发电机测速模块测量转速","yc_hs_0039","cur_10"]
[1248,"g_西潘一期Ⅱ-018 发电机有功功率","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WGEN.GenActivePW","有功功率","active_power","g_西潘一期Ⅱ-018 发电机有功功率","yc_hs_0039","cur_12"]
[1249,"g_西潘一期Ⅱ-018 发电机绕组温度1","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期Ⅱ-018 发电机绕组温度1","yc_hs_0039","cur_24"]
[1250,"g_西潘一期Ⅱ-018 发电机绕组温度2","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期Ⅱ-018 发电机绕组温度2","yc_hs_0039","cur_25"]
[1251,"g_西潘一期Ⅱ-018 发电机绕组温度3","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期Ⅱ-018 发电机绕组温度3","yc_hs_0039","cur_26"]
[1252,"g_西潘一期Ⅱ-018 舱内温度","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期Ⅱ-018 舱内温度","yc_hs_0039","cur_39"]
[1253,"g_西潘一期Ⅱ-018 发电机转速","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期Ⅱ-018 发电机转速","yc_hs_0039","cur_67"]
[1254,"g_西潘一期Ⅱ-018 发电机前轴承温度1","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期Ⅱ-018 发电机前轴承温度1","yc_hs_0039","cur_80"]
[1255,"g_西潘一期Ⅱ-018 发电机后轴承温度1","西潘风电场","WOF35300077",18,"YQXP.T1_L2.WTG018.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期Ⅱ-018 发电机后轴承温度1","yc_hs_0039","cur_82"]
[1256,"g_西潘一期Ⅱ-019 风速","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期Ⅱ-019 风速","yc_hs_0040","cur_02"]
[1257,"g_西潘一期Ⅱ-019 机舱与风向夹角","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期Ⅱ-019 机舱与风向夹角","yc_hs_0040","cur_03"]
[1258,"g_西潘一期Ⅱ-019 风向","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期Ⅱ-019 风向","yc_hs_0040","cur_04"]
[1259,"g_西潘一期Ⅱ-019 舱外温度","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期Ⅱ-019 舱外温度","yc_hs_0040","cur_05"]
[1260,"g_西潘一期Ⅱ-019 偏航角度(扭缆角度）","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期Ⅱ-019 偏航角度(扭缆角度）","yc_hs_0040","cur_06"]
[1261,"g_西潘一期Ⅱ-019 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期Ⅱ-019 1#桨叶片角度(桨距角)","yc_hs_0040","cur_07"]
[1262,"g_西潘一期Ⅱ-019 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期Ⅱ-019 2#桨叶片角度(桨距角)","yc_hs_0040","cur_08"]
[1263,"g_西潘一期Ⅱ-019 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期Ⅱ-019 3#桨叶片角度(桨距角)","yc_hs_0040","cur_09"]
[1264,"g_西潘一期Ⅱ-019 发电机测速模块测量转速","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期Ⅱ-019 发电机测速模块测量转速","yc_hs_0040","cur_10"]
[1265,"g_西潘一期Ⅱ-019 发电机有功功率","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WGEN.GenActivePW","有功功率","active_power","g_西潘一期Ⅱ-019 发电机有功功率","yc_hs_0040","cur_12"]
[1266,"g_西潘一期Ⅱ-019 发电机绕组温度1","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期Ⅱ-019 发电机绕组温度1","yc_hs_0040","cur_24"]
[1267,"g_西潘一期Ⅱ-019 发电机绕组温度2","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期Ⅱ-019 发电机绕组温度2","yc_hs_0040","cur_25"]
[1268,"g_西潘一期Ⅱ-019 发电机绕组温度3","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期Ⅱ-019 发电机绕组温度3","yc_hs_0040","cur_26"]
[1269,"g_西潘一期Ⅱ-019 舱内温度","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期Ⅱ-019 舱内温度","yc_hs_0040","cur_39"]
[1270,"g_西潘一期Ⅱ-019 发电机转速","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期Ⅱ-019 发电机转速","yc_hs_0040","cur_67"]
[1271,"g_西潘一期Ⅱ-019 发电机前轴承温度1","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期Ⅱ-019 发电机前轴承温度1","yc_hs_0040","cur_80"]
[1272,"g_西潘一期Ⅱ-019 发电机后轴承温度1","西潘风电场","WOF35300077",19,"YQXP.T1_L2.WTG019.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期Ⅱ-019 发电机后轴承温度1","yc_hs_0040","cur_82"]
[1273,"g_西潘一期Ⅱ-020 风速","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期Ⅱ-020 风速","yc_hs_0126","cur_02"]
[1274,"g_西潘一期Ⅱ-020 机舱与风向夹角","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期Ⅱ-020 机舱与风向夹角","yc_hs_0126","cur_03"]
[1275,"g_西潘一期Ⅱ-020 风向","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期Ⅱ-020 风向","yc_hs_0126","cur_04"]
[1276,"g_西潘一期Ⅱ-020 舱外温度","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期Ⅱ-020 舱外温度","yc_hs_0126","cur_05"]
[1277,"g_西潘一期Ⅱ-020 偏航角度(扭缆角度）","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期Ⅱ-020 偏航角度(扭缆角度）","yc_hs_0126","cur_06"]
[1278,"g_西潘一期Ⅱ-020 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期Ⅱ-020 1#桨叶片角度(桨距角)","yc_hs_0126","cur_07"]
[1279,"g_西潘一期Ⅱ-020 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期Ⅱ-020 2#桨叶片角度(桨距角)","yc_hs_0126","cur_08"]
[1280,"g_西潘一期Ⅱ-020 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期Ⅱ-020 3#桨叶片角度(桨距角)","yc_hs_0126","cur_09"]
[1281,"g_西潘一期Ⅱ-020 发电机测速模块测量转速","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期Ⅱ-020 发电机测速模块测量转速","yc_hs_0126","cur_10"]
[1282,"g_西潘一期Ⅱ-020 发电机有功功率","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WGEN.GenActivePW","有功功率","active_power","g_西潘一期Ⅱ-020 发电机有功功率","yc_hs_0126","cur_12"]
[1283,"g_西潘一期Ⅱ-020 发电机绕组温度1","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期Ⅱ-020 发电机绕组温度1","yc_hs_0126","cur_24"]
[1284,"g_西潘一期Ⅱ-020 发电机绕组温度2","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期Ⅱ-020 发电机绕组温度2","yc_hs_0126","cur_25"]
[1285,"g_西潘一期Ⅱ-020 发电机绕组温度3","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期Ⅱ-020 发电机绕组温度3","yc_hs_0126","cur_26"]
[1286,"g_西潘一期Ⅱ-020 舱内温度","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期Ⅱ-020 舱内温度","yc_hs_0126","cur_39"]
[1287,"g_西潘一期Ⅱ-020 发电机转速","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期Ⅱ-020 发电机转速","yc_hs_0126","cur_67"]
[1288,"g_西潘一期Ⅱ-020 发电机前轴承温度1","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期Ⅱ-020 发电机前轴承温度1","yc_hs_0126","cur_80"]
[1289,"g_西潘一期Ⅱ-020 发电机后轴承温度1","西潘风电场","WOF35300077",20,"YQXP.T1_L2.WTG020.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期Ⅱ-020 发电机后轴承温度1","yc_hs_0126","cur_82"]
[1290,"g_西潘一期Ⅱ-021 风速","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期Ⅱ-021 风速","yc_hs_0127","cur_02"]
[1291,"g_西潘一期Ⅱ-021 机舱与风向夹角","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期Ⅱ-021 机舱与风向夹角","yc_hs_0127","cur_03"]
[1292,"g_西潘一期Ⅱ-021 风向","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期Ⅱ-021 风向","yc_hs_0127","cur_04"]
[1293,"g_西潘一期Ⅱ-021 舱外温度","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期Ⅱ-021 舱外温度","yc_hs_0127","cur_05"]
[1294,"g_西潘一期Ⅱ-021 偏航角度(扭缆角度）","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期Ⅱ-021 偏航角度(扭缆角度）","yc_hs_0127","cur_06"]
[1295,"g_西潘一期Ⅱ-021 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期Ⅱ-021 1#桨叶片角度(桨距角)","yc_hs_0127","cur_07"]
[1296,"g_西潘一期Ⅱ-021 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期Ⅱ-021 2#桨叶片角度(桨距角)","yc_hs_0127","cur_08"]
[1297,"g_西潘一期Ⅱ-021 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期Ⅱ-021 3#桨叶片角度(桨距角)","yc_hs_0127","cur_09"]
[1298,"g_西潘一期Ⅱ-021 发电机测速模块测量转速","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期Ⅱ-021 发电机测速模块测量转速","yc_hs_0127","cur_10"]
[1299,"g_西潘一期Ⅱ-021 发电机有功功率","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WGEN.GenActivePW","有功功率","active_power","g_西潘一期Ⅱ-021 发电机有功功率","yc_hs_0127","cur_12"]
[1300,"g_西潘一期Ⅱ-021 发电机绕组温度1","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期Ⅱ-021 发电机绕组温度1","yc_hs_0127","cur_24"]
[1301,"g_西潘一期Ⅱ-021 发电机绕组温度2","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期Ⅱ-021 发电机绕组温度2","yc_hs_0127","cur_25"]
[1302,"g_西潘一期Ⅱ-021 发电机绕组温度3","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期Ⅱ-021 发电机绕组温度3","yc_hs_0127","cur_26"]
[1303,"g_西潘一期Ⅱ-021 舱内温度","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期Ⅱ-021 舱内温度","yc_hs_0127","cur_39"]
[1304,"g_西潘一期Ⅱ-021 发电机转速","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期Ⅱ-021 发电机转速","yc_hs_0127","cur_67"]
[1305,"g_西潘一期Ⅱ-021 发电机前轴承温度1","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期Ⅱ-021 发电机前轴承温度1","yc_hs_0127","cur_80"]
[1306,"g_西潘一期Ⅱ-021 发电机后轴承温度1","西潘风电场","WOF35300077",21,"YQXP.T1_L2.WTG021.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期Ⅱ-021 发电机后轴承温度1","yc_hs_0127","cur_82"]
[1307,"g_西潘一期Ⅱ-022 风速","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期Ⅱ-022 风速","yc_hs_0128","cur_02"]
[1308,"g_西潘一期Ⅱ-022 机舱与风向夹角","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期Ⅱ-022 机舱与风向夹角","yc_hs_0128","cur_03"]
[1309,"g_西潘一期Ⅱ-022 风向","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期Ⅱ-022 风向","yc_hs_0128","cur_04"]
[1310,"g_西潘一期Ⅱ-022 舱外温度","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期Ⅱ-022 舱外温度","yc_hs_0128","cur_05"]
[1311,"g_西潘一期Ⅱ-022 偏航角度(扭缆角度）","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期Ⅱ-022 偏航角度(扭缆角度）","yc_hs_0128","cur_06"]
[1312,"g_西潘一期Ⅱ-022 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期Ⅱ-022 1#桨叶片角度(桨距角)","yc_hs_0128","cur_07"]
[1313,"g_西潘一期Ⅱ-022 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期Ⅱ-022 2#桨叶片角度(桨距角)","yc_hs_0128","cur_08"]
[1314,"g_西潘一期Ⅱ-022 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期Ⅱ-022 3#桨叶片角度(桨距角)","yc_hs_0128","cur_09"]
[1315,"g_西潘一期Ⅱ-022 发电机测速模块测量转速","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期Ⅱ-022 发电机测速模块测量转速","yc_hs_0128","cur_10"]
[1316,"g_西潘一期Ⅱ-022 发电机有功功率","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WGEN.GenActivePW","有功功率","active_power","g_西潘一期Ⅱ-022 发电机有功功率","yc_hs_0128","cur_12"]
[1317,"g_西潘一期Ⅱ-022 发电机绕组温度1","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期Ⅱ-022 发电机绕组温度1","yc_hs_0128","cur_24"]
[1318,"g_西潘一期Ⅱ-022 发电机绕组温度2","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期Ⅱ-022 发电机绕组温度2","yc_hs_0128","cur_25"]
[1319,"g_西潘一期Ⅱ-022 发电机绕组温度3","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期Ⅱ-022 发电机绕组温度3","yc_hs_0128","cur_26"]
[1320,"g_西潘一期Ⅱ-022 舱内温度","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期Ⅱ-022 舱内温度","yc_hs_0128","cur_39"]
[1321,"g_西潘一期Ⅱ-022 发电机转速","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期Ⅱ-022 发电机转速","yc_hs_0128","cur_67"]
[1322,"g_西潘一期Ⅱ-022 发电机前轴承温度1","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期Ⅱ-022 发电机前轴承温度1","yc_hs_0128","cur_80"]
[1323,"g_西潘一期Ⅱ-022 发电机后轴承温度1","西潘风电场","WOF35300077",22,"YQXP.T1_L2.WTG022.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期Ⅱ-022 发电机后轴承温度1","yc_hs_0128","cur_82"]
[1324,"g_西潘一期Ⅱ-023 风速","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期Ⅱ-023 风速","yc_hs_0129","cur_02"]
[1325,"g_西潘一期Ⅱ-023 机舱与风向夹角","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期Ⅱ-023 机舱与风向夹角","yc_hs_0129","cur_03"]
[1326,"g_西潘一期Ⅱ-023 风向","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期Ⅱ-023 风向","yc_hs_0129","cur_04"]
[1327,"g_西潘一期Ⅱ-023 舱外温度","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期Ⅱ-023 舱外温度","yc_hs_0129","cur_05"]
[1328,"g_西潘一期Ⅱ-023 偏航角度(扭缆角度）","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期Ⅱ-023 偏航角度(扭缆角度）","yc_hs_0129","cur_06"]
[1329,"g_西潘一期Ⅱ-023 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期Ⅱ-023 1#桨叶片角度(桨距角)","yc_hs_0129","cur_07"]
[1330,"g_西潘一期Ⅱ-023 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期Ⅱ-023 2#桨叶片角度(桨距角)","yc_hs_0129","cur_08"]
[1331,"g_西潘一期Ⅱ-023 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期Ⅱ-023 3#桨叶片角度(桨距角)","yc_hs_0129","cur_09"]
[1332,"g_西潘一期Ⅱ-023 发电机测速模块测量转速","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期Ⅱ-023 发电机测速模块测量转速","yc_hs_0129","cur_10"]
[1333,"g_西潘一期Ⅱ-023 发电机有功功率","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WGEN.GenActivePW","有功功率","active_power","g_西潘一期Ⅱ-023 发电机有功功率","yc_hs_0129","cur_12"]
[1334,"g_西潘一期Ⅱ-023 发电机绕组温度1","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期Ⅱ-023 发电机绕组温度1","yc_hs_0129","cur_24"]
[1335,"g_西潘一期Ⅱ-023 发电机绕组温度2","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期Ⅱ-023 发电机绕组温度2","yc_hs_0129","cur_25"]
[1336,"g_西潘一期Ⅱ-023 发电机绕组温度3","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期Ⅱ-023 发电机绕组温度3","yc_hs_0129","cur_26"]
[1337,"g_西潘一期Ⅱ-023 舱内温度","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期Ⅱ-023 舱内温度","yc_hs_0129","cur_39"]
[1338,"g_西潘一期Ⅱ-023 发电机转速","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期Ⅱ-023 发电机转速","yc_hs_0129","cur_67"]
[1339,"g_西潘一期Ⅱ-023 发电机前轴承温度1","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期Ⅱ-023 发电机前轴承温度1","yc_hs_0129","cur_80"]
[1340,"g_西潘一期Ⅱ-023 发电机后轴承温度1","西潘风电场","WOF35300077",23,"YQXP.T1_L2.WTG023.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期Ⅱ-023 发电机后轴承温度1","yc_hs_0129","cur_82"]
[1341,"g_西潘一期Ⅱ-024 风速","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期Ⅱ-024 风速","yc_hs_0130","cur_02"]
[1342,"g_西潘一期Ⅱ-024 机舱与风向夹角","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期Ⅱ-024 机舱与风向夹角","yc_hs_0130","cur_03"]
[1343,"g_西潘一期Ⅱ-024 风向","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期Ⅱ-024 风向","yc_hs_0130","cur_04"]
[1344,"g_西潘一期Ⅱ-024 舱外温度","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期Ⅱ-024 舱外温度","yc_hs_0130","cur_05"]
[1345,"g_西潘一期Ⅱ-024 偏航角度(扭缆角度）","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期Ⅱ-024 偏航角度(扭缆角度）","yc_hs_0130","cur_06"]
[1346,"g_西潘一期Ⅱ-024 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期Ⅱ-024 1#桨叶片角度(桨距角)","yc_hs_0130","cur_07"]
[1347,"g_西潘一期Ⅱ-024 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期Ⅱ-024 2#桨叶片角度(桨距角)","yc_hs_0130","cur_08"]
[1348,"g_西潘一期Ⅱ-024 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期Ⅱ-024 3#桨叶片角度(桨距角)","yc_hs_0130","cur_09"]
[1349,"g_西潘一期Ⅱ-024 发电机测速模块测量转速","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期Ⅱ-024 发电机测速模块测量转速","yc_hs_0130","cur_10"]
[1350,"g_西潘一期Ⅱ-024 发电机有功功率","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WGEN.GenActivePW","有功功率","active_power","g_西潘一期Ⅱ-024 发电机有功功率","yc_hs_0130","cur_12"]
[1351,"g_西潘一期Ⅱ-024 发电机绕组温度1","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期Ⅱ-024 发电机绕组温度1","yc_hs_0130","cur_24"]
[1352,"g_西潘一期Ⅱ-024 发电机绕组温度2","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期Ⅱ-024 发电机绕组温度2","yc_hs_0130","cur_25"]
[1353,"g_西潘一期Ⅱ-024 发电机绕组温度3","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期Ⅱ-024 发电机绕组温度3","yc_hs_0130","cur_26"]
[1354,"g_西潘一期Ⅱ-024 舱内温度","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期Ⅱ-024 舱内温度","yc_hs_0130","cur_39"]
[1355,"g_西潘一期Ⅱ-024 发电机转速","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期Ⅱ-024 发电机转速","yc_hs_0130","cur_67"]
[1356,"g_西潘一期Ⅱ-024 发电机前轴承温度1","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期Ⅱ-024 发电机前轴承温度1","yc_hs_0130","cur_80"]
[1357,"g_西潘一期Ⅱ-024 发电机后轴承温度1","西潘风电场","WOF35300077",24,"YQXP.T1_L2.WTG024.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期Ⅱ-024 发电机后轴承温度1","yc_hs_0130","cur_82"]
[1358,"g_西潘一期Ⅱ-025 风速","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WNAC.WindSpeed","风速","wind_velocity","g_西潘一期Ⅱ-025 风速","yc_hs_0131","cur_02"]
[1359,"g_西潘一期Ⅱ-025 机舱与风向夹角","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WNAC.WindVaneDirection","对风角度","yaw_error1","g_西潘一期Ⅱ-025 机舱与风向夹角","yc_hs_0131","cur_03"]
[1360,"g_西潘一期Ⅱ-025 风向","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WNAC.WindDirection","绝对风向","true_wind_direction","g_西潘一期Ⅱ-025 风向","yc_hs_0131","cur_04"]
[1361,"g_西潘一期Ⅱ-025 舱外温度","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘一期Ⅱ-025 舱外温度","yc_hs_0131","cur_05"]
[1362,"g_西潘一期Ⅱ-025 偏航角度(扭缆角度）","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","g_西潘一期Ⅱ-025 偏航角度(扭缆角度）","yc_hs_0131","cur_06"]
[1363,"g_西潘一期Ⅱ-025 1#桨叶片角度(桨距角)","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","g_西潘一期Ⅱ-025 1#桨叶片角度(桨距角)","yc_hs_0131","cur_07"]
[1364,"g_西潘一期Ⅱ-025 2#桨叶片角度(桨距角)","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","g_西潘一期Ⅱ-025 2#桨叶片角度(桨距角)","yc_hs_0131","cur_08"]
[1365,"g_西潘一期Ⅱ-025 3#桨叶片角度(桨距角)","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","g_西潘一期Ⅱ-025 3#桨叶片角度(桨距角)","yc_hs_0131","cur_09"]
[1366,"g_西潘一期Ⅱ-025 发电机测速模块测量转速","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WGEN.Spd.Ra","风轮转速","rotor_speed","g_西潘一期Ⅱ-025 发电机测速模块测量转速","yc_hs_0131","cur_10"]
[1367,"g_西潘一期Ⅱ-025 发电机有功功率","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WGEN.GenActivePW","有功功率","active_power","g_西潘一期Ⅱ-025 发电机有功功率","yc_hs_0131","cur_12"]
[1368,"g_西潘一期Ⅱ-025 发电机绕组温度1","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","g_西潘一期Ⅱ-025 发电机绕组温度1","yc_hs_0131","cur_24"]
[1369,"g_西潘一期Ⅱ-025 发电机绕组温度2","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","g_西潘一期Ⅱ-025 发电机绕组温度2","yc_hs_0131","cur_25"]
[1370,"g_西潘一期Ⅱ-025 发电机绕组温度3","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","g_西潘一期Ⅱ-025 发电机绕组温度3","yc_hs_0131","cur_26"]
[1371,"g_西潘一期Ⅱ-025 舱内温度","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WNAC.TemNacelle","机舱内温度","cabin_temperature","g_西潘一期Ⅱ-025 舱内温度","yc_hs_0131","cur_39"]
[1372,"g_西潘一期Ⅱ-025 发电机转速","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WGEN.GenSpd","发电机转速","generator_speed","g_西潘一期Ⅱ-025 发电机转速","yc_hs_0131","cur_67"]
[1373,"g_西潘一期Ⅱ-025 发电机前轴承温度1","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘一期Ⅱ-025 发电机前轴承温度1","yc_hs_0131","cur_80"]
[1374,"g_西潘一期Ⅱ-025 发电机后轴承温度1","西潘风电场","WOF35300077",25,"YQXP.T1_L2.WTG025.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘一期Ⅱ-025 发电机后轴承温度1","yc_hs_0131","cur_82"]
[1375,"a_马家梁一期Ⅰ-001 风速","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅰ-001 风速","yc_hs_0133","cur_02"]
[1376,"a_马家梁一期Ⅰ-001 机舱与风向夹角","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅰ-001 机舱与风向夹角","yc_hs_0133","cur_03"]
[1377,"a_马家梁一期Ⅰ-001 风向","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅰ-001 风向","yc_hs_0133","cur_04"]
[1378,"a_马家梁一期Ⅰ-001 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅰ-001 偏航角度(扭缆角度）","yc_hs_0133","cur_06"]
[1379,"a_马家梁一期Ⅰ-001 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅰ-001 1#桨叶片角度(桨距角)","yc_hs_0133","cur_07"]
[1380,"a_马家梁一期Ⅰ-001 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅰ-001 2#桨叶片角度(桨距角)","yc_hs_0133","cur_08"]
[1381,"a_马家梁一期Ⅰ-001 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅰ-001 3#桨叶片角度(桨距角)","yc_hs_0133","cur_09"]
[1382,"a_马家梁一期Ⅰ-001 发电机测速模块测量转速","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅰ-001 发电机测速模块测量转速","yc_hs_0133","cur_10"]
[1383,"a_马家梁一期Ⅰ-001 发电机有功功率","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅰ-001 发电机有功功率","yc_hs_0133","cur_11"]
[1384,"a_马家梁一期Ⅰ-001 发电机绕组温度1","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅰ-001 发电机绕组温度1","yc_hs_0133","cur_23"]
[1385,"a_马家梁一期Ⅰ-001 发电机绕组温度2","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅰ-001 发电机绕组温度2","yc_hs_0133","cur_24"]
[1386,"a_马家梁一期Ⅰ-001 发电机绕组温度3","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅰ-001 发电机绕组温度3","yc_hs_0133","cur_25"]
[1387,"a_马家梁一期Ⅰ-001 机舱柜温度","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅰ-001 机舱柜温度","yc_hs_0133","cur_36"]
[1388,"a_马家梁一期Ⅰ-001 环境温度","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅰ-001 环境温度","yc_hs_0133","cur_69"]
[1389,"a_马家梁一期Ⅰ-001 发电机前轴承温度1","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅰ-001 发电机前轴承温度1","yc_hs_0133","cur_70"]
[1390,"a_马家梁一期Ⅰ-001 发电机后轴承温度1","马家梁风电场","WOF35200074",1,"MJLFD.T1_L1.WTG001.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅰ-001 发电机后轴承温度1","yc_hs_0133","cur_72"]
[1391,"a_马家梁一期Ⅰ-002 风速","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅰ-002 风速","yc_hs_0133","cur_92"]
[1392,"a_马家梁一期Ⅰ-002 机舱与风向夹角","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅰ-002 机舱与风向夹角","yc_hs_0133","cur_93"]
[1393,"a_马家梁一期Ⅰ-002 风向","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅰ-002 风向","yc_hs_0133","cur_94"]
[1394,"a_马家梁一期Ⅰ-002 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅰ-002 偏航角度(扭缆角度）","yc_hs_0133","cur_96"]
[1395,"a_马家梁一期Ⅰ-002 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅰ-002 1#桨叶片角度(桨距角)","yc_hs_0133","cur_97"]
[1396,"a_马家梁一期Ⅰ-002 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅰ-002 2#桨叶片角度(桨距角)","yc_hs_0133","cur_98"]
[1397,"a_马家梁一期Ⅰ-002 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅰ-002 3#桨叶片角度(桨距角)","yc_hs_0133","cur_99"]
[1398,"a_马家梁一期Ⅰ-002 发电机测速模块测量转速","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅰ-002 发电机测速模块测量转速","yc_hs_0133","cur_100"]
[1399,"a_马家梁一期Ⅰ-002 发电机有功功率","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅰ-002 发电机有功功率","yc_hs_0134","cur_01"]
[1400,"a_马家梁一期Ⅰ-002 发电机绕组温度1","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅰ-002 发电机绕组温度1","yc_hs_0134","cur_13"]
[1401,"a_马家梁一期Ⅰ-002 发电机绕组温度2","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅰ-002 发电机绕组温度2","yc_hs_0134","cur_14"]
[1402,"a_马家梁一期Ⅰ-002 发电机绕组温度3","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅰ-002 发电机绕组温度3","yc_hs_0134","cur_15"]
[1403,"a_马家梁一期Ⅰ-002 机舱柜温度","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅰ-002 机舱柜温度","yc_hs_0134","cur_26"]
[1404,"a_马家梁一期Ⅰ-002 环境温度","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅰ-002 环境温度","yc_hs_0134","cur_59"]
[1405,"a_马家梁一期Ⅰ-002 发电机前轴承温度1","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅰ-002 发电机前轴承温度1","yc_hs_0134","cur_60"]
[1406,"a_马家梁一期Ⅰ-002 发电机后轴承温度1","马家梁风电场","WOF35200074",2,"MJLFD.T1_L1.WTG002.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅰ-002 发电机后轴承温度1","yc_hs_0134","cur_62"]
[1407,"a_马家梁一期Ⅰ-003 风速","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅰ-003 风速","yc_hs_0134","cur_82"]
[1408,"a_马家梁一期Ⅰ-003 机舱与风向夹角","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅰ-003 机舱与风向夹角","yc_hs_0134","cur_83"]
[1409,"a_马家梁一期Ⅰ-003 风向","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅰ-003 风向","yc_hs_0134","cur_84"]
[1410,"a_马家梁一期Ⅰ-003 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅰ-003 偏航角度(扭缆角度）","yc_hs_0134","cur_86"]
[1411,"a_马家梁一期Ⅰ-003 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅰ-003 1#桨叶片角度(桨距角)","yc_hs_0134","cur_87"]
[1412,"a_马家梁一期Ⅰ-003 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅰ-003 2#桨叶片角度(桨距角)","yc_hs_0134","cur_88"]
[1413,"a_马家梁一期Ⅰ-003 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅰ-003 3#桨叶片角度(桨距角)","yc_hs_0134","cur_89"]
[1414,"a_马家梁一期Ⅰ-003 发电机测速模块测量转速","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅰ-003 发电机测速模块测量转速","yc_hs_0134","cur_90"]
[1415,"a_马家梁一期Ⅰ-003 发电机有功功率","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅰ-003 发电机有功功率","yc_hs_0134","cur_91"]
[1416,"a_马家梁一期Ⅰ-003 发电机绕组温度1","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅰ-003 发电机绕组温度1","yc_hs_0135","cur_03"]
[1417,"a_马家梁一期Ⅰ-003 发电机绕组温度2","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅰ-003 发电机绕组温度2","yc_hs_0135","cur_04"]
[1418,"a_马家梁一期Ⅰ-003 发电机绕组温度3","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅰ-003 发电机绕组温度3","yc_hs_0135","cur_05"]
[1419,"a_马家梁一期Ⅰ-003 机舱柜温度","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅰ-003 机舱柜温度","yc_hs_0135","cur_16"]
[1420,"a_马家梁一期Ⅰ-003 环境温度","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅰ-003 环境温度","yc_hs_0135","cur_49"]
[1421,"a_马家梁一期Ⅰ-003 发电机前轴承温度1","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅰ-003 发电机前轴承温度1","yc_hs_0135","cur_50"]
[1422,"a_马家梁一期Ⅰ-003 发电机后轴承温度1","马家梁风电场","WOF35200074",3,"MJLFD.T1_L1.WTG003.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅰ-003 发电机后轴承温度1","yc_hs_0135","cur_52"]
[1423,"a_马家梁一期Ⅰ-004 风速","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅰ-004 风速","yc_hs_0135","cur_72"]
[1424,"a_马家梁一期Ⅰ-004 机舱与风向夹角","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅰ-004 机舱与风向夹角","yc_hs_0135","cur_73"]
[1425,"a_马家梁一期Ⅰ-004 风向","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅰ-004 风向","yc_hs_0135","cur_74"]
[1426,"a_马家梁一期Ⅰ-004 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅰ-004 偏航角度(扭缆角度）","yc_hs_0135","cur_76"]
[1427,"a_马家梁一期Ⅰ-004 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅰ-004 1#桨叶片角度(桨距角)","yc_hs_0135","cur_77"]
[1428,"a_马家梁一期Ⅰ-004 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅰ-004 2#桨叶片角度(桨距角)","yc_hs_0135","cur_78"]
[1429,"a_马家梁一期Ⅰ-004 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅰ-004 3#桨叶片角度(桨距角)","yc_hs_0135","cur_79"]
[1430,"a_马家梁一期Ⅰ-004 发电机测速模块测量转速","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅰ-004 发电机测速模块测量转速","yc_hs_0135","cur_80"]
[1431,"a_马家梁一期Ⅰ-004 发电机有功功率","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅰ-004 发电机有功功率","yc_hs_0135","cur_81"]
[1432,"a_马家梁一期Ⅰ-004 发电机绕组温度1","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅰ-004 发电机绕组温度1","yc_hs_0135","cur_93"]
[1433,"a_马家梁一期Ⅰ-004 发电机绕组温度2","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅰ-004 发电机绕组温度2","yc_hs_0135","cur_94"]
[1434,"a_马家梁一期Ⅰ-004 发电机绕组温度3","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅰ-004 发电机绕组温度3","yc_hs_0135","cur_95"]
[1435,"a_马家梁一期Ⅰ-004 机舱柜温度","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅰ-004 机舱柜温度","yc_hs_0136","cur_06"]
[1436,"a_马家梁一期Ⅰ-004 环境温度","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅰ-004 环境温度","yc_hs_0136","cur_39"]
[1437,"a_马家梁一期Ⅰ-004 发电机前轴承温度1","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅰ-004 发电机前轴承温度1","yc_hs_0136","cur_40"]
[1438,"a_马家梁一期Ⅰ-004 发电机后轴承温度1","马家梁风电场","WOF35200074",4,"MJLFD.T1_L1.WTG004.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅰ-004 发电机后轴承温度1","yc_hs_0136","cur_42"]
[1439,"a_马家梁一期Ⅰ-005 风速","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅰ-005 风速","yc_hs_0136","cur_62"]
[1440,"a_马家梁一期Ⅰ-005 机舱与风向夹角","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅰ-005 机舱与风向夹角","yc_hs_0136","cur_63"]
[1441,"a_马家梁一期Ⅰ-005 风向","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅰ-005 风向","yc_hs_0136","cur_64"]
[1442,"a_马家梁一期Ⅰ-005 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅰ-005 偏航角度(扭缆角度）","yc_hs_0136","cur_66"]
[1443,"a_马家梁一期Ⅰ-005 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅰ-005 1#桨叶片角度(桨距角)","yc_hs_0136","cur_67"]
[1444,"a_马家梁一期Ⅰ-005 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅰ-005 2#桨叶片角度(桨距角)","yc_hs_0136","cur_68"]
[1445,"a_马家梁一期Ⅰ-005 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅰ-005 3#桨叶片角度(桨距角)","yc_hs_0136","cur_69"]
[1446,"a_马家梁一期Ⅰ-005 发电机测速模块测量转速","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅰ-005 发电机测速模块测量转速","yc_hs_0136","cur_70"]
[1447,"a_马家梁一期Ⅰ-005 发电机有功功率","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅰ-005 发电机有功功率","yc_hs_0136","cur_71"]
[1448,"a_马家梁一期Ⅰ-005 发电机绕组温度1","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅰ-005 发电机绕组温度1","yc_hs_0136","cur_83"]
[1449,"a_马家梁一期Ⅰ-005 发电机绕组温度2","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅰ-005 发电机绕组温度2","yc_hs_0136","cur_84"]
[1450,"a_马家梁一期Ⅰ-005 发电机绕组温度3","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅰ-005 发电机绕组温度3","yc_hs_0136","cur_85"]
[1451,"a_马家梁一期Ⅰ-005 机舱柜温度","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅰ-005 机舱柜温度","yc_hs_0136","cur_96"]
[1452,"a_马家梁一期Ⅰ-005 环境温度","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅰ-005 环境温度","yc_hs_0137","cur_29"]
[1453,"a_马家梁一期Ⅰ-005 发电机前轴承温度1","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅰ-005 发电机前轴承温度1","yc_hs_0137","cur_30"]
[1454,"a_马家梁一期Ⅰ-005 发电机后轴承温度1","马家梁风电场","WOF35200074",5,"MJLFD.T1_L1.WTG005.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅰ-005 发电机后轴承温度1","yc_hs_0137","cur_32"]
[1455,"a_马家梁一期Ⅰ-006 风速","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅰ-006 风速","yc_hs_0137","cur_52"]
[1456,"a_马家梁一期Ⅰ-006 机舱与风向夹角","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅰ-006 机舱与风向夹角","yc_hs_0137","cur_53"]
[1457,"a_马家梁一期Ⅰ-006 风向","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅰ-006 风向","yc_hs_0137","cur_54"]
[1458,"a_马家梁一期Ⅰ-006 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅰ-006 偏航角度(扭缆角度）","yc_hs_0137","cur_56"]
[1459,"a_马家梁一期Ⅰ-006 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅰ-006 1#桨叶片角度(桨距角)","yc_hs_0137","cur_57"]
[1460,"a_马家梁一期Ⅰ-006 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅰ-006 2#桨叶片角度(桨距角)","yc_hs_0137","cur_58"]
[1461,"a_马家梁一期Ⅰ-006 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅰ-006 3#桨叶片角度(桨距角)","yc_hs_0137","cur_59"]
[1462,"a_马家梁一期Ⅰ-006 发电机测速模块测量转速","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅰ-006 发电机测速模块测量转速","yc_hs_0137","cur_60"]
[1463,"a_马家梁一期Ⅰ-006 发电机有功功率","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅰ-006 发电机有功功率","yc_hs_0137","cur_61"]
[1464,"a_马家梁一期Ⅰ-006 发电机绕组温度1","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅰ-006 发电机绕组温度1","yc_hs_0137","cur_73"]
[1465,"a_马家梁一期Ⅰ-006 发电机绕组温度2","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅰ-006 发电机绕组温度2","yc_hs_0137","cur_74"]
[1466,"a_马家梁一期Ⅰ-006 发电机绕组温度3","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅰ-006 发电机绕组温度3","yc_hs_0137","cur_75"]
[1467,"a_马家梁一期Ⅰ-006 机舱柜温度","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅰ-006 机舱柜温度","yc_hs_0137","cur_86"]
[1468,"a_马家梁一期Ⅰ-006 环境温度","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅰ-006 环境温度","yc_hs_0138","cur_19"]
[1469,"a_马家梁一期Ⅰ-006 发电机前轴承温度1","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅰ-006 发电机前轴承温度1","yc_hs_0138","cur_20"]
[1470,"a_马家梁一期Ⅰ-006 发电机后轴承温度1","马家梁风电场","WOF35200074",6,"MJLFD.T1_L1.WTG006.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅰ-006 发电机后轴承温度1","yc_hs_0138","cur_22"]
[1471,"a_马家梁一期Ⅰ-007 风速","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅰ-007 风速","yc_hs_0138","cur_42"]
[1472,"a_马家梁一期Ⅰ-007 机舱与风向夹角","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅰ-007 机舱与风向夹角","yc_hs_0138","cur_43"]
[1473,"a_马家梁一期Ⅰ-007 风向","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅰ-007 风向","yc_hs_0138","cur_44"]
[1474,"a_马家梁一期Ⅰ-007 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅰ-007 偏航角度(扭缆角度）","yc_hs_0138","cur_46"]
[1475,"a_马家梁一期Ⅰ-007 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅰ-007 1#桨叶片角度(桨距角)","yc_hs_0138","cur_47"]
[1476,"a_马家梁一期Ⅰ-007 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅰ-007 2#桨叶片角度(桨距角)","yc_hs_0138","cur_48"]
[1477,"a_马家梁一期Ⅰ-007 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅰ-007 3#桨叶片角度(桨距角)","yc_hs_0138","cur_49"]
[1478,"a_马家梁一期Ⅰ-007 发电机测速模块测量转速","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅰ-007 发电机测速模块测量转速","yc_hs_0138","cur_50"]
[1479,"a_马家梁一期Ⅰ-007 发电机有功功率","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅰ-007 发电机有功功率","yc_hs_0138","cur_51"]
[1480,"a_马家梁一期Ⅰ-007 发电机绕组温度1","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅰ-007 发电机绕组温度1","yc_hs_0138","cur_63"]
[1481,"a_马家梁一期Ⅰ-007 发电机绕组温度2","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅰ-007 发电机绕组温度2","yc_hs_0138","cur_64"]
[1482,"a_马家梁一期Ⅰ-007 发电机绕组温度3","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅰ-007 发电机绕组温度3","yc_hs_0138","cur_65"]
[1483,"a_马家梁一期Ⅰ-007 机舱柜温度","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅰ-007 机舱柜温度","yc_hs_0138","cur_76"]
[1484,"a_马家梁一期Ⅰ-007 环境温度","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅰ-007 环境温度","yc_hs_0139","cur_09"]
[1485,"a_马家梁一期Ⅰ-007 发电机前轴承温度1","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅰ-007 发电机前轴承温度1","yc_hs_0139","cur_10"]
[1486,"a_马家梁一期Ⅰ-007 发电机后轴承温度1","马家梁风电场","WOF35200074",7,"MJLFD.T1_L1.WTG007.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅰ-007 发电机后轴承温度1","yc_hs_0139","cur_12"]
[1487,"a_马家梁一期Ⅰ-008 风速","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅰ-008 风速","yc_hs_0139","cur_32"]
[1488,"a_马家梁一期Ⅰ-008 机舱与风向夹角","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅰ-008 机舱与风向夹角","yc_hs_0139","cur_33"]
[1489,"a_马家梁一期Ⅰ-008 风向","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅰ-008 风向","yc_hs_0139","cur_34"]
[1490,"a_马家梁一期Ⅰ-008 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅰ-008 偏航角度(扭缆角度）","yc_hs_0139","cur_36"]
[1491,"a_马家梁一期Ⅰ-008 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅰ-008 1#桨叶片角度(桨距角)","yc_hs_0139","cur_37"]
[1492,"a_马家梁一期Ⅰ-008 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅰ-008 2#桨叶片角度(桨距角)","yc_hs_0139","cur_38"]
[1493,"a_马家梁一期Ⅰ-008 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅰ-008 3#桨叶片角度(桨距角)","yc_hs_0139","cur_39"]
[1494,"a_马家梁一期Ⅰ-008 发电机测速模块测量转速","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅰ-008 发电机测速模块测量转速","yc_hs_0139","cur_40"]
[1495,"a_马家梁一期Ⅰ-008 发电机有功功率","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅰ-008 发电机有功功率","yc_hs_0139","cur_41"]
[1496,"a_马家梁一期Ⅰ-008 发电机绕组温度1","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅰ-008 发电机绕组温度1","yc_hs_0139","cur_53"]
[1497,"a_马家梁一期Ⅰ-008 发电机绕组温度2","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅰ-008 发电机绕组温度2","yc_hs_0139","cur_54"]
[1498,"a_马家梁一期Ⅰ-008 发电机绕组温度3","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅰ-008 发电机绕组温度3","yc_hs_0139","cur_55"]
[1499,"a_马家梁一期Ⅰ-008 机舱柜温度","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅰ-008 机舱柜温度","yc_hs_0139","cur_66"]
[1500,"a_马家梁一期Ⅰ-008 环境温度","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅰ-008 环境温度","yc_hs_0139","cur_99"]
[1501,"a_马家梁一期Ⅰ-008 发电机前轴承温度1","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅰ-008 发电机前轴承温度1","yc_hs_0139","cur_100"]
[1502,"a_马家梁一期Ⅰ-008 发电机后轴承温度1","马家梁风电场","WOF35200074",8,"MJLFD.T1_L1.WTG008.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅰ-008 发电机后轴承温度1","yc_hs_0140","cur_02"]
[1503,"a_马家梁一期Ⅰ-009 风速","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅰ-009 风速","yc_hs_0140","cur_22"]
[1504,"a_马家梁一期Ⅰ-009 机舱与风向夹角","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅰ-009 机舱与风向夹角","yc_hs_0140","cur_23"]
[1505,"a_马家梁一期Ⅰ-009 风向","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅰ-009 风向","yc_hs_0140","cur_24"]
[1506,"a_马家梁一期Ⅰ-009 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅰ-009 偏航角度(扭缆角度）","yc_hs_0140","cur_26"]
[1507,"a_马家梁一期Ⅰ-009 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅰ-009 1#桨叶片角度(桨距角)","yc_hs_0140","cur_27"]
[1508,"a_马家梁一期Ⅰ-009 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅰ-009 2#桨叶片角度(桨距角)","yc_hs_0140","cur_28"]
[1509,"a_马家梁一期Ⅰ-009 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅰ-009 3#桨叶片角度(桨距角)","yc_hs_0140","cur_29"]
[1510,"a_马家梁一期Ⅰ-009 发电机测速模块测量转速","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅰ-009 发电机测速模块测量转速","yc_hs_0140","cur_30"]
[1511,"a_马家梁一期Ⅰ-009 发电机有功功率","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅰ-009 发电机有功功率","yc_hs_0140","cur_31"]
[1512,"a_马家梁一期Ⅰ-009 发电机绕组温度1","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅰ-009 发电机绕组温度1","yc_hs_0140","cur_43"]
[1513,"a_马家梁一期Ⅰ-009 发电机绕组温度2","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅰ-009 发电机绕组温度2","yc_hs_0140","cur_44"]
[1514,"a_马家梁一期Ⅰ-009 发电机绕组温度3","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅰ-009 发电机绕组温度3","yc_hs_0140","cur_45"]
[1515,"a_马家梁一期Ⅰ-009 机舱柜温度","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅰ-009 机舱柜温度","yc_hs_0140","cur_56"]
[1516,"a_马家梁一期Ⅰ-009 环境温度","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅰ-009 环境温度","yc_hs_0140","cur_89"]
[1517,"a_马家梁一期Ⅰ-009 发电机前轴承温度1","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅰ-009 发电机前轴承温度1","yc_hs_0140","cur_90"]
[1518,"a_马家梁一期Ⅰ-009 发电机后轴承温度1","马家梁风电场","WOF35200074",9,"MJLFD.T1_L1.WTG009.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅰ-009 发电机后轴承温度1","yc_hs_0140","cur_92"]
[1519,"a_马家梁一期Ⅰ-010 风速","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅰ-010 风速","yc_hs_0141","cur_12"]
[1520,"a_马家梁一期Ⅰ-010 机舱与风向夹角","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅰ-010 机舱与风向夹角","yc_hs_0141","cur_13"]
[1521,"a_马家梁一期Ⅰ-010 风向","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅰ-010 风向","yc_hs_0141","cur_14"]
[1522,"a_马家梁一期Ⅰ-010 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅰ-010 偏航角度(扭缆角度）","yc_hs_0141","cur_16"]
[1523,"a_马家梁一期Ⅰ-010 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅰ-010 1#桨叶片角度(桨距角)","yc_hs_0141","cur_17"]
[1524,"a_马家梁一期Ⅰ-010 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅰ-010 2#桨叶片角度(桨距角)","yc_hs_0141","cur_18"]
[1525,"a_马家梁一期Ⅰ-010 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅰ-010 3#桨叶片角度(桨距角)","yc_hs_0141","cur_19"]
[1526,"a_马家梁一期Ⅰ-010 发电机测速模块测量转速","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅰ-010 发电机测速模块测量转速","yc_hs_0141","cur_20"]
[1527,"a_马家梁一期Ⅰ-010 发电机有功功率","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅰ-010 发电机有功功率","yc_hs_0141","cur_21"]
[1528,"a_马家梁一期Ⅰ-010 发电机绕组温度1","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅰ-010 发电机绕组温度1","yc_hs_0141","cur_33"]
[1529,"a_马家梁一期Ⅰ-010 发电机绕组温度2","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅰ-010 发电机绕组温度2","yc_hs_0141","cur_34"]
[1530,"a_马家梁一期Ⅰ-010 发电机绕组温度3","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅰ-010 发电机绕组温度3","yc_hs_0141","cur_35"]
[1531,"a_马家梁一期Ⅰ-010 机舱柜温度","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅰ-010 机舱柜温度","yc_hs_0141","cur_46"]
[1532,"a_马家梁一期Ⅰ-010 环境温度","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅰ-010 环境温度","yc_hs_0141","cur_79"]
[1533,"a_马家梁一期Ⅰ-010 发电机前轴承温度1","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅰ-010 发电机前轴承温度1","yc_hs_0141","cur_80"]
[1534,"a_马家梁一期Ⅰ-010 发电机后轴承温度1","马家梁风电场","WOF35200074",10,"MJLFD.T1_L1.WTG010.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅰ-010 发电机后轴承温度1","yc_hs_0141","cur_82"]
[1535,"a_马家梁一期Ⅰ-011 风速","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅰ-011 风速","yc_hs_0142","cur_02"]
[1536,"a_马家梁一期Ⅰ-011 机舱与风向夹角","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅰ-011 机舱与风向夹角","yc_hs_0142","cur_03"]
[1537,"a_马家梁一期Ⅰ-011 风向","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅰ-011 风向","yc_hs_0142","cur_04"]
[1538,"a_马家梁一期Ⅰ-011 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅰ-011 偏航角度(扭缆角度）","yc_hs_0142","cur_06"]
[1539,"a_马家梁一期Ⅰ-011 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅰ-011 1#桨叶片角度(桨距角)","yc_hs_0142","cur_07"]
[1540,"a_马家梁一期Ⅰ-011 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅰ-011 2#桨叶片角度(桨距角)","yc_hs_0142","cur_08"]
[1541,"a_马家梁一期Ⅰ-011 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅰ-011 3#桨叶片角度(桨距角)","yc_hs_0142","cur_09"]
[1542,"a_马家梁一期Ⅰ-011 发电机测速模块测量转速","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅰ-011 发电机测速模块测量转速","yc_hs_0142","cur_10"]
[1543,"a_马家梁一期Ⅰ-011 发电机有功功率","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅰ-011 发电机有功功率","yc_hs_0142","cur_11"]
[1544,"a_马家梁一期Ⅰ-011 发电机绕组温度1","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅰ-011 发电机绕组温度1","yc_hs_0142","cur_23"]
[1545,"a_马家梁一期Ⅰ-011 发电机绕组温度2","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅰ-011 发电机绕组温度2","yc_hs_0142","cur_24"]
[1546,"a_马家梁一期Ⅰ-011 发电机绕组温度3","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅰ-011 发电机绕组温度3","yc_hs_0142","cur_25"]
[1547,"a_马家梁一期Ⅰ-011 机舱柜温度","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅰ-011 机舱柜温度","yc_hs_0142","cur_36"]
[1548,"a_马家梁一期Ⅰ-011 环境温度","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅰ-011 环境温度","yc_hs_0142","cur_69"]
[1549,"a_马家梁一期Ⅰ-011 发电机前轴承温度1","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅰ-011 发电机前轴承温度1","yc_hs_0142","cur_70"]
[1550,"a_马家梁一期Ⅰ-011 发电机后轴承温度1","马家梁风电场","WOF35200074",11,"MJLFD.T1_L1.WTG011.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅰ-011 发电机后轴承温度1","yc_hs_0142","cur_72"]
[1551,"a_马家梁一期Ⅰ-012 风速","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅰ-012 风速","yc_hs_0142","cur_92"]
[1552,"a_马家梁一期Ⅰ-012 机舱与风向夹角","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅰ-012 机舱与风向夹角","yc_hs_0142","cur_93"]
[1553,"a_马家梁一期Ⅰ-012 风向","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅰ-012 风向","yc_hs_0142","cur_94"]
[1554,"a_马家梁一期Ⅰ-012 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅰ-012 偏航角度(扭缆角度）","yc_hs_0142","cur_96"]
[1555,"a_马家梁一期Ⅰ-012 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅰ-012 1#桨叶片角度(桨距角)","yc_hs_0142","cur_97"]
[1556,"a_马家梁一期Ⅰ-012 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅰ-012 2#桨叶片角度(桨距角)","yc_hs_0142","cur_98"]
[1557,"a_马家梁一期Ⅰ-012 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅰ-012 3#桨叶片角度(桨距角)","yc_hs_0142","cur_99"]
[1558,"a_马家梁一期Ⅰ-012 发电机测速模块测量转速","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅰ-012 发电机测速模块测量转速","yc_hs_0142","cur_100"]
[1559,"a_马家梁一期Ⅰ-012 发电机有功功率","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅰ-012 发电机有功功率","yc_hs_0143","cur_01"]
[1560,"a_马家梁一期Ⅰ-012 发电机绕组温度1","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅰ-012 发电机绕组温度1","yc_hs_0143","cur_13"]
[1561,"a_马家梁一期Ⅰ-012 发电机绕组温度2","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅰ-012 发电机绕组温度2","yc_hs_0143","cur_14"]
[1562,"a_马家梁一期Ⅰ-012 发电机绕组温度3","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅰ-012 发电机绕组温度3","yc_hs_0143","cur_15"]
[1563,"a_马家梁一期Ⅰ-012 机舱柜温度","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅰ-012 机舱柜温度","yc_hs_0143","cur_26"]
[1564,"a_马家梁一期Ⅰ-012 环境温度","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅰ-012 环境温度","yc_hs_0143","cur_59"]
[1565,"a_马家梁一期Ⅰ-012 发电机前轴承温度1","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅰ-012 发电机前轴承温度1","yc_hs_0143","cur_60"]
[1566,"a_马家梁一期Ⅰ-012 发电机后轴承温度1","马家梁风电场","WOF35200074",12,"MJLFD.T1_L1.WTG012.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅰ-012 发电机后轴承温度1","yc_hs_0143","cur_62"]
[1567,"a_马家梁一期Ⅰ-013 风速","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅰ-013 风速","yc_hs_0143","cur_82"]
[1568,"a_马家梁一期Ⅰ-013 机舱与风向夹角","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅰ-013 机舱与风向夹角","yc_hs_0143","cur_83"]
[1569,"a_马家梁一期Ⅰ-013 风向","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅰ-013 风向","yc_hs_0143","cur_84"]
[1570,"a_马家梁一期Ⅰ-013 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅰ-013 偏航角度(扭缆角度）","yc_hs_0143","cur_86"]
[1571,"a_马家梁一期Ⅰ-013 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅰ-013 1#桨叶片角度(桨距角)","yc_hs_0143","cur_87"]
[1572,"a_马家梁一期Ⅰ-013 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅰ-013 2#桨叶片角度(桨距角)","yc_hs_0143","cur_88"]
[1573,"a_马家梁一期Ⅰ-013 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅰ-013 3#桨叶片角度(桨距角)","yc_hs_0143","cur_89"]
[1574,"a_马家梁一期Ⅰ-013 发电机测速模块测量转速","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅰ-013 发电机测速模块测量转速","yc_hs_0143","cur_90"]
[1575,"a_马家梁一期Ⅰ-013 发电机有功功率","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅰ-013 发电机有功功率","yc_hs_0143","cur_91"]
[1576,"a_马家梁一期Ⅰ-013 发电机绕组温度1","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅰ-013 发电机绕组温度1","yc_hs_0144","cur_03"]
[1577,"a_马家梁一期Ⅰ-013 发电机绕组温度2","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅰ-013 发电机绕组温度2","yc_hs_0144","cur_04"]
[1578,"a_马家梁一期Ⅰ-013 发电机绕组温度3","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅰ-013 发电机绕组温度3","yc_hs_0144","cur_05"]
[1579,"a_马家梁一期Ⅰ-013 机舱柜温度","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅰ-013 机舱柜温度","yc_hs_0144","cur_16"]
[1580,"a_马家梁一期Ⅰ-013 环境温度","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅰ-013 环境温度","yc_hs_0144","cur_49"]
[1581,"a_马家梁一期Ⅰ-013 发电机前轴承温度1","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅰ-013 发电机前轴承温度1","yc_hs_0144","cur_50"]
[1582,"a_马家梁一期Ⅰ-013 发电机后轴承温度1","马家梁风电场","WOF35200074",13,"MJLFD.T1_L1.WTG013.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅰ-013 发电机后轴承温度1","yc_hs_0144","cur_52"]
[1583,"a_马家梁一期Ⅱ-014 风速","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅱ-014 风速","yc_hs_0144","cur_72"]
[1584,"a_马家梁一期Ⅱ-014 机舱与风向夹角","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅱ-014 机舱与风向夹角","yc_hs_0144","cur_73"]
[1585,"a_马家梁一期Ⅱ-014 风向","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅱ-014 风向","yc_hs_0144","cur_74"]
[1586,"a_马家梁一期Ⅱ-014 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅱ-014 偏航角度(扭缆角度）","yc_hs_0144","cur_76"]
[1587,"a_马家梁一期Ⅱ-014 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅱ-014 1#桨叶片角度(桨距角)","yc_hs_0144","cur_77"]
[1588,"a_马家梁一期Ⅱ-014 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅱ-014 2#桨叶片角度(桨距角)","yc_hs_0144","cur_78"]
[1589,"a_马家梁一期Ⅱ-014 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅱ-014 3#桨叶片角度(桨距角)","yc_hs_0144","cur_79"]
[1590,"a_马家梁一期Ⅱ-014 发电机测速模块测量转速","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅱ-014 发电机测速模块测量转速","yc_hs_0144","cur_80"]
[1591,"a_马家梁一期Ⅱ-014 发电机有功功率","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅱ-014 发电机有功功率","yc_hs_0144","cur_81"]
[1592,"a_马家梁一期Ⅱ-014 发电机绕组温度1","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅱ-014 发电机绕组温度1","yc_hs_0144","cur_93"]
[1593,"a_马家梁一期Ⅱ-014 发电机绕组温度2","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅱ-014 发电机绕组温度2","yc_hs_0144","cur_94"]
[1594,"a_马家梁一期Ⅱ-014 发电机绕组温度3","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅱ-014 发电机绕组温度3","yc_hs_0144","cur_95"]
[1595,"a_马家梁一期Ⅱ-014 机舱柜温度","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅱ-014 机舱柜温度","yc_hs_0145","cur_06"]
[1596,"a_马家梁一期Ⅱ-014 环境温度","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅱ-014 环境温度","yc_hs_0145","cur_39"]
[1597,"a_马家梁一期Ⅱ-014 发电机前轴承温度1","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅱ-014 发电机前轴承温度1","yc_hs_0145","cur_40"]
[1598,"a_马家梁一期Ⅱ-014 发电机后轴承温度1","马家梁风电场","WOF35200074",14,"MJLFD.T1_L2.WTG014.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅱ-014 发电机后轴承温度1","yc_hs_0145","cur_42"]
[1599,"a_马家梁一期Ⅱ-015 风速","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅱ-015 风速","yc_hs_0145","cur_62"]
[1600,"a_马家梁一期Ⅱ-015 机舱与风向夹角","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅱ-015 机舱与风向夹角","yc_hs_0145","cur_63"]
[1601,"a_马家梁一期Ⅱ-015 风向","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅱ-015 风向","yc_hs_0145","cur_64"]
[1602,"a_马家梁一期Ⅱ-015 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅱ-015 偏航角度(扭缆角度）","yc_hs_0145","cur_66"]
[1603,"a_马家梁一期Ⅱ-015 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅱ-015 1#桨叶片角度(桨距角)","yc_hs_0145","cur_67"]
[1604,"a_马家梁一期Ⅱ-015 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅱ-015 2#桨叶片角度(桨距角)","yc_hs_0145","cur_68"]
[1605,"a_马家梁一期Ⅱ-015 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅱ-015 3#桨叶片角度(桨距角)","yc_hs_0145","cur_69"]
[1606,"a_马家梁一期Ⅱ-015 发电机测速模块测量转速","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅱ-015 发电机测速模块测量转速","yc_hs_0145","cur_70"]
[1607,"a_马家梁一期Ⅱ-015 发电机有功功率","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅱ-015 发电机有功功率","yc_hs_0145","cur_71"]
[1608,"a_马家梁一期Ⅱ-015 发电机绕组温度1","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅱ-015 发电机绕组温度1","yc_hs_0145","cur_83"]
[1609,"a_马家梁一期Ⅱ-015 发电机绕组温度2","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅱ-015 发电机绕组温度2","yc_hs_0145","cur_84"]
[1610,"a_马家梁一期Ⅱ-015 发电机绕组温度3","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅱ-015 发电机绕组温度3","yc_hs_0145","cur_85"]
[1611,"a_马家梁一期Ⅱ-015 机舱柜温度","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅱ-015 机舱柜温度","yc_hs_0145","cur_96"]
[1612,"a_马家梁一期Ⅱ-015 环境温度","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅱ-015 环境温度","yc_hs_0146","cur_29"]
[1613,"a_马家梁一期Ⅱ-015 发电机前轴承温度1","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅱ-015 发电机前轴承温度1","yc_hs_0146","cur_30"]
[1614,"a_马家梁一期Ⅱ-015 发电机后轴承温度1","马家梁风电场","WOF35200074",15,"MJLFD.T1_L2.WTG015.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅱ-015 发电机后轴承温度1","yc_hs_0146","cur_32"]
[1615,"a_马家梁一期Ⅱ-016 风速","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅱ-016 风速","yc_hs_0146","cur_52"]
[1616,"a_马家梁一期Ⅱ-016 机舱与风向夹角","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅱ-016 机舱与风向夹角","yc_hs_0146","cur_53"]
[1617,"a_马家梁一期Ⅱ-016 风向","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅱ-016 风向","yc_hs_0146","cur_54"]
[1618,"a_马家梁一期Ⅱ-016 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅱ-016 偏航角度(扭缆角度）","yc_hs_0146","cur_56"]
[1619,"a_马家梁一期Ⅱ-016 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅱ-016 1#桨叶片角度(桨距角)","yc_hs_0146","cur_57"]
[1620,"a_马家梁一期Ⅱ-016 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅱ-016 2#桨叶片角度(桨距角)","yc_hs_0146","cur_58"]
[1621,"a_马家梁一期Ⅱ-016 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅱ-016 3#桨叶片角度(桨距角)","yc_hs_0146","cur_59"]
[1622,"a_马家梁一期Ⅱ-016 发电机测速模块测量转速","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅱ-016 发电机测速模块测量转速","yc_hs_0146","cur_60"]
[1623,"a_马家梁一期Ⅱ-016 发电机有功功率","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅱ-016 发电机有功功率","yc_hs_0146","cur_61"]
[1624,"a_马家梁一期Ⅱ-016 发电机绕组温度1","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅱ-016 发电机绕组温度1","yc_hs_0146","cur_73"]
[1625,"a_马家梁一期Ⅱ-016 发电机绕组温度2","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅱ-016 发电机绕组温度2","yc_hs_0146","cur_74"]
[1626,"a_马家梁一期Ⅱ-016 发电机绕组温度3","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅱ-016 发电机绕组温度3","yc_hs_0146","cur_75"]
[1627,"a_马家梁一期Ⅱ-016 机舱柜温度","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅱ-016 机舱柜温度","yc_hs_0146","cur_86"]
[1628,"a_马家梁一期Ⅱ-016 环境温度","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅱ-016 环境温度","yc_hs_0147","cur_19"]
[1629,"a_马家梁一期Ⅱ-016 发电机前轴承温度1","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅱ-016 发电机前轴承温度1","yc_hs_0147","cur_20"]
[1630,"a_马家梁一期Ⅱ-016 发电机后轴承温度1","马家梁风电场","WOF35200074",16,"MJLFD.T1_L2.WTG016.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅱ-016 发电机后轴承温度1","yc_hs_0147","cur_22"]
[1631,"a_马家梁一期Ⅱ-017 风速","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅱ-017 风速","yc_hs_0147","cur_42"]
[1632,"a_马家梁一期Ⅱ-017 机舱与风向夹角","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅱ-017 机舱与风向夹角","yc_hs_0147","cur_43"]
[1633,"a_马家梁一期Ⅱ-017 风向","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅱ-017 风向","yc_hs_0147","cur_44"]
[1634,"a_马家梁一期Ⅱ-017 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅱ-017 偏航角度(扭缆角度）","yc_hs_0147","cur_46"]
[1635,"a_马家梁一期Ⅱ-017 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅱ-017 1#桨叶片角度(桨距角)","yc_hs_0147","cur_47"]
[1636,"a_马家梁一期Ⅱ-017 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅱ-017 2#桨叶片角度(桨距角)","yc_hs_0147","cur_48"]
[1637,"a_马家梁一期Ⅱ-017 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅱ-017 3#桨叶片角度(桨距角)","yc_hs_0147","cur_49"]
[1638,"a_马家梁一期Ⅱ-017 发电机测速模块测量转速","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅱ-017 发电机测速模块测量转速","yc_hs_0147","cur_50"]
[1639,"a_马家梁一期Ⅱ-017 发电机有功功率","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅱ-017 发电机有功功率","yc_hs_0147","cur_51"]
[1640,"a_马家梁一期Ⅱ-017 发电机绕组温度1","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅱ-017 发电机绕组温度1","yc_hs_0147","cur_63"]
[1641,"a_马家梁一期Ⅱ-017 发电机绕组温度2","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅱ-017 发电机绕组温度2","yc_hs_0147","cur_64"]
[1642,"a_马家梁一期Ⅱ-017 发电机绕组温度3","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅱ-017 发电机绕组温度3","yc_hs_0147","cur_65"]
[1643,"a_马家梁一期Ⅱ-017 机舱柜温度","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅱ-017 机舱柜温度","yc_hs_0147","cur_76"]
[1644,"a_马家梁一期Ⅱ-017 环境温度","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅱ-017 环境温度","yc_hs_0148","cur_09"]
[1645,"a_马家梁一期Ⅱ-017 发电机前轴承温度1","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅱ-017 发电机前轴承温度1","yc_hs_0148","cur_10"]
[1646,"a_马家梁一期Ⅱ-017 发电机后轴承温度1","马家梁风电场","WOF35200074",17,"MJLFD.T1_L2.WTG017.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅱ-017 发电机后轴承温度1","yc_hs_0148","cur_12"]
[1647,"a_马家梁一期Ⅱ-018 风速","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅱ-018 风速","yc_hs_0148","cur_32"]
[1648,"a_马家梁一期Ⅱ-018 机舱与风向夹角","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅱ-018 机舱与风向夹角","yc_hs_0148","cur_33"]
[1649,"a_马家梁一期Ⅱ-018 风向","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅱ-018 风向","yc_hs_0148","cur_34"]
[1650,"a_马家梁一期Ⅱ-018 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅱ-018 偏航角度(扭缆角度）","yc_hs_0148","cur_36"]
[1651,"a_马家梁一期Ⅱ-018 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅱ-018 1#桨叶片角度(桨距角)","yc_hs_0148","cur_37"]
[1652,"a_马家梁一期Ⅱ-018 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅱ-018 2#桨叶片角度(桨距角)","yc_hs_0148","cur_38"]
[1653,"a_马家梁一期Ⅱ-018 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅱ-018 3#桨叶片角度(桨距角)","yc_hs_0148","cur_39"]
[1654,"a_马家梁一期Ⅱ-018 发电机测速模块测量转速","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅱ-018 发电机测速模块测量转速","yc_hs_0148","cur_40"]
[1655,"a_马家梁一期Ⅱ-018 发电机有功功率","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅱ-018 发电机有功功率","yc_hs_0148","cur_41"]
[1656,"a_马家梁一期Ⅱ-018 发电机绕组温度1","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅱ-018 发电机绕组温度1","yc_hs_0148","cur_53"]
[1657,"a_马家梁一期Ⅱ-018 发电机绕组温度2","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅱ-018 发电机绕组温度2","yc_hs_0148","cur_54"]
[1658,"a_马家梁一期Ⅱ-018 发电机绕组温度3","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅱ-018 发电机绕组温度3","yc_hs_0148","cur_55"]
[1659,"a_马家梁一期Ⅱ-018 机舱柜温度","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅱ-018 机舱柜温度","yc_hs_0148","cur_66"]
[1660,"a_马家梁一期Ⅱ-018 环境温度","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅱ-018 环境温度","yc_hs_0148","cur_99"]
[1661,"a_马家梁一期Ⅱ-018 发电机前轴承温度1","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅱ-018 发电机前轴承温度1","yc_hs_0148","cur_100"]
[1662,"a_马家梁一期Ⅱ-018 发电机后轴承温度1","马家梁风电场","WOF35200074",18,"MJLFD.T1_L2.WTG018.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅱ-018 发电机后轴承温度1","yc_hs_0149","cur_02"]
[1663,"a_马家梁一期Ⅱ-019 风速","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅱ-019 风速","yc_hs_0149","cur_22"]
[1664,"a_马家梁一期Ⅱ-019 机舱与风向夹角","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅱ-019 机舱与风向夹角","yc_hs_0149","cur_23"]
[1665,"a_马家梁一期Ⅱ-019 风向","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅱ-019 风向","yc_hs_0149","cur_24"]
[1666,"a_马家梁一期Ⅱ-019 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅱ-019 偏航角度(扭缆角度）","yc_hs_0149","cur_26"]
[1667,"a_马家梁一期Ⅱ-019 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅱ-019 1#桨叶片角度(桨距角)","yc_hs_0149","cur_27"]
[1668,"a_马家梁一期Ⅱ-019 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅱ-019 2#桨叶片角度(桨距角)","yc_hs_0149","cur_28"]
[1669,"a_马家梁一期Ⅱ-019 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅱ-019 3#桨叶片角度(桨距角)","yc_hs_0149","cur_29"]
[1670,"a_马家梁一期Ⅱ-019 发电机测速模块测量转速","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅱ-019 发电机测速模块测量转速","yc_hs_0149","cur_30"]
[1671,"a_马家梁一期Ⅱ-019 发电机有功功率","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅱ-019 发电机有功功率","yc_hs_0149","cur_31"]
[1672,"a_马家梁一期Ⅱ-019 发电机绕组温度1","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅱ-019 发电机绕组温度1","yc_hs_0149","cur_43"]
[1673,"a_马家梁一期Ⅱ-019 发电机绕组温度2","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅱ-019 发电机绕组温度2","yc_hs_0149","cur_44"]
[1674,"a_马家梁一期Ⅱ-019 发电机绕组温度3","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅱ-019 发电机绕组温度3","yc_hs_0149","cur_45"]
[1675,"a_马家梁一期Ⅱ-019 机舱柜温度","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅱ-019 机舱柜温度","yc_hs_0149","cur_56"]
[1676,"a_马家梁一期Ⅱ-019 环境温度","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅱ-019 环境温度","yc_hs_0149","cur_89"]
[1677,"a_马家梁一期Ⅱ-019 发电机前轴承温度1","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅱ-019 发电机前轴承温度1","yc_hs_0149","cur_90"]
[1678,"a_马家梁一期Ⅱ-019 发电机后轴承温度1","马家梁风电场","WOF35200074",19,"MJLFD.T1_L2.WTG019.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅱ-019 发电机后轴承温度1","yc_hs_0149","cur_92"]
[1679,"a_马家梁一期Ⅱ-020 风速","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅱ-020 风速","yc_hs_0150","cur_12"]
[1680,"a_马家梁一期Ⅱ-020 机舱与风向夹角","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅱ-020 机舱与风向夹角","yc_hs_0150","cur_13"]
[1681,"a_马家梁一期Ⅱ-020 风向","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅱ-020 风向","yc_hs_0150","cur_14"]
[1682,"a_马家梁一期Ⅱ-020 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅱ-020 偏航角度(扭缆角度）","yc_hs_0150","cur_16"]
[1683,"a_马家梁一期Ⅱ-020 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅱ-020 1#桨叶片角度(桨距角)","yc_hs_0150","cur_17"]
[1684,"a_马家梁一期Ⅱ-020 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅱ-020 2#桨叶片角度(桨距角)","yc_hs_0150","cur_18"]
[1685,"a_马家梁一期Ⅱ-020 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅱ-020 3#桨叶片角度(桨距角)","yc_hs_0150","cur_19"]
[1686,"a_马家梁一期Ⅱ-020 发电机测速模块测量转速","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅱ-020 发电机测速模块测量转速","yc_hs_0150","cur_20"]
[1687,"a_马家梁一期Ⅱ-020 发电机有功功率","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅱ-020 发电机有功功率","yc_hs_0150","cur_21"]
[1688,"a_马家梁一期Ⅱ-020 发电机绕组温度1","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅱ-020 发电机绕组温度1","yc_hs_0150","cur_33"]
[1689,"a_马家梁一期Ⅱ-020 发电机绕组温度2","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅱ-020 发电机绕组温度2","yc_hs_0150","cur_34"]
[1690,"a_马家梁一期Ⅱ-020 发电机绕组温度3","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅱ-020 发电机绕组温度3","yc_hs_0150","cur_35"]
[1691,"a_马家梁一期Ⅱ-020 机舱柜温度","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅱ-020 机舱柜温度","yc_hs_0150","cur_46"]
[1692,"a_马家梁一期Ⅱ-020 环境温度","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅱ-020 环境温度","yc_hs_0150","cur_79"]
[1693,"a_马家梁一期Ⅱ-020 发电机前轴承温度1","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅱ-020 发电机前轴承温度1","yc_hs_0150","cur_80"]
[1694,"a_马家梁一期Ⅱ-020 发电机后轴承温度1","马家梁风电场","WOF35200074",20,"MJLFD.T1_L2.WTG020.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅱ-020 发电机后轴承温度1","yc_hs_0150","cur_82"]
[1695,"a_马家梁一期Ⅱ-021 风速","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅱ-021 风速","yc_hs_0151","cur_02"]
[1696,"a_马家梁一期Ⅱ-021 机舱与风向夹角","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅱ-021 机舱与风向夹角","yc_hs_0151","cur_03"]
[1697,"a_马家梁一期Ⅱ-021 风向","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅱ-021 风向","yc_hs_0151","cur_04"]
[1698,"a_马家梁一期Ⅱ-021 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅱ-021 偏航角度(扭缆角度）","yc_hs_0151","cur_06"]
[1699,"a_马家梁一期Ⅱ-021 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅱ-021 1#桨叶片角度(桨距角)","yc_hs_0151","cur_07"]
[1700,"a_马家梁一期Ⅱ-021 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅱ-021 2#桨叶片角度(桨距角)","yc_hs_0151","cur_08"]
[1701,"a_马家梁一期Ⅱ-021 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅱ-021 3#桨叶片角度(桨距角)","yc_hs_0151","cur_09"]
[1702,"a_马家梁一期Ⅱ-021 发电机测速模块测量转速","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅱ-021 发电机测速模块测量转速","yc_hs_0151","cur_10"]
[1703,"a_马家梁一期Ⅱ-021 发电机有功功率","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅱ-021 发电机有功功率","yc_hs_0151","cur_11"]
[1704,"a_马家梁一期Ⅱ-021 发电机绕组温度1","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅱ-021 发电机绕组温度1","yc_hs_0151","cur_23"]
[1705,"a_马家梁一期Ⅱ-021 发电机绕组温度2","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅱ-021 发电机绕组温度2","yc_hs_0151","cur_24"]
[1706,"a_马家梁一期Ⅱ-021 发电机绕组温度3","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅱ-021 发电机绕组温度3","yc_hs_0151","cur_25"]
[1707,"a_马家梁一期Ⅱ-021 机舱柜温度","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅱ-021 机舱柜温度","yc_hs_0151","cur_36"]
[1708,"a_马家梁一期Ⅱ-021 环境温度","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅱ-021 环境温度","yc_hs_0151","cur_69"]
[1709,"a_马家梁一期Ⅱ-021 发电机前轴承温度1","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅱ-021 发电机前轴承温度1","yc_hs_0151","cur_70"]
[1710,"a_马家梁一期Ⅱ-021 发电机后轴承温度1","马家梁风电场","WOF35200074",21,"MJLFD.T1_L2.WTG021.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅱ-021 发电机后轴承温度1","yc_hs_0151","cur_72"]
[1711,"a_马家梁一期Ⅱ-022 风速","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅱ-022 风速","yc_hs_0151","cur_92"]
[1712,"a_马家梁一期Ⅱ-022 机舱与风向夹角","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅱ-022 机舱与风向夹角","yc_hs_0151","cur_93"]
[1713,"a_马家梁一期Ⅱ-022 风向","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅱ-022 风向","yc_hs_0151","cur_94"]
[1714,"a_马家梁一期Ⅱ-022 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅱ-022 偏航角度(扭缆角度）","yc_hs_0151","cur_96"]
[1715,"a_马家梁一期Ⅱ-022 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅱ-022 1#桨叶片角度(桨距角)","yc_hs_0151","cur_97"]
[1716,"a_马家梁一期Ⅱ-022 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅱ-022 2#桨叶片角度(桨距角)","yc_hs_0151","cur_98"]
[1717,"a_马家梁一期Ⅱ-022 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅱ-022 3#桨叶片角度(桨距角)","yc_hs_0151","cur_99"]
[1718,"a_马家梁一期Ⅱ-022 发电机测速模块测量转速","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅱ-022 发电机测速模块测量转速","yc_hs_0151","cur_100"]
[1719,"a_马家梁一期Ⅱ-022 发电机有功功率","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅱ-022 发电机有功功率","yc_hs_0152","cur_01"]
[1720,"a_马家梁一期Ⅱ-022 发电机绕组温度1","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅱ-022 发电机绕组温度1","yc_hs_0152","cur_13"]
[1721,"a_马家梁一期Ⅱ-022 发电机绕组温度2","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅱ-022 发电机绕组温度2","yc_hs_0152","cur_14"]
[1722,"a_马家梁一期Ⅱ-022 发电机绕组温度3","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅱ-022 发电机绕组温度3","yc_hs_0152","cur_15"]
[1723,"a_马家梁一期Ⅱ-022 机舱柜温度","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅱ-022 机舱柜温度","yc_hs_0152","cur_26"]
[1724,"a_马家梁一期Ⅱ-022 环境温度","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅱ-022 环境温度","yc_hs_0152","cur_59"]
[1725,"a_马家梁一期Ⅱ-022 发电机前轴承温度1","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅱ-022 发电机前轴承温度1","yc_hs_0152","cur_60"]
[1726,"a_马家梁一期Ⅱ-022 发电机后轴承温度1","马家梁风电场","WOF35200074",22,"MJLFD.T1_L2.WTG022.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅱ-022 发电机后轴承温度1","yc_hs_0152","cur_62"]
[1727,"a_马家梁一期Ⅱ-023 风速","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅱ-023 风速","yc_hs_0152","cur_82"]
[1728,"a_马家梁一期Ⅱ-023 机舱与风向夹角","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅱ-023 机舱与风向夹角","yc_hs_0152","cur_83"]
[1729,"a_马家梁一期Ⅱ-023 风向","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅱ-023 风向","yc_hs_0152","cur_84"]
[1730,"a_马家梁一期Ⅱ-023 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅱ-023 偏航角度(扭缆角度）","yc_hs_0152","cur_86"]
[1731,"a_马家梁一期Ⅱ-023 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅱ-023 1#桨叶片角度(桨距角)","yc_hs_0152","cur_87"]
[1732,"a_马家梁一期Ⅱ-023 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅱ-023 2#桨叶片角度(桨距角)","yc_hs_0152","cur_88"]
[1733,"a_马家梁一期Ⅱ-023 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅱ-023 3#桨叶片角度(桨距角)","yc_hs_0152","cur_89"]
[1734,"a_马家梁一期Ⅱ-023 发电机测速模块测量转速","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅱ-023 发电机测速模块测量转速","yc_hs_0152","cur_90"]
[1735,"a_马家梁一期Ⅱ-023 发电机有功功率","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅱ-023 发电机有功功率","yc_hs_0152","cur_91"]
[1736,"a_马家梁一期Ⅱ-023 发电机绕组温度1","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅱ-023 发电机绕组温度1","yc_hs_0153","cur_03"]
[1737,"a_马家梁一期Ⅱ-023 发电机绕组温度2","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅱ-023 发电机绕组温度2","yc_hs_0153","cur_04"]
[1738,"a_马家梁一期Ⅱ-023 发电机绕组温度3","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅱ-023 发电机绕组温度3","yc_hs_0153","cur_05"]
[1739,"a_马家梁一期Ⅱ-023 机舱柜温度","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅱ-023 机舱柜温度","yc_hs_0153","cur_16"]
[1740,"a_马家梁一期Ⅱ-023 环境温度","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅱ-023 环境温度","yc_hs_0153","cur_49"]
[1741,"a_马家梁一期Ⅱ-023 发电机前轴承温度1","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅱ-023 发电机前轴承温度1","yc_hs_0153","cur_50"]
[1742,"a_马家梁一期Ⅱ-023 发电机后轴承温度1","马家梁风电场","WOF35200074",23,"MJLFD.T1_L2.WTG023.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅱ-023 发电机后轴承温度1","yc_hs_0153","cur_52"]
[1743,"a_马家梁一期Ⅱ-024 风速","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅱ-024 风速","yc_hs_0153","cur_72"]
[1744,"a_马家梁一期Ⅱ-024 机舱与风向夹角","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅱ-024 机舱与风向夹角","yc_hs_0153","cur_73"]
[1745,"a_马家梁一期Ⅱ-024 风向","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅱ-024 风向","yc_hs_0153","cur_74"]
[1746,"a_马家梁一期Ⅱ-024 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅱ-024 偏航角度(扭缆角度）","yc_hs_0153","cur_76"]
[1747,"a_马家梁一期Ⅱ-024 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅱ-024 1#桨叶片角度(桨距角)","yc_hs_0153","cur_77"]
[1748,"a_马家梁一期Ⅱ-024 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅱ-024 2#桨叶片角度(桨距角)","yc_hs_0153","cur_78"]
[1749,"a_马家梁一期Ⅱ-024 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅱ-024 3#桨叶片角度(桨距角)","yc_hs_0153","cur_79"]
[1750,"a_马家梁一期Ⅱ-024 发电机测速模块测量转速","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅱ-024 发电机测速模块测量转速","yc_hs_0153","cur_80"]
[1751,"a_马家梁一期Ⅱ-024 发电机有功功率","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅱ-024 发电机有功功率","yc_hs_0153","cur_81"]
[1752,"a_马家梁一期Ⅱ-024 发电机绕组温度1","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅱ-024 发电机绕组温度1","yc_hs_0153","cur_93"]
[1753,"a_马家梁一期Ⅱ-024 发电机绕组温度2","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅱ-024 发电机绕组温度2","yc_hs_0153","cur_94"]
[1754,"a_马家梁一期Ⅱ-024 发电机绕组温度3","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅱ-024 发电机绕组温度3","yc_hs_0153","cur_95"]
[1755,"a_马家梁一期Ⅱ-024 机舱柜温度","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅱ-024 机舱柜温度","yc_hs_0154","cur_06"]
[1756,"a_马家梁一期Ⅱ-024 环境温度","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅱ-024 环境温度","yc_hs_0154","cur_39"]
[1757,"a_马家梁一期Ⅱ-024 发电机前轴承温度1","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅱ-024 发电机前轴承温度1","yc_hs_0154","cur_40"]
[1758,"a_马家梁一期Ⅱ-024 发电机后轴承温度1","马家梁风电场","WOF35200074",24,"MJLFD.T1_L2.WTG024.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅱ-024 发电机后轴承温度1","yc_hs_0154","cur_42"]
[1759,"a_马家梁一期Ⅱ-025 风速","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WNAC.WindSpeed","风速","wind_velocity","a_马家梁一期Ⅱ-025 风速","yc_hs_0154","cur_62"]
[1760,"a_马家梁一期Ⅱ-025 机舱与风向夹角","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁一期Ⅱ-025 机舱与风向夹角","yc_hs_0154","cur_63"]
[1761,"a_马家梁一期Ⅱ-025 风向","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WNAC.WindDirection","绝对风向","true_wind_direction","a_马家梁一期Ⅱ-025 风向","yc_hs_0154","cur_64"]
[1762,"a_马家梁一期Ⅱ-025 偏航角度(扭缆角度）","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","a_马家梁一期Ⅱ-025 偏航角度(扭缆角度）","yc_hs_0154","cur_66"]
[1763,"a_马家梁一期Ⅱ-025 1#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁一期Ⅱ-025 1#桨叶片角度(桨距角)","yc_hs_0154","cur_67"]
[1764,"a_马家梁一期Ⅱ-025 2#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁一期Ⅱ-025 2#桨叶片角度(桨距角)","yc_hs_0154","cur_68"]
[1765,"a_马家梁一期Ⅱ-025 3#桨叶片角度(桨距角)","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁一期Ⅱ-025 3#桨叶片角度(桨距角)","yc_hs_0154","cur_69"]
[1766,"a_马家梁一期Ⅱ-025 发电机测速模块测量转速","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WGEN.Spd.Ra","风轮转速","rotor_speed","a_马家梁一期Ⅱ-025 发电机测速模块测量转速","yc_hs_0154","cur_70"]
[1767,"a_马家梁一期Ⅱ-025 发电机有功功率","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WGEN.GenActivePW","有功功率","active_power","a_马家梁一期Ⅱ-025 发电机有功功率","yc_hs_0154","cur_71"]
[1768,"a_马家梁一期Ⅱ-025 发电机绕组温度1","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","a_马家梁一期Ⅱ-025 发电机绕组温度1","yc_hs_0154","cur_83"]
[1769,"a_马家梁一期Ⅱ-025 发电机绕组温度2","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","a_马家梁一期Ⅱ-025 发电机绕组温度2","yc_hs_0154","cur_84"]
[1770,"a_马家梁一期Ⅱ-025 发电机绕组温度3","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","a_马家梁一期Ⅱ-025 发电机绕组温度3","yc_hs_0154","cur_85"]
[1771,"a_马家梁一期Ⅱ-025 机舱柜温度","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁一期Ⅱ-025 机舱柜温度","yc_hs_0154","cur_96"]
[1772,"a_马家梁一期Ⅱ-025 环境温度","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WTUR.Temp.TowerBase","环境温度","outside_cabin_temperature","a_马家梁一期Ⅱ-025 环境温度","yc_hs_0155","cur_29"]
[1773,"a_马家梁一期Ⅱ-025 发电机前轴承温度1","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WGEN.Temp.FrontAxis1","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁一期Ⅱ-025 发电机前轴承温度1","yc_hs_0155","cur_30"]
[1774,"a_马家梁一期Ⅱ-025 发电机后轴承温度1","马家梁风电场","WOF35200074",25,"MJLFD.T1_L2.WTG025.WGEN.Temp.BackAxis1","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁一期Ⅱ-025 发电机后轴承温度1","yc_hs_0155","cur_32"]
[1775,"富风风场_A1-1 机组有功功率","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-1 机组有功功率","yc_hs_0167","cur_07"]
[1776,"富风风场_A1-1 机组风轮转速","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-1 机组风轮转速","yc_hs_0167","cur_10"]
[1777,"富风风场_A1-1 机组1#叶片变桨角度","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-1 机组1#叶片变桨角度","yc_hs_0167","cur_12"]
[1778,"富风风场_A1-1 机组2#叶片变桨角度","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-1 机组2#叶片变桨角度","yc_hs_0167","cur_13"]
[1779,"富风风场_A1-1 机组3#叶片变桨角度","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-1 机组3#叶片变桨角度","yc_hs_0167","cur_14"]
[1780,"富风风场_A1-1 机组主轴前轴承温度","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-1 机组主轴前轴承温度","yc_hs_0167","cur_38"]
[1781,"富风风场_A1-1 机组齿轮箱油池温度","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-1 机组齿轮箱油池温度","yc_hs_0167","cur_40"]
[1782,"富风风场_A1-1 机组发电机转速","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-1 机组发电机转速","yc_hs_0167","cur_43"]
[1783,"富风风场_A1-1 机组发电机绕组u1温度","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-1 机组发电机绕组u1温度","yc_hs_0167","cur_46"]
[1784,"富风风场_A1-1 机组发电机绕组v1温度","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-1 机组发电机绕组v1温度","yc_hs_0167","cur_48"]
[1785,"富风风场_A1-1 机组发电机绕组w1温度","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-1 机组发电机绕组w1温度","yc_hs_0167","cur_50"]
[1786,"富风风场_A1-1 机组发电机前轴承温度","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-1 机组发电机前轴承温度","yc_hs_0167","cur_52"]
[1787,"富风风场_A1-1 机组发电机后轴承温度","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-1 机组发电机后轴承温度","yc_hs_0167","cur_53"]
[1788,"富风风场_A1-1 机组瞬时风速","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-1 机组瞬时风速","yc_hs_0167","cur_66"]
[1789,"富风风场_A1-1 机组瞬时风向","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-1 机组瞬时风向","yc_hs_0167","cur_70"]
[1790,"富风风场_A1-1 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WROT.YC5","对风角度","yaw_error1","富风风场_A1-1 机组1#风向仪瞬时风向","yc_hs_0167","cur_71"]
[1791,"富风风场_A1-1 机组环境温度","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-1 机组环境温度","yc_hs_0167","cur_74"]
[1792,"富风风场_A1-1 机组机舱温度","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-1 机组机舱温度","yc_hs_0167","cur_75"]
[1793,"富风风场_A1-1 机组机舱X方向振动","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-1 机组机舱X方向振动","yc_hs_0167","cur_77"]
[1794,"富风风场_A1-1 机组机舱Y方向振动","太谷风电场","WOF35400075",1,"FFFD.T1_L1.WTG001.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-1 机组机舱Y方向振动","yc_hs_0167","cur_78"]
[1795,"富风风场_A1-2 机组有功功率","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-2 机组有功功率","yc_hs_0168","cur_44"]
[1796,"富风风场_A1-2 机组风轮转速","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-2 机组风轮转速","yc_hs_0168","cur_47"]
[1797,"富风风场_A1-2 机组1#叶片变桨角度","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-2 机组1#叶片变桨角度","yc_hs_0168","cur_49"]
[1798,"富风风场_A1-2 机组2#叶片变桨角度","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-2 机组2#叶片变桨角度","yc_hs_0168","cur_50"]
[1799,"富风风场_A1-2 机组3#叶片变桨角度","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-2 机组3#叶片变桨角度","yc_hs_0168","cur_51"]
[1800,"富风风场_A1-2 机组主轴前轴承温度","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-2 机组主轴前轴承温度","yc_hs_0168","cur_75"]
[1801,"富风风场_A1-2 机组齿轮箱油池温度","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-2 机组齿轮箱油池温度","yc_hs_0168","cur_77"]
[1802,"富风风场_A1-2 机组发电机转速","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-2 机组发电机转速","yc_hs_0168","cur_80"]
[1803,"富风风场_A1-2 机组发电机绕组u1温度","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-2 机组发电机绕组u1温度","yc_hs_0168","cur_83"]
[1804,"富风风场_A1-2 机组发电机绕组v1温度","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-2 机组发电机绕组v1温度","yc_hs_0168","cur_85"]
[1805,"富风风场_A1-2 机组发电机绕组w1温度","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-2 机组发电机绕组w1温度","yc_hs_0168","cur_87"]
[1806,"富风风场_A1-2 机组发电机前轴承温度","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-2 机组发电机前轴承温度","yc_hs_0168","cur_89"]
[1807,"富风风场_A1-2 机组发电机后轴承温度","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-2 机组发电机后轴承温度","yc_hs_0168","cur_90"]
[1808,"富风风场_A1-2 机组瞬时风速","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-2 机组瞬时风速","yc_hs_0169","cur_03"]
[1809,"富风风场_A1-2 机组瞬时风向","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-2 机组瞬时风向","yc_hs_0169","cur_07"]
[1810,"富风风场_A1-2 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WROT.YC5","对风角度","yaw_error1","富风风场_A1-2 机组1#风向仪瞬时风向","yc_hs_0169","cur_08"]
[1811,"富风风场_A1-2 机组环境温度","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-2 机组环境温度","yc_hs_0169","cur_11"]
[1812,"富风风场_A1-2 机组机舱温度","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-2 机组机舱温度","yc_hs_0169","cur_12"]
[1813,"富风风场_A1-2 机组机舱X方向振动","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-2 机组机舱X方向振动","yc_hs_0169","cur_14"]
[1814,"富风风场_A1-2 机组机舱Y方向振动","太谷风电场","WOF35400075",2,"FFFD.T1_L1.WTG002.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-2 机组机舱Y方向振动","yc_hs_0169","cur_15"]
[1815,"富风风场_A1-3 机组有功功率","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-3 机组有功功率","yc_hs_0169","cur_81"]
[1816,"富风风场_A1-3 机组风轮转速","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-3 机组风轮转速","yc_hs_0169","cur_84"]
[1817,"富风风场_A1-3 机组1#叶片变桨角度","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-3 机组1#叶片变桨角度","yc_hs_0169","cur_86"]
[1818,"富风风场_A1-3 机组2#叶片变桨角度","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-3 机组2#叶片变桨角度","yc_hs_0169","cur_87"]
[1819,"富风风场_A1-3 机组3#叶片变桨角度","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-3 机组3#叶片变桨角度","yc_hs_0169","cur_88"]
[1820,"富风风场_A1-3 机组主轴前轴承温度","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-3 机组主轴前轴承温度","yc_hs_0170","cur_12"]
[1821,"富风风场_A1-3 机组齿轮箱油池温度","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-3 机组齿轮箱油池温度","yc_hs_0170","cur_14"]
[1822,"富风风场_A1-3 机组发电机转速","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-3 机组发电机转速","yc_hs_0170","cur_17"]
[1823,"富风风场_A1-3 机组发电机绕组u1温度","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-3 机组发电机绕组u1温度","yc_hs_0170","cur_20"]
[1824,"富风风场_A1-3 机组发电机绕组v1温度","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-3 机组发电机绕组v1温度","yc_hs_0170","cur_22"]
[1825,"富风风场_A1-3 机组发电机绕组w1温度","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-3 机组发电机绕组w1温度","yc_hs_0170","cur_24"]
[1826,"富风风场_A1-3 机组发电机前轴承温度","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-3 机组发电机前轴承温度","yc_hs_0170","cur_26"]
[1827,"富风风场_A1-3 机组发电机后轴承温度","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-3 机组发电机后轴承温度","yc_hs_0170","cur_27"]
[1828,"富风风场_A1-3 机组瞬时风速","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-3 机组瞬时风速","yc_hs_0170","cur_40"]
[1829,"富风风场_A1-3 机组瞬时风向","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-3 机组瞬时风向","yc_hs_0170","cur_44"]
[1830,"富风风场_A1-3 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WROT.YC5","对风角度","yaw_error1","富风风场_A1-3 机组1#风向仪瞬时风向","yc_hs_0170","cur_45"]
[1831,"富风风场_A1-3 机组环境温度","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-3 机组环境温度","yc_hs_0170","cur_48"]
[1832,"富风风场_A1-3 机组机舱温度","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-3 机组机舱温度","yc_hs_0170","cur_49"]
[1833,"富风风场_A1-3 机组机舱X方向振动","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-3 机组机舱X方向振动","yc_hs_0170","cur_51"]
[1834,"富风风场_A1-3 机组机舱Y方向振动","太谷风电场","WOF35400075",3,"FFFD.T1_L1.WTG003.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-3 机组机舱Y方向振动","yc_hs_0170","cur_52"]
[1835,"富风风场_A1-4 机组有功功率","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-4 机组有功功率","yc_hs_0171","cur_18"]
[1836,"富风风场_A1-4 机组风轮转速","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-4 机组风轮转速","yc_hs_0171","cur_21"]
[1837,"富风风场_A1-4 机组1#叶片变桨角度","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-4 机组1#叶片变桨角度","yc_hs_0171","cur_23"]
[1838,"富风风场_A1-4 机组2#叶片变桨角度","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-4 机组2#叶片变桨角度","yc_hs_0171","cur_24"]
[1839,"富风风场_A1-4 机组3#叶片变桨角度","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-4 机组3#叶片变桨角度","yc_hs_0171","cur_25"]
[1840,"富风风场_A1-4 机组主轴前轴承温度","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-4 机组主轴前轴承温度","yc_hs_0171","cur_49"]
[1841,"富风风场_A1-4 机组齿轮箱油池温度","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-4 机组齿轮箱油池温度","yc_hs_0171","cur_51"]
[1842,"富风风场_A1-4 机组发电机转速","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-4 机组发电机转速","yc_hs_0171","cur_54"]
[1843,"富风风场_A1-4 机组发电机绕组u1温度","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-4 机组发电机绕组u1温度","yc_hs_0171","cur_57"]
[1844,"富风风场_A1-4 机组发电机绕组v1温度","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-4 机组发电机绕组v1温度","yc_hs_0171","cur_59"]
[1845,"富风风场_A1-4 机组发电机绕组w1温度","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-4 机组发电机绕组w1温度","yc_hs_0171","cur_61"]
[1846,"富风风场_A1-4 机组发电机前轴承温度","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-4 机组发电机前轴承温度","yc_hs_0171","cur_63"]
[1847,"富风风场_A1-4 机组发电机后轴承温度","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-4 机组发电机后轴承温度","yc_hs_0171","cur_64"]
[1848,"富风风场_A1-4 机组瞬时风速","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-4 机组瞬时风速","yc_hs_0171","cur_77"]
[1849,"富风风场_A1-4 机组瞬时风向","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-4 机组瞬时风向","yc_hs_0171","cur_81"]
[1850,"富风风场_A1-4 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WROT.YC5","对风角度","yaw_error1","富风风场_A1-4 机组1#风向仪瞬时风向","yc_hs_0171","cur_82"]
[1851,"富风风场_A1-4 机组环境温度","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-4 机组环境温度","yc_hs_0171","cur_85"]
[1852,"富风风场_A1-4 机组机舱温度","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-4 机组机舱温度","yc_hs_0171","cur_86"]
[1853,"富风风场_A1-4 机组机舱X方向振动","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-4 机组机舱X方向振动","yc_hs_0171","cur_88"]
[1854,"富风风场_A1-4 机组机舱Y方向振动","太谷风电场","WOF35400075",4,"FFFD.T1_L1.WTG004.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-4 机组机舱Y方向振动","yc_hs_0171","cur_89"]
[1855,"富风风场_A1-5 机组有功功率","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-5 机组有功功率","yc_hs_0172","cur_55"]
[1856,"富风风场_A1-5 机组风轮转速","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-5 机组风轮转速","yc_hs_0172","cur_58"]
[1857,"富风风场_A1-5 机组1#叶片变桨角度","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-5 机组1#叶片变桨角度","yc_hs_0172","cur_60"]
[1858,"富风风场_A1-5 机组2#叶片变桨角度","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-5 机组2#叶片变桨角度","yc_hs_0172","cur_61"]
[1859,"富风风场_A1-5 机组3#叶片变桨角度","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-5 机组3#叶片变桨角度","yc_hs_0172","cur_62"]
[1860,"富风风场_A1-5 机组主轴前轴承温度","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-5 机组主轴前轴承温度","yc_hs_0172","cur_86"]
[1861,"富风风场_A1-5 机组齿轮箱油池温度","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-5 机组齿轮箱油池温度","yc_hs_0172","cur_88"]
[1862,"富风风场_A1-5 机组发电机转速","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-5 机组发电机转速","yc_hs_0172","cur_91"]
[1863,"富风风场_A1-5 机组发电机绕组u1温度","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-5 机组发电机绕组u1温度","yc_hs_0172","cur_94"]
[1864,"富风风场_A1-5 机组发电机绕组v1温度","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-5 机组发电机绕组v1温度","yc_hs_0172","cur_96"]
[1865,"富风风场_A1-5 机组发电机绕组w1温度","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-5 机组发电机绕组w1温度","yc_hs_0172","cur_98"]
[1866,"富风风场_A1-5 机组发电机前轴承温度","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-5 机组发电机前轴承温度","yc_hs_0172","cur_100"]
[1867,"富风风场_A1-5 机组发电机后轴承温度","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-5 机组发电机后轴承温度","yc_hs_0173","cur_01"]
[1868,"富风风场_A1-5 机组瞬时风速","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-5 机组瞬时风速","yc_hs_0173","cur_14"]
[1869,"富风风场_A1-5 机组瞬时风向","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-5 机组瞬时风向","yc_hs_0173","cur_18"]
[1870,"富风风场_A1-5 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WROT.YC5","对风角度","yaw_error1","富风风场_A1-5 机组1#风向仪瞬时风向","yc_hs_0173","cur_19"]
[1871,"富风风场_A1-5 机组环境温度","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-5 机组环境温度","yc_hs_0173","cur_22"]
[1872,"富风风场_A1-5 机组机舱温度","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-5 机组机舱温度","yc_hs_0173","cur_23"]
[1873,"富风风场_A1-5 机组机舱X方向振动","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-5 机组机舱X方向振动","yc_hs_0173","cur_25"]
[1874,"富风风场_A1-5 机组机舱Y方向振动","太谷风电场","WOF35400075",5,"FFFD.T1_L1.WTG005.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-5 机组机舱Y方向振动","yc_hs_0173","cur_26"]
[1875,"富风风场_A1-6 机组有功功率","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-6 机组有功功率","yc_hs_0173","cur_92"]
[1876,"富风风场_A1-6 机组风轮转速","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-6 机组风轮转速","yc_hs_0173","cur_95"]
[1877,"富风风场_A1-6 机组1#叶片变桨角度","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-6 机组1#叶片变桨角度","yc_hs_0173","cur_97"]
[1878,"富风风场_A1-6 机组2#叶片变桨角度","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-6 机组2#叶片变桨角度","yc_hs_0173","cur_98"]
[1879,"富风风场_A1-6 机组3#叶片变桨角度","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-6 机组3#叶片变桨角度","yc_hs_0173","cur_99"]
[1880,"富风风场_A1-6 机组主轴前轴承温度","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-6 机组主轴前轴承温度","yc_hs_0174","cur_23"]
[1881,"富风风场_A1-6 机组齿轮箱油池温度","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-6 机组齿轮箱油池温度","yc_hs_0174","cur_25"]
[1882,"富风风场_A1-6 机组发电机转速","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-6 机组发电机转速","yc_hs_0174","cur_28"]
[1883,"富风风场_A1-6 机组发电机绕组u1温度","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-6 机组发电机绕组u1温度","yc_hs_0174","cur_31"]
[1884,"富风风场_A1-6 机组发电机绕组v1温度","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-6 机组发电机绕组v1温度","yc_hs_0174","cur_33"]
[1885,"富风风场_A1-6 机组发电机绕组w1温度","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-6 机组发电机绕组w1温度","yc_hs_0174","cur_35"]
[1886,"富风风场_A1-6 机组发电机前轴承温度","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-6 机组发电机前轴承温度","yc_hs_0174","cur_37"]
[1887,"富风风场_A1-6 机组发电机后轴承温度","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-6 机组发电机后轴承温度","yc_hs_0174","cur_38"]
[1888,"富风风场_A1-6 机组瞬时风速","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-6 机组瞬时风速","yc_hs_0174","cur_51"]
[1889,"富风风场_A1-6 机组瞬时风向","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-6 机组瞬时风向","yc_hs_0174","cur_55"]
[1890,"富风风场_A1-6 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WROT.YC5","对风角度","yaw_error1","富风风场_A1-6 机组1#风向仪瞬时风向","yc_hs_0174","cur_56"]
[1891,"富风风场_A1-6 机组环境温度","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-6 机组环境温度","yc_hs_0174","cur_59"]
[1892,"富风风场_A1-6 机组机舱温度","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-6 机组机舱温度","yc_hs_0174","cur_60"]
[1893,"富风风场_A1-6 机组机舱X方向振动","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-6 机组机舱X方向振动","yc_hs_0174","cur_62"]
[1894,"富风风场_A1-6 机组机舱Y方向振动","太谷风电场","WOF35400075",6,"FFFD.T1_L1.WTG006.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-6 机组机舱Y方向振动","yc_hs_0174","cur_63"]
[1895,"富风风场_A1-7 机组有功功率","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-7 机组有功功率","yc_hs_0176","cur_29"]
[1896,"富风风场_A1-7 机组风轮转速","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-7 机组风轮转速","yc_hs_0176","cur_32"]
[1897,"富风风场_A1-7 机组1#叶片变桨角度","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-7 机组1#叶片变桨角度","yc_hs_0176","cur_34"]
[1898,"富风风场_A1-7 机组2#叶片变桨角度","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-7 机组2#叶片变桨角度","yc_hs_0176","cur_35"]
[1899,"富风风场_A1-7 机组3#叶片变桨角度","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-7 机组3#叶片变桨角度","yc_hs_0176","cur_36"]
[1900,"富风风场_A1-7 机组主轴前轴承温度","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-7 机组主轴前轴承温度","yc_hs_0176","cur_60"]
[1901,"富风风场_A1-7 机组齿轮箱油池温度","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-7 机组齿轮箱油池温度","yc_hs_0176","cur_62"]
[1902,"富风风场_A1-7 机组发电机转速","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-7 机组发电机转速","yc_hs_0176","cur_65"]
[1903,"富风风场_A1-7 机组发电机绕组u1温度","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-7 机组发电机绕组u1温度","yc_hs_0176","cur_68"]
[1904,"富风风场_A1-7 机组发电机绕组v1温度","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-7 机组发电机绕组v1温度","yc_hs_0176","cur_70"]
[1905,"富风风场_A1-7 机组发电机绕组w1温度","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-7 机组发电机绕组w1温度","yc_hs_0176","cur_72"]
[1906,"富风风场_A1-7 机组发电机前轴承温度","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-7 机组发电机前轴承温度","yc_hs_0176","cur_74"]
[1907,"富风风场_A1-7 机组发电机后轴承温度","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-7 机组发电机后轴承温度","yc_hs_0176","cur_75"]
[1908,"富风风场_A1-7 机组瞬时风速","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-7 机组瞬时风速","yc_hs_0176","cur_88"]
[1909,"富风风场_A1-7 机组瞬时风向","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-7 机组瞬时风向","yc_hs_0176","cur_92"]
[1910,"富风风场_A1-7 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WROT.YC5","对风角度","yaw_error1","富风风场_A1-7 机组1#风向仪瞬时风向","yc_hs_0176","cur_93"]
[1911,"富风风场_A1-7 机组环境温度","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-7 机组环境温度","yc_hs_0176","cur_96"]
[1912,"富风风场_A1-7 机组机舱温度","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-7 机组机舱温度","yc_hs_0176","cur_97"]
[1913,"富风风场_A1-7 机组机舱X方向振动","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-7 机组机舱X方向振动","yc_hs_0176","cur_99"]
[1914,"富风风场_A1-7 机组机舱Y方向振动","太谷风电场","WOF35400075",7,"FFFD.T1_L1.WTG007.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-7 机组机舱Y方向振动","yc_hs_0176","cur_100"]
[1915,"富风风场_A1-8 机组有功功率","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-8 机组有功功率","yc_hs_0177","cur_66"]
[1916,"富风风场_A1-8 机组风轮转速","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-8 机组风轮转速","yc_hs_0177","cur_69"]
[1917,"富风风场_A1-8 机组1#叶片变桨角度","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-8 机组1#叶片变桨角度","yc_hs_0177","cur_71"]
[1918,"富风风场_A1-8 机组2#叶片变桨角度","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-8 机组2#叶片变桨角度","yc_hs_0177","cur_72"]
[1919,"富风风场_A1-8 机组3#叶片变桨角度","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-8 机组3#叶片变桨角度","yc_hs_0177","cur_73"]
[1920,"富风风场_A1-8 机组主轴前轴承温度","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-8 机组主轴前轴承温度","yc_hs_0177","cur_97"]
[1921,"富风风场_A1-8 机组齿轮箱油池温度","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-8 机组齿轮箱油池温度","yc_hs_0177","cur_99"]
[1922,"富风风场_A1-8 机组发电机转速","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-8 机组发电机转速","yc_hs_0178","cur_02"]
[1923,"富风风场_A1-8 机组发电机绕组u1温度","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-8 机组发电机绕组u1温度","yc_hs_0178","cur_05"]
[1924,"富风风场_A1-8 机组发电机绕组v1温度","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-8 机组发电机绕组v1温度","yc_hs_0178","cur_07"]
[1925,"富风风场_A1-8 机组发电机绕组w1温度","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-8 机组发电机绕组w1温度","yc_hs_0178","cur_09"]
[1926,"富风风场_A1-8 机组发电机前轴承温度","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-8 机组发电机前轴承温度","yc_hs_0178","cur_11"]
[1927,"富风风场_A1-8 机组发电机后轴承温度","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-8 机组发电机后轴承温度","yc_hs_0178","cur_12"]
[1928,"富风风场_A1-8 机组瞬时风速","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-8 机组瞬时风速","yc_hs_0178","cur_25"]
[1929,"富风风场_A1-8 机组瞬时风向","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-8 机组瞬时风向","yc_hs_0178","cur_29"]
[1930,"富风风场_A1-8 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WROT.YC5","对风角度","yaw_error1","富风风场_A1-8 机组1#风向仪瞬时风向","yc_hs_0178","cur_30"]
[1931,"富风风场_A1-8 机组环境温度","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-8 机组环境温度","yc_hs_0178","cur_33"]
[1932,"富风风场_A1-8 机组机舱温度","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-8 机组机舱温度","yc_hs_0178","cur_34"]
[1933,"富风风场_A1-8 机组机舱X方向振动","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-8 机组机舱X方向振动","yc_hs_0178","cur_36"]
[1934,"富风风场_A1-8 机组机舱Y方向振动","太谷风电场","WOF35400075",8,"FFFD.T1_L1.WTG008.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-8 机组机舱Y方向振动","yc_hs_0178","cur_37"]
[1935,"富风风场_A1-9 机组有功功率","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-9 机组有功功率","yc_hs_0179","cur_03"]
[1936,"富风风场_A1-9 机组风轮转速","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-9 机组风轮转速","yc_hs_0179","cur_06"]
[1937,"富风风场_A1-9 机组1#叶片变桨角度","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-9 机组1#叶片变桨角度","yc_hs_0179","cur_08"]
[1938,"富风风场_A1-9 机组2#叶片变桨角度","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-9 机组2#叶片变桨角度","yc_hs_0179","cur_09"]
[1939,"富风风场_A1-9 机组3#叶片变桨角度","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-9 机组3#叶片变桨角度","yc_hs_0179","cur_10"]
[1940,"富风风场_A1-9 机组主轴前轴承温度","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-9 机组主轴前轴承温度","yc_hs_0179","cur_34"]
[1941,"富风风场_A1-9 机组齿轮箱油池温度","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-9 机组齿轮箱油池温度","yc_hs_0179","cur_36"]
[1942,"富风风场_A1-9 机组发电机转速","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-9 机组发电机转速","yc_hs_0179","cur_39"]
[1943,"富风风场_A1-9 机组发电机绕组u1温度","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-9 机组发电机绕组u1温度","yc_hs_0179","cur_42"]
[1944,"富风风场_A1-9 机组发电机绕组v1温度","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-9 机组发电机绕组v1温度","yc_hs_0179","cur_44"]
[1945,"富风风场_A1-9 机组发电机绕组w1温度","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-9 机组发电机绕组w1温度","yc_hs_0179","cur_46"]
[1946,"富风风场_A1-9 机组发电机前轴承温度","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-9 机组发电机前轴承温度","yc_hs_0179","cur_48"]
[1947,"富风风场_A1-9 机组发电机后轴承温度","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-9 机组发电机后轴承温度","yc_hs_0179","cur_49"]
[1948,"富风风场_A1-9 机组瞬时风速","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-9 机组瞬时风速","yc_hs_0179","cur_62"]
[1949,"富风风场_A1-9 机组瞬时风向","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-9 机组瞬时风向","yc_hs_0179","cur_66"]
[1950,"富风风场_A1-9 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WROT.YC5","对风角度","yaw_error1","富风风场_A1-9 机组1#风向仪瞬时风向","yc_hs_0179","cur_67"]
[1951,"富风风场_A1-9 机组环境温度","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-9 机组环境温度","yc_hs_0179","cur_70"]
[1952,"富风风场_A1-9 机组机舱温度","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-9 机组机舱温度","yc_hs_0179","cur_71"]
[1953,"富风风场_A1-9 机组机舱X方向振动","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-9 机组机舱X方向振动","yc_hs_0179","cur_73"]
[1954,"富风风场_A1-9 机组机舱Y方向振动","太谷风电场","WOF35400075",9,"FFFD.T1_L1.WTG009.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-9 机组机舱Y方向振动","yc_hs_0179","cur_74"]
[1955,"富风风场_A1-10 机组有功功率","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-10 机组有功功率","yc_hs_0180","cur_40"]
[1956,"富风风场_A1-10 机组风轮转速","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-10 机组风轮转速","yc_hs_0180","cur_43"]
[1957,"富风风场_A1-10 机组1#叶片变桨角度","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-10 机组1#叶片变桨角度","yc_hs_0180","cur_45"]
[1958,"富风风场_A1-10 机组2#叶片变桨角度","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-10 机组2#叶片变桨角度","yc_hs_0180","cur_46"]
[1959,"富风风场_A1-10 机组3#叶片变桨角度","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-10 机组3#叶片变桨角度","yc_hs_0180","cur_47"]
[1960,"富风风场_A1-10 机组主轴前轴承温度","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-10 机组主轴前轴承温度","yc_hs_0180","cur_71"]
[1961,"富风风场_A1-10 机组齿轮箱油池温度","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-10 机组齿轮箱油池温度","yc_hs_0180","cur_73"]
[1962,"富风风场_A1-10 机组发电机转速","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-10 机组发电机转速","yc_hs_0180","cur_76"]
[1963,"富风风场_A1-10 机组发电机绕组u1温度","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-10 机组发电机绕组u1温度","yc_hs_0180","cur_79"]
[1964,"富风风场_A1-10 机组发电机绕组v1温度","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-10 机组发电机绕组v1温度","yc_hs_0180","cur_81"]
[1965,"富风风场_A1-10 机组发电机绕组w1温度","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-10 机组发电机绕组w1温度","yc_hs_0180","cur_83"]
[1966,"富风风场_A1-10 机组发电机前轴承温度","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-10 机组发电机前轴承温度","yc_hs_0180","cur_85"]
[1967,"富风风场_A1-10 机组发电机后轴承温度","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-10 机组发电机后轴承温度","yc_hs_0180","cur_86"]
[1968,"富风风场_A1-10 机组瞬时风速","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-10 机组瞬时风速","yc_hs_0180","cur_99"]
[1969,"富风风场_A1-10 机组瞬时风向","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-10 机组瞬时风向","yc_hs_0181","cur_03"]
[1970,"富风风场_A1-10 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WROT.YC5","对风角度","yaw_error1","富风风场_A1-10 机组1#风向仪瞬时风向","yc_hs_0181","cur_04"]
[1971,"富风风场_A1-10 机组环境温度","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-10 机组环境温度","yc_hs_0181","cur_07"]
[1972,"富风风场_A1-10 机组机舱温度","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-10 机组机舱温度","yc_hs_0181","cur_08"]
[1973,"富风风场_A1-10 机组机舱X方向振动","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-10 机组机舱X方向振动","yc_hs_0181","cur_10"]
[1974,"富风风场_A1-10 机组机舱Y方向振动","太谷风电场","WOF35400075",10,"FFFD.T1_L1.WTG010.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-10 机组机舱Y方向振动","yc_hs_0181","cur_11"]
[1975,"富风风场_A1-11 机组有功功率","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-11 机组有功功率","yc_hs_0181","cur_77"]
[1976,"富风风场_A1-11 机组风轮转速","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-11 机组风轮转速","yc_hs_0181","cur_80"]
[1977,"富风风场_A1-11 机组1#叶片变桨角度","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-11 机组1#叶片变桨角度","yc_hs_0181","cur_82"]
[1978,"富风风场_A1-11 机组2#叶片变桨角度","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-11 机组2#叶片变桨角度","yc_hs_0181","cur_83"]
[1979,"富风风场_A1-11 机组3#叶片变桨角度","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-11 机组3#叶片变桨角度","yc_hs_0181","cur_84"]
[1980,"富风风场_A1-11 机组主轴前轴承温度","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-11 机组主轴前轴承温度","yc_hs_0182","cur_08"]
[1981,"富风风场_A1-11 机组齿轮箱油池温度","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-11 机组齿轮箱油池温度","yc_hs_0182","cur_10"]
[1982,"富风风场_A1-11 机组发电机转速","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-11 机组发电机转速","yc_hs_0182","cur_13"]
[1983,"富风风场_A1-11 机组发电机绕组u1温度","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-11 机组发电机绕组u1温度","yc_hs_0182","cur_16"]
[1984,"富风风场_A1-11 机组发电机绕组v1温度","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-11 机组发电机绕组v1温度","yc_hs_0182","cur_18"]
[1985,"富风风场_A1-11 机组发电机绕组w1温度","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-11 机组发电机绕组w1温度","yc_hs_0182","cur_20"]
[1986,"富风风场_A1-11 机组发电机前轴承温度","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-11 机组发电机前轴承温度","yc_hs_0182","cur_22"]
[1987,"富风风场_A1-11 机组发电机后轴承温度","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-11 机组发电机后轴承温度","yc_hs_0182","cur_23"]
[1988,"富风风场_A1-11 机组瞬时风速","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-11 机组瞬时风速","yc_hs_0182","cur_36"]
[1989,"富风风场_A1-11 机组瞬时风向","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-11 机组瞬时风向","yc_hs_0182","cur_40"]
[1990,"富风风场_A1-11 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WROT.YC5","对风角度","yaw_error1","富风风场_A1-11 机组1#风向仪瞬时风向","yc_hs_0182","cur_41"]
[1991,"富风风场_A1-11 机组环境温度","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-11 机组环境温度","yc_hs_0182","cur_44"]
[1992,"富风风场_A1-11 机组机舱温度","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-11 机组机舱温度","yc_hs_0182","cur_45"]
[1993,"富风风场_A1-11 机组机舱X方向振动","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-11 机组机舱X方向振动","yc_hs_0182","cur_47"]
[1994,"富风风场_A1-11 机组机舱Y方向振动","太谷风电场","WOF35400075",11,"FFFD.T1_L1.WTG011.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-11 机组机舱Y方向振动","yc_hs_0182","cur_48"]
[1995,"富风风场_A1-12 机组有功功率","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-12 机组有功功率","yc_hs_0183","cur_14"]
[1996,"富风风场_A1-12 机组风轮转速","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-12 机组风轮转速","yc_hs_0183","cur_17"]
[1997,"富风风场_A1-12 机组1#叶片变桨角度","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-12 机组1#叶片变桨角度","yc_hs_0183","cur_19"]
[1998,"富风风场_A1-12 机组2#叶片变桨角度","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-12 机组2#叶片变桨角度","yc_hs_0183","cur_20"]
[1999,"富风风场_A1-12 机组3#叶片变桨角度","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-12 机组3#叶片变桨角度","yc_hs_0183","cur_21"]
[2000,"富风风场_A1-12 机组主轴前轴承温度","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-12 机组主轴前轴承温度","yc_hs_0183","cur_45"]
[2001,"富风风场_A1-12 机组齿轮箱油池温度","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-12 机组齿轮箱油池温度","yc_hs_0183","cur_47"]
[2002,"富风风场_A1-12 机组发电机转速","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-12 机组发电机转速","yc_hs_0183","cur_50"]
[2003,"富风风场_A1-12 机组发电机绕组u1温度","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-12 机组发电机绕组u1温度","yc_hs_0183","cur_53"]
[2004,"富风风场_A1-12 机组发电机绕组v1温度","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-12 机组发电机绕组v1温度","yc_hs_0183","cur_55"]
[2005,"富风风场_A1-12 机组发电机绕组w1温度","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-12 机组发电机绕组w1温度","yc_hs_0183","cur_57"]
[2006,"富风风场_A1-12 机组发电机前轴承温度","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-12 机组发电机前轴承温度","yc_hs_0183","cur_59"]
[2007,"富风风场_A1-12 机组发电机后轴承温度","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-12 机组发电机后轴承温度","yc_hs_0183","cur_60"]
[2008,"富风风场_A1-12 机组瞬时风速","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-12 机组瞬时风速","yc_hs_0183","cur_73"]
[2009,"富风风场_A1-12 机组瞬时风向","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-12 机组瞬时风向","yc_hs_0183","cur_77"]
[2010,"富风风场_A1-12 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WROT.YC5","对风角度","yaw_error1","富风风场_A1-12 机组1#风向仪瞬时风向","yc_hs_0183","cur_78"]
[2011,"富风风场_A1-12 机组环境温度","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-12 机组环境温度","yc_hs_0183","cur_81"]
[2012,"富风风场_A1-12 机组机舱温度","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-12 机组机舱温度","yc_hs_0183","cur_82"]
[2013,"富风风场_A1-12 机组机舱X方向振动","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-12 机组机舱X方向振动","yc_hs_0183","cur_84"]
[2014,"富风风场_A1-12 机组机舱Y方向振动","太谷风电场","WOF35400075",12,"FFFD.T1_L1.WTG012.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-12 机组机舱Y方向振动","yc_hs_0183","cur_85"]
[2015,"富风风场_A1-13 机组有功功率","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-13 机组有功功率","yc_hs_0184","cur_51"]
[2016,"富风风场_A1-13 机组风轮转速","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-13 机组风轮转速","yc_hs_0184","cur_54"]
[2017,"富风风场_A1-13 机组1#叶片变桨角度","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-13 机组1#叶片变桨角度","yc_hs_0184","cur_56"]
[2018,"富风风场_A1-13 机组2#叶片变桨角度","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-13 机组2#叶片变桨角度","yc_hs_0184","cur_57"]
[2019,"富风风场_A1-13 机组3#叶片变桨角度","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-13 机组3#叶片变桨角度","yc_hs_0184","cur_58"]
[2020,"富风风场_A1-13 机组主轴前轴承温度","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-13 机组主轴前轴承温度","yc_hs_0184","cur_82"]
[2021,"富风风场_A1-13 机组齿轮箱油池温度","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-13 机组齿轮箱油池温度","yc_hs_0184","cur_84"]
[2022,"富风风场_A1-13 机组发电机转速","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-13 机组发电机转速","yc_hs_0184","cur_87"]
[2023,"富风风场_A1-13 机组发电机绕组u1温度","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-13 机组发电机绕组u1温度","yc_hs_0184","cur_90"]
[2024,"富风风场_A1-13 机组发电机绕组v1温度","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-13 机组发电机绕组v1温度","yc_hs_0184","cur_92"]
[2025,"富风风场_A1-13 机组发电机绕组w1温度","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-13 机组发电机绕组w1温度","yc_hs_0184","cur_94"]
[2026,"富风风场_A1-13 机组发电机前轴承温度","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-13 机组发电机前轴承温度","yc_hs_0184","cur_96"]
[2027,"富风风场_A1-13 机组发电机后轴承温度","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-13 机组发电机后轴承温度","yc_hs_0184","cur_97"]
[2028,"富风风场_A1-13 机组瞬时风速","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-13 机组瞬时风速","yc_hs_0185","cur_10"]
[2029,"富风风场_A1-13 机组瞬时风向","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-13 机组瞬时风向","yc_hs_0185","cur_14"]
[2030,"富风风场_A1-13 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WROT.YC5","对风角度","yaw_error1","富风风场_A1-13 机组1#风向仪瞬时风向","yc_hs_0185","cur_15"]
[2031,"富风风场_A1-13 机组环境温度","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-13 机组环境温度","yc_hs_0185","cur_18"]
[2032,"富风风场_A1-13 机组机舱温度","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-13 机组机舱温度","yc_hs_0185","cur_19"]
[2033,"富风风场_A1-13 机组机舱X方向振动","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-13 机组机舱X方向振动","yc_hs_0185","cur_21"]
[2034,"富风风场_A1-13 机组机舱Y方向振动","太谷风电场","WOF35400075",13,"FFFD.T1_L1.WTG013.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-13 机组机舱Y方向振动","yc_hs_0185","cur_22"]
[2035,"富风风场_A1-14 机组有功功率","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-14 机组有功功率","yc_hs_0185","cur_88"]
[2036,"富风风场_A1-14 机组风轮转速","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-14 机组风轮转速","yc_hs_0185","cur_91"]
[2037,"富风风场_A1-14 机组1#叶片变桨角度","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-14 机组1#叶片变桨角度","yc_hs_0185","cur_93"]
[2038,"富风风场_A1-14 机组2#叶片变桨角度","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-14 机组2#叶片变桨角度","yc_hs_0185","cur_94"]
[2039,"富风风场_A1-14 机组3#叶片变桨角度","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-14 机组3#叶片变桨角度","yc_hs_0185","cur_95"]
[2040,"富风风场_A1-14 机组主轴前轴承温度","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-14 机组主轴前轴承温度","yc_hs_0186","cur_19"]
[2041,"富风风场_A1-14 机组齿轮箱油池温度","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-14 机组齿轮箱油池温度","yc_hs_0186","cur_21"]
[2042,"富风风场_A1-14 机组发电机转速","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-14 机组发电机转速","yc_hs_0186","cur_24"]
[2043,"富风风场_A1-14 机组发电机绕组u1温度","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-14 机组发电机绕组u1温度","yc_hs_0186","cur_27"]
[2044,"富风风场_A1-14 机组发电机绕组v1温度","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-14 机组发电机绕组v1温度","yc_hs_0186","cur_29"]
[2045,"富风风场_A1-14 机组发电机绕组w1温度","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-14 机组发电机绕组w1温度","yc_hs_0186","cur_31"]
[2046,"富风风场_A1-14 机组发电机前轴承温度","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-14 机组发电机前轴承温度","yc_hs_0186","cur_33"]
[2047,"富风风场_A1-14 机组发电机后轴承温度","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-14 机组发电机后轴承温度","yc_hs_0186","cur_34"]
[2048,"富风风场_A1-14 机组瞬时风速","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-14 机组瞬时风速","yc_hs_0186","cur_47"]
[2049,"富风风场_A1-14 机组瞬时风向","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-14 机组瞬时风向","yc_hs_0186","cur_51"]
[2050,"富风风场_A1-14 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WROT.YC5","对风角度","yaw_error1","富风风场_A1-14 机组1#风向仪瞬时风向","yc_hs_0186","cur_52"]
[2051,"富风风场_A1-14 机组环境温度","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-14 机组环境温度","yc_hs_0186","cur_55"]
[2052,"富风风场_A1-14 机组机舱温度","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-14 机组机舱温度","yc_hs_0186","cur_56"]
[2053,"富风风场_A1-14 机组机舱X方向振动","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-14 机组机舱X方向振动","yc_hs_0186","cur_58"]
[2054,"富风风场_A1-14 机组机舱Y方向振动","太谷风电场","WOF35400075",14,"FFFD.T1_L1.WTG014.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-14 机组机舱Y方向振动","yc_hs_0186","cur_59"]
[2055,"富风风场_A1-15 机组有功功率","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WCNV.GridActivePW","有功功率","active_power","富风风场_A1-15 机组有功功率","yc_hs_0187","cur_25"]
[2056,"富风风场_A1-15 机组风轮转速","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A1-15 机组风轮转速","yc_hs_0187","cur_28"]
[2057,"富风风场_A1-15 机组1#叶片变桨角度","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A1-15 机组1#叶片变桨角度","yc_hs_0187","cur_30"]
[2058,"富风风场_A1-15 机组2#叶片变桨角度","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A1-15 机组2#叶片变桨角度","yc_hs_0187","cur_31"]
[2059,"富风风场_A1-15 机组3#叶片变桨角度","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A1-15 机组3#叶片变桨角度","yc_hs_0187","cur_32"]
[2060,"富风风场_A1-15 机组主轴前轴承温度","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A1-15 机组主轴前轴承温度","yc_hs_0187","cur_56"]
[2061,"富风风场_A1-15 机组齿轮箱油池温度","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A1-15 机组齿轮箱油池温度","yc_hs_0187","cur_58"]
[2062,"富风风场_A1-15 机组发电机转速","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A1-15 机组发电机转速","yc_hs_0187","cur_61"]
[2063,"富风风场_A1-15 机组发电机绕组u1温度","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A1-15 机组发电机绕组u1温度","yc_hs_0187","cur_64"]
[2064,"富风风场_A1-15 机组发电机绕组v1温度","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A1-15 机组发电机绕组v1温度","yc_hs_0187","cur_66"]
[2065,"富风风场_A1-15 机组发电机绕组w1温度","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A1-15 机组发电机绕组w1温度","yc_hs_0187","cur_68"]
[2066,"富风风场_A1-15 机组发电机前轴承温度","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A1-15 机组发电机前轴承温度","yc_hs_0187","cur_70"]
[2067,"富风风场_A1-15 机组发电机后轴承温度","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A1-15 机组发电机后轴承温度","yc_hs_0187","cur_71"]
[2068,"富风风场_A1-15 机组瞬时风速","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WNAC.WindSpeed","风速","wind_velocity","富风风场_A1-15 机组瞬时风速","yc_hs_0187","cur_84"]
[2069,"富风风场_A1-15 机组瞬时风向","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A1-15 机组瞬时风向","yc_hs_0187","cur_88"]
[2070,"富风风场_A1-15 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WROT.YC5","对风角度","yaw_error1","富风风场_A1-15 机组1#风向仪瞬时风向","yc_hs_0187","cur_89"]
[2071,"富风风场_A1-15 机组环境温度","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A1-15 机组环境温度","yc_hs_0187","cur_92"]
[2072,"富风风场_A1-15 机组机舱温度","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A1-15 机组机舱温度","yc_hs_0187","cur_93"]
[2073,"富风风场_A1-15 机组机舱X方向振动","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A1-15 机组机舱X方向振动","yc_hs_0187","cur_95"]
[2074,"富风风场_A1-15 机组机舱Y方向振动","太谷风电场","WOF35400075",15,"FFFD.T1_L1.WTG015.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A1-15 机组机舱Y方向振动","yc_hs_0187","cur_96"]
[2075,"富风风场_A2-16 机组有功功率","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-16 机组有功功率","yc_hs_0188","cur_62"]
[2076,"富风风场_A2-16 机组风轮转速","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-16 机组风轮转速","yc_hs_0188","cur_65"]
[2077,"富风风场_A2-16 机组1#叶片变桨角度","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-16 机组1#叶片变桨角度","yc_hs_0188","cur_67"]
[2078,"富风风场_A2-16 机组2#叶片变桨角度","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-16 机组2#叶片变桨角度","yc_hs_0188","cur_68"]
[2079,"富风风场_A2-16 机组3#叶片变桨角度","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-16 机组3#叶片变桨角度","yc_hs_0188","cur_69"]
[2080,"富风风场_A2-16 机组主轴前轴承温度","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-16 机组主轴前轴承温度","yc_hs_0188","cur_93"]
[2081,"富风风场_A2-16 机组齿轮箱油池温度","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-16 机组齿轮箱油池温度","yc_hs_0188","cur_95"]
[2082,"富风风场_A2-16 机组发电机转速","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-16 机组发电机转速","yc_hs_0188","cur_98"]
[2083,"富风风场_A2-16 机组发电机绕组u1温度","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-16 机组发电机绕组u1温度","yc_hs_0189","cur_01"]
[2084,"富风风场_A2-16 机组发电机绕组v1温度","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-16 机组发电机绕组v1温度","yc_hs_0189","cur_03"]
[2085,"富风风场_A2-16 机组发电机绕组w1温度","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-16 机组发电机绕组w1温度","yc_hs_0189","cur_05"]
[2086,"富风风场_A2-16 机组发电机前轴承温度","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-16 机组发电机前轴承温度","yc_hs_0189","cur_07"]
[2087,"富风风场_A2-16 机组发电机后轴承温度","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-16 机组发电机后轴承温度","yc_hs_0189","cur_08"]
[2088,"富风风场_A2-16 机组瞬时风速","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-16 机组瞬时风速","yc_hs_0189","cur_21"]
[2089,"富风风场_A2-16 机组瞬时风向","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-16 机组瞬时风向","yc_hs_0189","cur_25"]
[2090,"富风风场_A2-16 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WROT.YC5","对风角度","yaw_error1","富风风场_A2-16 机组1#风向仪瞬时风向","yc_hs_0189","cur_26"]
[2091,"富风风场_A2-16 机组环境温度","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-16 机组环境温度","yc_hs_0189","cur_29"]
[2092,"富风风场_A2-16 机组机舱温度","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-16 机组机舱温度","yc_hs_0189","cur_30"]
[2093,"富风风场_A2-16 机组机舱X方向振动","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-16 机组机舱X方向振动","yc_hs_0189","cur_32"]
[2094,"富风风场_A2-16 机组机舱Y方向振动","太谷风电场","WOF35400075",16,"FFFD.T1_L2.WTG016.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-16 机组机舱Y方向振动","yc_hs_0189","cur_33"]
[2095,"富风风场_A2-17 机组有功功率","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-17 机组有功功率","yc_hs_0189","cur_99"]
[2096,"富风风场_A2-17 机组风轮转速","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-17 机组风轮转速","yc_hs_0190","cur_02"]
[2097,"富风风场_A2-17 机组1#叶片变桨角度","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-17 机组1#叶片变桨角度","yc_hs_0190","cur_04"]
[2098,"富风风场_A2-17 机组2#叶片变桨角度","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-17 机组2#叶片变桨角度","yc_hs_0190","cur_05"]
[2099,"富风风场_A2-17 机组3#叶片变桨角度","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-17 机组3#叶片变桨角度","yc_hs_0190","cur_06"]
[2100,"富风风场_A2-17 机组主轴前轴承温度","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-17 机组主轴前轴承温度","yc_hs_0190","cur_30"]
[2101,"富风风场_A2-17 机组齿轮箱油池温度","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-17 机组齿轮箱油池温度","yc_hs_0190","cur_32"]
[2102,"富风风场_A2-17 机组发电机转速","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-17 机组发电机转速","yc_hs_0190","cur_35"]
[2103,"富风风场_A2-17 机组发电机绕组u1温度","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-17 机组发电机绕组u1温度","yc_hs_0190","cur_38"]
[2104,"富风风场_A2-17 机组发电机绕组v1温度","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-17 机组发电机绕组v1温度","yc_hs_0190","cur_40"]
[2105,"富风风场_A2-17 机组发电机绕组w1温度","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-17 机组发电机绕组w1温度","yc_hs_0190","cur_42"]
[2106,"富风风场_A2-17 机组发电机前轴承温度","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-17 机组发电机前轴承温度","yc_hs_0190","cur_44"]
[2107,"富风风场_A2-17 机组发电机后轴承温度","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-17 机组发电机后轴承温度","yc_hs_0190","cur_45"]
[2108,"富风风场_A2-17 机组瞬时风速","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-17 机组瞬时风速","yc_hs_0190","cur_58"]
[2109,"富风风场_A2-17 机组瞬时风向","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-17 机组瞬时风向","yc_hs_0190","cur_62"]
[2110,"富风风场_A2-17 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WROT.YC5","对风角度","yaw_error1","富风风场_A2-17 机组1#风向仪瞬时风向","yc_hs_0190","cur_63"]
[2111,"富风风场_A2-17 机组环境温度","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-17 机组环境温度","yc_hs_0190","cur_66"]
[2112,"富风风场_A2-17 机组机舱温度","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-17 机组机舱温度","yc_hs_0190","cur_67"]
[2113,"富风风场_A2-17 机组机舱X方向振动","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-17 机组机舱X方向振动","yc_hs_0190","cur_69"]
[2114,"富风风场_A2-17 机组机舱Y方向振动","太谷风电场","WOF35400075",17,"FFFD.T1_L2.WTG017.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-17 机组机舱Y方向振动","yc_hs_0190","cur_70"]
[2115,"富风风场_A2-18 机组有功功率","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-18 机组有功功率","yc_hs_0191","cur_36"]
[2116,"富风风场_A2-18 机组风轮转速","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-18 机组风轮转速","yc_hs_0191","cur_39"]
[2117,"富风风场_A2-18 机组1#叶片变桨角度","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-18 机组1#叶片变桨角度","yc_hs_0191","cur_41"]
[2118,"富风风场_A2-18 机组2#叶片变桨角度","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-18 机组2#叶片变桨角度","yc_hs_0191","cur_42"]
[2119,"富风风场_A2-18 机组3#叶片变桨角度","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-18 机组3#叶片变桨角度","yc_hs_0191","cur_43"]
[2120,"富风风场_A2-18 机组主轴前轴承温度","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-18 机组主轴前轴承温度","yc_hs_0191","cur_67"]
[2121,"富风风场_A2-18 机组齿轮箱油池温度","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-18 机组齿轮箱油池温度","yc_hs_0191","cur_69"]
[2122,"富风风场_A2-18 机组发电机转速","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-18 机组发电机转速","yc_hs_0191","cur_72"]
[2123,"富风风场_A2-18 机组发电机绕组u1温度","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-18 机组发电机绕组u1温度","yc_hs_0191","cur_75"]
[2124,"富风风场_A2-18 机组发电机绕组v1温度","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-18 机组发电机绕组v1温度","yc_hs_0191","cur_77"]
[2125,"富风风场_A2-18 机组发电机绕组w1温度","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-18 机组发电机绕组w1温度","yc_hs_0191","cur_79"]
[2126,"富风风场_A2-18 机组发电机前轴承温度","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-18 机组发电机前轴承温度","yc_hs_0191","cur_81"]
[2127,"富风风场_A2-18 机组发电机后轴承温度","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-18 机组发电机后轴承温度","yc_hs_0191","cur_82"]
[2128,"富风风场_A2-18 机组瞬时风速","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-18 机组瞬时风速","yc_hs_0191","cur_95"]
[2129,"富风风场_A2-18 机组瞬时风向","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-18 机组瞬时风向","yc_hs_0191","cur_99"]
[2130,"富风风场_A2-18 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WROT.YC5","对风角度","yaw_error1","富风风场_A2-18 机组1#风向仪瞬时风向","yc_hs_0191","cur_100"]
[2131,"富风风场_A2-18 机组环境温度","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-18 机组环境温度","yc_hs_0192","cur_03"]
[2132,"富风风场_A2-18 机组机舱温度","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-18 机组机舱温度","yc_hs_0192","cur_04"]
[2133,"富风风场_A2-18 机组机舱X方向振动","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-18 机组机舱X方向振动","yc_hs_0192","cur_06"]
[2134,"富风风场_A2-18 机组机舱Y方向振动","太谷风电场","WOF35400075",18,"FFFD.T1_L2.WTG018.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-18 机组机舱Y方向振动","yc_hs_0192","cur_07"]
[2135,"富风风场_A2-19 机组有功功率","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-19 机组有功功率","yc_hs_0192","cur_73"]
[2136,"富风风场_A2-19 机组风轮转速","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-19 机组风轮转速","yc_hs_0192","cur_76"]
[2137,"富风风场_A2-19 机组1#叶片变桨角度","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-19 机组1#叶片变桨角度","yc_hs_0192","cur_78"]
[2138,"富风风场_A2-19 机组2#叶片变桨角度","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-19 机组2#叶片变桨角度","yc_hs_0192","cur_79"]
[2139,"富风风场_A2-19 机组3#叶片变桨角度","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-19 机组3#叶片变桨角度","yc_hs_0192","cur_80"]
[2140,"富风风场_A2-19 机组主轴前轴承温度","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-19 机组主轴前轴承温度","yc_hs_0193","cur_04"]
[2141,"富风风场_A2-19 机组齿轮箱油池温度","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-19 机组齿轮箱油池温度","yc_hs_0193","cur_06"]
[2142,"富风风场_A2-19 机组发电机转速","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-19 机组发电机转速","yc_hs_0193","cur_09"]
[2143,"富风风场_A2-19 机组发电机绕组u1温度","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-19 机组发电机绕组u1温度","yc_hs_0193","cur_12"]
[2144,"富风风场_A2-19 机组发电机绕组v1温度","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-19 机组发电机绕组v1温度","yc_hs_0193","cur_14"]
[2145,"富风风场_A2-19 机组发电机绕组w1温度","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-19 机组发电机绕组w1温度","yc_hs_0193","cur_16"]
[2146,"富风风场_A2-19 机组发电机前轴承温度","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-19 机组发电机前轴承温度","yc_hs_0193","cur_18"]
[2147,"富风风场_A2-19 机组发电机后轴承温度","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-19 机组发电机后轴承温度","yc_hs_0193","cur_19"]
[2148,"富风风场_A2-19 机组瞬时风速","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-19 机组瞬时风速","yc_hs_0193","cur_32"]
[2149,"富风风场_A2-19 机组瞬时风向","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-19 机组瞬时风向","yc_hs_0193","cur_36"]
[2150,"富风风场_A2-19 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WROT.YC5","对风角度","yaw_error1","富风风场_A2-19 机组1#风向仪瞬时风向","yc_hs_0193","cur_37"]
[2151,"富风风场_A2-19 机组环境温度","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-19 机组环境温度","yc_hs_0193","cur_40"]
[2152,"富风风场_A2-19 机组机舱温度","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-19 机组机舱温度","yc_hs_0193","cur_41"]
[2153,"富风风场_A2-19 机组机舱X方向振动","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-19 机组机舱X方向振动","yc_hs_0193","cur_43"]
[2154,"富风风场_A2-19 机组机舱Y方向振动","太谷风电场","WOF35400075",19,"FFFD.T1_L2.WTG019.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-19 机组机舱Y方向振动","yc_hs_0193","cur_44"]
[2155,"富风风场_A2-20 机组有功功率","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-20 机组有功功率","yc_hs_0194","cur_10"]
[2156,"富风风场_A2-20 机组风轮转速","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-20 机组风轮转速","yc_hs_0194","cur_13"]
[2157,"富风风场_A2-20 机组1#叶片变桨角度","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-20 机组1#叶片变桨角度","yc_hs_0194","cur_15"]
[2158,"富风风场_A2-20 机组2#叶片变桨角度","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-20 机组2#叶片变桨角度","yc_hs_0194","cur_16"]
[2159,"富风风场_A2-20 机组3#叶片变桨角度","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-20 机组3#叶片变桨角度","yc_hs_0194","cur_17"]
[2160,"富风风场_A2-20 机组主轴前轴承温度","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-20 机组主轴前轴承温度","yc_hs_0194","cur_41"]
[2161,"富风风场_A2-20 机组齿轮箱油池温度","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-20 机组齿轮箱油池温度","yc_hs_0194","cur_43"]
[2162,"富风风场_A2-20 机组发电机转速","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-20 机组发电机转速","yc_hs_0194","cur_46"]
[2163,"富风风场_A2-20 机组发电机绕组u1温度","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-20 机组发电机绕组u1温度","yc_hs_0194","cur_49"]
[2164,"富风风场_A2-20 机组发电机绕组v1温度","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-20 机组发电机绕组v1温度","yc_hs_0194","cur_51"]
[2165,"富风风场_A2-20 机组发电机绕组w1温度","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-20 机组发电机绕组w1温度","yc_hs_0194","cur_53"]
[2166,"富风风场_A2-20 机组发电机前轴承温度","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-20 机组发电机前轴承温度","yc_hs_0194","cur_55"]
[2167,"富风风场_A2-20 机组发电机后轴承温度","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-20 机组发电机后轴承温度","yc_hs_0194","cur_56"]
[2168,"富风风场_A2-20 机组瞬时风速","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-20 机组瞬时风速","yc_hs_0194","cur_69"]
[2169,"富风风场_A2-20 机组瞬时风向","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-20 机组瞬时风向","yc_hs_0194","cur_73"]
[2170,"富风风场_A2-20 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WROT.YC5","对风角度","yaw_error1","富风风场_A2-20 机组1#风向仪瞬时风向","yc_hs_0194","cur_74"]
[2171,"富风风场_A2-20 机组环境温度","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-20 机组环境温度","yc_hs_0194","cur_77"]
[2172,"富风风场_A2-20 机组机舱温度","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-20 机组机舱温度","yc_hs_0194","cur_78"]
[2173,"富风风场_A2-20 机组机舱X方向振动","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-20 机组机舱X方向振动","yc_hs_0194","cur_80"]
[2174,"富风风场_A2-20 机组机舱Y方向振动","太谷风电场","WOF35400075",20,"FFFD.T1_L2.WTG020.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-20 机组机舱Y方向振动","yc_hs_0194","cur_81"]
[2175,"富风风场_A2-21 机组有功功率","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-21 机组有功功率","yc_hs_0195","cur_47"]
[2176,"富风风场_A2-21 机组风轮转速","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-21 机组风轮转速","yc_hs_0195","cur_50"]
[2177,"富风风场_A2-21 机组1#叶片变桨角度","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-21 机组1#叶片变桨角度","yc_hs_0195","cur_52"]
[2178,"富风风场_A2-21 机组2#叶片变桨角度","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-21 机组2#叶片变桨角度","yc_hs_0195","cur_53"]
[2179,"富风风场_A2-21 机组3#叶片变桨角度","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-21 机组3#叶片变桨角度","yc_hs_0195","cur_54"]
[2180,"富风风场_A2-21 机组主轴前轴承温度","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-21 机组主轴前轴承温度","yc_hs_0195","cur_78"]
[2181,"富风风场_A2-21 机组齿轮箱油池温度","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-21 机组齿轮箱油池温度","yc_hs_0195","cur_80"]
[2182,"富风风场_A2-21 机组发电机转速","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-21 机组发电机转速","yc_hs_0195","cur_83"]
[2183,"富风风场_A2-21 机组发电机绕组u1温度","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-21 机组发电机绕组u1温度","yc_hs_0195","cur_86"]
[2184,"富风风场_A2-21 机组发电机绕组v1温度","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-21 机组发电机绕组v1温度","yc_hs_0195","cur_88"]
[2185,"富风风场_A2-21 机组发电机绕组w1温度","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-21 机组发电机绕组w1温度","yc_hs_0195","cur_90"]
[2186,"富风风场_A2-21 机组发电机前轴承温度","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-21 机组发电机前轴承温度","yc_hs_0195","cur_92"]
[2187,"富风风场_A2-21 机组发电机后轴承温度","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-21 机组发电机后轴承温度","yc_hs_0195","cur_93"]
[2188,"富风风场_A2-21 机组瞬时风速","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-21 机组瞬时风速","yc_hs_0196","cur_06"]
[2189,"富风风场_A2-21 机组瞬时风向","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-21 机组瞬时风向","yc_hs_0196","cur_10"]
[2190,"富风风场_A2-21 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WROT.YC5","对风角度","yaw_error1","富风风场_A2-21 机组1#风向仪瞬时风向","yc_hs_0196","cur_11"]
[2191,"富风风场_A2-21 机组环境温度","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-21 机组环境温度","yc_hs_0196","cur_14"]
[2192,"富风风场_A2-21 机组机舱温度","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-21 机组机舱温度","yc_hs_0196","cur_15"]
[2193,"富风风场_A2-21 机组机舱X方向振动","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-21 机组机舱X方向振动","yc_hs_0196","cur_17"]
[2194,"富风风场_A2-21 机组机舱Y方向振动","太谷风电场","WOF35400075",21,"FFFD.T1_L2.WTG021.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-21 机组机舱Y方向振动","yc_hs_0196","cur_18"]
[2195,"富风风场_A2-22 机组有功功率","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-22 机组有功功率","yc_hs_0196","cur_84"]
[2196,"富风风场_A2-22 机组风轮转速","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-22 机组风轮转速","yc_hs_0196","cur_87"]
[2197,"富风风场_A2-22 机组1#叶片变桨角度","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-22 机组1#叶片变桨角度","yc_hs_0196","cur_89"]
[2198,"富风风场_A2-22 机组2#叶片变桨角度","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-22 机组2#叶片变桨角度","yc_hs_0196","cur_90"]
[2199,"富风风场_A2-22 机组3#叶片变桨角度","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-22 机组3#叶片变桨角度","yc_hs_0196","cur_91"]
[2200,"富风风场_A2-22 机组主轴前轴承温度","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-22 机组主轴前轴承温度","yc_hs_0197","cur_15"]
[2201,"富风风场_A2-22 机组齿轮箱油池温度","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-22 机组齿轮箱油池温度","yc_hs_0197","cur_17"]
[2202,"富风风场_A2-22 机组发电机转速","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-22 机组发电机转速","yc_hs_0197","cur_20"]
[2203,"富风风场_A2-22 机组发电机绕组u1温度","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-22 机组发电机绕组u1温度","yc_hs_0197","cur_23"]
[2204,"富风风场_A2-22 机组发电机绕组v1温度","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-22 机组发电机绕组v1温度","yc_hs_0197","cur_25"]
[2205,"富风风场_A2-22 机组发电机绕组w1温度","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-22 机组发电机绕组w1温度","yc_hs_0197","cur_27"]
[2206,"富风风场_A2-22 机组发电机前轴承温度","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-22 机组发电机前轴承温度","yc_hs_0197","cur_29"]
[2207,"富风风场_A2-22 机组发电机后轴承温度","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-22 机组发电机后轴承温度","yc_hs_0197","cur_30"]
[2208,"富风风场_A2-22 机组瞬时风速","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-22 机组瞬时风速","yc_hs_0197","cur_43"]
[2209,"富风风场_A2-22 机组瞬时风向","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-22 机组瞬时风向","yc_hs_0197","cur_47"]
[2210,"富风风场_A2-22 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WROT.YC5","对风角度","yaw_error1","富风风场_A2-22 机组1#风向仪瞬时风向","yc_hs_0197","cur_48"]
[2211,"富风风场_A2-22 机组环境温度","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-22 机组环境温度","yc_hs_0197","cur_51"]
[2212,"富风风场_A2-22 机组机舱温度","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-22 机组机舱温度","yc_hs_0197","cur_52"]
[2213,"富风风场_A2-22 机组机舱X方向振动","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-22 机组机舱X方向振动","yc_hs_0197","cur_54"]
[2214,"富风风场_A2-22 机组机舱Y方向振动","太谷风电场","WOF35400075",22,"FFFD.T1_L2.WTG022.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-22 机组机舱Y方向振动","yc_hs_0197","cur_55"]
[2215,"富风风场_A2-23 机组有功功率","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-23 机组有功功率","yc_hs_0198","cur_21"]
[2216,"富风风场_A2-23 机组风轮转速","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-23 机组风轮转速","yc_hs_0198","cur_24"]
[2217,"富风风场_A2-23 机组1#叶片变桨角度","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-23 机组1#叶片变桨角度","yc_hs_0198","cur_26"]
[2218,"富风风场_A2-23 机组2#叶片变桨角度","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-23 机组2#叶片变桨角度","yc_hs_0198","cur_27"]
[2219,"富风风场_A2-23 机组3#叶片变桨角度","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-23 机组3#叶片变桨角度","yc_hs_0198","cur_28"]
[2220,"富风风场_A2-23 机组主轴前轴承温度","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-23 机组主轴前轴承温度","yc_hs_0198","cur_52"]
[2221,"富风风场_A2-23 机组齿轮箱油池温度","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-23 机组齿轮箱油池温度","yc_hs_0198","cur_54"]
[2222,"富风风场_A2-23 机组发电机转速","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-23 机组发电机转速","yc_hs_0198","cur_57"]
[2223,"富风风场_A2-23 机组发电机绕组u1温度","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-23 机组发电机绕组u1温度","yc_hs_0198","cur_60"]
[2224,"富风风场_A2-23 机组发电机绕组v1温度","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-23 机组发电机绕组v1温度","yc_hs_0198","cur_62"]
[2225,"富风风场_A2-23 机组发电机绕组w1温度","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-23 机组发电机绕组w1温度","yc_hs_0198","cur_64"]
[2226,"富风风场_A2-23 机组发电机前轴承温度","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-23 机组发电机前轴承温度","yc_hs_0198","cur_66"]
[2227,"富风风场_A2-23 机组发电机后轴承温度","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-23 机组发电机后轴承温度","yc_hs_0198","cur_67"]
[2228,"富风风场_A2-23 机组瞬时风速","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-23 机组瞬时风速","yc_hs_0198","cur_80"]
[2229,"富风风场_A2-23 机组瞬时风向","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-23 机组瞬时风向","yc_hs_0198","cur_84"]
[2230,"富风风场_A2-23 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WROT.YC5","对风角度","yaw_error1","富风风场_A2-23 机组1#风向仪瞬时风向","yc_hs_0198","cur_85"]
[2231,"富风风场_A2-23 机组环境温度","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-23 机组环境温度","yc_hs_0198","cur_88"]
[2232,"富风风场_A2-23 机组机舱温度","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-23 机组机舱温度","yc_hs_0198","cur_89"]
[2233,"富风风场_A2-23 机组机舱X方向振动","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-23 机组机舱X方向振动","yc_hs_0198","cur_91"]
[2234,"富风风场_A2-23 机组机舱Y方向振动","太谷风电场","WOF35400075",23,"FFFD.T1_L2.WTG023.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-23 机组机舱Y方向振动","yc_hs_0198","cur_92"]
[2235,"富风风场_A2-24 机组有功功率","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-24 机组有功功率","yc_hs_0199","cur_58"]
[2236,"富风风场_A2-24 机组风轮转速","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-24 机组风轮转速","yc_hs_0199","cur_61"]
[2237,"富风风场_A2-24 机组1#叶片变桨角度","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-24 机组1#叶片变桨角度","yc_hs_0199","cur_63"]
[2238,"富风风场_A2-24 机组2#叶片变桨角度","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-24 机组2#叶片变桨角度","yc_hs_0199","cur_64"]
[2239,"富风风场_A2-24 机组3#叶片变桨角度","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-24 机组3#叶片变桨角度","yc_hs_0199","cur_65"]
[2240,"富风风场_A2-24 机组主轴前轴承温度","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-24 机组主轴前轴承温度","yc_hs_0199","cur_89"]
[2241,"富风风场_A2-24 机组齿轮箱油池温度","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-24 机组齿轮箱油池温度","yc_hs_0199","cur_91"]
[2242,"富风风场_A2-24 机组发电机转速","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-24 机组发电机转速","yc_hs_0199","cur_94"]
[2243,"富风风场_A2-24 机组发电机绕组u1温度","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-24 机组发电机绕组u1温度","yc_hs_0199","cur_97"]
[2244,"富风风场_A2-24 机组发电机绕组v1温度","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-24 机组发电机绕组v1温度","yc_hs_0199","cur_99"]
[2245,"富风风场_A2-24 机组发电机绕组w1温度","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-24 机组发电机绕组w1温度","yc_hs_0200","cur_01"]
[2246,"富风风场_A2-24 机组发电机前轴承温度","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-24 机组发电机前轴承温度","yc_hs_0200","cur_03"]
[2247,"富风风场_A2-24 机组发电机后轴承温度","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-24 机组发电机后轴承温度","yc_hs_0200","cur_04"]
[2248,"富风风场_A2-24 机组瞬时风速","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-24 机组瞬时风速","yc_hs_0200","cur_17"]
[2249,"富风风场_A2-24 机组瞬时风向","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-24 机组瞬时风向","yc_hs_0200","cur_21"]
[2250,"富风风场_A2-24 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WROT.YC5","对风角度","yaw_error1","富风风场_A2-24 机组1#风向仪瞬时风向","yc_hs_0200","cur_22"]
[2251,"富风风场_A2-24 机组环境温度","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-24 机组环境温度","yc_hs_0200","cur_25"]
[2252,"富风风场_A2-24 机组机舱温度","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-24 机组机舱温度","yc_hs_0200","cur_26"]
[2253,"富风风场_A2-24 机组机舱X方向振动","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-24 机组机舱X方向振动","yc_hs_0200","cur_28"]
[2254,"富风风场_A2-24 机组机舱Y方向振动","太谷风电场","WOF35400075",24,"FFFD.T1_L2.WTG024.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-24 机组机舱Y方向振动","yc_hs_0200","cur_29"]
[2255,"富风风场_A2-25 机组有功功率","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-25 机组有功功率","yc_hs_0200","cur_95"]
[2256,"富风风场_A2-25 机组风轮转速","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-25 机组风轮转速","yc_hs_0200","cur_98"]
[2257,"富风风场_A2-25 机组1#叶片变桨角度","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-25 机组1#叶片变桨角度","yc_hs_0200","cur_100"]
[2258,"富风风场_A2-25 机组2#叶片变桨角度","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-25 机组2#叶片变桨角度","yc_hs_0201","cur_01"]
[2259,"富风风场_A2-25 机组3#叶片变桨角度","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-25 机组3#叶片变桨角度","yc_hs_0201","cur_02"]
[2260,"富风风场_A2-25 机组主轴前轴承温度","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-25 机组主轴前轴承温度","yc_hs_0201","cur_26"]
[2261,"富风风场_A2-25 机组齿轮箱油池温度","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-25 机组齿轮箱油池温度","yc_hs_0201","cur_28"]
[2262,"富风风场_A2-25 机组发电机转速","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-25 机组发电机转速","yc_hs_0201","cur_31"]
[2263,"富风风场_A2-25 机组发电机绕组u1温度","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-25 机组发电机绕组u1温度","yc_hs_0201","cur_34"]
[2264,"富风风场_A2-25 机组发电机绕组v1温度","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-25 机组发电机绕组v1温度","yc_hs_0201","cur_36"]
[2265,"富风风场_A2-25 机组发电机绕组w1温度","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-25 机组发电机绕组w1温度","yc_hs_0201","cur_38"]
[2266,"富风风场_A2-25 机组发电机前轴承温度","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-25 机组发电机前轴承温度","yc_hs_0201","cur_40"]
[2267,"富风风场_A2-25 机组发电机后轴承温度","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-25 机组发电机后轴承温度","yc_hs_0201","cur_41"]
[2268,"富风风场_A2-25 机组瞬时风速","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-25 机组瞬时风速","yc_hs_0201","cur_54"]
[2269,"富风风场_A2-25 机组瞬时风向","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-25 机组瞬时风向","yc_hs_0201","cur_58"]
[2270,"富风风场_A2-25 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WROT.YC5","对风角度","yaw_error1","富风风场_A2-25 机组1#风向仪瞬时风向","yc_hs_0201","cur_59"]
[2271,"富风风场_A2-25 机组环境温度","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-25 机组环境温度","yc_hs_0201","cur_62"]
[2272,"富风风场_A2-25 机组机舱温度","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-25 机组机舱温度","yc_hs_0201","cur_63"]
[2273,"富风风场_A2-25 机组机舱X方向振动","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-25 机组机舱X方向振动","yc_hs_0201","cur_65"]
[2274,"富风风场_A2-25 机组机舱Y方向振动","太谷风电场","WOF35400075",25,"FFFD.T1_L2.WTG025.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-25 机组机舱Y方向振动","yc_hs_0201","cur_66"]
[2275,"富风风场_A2-26 机组有功功率","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-26 机组有功功率","yc_hs_0202","cur_32"]
[2276,"富风风场_A2-26 机组风轮转速","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-26 机组风轮转速","yc_hs_0202","cur_35"]
[2277,"富风风场_A2-26 机组1#叶片变桨角度","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-26 机组1#叶片变桨角度","yc_hs_0202","cur_37"]
[2278,"富风风场_A2-26 机组2#叶片变桨角度","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-26 机组2#叶片变桨角度","yc_hs_0202","cur_38"]
[2279,"富风风场_A2-26 机组3#叶片变桨角度","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-26 机组3#叶片变桨角度","yc_hs_0202","cur_39"]
[2280,"富风风场_A2-26 机组主轴前轴承温度","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-26 机组主轴前轴承温度","yc_hs_0202","cur_63"]
[2281,"富风风场_A2-26 机组齿轮箱油池温度","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-26 机组齿轮箱油池温度","yc_hs_0202","cur_65"]
[2282,"富风风场_A2-26 机组发电机转速","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-26 机组发电机转速","yc_hs_0202","cur_68"]
[2283,"富风风场_A2-26 机组发电机绕组u1温度","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-26 机组发电机绕组u1温度","yc_hs_0202","cur_71"]
[2284,"富风风场_A2-26 机组发电机绕组v1温度","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-26 机组发电机绕组v1温度","yc_hs_0202","cur_73"]
[2285,"富风风场_A2-26 机组发电机绕组w1温度","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-26 机组发电机绕组w1温度","yc_hs_0202","cur_75"]
[2286,"富风风场_A2-26 机组发电机前轴承温度","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-26 机组发电机前轴承温度","yc_hs_0202","cur_77"]
[2287,"富风风场_A2-26 机组发电机后轴承温度","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-26 机组发电机后轴承温度","yc_hs_0202","cur_78"]
[2288,"富风风场_A2-26 机组瞬时风速","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-26 机组瞬时风速","yc_hs_0202","cur_91"]
[2289,"富风风场_A2-26 机组瞬时风向","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-26 机组瞬时风向","yc_hs_0202","cur_95"]
[2290,"富风风场_A2-26 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WROT.YC5","对风角度","yaw_error1","富风风场_A2-26 机组1#风向仪瞬时风向","yc_hs_0202","cur_96"]
[2291,"富风风场_A2-26 机组环境温度","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-26 机组环境温度","yc_hs_0202","cur_99"]
[2292,"富风风场_A2-26 机组机舱温度","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-26 机组机舱温度","yc_hs_0202","cur_100"]
[2293,"富风风场_A2-26 机组机舱X方向振动","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-26 机组机舱X方向振动","yc_hs_0203","cur_02"]
[2294,"富风风场_A2-26 机组机舱Y方向振动","太谷风电场","WOF35400075",26,"FFFD.T1_L2.WTG026.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-26 机组机舱Y方向振动","yc_hs_0203","cur_03"]
[2295,"富风风场_A2-27 机组有功功率","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-27 机组有功功率","yc_hs_0203","cur_69"]
[2296,"富风风场_A2-27 机组风轮转速","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-27 机组风轮转速","yc_hs_0203","cur_72"]
[2297,"富风风场_A2-27 机组1#叶片变桨角度","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-27 机组1#叶片变桨角度","yc_hs_0203","cur_74"]
[2298,"富风风场_A2-27 机组2#叶片变桨角度","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-27 机组2#叶片变桨角度","yc_hs_0203","cur_75"]
[2299,"富风风场_A2-27 机组3#叶片变桨角度","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-27 机组3#叶片变桨角度","yc_hs_0203","cur_76"]
[2300,"富风风场_A2-27 机组主轴前轴承温度","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-27 机组主轴前轴承温度","yc_hs_0203","cur_100"]
[2301,"富风风场_A2-27 机组齿轮箱油池温度","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-27 机组齿轮箱油池温度","yc_hs_0204","cur_02"]
[2302,"富风风场_A2-27 机组发电机转速","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-27 机组发电机转速","yc_hs_0204","cur_05"]
[2303,"富风风场_A2-27 机组发电机绕组u1温度","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-27 机组发电机绕组u1温度","yc_hs_0204","cur_08"]
[2304,"富风风场_A2-27 机组发电机绕组v1温度","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-27 机组发电机绕组v1温度","yc_hs_0204","cur_10"]
[2305,"富风风场_A2-27 机组发电机绕组w1温度","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-27 机组发电机绕组w1温度","yc_hs_0204","cur_12"]
[2306,"富风风场_A2-27 机组发电机前轴承温度","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-27 机组发电机前轴承温度","yc_hs_0204","cur_14"]
[2307,"富风风场_A2-27 机组发电机后轴承温度","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-27 机组发电机后轴承温度","yc_hs_0204","cur_15"]
[2308,"富风风场_A2-27 机组瞬时风速","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-27 机组瞬时风速","yc_hs_0204","cur_28"]
[2309,"富风风场_A2-27 机组瞬时风向","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-27 机组瞬时风向","yc_hs_0204","cur_32"]
[2310,"富风风场_A2-27 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WROT.YC5","对风角度","yaw_error1","富风风场_A2-27 机组1#风向仪瞬时风向","yc_hs_0204","cur_33"]
[2311,"富风风场_A2-27 机组环境温度","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-27 机组环境温度","yc_hs_0204","cur_36"]
[2312,"富风风场_A2-27 机组机舱温度","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-27 机组机舱温度","yc_hs_0204","cur_37"]
[2313,"富风风场_A2-27 机组机舱X方向振动","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-27 机组机舱X方向振动","yc_hs_0204","cur_39"]
[2314,"富风风场_A2-27 机组机舱Y方向振动","太谷风电场","WOF35400075",27,"FFFD.T1_L2.WTG027.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-27 机组机舱Y方向振动","yc_hs_0204","cur_40"]
[2315,"富风风场_A2-28 机组有功功率","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-28 机组有功功率","yc_hs_0205","cur_06"]
[2316,"富风风场_A2-28 机组风轮转速","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-28 机组风轮转速","yc_hs_0205","cur_09"]
[2317,"富风风场_A2-28 机组1#叶片变桨角度","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-28 机组1#叶片变桨角度","yc_hs_0205","cur_11"]
[2318,"富风风场_A2-28 机组2#叶片变桨角度","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-28 机组2#叶片变桨角度","yc_hs_0205","cur_12"]
[2319,"富风风场_A2-28 机组3#叶片变桨角度","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-28 机组3#叶片变桨角度","yc_hs_0205","cur_13"]
[2320,"富风风场_A2-28 机组主轴前轴承温度","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-28 机组主轴前轴承温度","yc_hs_0205","cur_37"]
[2321,"富风风场_A2-28 机组齿轮箱油池温度","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-28 机组齿轮箱油池温度","yc_hs_0205","cur_39"]
[2322,"富风风场_A2-28 机组发电机转速","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-28 机组发电机转速","yc_hs_0205","cur_42"]
[2323,"富风风场_A2-28 机组发电机绕组u1温度","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-28 机组发电机绕组u1温度","yc_hs_0205","cur_45"]
[2324,"富风风场_A2-28 机组发电机绕组v1温度","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-28 机组发电机绕组v1温度","yc_hs_0205","cur_47"]
[2325,"富风风场_A2-28 机组发电机绕组w1温度","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-28 机组发电机绕组w1温度","yc_hs_0205","cur_49"]
[2326,"富风风场_A2-28 机组发电机前轴承温度","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-28 机组发电机前轴承温度","yc_hs_0205","cur_51"]
[2327,"富风风场_A2-28 机组发电机后轴承温度","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-28 机组发电机后轴承温度","yc_hs_0205","cur_52"]
[2328,"富风风场_A2-28 机组瞬时风速","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-28 机组瞬时风速","yc_hs_0205","cur_65"]
[2329,"富风风场_A2-28 机组瞬时风向","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-28 机组瞬时风向","yc_hs_0205","cur_69"]
[2330,"富风风场_A2-28 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WROT.YC5","对风角度","yaw_error1","富风风场_A2-28 机组1#风向仪瞬时风向","yc_hs_0205","cur_70"]
[2331,"富风风场_A2-28 机组环境温度","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-28 机组环境温度","yc_hs_0205","cur_73"]
[2332,"富风风场_A2-28 机组机舱温度","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-28 机组机舱温度","yc_hs_0205","cur_74"]
[2333,"富风风场_A2-28 机组机舱X方向振动","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-28 机组机舱X方向振动","yc_hs_0205","cur_76"]
[2334,"富风风场_A2-28 机组机舱Y方向振动","太谷风电场","WOF35400075",28,"FFFD.T1_L2.WTG028.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-28 机组机舱Y方向振动","yc_hs_0205","cur_77"]
[2335,"富风风场_A2-29 机组有功功率","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-29 机组有功功率","yc_hs_0206","cur_43"]
[2336,"富风风场_A2-29 机组风轮转速","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-29 机组风轮转速","yc_hs_0206","cur_46"]
[2337,"富风风场_A2-29 机组1#叶片变桨角度","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-29 机组1#叶片变桨角度","yc_hs_0206","cur_48"]
[2338,"富风风场_A2-29 机组2#叶片变桨角度","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-29 机组2#叶片变桨角度","yc_hs_0206","cur_49"]
[2339,"富风风场_A2-29 机组3#叶片变桨角度","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-29 机组3#叶片变桨角度","yc_hs_0206","cur_50"]
[2340,"富风风场_A2-29 机组主轴前轴承温度","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-29 机组主轴前轴承温度","yc_hs_0206","cur_74"]
[2341,"富风风场_A2-29 机组齿轮箱油池温度","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-29 机组齿轮箱油池温度","yc_hs_0206","cur_76"]
[2342,"富风风场_A2-29 机组发电机转速","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-29 机组发电机转速","yc_hs_0206","cur_79"]
[2343,"富风风场_A2-29 机组发电机绕组u1温度","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-29 机组发电机绕组u1温度","yc_hs_0206","cur_82"]
[2344,"富风风场_A2-29 机组发电机绕组v1温度","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-29 机组发电机绕组v1温度","yc_hs_0206","cur_84"]
[2345,"富风风场_A2-29 机组发电机绕组w1温度","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-29 机组发电机绕组w1温度","yc_hs_0206","cur_86"]
[2346,"富风风场_A2-29 机组发电机前轴承温度","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-29 机组发电机前轴承温度","yc_hs_0206","cur_88"]
[2347,"富风风场_A2-29 机组发电机后轴承温度","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-29 机组发电机后轴承温度","yc_hs_0206","cur_89"]
[2348,"富风风场_A2-29 机组瞬时风速","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-29 机组瞬时风速","yc_hs_0207","cur_02"]
[2349,"富风风场_A2-29 机组瞬时风向","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-29 机组瞬时风向","yc_hs_0207","cur_06"]
[2350,"富风风场_A2-29 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WROT.YC5","对风角度","yaw_error1","富风风场_A2-29 机组1#风向仪瞬时风向","yc_hs_0207","cur_07"]
[2351,"富风风场_A2-29 机组环境温度","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-29 机组环境温度","yc_hs_0207","cur_10"]
[2352,"富风风场_A2-29 机组机舱温度","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-29 机组机舱温度","yc_hs_0207","cur_11"]
[2353,"富风风场_A2-29 机组机舱X方向振动","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-29 机组机舱X方向振动","yc_hs_0207","cur_13"]
[2354,"富风风场_A2-29 机组机舱Y方向振动","太谷风电场","WOF35400075",29,"FFFD.T1_L2.WTG029.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-29 机组机舱Y方向振动","yc_hs_0207","cur_14"]
[2355,"富风风场_A2-30 机组有功功率","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WCNV.GridActivePW","有功功率","active_power","富风风场_A2-30 机组有功功率","yc_hs_0207","cur_80"]
[2356,"富风风场_A2-30 机组风轮转速","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A2-30 机组风轮转速","yc_hs_0207","cur_83"]
[2357,"富风风场_A2-30 机组1#叶片变桨角度","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A2-30 机组1#叶片变桨角度","yc_hs_0207","cur_85"]
[2358,"富风风场_A2-30 机组2#叶片变桨角度","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A2-30 机组2#叶片变桨角度","yc_hs_0207","cur_86"]
[2359,"富风风场_A2-30 机组3#叶片变桨角度","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A2-30 机组3#叶片变桨角度","yc_hs_0207","cur_87"]
[2360,"富风风场_A2-30 机组主轴前轴承温度","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A2-30 机组主轴前轴承温度","yc_hs_0208","cur_11"]
[2361,"富风风场_A2-30 机组齿轮箱油池温度","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A2-30 机组齿轮箱油池温度","yc_hs_0208","cur_13"]
[2362,"富风风场_A2-30 机组发电机转速","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A2-30 机组发电机转速","yc_hs_0208","cur_16"]
[2363,"富风风场_A2-30 机组发电机绕组u1温度","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A2-30 机组发电机绕组u1温度","yc_hs_0208","cur_19"]
[2364,"富风风场_A2-30 机组发电机绕组v1温度","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A2-30 机组发电机绕组v1温度","yc_hs_0208","cur_21"]
[2365,"富风风场_A2-30 机组发电机绕组w1温度","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A2-30 机组发电机绕组w1温度","yc_hs_0208","cur_23"]
[2366,"富风风场_A2-30 机组发电机前轴承温度","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A2-30 机组发电机前轴承温度","yc_hs_0208","cur_25"]
[2367,"富风风场_A2-30 机组发电机后轴承温度","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A2-30 机组发电机后轴承温度","yc_hs_0208","cur_26"]
[2368,"富风风场_A2-30 机组瞬时风速","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WNAC.WindSpeed","风速","wind_velocity","富风风场_A2-30 机组瞬时风速","yc_hs_0208","cur_39"]
[2369,"富风风场_A2-30 机组瞬时风向","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A2-30 机组瞬时风向","yc_hs_0208","cur_43"]
[2370,"富风风场_A2-30 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WROT.YC5","对风角度","yaw_error1","富风风场_A2-30 机组1#风向仪瞬时风向","yc_hs_0208","cur_44"]
[2371,"富风风场_A2-30 机组环境温度","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A2-30 机组环境温度","yc_hs_0208","cur_47"]
[2372,"富风风场_A2-30 机组机舱温度","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A2-30 机组机舱温度","yc_hs_0208","cur_48"]
[2373,"富风风场_A2-30 机组机舱X方向振动","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A2-30 机组机舱X方向振动","yc_hs_0208","cur_50"]
[2374,"富风风场_A2-30 机组机舱Y方向振动","太谷风电场","WOF35400075",30,"FFFD.T1_L2.WTG030.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A2-30 机组机舱Y方向振动","yc_hs_0208","cur_51"]
[2375,"富风风场_A3-31 机组有功功率","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-31 机组有功功率","yc_hs_0209","cur_17"]
[2376,"富风风场_A3-31 机组风轮转速","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-31 机组风轮转速","yc_hs_0209","cur_20"]
[2377,"富风风场_A3-31 机组1#叶片变桨角度","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-31 机组1#叶片变桨角度","yc_hs_0209","cur_22"]
[2378,"富风风场_A3-31 机组2#叶片变桨角度","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-31 机组2#叶片变桨角度","yc_hs_0209","cur_23"]
[2379,"富风风场_A3-31 机组3#叶片变桨角度","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-31 机组3#叶片变桨角度","yc_hs_0209","cur_24"]
[2380,"富风风场_A3-31 机组主轴前轴承温度","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-31 机组主轴前轴承温度","yc_hs_0209","cur_48"]
[2381,"富风风场_A3-31 机组齿轮箱油池温度","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-31 机组齿轮箱油池温度","yc_hs_0209","cur_50"]
[2382,"富风风场_A3-31 机组发电机转速","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-31 机组发电机转速","yc_hs_0209","cur_53"]
[2383,"富风风场_A3-31 机组发电机绕组u1温度","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-31 机组发电机绕组u1温度","yc_hs_0209","cur_56"]
[2384,"富风风场_A3-31 机组发电机绕组v1温度","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-31 机组发电机绕组v1温度","yc_hs_0209","cur_58"]
[2385,"富风风场_A3-31 机组发电机绕组w1温度","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-31 机组发电机绕组w1温度","yc_hs_0209","cur_60"]
[2386,"富风风场_A3-31 机组发电机前轴承温度","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-31 机组发电机前轴承温度","yc_hs_0209","cur_62"]
[2387,"富风风场_A3-31 机组发电机后轴承温度","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-31 机组发电机后轴承温度","yc_hs_0209","cur_63"]
[2388,"富风风场_A3-31 机组瞬时风速","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-31 机组瞬时风速","yc_hs_0209","cur_76"]
[2389,"富风风场_A3-31 机组瞬时风向","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-31 机组瞬时风向","yc_hs_0209","cur_80"]
[2390,"富风风场_A3-31 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WROT.YC5","对风角度","yaw_error1","富风风场_A3-31 机组1#风向仪瞬时风向","yc_hs_0209","cur_81"]
[2391,"富风风场_A3-31 机组环境温度","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-31 机组环境温度","yc_hs_0209","cur_84"]
[2392,"富风风场_A3-31 机组机舱温度","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-31 机组机舱温度","yc_hs_0209","cur_85"]
[2393,"富风风场_A3-31 机组机舱X方向振动","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-31 机组机舱X方向振动","yc_hs_0209","cur_87"]
[2394,"富风风场_A3-31 机组机舱Y方向振动","太谷风电场","WOF35400075",31,"FFFD.T1_L3.WTG031.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-31 机组机舱Y方向振动","yc_hs_0209","cur_88"]
[2395,"富风风场_A3-32 机组有功功率","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-32 机组有功功率","yc_hs_0210","cur_54"]
[2396,"富风风场_A3-32 机组风轮转速","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-32 机组风轮转速","yc_hs_0210","cur_57"]
[2397,"富风风场_A3-32 机组1#叶片变桨角度","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-32 机组1#叶片变桨角度","yc_hs_0210","cur_59"]
[2398,"富风风场_A3-32 机组2#叶片变桨角度","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-32 机组2#叶片变桨角度","yc_hs_0210","cur_60"]
[2399,"富风风场_A3-32 机组3#叶片变桨角度","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-32 机组3#叶片变桨角度","yc_hs_0210","cur_61"]
[2400,"富风风场_A3-32 机组主轴前轴承温度","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-32 机组主轴前轴承温度","yc_hs_0210","cur_85"]
[2401,"富风风场_A3-32 机组齿轮箱油池温度","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-32 机组齿轮箱油池温度","yc_hs_0210","cur_87"]
[2402,"富风风场_A3-32 机组发电机转速","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-32 机组发电机转速","yc_hs_0210","cur_90"]
[2403,"富风风场_A3-32 机组发电机绕组u1温度","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-32 机组发电机绕组u1温度","yc_hs_0210","cur_93"]
[2404,"富风风场_A3-32 机组发电机绕组v1温度","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-32 机组发电机绕组v1温度","yc_hs_0210","cur_95"]
[2405,"富风风场_A3-32 机组发电机绕组w1温度","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-32 机组发电机绕组w1温度","yc_hs_0210","cur_97"]
[2406,"富风风场_A3-32 机组发电机前轴承温度","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-32 机组发电机前轴承温度","yc_hs_0210","cur_99"]
[2407,"富风风场_A3-32 机组发电机后轴承温度","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-32 机组发电机后轴承温度","yc_hs_0210","cur_100"]
[2408,"富风风场_A3-32 机组瞬时风速","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-32 机组瞬时风速","yc_hs_0211","cur_13"]
[2409,"富风风场_A3-32 机组瞬时风向","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-32 机组瞬时风向","yc_hs_0211","cur_17"]
[2410,"富风风场_A3-32 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WROT.YC5","对风角度","yaw_error1","富风风场_A3-32 机组1#风向仪瞬时风向","yc_hs_0211","cur_18"]
[2411,"富风风场_A3-32 机组环境温度","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-32 机组环境温度","yc_hs_0211","cur_21"]
[2412,"富风风场_A3-32 机组机舱温度","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-32 机组机舱温度","yc_hs_0211","cur_22"]
[2413,"富风风场_A3-32 机组机舱X方向振动","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-32 机组机舱X方向振动","yc_hs_0211","cur_24"]
[2414,"富风风场_A3-32 机组机舱Y方向振动","太谷风电场","WOF35400075",32,"FFFD.T1_L3.WTG032.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-32 机组机舱Y方向振动","yc_hs_0211","cur_25"]
[2415,"富风风场_A3-33 机组有功功率","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-33 机组有功功率","yc_hs_0211","cur_91"]
[2416,"富风风场_A3-33 机组风轮转速","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-33 机组风轮转速","yc_hs_0211","cur_94"]
[2417,"富风风场_A3-33 机组1#叶片变桨角度","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-33 机组1#叶片变桨角度","yc_hs_0211","cur_96"]
[2418,"富风风场_A3-33 机组2#叶片变桨角度","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-33 机组2#叶片变桨角度","yc_hs_0211","cur_97"]
[2419,"富风风场_A3-33 机组3#叶片变桨角度","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-33 机组3#叶片变桨角度","yc_hs_0211","cur_98"]
[2420,"富风风场_A3-33 机组主轴前轴承温度","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-33 机组主轴前轴承温度","yc_hs_0212","cur_22"]
[2421,"富风风场_A3-33 机组齿轮箱油池温度","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-33 机组齿轮箱油池温度","yc_hs_0212","cur_24"]
[2422,"富风风场_A3-33 机组发电机转速","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-33 机组发电机转速","yc_hs_0212","cur_27"]
[2423,"富风风场_A3-33 机组发电机绕组u1温度","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-33 机组发电机绕组u1温度","yc_hs_0212","cur_30"]
[2424,"富风风场_A3-33 机组发电机绕组v1温度","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-33 机组发电机绕组v1温度","yc_hs_0212","cur_32"]
[2425,"富风风场_A3-33 机组发电机绕组w1温度","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-33 机组发电机绕组w1温度","yc_hs_0212","cur_34"]
[2426,"富风风场_A3-33 机组发电机前轴承温度","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-33 机组发电机前轴承温度","yc_hs_0212","cur_36"]
[2427,"富风风场_A3-33 机组发电机后轴承温度","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-33 机组发电机后轴承温度","yc_hs_0212","cur_37"]
[2428,"富风风场_A3-33 机组瞬时风速","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-33 机组瞬时风速","yc_hs_0212","cur_50"]
[2429,"富风风场_A3-33 机组瞬时风向","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-33 机组瞬时风向","yc_hs_0212","cur_54"]
[2430,"富风风场_A3-33 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WROT.YC5","对风角度","yaw_error1","富风风场_A3-33 机组1#风向仪瞬时风向","yc_hs_0212","cur_55"]
[2431,"富风风场_A3-33 机组环境温度","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-33 机组环境温度","yc_hs_0212","cur_58"]
[2432,"富风风场_A3-33 机组机舱温度","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-33 机组机舱温度","yc_hs_0212","cur_59"]
[2433,"富风风场_A3-33 机组机舱X方向振动","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-33 机组机舱X方向振动","yc_hs_0212","cur_61"]
[2434,"富风风场_A3-33 机组机舱Y方向振动","太谷风电场","WOF35400075",33,"FFFD.T1_L3.WTG033.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-33 机组机舱Y方向振动","yc_hs_0212","cur_62"]
[2435,"富风风场_A3-34 机组有功功率","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-34 机组有功功率","yc_hs_0213","cur_28"]
[2436,"富风风场_A3-34 机组风轮转速","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-34 机组风轮转速","yc_hs_0213","cur_31"]
[2437,"富风风场_A3-34 机组1#叶片变桨角度","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-34 机组1#叶片变桨角度","yc_hs_0213","cur_33"]
[2438,"富风风场_A3-34 机组2#叶片变桨角度","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-34 机组2#叶片变桨角度","yc_hs_0213","cur_34"]
[2439,"富风风场_A3-34 机组3#叶片变桨角度","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-34 机组3#叶片变桨角度","yc_hs_0213","cur_35"]
[2440,"富风风场_A3-34 机组主轴前轴承温度","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-34 机组主轴前轴承温度","yc_hs_0213","cur_59"]
[2441,"富风风场_A3-34 机组齿轮箱油池温度","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-34 机组齿轮箱油池温度","yc_hs_0213","cur_61"]
[2442,"富风风场_A3-34 机组发电机转速","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-34 机组发电机转速","yc_hs_0213","cur_64"]
[2443,"富风风场_A3-34 机组发电机绕组u1温度","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-34 机组发电机绕组u1温度","yc_hs_0213","cur_67"]
[2444,"富风风场_A3-34 机组发电机绕组v1温度","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-34 机组发电机绕组v1温度","yc_hs_0213","cur_69"]
[2445,"富风风场_A3-34 机组发电机绕组w1温度","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-34 机组发电机绕组w1温度","yc_hs_0213","cur_71"]
[2446,"富风风场_A3-34 机组发电机前轴承温度","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-34 机组发电机前轴承温度","yc_hs_0213","cur_73"]
[2447,"富风风场_A3-34 机组发电机后轴承温度","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-34 机组发电机后轴承温度","yc_hs_0213","cur_74"]
[2448,"富风风场_A3-34 机组瞬时风速","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-34 机组瞬时风速","yc_hs_0213","cur_87"]
[2449,"富风风场_A3-34 机组瞬时风向","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-34 机组瞬时风向","yc_hs_0213","cur_91"]
[2450,"富风风场_A3-34 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WROT.YC5","对风角度","yaw_error1","富风风场_A3-34 机组1#风向仪瞬时风向","yc_hs_0213","cur_92"]
[2451,"富风风场_A3-34 机组环境温度","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-34 机组环境温度","yc_hs_0213","cur_95"]
[2452,"富风风场_A3-34 机组机舱温度","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-34 机组机舱温度","yc_hs_0213","cur_96"]
[2453,"富风风场_A3-34 机组机舱X方向振动","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-34 机组机舱X方向振动","yc_hs_0213","cur_98"]
[2454,"富风风场_A3-34 机组机舱Y方向振动","太谷风电场","WOF35400075",34,"FFFD.T1_L3.WTG034.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-34 机组机舱Y方向振动","yc_hs_0213","cur_99"]
[2455,"富风风场_A3-35 机组有功功率","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-35 机组有功功率","yc_hs_0214","cur_65"]
[2456,"富风风场_A3-35 机组风轮转速","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-35 机组风轮转速","yc_hs_0214","cur_68"]
[2457,"富风风场_A3-35 机组1#叶片变桨角度","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-35 机组1#叶片变桨角度","yc_hs_0214","cur_70"]
[2458,"富风风场_A3-35 机组2#叶片变桨角度","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-35 机组2#叶片变桨角度","yc_hs_0214","cur_71"]
[2459,"富风风场_A3-35 机组3#叶片变桨角度","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-35 机组3#叶片变桨角度","yc_hs_0214","cur_72"]
[2460,"富风风场_A3-35 机组主轴前轴承温度","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-35 机组主轴前轴承温度","yc_hs_0214","cur_96"]
[2461,"富风风场_A3-35 机组齿轮箱油池温度","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-35 机组齿轮箱油池温度","yc_hs_0214","cur_98"]
[2462,"富风风场_A3-35 机组发电机转速","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-35 机组发电机转速","yc_hs_0215","cur_01"]
[2463,"富风风场_A3-35 机组发电机绕组u1温度","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-35 机组发电机绕组u1温度","yc_hs_0215","cur_04"]
[2464,"富风风场_A3-35 机组发电机绕组v1温度","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-35 机组发电机绕组v1温度","yc_hs_0215","cur_06"]
[2465,"富风风场_A3-35 机组发电机绕组w1温度","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-35 机组发电机绕组w1温度","yc_hs_0215","cur_08"]
[2466,"富风风场_A3-35 机组发电机前轴承温度","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-35 机组发电机前轴承温度","yc_hs_0215","cur_10"]
[2467,"富风风场_A3-35 机组发电机后轴承温度","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-35 机组发电机后轴承温度","yc_hs_0215","cur_11"]
[2468,"富风风场_A3-35 机组瞬时风速","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-35 机组瞬时风速","yc_hs_0215","cur_24"]
[2469,"富风风场_A3-35 机组瞬时风向","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-35 机组瞬时风向","yc_hs_0215","cur_28"]
[2470,"富风风场_A3-35 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WROT.YC5","对风角度","yaw_error1","富风风场_A3-35 机组1#风向仪瞬时风向","yc_hs_0215","cur_29"]
[2471,"富风风场_A3-35 机组环境温度","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-35 机组环境温度","yc_hs_0215","cur_32"]
[2472,"富风风场_A3-35 机组机舱温度","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-35 机组机舱温度","yc_hs_0215","cur_33"]
[2473,"富风风场_A3-35 机组机舱X方向振动","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-35 机组机舱X方向振动","yc_hs_0215","cur_35"]
[2474,"富风风场_A3-35 机组机舱Y方向振动","太谷风电场","WOF35400075",35,"FFFD.T1_L3.WTG035.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-35 机组机舱Y方向振动","yc_hs_0215","cur_36"]
[2475,"富风风场_A3-36 机组有功功率","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-36 机组有功功率","yc_hs_0216","cur_02"]
[2476,"富风风场_A3-36 机组风轮转速","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-36 机组风轮转速","yc_hs_0216","cur_05"]
[2477,"富风风场_A3-36 机组1#叶片变桨角度","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-36 机组1#叶片变桨角度","yc_hs_0216","cur_07"]
[2478,"富风风场_A3-36 机组2#叶片变桨角度","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-36 机组2#叶片变桨角度","yc_hs_0216","cur_08"]
[2479,"富风风场_A3-36 机组3#叶片变桨角度","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-36 机组3#叶片变桨角度","yc_hs_0216","cur_09"]
[2480,"富风风场_A3-36 机组主轴前轴承温度","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-36 机组主轴前轴承温度","yc_hs_0216","cur_33"]
[2481,"富风风场_A3-36 机组齿轮箱油池温度","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-36 机组齿轮箱油池温度","yc_hs_0216","cur_35"]
[2482,"富风风场_A3-36 机组发电机转速","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-36 机组发电机转速","yc_hs_0216","cur_38"]
[2483,"富风风场_A3-36 机组发电机绕组u1温度","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-36 机组发电机绕组u1温度","yc_hs_0216","cur_41"]
[2484,"富风风场_A3-36 机组发电机绕组v1温度","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-36 机组发电机绕组v1温度","yc_hs_0216","cur_43"]
[2485,"富风风场_A3-36 机组发电机绕组w1温度","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-36 机组发电机绕组w1温度","yc_hs_0216","cur_45"]
[2486,"富风风场_A3-36 机组发电机前轴承温度","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-36 机组发电机前轴承温度","yc_hs_0216","cur_47"]
[2487,"富风风场_A3-36 机组发电机后轴承温度","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-36 机组发电机后轴承温度","yc_hs_0216","cur_48"]
[2488,"富风风场_A3-36 机组瞬时风速","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-36 机组瞬时风速","yc_hs_0216","cur_61"]
[2489,"富风风场_A3-36 机组瞬时风向","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-36 机组瞬时风向","yc_hs_0216","cur_65"]
[2490,"富风风场_A3-36 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WROT.YC5","对风角度","yaw_error1","富风风场_A3-36 机组1#风向仪瞬时风向","yc_hs_0216","cur_66"]
[2491,"富风风场_A3-36 机组环境温度","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-36 机组环境温度","yc_hs_0216","cur_69"]
[2492,"富风风场_A3-36 机组机舱温度","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-36 机组机舱温度","yc_hs_0216","cur_70"]
[2493,"富风风场_A3-36 机组机舱X方向振动","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-36 机组机舱X方向振动","yc_hs_0216","cur_72"]
[2494,"富风风场_A3-36 机组机舱Y方向振动","太谷风电场","WOF35400075",36,"FFFD.T1_L3.WTG036.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-36 机组机舱Y方向振动","yc_hs_0216","cur_73"]
[2495,"富风风场_A3-37 机组有功功率","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-37 机组有功功率","yc_hs_0217","cur_39"]
[2496,"富风风场_A3-37 机组风轮转速","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-37 机组风轮转速","yc_hs_0217","cur_42"]
[2497,"富风风场_A3-37 机组1#叶片变桨角度","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-37 机组1#叶片变桨角度","yc_hs_0217","cur_44"]
[2498,"富风风场_A3-37 机组2#叶片变桨角度","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-37 机组2#叶片变桨角度","yc_hs_0217","cur_45"]
[2499,"富风风场_A3-37 机组3#叶片变桨角度","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-37 机组3#叶片变桨角度","yc_hs_0217","cur_46"]
[2500,"富风风场_A3-37 机组主轴前轴承温度","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-37 机组主轴前轴承温度","yc_hs_0217","cur_70"]
[2501,"富风风场_A3-37 机组齿轮箱油池温度","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-37 机组齿轮箱油池温度","yc_hs_0217","cur_72"]
[2502,"富风风场_A3-37 机组发电机转速","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-37 机组发电机转速","yc_hs_0217","cur_75"]
[2503,"富风风场_A3-37 机组发电机绕组u1温度","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-37 机组发电机绕组u1温度","yc_hs_0217","cur_78"]
[2504,"富风风场_A3-37 机组发电机绕组v1温度","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-37 机组发电机绕组v1温度","yc_hs_0217","cur_80"]
[2505,"富风风场_A3-37 机组发电机绕组w1温度","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-37 机组发电机绕组w1温度","yc_hs_0217","cur_82"]
[2506,"富风风场_A3-37 机组发电机前轴承温度","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-37 机组发电机前轴承温度","yc_hs_0217","cur_84"]
[2507,"富风风场_A3-37 机组发电机后轴承温度","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-37 机组发电机后轴承温度","yc_hs_0217","cur_85"]
[2508,"富风风场_A3-37 机组瞬时风速","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-37 机组瞬时风速","yc_hs_0217","cur_98"]
[2509,"富风风场_A3-37 机组瞬时风向","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-37 机组瞬时风向","yc_hs_0218","cur_02"]
[2510,"富风风场_A3-37 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WROT.YC5","对风角度","yaw_error1","富风风场_A3-37 机组1#风向仪瞬时风向","yc_hs_0218","cur_03"]
[2511,"富风风场_A3-37 机组环境温度","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-37 机组环境温度","yc_hs_0218","cur_06"]
[2512,"富风风场_A3-37 机组机舱温度","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-37 机组机舱温度","yc_hs_0218","cur_07"]
[2513,"富风风场_A3-37 机组机舱X方向振动","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-37 机组机舱X方向振动","yc_hs_0218","cur_09"]
[2514,"富风风场_A3-37 机组机舱Y方向振动","太谷风电场","WOF35400075",37,"FFFD.T1_L3.WTG037.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-37 机组机舱Y方向振动","yc_hs_0218","cur_10"]
[2515,"富风风场_A3-38 机组有功功率","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-38 机组有功功率","yc_hs_0218","cur_76"]
[2516,"富风风场_A3-38 机组风轮转速","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-38 机组风轮转速","yc_hs_0218","cur_79"]
[2517,"富风风场_A3-38 机组1#叶片变桨角度","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-38 机组1#叶片变桨角度","yc_hs_0218","cur_81"]
[2518,"富风风场_A3-38 机组2#叶片变桨角度","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-38 机组2#叶片变桨角度","yc_hs_0218","cur_82"]
[2519,"富风风场_A3-38 机组3#叶片变桨角度","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-38 机组3#叶片变桨角度","yc_hs_0218","cur_83"]
[2520,"富风风场_A3-38 机组主轴前轴承温度","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-38 机组主轴前轴承温度","yc_hs_0219","cur_07"]
[2521,"富风风场_A3-38 机组齿轮箱油池温度","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-38 机组齿轮箱油池温度","yc_hs_0219","cur_09"]
[2522,"富风风场_A3-38 机组发电机转速","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-38 机组发电机转速","yc_hs_0219","cur_12"]
[2523,"富风风场_A3-38 机组发电机绕组u1温度","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-38 机组发电机绕组u1温度","yc_hs_0219","cur_15"]
[2524,"富风风场_A3-38 机组发电机绕组v1温度","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-38 机组发电机绕组v1温度","yc_hs_0219","cur_17"]
[2525,"富风风场_A3-38 机组发电机绕组w1温度","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-38 机组发电机绕组w1温度","yc_hs_0219","cur_19"]
[2526,"富风风场_A3-38 机组发电机前轴承温度","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-38 机组发电机前轴承温度","yc_hs_0219","cur_21"]
[2527,"富风风场_A3-38 机组发电机后轴承温度","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-38 机组发电机后轴承温度","yc_hs_0219","cur_22"]
[2528,"富风风场_A3-38 机组瞬时风速","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-38 机组瞬时风速","yc_hs_0219","cur_35"]
[2529,"富风风场_A3-38 机组瞬时风向","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-38 机组瞬时风向","yc_hs_0219","cur_39"]
[2530,"富风风场_A3-38 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WROT.YC5","对风角度","yaw_error1","富风风场_A3-38 机组1#风向仪瞬时风向","yc_hs_0219","cur_40"]
[2531,"富风风场_A3-38 机组环境温度","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-38 机组环境温度","yc_hs_0219","cur_43"]
[2532,"富风风场_A3-38 机组机舱温度","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-38 机组机舱温度","yc_hs_0219","cur_44"]
[2533,"富风风场_A3-38 机组机舱X方向振动","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-38 机组机舱X方向振动","yc_hs_0219","cur_46"]
[2534,"富风风场_A3-38 机组机舱Y方向振动","太谷风电场","WOF35400075",38,"FFFD.T1_L3.WTG038.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-38 机组机舱Y方向振动","yc_hs_0219","cur_47"]
[2535,"富风风场_A3-39 机组有功功率","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-39 机组有功功率","yc_hs_0220","cur_13"]
[2536,"富风风场_A3-39 机组风轮转速","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-39 机组风轮转速","yc_hs_0220","cur_16"]
[2537,"富风风场_A3-39 机组1#叶片变桨角度","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-39 机组1#叶片变桨角度","yc_hs_0220","cur_18"]
[2538,"富风风场_A3-39 机组2#叶片变桨角度","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-39 机组2#叶片变桨角度","yc_hs_0220","cur_19"]
[2539,"富风风场_A3-39 机组3#叶片变桨角度","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-39 机组3#叶片变桨角度","yc_hs_0220","cur_20"]
[2540,"富风风场_A3-39 机组主轴前轴承温度","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-39 机组主轴前轴承温度","yc_hs_0220","cur_44"]
[2541,"富风风场_A3-39 机组齿轮箱油池温度","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-39 机组齿轮箱油池温度","yc_hs_0220","cur_46"]
[2542,"富风风场_A3-39 机组发电机转速","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-39 机组发电机转速","yc_hs_0220","cur_49"]
[2543,"富风风场_A3-39 机组发电机绕组u1温度","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-39 机组发电机绕组u1温度","yc_hs_0220","cur_52"]
[2544,"富风风场_A3-39 机组发电机绕组v1温度","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-39 机组发电机绕组v1温度","yc_hs_0220","cur_54"]
[2545,"富风风场_A3-39 机组发电机绕组w1温度","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-39 机组发电机绕组w1温度","yc_hs_0220","cur_56"]
[2546,"富风风场_A3-39 机组发电机前轴承温度","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-39 机组发电机前轴承温度","yc_hs_0220","cur_58"]
[2547,"富风风场_A3-39 机组发电机后轴承温度","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-39 机组发电机后轴承温度","yc_hs_0220","cur_59"]
[2548,"富风风场_A3-39 机组瞬时风速","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-39 机组瞬时风速","yc_hs_0220","cur_72"]
[2549,"富风风场_A3-39 机组瞬时风向","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-39 机组瞬时风向","yc_hs_0220","cur_76"]
[2550,"富风风场_A3-39 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WROT.YC5","对风角度","yaw_error1","富风风场_A3-39 机组1#风向仪瞬时风向","yc_hs_0220","cur_77"]
[2551,"富风风场_A3-39 机组环境温度","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-39 机组环境温度","yc_hs_0220","cur_80"]
[2552,"富风风场_A3-39 机组机舱温度","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-39 机组机舱温度","yc_hs_0220","cur_81"]
[2553,"富风风场_A3-39 机组机舱X方向振动","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-39 机组机舱X方向振动","yc_hs_0220","cur_83"]
[2554,"富风风场_A3-39 机组机舱Y方向振动","太谷风电场","WOF35400075",39,"FFFD.T1_L3.WTG039.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-39 机组机舱Y方向振动","yc_hs_0220","cur_84"]
[2555,"富风风场_A3-40 机组有功功率","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-40 机组有功功率","yc_hs_0221","cur_50"]
[2556,"富风风场_A3-40 机组风轮转速","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-40 机组风轮转速","yc_hs_0221","cur_53"]
[2557,"富风风场_A3-40 机组1#叶片变桨角度","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-40 机组1#叶片变桨角度","yc_hs_0221","cur_55"]
[2558,"富风风场_A3-40 机组2#叶片变桨角度","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-40 机组2#叶片变桨角度","yc_hs_0221","cur_56"]
[2559,"富风风场_A3-40 机组3#叶片变桨角度","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-40 机组3#叶片变桨角度","yc_hs_0221","cur_57"]
[2560,"富风风场_A3-40 机组主轴前轴承温度","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-40 机组主轴前轴承温度","yc_hs_0221","cur_81"]
[2561,"富风风场_A3-40 机组齿轮箱油池温度","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-40 机组齿轮箱油池温度","yc_hs_0221","cur_83"]
[2562,"富风风场_A3-40 机组发电机转速","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-40 机组发电机转速","yc_hs_0221","cur_86"]
[2563,"富风风场_A3-40 机组发电机绕组u1温度","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-40 机组发电机绕组u1温度","yc_hs_0221","cur_89"]
[2564,"富风风场_A3-40 机组发电机绕组v1温度","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-40 机组发电机绕组v1温度","yc_hs_0221","cur_91"]
[2565,"富风风场_A3-40 机组发电机绕组w1温度","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-40 机组发电机绕组w1温度","yc_hs_0221","cur_93"]
[2566,"富风风场_A3-40 机组发电机前轴承温度","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-40 机组发电机前轴承温度","yc_hs_0221","cur_95"]
[2567,"富风风场_A3-40 机组发电机后轴承温度","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-40 机组发电机后轴承温度","yc_hs_0221","cur_96"]
[2568,"富风风场_A3-40 机组瞬时风速","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-40 机组瞬时风速","yc_hs_0222","cur_09"]
[2569,"富风风场_A3-40 机组瞬时风向","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-40 机组瞬时风向","yc_hs_0222","cur_13"]
[2570,"富风风场_A3-40 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WROT.YC5","对风角度","yaw_error1","富风风场_A3-40 机组1#风向仪瞬时风向","yc_hs_0222","cur_14"]
[2571,"富风风场_A3-40 机组环境温度","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-40 机组环境温度","yc_hs_0222","cur_17"]
[2572,"富风风场_A3-40 机组机舱温度","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-40 机组机舱温度","yc_hs_0222","cur_18"]
[2573,"富风风场_A3-40 机组机舱X方向振动","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-40 机组机舱X方向振动","yc_hs_0222","cur_20"]
[2574,"富风风场_A3-40 机组机舱Y方向振动","太谷风电场","WOF35400075",40,"FFFD.T1_L3.WTG040.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-40 机组机舱Y方向振动","yc_hs_0222","cur_21"]
[2575,"富风风场_A3-41 机组有功功率","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-41 机组有功功率","yc_hs_0222","cur_87"]
[2576,"富风风场_A3-41 机组风轮转速","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-41 机组风轮转速","yc_hs_0222","cur_90"]
[2577,"富风风场_A3-41 机组1#叶片变桨角度","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-41 机组1#叶片变桨角度","yc_hs_0222","cur_92"]
[2578,"富风风场_A3-41 机组2#叶片变桨角度","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-41 机组2#叶片变桨角度","yc_hs_0222","cur_93"]
[2579,"富风风场_A3-41 机组3#叶片变桨角度","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-41 机组3#叶片变桨角度","yc_hs_0222","cur_94"]
[2580,"富风风场_A3-41 机组主轴前轴承温度","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-41 机组主轴前轴承温度","yc_hs_0223","cur_18"]
[2581,"富风风场_A3-41 机组齿轮箱油池温度","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-41 机组齿轮箱油池温度","yc_hs_0223","cur_20"]
[2582,"富风风场_A3-41 机组发电机转速","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-41 机组发电机转速","yc_hs_0223","cur_23"]
[2583,"富风风场_A3-41 机组发电机绕组u1温度","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-41 机组发电机绕组u1温度","yc_hs_0223","cur_26"]
[2584,"富风风场_A3-41 机组发电机绕组v1温度","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-41 机组发电机绕组v1温度","yc_hs_0223","cur_28"]
[2585,"富风风场_A3-41 机组发电机绕组w1温度","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-41 机组发电机绕组w1温度","yc_hs_0223","cur_30"]
[2586,"富风风场_A3-41 机组发电机前轴承温度","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-41 机组发电机前轴承温度","yc_hs_0223","cur_32"]
[2587,"富风风场_A3-41 机组发电机后轴承温度","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-41 机组发电机后轴承温度","yc_hs_0223","cur_33"]
[2588,"富风风场_A3-41 机组瞬时风速","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-41 机组瞬时风速","yc_hs_0223","cur_46"]
[2589,"富风风场_A3-41 机组瞬时风向","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-41 机组瞬时风向","yc_hs_0223","cur_50"]
[2590,"富风风场_A3-41 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WROT.YC5","对风角度","yaw_error1","富风风场_A3-41 机组1#风向仪瞬时风向","yc_hs_0223","cur_51"]
[2591,"富风风场_A3-41 机组环境温度","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-41 机组环境温度","yc_hs_0223","cur_54"]
[2592,"富风风场_A3-41 机组机舱温度","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-41 机组机舱温度","yc_hs_0223","cur_55"]
[2593,"富风风场_A3-41 机组机舱X方向振动","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-41 机组机舱X方向振动","yc_hs_0223","cur_57"]
[2594,"富风风场_A3-41 机组机舱Y方向振动","太谷风电场","WOF35400075",41,"FFFD.T1_L3.WTG041.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-41 机组机舱Y方向振动","yc_hs_0223","cur_58"]
[2595,"富风风场_A3-42 机组有功功率","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-42 机组有功功率","yc_hs_0224","cur_24"]
[2596,"富风风场_A3-42 机组风轮转速","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-42 机组风轮转速","yc_hs_0224","cur_27"]
[2597,"富风风场_A3-42 机组1#叶片变桨角度","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-42 机组1#叶片变桨角度","yc_hs_0224","cur_29"]
[2598,"富风风场_A3-42 机组2#叶片变桨角度","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-42 机组2#叶片变桨角度","yc_hs_0224","cur_30"]
[2599,"富风风场_A3-42 机组3#叶片变桨角度","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-42 机组3#叶片变桨角度","yc_hs_0224","cur_31"]
[2600,"富风风场_A3-42 机组主轴前轴承温度","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-42 机组主轴前轴承温度","yc_hs_0224","cur_55"]
[2601,"富风风场_A3-42 机组齿轮箱油池温度","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-42 机组齿轮箱油池温度","yc_hs_0224","cur_57"]
[2602,"富风风场_A3-42 机组发电机转速","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-42 机组发电机转速","yc_hs_0224","cur_60"]
[2603,"富风风场_A3-42 机组发电机绕组u1温度","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-42 机组发电机绕组u1温度","yc_hs_0224","cur_63"]
[2604,"富风风场_A3-42 机组发电机绕组v1温度","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-42 机组发电机绕组v1温度","yc_hs_0224","cur_65"]
[2605,"富风风场_A3-42 机组发电机绕组w1温度","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-42 机组发电机绕组w1温度","yc_hs_0224","cur_67"]
[2606,"富风风场_A3-42 机组发电机前轴承温度","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-42 机组发电机前轴承温度","yc_hs_0224","cur_69"]
[2607,"富风风场_A3-42 机组发电机后轴承温度","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-42 机组发电机后轴承温度","yc_hs_0224","cur_70"]
[2608,"富风风场_A3-42 机组瞬时风速","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-42 机组瞬时风速","yc_hs_0224","cur_83"]
[2609,"富风风场_A3-42 机组瞬时风向","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-42 机组瞬时风向","yc_hs_0224","cur_87"]
[2610,"富风风场_A3-42 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WROT.YC5","对风角度","yaw_error1","富风风场_A3-42 机组1#风向仪瞬时风向","yc_hs_0224","cur_88"]
[2611,"富风风场_A3-42 机组环境温度","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-42 机组环境温度","yc_hs_0224","cur_91"]
[2612,"富风风场_A3-42 机组机舱温度","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-42 机组机舱温度","yc_hs_0224","cur_92"]
[2613,"富风风场_A3-42 机组机舱X方向振动","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-42 机组机舱X方向振动","yc_hs_0224","cur_94"]
[2614,"富风风场_A3-42 机组机舱Y方向振动","太谷风电场","WOF35400075",42,"FFFD.T1_L3.WTG042.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-42 机组机舱Y方向振动","yc_hs_0224","cur_95"]
[2615,"富风风场_A3-43 机组有功功率","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-43 机组有功功率","yc_hs_0225","cur_61"]
[2616,"富风风场_A3-43 机组风轮转速","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-43 机组风轮转速","yc_hs_0225","cur_64"]
[2617,"富风风场_A3-43 机组1#叶片变桨角度","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-43 机组1#叶片变桨角度","yc_hs_0225","cur_66"]
[2618,"富风风场_A3-43 机组2#叶片变桨角度","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-43 机组2#叶片变桨角度","yc_hs_0225","cur_67"]
[2619,"富风风场_A3-43 机组3#叶片变桨角度","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-43 机组3#叶片变桨角度","yc_hs_0225","cur_68"]
[2620,"富风风场_A3-43 机组主轴前轴承温度","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-43 机组主轴前轴承温度","yc_hs_0225","cur_92"]
[2621,"富风风场_A3-43 机组齿轮箱油池温度","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-43 机组齿轮箱油池温度","yc_hs_0225","cur_94"]
[2622,"富风风场_A3-43 机组发电机转速","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-43 机组发电机转速","yc_hs_0225","cur_97"]
[2623,"富风风场_A3-43 机组发电机绕组u1温度","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-43 机组发电机绕组u1温度","yc_hs_0225","cur_100"]
[2624,"富风风场_A3-43 机组发电机绕组v1温度","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-43 机组发电机绕组v1温度","yc_hs_0226","cur_02"]
[2625,"富风风场_A3-43 机组发电机绕组w1温度","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-43 机组发电机绕组w1温度","yc_hs_0226","cur_04"]
[2626,"富风风场_A3-43 机组发电机前轴承温度","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-43 机组发电机前轴承温度","yc_hs_0226","cur_06"]
[2627,"富风风场_A3-43 机组发电机后轴承温度","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-43 机组发电机后轴承温度","yc_hs_0226","cur_07"]
[2628,"富风风场_A3-43 机组瞬时风速","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-43 机组瞬时风速","yc_hs_0226","cur_20"]
[2629,"富风风场_A3-43 机组瞬时风向","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-43 机组瞬时风向","yc_hs_0226","cur_24"]
[2630,"富风风场_A3-43 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WROT.YC5","对风角度","yaw_error1","富风风场_A3-43 机组1#风向仪瞬时风向","yc_hs_0226","cur_25"]
[2631,"富风风场_A3-43 机组环境温度","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-43 机组环境温度","yc_hs_0226","cur_28"]
[2632,"富风风场_A3-43 机组机舱温度","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-43 机组机舱温度","yc_hs_0226","cur_29"]
[2633,"富风风场_A3-43 机组机舱X方向振动","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-43 机组机舱X方向振动","yc_hs_0226","cur_31"]
[2634,"富风风场_A3-43 机组机舱Y方向振动","太谷风电场","WOF35400075",43,"FFFD.T1_L3.WTG043.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-43 机组机舱Y方向振动","yc_hs_0226","cur_32"]
[2635,"富风风场_A3-44 机组有功功率","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-44 机组有功功率","yc_hs_0226","cur_98"]
[2636,"富风风场_A3-44 机组风轮转速","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-44 机组风轮转速","yc_hs_0227","cur_01"]
[2637,"富风风场_A3-44 机组1#叶片变桨角度","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-44 机组1#叶片变桨角度","yc_hs_0227","cur_03"]
[2638,"富风风场_A3-44 机组2#叶片变桨角度","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-44 机组2#叶片变桨角度","yc_hs_0227","cur_04"]
[2639,"富风风场_A3-44 机组3#叶片变桨角度","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-44 机组3#叶片变桨角度","yc_hs_0227","cur_05"]
[2640,"富风风场_A3-44 机组主轴前轴承温度","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-44 机组主轴前轴承温度","yc_hs_0227","cur_29"]
[2641,"富风风场_A3-44 机组齿轮箱油池温度","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-44 机组齿轮箱油池温度","yc_hs_0227","cur_31"]
[2642,"富风风场_A3-44 机组发电机转速","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-44 机组发电机转速","yc_hs_0227","cur_34"]
[2643,"富风风场_A3-44 机组发电机绕组u1温度","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-44 机组发电机绕组u1温度","yc_hs_0227","cur_37"]
[2644,"富风风场_A3-44 机组发电机绕组v1温度","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-44 机组发电机绕组v1温度","yc_hs_0227","cur_39"]
[2645,"富风风场_A3-44 机组发电机绕组w1温度","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-44 机组发电机绕组w1温度","yc_hs_0227","cur_41"]
[2646,"富风风场_A3-44 机组发电机前轴承温度","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-44 机组发电机前轴承温度","yc_hs_0227","cur_43"]
[2647,"富风风场_A3-44 机组发电机后轴承温度","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-44 机组发电机后轴承温度","yc_hs_0227","cur_44"]
[2648,"富风风场_A3-44 机组瞬时风速","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-44 机组瞬时风速","yc_hs_0227","cur_57"]
[2649,"富风风场_A3-44 机组瞬时风向","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-44 机组瞬时风向","yc_hs_0227","cur_61"]
[2650,"富风风场_A3-44 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WROT.YC5","对风角度","yaw_error1","富风风场_A3-44 机组1#风向仪瞬时风向","yc_hs_0227","cur_62"]
[2651,"富风风场_A3-44 机组环境温度","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-44 机组环境温度","yc_hs_0227","cur_65"]
[2652,"富风风场_A3-44 机组机舱温度","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-44 机组机舱温度","yc_hs_0227","cur_66"]
[2653,"富风风场_A3-44 机组机舱X方向振动","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-44 机组机舱X方向振动","yc_hs_0227","cur_68"]
[2654,"富风风场_A3-44 机组机舱Y方向振动","太谷风电场","WOF35400075",44,"FFFD.T1_L3.WTG044.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-44 机组机舱Y方向振动","yc_hs_0227","cur_69"]
[2655,"富风风场_A3-45 机组有功功率","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WCNV.GridActivePW","有功功率","active_power","富风风场_A3-45 机组有功功率","yc_hs_0228","cur_35"]
[2656,"富风风场_A3-45 机组风轮转速","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WTRM.RotorSpd","风轮转速","rotor_speed","富风风场_A3-45 机组风轮转速","yc_hs_0228","cur_38"]
[2657,"富风风场_A3-45 机组1#叶片变桨角度","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","富风风场_A3-45 机组1#叶片变桨角度","yc_hs_0228","cur_40"]
[2658,"富风风场_A3-45 机组2#叶片变桨角度","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","富风风场_A3-45 机组2#叶片变桨角度","yc_hs_0228","cur_41"]
[2659,"富风风场_A3-45 机组3#叶片变桨角度","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","富风风场_A3-45 机组3#叶片变桨角度","yc_hs_0228","cur_42"]
[2660,"富风风场_A3-45 机组主轴前轴承温度","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","富风风场_A3-45 机组主轴前轴承温度","yc_hs_0228","cur_66"]
[2661,"富风风场_A3-45 机组齿轮箱油池温度","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","富风风场_A3-45 机组齿轮箱油池温度","yc_hs_0228","cur_68"]
[2662,"富风风场_A3-45 机组发电机转速","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WGEN.GenSpd","发电机转速","generator_speed","富风风场_A3-45 机组发电机转速","yc_hs_0228","cur_71"]
[2663,"富风风场_A3-45 机组发电机绕组u1温度","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","富风风场_A3-45 机组发电机绕组u1温度","yc_hs_0228","cur_74"]
[2664,"富风风场_A3-45 机组发电机绕组v1温度","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WGEN.GenSenTmp3","发电机绕组2温度","generator_winding2_temperature","富风风场_A3-45 机组发电机绕组v1温度","yc_hs_0228","cur_76"]
[2665,"富风风场_A3-45 机组发电机绕组w1温度","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WGEN.GenSenTmp5","发电机绕组3温度","generator_winding3_temperature","富风风场_A3-45 机组发电机绕组w1温度","yc_hs_0228","cur_78"]
[2666,"富风风场_A3-45 机组发电机前轴承温度","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","富风风场_A3-45 机组发电机前轴承温度","yc_hs_0228","cur_80"]
[2667,"富风风场_A3-45 机组发电机后轴承温度","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","富风风场_A3-45 机组发电机后轴承温度","yc_hs_0228","cur_81"]
[2668,"富风风场_A3-45 机组瞬时风速","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WNAC.WindSpeed","风速","wind_velocity","富风风场_A3-45 机组瞬时风速","yc_hs_0228","cur_94"]
[2669,"富风风场_A3-45 机组瞬时风向","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WNAC.WindDirection","绝对风向","true_wind_direction","富风风场_A3-45 机组瞬时风向","yc_hs_0228","cur_98"]
[2670,"富风风场_A3-45 机组1#风向仪瞬时风向","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WROT.YC5","对风角度","yaw_error1","富风风场_A3-45 机组1#风向仪瞬时风向","yc_hs_0228","cur_99"]
[2671,"富风风场_A3-45 机组环境温度","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WNAC.TemOut","环境温度","outside_cabin_temperature","富风风场_A3-45 机组环境温度","yc_hs_0229","cur_02"]
[2672,"富风风场_A3-45 机组机舱温度","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WNAC.TemNacelle","机舱内温度","cabin_temperature","富风风场_A3-45 机组机舱温度","yc_hs_0229","cur_03"]
[2673,"富风风场_A3-45 机组机舱X方向振动","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WROT.YC9","机舱左右振动","side_to_side_vibration_of_the_cabin","富风风场_A3-45 机组机舱X方向振动","yc_hs_0229","cur_05"]
[2674,"富风风场_A3-45 机组机舱Y方向振动","太谷风电场","WOF35400075",45,"FFFD.T1_L3.WTG045.WROT.YC10","机舱前后振动","front_back_vibration_of_the_cabin","富风风场_A3-45 机组机舱Y方向振动","yc_hs_0229","cur_06"]
[2675,"g_西潘二期Ⅲ-026 桨叶1位置给定","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅲ-026 桨叶1位置给定","yc_hs_0558","cur_09"]
[2676,"g_西潘二期Ⅲ-026 桨叶2位置给定","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅲ-026 桨叶2位置给定","yc_hs_0558","cur_10"]
[2677,"g_西潘二期Ⅲ-026 桨叶3位置给定","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅲ-026 桨叶3位置给定","yc_hs_0558","cur_11"]
[2678,"g_西潘二期Ⅲ-026 机舱位置","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅲ-026 机舱位置","yc_hs_0558","cur_44"]
[2679,"g_西潘二期Ⅲ-026 齿轮箱油温","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅲ-026 齿轮箱油温","yc_hs_0558","cur_47"]
[2680,"g_西潘二期Ⅲ-026 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅲ-026 齿轮箱高速轴轴承后端温度","yc_hs_0558","cur_49"]
[2681,"g_西潘二期Ⅲ-026 舱内温度","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅲ-026 舱内温度","yc_hs_0558","cur_53"]
[2682,"g_西潘二期Ⅲ-026 舱外温度","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅲ-026 舱外温度","yc_hs_0558","cur_55"]
[2683,"g_西潘二期Ⅲ-026 发电机转速","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅲ-026 发电机转速","yc_hs_0558","cur_58"]
[2684,"g_西潘二期Ⅲ-026 风轮转速","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅲ-026 风轮转速","yc_hs_0558","cur_59"]
[2685,"g_西潘二期Ⅲ-026 发电机定子L1绕组温度","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅲ-026 发电机定子L1绕组温度","yc_hs_0558","cur_60"]
[2686,"g_西潘二期Ⅲ-026 发电机定子L2绕组温度","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅲ-026 发电机定子L2绕组温度","yc_hs_0558","cur_61"]
[2687,"g_西潘二期Ⅲ-026 发电机定子L3绕组温度","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅲ-026 发电机定子L3绕组温度","yc_hs_0558","cur_62"]
[2688,"g_西潘二期Ⅲ-026 发电机驱动端轴承温度","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅲ-026 发电机驱动端轴承温度","yc_hs_0558","cur_63"]
[2689,"g_西潘二期Ⅲ-026 发电机非驱动端轴承温度","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅲ-026 发电机非驱动端轴承温度","yc_hs_0558","cur_64"]
[2690,"g_西潘二期Ⅲ-026 电网有功功率","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅲ-026 电网有功功率","yc_hs_0558","cur_80"]
[2691,"g_西潘二期Ⅲ-026 实时风速","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅲ-026 实时风速","yc_hs_0558","cur_93"]
[2692,"g_西潘二期Ⅲ-026 对风误差","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅲ-026 对风误差","yc_hs_0558","cur_97"]
[2693,"g_西潘二期Ⅲ-026 3s风向(0-360度)","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅲ-026 3s风向(0-360度)","yc_hs_0559","cur_02"]
[2694,"g_西潘二期Ⅲ-026 主轴温度","西潘风电场","WOF35300077",26,"YQXP.T2_L3.WTG026.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅲ-026 主轴温度","yc_hs_0559","cur_60"]
[2695,"g_西潘二期Ⅲ-027 桨叶1位置给定","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅲ-027 桨叶1位置给定","yc_hs_0560","cur_01"]
[2696,"g_西潘二期Ⅲ-027 桨叶2位置给定","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅲ-027 桨叶2位置给定","yc_hs_0560","cur_02"]
[2697,"g_西潘二期Ⅲ-027 桨叶3位置给定","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅲ-027 桨叶3位置给定","yc_hs_0560","cur_03"]
[2698,"g_西潘二期Ⅲ-027 机舱位置","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅲ-027 机舱位置","yc_hs_0560","cur_36"]
[2699,"g_西潘二期Ⅲ-027 齿轮箱油温","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅲ-027 齿轮箱油温","yc_hs_0560","cur_39"]
[2700,"g_西潘二期Ⅲ-027 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅲ-027 齿轮箱高速轴轴承后端温度","yc_hs_0560","cur_41"]
[2701,"g_西潘二期Ⅲ-027 舱内温度","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅲ-027 舱内温度","yc_hs_0560","cur_45"]
[2702,"g_西潘二期Ⅲ-027 舱外温度","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅲ-027 舱外温度","yc_hs_0560","cur_47"]
[2703,"g_西潘二期Ⅲ-027 发电机转速","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅲ-027 发电机转速","yc_hs_0560","cur_50"]
[2704,"g_西潘二期Ⅲ-027 风轮转速","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅲ-027 风轮转速","yc_hs_0560","cur_51"]
[2705,"g_西潘二期Ⅲ-027 发电机定子L1绕组温度","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅲ-027 发电机定子L1绕组温度","yc_hs_0560","cur_52"]
[2706,"g_西潘二期Ⅲ-027 发电机定子L2绕组温度","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅲ-027 发电机定子L2绕组温度","yc_hs_0560","cur_53"]
[2707,"g_西潘二期Ⅲ-027 发电机定子L3绕组温度","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅲ-027 发电机定子L3绕组温度","yc_hs_0560","cur_54"]
[2708,"g_西潘二期Ⅲ-027 发电机驱动端轴承温度","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅲ-027 发电机驱动端轴承温度","yc_hs_0560","cur_55"]
[2709,"g_西潘二期Ⅲ-027 发电机非驱动端轴承温度","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅲ-027 发电机非驱动端轴承温度","yc_hs_0560","cur_56"]
[2710,"g_西潘二期Ⅲ-027 电网有功功率","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅲ-027 电网有功功率","yc_hs_0560","cur_72"]
[2711,"g_西潘二期Ⅲ-027 实时风速","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅲ-027 实时风速","yc_hs_0560","cur_85"]
[2712,"g_西潘二期Ⅲ-027 对风误差","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅲ-027 对风误差","yc_hs_0560","cur_89"]
[2713,"g_西潘二期Ⅲ-027 3s风向(0-360度)","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅲ-027 3s风向(0-360度)","yc_hs_0560","cur_94"]
[2714,"g_西潘二期Ⅲ-027 主轴温度","西潘风电场","WOF35300077",27,"YQXP.T2_L3.WTG027.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅲ-027 主轴温度","yc_hs_0561","cur_52"]
[2715,"g_西潘二期Ⅲ-028 桨叶1位置给定","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅲ-028 桨叶1位置给定","yc_hs_0561","cur_93"]
[2716,"g_西潘二期Ⅲ-028 桨叶2位置给定","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅲ-028 桨叶2位置给定","yc_hs_0561","cur_94"]
[2717,"g_西潘二期Ⅲ-028 桨叶3位置给定","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅲ-028 桨叶3位置给定","yc_hs_0561","cur_95"]
[2718,"g_西潘二期Ⅲ-028 机舱位置","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅲ-028 机舱位置","yc_hs_0562","cur_28"]
[2719,"g_西潘二期Ⅲ-028 齿轮箱油温","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅲ-028 齿轮箱油温","yc_hs_0562","cur_31"]
[2720,"g_西潘二期Ⅲ-028 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅲ-028 齿轮箱高速轴轴承后端温度","yc_hs_0562","cur_33"]
[2721,"g_西潘二期Ⅲ-028 舱内温度","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅲ-028 舱内温度","yc_hs_0562","cur_37"]
[2722,"g_西潘二期Ⅲ-028 舱外温度","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅲ-028 舱外温度","yc_hs_0562","cur_39"]
[2723,"g_西潘二期Ⅲ-028 发电机转速","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅲ-028 发电机转速","yc_hs_0562","cur_42"]
[2724,"g_西潘二期Ⅲ-028 风轮转速","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅲ-028 风轮转速","yc_hs_0562","cur_43"]
[2725,"g_西潘二期Ⅲ-028 发电机定子L1绕组温度","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅲ-028 发电机定子L1绕组温度","yc_hs_0562","cur_44"]
[2726,"g_西潘二期Ⅲ-028 发电机定子L2绕组温度","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅲ-028 发电机定子L2绕组温度","yc_hs_0562","cur_45"]
[2727,"g_西潘二期Ⅲ-028 发电机定子L3绕组温度","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅲ-028 发电机定子L3绕组温度","yc_hs_0562","cur_46"]
[2728,"g_西潘二期Ⅲ-028 发电机驱动端轴承温度","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅲ-028 发电机驱动端轴承温度","yc_hs_0562","cur_47"]
[2729,"g_西潘二期Ⅲ-028 发电机非驱动端轴承温度","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅲ-028 发电机非驱动端轴承温度","yc_hs_0562","cur_48"]
[2730,"g_西潘二期Ⅲ-028 电网有功功率","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅲ-028 电网有功功率","yc_hs_0562","cur_64"]
[2731,"g_西潘二期Ⅲ-028 实时风速","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅲ-028 实时风速","yc_hs_0562","cur_77"]
[2732,"g_西潘二期Ⅲ-028 对风误差","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅲ-028 对风误差","yc_hs_0562","cur_81"]
[2733,"g_西潘二期Ⅲ-028 3s风向(0-360度)","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅲ-028 3s风向(0-360度)","yc_hs_0562","cur_86"]
[2734,"g_西潘二期Ⅲ-028 主轴温度","西潘风电场","WOF35300077",28,"YQXP.T2_L3.WTG028.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅲ-028 主轴温度","yc_hs_0563","cur_44"]
[2735,"g_西潘二期Ⅲ-029 桨叶1位置给定","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅲ-029 桨叶1位置给定","yc_hs_0563","cur_85"]
[2736,"g_西潘二期Ⅲ-029 桨叶2位置给定","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅲ-029 桨叶2位置给定","yc_hs_0563","cur_86"]
[2737,"g_西潘二期Ⅲ-029 桨叶3位置给定","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅲ-029 桨叶3位置给定","yc_hs_0563","cur_87"]
[2738,"g_西潘二期Ⅲ-029 机舱位置","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅲ-029 机舱位置","yc_hs_0564","cur_20"]
[2739,"g_西潘二期Ⅲ-029 齿轮箱油温","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅲ-029 齿轮箱油温","yc_hs_0564","cur_23"]
[2740,"g_西潘二期Ⅲ-029 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅲ-029 齿轮箱高速轴轴承后端温度","yc_hs_0564","cur_25"]
[2741,"g_西潘二期Ⅲ-029 舱内温度","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅲ-029 舱内温度","yc_hs_0564","cur_29"]
[2742,"g_西潘二期Ⅲ-029 舱外温度","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅲ-029 舱外温度","yc_hs_0564","cur_31"]
[2743,"g_西潘二期Ⅲ-029 发电机转速","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅲ-029 发电机转速","yc_hs_0564","cur_34"]
[2744,"g_西潘二期Ⅲ-029 风轮转速","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅲ-029 风轮转速","yc_hs_0564","cur_35"]
[2745,"g_西潘二期Ⅲ-029 发电机定子L1绕组温度","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅲ-029 发电机定子L1绕组温度","yc_hs_0564","cur_36"]
[2746,"g_西潘二期Ⅲ-029 发电机定子L2绕组温度","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅲ-029 发电机定子L2绕组温度","yc_hs_0564","cur_37"]
[2747,"g_西潘二期Ⅲ-029 发电机定子L3绕组温度","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅲ-029 发电机定子L3绕组温度","yc_hs_0564","cur_38"]
[2748,"g_西潘二期Ⅲ-029 发电机驱动端轴承温度","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅲ-029 发电机驱动端轴承温度","yc_hs_0564","cur_39"]
[2749,"g_西潘二期Ⅲ-029 发电机非驱动端轴承温度","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅲ-029 发电机非驱动端轴承温度","yc_hs_0564","cur_40"]
[2750,"g_西潘二期Ⅲ-029 电网有功功率","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅲ-029 电网有功功率","yc_hs_0564","cur_56"]
[2751,"g_西潘二期Ⅲ-029 实时风速","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅲ-029 实时风速","yc_hs_0564","cur_69"]
[2752,"g_西潘二期Ⅲ-029 对风误差","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅲ-029 对风误差","yc_hs_0564","cur_73"]
[2753,"g_西潘二期Ⅲ-029 3s风向(0-360度)","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅲ-029 3s风向(0-360度)","yc_hs_0564","cur_78"]
[2754,"g_西潘二期Ⅲ-029 主轴温度","西潘风电场","WOF35300077",29,"YQXP.T2_L3.WTG029.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅲ-029 主轴温度","yc_hs_0565","cur_36"]
[2755,"g_西潘二期Ⅲ-030 桨叶1位置给定","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅲ-030 桨叶1位置给定","yc_hs_0565","cur_77"]
[2756,"g_西潘二期Ⅲ-030 桨叶2位置给定","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅲ-030 桨叶2位置给定","yc_hs_0565","cur_78"]
[2757,"g_西潘二期Ⅲ-030 桨叶3位置给定","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅲ-030 桨叶3位置给定","yc_hs_0565","cur_79"]
[2758,"g_西潘二期Ⅲ-030 机舱位置","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅲ-030 机舱位置","yc_hs_0566","cur_12"]
[2759,"g_西潘二期Ⅲ-030 齿轮箱油温","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅲ-030 齿轮箱油温","yc_hs_0566","cur_15"]
[2760,"g_西潘二期Ⅲ-030 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅲ-030 齿轮箱高速轴轴承后端温度","yc_hs_0566","cur_17"]
[2761,"g_西潘二期Ⅲ-030 舱内温度","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅲ-030 舱内温度","yc_hs_0566","cur_21"]
[2762,"g_西潘二期Ⅲ-030 舱外温度","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅲ-030 舱外温度","yc_hs_0566","cur_23"]
[2763,"g_西潘二期Ⅲ-030 发电机转速","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅲ-030 发电机转速","yc_hs_0566","cur_26"]
[2764,"g_西潘二期Ⅲ-030 风轮转速","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅲ-030 风轮转速","yc_hs_0566","cur_27"]
[2765,"g_西潘二期Ⅲ-030 发电机定子L1绕组温度","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅲ-030 发电机定子L1绕组温度","yc_hs_0566","cur_28"]
[2766,"g_西潘二期Ⅲ-030 发电机定子L2绕组温度","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅲ-030 发电机定子L2绕组温度","yc_hs_0566","cur_29"]
[2767,"g_西潘二期Ⅲ-030 发电机定子L3绕组温度","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅲ-030 发电机定子L3绕组温度","yc_hs_0566","cur_30"]
[2768,"g_西潘二期Ⅲ-030 发电机驱动端轴承温度","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅲ-030 发电机驱动端轴承温度","yc_hs_0566","cur_31"]
[2769,"g_西潘二期Ⅲ-030 发电机非驱动端轴承温度","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅲ-030 发电机非驱动端轴承温度","yc_hs_0566","cur_32"]
[2770,"g_西潘二期Ⅲ-030 电网有功功率","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅲ-030 电网有功功率","yc_hs_0566","cur_48"]
[2771,"g_西潘二期Ⅲ-030 实时风速","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅲ-030 实时风速","yc_hs_0566","cur_61"]
[2772,"g_西潘二期Ⅲ-030 对风误差","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅲ-030 对风误差","yc_hs_0566","cur_65"]
[2773,"g_西潘二期Ⅲ-030 3s风向(0-360度)","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅲ-030 3s风向(0-360度)","yc_hs_0566","cur_70"]
[2774,"g_西潘二期Ⅲ-030 主轴温度","西潘风电场","WOF35300077",30,"YQXP.T2_L3.WTG030.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅲ-030 主轴温度","yc_hs_0567","cur_28"]
[2775,"g_西潘二期Ⅲ-031 桨叶1位置给定","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅲ-031 桨叶1位置给定","yc_hs_0567","cur_69"]
[2776,"g_西潘二期Ⅲ-031 桨叶2位置给定","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅲ-031 桨叶2位置给定","yc_hs_0567","cur_70"]
[2777,"g_西潘二期Ⅲ-031 桨叶3位置给定","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅲ-031 桨叶3位置给定","yc_hs_0567","cur_71"]
[2778,"g_西潘二期Ⅲ-031 机舱位置","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅲ-031 机舱位置","yc_hs_0568","cur_04"]
[2779,"g_西潘二期Ⅲ-031 齿轮箱油温","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅲ-031 齿轮箱油温","yc_hs_0568","cur_07"]
[2780,"g_西潘二期Ⅲ-031 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅲ-031 齿轮箱高速轴轴承后端温度","yc_hs_0568","cur_09"]
[2781,"g_西潘二期Ⅲ-031 舱内温度","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅲ-031 舱内温度","yc_hs_0568","cur_13"]
[2782,"g_西潘二期Ⅲ-031 舱外温度","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅲ-031 舱外温度","yc_hs_0568","cur_15"]
[2783,"g_西潘二期Ⅲ-031 发电机转速","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅲ-031 发电机转速","yc_hs_0568","cur_18"]
[2784,"g_西潘二期Ⅲ-031 风轮转速","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅲ-031 风轮转速","yc_hs_0568","cur_19"]
[2785,"g_西潘二期Ⅲ-031 发电机定子L1绕组温度","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅲ-031 发电机定子L1绕组温度","yc_hs_0568","cur_20"]
[2786,"g_西潘二期Ⅲ-031 发电机定子L2绕组温度","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅲ-031 发电机定子L2绕组温度","yc_hs_0568","cur_21"]
[2787,"g_西潘二期Ⅲ-031 发电机定子L3绕组温度","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅲ-031 发电机定子L3绕组温度","yc_hs_0568","cur_22"]
[2788,"g_西潘二期Ⅲ-031 发电机驱动端轴承温度","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅲ-031 发电机驱动端轴承温度","yc_hs_0568","cur_23"]
[2789,"g_西潘二期Ⅲ-031 发电机非驱动端轴承温度","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅲ-031 发电机非驱动端轴承温度","yc_hs_0568","cur_24"]
[2790,"g_西潘二期Ⅲ-031 电网有功功率","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅲ-031 电网有功功率","yc_hs_0568","cur_40"]
[2791,"g_西潘二期Ⅲ-031 实时风速","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅲ-031 实时风速","yc_hs_0568","cur_53"]
[2792,"g_西潘二期Ⅲ-031 对风误差","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅲ-031 对风误差","yc_hs_0568","cur_57"]
[2793,"g_西潘二期Ⅲ-031 3s风向(0-360度)","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅲ-031 3s风向(0-360度)","yc_hs_0568","cur_62"]
[2794,"g_西潘二期Ⅲ-031 主轴温度","西潘风电场","WOF35300077",31,"YQXP.T2_L3.WTG031.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅲ-031 主轴温度","yc_hs_0569","cur_20"]
[2795,"g_西潘二期Ⅲ-032 桨叶1位置给定","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅲ-032 桨叶1位置给定","yc_hs_0569","cur_61"]
[2796,"g_西潘二期Ⅲ-032 桨叶2位置给定","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅲ-032 桨叶2位置给定","yc_hs_0569","cur_62"]
[2797,"g_西潘二期Ⅲ-032 桨叶3位置给定","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅲ-032 桨叶3位置给定","yc_hs_0569","cur_63"]
[2798,"g_西潘二期Ⅲ-032 机舱位置","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅲ-032 机舱位置","yc_hs_0569","cur_96"]
[2799,"g_西潘二期Ⅲ-032 齿轮箱油温","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅲ-032 齿轮箱油温","yc_hs_0569","cur_99"]
[2800,"g_西潘二期Ⅲ-032 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅲ-032 齿轮箱高速轴轴承后端温度","yc_hs_0570","cur_01"]
[2801,"g_西潘二期Ⅲ-032 舱内温度","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅲ-032 舱内温度","yc_hs_0570","cur_05"]
[2802,"g_西潘二期Ⅲ-032 舱外温度","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅲ-032 舱外温度","yc_hs_0570","cur_07"]
[2803,"g_西潘二期Ⅲ-032 发电机转速","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅲ-032 发电机转速","yc_hs_0570","cur_10"]
[2804,"g_西潘二期Ⅲ-032 风轮转速","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅲ-032 风轮转速","yc_hs_0570","cur_11"]
[2805,"g_西潘二期Ⅲ-032 发电机定子L1绕组温度","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅲ-032 发电机定子L1绕组温度","yc_hs_0570","cur_12"]
[2806,"g_西潘二期Ⅲ-032 发电机定子L2绕组温度","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅲ-032 发电机定子L2绕组温度","yc_hs_0570","cur_13"]
[2807,"g_西潘二期Ⅲ-032 发电机定子L3绕组温度","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅲ-032 发电机定子L3绕组温度","yc_hs_0570","cur_14"]
[2808,"g_西潘二期Ⅲ-032 发电机驱动端轴承温度","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅲ-032 发电机驱动端轴承温度","yc_hs_0570","cur_15"]
[2809,"g_西潘二期Ⅲ-032 发电机非驱动端轴承温度","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅲ-032 发电机非驱动端轴承温度","yc_hs_0570","cur_16"]
[2810,"g_西潘二期Ⅲ-032 电网有功功率","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅲ-032 电网有功功率","yc_hs_0570","cur_32"]
[2811,"g_西潘二期Ⅲ-032 实时风速","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅲ-032 实时风速","yc_hs_0570","cur_45"]
[2812,"g_西潘二期Ⅲ-032 对风误差","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅲ-032 对风误差","yc_hs_0570","cur_49"]
[2813,"g_西潘二期Ⅲ-032 3s风向(0-360度)","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅲ-032 3s风向(0-360度)","yc_hs_0570","cur_54"]
[2814,"g_西潘二期Ⅲ-032 主轴温度","西潘风电场","WOF35300077",32,"YQXP.T2_L3.WTG032.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅲ-032 主轴温度","yc_hs_0571","cur_12"]
[2815,"g_西潘二期Ⅳ-034 桨叶1位置给定","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅳ-034 桨叶1位置给定","yc_hs_0571","cur_53"]
[2816,"g_西潘二期Ⅳ-034 桨叶2位置给定","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅳ-034 桨叶2位置给定","yc_hs_0571","cur_54"]
[2817,"g_西潘二期Ⅳ-034 桨叶3位置给定","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅳ-034 桨叶3位置给定","yc_hs_0571","cur_55"]
[2818,"g_西潘二期Ⅳ-034 机舱位置","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅳ-034 机舱位置","yc_hs_0571","cur_88"]
[2819,"g_西潘二期Ⅳ-034 齿轮箱油温","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅳ-034 齿轮箱油温","yc_hs_0571","cur_91"]
[2820,"g_西潘二期Ⅳ-034 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅳ-034 齿轮箱高速轴轴承后端温度","yc_hs_0571","cur_93"]
[2821,"g_西潘二期Ⅳ-034 舱内温度","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅳ-034 舱内温度","yc_hs_0571","cur_97"]
[2822,"g_西潘二期Ⅳ-034 舱外温度","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅳ-034 舱外温度","yc_hs_0571","cur_99"]
[2823,"g_西潘二期Ⅳ-034 发电机转速","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅳ-034 发电机转速","yc_hs_0572","cur_02"]
[2824,"g_西潘二期Ⅳ-034 风轮转速","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅳ-034 风轮转速","yc_hs_0572","cur_03"]
[2825,"g_西潘二期Ⅳ-034 发电机定子L1绕组温度","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅳ-034 发电机定子L1绕组温度","yc_hs_0572","cur_04"]
[2826,"g_西潘二期Ⅳ-034 发电机定子L2绕组温度","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅳ-034 发电机定子L2绕组温度","yc_hs_0572","cur_05"]
[2827,"g_西潘二期Ⅳ-034 发电机定子L3绕组温度","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅳ-034 发电机定子L3绕组温度","yc_hs_0572","cur_06"]
[2828,"g_西潘二期Ⅳ-034 发电机驱动端轴承温度","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅳ-034 发电机驱动端轴承温度","yc_hs_0572","cur_07"]
[2829,"g_西潘二期Ⅳ-034 发电机非驱动端轴承温度","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅳ-034 发电机非驱动端轴承温度","yc_hs_0572","cur_08"]
[2830,"g_西潘二期Ⅳ-034 电网有功功率","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅳ-034 电网有功功率","yc_hs_0572","cur_24"]
[2831,"g_西潘二期Ⅳ-034 实时风速","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅳ-034 实时风速","yc_hs_0572","cur_37"]
[2832,"g_西潘二期Ⅳ-034 对风误差","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅳ-034 对风误差","yc_hs_0572","cur_41"]
[2833,"g_西潘二期Ⅳ-034 3s风向(0-360度)","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅳ-034 3s风向(0-360度)","yc_hs_0572","cur_46"]
[2834,"g_西潘二期Ⅳ-034 主轴温度","西潘风电场","WOF35300077",34,"YQXP.T2_L4.WTG034.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅳ-034 主轴温度","yc_hs_0573","cur_04"]
[2835,"g_西潘二期Ⅳ-035 桨叶1位置给定","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅳ-035 桨叶1位置给定","yc_hs_0573","cur_45"]
[2836,"g_西潘二期Ⅳ-035 桨叶2位置给定","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅳ-035 桨叶2位置给定","yc_hs_0573","cur_46"]
[2837,"g_西潘二期Ⅳ-035 桨叶3位置给定","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅳ-035 桨叶3位置给定","yc_hs_0573","cur_47"]
[2838,"g_西潘二期Ⅳ-035 机舱位置","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅳ-035 机舱位置","yc_hs_0573","cur_80"]
[2839,"g_西潘二期Ⅳ-035 齿轮箱油温","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅳ-035 齿轮箱油温","yc_hs_0573","cur_83"]
[2840,"g_西潘二期Ⅳ-035 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅳ-035 齿轮箱高速轴轴承后端温度","yc_hs_0573","cur_85"]
[2841,"g_西潘二期Ⅳ-035 舱内温度","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅳ-035 舱内温度","yc_hs_0573","cur_89"]
[2842,"g_西潘二期Ⅳ-035 舱外温度","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅳ-035 舱外温度","yc_hs_0573","cur_91"]
[2843,"g_西潘二期Ⅳ-035 发电机转速","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅳ-035 发电机转速","yc_hs_0573","cur_94"]
[2844,"g_西潘二期Ⅳ-035 风轮转速","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅳ-035 风轮转速","yc_hs_0573","cur_95"]
[2845,"g_西潘二期Ⅳ-035 发电机定子L1绕组温度","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅳ-035 发电机定子L1绕组温度","yc_hs_0573","cur_96"]
[2846,"g_西潘二期Ⅳ-035 发电机定子L2绕组温度","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅳ-035 发电机定子L2绕组温度","yc_hs_0573","cur_97"]
[2847,"g_西潘二期Ⅳ-035 发电机定子L3绕组温度","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅳ-035 发电机定子L3绕组温度","yc_hs_0573","cur_98"]
[2848,"g_西潘二期Ⅳ-035 发电机驱动端轴承温度","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅳ-035 发电机驱动端轴承温度","yc_hs_0573","cur_99"]
[2849,"g_西潘二期Ⅳ-035 发电机非驱动端轴承温度","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅳ-035 发电机非驱动端轴承温度","yc_hs_0573","cur_100"]
[2850,"g_西潘二期Ⅳ-035 电网有功功率","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅳ-035 电网有功功率","yc_hs_0574","cur_16"]
[2851,"g_西潘二期Ⅳ-035 实时风速","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅳ-035 实时风速","yc_hs_0574","cur_29"]
[2852,"g_西潘二期Ⅳ-035 对风误差","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅳ-035 对风误差","yc_hs_0574","cur_33"]
[2853,"g_西潘二期Ⅳ-035 3s风向(0-360度)","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅳ-035 3s风向(0-360度)","yc_hs_0574","cur_38"]
[2854,"g_西潘二期Ⅳ-035 主轴温度","西潘风电场","WOF35300077",35,"YQXP.T2_L4.WTG035.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅳ-035 主轴温度","yc_hs_0574","cur_96"]
[2855,"g_西潘二期Ⅳ-036 桨叶1位置给定","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅳ-036 桨叶1位置给定","yc_hs_0575","cur_37"]
[2856,"g_西潘二期Ⅳ-036 桨叶2位置给定","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅳ-036 桨叶2位置给定","yc_hs_0575","cur_38"]
[2857,"g_西潘二期Ⅳ-036 桨叶3位置给定","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅳ-036 桨叶3位置给定","yc_hs_0575","cur_39"]
[2858,"g_西潘二期Ⅳ-036 机舱位置","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅳ-036 机舱位置","yc_hs_0575","cur_72"]
[2859,"g_西潘二期Ⅳ-036 齿轮箱油温","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅳ-036 齿轮箱油温","yc_hs_0575","cur_75"]
[2860,"g_西潘二期Ⅳ-036 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅳ-036 齿轮箱高速轴轴承后端温度","yc_hs_0575","cur_77"]
[2861,"g_西潘二期Ⅳ-036 舱内温度","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅳ-036 舱内温度","yc_hs_0575","cur_81"]
[2862,"g_西潘二期Ⅳ-036 舱外温度","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅳ-036 舱外温度","yc_hs_0575","cur_83"]
[2863,"g_西潘二期Ⅳ-036 发电机转速","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅳ-036 发电机转速","yc_hs_0575","cur_86"]
[2864,"g_西潘二期Ⅳ-036 风轮转速","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅳ-036 风轮转速","yc_hs_0575","cur_87"]
[2865,"g_西潘二期Ⅳ-036 发电机定子L1绕组温度","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅳ-036 发电机定子L1绕组温度","yc_hs_0575","cur_88"]
[2866,"g_西潘二期Ⅳ-036 发电机定子L2绕组温度","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅳ-036 发电机定子L2绕组温度","yc_hs_0575","cur_89"]
[2867,"g_西潘二期Ⅳ-036 发电机定子L3绕组温度","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅳ-036 发电机定子L3绕组温度","yc_hs_0575","cur_90"]
[2868,"g_西潘二期Ⅳ-036 发电机驱动端轴承温度","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅳ-036 发电机驱动端轴承温度","yc_hs_0575","cur_91"]
[2869,"g_西潘二期Ⅳ-036 发电机非驱动端轴承温度","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅳ-036 发电机非驱动端轴承温度","yc_hs_0575","cur_92"]
[2870,"g_西潘二期Ⅳ-036 电网有功功率","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅳ-036 电网有功功率","yc_hs_0576","cur_08"]
[2871,"g_西潘二期Ⅳ-036 实时风速","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅳ-036 实时风速","yc_hs_0576","cur_21"]
[2872,"g_西潘二期Ⅳ-036 对风误差","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅳ-036 对风误差","yc_hs_0576","cur_25"]
[2873,"g_西潘二期Ⅳ-036 3s风向(0-360度)","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅳ-036 3s风向(0-360度)","yc_hs_0576","cur_30"]
[2874,"g_西潘二期Ⅳ-036 主轴温度","西潘风电场","WOF35300077",36,"YQXP.T2_L4.WTG036.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅳ-036 主轴温度","yc_hs_0576","cur_88"]
[2875,"g_西潘二期Ⅳ-037 桨叶1位置给定","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅳ-037 桨叶1位置给定","yc_hs_0577","cur_29"]
[2876,"g_西潘二期Ⅳ-037 桨叶2位置给定","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅳ-037 桨叶2位置给定","yc_hs_0577","cur_30"]
[2877,"g_西潘二期Ⅳ-037 桨叶3位置给定","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅳ-037 桨叶3位置给定","yc_hs_0577","cur_31"]
[2878,"g_西潘二期Ⅳ-037 机舱位置","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅳ-037 机舱位置","yc_hs_0577","cur_64"]
[2879,"g_西潘二期Ⅳ-037 齿轮箱油温","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅳ-037 齿轮箱油温","yc_hs_0577","cur_67"]
[2880,"g_西潘二期Ⅳ-037 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅳ-037 齿轮箱高速轴轴承后端温度","yc_hs_0577","cur_69"]
[2881,"g_西潘二期Ⅳ-037 舱内温度","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅳ-037 舱内温度","yc_hs_0577","cur_73"]
[2882,"g_西潘二期Ⅳ-037 舱外温度","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅳ-037 舱外温度","yc_hs_0577","cur_75"]
[2883,"g_西潘二期Ⅳ-037 发电机转速","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅳ-037 发电机转速","yc_hs_0577","cur_78"]
[2884,"g_西潘二期Ⅳ-037 风轮转速","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅳ-037 风轮转速","yc_hs_0577","cur_79"]
[2885,"g_西潘二期Ⅳ-037 发电机定子L1绕组温度","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅳ-037 发电机定子L1绕组温度","yc_hs_0577","cur_80"]
[2886,"g_西潘二期Ⅳ-037 发电机定子L2绕组温度","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅳ-037 发电机定子L2绕组温度","yc_hs_0577","cur_81"]
[2887,"g_西潘二期Ⅳ-037 发电机定子L3绕组温度","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅳ-037 发电机定子L3绕组温度","yc_hs_0577","cur_82"]
[2888,"g_西潘二期Ⅳ-037 发电机驱动端轴承温度","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅳ-037 发电机驱动端轴承温度","yc_hs_0577","cur_83"]
[2889,"g_西潘二期Ⅳ-037 发电机非驱动端轴承温度","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅳ-037 发电机非驱动端轴承温度","yc_hs_0577","cur_84"]
[2890,"g_西潘二期Ⅳ-037 电网有功功率","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅳ-037 电网有功功率","yc_hs_0577","cur_100"]
[2891,"g_西潘二期Ⅳ-037 实时风速","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅳ-037 实时风速","yc_hs_0578","cur_13"]
[2892,"g_西潘二期Ⅳ-037 对风误差","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅳ-037 对风误差","yc_hs_0578","cur_17"]
[2893,"g_西潘二期Ⅳ-037 3s风向(0-360度)","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅳ-037 3s风向(0-360度)","yc_hs_0578","cur_22"]
[2894,"g_西潘二期Ⅳ-037 主轴温度","西潘风电场","WOF35300077",37,"YQXP.T2_L4.WTG037.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅳ-037 主轴温度","yc_hs_0578","cur_80"]
[2895,"g_西潘二期Ⅳ-038 桨叶1位置给定","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅳ-038 桨叶1位置给定","yc_hs_0579","cur_21"]
[2896,"g_西潘二期Ⅳ-038 桨叶2位置给定","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅳ-038 桨叶2位置给定","yc_hs_0579","cur_22"]
[2897,"g_西潘二期Ⅳ-038 桨叶3位置给定","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅳ-038 桨叶3位置给定","yc_hs_0579","cur_23"]
[2898,"g_西潘二期Ⅳ-038 机舱位置","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅳ-038 机舱位置","yc_hs_0579","cur_56"]
[2899,"g_西潘二期Ⅳ-038 齿轮箱油温","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅳ-038 齿轮箱油温","yc_hs_0579","cur_59"]
[2900,"g_西潘二期Ⅳ-038 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅳ-038 齿轮箱高速轴轴承后端温度","yc_hs_0579","cur_61"]
[2901,"g_西潘二期Ⅳ-038 舱内温度","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅳ-038 舱内温度","yc_hs_0579","cur_65"]
[2902,"g_西潘二期Ⅳ-038 舱外温度","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅳ-038 舱外温度","yc_hs_0579","cur_67"]
[2903,"g_西潘二期Ⅳ-038 发电机转速","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅳ-038 发电机转速","yc_hs_0579","cur_70"]
[2904,"g_西潘二期Ⅳ-038 风轮转速","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅳ-038 风轮转速","yc_hs_0579","cur_71"]
[2905,"g_西潘二期Ⅳ-038 发电机定子L1绕组温度","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅳ-038 发电机定子L1绕组温度","yc_hs_0579","cur_72"]
[2906,"g_西潘二期Ⅳ-038 发电机定子L2绕组温度","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅳ-038 发电机定子L2绕组温度","yc_hs_0579","cur_73"]
[2907,"g_西潘二期Ⅳ-038 发电机定子L3绕组温度","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅳ-038 发电机定子L3绕组温度","yc_hs_0579","cur_74"]
[2908,"g_西潘二期Ⅳ-038 发电机驱动端轴承温度","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅳ-038 发电机驱动端轴承温度","yc_hs_0579","cur_75"]
[2909,"g_西潘二期Ⅳ-038 发电机非驱动端轴承温度","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅳ-038 发电机非驱动端轴承温度","yc_hs_0579","cur_76"]
[2910,"g_西潘二期Ⅳ-038 电网有功功率","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅳ-038 电网有功功率","yc_hs_0579","cur_92"]
[2911,"g_西潘二期Ⅳ-038 实时风速","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅳ-038 实时风速","yc_hs_0580","cur_05"]
[2912,"g_西潘二期Ⅳ-038 对风误差","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅳ-038 对风误差","yc_hs_0580","cur_09"]
[2913,"g_西潘二期Ⅳ-038 3s风向(0-360度)","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅳ-038 3s风向(0-360度)","yc_hs_0580","cur_14"]
[2914,"g_西潘二期Ⅳ-038 主轴温度","西潘风电场","WOF35300077",38,"YQXP.T2_L4.WTG038.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅳ-038 主轴温度","yc_hs_0580","cur_72"]
[2915,"g_西潘二期Ⅳ-039 桨叶1位置给定","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅳ-039 桨叶1位置给定","yc_hs_0581","cur_13"]
[2916,"g_西潘二期Ⅳ-039 桨叶2位置给定","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅳ-039 桨叶2位置给定","yc_hs_0581","cur_14"]
[2917,"g_西潘二期Ⅳ-039 桨叶3位置给定","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅳ-039 桨叶3位置给定","yc_hs_0581","cur_15"]
[2918,"g_西潘二期Ⅳ-039 机舱位置","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅳ-039 机舱位置","yc_hs_0581","cur_48"]
[2919,"g_西潘二期Ⅳ-039 齿轮箱油温","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅳ-039 齿轮箱油温","yc_hs_0581","cur_51"]
[2920,"g_西潘二期Ⅳ-039 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅳ-039 齿轮箱高速轴轴承后端温度","yc_hs_0581","cur_53"]
[2921,"g_西潘二期Ⅳ-039 舱内温度","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅳ-039 舱内温度","yc_hs_0581","cur_57"]
[2922,"g_西潘二期Ⅳ-039 舱外温度","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅳ-039 舱外温度","yc_hs_0581","cur_59"]
[2923,"g_西潘二期Ⅳ-039 发电机转速","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅳ-039 发电机转速","yc_hs_0581","cur_62"]
[2924,"g_西潘二期Ⅳ-039 风轮转速","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅳ-039 风轮转速","yc_hs_0581","cur_63"]
[2925,"g_西潘二期Ⅳ-039 发电机定子L1绕组温度","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅳ-039 发电机定子L1绕组温度","yc_hs_0581","cur_64"]
[2926,"g_西潘二期Ⅳ-039 发电机定子L2绕组温度","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅳ-039 发电机定子L2绕组温度","yc_hs_0581","cur_65"]
[2927,"g_西潘二期Ⅳ-039 发电机定子L3绕组温度","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅳ-039 发电机定子L3绕组温度","yc_hs_0581","cur_66"]
[2928,"g_西潘二期Ⅳ-039 发电机驱动端轴承温度","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅳ-039 发电机驱动端轴承温度","yc_hs_0581","cur_67"]
[2929,"g_西潘二期Ⅳ-039 发电机非驱动端轴承温度","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅳ-039 发电机非驱动端轴承温度","yc_hs_0581","cur_68"]
[2930,"g_西潘二期Ⅳ-039 电网有功功率","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅳ-039 电网有功功率","yc_hs_0581","cur_84"]
[2931,"g_西潘二期Ⅳ-039 实时风速","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅳ-039 实时风速","yc_hs_0581","cur_97"]
[2932,"g_西潘二期Ⅳ-039 对风误差","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅳ-039 对风误差","yc_hs_0582","cur_01"]
[2933,"g_西潘二期Ⅳ-039 3s风向(0-360度)","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅳ-039 3s风向(0-360度)","yc_hs_0582","cur_06"]
[2934,"g_西潘二期Ⅳ-039 主轴温度","西潘风电场","WOF35300077",39,"YQXP.T2_L4.WTG039.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅳ-039 主轴温度","yc_hs_0582","cur_64"]
[2935,"g_西潘二期Ⅳ-040 桨叶1位置给定","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WROT.Blade1PositionGiven","桨距角1","pitch_angle_blade_1","g_西潘二期Ⅳ-040 桨叶1位置给定","yc_hs_0583","cur_05"]
[2936,"g_西潘二期Ⅳ-040 桨叶2位置给定","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WROT.Blade2PositionGiven","桨距角2","pitch_angle_blade_2","g_西潘二期Ⅳ-040 桨叶2位置给定","yc_hs_0583","cur_06"]
[2937,"g_西潘二期Ⅳ-040 桨叶3位置给定","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WROT.Blade3PositionGiven","桨距角3","pitch_angle_blade_3","g_西潘二期Ⅳ-040 桨叶3位置给定","yc_hs_0583","cur_07"]
[2938,"g_西潘二期Ⅳ-040 机舱位置","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WYAW.NacellePosition","机舱位置","cabin_position","g_西潘二期Ⅳ-040 机舱位置","yc_hs_0583","cur_40"]
[2939,"g_西潘二期Ⅳ-040 齿轮箱油温","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","g_西潘二期Ⅳ-040 齿轮箱油温","yc_hs_0583","cur_43"]
[2940,"g_西潘二期Ⅳ-040 齿轮箱高速轴轴承后端温度","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","g_西潘二期Ⅳ-040 齿轮箱高速轴轴承后端温度","yc_hs_0583","cur_45"]
[2941,"g_西潘二期Ⅳ-040 舱内温度","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WNAC.HumNacelle","机舱内温度","cabin_temperature","g_西潘二期Ⅳ-040 舱内温度","yc_hs_0583","cur_49"]
[2942,"g_西潘二期Ⅳ-040 舱外温度","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WNAC.TemOut","环境温度","outside_cabin_temperature","g_西潘二期Ⅳ-040 舱外温度","yc_hs_0583","cur_51"]
[2943,"g_西潘二期Ⅳ-040 发电机转速","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WGEN.GenSpd","发电机转速","generator_speed","g_西潘二期Ⅳ-040 发电机转速","yc_hs_0583","cur_54"]
[2944,"g_西潘二期Ⅳ-040 风轮转速","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WTRM.RotorSpd","风轮转速","rotor_speed","g_西潘二期Ⅳ-040 风轮转速","yc_hs_0583","cur_55"]
[2945,"g_西潘二期Ⅳ-040 发电机定子L1绕组温度","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WGEN.TemWindingL1","发电机绕组1温度","generator_winding1_temperature","g_西潘二期Ⅳ-040 发电机定子L1绕组温度","yc_hs_0583","cur_56"]
[2946,"g_西潘二期Ⅳ-040 发电机定子L2绕组温度","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WGEN.TemWindingL2","发电机绕组2温度","generator_winding2_temperature","g_西潘二期Ⅳ-040 发电机定子L2绕组温度","yc_hs_0583","cur_57"]
[2947,"g_西潘二期Ⅳ-040 发电机定子L3绕组温度","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WGEN.TemWindingL3","发电机绕组3温度","generator_winding3_temperature","g_西潘二期Ⅳ-040 发电机定子L3绕组温度","yc_hs_0583","cur_58"]
[2948,"g_西潘二期Ⅳ-040 发电机驱动端轴承温度","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","g_西潘二期Ⅳ-040 发电机驱动端轴承温度","yc_hs_0583","cur_59"]
[2949,"g_西潘二期Ⅳ-040 发电机非驱动端轴承温度","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","g_西潘二期Ⅳ-040 发电机非驱动端轴承温度","yc_hs_0583","cur_60"]
[2950,"g_西潘二期Ⅳ-040 电网有功功率","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WGEN.GenActivePW","有功功率","active_power","g_西潘二期Ⅳ-040 电网有功功率","yc_hs_0583","cur_76"]
[2951,"g_西潘二期Ⅳ-040 实时风速","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WNAC.WindSpeed","风速","wind_velocity","g_西潘二期Ⅳ-040 实时风速","yc_hs_0583","cur_89"]
[2952,"g_西潘二期Ⅳ-040 对风误差","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WNAC.WindVaneDevia","对风角度","yaw_error1","g_西潘二期Ⅳ-040 对风误差","yc_hs_0583","cur_93"]
[2953,"g_西潘二期Ⅳ-040 3s风向(0-360度)","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WNAC.WindDirection3S","绝对风向","true_wind_direction","g_西潘二期Ⅳ-040 3s风向(0-360度)","yc_hs_0583","cur_98"]
[2954,"g_西潘二期Ⅳ-040 主轴温度","西潘风电场","WOF35300077",40,"YQXP.T2_L4.WTG040.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","g_西潘二期Ⅳ-040 主轴温度","yc_hs_0584","cur_56"]
[2955,"a_马家梁二期Ⅲ-026 有功功率","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅲ-026 有功功率","yc_hs_0586","cur_01"]
[2956,"a_马家梁二期Ⅲ-026 瞬时风速","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅲ-026 瞬时风速","yc_hs_0586","cur_11"]
[2957,"a_马家梁二期Ⅲ-026 风向角","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅲ-026 风向角","yc_hs_0586","cur_13"]
[2958,"a_马家梁二期Ⅲ-026 风轮转速","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅲ-026 风轮转速","yc_hs_0586","cur_14"]
[2959,"a_马家梁二期Ⅲ-026 桨距角1","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅲ-026 桨距角1","yc_hs_0586","cur_17"]
[2960,"a_马家梁二期Ⅲ-026 桨距角2","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅲ-026 桨距角2","yc_hs_0586","cur_18"]
[2961,"a_马家梁二期Ⅲ-026 桨距角3","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅲ-026 桨距角3","yc_hs_0586","cur_19"]
[2962,"a_马家梁二期Ⅲ-026 发电机转速","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅲ-026 发电机转速","yc_hs_0586","cur_20"]
[2963,"a_马家梁二期Ⅲ-026 发电机定子U温度","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅲ-026 发电机定子U温度","yc_hs_0586","cur_21"]
[2964,"a_马家梁二期Ⅲ-026 发电机定子V温度","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅲ-026 发电机定子V温度","yc_hs_0586","cur_22"]
[2965,"a_马家梁二期Ⅲ-026 发电机定子W温度","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅲ-026 发电机定子W温度","yc_hs_0586","cur_23"]
[2966,"a_马家梁二期Ⅲ-026 机舱位置","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅲ-026 机舱位置","yc_hs_0586","cur_25"]
[2967,"a_马家梁二期Ⅲ-026 自由端轴承温度","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅲ-026 自由端轴承温度","yc_hs_0586","cur_26"]
[2968,"a_马家梁二期Ⅲ-026 驱动端轴承温度","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅲ-026 驱动端轴承温度","yc_hs_0586","cur_27"]
[2969,"a_马家梁二期Ⅲ-026 高速轴承温度","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅲ-026 高速轴承温度","yc_hs_0586","cur_28"]
[2970,"a_马家梁二期Ⅲ-026 齿轮箱油温","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅲ-026 齿轮箱油温","yc_hs_0586","cur_30"]
[2971,"a_马家梁二期Ⅲ-026 舱外温度","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅲ-026 舱外温度","yc_hs_0586","cur_35"]
[2972,"a_马家梁二期Ⅲ-026 舱内温度","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅲ-026 舱内温度","yc_hs_0586","cur_36"]
[2973,"a_马家梁二期Ⅲ-026 机舱X方向振动加速度","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅲ-026 机舱X方向振动加速度","yc_hs_0586","cur_40"]
[2974,"a_马家梁二期Ⅲ-026 机舱振动有效值","马家梁风电场","WOF35200074",26,"MJLFD.T2_L3.WTG026.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅲ-026 机舱振动有效值","yc_hs_0586","cur_42"]
[2975,"a_马家梁二期Ⅲ-027 有功功率","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅲ-027 有功功率","yc_hs_0587","cur_13"]
[2976,"a_马家梁二期Ⅲ-027 瞬时风速","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅲ-027 瞬时风速","yc_hs_0587","cur_23"]
[2977,"a_马家梁二期Ⅲ-027 风向角","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅲ-027 风向角","yc_hs_0587","cur_25"]
[2978,"a_马家梁二期Ⅲ-027 风轮转速","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅲ-027 风轮转速","yc_hs_0587","cur_26"]
[2979,"a_马家梁二期Ⅲ-027 桨距角1","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅲ-027 桨距角1","yc_hs_0587","cur_29"]
[2980,"a_马家梁二期Ⅲ-027 桨距角2","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅲ-027 桨距角2","yc_hs_0587","cur_30"]
[2981,"a_马家梁二期Ⅲ-027 桨距角3","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅲ-027 桨距角3","yc_hs_0587","cur_31"]
[2982,"a_马家梁二期Ⅲ-027 发电机转速","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅲ-027 发电机转速","yc_hs_0587","cur_32"]
[2983,"a_马家梁二期Ⅲ-027 发电机定子U温度","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅲ-027 发电机定子U温度","yc_hs_0587","cur_33"]
[2984,"a_马家梁二期Ⅲ-027 发电机定子V温度","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅲ-027 发电机定子V温度","yc_hs_0587","cur_34"]
[2985,"a_马家梁二期Ⅲ-027 发电机定子W温度","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅲ-027 发电机定子W温度","yc_hs_0587","cur_35"]
[2986,"a_马家梁二期Ⅲ-027 机舱位置","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅲ-027 机舱位置","yc_hs_0587","cur_37"]
[2987,"a_马家梁二期Ⅲ-027 自由端轴承温度","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅲ-027 自由端轴承温度","yc_hs_0587","cur_38"]
[2988,"a_马家梁二期Ⅲ-027 驱动端轴承温度","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅲ-027 驱动端轴承温度","yc_hs_0587","cur_39"]
[2989,"a_马家梁二期Ⅲ-027 高速轴承温度","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅲ-027 高速轴承温度","yc_hs_0587","cur_40"]
[2990,"a_马家梁二期Ⅲ-027 齿轮箱油温","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅲ-027 齿轮箱油温","yc_hs_0587","cur_42"]
[2991,"a_马家梁二期Ⅲ-027 舱外温度","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅲ-027 舱外温度","yc_hs_0587","cur_47"]
[2992,"a_马家梁二期Ⅲ-027 舱内温度","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅲ-027 舱内温度","yc_hs_0587","cur_48"]
[2993,"a_马家梁二期Ⅲ-027 机舱X方向振动加速度","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅲ-027 机舱X方向振动加速度","yc_hs_0587","cur_52"]
[2994,"a_马家梁二期Ⅲ-027 机舱振动有效值","马家梁风电场","WOF35200074",27,"MJLFD.T2_L3.WTG027.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅲ-027 机舱振动有效值","yc_hs_0587","cur_54"]
[2995,"a_马家梁二期Ⅲ-028 有功功率","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅲ-028 有功功率","yc_hs_0588","cur_25"]
[2996,"a_马家梁二期Ⅲ-028 瞬时风速","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅲ-028 瞬时风速","yc_hs_0588","cur_35"]
[2997,"a_马家梁二期Ⅲ-028 风向角","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅲ-028 风向角","yc_hs_0588","cur_37"]
[2998,"a_马家梁二期Ⅲ-028 风轮转速","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅲ-028 风轮转速","yc_hs_0588","cur_38"]
[2999,"a_马家梁二期Ⅲ-028 桨距角1","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅲ-028 桨距角1","yc_hs_0588","cur_41"]
[3000,"a_马家梁二期Ⅲ-028 桨距角2","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅲ-028 桨距角2","yc_hs_0588","cur_42"]
[3001,"a_马家梁二期Ⅲ-028 桨距角3","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅲ-028 桨距角3","yc_hs_0588","cur_43"]
[3002,"a_马家梁二期Ⅲ-028 发电机转速","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅲ-028 发电机转速","yc_hs_0588","cur_44"]
[3003,"a_马家梁二期Ⅲ-028 发电机定子U温度","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅲ-028 发电机定子U温度","yc_hs_0588","cur_45"]
[3004,"a_马家梁二期Ⅲ-028 发电机定子V温度","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅲ-028 发电机定子V温度","yc_hs_0588","cur_46"]
[3005,"a_马家梁二期Ⅲ-028 发电机定子W温度","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅲ-028 发电机定子W温度","yc_hs_0588","cur_47"]
[3006,"a_马家梁二期Ⅲ-028 机舱位置","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅲ-028 机舱位置","yc_hs_0588","cur_49"]
[3007,"a_马家梁二期Ⅲ-028 自由端轴承温度","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅲ-028 自由端轴承温度","yc_hs_0588","cur_50"]
[3008,"a_马家梁二期Ⅲ-028 驱动端轴承温度","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅲ-028 驱动端轴承温度","yc_hs_0588","cur_51"]
[3009,"a_马家梁二期Ⅲ-028 高速轴承温度","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅲ-028 高速轴承温度","yc_hs_0588","cur_52"]
[3010,"a_马家梁二期Ⅲ-028 齿轮箱油温","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅲ-028 齿轮箱油温","yc_hs_0588","cur_54"]
[3011,"a_马家梁二期Ⅲ-028 舱外温度","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅲ-028 舱外温度","yc_hs_0588","cur_59"]
[3012,"a_马家梁二期Ⅲ-028 舱内温度","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅲ-028 舱内温度","yc_hs_0588","cur_60"]
[3013,"a_马家梁二期Ⅲ-028 机舱X方向振动加速度","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅲ-028 机舱X方向振动加速度","yc_hs_0588","cur_64"]
[3014,"a_马家梁二期Ⅲ-028 机舱振动有效值","马家梁风电场","WOF35200074",28,"MJLFD.T2_L3.WTG028.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅲ-028 机舱振动有效值","yc_hs_0588","cur_66"]
[3015,"a_马家梁二期Ⅲ-029 有功功率","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅲ-029 有功功率","yc_hs_0589","cur_37"]
[3016,"a_马家梁二期Ⅲ-029 瞬时风速","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅲ-029 瞬时风速","yc_hs_0589","cur_47"]
[3017,"a_马家梁二期Ⅲ-029 风向角","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅲ-029 风向角","yc_hs_0589","cur_49"]
[3018,"a_马家梁二期Ⅲ-029 风轮转速","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅲ-029 风轮转速","yc_hs_0589","cur_50"]
[3019,"a_马家梁二期Ⅲ-029 桨距角1","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅲ-029 桨距角1","yc_hs_0589","cur_53"]
[3020,"a_马家梁二期Ⅲ-029 桨距角2","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅲ-029 桨距角2","yc_hs_0589","cur_54"]
[3021,"a_马家梁二期Ⅲ-029 桨距角3","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅲ-029 桨距角3","yc_hs_0589","cur_55"]
[3022,"a_马家梁二期Ⅲ-029 发电机转速","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅲ-029 发电机转速","yc_hs_0589","cur_56"]
[3023,"a_马家梁二期Ⅲ-029 发电机定子U温度","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅲ-029 发电机定子U温度","yc_hs_0589","cur_57"]
[3024,"a_马家梁二期Ⅲ-029 发电机定子V温度","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅲ-029 发电机定子V温度","yc_hs_0589","cur_58"]
[3025,"a_马家梁二期Ⅲ-029 发电机定子W温度","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅲ-029 发电机定子W温度","yc_hs_0589","cur_59"]
[3026,"a_马家梁二期Ⅲ-029 机舱位置","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅲ-029 机舱位置","yc_hs_0589","cur_61"]
[3027,"a_马家梁二期Ⅲ-029 自由端轴承温度","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅲ-029 自由端轴承温度","yc_hs_0589","cur_62"]
[3028,"a_马家梁二期Ⅲ-029 驱动端轴承温度","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅲ-029 驱动端轴承温度","yc_hs_0589","cur_63"]
[3029,"a_马家梁二期Ⅲ-029 高速轴承温度","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅲ-029 高速轴承温度","yc_hs_0589","cur_64"]
[3030,"a_马家梁二期Ⅲ-029 齿轮箱油温","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅲ-029 齿轮箱油温","yc_hs_0589","cur_66"]
[3031,"a_马家梁二期Ⅲ-029 舱外温度","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅲ-029 舱外温度","yc_hs_0589","cur_71"]
[3032,"a_马家梁二期Ⅲ-029 舱内温度","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅲ-029 舱内温度","yc_hs_0589","cur_72"]
[3033,"a_马家梁二期Ⅲ-029 机舱X方向振动加速度","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅲ-029 机舱X方向振动加速度","yc_hs_0589","cur_76"]
[3034,"a_马家梁二期Ⅲ-029 机舱振动有效值","马家梁风电场","WOF35200074",29,"MJLFD.T2_L3.WTG029.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅲ-029 机舱振动有效值","yc_hs_0589","cur_78"]
[3035,"a_马家梁二期Ⅲ-030 有功功率","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅲ-030 有功功率","yc_hs_0590","cur_49"]
[3036,"a_马家梁二期Ⅲ-030 瞬时风速","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅲ-030 瞬时风速","yc_hs_0590","cur_59"]
[3037,"a_马家梁二期Ⅲ-030 风向角","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅲ-030 风向角","yc_hs_0590","cur_61"]
[3038,"a_马家梁二期Ⅲ-030 风轮转速","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅲ-030 风轮转速","yc_hs_0590","cur_62"]
[3039,"a_马家梁二期Ⅲ-030 桨距角1","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅲ-030 桨距角1","yc_hs_0590","cur_65"]
[3040,"a_马家梁二期Ⅲ-030 桨距角2","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅲ-030 桨距角2","yc_hs_0590","cur_66"]
[3041,"a_马家梁二期Ⅲ-030 桨距角3","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅲ-030 桨距角3","yc_hs_0590","cur_67"]
[3042,"a_马家梁二期Ⅲ-030 发电机转速","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅲ-030 发电机转速","yc_hs_0590","cur_68"]
[3043,"a_马家梁二期Ⅲ-030 发电机定子U温度","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅲ-030 发电机定子U温度","yc_hs_0590","cur_69"]
[3044,"a_马家梁二期Ⅲ-030 发电机定子V温度","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅲ-030 发电机定子V温度","yc_hs_0590","cur_70"]
[3045,"a_马家梁二期Ⅲ-030 发电机定子W温度","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅲ-030 发电机定子W温度","yc_hs_0590","cur_71"]
[3046,"a_马家梁二期Ⅲ-030 机舱位置","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅲ-030 机舱位置","yc_hs_0590","cur_73"]
[3047,"a_马家梁二期Ⅲ-030 自由端轴承温度","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅲ-030 自由端轴承温度","yc_hs_0590","cur_74"]
[3048,"a_马家梁二期Ⅲ-030 驱动端轴承温度","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅲ-030 驱动端轴承温度","yc_hs_0590","cur_75"]
[3049,"a_马家梁二期Ⅲ-030 高速轴承温度","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅲ-030 高速轴承温度","yc_hs_0590","cur_76"]
[3050,"a_马家梁二期Ⅲ-030 齿轮箱油温","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅲ-030 齿轮箱油温","yc_hs_0590","cur_78"]
[3051,"a_马家梁二期Ⅲ-030 舱外温度","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅲ-030 舱外温度","yc_hs_0590","cur_83"]
[3052,"a_马家梁二期Ⅲ-030 舱内温度","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅲ-030 舱内温度","yc_hs_0590","cur_84"]
[3053,"a_马家梁二期Ⅲ-030 机舱X方向振动加速度","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅲ-030 机舱X方向振动加速度","yc_hs_0590","cur_88"]
[3054,"a_马家梁二期Ⅲ-030 机舱振动有效值","马家梁风电场","WOF35200074",30,"MJLFD.T2_L3.WTG030.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅲ-030 机舱振动有效值","yc_hs_0590","cur_90"]
[3055,"a_马家梁二期Ⅲ-031 有功功率","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅲ-031 有功功率","yc_hs_0591","cur_61"]
[3056,"a_马家梁二期Ⅲ-031 瞬时风速","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅲ-031 瞬时风速","yc_hs_0591","cur_71"]
[3057,"a_马家梁二期Ⅲ-031 风向角","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅲ-031 风向角","yc_hs_0591","cur_73"]
[3058,"a_马家梁二期Ⅲ-031 风轮转速","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅲ-031 风轮转速","yc_hs_0591","cur_74"]
[3059,"a_马家梁二期Ⅲ-031 桨距角1","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅲ-031 桨距角1","yc_hs_0591","cur_77"]
[3060,"a_马家梁二期Ⅲ-031 桨距角2","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅲ-031 桨距角2","yc_hs_0591","cur_78"]
[3061,"a_马家梁二期Ⅲ-031 桨距角3","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅲ-031 桨距角3","yc_hs_0591","cur_79"]
[3062,"a_马家梁二期Ⅲ-031 发电机转速","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅲ-031 发电机转速","yc_hs_0591","cur_80"]
[3063,"a_马家梁二期Ⅲ-031 发电机定子U温度","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅲ-031 发电机定子U温度","yc_hs_0591","cur_81"]
[3064,"a_马家梁二期Ⅲ-031 发电机定子V温度","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅲ-031 发电机定子V温度","yc_hs_0591","cur_82"]
[3065,"a_马家梁二期Ⅲ-031 发电机定子W温度","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅲ-031 发电机定子W温度","yc_hs_0591","cur_83"]
[3066,"a_马家梁二期Ⅲ-031 机舱位置","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅲ-031 机舱位置","yc_hs_0591","cur_85"]
[3067,"a_马家梁二期Ⅲ-031 自由端轴承温度","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅲ-031 自由端轴承温度","yc_hs_0591","cur_86"]
[3068,"a_马家梁二期Ⅲ-031 驱动端轴承温度","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅲ-031 驱动端轴承温度","yc_hs_0591","cur_87"]
[3069,"a_马家梁二期Ⅲ-031 高速轴承温度","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅲ-031 高速轴承温度","yc_hs_0591","cur_88"]
[3070,"a_马家梁二期Ⅲ-031 齿轮箱油温","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅲ-031 齿轮箱油温","yc_hs_0591","cur_90"]
[3071,"a_马家梁二期Ⅲ-031 舱外温度","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅲ-031 舱外温度","yc_hs_0591","cur_95"]
[3072,"a_马家梁二期Ⅲ-031 舱内温度","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅲ-031 舱内温度","yc_hs_0591","cur_96"]
[3073,"a_马家梁二期Ⅲ-031 机舱X方向振动加速度","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅲ-031 机舱X方向振动加速度","yc_hs_0591","cur_100"]
[3074,"a_马家梁二期Ⅲ-031 机舱振动有效值","马家梁风电场","WOF35200074",31,"MJLFD.T2_L3.WTG031.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅲ-031 机舱振动有效值","yc_hs_0592","cur_02"]
[3075,"a_马家梁二期Ⅲ-032 有功功率","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅲ-032 有功功率","yc_hs_0592","cur_73"]
[3076,"a_马家梁二期Ⅲ-032 瞬时风速","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅲ-032 瞬时风速","yc_hs_0592","cur_83"]
[3077,"a_马家梁二期Ⅲ-032 风向角","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅲ-032 风向角","yc_hs_0592","cur_85"]
[3078,"a_马家梁二期Ⅲ-032 风轮转速","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅲ-032 风轮转速","yc_hs_0592","cur_86"]
[3079,"a_马家梁二期Ⅲ-032 桨距角1","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅲ-032 桨距角1","yc_hs_0592","cur_89"]
[3080,"a_马家梁二期Ⅲ-032 桨距角2","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅲ-032 桨距角2","yc_hs_0592","cur_90"]
[3081,"a_马家梁二期Ⅲ-032 桨距角3","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅲ-032 桨距角3","yc_hs_0592","cur_91"]
[3082,"a_马家梁二期Ⅲ-032 发电机转速","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅲ-032 发电机转速","yc_hs_0592","cur_92"]
[3083,"a_马家梁二期Ⅲ-032 发电机定子U温度","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅲ-032 发电机定子U温度","yc_hs_0592","cur_93"]
[3084,"a_马家梁二期Ⅲ-032 发电机定子V温度","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅲ-032 发电机定子V温度","yc_hs_0592","cur_94"]
[3085,"a_马家梁二期Ⅲ-032 发电机定子W温度","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅲ-032 发电机定子W温度","yc_hs_0592","cur_95"]
[3086,"a_马家梁二期Ⅲ-032 机舱位置","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅲ-032 机舱位置","yc_hs_0592","cur_97"]
[3087,"a_马家梁二期Ⅲ-032 自由端轴承温度","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅲ-032 自由端轴承温度","yc_hs_0592","cur_98"]
[3088,"a_马家梁二期Ⅲ-032 驱动端轴承温度","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅲ-032 驱动端轴承温度","yc_hs_0592","cur_99"]
[3089,"a_马家梁二期Ⅲ-032 高速轴承温度","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅲ-032 高速轴承温度","yc_hs_0592","cur_100"]
[3090,"a_马家梁二期Ⅲ-032 齿轮箱油温","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅲ-032 齿轮箱油温","yc_hs_0593","cur_02"]
[3091,"a_马家梁二期Ⅲ-032 舱外温度","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅲ-032 舱外温度","yc_hs_0593","cur_07"]
[3092,"a_马家梁二期Ⅲ-032 舱内温度","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅲ-032 舱内温度","yc_hs_0593","cur_08"]
[3093,"a_马家梁二期Ⅲ-032 机舱X方向振动加速度","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅲ-032 机舱X方向振动加速度","yc_hs_0593","cur_12"]
[3094,"a_马家梁二期Ⅲ-032 机舱振动有效值","马家梁风电场","WOF35200074",32,"MJLFD.T2_L3.WTG032.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅲ-032 机舱振动有效值","yc_hs_0593","cur_14"]
[3095,"a_马家梁二期Ⅲ-033 有功功率","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅲ-033 有功功率","yc_hs_0593","cur_85"]
[3096,"a_马家梁二期Ⅲ-033 瞬时风速","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅲ-033 瞬时风速","yc_hs_0593","cur_95"]
[3097,"a_马家梁二期Ⅲ-033 风向角","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅲ-033 风向角","yc_hs_0593","cur_97"]
[3098,"a_马家梁二期Ⅲ-033 风轮转速","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅲ-033 风轮转速","yc_hs_0593","cur_98"]
[3099,"a_马家梁二期Ⅲ-033 桨距角1","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅲ-033 桨距角1","yc_hs_0594","cur_01"]
[3100,"a_马家梁二期Ⅲ-033 桨距角2","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅲ-033 桨距角2","yc_hs_0594","cur_02"]
[3101,"a_马家梁二期Ⅲ-033 桨距角3","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅲ-033 桨距角3","yc_hs_0594","cur_03"]
[3102,"a_马家梁二期Ⅲ-033 发电机转速","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅲ-033 发电机转速","yc_hs_0594","cur_04"]
[3103,"a_马家梁二期Ⅲ-033 发电机定子U温度","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅲ-033 发电机定子U温度","yc_hs_0594","cur_05"]
[3104,"a_马家梁二期Ⅲ-033 发电机定子V温度","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅲ-033 发电机定子V温度","yc_hs_0594","cur_06"]
[3105,"a_马家梁二期Ⅲ-033 发电机定子W温度","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅲ-033 发电机定子W温度","yc_hs_0594","cur_07"]
[3106,"a_马家梁二期Ⅲ-033 机舱位置","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅲ-033 机舱位置","yc_hs_0594","cur_09"]
[3107,"a_马家梁二期Ⅲ-033 自由端轴承温度","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅲ-033 自由端轴承温度","yc_hs_0594","cur_10"]
[3108,"a_马家梁二期Ⅲ-033 驱动端轴承温度","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅲ-033 驱动端轴承温度","yc_hs_0594","cur_11"]
[3109,"a_马家梁二期Ⅲ-033 高速轴承温度","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅲ-033 高速轴承温度","yc_hs_0594","cur_12"]
[3110,"a_马家梁二期Ⅲ-033 齿轮箱油温","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅲ-033 齿轮箱油温","yc_hs_0594","cur_14"]
[3111,"a_马家梁二期Ⅲ-033 舱外温度","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅲ-033 舱外温度","yc_hs_0594","cur_19"]
[3112,"a_马家梁二期Ⅲ-033 舱内温度","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅲ-033 舱内温度","yc_hs_0594","cur_20"]
[3113,"a_马家梁二期Ⅲ-033 机舱X方向振动加速度","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅲ-033 机舱X方向振动加速度","yc_hs_0594","cur_24"]
[3114,"a_马家梁二期Ⅲ-033 机舱振动有效值","马家梁风电场","WOF35200074",33,"MJLFD.T2_L3.WTG033.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅲ-033 机舱振动有效值","yc_hs_0594","cur_26"]
[3115,"a_马家梁二期Ⅲ-034 有功功率","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅲ-034 有功功率","yc_hs_0594","cur_97"]
[3116,"a_马家梁二期Ⅲ-034 瞬时风速","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅲ-034 瞬时风速","yc_hs_0595","cur_07"]
[3117,"a_马家梁二期Ⅲ-034 风向角","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅲ-034 风向角","yc_hs_0595","cur_09"]
[3118,"a_马家梁二期Ⅲ-034 风轮转速","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅲ-034 风轮转速","yc_hs_0595","cur_10"]
[3119,"a_马家梁二期Ⅲ-034 桨距角1","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅲ-034 桨距角1","yc_hs_0595","cur_13"]
[3120,"a_马家梁二期Ⅲ-034 桨距角2","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅲ-034 桨距角2","yc_hs_0595","cur_14"]
[3121,"a_马家梁二期Ⅲ-034 桨距角3","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅲ-034 桨距角3","yc_hs_0595","cur_15"]
[3122,"a_马家梁二期Ⅲ-034 发电机转速","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅲ-034 发电机转速","yc_hs_0595","cur_16"]
[3123,"a_马家梁二期Ⅲ-034 发电机定子U温度","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅲ-034 发电机定子U温度","yc_hs_0595","cur_17"]
[3124,"a_马家梁二期Ⅲ-034 发电机定子V温度","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅲ-034 发电机定子V温度","yc_hs_0595","cur_18"]
[3125,"a_马家梁二期Ⅲ-034 发电机定子W温度","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅲ-034 发电机定子W温度","yc_hs_0595","cur_19"]
[3126,"a_马家梁二期Ⅲ-034 机舱位置","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅲ-034 机舱位置","yc_hs_0595","cur_21"]
[3127,"a_马家梁二期Ⅲ-034 自由端轴承温度","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅲ-034 自由端轴承温度","yc_hs_0595","cur_22"]
[3128,"a_马家梁二期Ⅲ-034 驱动端轴承温度","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅲ-034 驱动端轴承温度","yc_hs_0595","cur_23"]
[3129,"a_马家梁二期Ⅲ-034 高速轴承温度","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅲ-034 高速轴承温度","yc_hs_0595","cur_24"]
[3130,"a_马家梁二期Ⅲ-034 齿轮箱油温","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅲ-034 齿轮箱油温","yc_hs_0595","cur_26"]
[3131,"a_马家梁二期Ⅲ-034 舱外温度","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅲ-034 舱外温度","yc_hs_0595","cur_31"]
[3132,"a_马家梁二期Ⅲ-034 舱内温度","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅲ-034 舱内温度","yc_hs_0595","cur_32"]
[3133,"a_马家梁二期Ⅲ-034 机舱X方向振动加速度","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅲ-034 机舱X方向振动加速度","yc_hs_0595","cur_36"]
[3134,"a_马家梁二期Ⅲ-034 机舱振动有效值","马家梁风电场","WOF35200074",34,"MJLFD.T2_L3.WTG034.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅲ-034 机舱振动有效值","yc_hs_0595","cur_38"]
[3135,"a_马家梁二期Ⅲ-035 有功功率","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅲ-035 有功功率","yc_hs_0596","cur_09"]
[3136,"a_马家梁二期Ⅲ-035 瞬时风速","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅲ-035 瞬时风速","yc_hs_0596","cur_19"]
[3137,"a_马家梁二期Ⅲ-035 风向角","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅲ-035 风向角","yc_hs_0596","cur_21"]
[3138,"a_马家梁二期Ⅲ-035 风轮转速","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅲ-035 风轮转速","yc_hs_0596","cur_22"]
[3139,"a_马家梁二期Ⅲ-035 桨距角1","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅲ-035 桨距角1","yc_hs_0596","cur_25"]
[3140,"a_马家梁二期Ⅲ-035 桨距角2","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅲ-035 桨距角2","yc_hs_0596","cur_26"]
[3141,"a_马家梁二期Ⅲ-035 桨距角3","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅲ-035 桨距角3","yc_hs_0596","cur_27"]
[3142,"a_马家梁二期Ⅲ-035 发电机转速","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅲ-035 发电机转速","yc_hs_0596","cur_28"]
[3143,"a_马家梁二期Ⅲ-035 发电机定子U温度","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅲ-035 发电机定子U温度","yc_hs_0596","cur_29"]
[3144,"a_马家梁二期Ⅲ-035 发电机定子V温度","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅲ-035 发电机定子V温度","yc_hs_0596","cur_30"]
[3145,"a_马家梁二期Ⅲ-035 发电机定子W温度","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅲ-035 发电机定子W温度","yc_hs_0596","cur_31"]
[3146,"a_马家梁二期Ⅲ-035 机舱位置","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅲ-035 机舱位置","yc_hs_0596","cur_33"]
[3147,"a_马家梁二期Ⅲ-035 自由端轴承温度","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅲ-035 自由端轴承温度","yc_hs_0596","cur_34"]
[3148,"a_马家梁二期Ⅲ-035 驱动端轴承温度","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅲ-035 驱动端轴承温度","yc_hs_0596","cur_35"]
[3149,"a_马家梁二期Ⅲ-035 高速轴承温度","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅲ-035 高速轴承温度","yc_hs_0596","cur_36"]
[3150,"a_马家梁二期Ⅲ-035 齿轮箱油温","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅲ-035 齿轮箱油温","yc_hs_0596","cur_38"]
[3151,"a_马家梁二期Ⅲ-035 舱外温度","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅲ-035 舱外温度","yc_hs_0596","cur_43"]
[3152,"a_马家梁二期Ⅲ-035 舱内温度","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅲ-035 舱内温度","yc_hs_0596","cur_44"]
[3153,"a_马家梁二期Ⅲ-035 机舱X方向振动加速度","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅲ-035 机舱X方向振动加速度","yc_hs_0596","cur_48"]
[3154,"a_马家梁二期Ⅲ-035 机舱振动有效值","马家梁风电场","WOF35200074",35,"MJLFD.T2_L3.WTG035.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅲ-035 机舱振动有效值","yc_hs_0596","cur_50"]
[3155,"a_马家梁二期Ⅲ-036 有功功率","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅲ-036 有功功率","yc_hs_0597","cur_21"]
[3156,"a_马家梁二期Ⅲ-036 瞬时风速","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅲ-036 瞬时风速","yc_hs_0597","cur_31"]
[3157,"a_马家梁二期Ⅲ-036 风向角","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅲ-036 风向角","yc_hs_0597","cur_33"]
[3158,"a_马家梁二期Ⅲ-036 风轮转速","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅲ-036 风轮转速","yc_hs_0597","cur_34"]
[3159,"a_马家梁二期Ⅲ-036 桨距角1","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅲ-036 桨距角1","yc_hs_0597","cur_37"]
[3160,"a_马家梁二期Ⅲ-036 桨距角2","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅲ-036 桨距角2","yc_hs_0597","cur_38"]
[3161,"a_马家梁二期Ⅲ-036 桨距角3","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅲ-036 桨距角3","yc_hs_0597","cur_39"]
[3162,"a_马家梁二期Ⅲ-036 发电机转速","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅲ-036 发电机转速","yc_hs_0597","cur_40"]
[3163,"a_马家梁二期Ⅲ-036 发电机定子U温度","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅲ-036 发电机定子U温度","yc_hs_0597","cur_41"]
[3164,"a_马家梁二期Ⅲ-036 发电机定子V温度","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅲ-036 发电机定子V温度","yc_hs_0597","cur_42"]
[3165,"a_马家梁二期Ⅲ-036 发电机定子W温度","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅲ-036 发电机定子W温度","yc_hs_0597","cur_43"]
[3166,"a_马家梁二期Ⅲ-036 机舱位置","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅲ-036 机舱位置","yc_hs_0597","cur_45"]
[3167,"a_马家梁二期Ⅲ-036 自由端轴承温度","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅲ-036 自由端轴承温度","yc_hs_0597","cur_46"]
[3168,"a_马家梁二期Ⅲ-036 驱动端轴承温度","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅲ-036 驱动端轴承温度","yc_hs_0597","cur_47"]
[3169,"a_马家梁二期Ⅲ-036 高速轴承温度","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅲ-036 高速轴承温度","yc_hs_0597","cur_48"]
[3170,"a_马家梁二期Ⅲ-036 齿轮箱油温","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅲ-036 齿轮箱油温","yc_hs_0597","cur_50"]
[3171,"a_马家梁二期Ⅲ-036 舱外温度","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅲ-036 舱外温度","yc_hs_0597","cur_55"]
[3172,"a_马家梁二期Ⅲ-036 舱内温度","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅲ-036 舱内温度","yc_hs_0597","cur_56"]
[3173,"a_马家梁二期Ⅲ-036 机舱X方向振动加速度","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅲ-036 机舱X方向振动加速度","yc_hs_0597","cur_60"]
[3174,"a_马家梁二期Ⅲ-036 机舱振动有效值","马家梁风电场","WOF35200074",36,"MJLFD.T2_L3.WTG036.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅲ-036 机舱振动有效值","yc_hs_0597","cur_62"]
[3175,"a_马家梁二期Ⅳ-037 有功功率","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅳ-037 有功功率","yc_hs_0598","cur_33"]
[3176,"a_马家梁二期Ⅳ-037 瞬时风速","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅳ-037 瞬时风速","yc_hs_0598","cur_43"]
[3177,"a_马家梁二期Ⅳ-037 风向角","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅳ-037 风向角","yc_hs_0598","cur_45"]
[3178,"a_马家梁二期Ⅳ-037 风轮转速","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅳ-037 风轮转速","yc_hs_0598","cur_46"]
[3179,"a_马家梁二期Ⅳ-037 桨距角1","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅳ-037 桨距角1","yc_hs_0598","cur_49"]
[3180,"a_马家梁二期Ⅳ-037 桨距角2","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅳ-037 桨距角2","yc_hs_0598","cur_50"]
[3181,"a_马家梁二期Ⅳ-037 桨距角3","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅳ-037 桨距角3","yc_hs_0598","cur_51"]
[3182,"a_马家梁二期Ⅳ-037 发电机转速","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅳ-037 发电机转速","yc_hs_0598","cur_52"]
[3183,"a_马家梁二期Ⅳ-037 发电机定子U温度","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅳ-037 发电机定子U温度","yc_hs_0598","cur_53"]
[3184,"a_马家梁二期Ⅳ-037 发电机定子V温度","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅳ-037 发电机定子V温度","yc_hs_0598","cur_54"]
[3185,"a_马家梁二期Ⅳ-037 发电机定子W温度","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅳ-037 发电机定子W温度","yc_hs_0598","cur_55"]
[3186,"a_马家梁二期Ⅳ-037 机舱位置","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅳ-037 机舱位置","yc_hs_0598","cur_57"]
[3187,"a_马家梁二期Ⅳ-037 自由端轴承温度","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅳ-037 自由端轴承温度","yc_hs_0598","cur_58"]
[3188,"a_马家梁二期Ⅳ-037 驱动端轴承温度","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅳ-037 驱动端轴承温度","yc_hs_0598","cur_59"]
[3189,"a_马家梁二期Ⅳ-037 高速轴承温度","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅳ-037 高速轴承温度","yc_hs_0598","cur_60"]
[3190,"a_马家梁二期Ⅳ-037 齿轮箱油温","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅳ-037 齿轮箱油温","yc_hs_0598","cur_62"]
[3191,"a_马家梁二期Ⅳ-037 舱外温度","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅳ-037 舱外温度","yc_hs_0598","cur_67"]
[3192,"a_马家梁二期Ⅳ-037 舱内温度","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅳ-037 舱内温度","yc_hs_0598","cur_68"]
[3193,"a_马家梁二期Ⅳ-037 机舱X方向振动加速度","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅳ-037 机舱X方向振动加速度","yc_hs_0598","cur_72"]
[3194,"a_马家梁二期Ⅳ-037 机舱振动有效值","马家梁风电场","WOF35200074",37,"MJLFD.T2_L4.WTG037.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅳ-037 机舱振动有效值","yc_hs_0598","cur_74"]
[3195,"a_马家梁二期Ⅳ-038 有功功率","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅳ-038 有功功率","yc_hs_0599","cur_45"]
[3196,"a_马家梁二期Ⅳ-038 瞬时风速","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅳ-038 瞬时风速","yc_hs_0599","cur_55"]
[3197,"a_马家梁二期Ⅳ-038 风向角","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅳ-038 风向角","yc_hs_0599","cur_57"]
[3198,"a_马家梁二期Ⅳ-038 风轮转速","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅳ-038 风轮转速","yc_hs_0599","cur_58"]
[3199,"a_马家梁二期Ⅳ-038 桨距角1","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅳ-038 桨距角1","yc_hs_0599","cur_61"]
[3200,"a_马家梁二期Ⅳ-038 桨距角2","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅳ-038 桨距角2","yc_hs_0599","cur_62"]
[3201,"a_马家梁二期Ⅳ-038 桨距角3","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅳ-038 桨距角3","yc_hs_0599","cur_63"]
[3202,"a_马家梁二期Ⅳ-038 发电机转速","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅳ-038 发电机转速","yc_hs_0599","cur_64"]
[3203,"a_马家梁二期Ⅳ-038 发电机定子U温度","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅳ-038 发电机定子U温度","yc_hs_0599","cur_65"]
[3204,"a_马家梁二期Ⅳ-038 发电机定子V温度","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅳ-038 发电机定子V温度","yc_hs_0599","cur_66"]
[3205,"a_马家梁二期Ⅳ-038 发电机定子W温度","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅳ-038 发电机定子W温度","yc_hs_0599","cur_67"]
[3206,"a_马家梁二期Ⅳ-038 机舱位置","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅳ-038 机舱位置","yc_hs_0599","cur_69"]
[3207,"a_马家梁二期Ⅳ-038 自由端轴承温度","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅳ-038 自由端轴承温度","yc_hs_0599","cur_70"]
[3208,"a_马家梁二期Ⅳ-038 驱动端轴承温度","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅳ-038 驱动端轴承温度","yc_hs_0599","cur_71"]
[3209,"a_马家梁二期Ⅳ-038 高速轴承温度","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅳ-038 高速轴承温度","yc_hs_0599","cur_72"]
[3210,"a_马家梁二期Ⅳ-038 齿轮箱油温","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅳ-038 齿轮箱油温","yc_hs_0599","cur_74"]
[3211,"a_马家梁二期Ⅳ-038 舱外温度","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅳ-038 舱外温度","yc_hs_0599","cur_79"]
[3212,"a_马家梁二期Ⅳ-038 舱内温度","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅳ-038 舱内温度","yc_hs_0599","cur_80"]
[3213,"a_马家梁二期Ⅳ-038 机舱X方向振动加速度","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅳ-038 机舱X方向振动加速度","yc_hs_0599","cur_84"]
[3214,"a_马家梁二期Ⅳ-038 机舱振动有效值","马家梁风电场","WOF35200074",38,"MJLFD.T2_L4.WTG038.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅳ-038 机舱振动有效值","yc_hs_0599","cur_86"]
[3215,"a_马家梁二期Ⅳ-039 有功功率","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅳ-039 有功功率","yc_hs_0600","cur_57"]
[3216,"a_马家梁二期Ⅳ-039 瞬时风速","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅳ-039 瞬时风速","yc_hs_0600","cur_67"]
[3217,"a_马家梁二期Ⅳ-039 风向角","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅳ-039 风向角","yc_hs_0600","cur_69"]
[3218,"a_马家梁二期Ⅳ-039 风轮转速","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅳ-039 风轮转速","yc_hs_0600","cur_70"]
[3219,"a_马家梁二期Ⅳ-039 桨距角1","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅳ-039 桨距角1","yc_hs_0600","cur_73"]
[3220,"a_马家梁二期Ⅳ-039 桨距角2","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅳ-039 桨距角2","yc_hs_0600","cur_74"]
[3221,"a_马家梁二期Ⅳ-039 桨距角3","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅳ-039 桨距角3","yc_hs_0600","cur_75"]
[3222,"a_马家梁二期Ⅳ-039 发电机转速","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅳ-039 发电机转速","yc_hs_0600","cur_76"]
[3223,"a_马家梁二期Ⅳ-039 发电机定子U温度","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅳ-039 发电机定子U温度","yc_hs_0600","cur_77"]
[3224,"a_马家梁二期Ⅳ-039 发电机定子V温度","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅳ-039 发电机定子V温度","yc_hs_0600","cur_78"]
[3225,"a_马家梁二期Ⅳ-039 发电机定子W温度","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅳ-039 发电机定子W温度","yc_hs_0600","cur_79"]
[3226,"a_马家梁二期Ⅳ-039 机舱位置","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅳ-039 机舱位置","yc_hs_0600","cur_81"]
[3227,"a_马家梁二期Ⅳ-039 自由端轴承温度","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅳ-039 自由端轴承温度","yc_hs_0600","cur_82"]
[3228,"a_马家梁二期Ⅳ-039 驱动端轴承温度","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅳ-039 驱动端轴承温度","yc_hs_0600","cur_83"]
[3229,"a_马家梁二期Ⅳ-039 高速轴承温度","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅳ-039 高速轴承温度","yc_hs_0600","cur_84"]
[3230,"a_马家梁二期Ⅳ-039 齿轮箱油温","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅳ-039 齿轮箱油温","yc_hs_0600","cur_86"]
[3231,"a_马家梁二期Ⅳ-039 舱外温度","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅳ-039 舱外温度","yc_hs_0600","cur_91"]
[3232,"a_马家梁二期Ⅳ-039 舱内温度","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅳ-039 舱内温度","yc_hs_0600","cur_92"]
[3233,"a_马家梁二期Ⅳ-039 机舱X方向振动加速度","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅳ-039 机舱X方向振动加速度","yc_hs_0600","cur_96"]
[3234,"a_马家梁二期Ⅳ-039 机舱振动有效值","马家梁风电场","WOF35200074",39,"MJLFD.T2_L4.WTG039.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅳ-039 机舱振动有效值","yc_hs_0600","cur_98"]
[3235,"a_马家梁二期Ⅳ-040 有功功率","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅳ-040 有功功率","yc_hs_0601","cur_69"]
[3236,"a_马家梁二期Ⅳ-040 瞬时风速","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅳ-040 瞬时风速","yc_hs_0601","cur_79"]
[3237,"a_马家梁二期Ⅳ-040 风向角","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅳ-040 风向角","yc_hs_0601","cur_81"]
[3238,"a_马家梁二期Ⅳ-040 风轮转速","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅳ-040 风轮转速","yc_hs_0601","cur_82"]
[3239,"a_马家梁二期Ⅳ-040 桨距角1","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅳ-040 桨距角1","yc_hs_0601","cur_85"]
[3240,"a_马家梁二期Ⅳ-040 桨距角2","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅳ-040 桨距角2","yc_hs_0601","cur_86"]
[3241,"a_马家梁二期Ⅳ-040 桨距角3","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅳ-040 桨距角3","yc_hs_0601","cur_87"]
[3242,"a_马家梁二期Ⅳ-040 发电机转速","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅳ-040 发电机转速","yc_hs_0601","cur_88"]
[3243,"a_马家梁二期Ⅳ-040 发电机定子U温度","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅳ-040 发电机定子U温度","yc_hs_0601","cur_89"]
[3244,"a_马家梁二期Ⅳ-040 发电机定子V温度","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅳ-040 发电机定子V温度","yc_hs_0601","cur_90"]
[3245,"a_马家梁二期Ⅳ-040 发电机定子W温度","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅳ-040 发电机定子W温度","yc_hs_0601","cur_91"]
[3246,"a_马家梁二期Ⅳ-040 机舱位置","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅳ-040 机舱位置","yc_hs_0601","cur_93"]
[3247,"a_马家梁二期Ⅳ-040 自由端轴承温度","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅳ-040 自由端轴承温度","yc_hs_0601","cur_94"]
[3248,"a_马家梁二期Ⅳ-040 驱动端轴承温度","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅳ-040 驱动端轴承温度","yc_hs_0601","cur_95"]
[3249,"a_马家梁二期Ⅳ-040 高速轴承温度","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅳ-040 高速轴承温度","yc_hs_0601","cur_96"]
[3250,"a_马家梁二期Ⅳ-040 齿轮箱油温","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅳ-040 齿轮箱油温","yc_hs_0601","cur_98"]
[3251,"a_马家梁二期Ⅳ-040 舱外温度","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅳ-040 舱外温度","yc_hs_0602","cur_03"]
[3252,"a_马家梁二期Ⅳ-040 舱内温度","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅳ-040 舱内温度","yc_hs_0602","cur_04"]
[3253,"a_马家梁二期Ⅳ-040 机舱X方向振动加速度","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅳ-040 机舱X方向振动加速度","yc_hs_0602","cur_08"]
[3254,"a_马家梁二期Ⅳ-040 机舱振动有效值","马家梁风电场","WOF35200074",40,"MJLFD.T2_L4.WTG040.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅳ-040 机舱振动有效值","yc_hs_0602","cur_10"]
[3255,"a_马家梁二期Ⅳ-041 有功功率","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅳ-041 有功功率","yc_hs_0602","cur_81"]
[3256,"a_马家梁二期Ⅳ-041 瞬时风速","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅳ-041 瞬时风速","yc_hs_0602","cur_91"]
[3257,"a_马家梁二期Ⅳ-041 风向角","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅳ-041 风向角","yc_hs_0602","cur_93"]
[3258,"a_马家梁二期Ⅳ-041 风轮转速","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅳ-041 风轮转速","yc_hs_0602","cur_94"]
[3259,"a_马家梁二期Ⅳ-041 桨距角1","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅳ-041 桨距角1","yc_hs_0602","cur_97"]
[3260,"a_马家梁二期Ⅳ-041 桨距角2","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅳ-041 桨距角2","yc_hs_0602","cur_98"]
[3261,"a_马家梁二期Ⅳ-041 桨距角3","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅳ-041 桨距角3","yc_hs_0602","cur_99"]
[3262,"a_马家梁二期Ⅳ-041 发电机转速","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅳ-041 发电机转速","yc_hs_0602","cur_100"]
[3263,"a_马家梁二期Ⅳ-041 发电机定子U温度","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅳ-041 发电机定子U温度","yc_hs_0603","cur_01"]
[3264,"a_马家梁二期Ⅳ-041 发电机定子V温度","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅳ-041 发电机定子V温度","yc_hs_0603","cur_02"]
[3265,"a_马家梁二期Ⅳ-041 发电机定子W温度","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅳ-041 发电机定子W温度","yc_hs_0603","cur_03"]
[3266,"a_马家梁二期Ⅳ-041 机舱位置","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅳ-041 机舱位置","yc_hs_0603","cur_05"]
[3267,"a_马家梁二期Ⅳ-041 自由端轴承温度","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅳ-041 自由端轴承温度","yc_hs_0603","cur_06"]
[3268,"a_马家梁二期Ⅳ-041 驱动端轴承温度","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅳ-041 驱动端轴承温度","yc_hs_0603","cur_07"]
[3269,"a_马家梁二期Ⅳ-041 高速轴承温度","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅳ-041 高速轴承温度","yc_hs_0603","cur_08"]
[3270,"a_马家梁二期Ⅳ-041 齿轮箱油温","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅳ-041 齿轮箱油温","yc_hs_0603","cur_10"]
[3271,"a_马家梁二期Ⅳ-041 舱外温度","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅳ-041 舱外温度","yc_hs_0603","cur_15"]
[3272,"a_马家梁二期Ⅳ-041 舱内温度","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅳ-041 舱内温度","yc_hs_0603","cur_16"]
[3273,"a_马家梁二期Ⅳ-041 机舱X方向振动加速度","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅳ-041 机舱X方向振动加速度","yc_hs_0603","cur_20"]
[3274,"a_马家梁二期Ⅳ-041 机舱振动有效值","马家梁风电场","WOF35200074",41,"MJLFD.T2_L4.WTG041.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅳ-041 机舱振动有效值","yc_hs_0603","cur_22"]
[3275,"a_马家梁二期Ⅳ-042 有功功率","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅳ-042 有功功率","yc_hs_0603","cur_93"]
[3276,"a_马家梁二期Ⅳ-042 瞬时风速","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅳ-042 瞬时风速","yc_hs_0604","cur_03"]
[3277,"a_马家梁二期Ⅳ-042 风向角","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅳ-042 风向角","yc_hs_0604","cur_05"]
[3278,"a_马家梁二期Ⅳ-042 风轮转速","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅳ-042 风轮转速","yc_hs_0604","cur_06"]
[3279,"a_马家梁二期Ⅳ-042 桨距角1","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅳ-042 桨距角1","yc_hs_0604","cur_09"]
[3280,"a_马家梁二期Ⅳ-042 桨距角2","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅳ-042 桨距角2","yc_hs_0604","cur_10"]
[3281,"a_马家梁二期Ⅳ-042 桨距角3","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅳ-042 桨距角3","yc_hs_0604","cur_11"]
[3282,"a_马家梁二期Ⅳ-042 发电机转速","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅳ-042 发电机转速","yc_hs_0604","cur_12"]
[3283,"a_马家梁二期Ⅳ-042 发电机定子U温度","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅳ-042 发电机定子U温度","yc_hs_0604","cur_13"]
[3284,"a_马家梁二期Ⅳ-042 发电机定子V温度","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅳ-042 发电机定子V温度","yc_hs_0604","cur_14"]
[3285,"a_马家梁二期Ⅳ-042 发电机定子W温度","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅳ-042 发电机定子W温度","yc_hs_0604","cur_15"]
[3286,"a_马家梁二期Ⅳ-042 机舱位置","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅳ-042 机舱位置","yc_hs_0604","cur_17"]
[3287,"a_马家梁二期Ⅳ-042 自由端轴承温度","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅳ-042 自由端轴承温度","yc_hs_0604","cur_18"]
[3288,"a_马家梁二期Ⅳ-042 驱动端轴承温度","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅳ-042 驱动端轴承温度","yc_hs_0604","cur_19"]
[3289,"a_马家梁二期Ⅳ-042 高速轴承温度","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅳ-042 高速轴承温度","yc_hs_0604","cur_20"]
[3290,"a_马家梁二期Ⅳ-042 齿轮箱油温","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅳ-042 齿轮箱油温","yc_hs_0604","cur_22"]
[3291,"a_马家梁二期Ⅳ-042 舱外温度","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅳ-042 舱外温度","yc_hs_0604","cur_27"]
[3292,"a_马家梁二期Ⅳ-042 舱内温度","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅳ-042 舱内温度","yc_hs_0604","cur_28"]
[3293,"a_马家梁二期Ⅳ-042 机舱X方向振动加速度","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅳ-042 机舱X方向振动加速度","yc_hs_0604","cur_32"]
[3294,"a_马家梁二期Ⅳ-042 机舱振动有效值","马家梁风电场","WOF35200074",42,"MJLFD.T2_L4.WTG042.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅳ-042 机舱振动有效值","yc_hs_0604","cur_34"]
[3295,"a_马家梁二期Ⅳ-043 有功功率","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅳ-043 有功功率","yc_hs_0605","cur_05"]
[3296,"a_马家梁二期Ⅳ-043 瞬时风速","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅳ-043 瞬时风速","yc_hs_0605","cur_15"]
[3297,"a_马家梁二期Ⅳ-043 风向角","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅳ-043 风向角","yc_hs_0605","cur_17"]
[3298,"a_马家梁二期Ⅳ-043 风轮转速","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅳ-043 风轮转速","yc_hs_0605","cur_18"]
[3299,"a_马家梁二期Ⅳ-043 桨距角1","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅳ-043 桨距角1","yc_hs_0605","cur_21"]
[3300,"a_马家梁二期Ⅳ-043 桨距角2","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅳ-043 桨距角2","yc_hs_0605","cur_22"]
[3301,"a_马家梁二期Ⅳ-043 桨距角3","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅳ-043 桨距角3","yc_hs_0605","cur_23"]
[3302,"a_马家梁二期Ⅳ-043 发电机转速","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅳ-043 发电机转速","yc_hs_0605","cur_24"]
[3303,"a_马家梁二期Ⅳ-043 发电机定子U温度","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅳ-043 发电机定子U温度","yc_hs_0605","cur_25"]
[3304,"a_马家梁二期Ⅳ-043 发电机定子V温度","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅳ-043 发电机定子V温度","yc_hs_0605","cur_26"]
[3305,"a_马家梁二期Ⅳ-043 发电机定子W温度","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅳ-043 发电机定子W温度","yc_hs_0605","cur_27"]
[3306,"a_马家梁二期Ⅳ-043 机舱位置","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅳ-043 机舱位置","yc_hs_0605","cur_29"]
[3307,"a_马家梁二期Ⅳ-043 自由端轴承温度","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅳ-043 自由端轴承温度","yc_hs_0605","cur_30"]
[3308,"a_马家梁二期Ⅳ-043 驱动端轴承温度","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅳ-043 驱动端轴承温度","yc_hs_0605","cur_31"]
[3309,"a_马家梁二期Ⅳ-043 高速轴承温度","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅳ-043 高速轴承温度","yc_hs_0605","cur_32"]
[3310,"a_马家梁二期Ⅳ-043 齿轮箱油温","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅳ-043 齿轮箱油温","yc_hs_0605","cur_34"]
[3311,"a_马家梁二期Ⅳ-043 舱外温度","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅳ-043 舱外温度","yc_hs_0605","cur_39"]
[3312,"a_马家梁二期Ⅳ-043 舱内温度","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅳ-043 舱内温度","yc_hs_0605","cur_40"]
[3313,"a_马家梁二期Ⅳ-043 机舱X方向振动加速度","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅳ-043 机舱X方向振动加速度","yc_hs_0605","cur_44"]
[3314,"a_马家梁二期Ⅳ-043 机舱振动有效值","马家梁风电场","WOF35200074",43,"MJLFD.T2_L4.WTG043.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅳ-043 机舱振动有效值","yc_hs_0605","cur_46"]
[3315,"a_马家梁二期Ⅳ-044 有功功率","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅳ-044 有功功率","yc_hs_0606","cur_17"]
[3316,"a_马家梁二期Ⅳ-044 瞬时风速","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅳ-044 瞬时风速","yc_hs_0606","cur_27"]
[3317,"a_马家梁二期Ⅳ-044 风向角","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅳ-044 风向角","yc_hs_0606","cur_29"]
[3318,"a_马家梁二期Ⅳ-044 风轮转速","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅳ-044 风轮转速","yc_hs_0606","cur_30"]
[3319,"a_马家梁二期Ⅳ-044 桨距角1","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅳ-044 桨距角1","yc_hs_0606","cur_33"]
[3320,"a_马家梁二期Ⅳ-044 桨距角2","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅳ-044 桨距角2","yc_hs_0606","cur_34"]
[3321,"a_马家梁二期Ⅳ-044 桨距角3","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅳ-044 桨距角3","yc_hs_0606","cur_35"]
[3322,"a_马家梁二期Ⅳ-044 发电机转速","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅳ-044 发电机转速","yc_hs_0606","cur_36"]
[3323,"a_马家梁二期Ⅳ-044 发电机定子U温度","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅳ-044 发电机定子U温度","yc_hs_0606","cur_37"]
[3324,"a_马家梁二期Ⅳ-044 发电机定子V温度","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅳ-044 发电机定子V温度","yc_hs_0606","cur_38"]
[3325,"a_马家梁二期Ⅳ-044 发电机定子W温度","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅳ-044 发电机定子W温度","yc_hs_0606","cur_39"]
[3326,"a_马家梁二期Ⅳ-044 机舱位置","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅳ-044 机舱位置","yc_hs_0606","cur_41"]
[3327,"a_马家梁二期Ⅳ-044 自由端轴承温度","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅳ-044 自由端轴承温度","yc_hs_0606","cur_42"]
[3328,"a_马家梁二期Ⅳ-044 驱动端轴承温度","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅳ-044 驱动端轴承温度","yc_hs_0606","cur_43"]
[3329,"a_马家梁二期Ⅳ-044 高速轴承温度","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅳ-044 高速轴承温度","yc_hs_0606","cur_44"]
[3330,"a_马家梁二期Ⅳ-044 齿轮箱油温","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅳ-044 齿轮箱油温","yc_hs_0606","cur_46"]
[3331,"a_马家梁二期Ⅳ-044 舱外温度","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅳ-044 舱外温度","yc_hs_0606","cur_51"]
[3332,"a_马家梁二期Ⅳ-044 舱内温度","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅳ-044 舱内温度","yc_hs_0606","cur_52"]
[3333,"a_马家梁二期Ⅳ-044 机舱X方向振动加速度","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅳ-044 机舱X方向振动加速度","yc_hs_0606","cur_56"]
[3334,"a_马家梁二期Ⅳ-044 机舱振动有效值","马家梁风电场","WOF35200074",44,"MJLFD.T2_L4.WTG044.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅳ-044 机舱振动有效值","yc_hs_0606","cur_58"]
[3335,"a_马家梁二期Ⅳ-045 有功功率","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅳ-045 有功功率","yc_hs_0607","cur_29"]
[3336,"a_马家梁二期Ⅳ-045 瞬时风速","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅳ-045 瞬时风速","yc_hs_0607","cur_39"]
[3337,"a_马家梁二期Ⅳ-045 风向角","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅳ-045 风向角","yc_hs_0607","cur_41"]
[3338,"a_马家梁二期Ⅳ-045 风轮转速","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅳ-045 风轮转速","yc_hs_0607","cur_42"]
[3339,"a_马家梁二期Ⅳ-045 桨距角1","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅳ-045 桨距角1","yc_hs_0607","cur_45"]
[3340,"a_马家梁二期Ⅳ-045 桨距角2","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅳ-045 桨距角2","yc_hs_0607","cur_46"]
[3341,"a_马家梁二期Ⅳ-045 桨距角3","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅳ-045 桨距角3","yc_hs_0607","cur_47"]
[3342,"a_马家梁二期Ⅳ-045 发电机转速","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅳ-045 发电机转速","yc_hs_0607","cur_48"]
[3343,"a_马家梁二期Ⅳ-045 发电机定子U温度","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅳ-045 发电机定子U温度","yc_hs_0607","cur_49"]
[3344,"a_马家梁二期Ⅳ-045 发电机定子V温度","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅳ-045 发电机定子V温度","yc_hs_0607","cur_50"]
[3345,"a_马家梁二期Ⅳ-045 发电机定子W温度","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅳ-045 发电机定子W温度","yc_hs_0607","cur_51"]
[3346,"a_马家梁二期Ⅳ-045 机舱位置","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅳ-045 机舱位置","yc_hs_0607","cur_53"]
[3347,"a_马家梁二期Ⅳ-045 自由端轴承温度","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅳ-045 自由端轴承温度","yc_hs_0607","cur_54"]
[3348,"a_马家梁二期Ⅳ-045 驱动端轴承温度","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅳ-045 驱动端轴承温度","yc_hs_0607","cur_55"]
[3349,"a_马家梁二期Ⅳ-045 高速轴承温度","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅳ-045 高速轴承温度","yc_hs_0607","cur_56"]
[3350,"a_马家梁二期Ⅳ-045 齿轮箱油温","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅳ-045 齿轮箱油温","yc_hs_0607","cur_58"]
[3351,"a_马家梁二期Ⅳ-045 舱外温度","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅳ-045 舱外温度","yc_hs_0607","cur_63"]
[3352,"a_马家梁二期Ⅳ-045 舱内温度","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅳ-045 舱内温度","yc_hs_0607","cur_64"]
[3353,"a_马家梁二期Ⅳ-045 机舱X方向振动加速度","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅳ-045 机舱X方向振动加速度","yc_hs_0607","cur_68"]
[3354,"a_马家梁二期Ⅳ-045 机舱振动有效值","马家梁风电场","WOF35200074",45,"MJLFD.T2_L4.WTG045.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅳ-045 机舱振动有效值","yc_hs_0607","cur_70"]
[3355,"a_马家梁二期Ⅳ-046 有功功率","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅳ-046 有功功率","yc_hs_0608","cur_41"]
[3356,"a_马家梁二期Ⅳ-046 瞬时风速","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅳ-046 瞬时风速","yc_hs_0608","cur_51"]
[3357,"a_马家梁二期Ⅳ-046 风向角","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅳ-046 风向角","yc_hs_0608","cur_53"]
[3358,"a_马家梁二期Ⅳ-046 风轮转速","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅳ-046 风轮转速","yc_hs_0608","cur_54"]
[3359,"a_马家梁二期Ⅳ-046 桨距角1","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅳ-046 桨距角1","yc_hs_0608","cur_57"]
[3360,"a_马家梁二期Ⅳ-046 桨距角2","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅳ-046 桨距角2","yc_hs_0608","cur_58"]
[3361,"a_马家梁二期Ⅳ-046 桨距角3","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅳ-046 桨距角3","yc_hs_0608","cur_59"]
[3362,"a_马家梁二期Ⅳ-046 发电机转速","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅳ-046 发电机转速","yc_hs_0608","cur_60"]
[3363,"a_马家梁二期Ⅳ-046 发电机定子U温度","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅳ-046 发电机定子U温度","yc_hs_0608","cur_61"]
[3364,"a_马家梁二期Ⅳ-046 发电机定子V温度","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅳ-046 发电机定子V温度","yc_hs_0608","cur_62"]
[3365,"a_马家梁二期Ⅳ-046 发电机定子W温度","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅳ-046 发电机定子W温度","yc_hs_0608","cur_63"]
[3366,"a_马家梁二期Ⅳ-046 机舱位置","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅳ-046 机舱位置","yc_hs_0608","cur_65"]
[3367,"a_马家梁二期Ⅳ-046 自由端轴承温度","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅳ-046 自由端轴承温度","yc_hs_0608","cur_66"]
[3368,"a_马家梁二期Ⅳ-046 驱动端轴承温度","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅳ-046 驱动端轴承温度","yc_hs_0608","cur_67"]
[3369,"a_马家梁二期Ⅳ-046 高速轴承温度","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅳ-046 高速轴承温度","yc_hs_0608","cur_68"]
[3370,"a_马家梁二期Ⅳ-046 齿轮箱油温","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅳ-046 齿轮箱油温","yc_hs_0608","cur_70"]
[3371,"a_马家梁二期Ⅳ-046 舱外温度","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅳ-046 舱外温度","yc_hs_0608","cur_75"]
[3372,"a_马家梁二期Ⅳ-046 舱内温度","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅳ-046 舱内温度","yc_hs_0608","cur_76"]
[3373,"a_马家梁二期Ⅳ-046 机舱X方向振动加速度","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅳ-046 机舱X方向振动加速度","yc_hs_0608","cur_80"]
[3374,"a_马家梁二期Ⅳ-046 机舱振动有效值","马家梁风电场","WOF35200074",46,"MJLFD.T2_L4.WTG046.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅳ-046 机舱振动有效值","yc_hs_0608","cur_82"]
[3375,"a_马家梁二期Ⅳ-047 有功功率","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅳ-047 有功功率","yc_hs_0609","cur_53"]
[3376,"a_马家梁二期Ⅳ-047 瞬时风速","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅳ-047 瞬时风速","yc_hs_0609","cur_63"]
[3377,"a_马家梁二期Ⅳ-047 风向角","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅳ-047 风向角","yc_hs_0609","cur_65"]
[3378,"a_马家梁二期Ⅳ-047 风轮转速","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅳ-047 风轮转速","yc_hs_0609","cur_66"]
[3379,"a_马家梁二期Ⅳ-047 桨距角1","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅳ-047 桨距角1","yc_hs_0609","cur_69"]
[3380,"a_马家梁二期Ⅳ-047 桨距角2","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅳ-047 桨距角2","yc_hs_0609","cur_70"]
[3381,"a_马家梁二期Ⅳ-047 桨距角3","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅳ-047 桨距角3","yc_hs_0609","cur_71"]
[3382,"a_马家梁二期Ⅳ-047 发电机转速","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅳ-047 发电机转速","yc_hs_0609","cur_72"]
[3383,"a_马家梁二期Ⅳ-047 发电机定子U温度","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅳ-047 发电机定子U温度","yc_hs_0609","cur_73"]
[3384,"a_马家梁二期Ⅳ-047 发电机定子V温度","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅳ-047 发电机定子V温度","yc_hs_0609","cur_74"]
[3385,"a_马家梁二期Ⅳ-047 发电机定子W温度","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅳ-047 发电机定子W温度","yc_hs_0609","cur_75"]
[3386,"a_马家梁二期Ⅳ-047 机舱位置","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅳ-047 机舱位置","yc_hs_0609","cur_77"]
[3387,"a_马家梁二期Ⅳ-047 自由端轴承温度","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅳ-047 自由端轴承温度","yc_hs_0609","cur_78"]
[3388,"a_马家梁二期Ⅳ-047 驱动端轴承温度","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅳ-047 驱动端轴承温度","yc_hs_0609","cur_79"]
[3389,"a_马家梁二期Ⅳ-047 高速轴承温度","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅳ-047 高速轴承温度","yc_hs_0609","cur_80"]
[3390,"a_马家梁二期Ⅳ-047 齿轮箱油温","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅳ-047 齿轮箱油温","yc_hs_0609","cur_82"]
[3391,"a_马家梁二期Ⅳ-047 舱外温度","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅳ-047 舱外温度","yc_hs_0609","cur_87"]
[3392,"a_马家梁二期Ⅳ-047 舱内温度","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅳ-047 舱内温度","yc_hs_0609","cur_88"]
[3393,"a_马家梁二期Ⅳ-047 机舱X方向振动加速度","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅳ-047 机舱X方向振动加速度","yc_hs_0609","cur_92"]
[3394,"a_马家梁二期Ⅳ-047 机舱振动有效值","马家梁风电场","WOF35200074",47,"MJLFD.T2_L4.WTG047.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅳ-047 机舱振动有效值","yc_hs_0609","cur_94"]
[3395,"a_马家梁二期Ⅳ-048 有功功率","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅳ-048 有功功率","yc_hs_0610","cur_65"]
[3396,"a_马家梁二期Ⅳ-048 瞬时风速","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅳ-048 瞬时风速","yc_hs_0610","cur_75"]
[3397,"a_马家梁二期Ⅳ-048 风向角","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅳ-048 风向角","yc_hs_0610","cur_77"]
[3398,"a_马家梁二期Ⅳ-048 风轮转速","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅳ-048 风轮转速","yc_hs_0610","cur_78"]
[3399,"a_马家梁二期Ⅳ-048 桨距角1","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅳ-048 桨距角1","yc_hs_0610","cur_81"]
[3400,"a_马家梁二期Ⅳ-048 桨距角2","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅳ-048 桨距角2","yc_hs_0610","cur_82"]
[3401,"a_马家梁二期Ⅳ-048 桨距角3","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅳ-048 桨距角3","yc_hs_0610","cur_83"]
[3402,"a_马家梁二期Ⅳ-048 发电机转速","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅳ-048 发电机转速","yc_hs_0610","cur_84"]
[3403,"a_马家梁二期Ⅳ-048 发电机定子U温度","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅳ-048 发电机定子U温度","yc_hs_0610","cur_85"]
[3404,"a_马家梁二期Ⅳ-048 发电机定子V温度","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅳ-048 发电机定子V温度","yc_hs_0610","cur_86"]
[3405,"a_马家梁二期Ⅳ-048 发电机定子W温度","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅳ-048 发电机定子W温度","yc_hs_0610","cur_87"]
[3406,"a_马家梁二期Ⅳ-048 机舱位置","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅳ-048 机舱位置","yc_hs_0610","cur_89"]
[3407,"a_马家梁二期Ⅳ-048 自由端轴承温度","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅳ-048 自由端轴承温度","yc_hs_0610","cur_90"]
[3408,"a_马家梁二期Ⅳ-048 驱动端轴承温度","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅳ-048 驱动端轴承温度","yc_hs_0610","cur_91"]
[3409,"a_马家梁二期Ⅳ-048 高速轴承温度","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅳ-048 高速轴承温度","yc_hs_0610","cur_92"]
[3410,"a_马家梁二期Ⅳ-048 齿轮箱油温","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅳ-048 齿轮箱油温","yc_hs_0610","cur_94"]
[3411,"a_马家梁二期Ⅳ-048 舱外温度","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅳ-048 舱外温度","yc_hs_0610","cur_99"]
[3412,"a_马家梁二期Ⅳ-048 舱内温度","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅳ-048 舱内温度","yc_hs_0610","cur_100"]
[3413,"a_马家梁二期Ⅳ-048 机舱X方向振动加速度","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅳ-048 机舱X方向振动加速度","yc_hs_0611","cur_04"]
[3414,"a_马家梁二期Ⅳ-048 机舱振动有效值","马家梁风电场","WOF35200074",48,"MJLFD.T2_L4.WTG048.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅳ-048 机舱振动有效值","yc_hs_0611","cur_06"]
[3415,"a_马家梁二期Ⅳ-049 有功功率","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WGEN.GenActivePW","有功功率","active_power","a_马家梁二期Ⅳ-049 有功功率","yc_hs_0611","cur_77"]
[3416,"a_马家梁二期Ⅳ-049 瞬时风速","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WNAC.WindSpeed","风速","wind_velocity","a_马家梁二期Ⅳ-049 瞬时风速","yc_hs_0611","cur_87"]
[3417,"a_马家梁二期Ⅳ-049 风向角","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WNAC.WindVaneDirection","对风角度","yaw_error1","a_马家梁二期Ⅳ-049 风向角","yc_hs_0611","cur_89"]
[3418,"a_马家梁二期Ⅳ-049 风轮转速","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","a_马家梁二期Ⅳ-049 风轮转速","yc_hs_0611","cur_90"]
[3419,"a_马家梁二期Ⅳ-049 桨距角1","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","a_马家梁二期Ⅳ-049 桨距角1","yc_hs_0611","cur_93"]
[3420,"a_马家梁二期Ⅳ-049 桨距角2","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","a_马家梁二期Ⅳ-049 桨距角2","yc_hs_0611","cur_94"]
[3421,"a_马家梁二期Ⅳ-049 桨距角3","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","a_马家梁二期Ⅳ-049 桨距角3","yc_hs_0611","cur_95"]
[3422,"a_马家梁二期Ⅳ-049 发电机转速","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WGEN.GenSpd","发电机转速","generator_speed","a_马家梁二期Ⅳ-049 发电机转速","yc_hs_0611","cur_96"]
[3423,"a_马家梁二期Ⅳ-049 发电机定子U温度","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WGEN.TemGenU","发电机绕组1温度","generator_winding1_temperature","a_马家梁二期Ⅳ-049 发电机定子U温度","yc_hs_0611","cur_97"]
[3424,"a_马家梁二期Ⅳ-049 发电机定子V温度","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WGEN.TemGenV","发电机绕组2温度","generator_winding2_temperature","a_马家梁二期Ⅳ-049 发电机定子V温度","yc_hs_0611","cur_98"]
[3425,"a_马家梁二期Ⅳ-049 发电机定子W温度","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WGEN.TemGenW","发电机绕组3温度","generator_winding3_temperature","a_马家梁二期Ⅳ-049 发电机定子W温度","yc_hs_0611","cur_99"]
[3426,"a_马家梁二期Ⅳ-049 机舱位置","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WYAW.NacellePosition","机舱位置","cabin_position","a_马家梁二期Ⅳ-049 机舱位置","yc_hs_0612","cur_01"]
[3427,"a_马家梁二期Ⅳ-049 自由端轴承温度","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WTRM.TGBAVisu","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","a_马家梁二期Ⅳ-049 自由端轴承温度","yc_hs_0612","cur_02"]
[3428,"a_马家梁二期Ⅳ-049 驱动端轴承温度","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WTRM.TGBBVisu","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","a_马家梁二期Ⅳ-049 驱动端轴承温度","yc_hs_0612","cur_03"]
[3429,"a_马家梁二期Ⅳ-049 高速轴承温度","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WTRM.TGBSOutVisu","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","a_马家梁二期Ⅳ-049 高速轴承温度","yc_hs_0612","cur_04"]
[3430,"a_马家梁二期Ⅳ-049 齿轮箱油温","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","a_马家梁二期Ⅳ-049 齿轮箱油温","yc_hs_0612","cur_06"]
[3431,"a_马家梁二期Ⅳ-049 舱外温度","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WNAC.TemOut","环境温度","outside_cabin_temperature","a_马家梁二期Ⅳ-049 舱外温度","yc_hs_0612","cur_11"]
[3432,"a_马家梁二期Ⅳ-049 舱内温度","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WNAC.TemNacelle","机舱内温度","cabin_temperature","a_马家梁二期Ⅳ-049 舱内温度","yc_hs_0612","cur_12"]
[3433,"a_马家梁二期Ⅳ-049 机舱X方向振动加速度","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","a_马家梁二期Ⅳ-049 机舱X方向振动加速度","yc_hs_0612","cur_16"]
[3434,"a_马家梁二期Ⅳ-049 机舱振动有效值","马家梁风电场","WOF35200074",49,"MJLFD.T2_L4.WTG049.WVIB.VibrationLFil","机舱前后振动","front_back_vibration_of_the_cabin","a_马家梁二期Ⅳ-049 机舱振动有效值","yc_hs_0612","cur_18"]
[3435,"坡底一期Ⅰ-01 主轴转速","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","坡底一期Ⅰ-01 主轴转速","yc_hs_0620","cur_01"]
[3436,"坡底一期Ⅰ-01 发电机转速","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WGEN.GenSpd","发电机转速","generator_speed","坡底一期Ⅰ-01 发电机转速","yc_hs_0620","cur_02"]
[3437,"坡底一期Ⅰ-01 风向","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WNAC.WindDirection","绝对风向","true_wind_direction","坡底一期Ⅰ-01 风向","yc_hs_0620","cur_03"]
[3438,"坡底一期Ⅰ-01 风速","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WNAC.WindSpeed","风速","wind_velocity","坡底一期Ⅰ-01 风速","yc_hs_0620","cur_04"]
[3439,"坡底一期Ⅰ-01 机舱温度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WNAC.TemNacelle","机舱内温度","cabin_temperature","坡底一期Ⅰ-01 机舱温度","yc_hs_0620","cur_14"]
[3440,"坡底一期Ⅰ-01 室外温度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WNAC.TemOut","环境温度","outside_cabin_temperature","坡底一期Ⅰ-01 室外温度","yc_hs_0620","cur_15"]
[3441,"坡底一期Ⅰ-01 主轴轴承温度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WTRM.RotorTemPrcs","主轴承轴承温度","main_bearing_temperature","坡底一期Ⅰ-01 主轴轴承温度","yc_hs_0620","cur_33"]
[3442,"坡底一期Ⅰ-01 齿轮箱高速轴承端温度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","坡底一期Ⅰ-01 齿轮箱高速轴承端温度","yc_hs_0620","cur_35"]
[3443,"坡底一期Ⅰ-01 齿轮箱油温","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","坡底一期Ⅰ-01 齿轮箱油温","yc_hs_0620","cur_36"]
[3444,"坡底一期Ⅰ-01 发电机驱动端温度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","坡底一期Ⅰ-01 发电机驱动端温度","yc_hs_0620","cur_37"]
[3445,"坡底一期Ⅰ-01 发电机非驱动端温度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","坡底一期Ⅰ-01 发电机非驱动端温度","yc_hs_0620","cur_38"]
[3446,"坡底一期Ⅰ-01 发电机L1温度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","坡底一期Ⅰ-01 发电机L1温度","yc_hs_0620","cur_39"]
[3447,"坡底一期Ⅰ-01 发电机L2温度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","坡底一期Ⅰ-01 发电机L2温度","yc_hs_0620","cur_40"]
[3448,"坡底一期Ⅰ-01 发电机L3温度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","坡底一期Ⅰ-01 发电机L3温度","yc_hs_0620","cur_41"]
[3449,"坡底一期Ⅰ-01 扭缆角度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","坡底一期Ⅰ-01 扭缆角度","yc_hs_0620","cur_43"]
[3450,"坡底一期Ⅰ-01 机舱位置","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WYAW.NacellePosition","机舱位置","cabin_position","坡底一期Ⅰ-01 机舱位置","yc_hs_0620","cur_44"]
[3451,"坡底一期Ⅰ-01 轴1桨叶实际角度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","坡底一期Ⅰ-01 轴1桨叶实际角度","yc_hs_0620","cur_56"]
[3452,"坡底一期Ⅰ-01 轴2桨叶实际角度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","坡底一期Ⅰ-01 轴2桨叶实际角度","yc_hs_0620","cur_59"]
[3453,"坡底一期Ⅰ-01 轴3桨叶实际角度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","坡底一期Ⅰ-01 轴3桨叶实际角度","yc_hs_0620","cur_62"]
[3454,"坡底一期Ⅰ-01 机舱Y方向振动值","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WVIB.VibrationV","机舱前后振动","front_back_vibration_of_the_cabin","坡底一期Ⅰ-01 机舱Y方向振动值","yc_hs_0620","cur_67"]
[3455,"坡底一期Ⅰ-01 机舱X方向振动值","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","坡底一期Ⅰ-01 机舱X方向振动值","yc_hs_0620","cur_68"]
[3456,"坡底一期Ⅰ-01 1秒风向平均值","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WNAC.WindDirection1S","对风角度","yaw_error1","坡底一期Ⅰ-01 1秒风向平均值","yc_hs_0620","cur_71"]
[3457,"坡底一期Ⅰ-01 齿轮箱中间轴发电机侧温度","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","坡底一期Ⅰ-01 齿轮箱中间轴发电机侧温度","yc_hs_0620","cur_94"]
[3458,"坡底一期Ⅰ-01 有功功率","坡底风电场","WOF35900076",1,"PLPFD.T1_L1.WTG001.WGEN.GenActivePW","有功功率","active_power","坡底一期Ⅰ-01 有功功率","yc_hs_0622","cur_11"]
[3459,"坡底一期Ⅰ-02 主轴转速","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","坡底一期Ⅰ-02 主轴转速","yc_hs_0622","cur_21"]
[3460,"坡底一期Ⅰ-02 发电机转速","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WGEN.GenSpd","发电机转速","generator_speed","坡底一期Ⅰ-02 发电机转速","yc_hs_0622","cur_22"]
[3461,"坡底一期Ⅰ-02 风向","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WNAC.WindDirection","绝对风向","true_wind_direction","坡底一期Ⅰ-02 风向","yc_hs_0622","cur_23"]
[3462,"坡底一期Ⅰ-02 风速","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WNAC.WindSpeed","风速","wind_velocity","坡底一期Ⅰ-02 风速","yc_hs_0622","cur_24"]
[3463,"坡底一期Ⅰ-02 机舱温度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WNAC.TemNacelle","机舱内温度","cabin_temperature","坡底一期Ⅰ-02 机舱温度","yc_hs_0622","cur_34"]
[3464,"坡底一期Ⅰ-02 室外温度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WNAC.TemOut","环境温度","outside_cabin_temperature","坡底一期Ⅰ-02 室外温度","yc_hs_0622","cur_35"]
[3465,"坡底一期Ⅰ-02 主轴轴承温度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WTRM.RotorTemPrcs","主轴承轴承温度","main_bearing_temperature","坡底一期Ⅰ-02 主轴轴承温度","yc_hs_0622","cur_53"]
[3466,"坡底一期Ⅰ-02 齿轮箱高速轴承端温度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","坡底一期Ⅰ-02 齿轮箱高速轴承端温度","yc_hs_0622","cur_55"]
[3467,"坡底一期Ⅰ-02 齿轮箱油温","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","坡底一期Ⅰ-02 齿轮箱油温","yc_hs_0622","cur_56"]
[3468,"坡底一期Ⅰ-02 发电机驱动端温度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","坡底一期Ⅰ-02 发电机驱动端温度","yc_hs_0622","cur_57"]
[3469,"坡底一期Ⅰ-02 发电机非驱动端温度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","坡底一期Ⅰ-02 发电机非驱动端温度","yc_hs_0622","cur_58"]
[3470,"坡底一期Ⅰ-02 发电机L1温度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","坡底一期Ⅰ-02 发电机L1温度","yc_hs_0622","cur_59"]
[3471,"坡底一期Ⅰ-02 发电机L2温度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","坡底一期Ⅰ-02 发电机L2温度","yc_hs_0622","cur_60"]
[3472,"坡底一期Ⅰ-02 发电机L3温度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","坡底一期Ⅰ-02 发电机L3温度","yc_hs_0622","cur_61"]
[3473,"坡底一期Ⅰ-02 扭缆角度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","坡底一期Ⅰ-02 扭缆角度","yc_hs_0622","cur_63"]
[3474,"坡底一期Ⅰ-02 机舱位置","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WYAW.NacellePosition","机舱位置","cabin_position","坡底一期Ⅰ-02 机舱位置","yc_hs_0622","cur_64"]
[3475,"坡底一期Ⅰ-02 轴1桨叶实际角度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","坡底一期Ⅰ-02 轴1桨叶实际角度","yc_hs_0622","cur_76"]
[3476,"坡底一期Ⅰ-02 轴2桨叶实际角度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","坡底一期Ⅰ-02 轴2桨叶实际角度","yc_hs_0622","cur_79"]
[3477,"坡底一期Ⅰ-02 轴3桨叶实际角度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","坡底一期Ⅰ-02 轴3桨叶实际角度","yc_hs_0622","cur_82"]
[3478,"坡底一期Ⅰ-02 机舱Y方向振动值","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WVIB.VibrationV","机舱前后振动","front_back_vibration_of_the_cabin","坡底一期Ⅰ-02 机舱Y方向振动值","yc_hs_0622","cur_87"]
[3479,"坡底一期Ⅰ-02 机舱X方向振动值","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","坡底一期Ⅰ-02 机舱X方向振动值","yc_hs_0622","cur_88"]
[3480,"坡底一期Ⅰ-02 1秒风向平均值","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WNAC.WindDirection1S","对风角度","yaw_error1","坡底一期Ⅰ-02 1秒风向平均值","yc_hs_0622","cur_91"]
[3481,"坡底一期Ⅰ-02 齿轮箱中间轴发电机侧温度","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","坡底一期Ⅰ-02 齿轮箱中间轴发电机侧温度","yc_hs_0623","cur_14"]
[3482,"坡底一期Ⅰ-02 有功功率","坡底风电场","WOF35900076",2,"PLPFD.T1_L1.WTG002.WGEN.GenActivePW","有功功率","active_power","坡底一期Ⅰ-02 有功功率","yc_hs_0624","cur_31"]
[3483,"坡底一期Ⅰ-03 主轴转速","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","坡底一期Ⅰ-03 主轴转速","yc_hs_0624","cur_41"]
[3484,"坡底一期Ⅰ-03 发电机转速","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WGEN.GenSpd","发电机转速","generator_speed","坡底一期Ⅰ-03 发电机转速","yc_hs_0624","cur_42"]
[3485,"坡底一期Ⅰ-03 风向","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WNAC.WindDirection","绝对风向","true_wind_direction","坡底一期Ⅰ-03 风向","yc_hs_0624","cur_43"]
[3486,"坡底一期Ⅰ-03 风速","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WNAC.WindSpeed","风速","wind_velocity","坡底一期Ⅰ-03 风速","yc_hs_0624","cur_44"]
[3487,"坡底一期Ⅰ-03 机舱温度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WNAC.TemNacelle","机舱内温度","cabin_temperature","坡底一期Ⅰ-03 机舱温度","yc_hs_0624","cur_54"]
[3488,"坡底一期Ⅰ-03 室外温度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WNAC.TemOut","环境温度","outside_cabin_temperature","坡底一期Ⅰ-03 室外温度","yc_hs_0624","cur_55"]
[3489,"坡底一期Ⅰ-03 主轴轴承温度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WTRM.RotorTemPrcs","主轴承轴承温度","main_bearing_temperature","坡底一期Ⅰ-03 主轴轴承温度","yc_hs_0624","cur_73"]
[3490,"坡底一期Ⅰ-03 齿轮箱高速轴承端温度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","坡底一期Ⅰ-03 齿轮箱高速轴承端温度","yc_hs_0624","cur_75"]
[3491,"坡底一期Ⅰ-03 齿轮箱油温","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","坡底一期Ⅰ-03 齿轮箱油温","yc_hs_0624","cur_76"]
[3492,"坡底一期Ⅰ-03 发电机驱动端温度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","坡底一期Ⅰ-03 发电机驱动端温度","yc_hs_0624","cur_77"]
[3493,"坡底一期Ⅰ-03 发电机非驱动端温度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","坡底一期Ⅰ-03 发电机非驱动端温度","yc_hs_0624","cur_78"]
[3494,"坡底一期Ⅰ-03 发电机L1温度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","坡底一期Ⅰ-03 发电机L1温度","yc_hs_0624","cur_79"]
[3495,"坡底一期Ⅰ-03 发电机L2温度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","坡底一期Ⅰ-03 发电机L2温度","yc_hs_0624","cur_80"]
[3496,"坡底一期Ⅰ-03 发电机L3温度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","坡底一期Ⅰ-03 发电机L3温度","yc_hs_0624","cur_81"]
[3497,"坡底一期Ⅰ-03 扭缆角度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","坡底一期Ⅰ-03 扭缆角度","yc_hs_0624","cur_83"]
[3498,"坡底一期Ⅰ-03 机舱位置","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WYAW.NacellePosition","机舱位置","cabin_position","坡底一期Ⅰ-03 机舱位置","yc_hs_0624","cur_84"]
[3499,"坡底一期Ⅰ-03 轴1桨叶实际角度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","坡底一期Ⅰ-03 轴1桨叶实际角度","yc_hs_0624","cur_96"]
[3500,"坡底一期Ⅰ-03 轴2桨叶实际角度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","坡底一期Ⅰ-03 轴2桨叶实际角度","yc_hs_0624","cur_99"]
[3501,"坡底一期Ⅰ-03 轴3桨叶实际角度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","坡底一期Ⅰ-03 轴3桨叶实际角度","yc_hs_0625","cur_02"]
[3502,"坡底一期Ⅰ-03 机舱Y方向振动值","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WVIB.VibrationV","机舱前后振动","front_back_vibration_of_the_cabin","坡底一期Ⅰ-03 机舱Y方向振动值","yc_hs_0625","cur_07"]
[3503,"坡底一期Ⅰ-03 机舱X方向振动值","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","坡底一期Ⅰ-03 机舱X方向振动值","yc_hs_0625","cur_08"]
[3504,"坡底一期Ⅰ-03 1秒风向平均值","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WNAC.WindDirection1S","对风角度","yaw_error1","坡底一期Ⅰ-03 1秒风向平均值","yc_hs_0625","cur_11"]
[3505,"坡底一期Ⅰ-03 齿轮箱中间轴发电机侧温度","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","坡底一期Ⅰ-03 齿轮箱中间轴发电机侧温度","yc_hs_0625","cur_34"]
[3506,"坡底一期Ⅰ-03 有功功率","坡底风电场","WOF35900076",3,"PLPFD.T1_L1.WTG003.WGEN.GenActivePW","有功功率","active_power","坡底一期Ⅰ-03 有功功率","yc_hs_0626","cur_51"]
[3507,"坡底一期Ⅰ-04 主轴转速","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","坡底一期Ⅰ-04 主轴转速","yc_hs_0626","cur_61"]
[3508,"坡底一期Ⅰ-04 发电机转速","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WGEN.GenSpd","发电机转速","generator_speed","坡底一期Ⅰ-04 发电机转速","yc_hs_0626","cur_62"]
[3509,"坡底一期Ⅰ-04 风向","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WNAC.WindDirection","绝对风向","true_wind_direction","坡底一期Ⅰ-04 风向","yc_hs_0626","cur_63"]
[3510,"坡底一期Ⅰ-04 风速","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WNAC.WindSpeed","风速","wind_velocity","坡底一期Ⅰ-04 风速","yc_hs_0626","cur_64"]
[3511,"坡底一期Ⅰ-04 机舱温度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WNAC.TemNacelle","机舱内温度","cabin_temperature","坡底一期Ⅰ-04 机舱温度","yc_hs_0626","cur_74"]
[3512,"坡底一期Ⅰ-04 室外温度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WNAC.TemOut","环境温度","outside_cabin_temperature","坡底一期Ⅰ-04 室外温度","yc_hs_0626","cur_75"]
[3513,"坡底一期Ⅰ-04 主轴轴承温度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WTRM.RotorTemPrcs","主轴承轴承温度","main_bearing_temperature","坡底一期Ⅰ-04 主轴轴承温度","yc_hs_0626","cur_93"]
[3514,"坡底一期Ⅰ-04 齿轮箱高速轴承端温度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","坡底一期Ⅰ-04 齿轮箱高速轴承端温度","yc_hs_0626","cur_95"]
[3515,"坡底一期Ⅰ-04 齿轮箱油温","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","坡底一期Ⅰ-04 齿轮箱油温","yc_hs_0626","cur_96"]
[3516,"坡底一期Ⅰ-04 发电机驱动端温度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","坡底一期Ⅰ-04 发电机驱动端温度","yc_hs_0626","cur_97"]
[3517,"坡底一期Ⅰ-04 发电机非驱动端温度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","坡底一期Ⅰ-04 发电机非驱动端温度","yc_hs_0626","cur_98"]
[3518,"坡底一期Ⅰ-04 发电机L1温度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","坡底一期Ⅰ-04 发电机L1温度","yc_hs_0626","cur_99"]
[3519,"坡底一期Ⅰ-04 发电机L2温度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","坡底一期Ⅰ-04 发电机L2温度","yc_hs_0626","cur_100"]
[3520,"坡底一期Ⅰ-04 发电机L3温度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","坡底一期Ⅰ-04 发电机L3温度","yc_hs_0627","cur_01"]
[3521,"坡底一期Ⅰ-04 扭缆角度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","坡底一期Ⅰ-04 扭缆角度","yc_hs_0627","cur_03"]
[3522,"坡底一期Ⅰ-04 机舱位置","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WYAW.NacellePosition","机舱位置","cabin_position","坡底一期Ⅰ-04 机舱位置","yc_hs_0627","cur_04"]
[3523,"坡底一期Ⅰ-04 轴1桨叶实际角度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","坡底一期Ⅰ-04 轴1桨叶实际角度","yc_hs_0627","cur_16"]
[3524,"坡底一期Ⅰ-04 轴2桨叶实际角度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","坡底一期Ⅰ-04 轴2桨叶实际角度","yc_hs_0627","cur_19"]
[3525,"坡底一期Ⅰ-04 轴3桨叶实际角度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","坡底一期Ⅰ-04 轴3桨叶实际角度","yc_hs_0627","cur_22"]
[3526,"坡底一期Ⅰ-04 机舱Y方向振动值","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WVIB.VibrationV","机舱前后振动","front_back_vibration_of_the_cabin","坡底一期Ⅰ-04 机舱Y方向振动值","yc_hs_0627","cur_27"]
[3527,"坡底一期Ⅰ-04 机舱X方向振动值","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","坡底一期Ⅰ-04 机舱X方向振动值","yc_hs_0627","cur_28"]
[3528,"坡底一期Ⅰ-04 1秒风向平均值","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WNAC.WindDirection1S","对风角度","yaw_error1","坡底一期Ⅰ-04 1秒风向平均值","yc_hs_0627","cur_31"]
[3529,"坡底一期Ⅰ-04 齿轮箱中间轴发电机侧温度","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","坡底一期Ⅰ-04 齿轮箱中间轴发电机侧温度","yc_hs_0627","cur_54"]
[3530,"坡底一期Ⅰ-04 有功功率","坡底风电场","WOF35900076",4,"PLPFD.T1_L1.WTG004.WGEN.GenActivePW","有功功率","active_power","坡底一期Ⅰ-04 有功功率","yc_hs_0628","cur_71"]
[3531,"坡底一期Ⅰ-05 主轴转速","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","坡底一期Ⅰ-05 主轴转速","yc_hs_0628","cur_81"]
[3532,"坡底一期Ⅰ-05 发电机转速","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WGEN.GenSpd","发电机转速","generator_speed","坡底一期Ⅰ-05 发电机转速","yc_hs_0628","cur_82"]
[3533,"坡底一期Ⅰ-05 风向","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WNAC.WindDirection","绝对风向","true_wind_direction","坡底一期Ⅰ-05 风向","yc_hs_0628","cur_83"]
[3534,"坡底一期Ⅰ-05 风速","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WNAC.WindSpeed","风速","wind_velocity","坡底一期Ⅰ-05 风速","yc_hs_0628","cur_84"]
[3535,"坡底一期Ⅰ-05 机舱温度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WNAC.TemNacelle","机舱内温度","cabin_temperature","坡底一期Ⅰ-05 机舱温度","yc_hs_0628","cur_94"]
[3536,"坡底一期Ⅰ-05 室外温度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WNAC.TemOut","环境温度","outside_cabin_temperature","坡底一期Ⅰ-05 室外温度","yc_hs_0628","cur_95"]
[3537,"坡底一期Ⅰ-05 主轴轴承温度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WTRM.RotorTemPrcs","主轴承轴承温度","main_bearing_temperature","坡底一期Ⅰ-05 主轴轴承温度","yc_hs_0629","cur_13"]
[3538,"坡底一期Ⅰ-05 齿轮箱高速轴承端温度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","坡底一期Ⅰ-05 齿轮箱高速轴承端温度","yc_hs_0629","cur_15"]
[3539,"坡底一期Ⅰ-05 齿轮箱油温","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","坡底一期Ⅰ-05 齿轮箱油温","yc_hs_0629","cur_16"]
[3540,"坡底一期Ⅰ-05 发电机驱动端温度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","坡底一期Ⅰ-05 发电机驱动端温度","yc_hs_0629","cur_17"]
[3541,"坡底一期Ⅰ-05 发电机非驱动端温度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","坡底一期Ⅰ-05 发电机非驱动端温度","yc_hs_0629","cur_18"]
[3542,"坡底一期Ⅰ-05 发电机L1温度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","坡底一期Ⅰ-05 发电机L1温度","yc_hs_0629","cur_19"]
[3543,"坡底一期Ⅰ-05 发电机L2温度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","坡底一期Ⅰ-05 发电机L2温度","yc_hs_0629","cur_20"]
[3544,"坡底一期Ⅰ-05 发电机L3温度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","坡底一期Ⅰ-05 发电机L3温度","yc_hs_0629","cur_21"]
[3545,"坡底一期Ⅰ-05 扭缆角度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","坡底一期Ⅰ-05 扭缆角度","yc_hs_0629","cur_23"]
[3546,"坡底一期Ⅰ-05 机舱位置","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WYAW.NacellePosition","机舱位置","cabin_position","坡底一期Ⅰ-05 机舱位置","yc_hs_0629","cur_24"]
[3547,"坡底一期Ⅰ-05 轴1桨叶实际角度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","坡底一期Ⅰ-05 轴1桨叶实际角度","yc_hs_0629","cur_36"]
[3548,"坡底一期Ⅰ-05 轴2桨叶实际角度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","坡底一期Ⅰ-05 轴2桨叶实际角度","yc_hs_0629","cur_39"]
[3549,"坡底一期Ⅰ-05 轴3桨叶实际角度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","坡底一期Ⅰ-05 轴3桨叶实际角度","yc_hs_0629","cur_42"]
[3550,"坡底一期Ⅰ-05 机舱Y方向振动值","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WVIB.VibrationV","机舱前后振动","front_back_vibration_of_the_cabin","坡底一期Ⅰ-05 机舱Y方向振动值","yc_hs_0629","cur_47"]
[3551,"坡底一期Ⅰ-05 机舱X方向振动值","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","坡底一期Ⅰ-05 机舱X方向振动值","yc_hs_0629","cur_48"]
[3552,"坡底一期Ⅰ-05 1秒风向平均值","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WNAC.WindDirection1S","对风角度","yaw_error1","坡底一期Ⅰ-05 1秒风向平均值","yc_hs_0629","cur_51"]
[3553,"坡底一期Ⅰ-05 齿轮箱中间轴发电机侧温度","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","坡底一期Ⅰ-05 齿轮箱中间轴发电机侧温度","yc_hs_0629","cur_74"]
[3554,"坡底一期Ⅰ-05 有功功率","坡底风电场","WOF35900076",5,"PLPFD.T1_L1.WTG005.WGEN.GenActivePW","有功功率","active_power","坡底一期Ⅰ-05 有功功率","yc_hs_0630","cur_91"]
[3555,"坡底一期Ⅰ-06 主轴转速","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","坡底一期Ⅰ-06 主轴转速","yc_hs_0631","cur_01"]
[3556,"坡底一期Ⅰ-06 发电机转速","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WGEN.GenSpd","发电机转速","generator_speed","坡底一期Ⅰ-06 发电机转速","yc_hs_0631","cur_02"]
[3557,"坡底一期Ⅰ-06 风向","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WNAC.WindDirection","绝对风向","true_wind_direction","坡底一期Ⅰ-06 风向","yc_hs_0631","cur_03"]
[3558,"坡底一期Ⅰ-06 风速","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WNAC.WindSpeed","风速","wind_velocity","坡底一期Ⅰ-06 风速","yc_hs_0631","cur_04"]
[3559,"坡底一期Ⅰ-06 机舱温度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WNAC.TemNacelle","机舱内温度","cabin_temperature","坡底一期Ⅰ-06 机舱温度","yc_hs_0631","cur_14"]
[3560,"坡底一期Ⅰ-06 室外温度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WNAC.TemOut","环境温度","outside_cabin_temperature","坡底一期Ⅰ-06 室外温度","yc_hs_0631","cur_15"]
[3561,"坡底一期Ⅰ-06 主轴轴承温度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WTRM.RotorTemPrcs","主轴承轴承温度","main_bearing_temperature","坡底一期Ⅰ-06 主轴轴承温度","yc_hs_0631","cur_33"]
[3562,"坡底一期Ⅰ-06 齿轮箱高速轴承端温度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","坡底一期Ⅰ-06 齿轮箱高速轴承端温度","yc_hs_0631","cur_35"]
[3563,"坡底一期Ⅰ-06 齿轮箱油温","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","坡底一期Ⅰ-06 齿轮箱油温","yc_hs_0631","cur_36"]
[3564,"坡底一期Ⅰ-06 发电机驱动端温度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","坡底一期Ⅰ-06 发电机驱动端温度","yc_hs_0631","cur_37"]
[3565,"坡底一期Ⅰ-06 发电机非驱动端温度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","坡底一期Ⅰ-06 发电机非驱动端温度","yc_hs_0631","cur_38"]
[3566,"坡底一期Ⅰ-06 发电机L1温度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","坡底一期Ⅰ-06 发电机L1温度","yc_hs_0631","cur_39"]
[3567,"坡底一期Ⅰ-06 发电机L2温度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","坡底一期Ⅰ-06 发电机L2温度","yc_hs_0631","cur_40"]
[3568,"坡底一期Ⅰ-06 发电机L3温度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","坡底一期Ⅰ-06 发电机L3温度","yc_hs_0631","cur_41"]
[3569,"坡底一期Ⅰ-06 扭缆角度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","坡底一期Ⅰ-06 扭缆角度","yc_hs_0631","cur_43"]
[3570,"坡底一期Ⅰ-06 机舱位置","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WYAW.NacellePosition","机舱位置","cabin_position","坡底一期Ⅰ-06 机舱位置","yc_hs_0631","cur_44"]
[3571,"坡底一期Ⅰ-06 轴1桨叶实际角度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","坡底一期Ⅰ-06 轴1桨叶实际角度","yc_hs_0631","cur_56"]
[3572,"坡底一期Ⅰ-06 轴2桨叶实际角度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","坡底一期Ⅰ-06 轴2桨叶实际角度","yc_hs_0631","cur_59"]
[3573,"坡底一期Ⅰ-06 轴3桨叶实际角度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","坡底一期Ⅰ-06 轴3桨叶实际角度","yc_hs_0631","cur_62"]
[3574,"坡底一期Ⅰ-06 机舱Y方向振动值","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WVIB.VibrationV","机舱前后振动","front_back_vibration_of_the_cabin","坡底一期Ⅰ-06 机舱Y方向振动值","yc_hs_0631","cur_67"]
[3575,"坡底一期Ⅰ-06 机舱X方向振动值","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WVIB.VibrationL","机舱左右振动","side_to_side_vibration_of_the_cabin","坡底一期Ⅰ-06 机舱X方向振动值","yc_hs_0631","cur_68"]
[3576,"坡底一期Ⅰ-06 1秒风向平均值","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WNAC.WindDirection1S","对风角度","yaw_error1","坡底一期Ⅰ-06 1秒风向平均值","yc_hs_0631","cur_71"]
[3577,"坡底一期Ⅰ-06 齿轮箱中间轴发电机侧温度","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","坡底一期Ⅰ-06 齿轮箱中间轴发电机侧温度","yc_hs_0631","cur_94"]
[3578,"坡底一期Ⅰ-06 有功功率","坡底风电场","WOF35900076",6,"PLPFD.T1_L1.WTG006.WGEN.GenActivePW","有功功率","active_power","坡底一期Ⅰ-06 有功功率","yc_hs_0633","cur_11"]
[3579,"l_贺家沟一期Ⅵ-01 环境温度","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WNAC.TemOut","环境温度","outside_cabin_temperature","l_贺家沟一期Ⅵ-01 环境温度","yc_hs_0635","cur_02"]
[3580,"l_贺家沟一期Ⅵ-01 风速1s","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WNAC.WindSpeed","风速","wind_velocity","l_贺家沟一期Ⅵ-01 风速1s","yc_hs_0635","cur_04"]
[3581,"l_贺家沟一期Ⅵ-01 绝对风向","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WNAC.WindDirection","绝对风向","true_wind_direction","l_贺家沟一期Ⅵ-01 绝对风向","yc_hs_0635","cur_06"]
[3582,"l_贺家沟一期Ⅵ-01 偏航误差","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WYAW.YawError","对风角度","yaw_error1","l_贺家沟一期Ⅵ-01 偏航误差","yc_hs_0635","cur_09"]
[3583,"l_贺家沟一期Ⅵ-01 桨角1","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","l_贺家沟一期Ⅵ-01 桨角1","yc_hs_0635","cur_10"]
[3584,"l_贺家沟一期Ⅵ-01 桨角2","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","l_贺家沟一期Ⅵ-01 桨角2","yc_hs_0635","cur_11"]
[3585,"l_贺家沟一期Ⅵ-01 桨角3","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","l_贺家沟一期Ⅵ-01 桨角3","yc_hs_0635","cur_12"]
[3586,"l_贺家沟一期Ⅵ-01 风轮转速","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WTRM.RotorSpd","风轮转速","rotor_speed","l_贺家沟一期Ⅵ-01 风轮转速","yc_hs_0635","cur_13"]
[3587,"l_贺家沟一期Ⅵ-01 发电机转速","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WGEN.GenSpd","发电机转速","generator_speed","l_贺家沟一期Ⅵ-01 发电机转速","yc_hs_0635","cur_14"]
[3588,"l_贺家沟一期Ⅵ-01 发电机U相温度","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","l_贺家沟一期Ⅵ-01 发电机U相温度","yc_hs_0635","cur_43"]
[3589,"l_贺家沟一期Ⅵ-01 发电机V相温度","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","l_贺家沟一期Ⅵ-01 发电机V相温度","yc_hs_0635","cur_44"]
[3590,"l_贺家沟一期Ⅵ-01 发电机W相温度","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","l_贺家沟一期Ⅵ-01 发电机W相温度","yc_hs_0635","cur_45"]
[3591,"l_贺家沟一期Ⅵ-01 发电机轴承温度","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","l_贺家沟一期Ⅵ-01 发电机轴承温度","yc_hs_0635","cur_46"]
[3592,"l_贺家沟一期Ⅵ-01 发电机轴承2温度","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","l_贺家沟一期Ⅵ-01 发电机轴承2温度","yc_hs_0635","cur_47"]
[3593,"l_贺家沟一期Ⅵ-01 齿轮箱高速轴前轴承温度","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","l_贺家沟一期Ⅵ-01 齿轮箱高速轴前轴承温度","yc_hs_0635","cur_48"]
[3594,"l_贺家沟一期Ⅵ-01 机舱内温度","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WNAC.TemNacelle","机舱内温度","cabin_temperature","l_贺家沟一期Ⅵ-01 机舱内温度","yc_hs_0635","cur_75"]
[3595,"l_贺家沟一期Ⅵ-01 变流器有功功率","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WCNV.DemandActPow","有功功率","active_power","l_贺家沟一期Ⅵ-01 变流器有功功率","yc_hs_0636","cur_05"]
[3596,"l_贺家沟一期Ⅵ-01 塔筒左右振动","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WTUR.YC032","机舱左右振动","side_to_side_vibration_of_the_cabin","l_贺家沟一期Ⅵ-01 塔筒左右振动","yc_hs_0636","cur_07"]
[3597,"l_贺家沟一期Ⅵ-01 塔筒前后振动","贺家沟","WOF35800080",1,"SSLF20219.T1_L6.WTG001.WTUR.YC033","机舱前后振动","front_back_vibration_of_the_cabin","l_贺家沟一期Ⅵ-01 塔筒前后振动","yc_hs_0636","cur_08"]
[3598,"l_贺家沟一期Ⅵ-02 环境温度","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WNAC.TemOut","环境温度","outside_cabin_temperature","l_贺家沟一期Ⅵ-02 环境温度","yc_hs_0636","cur_41"]
[3599,"l_贺家沟一期Ⅵ-02 风速1s","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WNAC.WindSpeed","风速","wind_velocity","l_贺家沟一期Ⅵ-02 风速1s","yc_hs_0636","cur_43"]
[3600,"l_贺家沟一期Ⅵ-02 绝对风向","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WNAC.WindDirection","绝对风向","true_wind_direction","l_贺家沟一期Ⅵ-02 绝对风向","yc_hs_0636","cur_45"]
[3601,"l_贺家沟一期Ⅵ-02 偏航误差","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WYAW.YawError","对风角度","yaw_error1","l_贺家沟一期Ⅵ-02 偏航误差","yc_hs_0636","cur_48"]
[3602,"l_贺家沟一期Ⅵ-02 桨角1","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","l_贺家沟一期Ⅵ-02 桨角1","yc_hs_0636","cur_49"]
[3603,"l_贺家沟一期Ⅵ-02 桨角2","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","l_贺家沟一期Ⅵ-02 桨角2","yc_hs_0636","cur_50"]
[3604,"l_贺家沟一期Ⅵ-02 桨角3","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","l_贺家沟一期Ⅵ-02 桨角3","yc_hs_0636","cur_51"]
[3605,"l_贺家沟一期Ⅵ-02 风轮转速","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WTRM.RotorSpd","风轮转速","rotor_speed","l_贺家沟一期Ⅵ-02 风轮转速","yc_hs_0636","cur_52"]
[3606,"l_贺家沟一期Ⅵ-02 发电机转速","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WGEN.GenSpd","发电机转速","generator_speed","l_贺家沟一期Ⅵ-02 发电机转速","yc_hs_0636","cur_53"]
[3607,"l_贺家沟一期Ⅵ-02 发电机U相温度","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","l_贺家沟一期Ⅵ-02 发电机U相温度","yc_hs_0636","cur_82"]
[3608,"l_贺家沟一期Ⅵ-02 发电机V相温度","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","l_贺家沟一期Ⅵ-02 发电机V相温度","yc_hs_0636","cur_83"]
[3609,"l_贺家沟一期Ⅵ-02 发电机W相温度","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","l_贺家沟一期Ⅵ-02 发电机W相温度","yc_hs_0636","cur_84"]
[3610,"l_贺家沟一期Ⅵ-02 发电机轴承温度","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","l_贺家沟一期Ⅵ-02 发电机轴承温度","yc_hs_0636","cur_85"]
[3611,"l_贺家沟一期Ⅵ-02 发电机轴承2温度","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","l_贺家沟一期Ⅵ-02 发电机轴承2温度","yc_hs_0636","cur_86"]
[3612,"l_贺家沟一期Ⅵ-02 齿轮箱高速轴前轴承温度","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","l_贺家沟一期Ⅵ-02 齿轮箱高速轴前轴承温度","yc_hs_0636","cur_87"]
[3613,"l_贺家沟一期Ⅵ-02 机舱内温度","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WNAC.TemNacelle","机舱内温度","cabin_temperature","l_贺家沟一期Ⅵ-02 机舱内温度","yc_hs_0637","cur_14"]
[3614,"l_贺家沟一期Ⅵ-02 变流器有功功率","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WCNV.DemandActPow","有功功率","active_power","l_贺家沟一期Ⅵ-02 变流器有功功率","yc_hs_0637","cur_44"]
[3615,"l_贺家沟一期Ⅵ-02 塔筒左右振动","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WTUR.YC032","机舱左右振动","side_to_side_vibration_of_the_cabin","l_贺家沟一期Ⅵ-02 塔筒左右振动","yc_hs_0637","cur_46"]
[3616,"l_贺家沟一期Ⅵ-02 塔筒前后振动","贺家沟","WOF35800080",2,"SSLF20219.T1_L6.WTG002.WTUR.YC033","机舱前后振动","front_back_vibration_of_the_cabin","l_贺家沟一期Ⅵ-02 塔筒前后振动","yc_hs_0637","cur_47"]
[3617,"l_贺家沟一期Ⅵ-03 环境温度","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WNAC.TemOut","环境温度","outside_cabin_temperature","l_贺家沟一期Ⅵ-03 环境温度","yc_hs_0637","cur_80"]
[3618,"l_贺家沟一期Ⅵ-03 风速1s","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WNAC.WindSpeed","风速","wind_velocity","l_贺家沟一期Ⅵ-03 风速1s","yc_hs_0637","cur_82"]
[3619,"l_贺家沟一期Ⅵ-03 绝对风向","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WNAC.WindDirection","绝对风向","true_wind_direction","l_贺家沟一期Ⅵ-03 绝对风向","yc_hs_0637","cur_84"]
[3620,"l_贺家沟一期Ⅵ-03 偏航误差","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WYAW.YawError","对风角度","yaw_error1","l_贺家沟一期Ⅵ-03 偏航误差","yc_hs_0637","cur_87"]
[3621,"l_贺家沟一期Ⅵ-03 桨角1","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","l_贺家沟一期Ⅵ-03 桨角1","yc_hs_0637","cur_88"]
[3622,"l_贺家沟一期Ⅵ-03 桨角2","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","l_贺家沟一期Ⅵ-03 桨角2","yc_hs_0637","cur_89"]
[3623,"l_贺家沟一期Ⅵ-03 桨角3","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","l_贺家沟一期Ⅵ-03 桨角3","yc_hs_0637","cur_90"]
[3624,"l_贺家沟一期Ⅵ-03 风轮转速","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WTRM.RotorSpd","风轮转速","rotor_speed","l_贺家沟一期Ⅵ-03 风轮转速","yc_hs_0637","cur_91"]
[3625,"l_贺家沟一期Ⅵ-03 发电机转速","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WGEN.GenSpd","发电机转速","generator_speed","l_贺家沟一期Ⅵ-03 发电机转速","yc_hs_0637","cur_92"]
[3626,"l_贺家沟一期Ⅵ-03 发电机U相温度","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","l_贺家沟一期Ⅵ-03 发电机U相温度","yc_hs_0638","cur_21"]
[3627,"l_贺家沟一期Ⅵ-03 发电机V相温度","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","l_贺家沟一期Ⅵ-03 发电机V相温度","yc_hs_0638","cur_22"]
[3628,"l_贺家沟一期Ⅵ-03 发电机W相温度","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","l_贺家沟一期Ⅵ-03 发电机W相温度","yc_hs_0638","cur_23"]
[3629,"l_贺家沟一期Ⅵ-03 发电机轴承温度","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","l_贺家沟一期Ⅵ-03 发电机轴承温度","yc_hs_0638","cur_24"]
[3630,"l_贺家沟一期Ⅵ-03 发电机轴承2温度","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","l_贺家沟一期Ⅵ-03 发电机轴承2温度","yc_hs_0638","cur_25"]
[3631,"l_贺家沟一期Ⅵ-03 齿轮箱高速轴前轴承温度","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","l_贺家沟一期Ⅵ-03 齿轮箱高速轴前轴承温度","yc_hs_0638","cur_26"]
[3632,"l_贺家沟一期Ⅵ-03 机舱内温度","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WNAC.TemNacelle","机舱内温度","cabin_temperature","l_贺家沟一期Ⅵ-03 机舱内温度","yc_hs_0638","cur_53"]
[3633,"l_贺家沟一期Ⅵ-03 变流器有功功率","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WCNV.DemandActPow","有功功率","active_power","l_贺家沟一期Ⅵ-03 变流器有功功率","yc_hs_0638","cur_83"]
[3634,"l_贺家沟一期Ⅵ-03 塔筒左右振动","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WTUR.YC032","机舱左右振动","side_to_side_vibration_of_the_cabin","l_贺家沟一期Ⅵ-03 塔筒左右振动","yc_hs_0638","cur_85"]
[3635,"l_贺家沟一期Ⅵ-03 塔筒前后振动","贺家沟","WOF35800080",3,"SSLF20219.T1_L6.WTG003.WTUR.YC033","机舱前后振动","front_back_vibration_of_the_cabin","l_贺家沟一期Ⅵ-03 塔筒前后振动","yc_hs_0638","cur_86"]
[3636,"l_贺家沟一期Ⅵ-04 环境温度","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WNAC.TemOut","环境温度","outside_cabin_temperature","l_贺家沟一期Ⅵ-04 环境温度","yc_hs_0639","cur_19"]
[3637,"l_贺家沟一期Ⅵ-04 风速1s","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WNAC.WindSpeed","风速","wind_velocity","l_贺家沟一期Ⅵ-04 风速1s","yc_hs_0639","cur_21"]
[3638,"l_贺家沟一期Ⅵ-04 绝对风向","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WNAC.WindDirection","绝对风向","true_wind_direction","l_贺家沟一期Ⅵ-04 绝对风向","yc_hs_0639","cur_23"]
[3639,"l_贺家沟一期Ⅵ-04 偏航误差","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WYAW.YawError","对风角度","yaw_error1","l_贺家沟一期Ⅵ-04 偏航误差","yc_hs_0639","cur_26"]
[3640,"l_贺家沟一期Ⅵ-04 桨角1","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","l_贺家沟一期Ⅵ-04 桨角1","yc_hs_0639","cur_27"]
[3641,"l_贺家沟一期Ⅵ-04 桨角2","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","l_贺家沟一期Ⅵ-04 桨角2","yc_hs_0639","cur_28"]
[3642,"l_贺家沟一期Ⅵ-04 桨角3","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","l_贺家沟一期Ⅵ-04 桨角3","yc_hs_0639","cur_29"]
[3643,"l_贺家沟一期Ⅵ-04 风轮转速","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WTRM.RotorSpd","风轮转速","rotor_speed","l_贺家沟一期Ⅵ-04 风轮转速","yc_hs_0639","cur_30"]
[3644,"l_贺家沟一期Ⅵ-04 发电机转速","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WGEN.GenSpd","发电机转速","generator_speed","l_贺家沟一期Ⅵ-04 发电机转速","yc_hs_0639","cur_31"]
[3645,"l_贺家沟一期Ⅵ-04 发电机U相温度","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","l_贺家沟一期Ⅵ-04 发电机U相温度","yc_hs_0639","cur_60"]
[3646,"l_贺家沟一期Ⅵ-04 发电机V相温度","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","l_贺家沟一期Ⅵ-04 发电机V相温度","yc_hs_0639","cur_61"]
[3647,"l_贺家沟一期Ⅵ-04 发电机W相温度","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","l_贺家沟一期Ⅵ-04 发电机W相温度","yc_hs_0639","cur_62"]
[3648,"l_贺家沟一期Ⅵ-04 发电机轴承温度","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","l_贺家沟一期Ⅵ-04 发电机轴承温度","yc_hs_0639","cur_63"]
[3649,"l_贺家沟一期Ⅵ-04 发电机轴承2温度","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","l_贺家沟一期Ⅵ-04 发电机轴承2温度","yc_hs_0639","cur_64"]
[3650,"l_贺家沟一期Ⅵ-04 齿轮箱高速轴前轴承温度","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","l_贺家沟一期Ⅵ-04 齿轮箱高速轴前轴承温度","yc_hs_0639","cur_65"]
[3651,"l_贺家沟一期Ⅵ-04 机舱内温度","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WNAC.TemNacelle","机舱内温度","cabin_temperature","l_贺家沟一期Ⅵ-04 机舱内温度","yc_hs_0639","cur_92"]
[3652,"l_贺家沟一期Ⅵ-04 变流器有功功率","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WCNV.DemandActPow","有功功率","active_power","l_贺家沟一期Ⅵ-04 变流器有功功率","yc_hs_0640","cur_22"]
[3653,"l_贺家沟一期Ⅵ-04 塔筒左右振动","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WTUR.YC032","机舱左右振动","side_to_side_vibration_of_the_cabin","l_贺家沟一期Ⅵ-04 塔筒左右振动","yc_hs_0640","cur_24"]
[3654,"l_贺家沟一期Ⅵ-04 塔筒前后振动","贺家沟","WOF35800080",4,"SSLF20219.T1_L6.WTG004.WTUR.YC033","机舱前后振动","front_back_vibration_of_the_cabin","l_贺家沟一期Ⅵ-04 塔筒前后振动","yc_hs_0640","cur_25"]
[3655,"l_贺家沟一期Ⅶ-05 环境温度","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WNAC.TemOut","环境温度","outside_cabin_temperature","l_贺家沟一期Ⅶ-05 环境温度","yc_hs_0640","cur_58"]
[3656,"l_贺家沟一期Ⅶ-05 风速1s","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WNAC.WindSpeed","风速","wind_velocity","l_贺家沟一期Ⅶ-05 风速1s","yc_hs_0640","cur_60"]
[3657,"l_贺家沟一期Ⅶ-05 绝对风向","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WNAC.WindDirection","绝对风向","true_wind_direction","l_贺家沟一期Ⅶ-05 绝对风向","yc_hs_0640","cur_62"]
[3658,"l_贺家沟一期Ⅶ-05 偏航误差","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WYAW.YawError","对风角度","yaw_error1","l_贺家沟一期Ⅶ-05 偏航误差","yc_hs_0640","cur_65"]
[3659,"l_贺家沟一期Ⅶ-05 桨角1","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","l_贺家沟一期Ⅶ-05 桨角1","yc_hs_0640","cur_66"]
[3660,"l_贺家沟一期Ⅶ-05 桨角2","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","l_贺家沟一期Ⅶ-05 桨角2","yc_hs_0640","cur_67"]
[3661,"l_贺家沟一期Ⅶ-05 桨角3","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","l_贺家沟一期Ⅶ-05 桨角3","yc_hs_0640","cur_68"]
[3662,"l_贺家沟一期Ⅶ-05 风轮转速","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WTRM.RotorSpd","风轮转速","rotor_speed","l_贺家沟一期Ⅶ-05 风轮转速","yc_hs_0640","cur_69"]
[3663,"l_贺家沟一期Ⅶ-05 发电机转速","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WGEN.GenSpd","发电机转速","generator_speed","l_贺家沟一期Ⅶ-05 发电机转速","yc_hs_0640","cur_70"]
[3664,"l_贺家沟一期Ⅶ-05 发电机U相温度","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","l_贺家沟一期Ⅶ-05 发电机U相温度","yc_hs_0640","cur_99"]
[3665,"l_贺家沟一期Ⅶ-05 发电机V相温度","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","l_贺家沟一期Ⅶ-05 发电机V相温度","yc_hs_0640","cur_100"]
[3666,"l_贺家沟一期Ⅶ-05 发电机W相温度","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","l_贺家沟一期Ⅶ-05 发电机W相温度","yc_hs_0641","cur_01"]
[3667,"l_贺家沟一期Ⅶ-05 发电机轴承温度","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","l_贺家沟一期Ⅶ-05 发电机轴承温度","yc_hs_0641","cur_02"]
[3668,"l_贺家沟一期Ⅶ-05 发电机轴承2温度","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","l_贺家沟一期Ⅶ-05 发电机轴承2温度","yc_hs_0641","cur_03"]
[3669,"l_贺家沟一期Ⅶ-05 齿轮箱高速轴前轴承温度","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","l_贺家沟一期Ⅶ-05 齿轮箱高速轴前轴承温度","yc_hs_0641","cur_04"]
[3670,"l_贺家沟一期Ⅶ-05 机舱内温度","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WNAC.TemNacelle","机舱内温度","cabin_temperature","l_贺家沟一期Ⅶ-05 机舱内温度","yc_hs_0641","cur_31"]
[3671,"l_贺家沟一期Ⅶ-05 变流器有功功率","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WCNV.DemandActPow","有功功率","active_power","l_贺家沟一期Ⅶ-05 变流器有功功率","yc_hs_0641","cur_61"]
[3672,"l_贺家沟一期Ⅶ-05 塔筒左右振动","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WTUR.YC032","机舱左右振动","side_to_side_vibration_of_the_cabin","l_贺家沟一期Ⅶ-05 塔筒左右振动","yc_hs_0641","cur_63"]
[3673,"l_贺家沟一期Ⅶ-05 塔筒前后振动","贺家沟","WOF35800080",5,"SSLF20219.T1_L7.WTG005.WTUR.YC033","机舱前后振动","front_back_vibration_of_the_cabin","l_贺家沟一期Ⅶ-05 塔筒前后振动","yc_hs_0641","cur_64"]
[3674,"l_贺家沟一期Ⅶ-06 环境温度","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WNAC.TemOut","环境温度","outside_cabin_temperature","l_贺家沟一期Ⅶ-06 环境温度","yc_hs_0641","cur_97"]
[3675,"l_贺家沟一期Ⅶ-06 风速1s","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WNAC.WindSpeed","风速","wind_velocity","l_贺家沟一期Ⅶ-06 风速1s","yc_hs_0641","cur_99"]
[3676,"l_贺家沟一期Ⅶ-06 绝对风向","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WNAC.WindDirection","绝对风向","true_wind_direction","l_贺家沟一期Ⅶ-06 绝对风向","yc_hs_0642","cur_01"]
[3677,"l_贺家沟一期Ⅶ-06 偏航误差","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WYAW.YawError","对风角度","yaw_error1","l_贺家沟一期Ⅶ-06 偏航误差","yc_hs_0642","cur_04"]
[3678,"l_贺家沟一期Ⅶ-06 桨角1","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","l_贺家沟一期Ⅶ-06 桨角1","yc_hs_0642","cur_05"]
[3679,"l_贺家沟一期Ⅶ-06 桨角2","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","l_贺家沟一期Ⅶ-06 桨角2","yc_hs_0642","cur_06"]
[3680,"l_贺家沟一期Ⅶ-06 桨角3","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","l_贺家沟一期Ⅶ-06 桨角3","yc_hs_0642","cur_07"]
[3681,"l_贺家沟一期Ⅶ-06 风轮转速","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WTRM.RotorSpd","风轮转速","rotor_speed","l_贺家沟一期Ⅶ-06 风轮转速","yc_hs_0642","cur_08"]
[3682,"l_贺家沟一期Ⅶ-06 发电机转速","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WGEN.GenSpd","发电机转速","generator_speed","l_贺家沟一期Ⅶ-06 发电机转速","yc_hs_0642","cur_09"]
[3683,"l_贺家沟一期Ⅶ-06 发电机U相温度","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","l_贺家沟一期Ⅶ-06 发电机U相温度","yc_hs_0642","cur_38"]
[3684,"l_贺家沟一期Ⅶ-06 发电机V相温度","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","l_贺家沟一期Ⅶ-06 发电机V相温度","yc_hs_0642","cur_39"]
[3685,"l_贺家沟一期Ⅶ-06 发电机W相温度","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","l_贺家沟一期Ⅶ-06 发电机W相温度","yc_hs_0642","cur_40"]
[3686,"l_贺家沟一期Ⅶ-06 发电机轴承温度","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","l_贺家沟一期Ⅶ-06 发电机轴承温度","yc_hs_0642","cur_41"]
[3687,"l_贺家沟一期Ⅶ-06 发电机轴承2温度","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","l_贺家沟一期Ⅶ-06 发电机轴承2温度","yc_hs_0642","cur_42"]
[3688,"l_贺家沟一期Ⅶ-06 齿轮箱高速轴前轴承温度","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","l_贺家沟一期Ⅶ-06 齿轮箱高速轴前轴承温度","yc_hs_0642","cur_43"]
[3689,"l_贺家沟一期Ⅶ-06 机舱内温度","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WNAC.TemNacelle","机舱内温度","cabin_temperature","l_贺家沟一期Ⅶ-06 机舱内温度","yc_hs_0642","cur_70"]
[3690,"l_贺家沟一期Ⅶ-06 变流器有功功率","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WCNV.DemandActPow","有功功率","active_power","l_贺家沟一期Ⅶ-06 变流器有功功率","yc_hs_0642","cur_100"]
[3691,"l_贺家沟一期Ⅶ-06 塔筒左右振动","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WTUR.YC032","机舱左右振动","side_to_side_vibration_of_the_cabin","l_贺家沟一期Ⅶ-06 塔筒左右振动","yc_hs_0643","cur_02"]
[3692,"l_贺家沟一期Ⅶ-06 塔筒前后振动","贺家沟","WOF35800080",6,"SSLF20219.T1_L7.WTG006.WTUR.YC033","机舱前后振动","front_back_vibration_of_the_cabin","l_贺家沟一期Ⅶ-06 塔筒前后振动","yc_hs_0643","cur_03"]
[3693,"l_贺家沟一期Ⅶ-07 环境温度","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WNAC.TemOut","环境温度","outside_cabin_temperature","l_贺家沟一期Ⅶ-07 环境温度","yc_hs_0643","cur_36"]
[3694,"l_贺家沟一期Ⅶ-07 风速1s","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WNAC.WindSpeed","风速","wind_velocity","l_贺家沟一期Ⅶ-07 风速1s","yc_hs_0643","cur_38"]
[3695,"l_贺家沟一期Ⅶ-07 绝对风向","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WNAC.WindDirection","绝对风向","true_wind_direction","l_贺家沟一期Ⅶ-07 绝对风向","yc_hs_0643","cur_40"]
[3696,"l_贺家沟一期Ⅶ-07 偏航误差","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WYAW.YawError","对风角度","yaw_error1","l_贺家沟一期Ⅶ-07 偏航误差","yc_hs_0643","cur_43"]
[3697,"l_贺家沟一期Ⅶ-07 桨角1","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","l_贺家沟一期Ⅶ-07 桨角1","yc_hs_0643","cur_44"]
[3698,"l_贺家沟一期Ⅶ-07 桨角2","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","l_贺家沟一期Ⅶ-07 桨角2","yc_hs_0643","cur_45"]
[3699,"l_贺家沟一期Ⅶ-07 桨角3","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","l_贺家沟一期Ⅶ-07 桨角3","yc_hs_0643","cur_46"]
[3700,"l_贺家沟一期Ⅶ-07 风轮转速","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WTRM.RotorSpd","风轮转速","rotor_speed","l_贺家沟一期Ⅶ-07 风轮转速","yc_hs_0643","cur_47"]
[3701,"l_贺家沟一期Ⅶ-07 发电机转速","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WGEN.GenSpd","发电机转速","generator_speed","l_贺家沟一期Ⅶ-07 发电机转速","yc_hs_0643","cur_48"]
[3702,"l_贺家沟一期Ⅶ-07 发电机U相温度","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","l_贺家沟一期Ⅶ-07 发电机U相温度","yc_hs_0643","cur_77"]
[3703,"l_贺家沟一期Ⅶ-07 发电机V相温度","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","l_贺家沟一期Ⅶ-07 发电机V相温度","yc_hs_0643","cur_78"]
[3704,"l_贺家沟一期Ⅶ-07 发电机W相温度","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","l_贺家沟一期Ⅶ-07 发电机W相温度","yc_hs_0643","cur_79"]
[3705,"l_贺家沟一期Ⅶ-07 发电机轴承温度","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","l_贺家沟一期Ⅶ-07 发电机轴承温度","yc_hs_0643","cur_80"]
[3706,"l_贺家沟一期Ⅶ-07 发电机轴承2温度","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","l_贺家沟一期Ⅶ-07 发电机轴承2温度","yc_hs_0643","cur_81"]
[3707,"l_贺家沟一期Ⅶ-07 齿轮箱高速轴前轴承温度","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","l_贺家沟一期Ⅶ-07 齿轮箱高速轴前轴承温度","yc_hs_0643","cur_82"]
[3708,"l_贺家沟一期Ⅶ-07 机舱内温度","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WNAC.TemNacelle","机舱内温度","cabin_temperature","l_贺家沟一期Ⅶ-07 机舱内温度","yc_hs_0644","cur_09"]
[3709,"l_贺家沟一期Ⅶ-07 变流器有功功率","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WCNV.DemandActPow","有功功率","active_power","l_贺家沟一期Ⅶ-07 变流器有功功率","yc_hs_0644","cur_39"]
[3710,"l_贺家沟一期Ⅶ-07 塔筒左右振动","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WTUR.YC032","机舱左右振动","side_to_side_vibration_of_the_cabin","l_贺家沟一期Ⅶ-07 塔筒左右振动","yc_hs_0644","cur_41"]
[3711,"l_贺家沟一期Ⅶ-07 塔筒前后振动","贺家沟","WOF35800080",7,"SSLF20219.T1_L7.WTG007.WTUR.YC033","机舱前后振动","front_back_vibration_of_the_cabin","l_贺家沟一期Ⅶ-07 塔筒前后振动","yc_hs_0644","cur_42"]
[3712,"l_贺家沟一期Ⅶ-08 环境温度","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WNAC.TemOut","环境温度","outside_cabin_temperature","l_贺家沟一期Ⅶ-08 环境温度","yc_hs_0644","cur_75"]
[3713,"l_贺家沟一期Ⅶ-08 风速1s","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WNAC.WindSpeed","风速","wind_velocity","l_贺家沟一期Ⅶ-08 风速1s","yc_hs_0644","cur_77"]
[3714,"l_贺家沟一期Ⅶ-08 绝对风向","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WNAC.WindDirection","绝对风向","true_wind_direction","l_贺家沟一期Ⅶ-08 绝对风向","yc_hs_0644","cur_79"]
[3715,"l_贺家沟一期Ⅶ-08 偏航误差","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WYAW.YawError","对风角度","yaw_error1","l_贺家沟一期Ⅶ-08 偏航误差","yc_hs_0644","cur_82"]
[3716,"l_贺家沟一期Ⅶ-08 桨角1","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","l_贺家沟一期Ⅶ-08 桨角1","yc_hs_0644","cur_83"]
[3717,"l_贺家沟一期Ⅶ-08 桨角2","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","l_贺家沟一期Ⅶ-08 桨角2","yc_hs_0644","cur_84"]
[3718,"l_贺家沟一期Ⅶ-08 桨角3","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","l_贺家沟一期Ⅶ-08 桨角3","yc_hs_0644","cur_85"]
[3719,"l_贺家沟一期Ⅶ-08 风轮转速","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WTRM.RotorSpd","风轮转速","rotor_speed","l_贺家沟一期Ⅶ-08 风轮转速","yc_hs_0644","cur_86"]
[3720,"l_贺家沟一期Ⅶ-08 发电机转速","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WGEN.GenSpd","发电机转速","generator_speed","l_贺家沟一期Ⅶ-08 发电机转速","yc_hs_0644","cur_87"]
[3721,"l_贺家沟一期Ⅶ-08 发电机U相温度","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WGEN.TemL1","发电机绕组1温度","generator_winding1_temperature","l_贺家沟一期Ⅶ-08 发电机U相温度","yc_hs_0645","cur_16"]
[3722,"l_贺家沟一期Ⅶ-08 发电机V相温度","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WGEN.TemL2","发电机绕组2温度","generator_winding2_temperature","l_贺家沟一期Ⅶ-08 发电机V相温度","yc_hs_0645","cur_17"]
[3723,"l_贺家沟一期Ⅶ-08 发电机W相温度","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WGEN.TemL3","发电机绕组3温度","generator_winding3_temperature","l_贺家沟一期Ⅶ-08 发电机W相温度","yc_hs_0645","cur_18"]
[3724,"l_贺家沟一期Ⅶ-08 发电机轴承温度","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","l_贺家沟一期Ⅶ-08 发电机轴承温度","yc_hs_0645","cur_19"]
[3725,"l_贺家沟一期Ⅶ-08 发电机轴承2温度","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","l_贺家沟一期Ⅶ-08 发电机轴承2温度","yc_hs_0645","cur_20"]
[3726,"l_贺家沟一期Ⅶ-08 齿轮箱高速轴前轴承温度","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","l_贺家沟一期Ⅶ-08 齿轮箱高速轴前轴承温度","yc_hs_0645","cur_21"]
[3727,"l_贺家沟一期Ⅶ-08 机舱内温度","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WNAC.TemNacelle","机舱内温度","cabin_temperature","l_贺家沟一期Ⅶ-08 机舱内温度","yc_hs_0645","cur_48"]
[3728,"l_贺家沟一期Ⅶ-08 变流器有功功率","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WCNV.DemandActPow","有功功率","active_power","l_贺家沟一期Ⅶ-08 变流器有功功率","yc_hs_0645","cur_78"]
[3729,"l_贺家沟一期Ⅶ-08 塔筒左右振动","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WTUR.YC032","机舱左右振动","side_to_side_vibration_of_the_cabin","l_贺家沟一期Ⅶ-08 塔筒左右振动","yc_hs_0645","cur_80"]
[3730,"l_贺家沟一期Ⅶ-08 塔筒前后振动","贺家沟","WOF35800080",8,"SSLF20219.T1_L7.WTG008.WTUR.YC033","机舱前后振动","front_back_vibration_of_the_cabin","l_贺家沟一期Ⅶ-08 塔筒前后振动","yc_hs_0645","cur_81"]