{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":6466,"n_cols":11,"rows_kept":6466,"cut":false,"hidden":false,"merged":[]}
["顺序号","遥测ID号","场站","场站标准化编号","风机号","遥测别名","标准化中文","标准化英文","遥测ID","历史采样表名","历史采样域名"]
[0,"b_右玉一期I-001 3#桨叶片角度","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期I-001 3#桨叶片角度","yc_hs_0359","cur_83"]
[1,"b_右玉一期I-001机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期I-001机舱侧向振动(已滤波)","yc_hs_0360","cur_11"]
[2,"b_右玉一期I-001机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期I-001机舱轴向振动(已滤波)","yc_hs_0360","cur_13"]
[3,"b_右玉一期I-001机舱角度","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期I-001机舱角度","yc_hs_0360","cur_14"]
[5,"b_右玉一期I-003机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期I-003机舱侧向振动(已滤波)","yc_hs_0361","cur_53"]
[6,"b_右玉一期I-003机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期I-003机舱轴向振动(已滤波)","yc_hs_0361","cur_55"]
[7,"b_右玉一期I-003机舱角度","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期I-003机舱角度","yc_hs_0361","cur_56"]
[9,"b_右玉一期I-004发电机有功功率","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WGEN.GenActivePW","有功功率","active_power","b_右玉一期I-004发电机有功功率","yc_hs_0361","cur_68"]
[10,"b_右玉一期I-004发电机 绕组温度1","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期I-004发电机 绕组温度1","yc_hs_0361","cur_71"]
[11,"b_右玉一期I-004发电机 绕组温度2","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期I-004发电机 绕组温度2","yc_hs_0361","cur_72"]
[12,"b_右玉一期I-005发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期I-005发电机驱动端轴承温度","yc_hs_0362","cur_49"]
[13,"b_右玉一期I-005发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期I-005发电机非驱动端轴承温度","yc_hs_0362","cur_50"]
[14,"b_右玉一期I-005舱内温度","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期I-005舱内温度","yc_hs_0362","cur_56"]
[15,"b_右玉一期I-005舱外温度","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期I-005舱外温度","yc_hs_0362","cur_58"]
[16,"b_右玉一期I-005风向","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期I-005风向","yc_hs_0362","cur_60"]
[17,"b_右玉一期I-005风速","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期I-005风速","yc_hs_0362","cur_61"]
[18,"b_右玉一期I-005机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期I-005机舱中轴线与风向夹角","yc_hs_0362","cur_62"]
[19,"b_右玉一期I-005 1#桨叶片角度","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期I-005 1#桨叶片角度","yc_hs_0362","cur_64"]
[20,"b_右玉一期I-005 2#桨叶片角度","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期I-005 2#桨叶片角度","yc_hs_0362","cur_66"]
[21,"b_右玉一期I-005 3#桨叶片角度","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期I-005 3#桨叶片角度","yc_hs_0362","cur_68"]
[22,"b_右玉一期I-006机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期I-006机舱侧向振动(已滤波)","yc_hs_0363","cur_69"]
[23,"b_右玉一期I-006机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期I-006机舱轴向振动(已滤波)","yc_hs_0363","cur_71"]
[24,"b_右玉一期I-006机舱角度","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期I-006机舱角度","yc_hs_0363","cur_72"]
[26,"b_右玉一期I-007发电机有功功率","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WGEN.GenActivePW","有功功率","active_power","b_右玉一期I-007发电机有功功率","yc_hs_0363","cur_84"]
[27,"b_右玉一期I-007发电机 绕组温度1","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期I-007发电机 绕组温度1","yc_hs_0363","cur_87"]
[28,"b_右玉一期I-007发电机 绕组温度2","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期I-007发电机 绕组温度2","yc_hs_0363","cur_88"]
[29,"b_右玉一期I-007发电机 绕组温度3","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期I-007发电机 绕组温度3","yc_hs_0363","cur_89"]
[30,"b_右玉一期I-007发电机转速","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期I-007发电机转速","yc_hs_0363","cur_93"]
[31,"b_右玉一期I-007发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期I-007发电机驱动端轴承温度","yc_hs_0363","cur_94"]
[32,"b_右玉一期I-007发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期I-007发电机非驱动端轴承温度","yc_hs_0363","cur_95"]
[33,"b_右玉一期I-002发电机有功功率","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WGEN.GenActivePW","有功功率","active_power","b_右玉一期I-002发电机有功功率","yc_hs_0360","cur_26"]
[34,"b_右玉一期I-002发电机 绕组温度1","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期I-002发电机 绕组温度1","yc_hs_0360","cur_29"]
[35,"b_右玉一期I-002发电机 绕组温度2","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期I-002发电机 绕组温度2","yc_hs_0360","cur_30"]
[36,"b_右玉一期I-002发电机 绕组温度3","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期I-002发电机 绕组温度3","yc_hs_0360","cur_31"]
[37,"b_右玉一期I-002发电机转速","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期I-002发电机转速","yc_hs_0360","cur_35"]
[38,"b_右玉一期I-002发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期I-002发电机驱动端轴承温度","yc_hs_0360","cur_36"]
[39,"b_右玉一期I-002发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期I-002发电机非驱动端轴承温度","yc_hs_0360","cur_37"]
[40,"b_右玉一期I-002舱内温度","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期I-002舱内温度","yc_hs_0360","cur_43"]
[41,"b_右玉一期I-002舱外温度","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期I-002舱外温度","yc_hs_0360","cur_45"]
[42,"b_右玉一期I-002风向","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期I-002风向","yc_hs_0360","cur_47"]
[43,"b_右玉一期I-002风速","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期I-002风速","yc_hs_0360","cur_48"]
[44,"b_右玉一期I-002机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期I-002机舱中轴线与风向夹角","yc_hs_0360","cur_49"]
[45,"b_右玉一期I-002 1#桨叶片角度","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期I-002 1#桨叶片角度","yc_hs_0360","cur_51"]
[46,"b_右玉一期I-002 2#桨叶片角度","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期I-002 2#桨叶片角度","yc_hs_0360","cur_53"]
[47,"b_右玉一期I-002 3#桨叶片角度","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期I-002 3#桨叶片角度","yc_hs_0360","cur_55"]
[48,"b_右玉一期I-008风速","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期I-008风速","yc_hs_0364","cur_76"]
[49,"b_右玉一期I-008机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期I-008机舱中轴线与风向夹角","yc_hs_0364","cur_77"]
[50,"b_右玉一期I-008 1#桨叶片角度","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期I-008 1#桨叶片角度","yc_hs_0364","cur_78"]
[51,"b_右玉一期I-008 2#桨叶片角度","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期I-008 2#桨叶片角度","yc_hs_0364","cur_80"]
[52,"b_右玉一期I-008 3#桨叶片角度","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期I-008 3#桨叶片角度","yc_hs_0364","cur_82"]
[53,"b_右玉一期I-008机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期I-008机舱侧向振动(已滤波)","yc_hs_0365","cur_10"]
[54,"b_右玉一期I-008机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期I-008机舱轴向振动(已滤波)","yc_hs_0365","cur_12"]
[55,"b_右玉一期I-008机舱角度","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期I-008机舱角度","yc_hs_0365","cur_13"]
[56,"b_右玉一期I-005机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期I-005机舱侧向振动(已滤波)","yc_hs_0362","cur_95"]
[57,"b_右玉一期I-005机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期I-005机舱轴向振动(已滤波)","yc_hs_0362","cur_97"]
[58,"b_右玉一期I-005机舱角度","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期I-005机舱角度","yc_hs_0362","cur_98"]
[60,"b_右玉一期I-006发电机有功功率","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WGEN.GenActivePW","有功功率","active_power","b_右玉一期I-006发电机有功功率","yc_hs_0363","cur_10"]
[61,"b_右玉一期I-006发电机 绕组温度1","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期I-006发电机 绕组温度1","yc_hs_0363","cur_13"]
[62,"b_右玉一期I-006发电机 绕组温度2","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期I-006发电机 绕组温度2","yc_hs_0363","cur_14"]
[63,"b_右玉一期I-006发电机 绕组温度3","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期I-006发电机 绕组温度3","yc_hs_0363","cur_15"]
[64,"b_右玉一期I-006发电机转速","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期I-006发电机转速","yc_hs_0363","cur_19"]
[65,"b_右玉一期I-006发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期I-006发电机驱动端轴承温度","yc_hs_0363","cur_20"]
[66,"b_右玉一期I-006发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期I-006发电机非驱动端轴承温度","yc_hs_0363","cur_21"]
[67,"b_右玉一期I-007舱内温度","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期I-007舱内温度","yc_hs_0364","cur_01"]
[68,"b_右玉一期I-007舱外温度","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期I-007舱外温度","yc_hs_0364","cur_03"]
[69,"b_右玉一期I-007风向","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期I-007风向","yc_hs_0364","cur_05"]
[70,"b_右玉一期I-007风速","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期I-007风速","yc_hs_0364","cur_06"]
[71,"b_右玉一期I-007机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期I-007机舱中轴线与风向夹角","yc_hs_0364","cur_07"]
[72,"b_右玉一期I-007 1#桨叶片角度","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期I-007 1#桨叶片角度","yc_hs_0364","cur_08"]
[73,"b_右玉一期I-007 2#桨叶片角度","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期I-007 2#桨叶片角度","yc_hs_0364","cur_10"]
[74,"b_右玉一期I-007 3#桨叶片角度","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期I-007 3#桨叶片角度","yc_hs_0364","cur_12"]
[75,"b_右玉一期I-007机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期I-007机舱侧向振动(已滤波)","yc_hs_0364","cur_39"]
[76,"b_右玉一期I-007机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期I-007机舱轴向振动(已滤波)","yc_hs_0364","cur_41"]
[77,"b_右玉一期I-007机舱角度","右玉风光互补电站","WOF34900079",7,"SXYY.T1_L1.WTG007.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期I-007机舱角度","yc_hs_0364","cur_42"]
[79,"b_右玉一期I-008发电机有功功率","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WGEN.GenActivePW","有功功率","active_power","b_右玉一期I-008发电机有功功率","yc_hs_0364","cur_54"]
[80,"b_右玉一期I-008发电机 绕组温度1","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期I-008发电机 绕组温度1","yc_hs_0364","cur_57"]
[81,"b_右玉一期I-008发电机 绕组温度2","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期I-008发电机 绕组温度2","yc_hs_0364","cur_58"]
[82,"b_右玉一期I-008发电机 绕组温度3","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期I-008发电机 绕组温度3","yc_hs_0364","cur_59"]
[83,"b_右玉一期I-008发电机转速","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期I-008发电机转速","yc_hs_0364","cur_63"]
[84,"b_右玉一期I-008发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期I-008发电机驱动端轴承温度","yc_hs_0364","cur_64"]
[85,"b_右玉一期I-008发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期I-008发电机非驱动端轴承温度","yc_hs_0364","cur_65"]
[86,"b_右玉一期I-008舱内温度","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期I-008舱内温度","yc_hs_0364","cur_71"]
[87,"b_右玉一期I-008舱外温度","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期I-008舱外温度","yc_hs_0364","cur_73"]
[88,"b_右玉一期I-008风向","右玉风光互补电站","WOF34900079",8,"SXYY.T1_L1.WTG008.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期I-008风向","yc_hs_0364","cur_75"]
[90,"b_右玉一期I-009发电机有功功率","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WGEN.GenActivePW","有功功率","active_power","b_右玉一期I-009发电机有功功率","yc_hs_0365","cur_25"]
[91,"b_右玉一期I-009发电机 绕组温度1","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期I-009发电机 绕组温度1","yc_hs_0365","cur_28"]
[92,"b_右玉一期I-009发电机 绕组温度2","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期I-009发电机 绕组温度2","yc_hs_0365","cur_29"]
[93,"b_右玉一期I-009发电机 绕组温度3","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期I-009发电机 绕组温度3","yc_hs_0365","cur_30"]
[94,"b_右玉一期I-009发电机转速","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期I-009发电机转速","yc_hs_0365","cur_34"]
[95,"b_右玉一期I-009发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期I-009发电机驱动端轴承温度","yc_hs_0365","cur_35"]
[96,"b_右玉一期I-009发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期I-009发电机非驱动端轴承温度","yc_hs_0365","cur_36"]
[97,"b_右玉一期I-009舱内温度","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期I-009舱内温度","yc_hs_0365","cur_42"]
[98,"b_右玉一期I-009舱外温度","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期I-009舱外温度","yc_hs_0365","cur_44"]
[99,"b_右玉一期I-009风向","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期I-009风向","yc_hs_0365","cur_46"]
[100,"b_右玉一期I-009风速","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期I-009风速","yc_hs_0365","cur_47"]
[101,"b_右玉一期I-009机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期I-009机舱中轴线与风向夹角","yc_hs_0365","cur_48"]
[102,"b_右玉一期I-009 1#桨叶片角度","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期I-009 1#桨叶片角度","yc_hs_0365","cur_49"]
[103,"b_右玉一期I-009 2#桨叶片角度","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期I-009 2#桨叶片角度","yc_hs_0365","cur_51"]
[104,"b_右玉一期I-009 3#桨叶片角度","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期I-009 3#桨叶片角度","yc_hs_0365","cur_53"]
[105,"b_右玉一期I-009机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期I-009机舱侧向振动(已滤波)","yc_hs_0365","cur_81"]
[106,"b_右玉一期I-009机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期I-009机舱轴向振动(已滤波)","yc_hs_0365","cur_83"]
[107,"b_右玉一期I-009机舱角度","右玉风光互补电站","WOF34900079",9,"SXYY.T1_L1.WTG009.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期I-009机舱角度","yc_hs_0365","cur_84"]
[109,"b_右玉一期I-010发电机有功功率","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WGEN.GenActivePW","有功功率","active_power","b_右玉一期I-010发电机有功功率","yc_hs_0365","cur_96"]
[110,"b_右玉一期I-010发电机 绕组温度1","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期I-010发电机 绕组温度1","yc_hs_0365","cur_99"]
[111,"b_右玉一期I-010发电机 绕组温度2","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期I-010发电机 绕组温度2","yc_hs_0365","cur_100"]
[112,"b_右玉一期I-010发电机 绕组温度3","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期I-010发电机 绕组温度3","yc_hs_0366","cur_01"]
[113,"b_右玉一期I-010发电机转速","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期I-010发电机转速","yc_hs_0366","cur_05"]
[114,"b_右玉一期I-010发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期I-010发电机驱动端轴承温度","yc_hs_0366","cur_06"]
[115,"b_右玉一期I-010发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期I-010发电机非驱动端轴承温度","yc_hs_0366","cur_07"]
[116,"b_右玉一期I-010舱内温度","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期I-010舱内温度","yc_hs_0366","cur_13"]
[117,"b_右玉一期I-010舱外温度","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期I-010舱外温度","yc_hs_0366","cur_15"]
[118,"b_右玉一期I-010风向","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期I-010风向","yc_hs_0366","cur_17"]
[119,"b_右玉一期I-010风速","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期I-010风速","yc_hs_0366","cur_18"]
[120,"b_右玉一期I-010机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期I-010机舱中轴线与风向夹角","yc_hs_0366","cur_19"]
[121,"b_右玉一期I-010 1#桨叶片角度","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期I-010 1#桨叶片角度","yc_hs_0366","cur_20"]
[122,"b_右玉一期I-010 2#桨叶片角度","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期I-010 2#桨叶片角度","yc_hs_0366","cur_22"]
[123,"b_右玉一期I-010 3#桨叶片角度","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期I-010 3#桨叶片角度","yc_hs_0366","cur_24"]
[124,"b_右玉一期Ⅲ-026发电机有功功率","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅲ-026发电机有功功率","yc_hs_0377","cur_32"]
[125,"b_右玉一期Ⅲ-026发电机 绕组温度1","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅲ-026发电机 绕组温度1","yc_hs_0377","cur_35"]
[126,"b_右玉一期Ⅲ-026发电机 绕组温度2","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅲ-026发电机 绕组温度2","yc_hs_0377","cur_36"]
[127,"b_右玉一期Ⅲ-026发电机 绕组温度3","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅲ-026发电机 绕组温度3","yc_hs_0377","cur_37"]
[128,"b_右玉一期Ⅲ-026发电机转速","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅲ-026发电机转速","yc_hs_0377","cur_41"]
[129,"b_右玉一期Ⅲ-026发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅲ-026发电机驱动端轴承温度","yc_hs_0377","cur_42"]
[130,"b_右玉一期Ⅲ-026发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅲ-026发电机非驱动端轴承温度","yc_hs_0377","cur_43"]
[131,"b_右玉一期Ⅲ-026舱内温度","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅲ-026舱内温度","yc_hs_0377","cur_49"]
[132,"b_右玉一期Ⅲ-026舱外温度","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅲ-026舱外温度","yc_hs_0377","cur_51"]
[133,"b_右玉一期Ⅲ-026风向","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅲ-026风向","yc_hs_0377","cur_53"]
[134,"b_右玉一期Ⅲ-026风速","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅲ-026风速","yc_hs_0377","cur_54"]
[135,"b_右玉一期Ⅲ-026机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅲ-026机舱中轴线与风向夹角","yc_hs_0377","cur_55"]
[136,"b_右玉一期Ⅲ-026 1#桨叶片角度","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅲ-026 1#桨叶片角度","yc_hs_0377","cur_56"]
[137,"b_右玉一期Ⅲ-026 2#桨叶片角度","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅲ-026 2#桨叶片角度","yc_hs_0377","cur_58"]
[138,"b_右玉一期Ⅲ-026 3#桨叶片角度","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅲ-026 3#桨叶片角度","yc_hs_0377","cur_60"]
[139,"b_右玉一期I-010机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期I-010机舱侧向振动(已滤波)","yc_hs_0366","cur_52"]
[140,"b_右玉一期I-010机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期I-010机舱轴向振动(已滤波)","yc_hs_0366","cur_54"]
[141,"b_右玉一期I-010机舱角度","右玉风光互补电站","WOF34900079",10,"SXYY.T1_L1.WTG010.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期I-010机舱角度","yc_hs_0366","cur_55"]
[143,"b_右玉一期Ⅱ-015机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅱ-015机舱侧向振动(已滤波)","yc_hs_0370","cur_07"]
[144,"b_右玉一期Ⅱ-015机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅱ-015机舱轴向振动(已滤波)","yc_hs_0370","cur_09"]
[145,"b_右玉一期Ⅱ-015机舱角度","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅱ-015机舱角度","yc_hs_0370","cur_10"]
[147,"b_右玉一期Ⅱ-016发电机有功功率","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅱ-016发电机有功功率","yc_hs_0370","cur_22"]
[148,"b_右玉一期Ⅱ-016发电机 绕组温度1","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅱ-016发电机 绕组温度1","yc_hs_0370","cur_25"]
[149,"b_右玉一期Ⅱ-016发电机 绕组温度2","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅱ-016发电机 绕组温度2","yc_hs_0370","cur_26"]
[150,"b_右玉一期Ⅱ-016发电机 绕组温度3","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅱ-016发电机 绕组温度3","yc_hs_0370","cur_27"]
[151,"b_右玉一期Ⅱ-016发电机转速","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅱ-016发电机转速","yc_hs_0370","cur_31"]
[152,"b_右玉一期Ⅱ-016发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅱ-016发电机驱动端轴承温度","yc_hs_0370","cur_32"]
[153,"b_右玉一期Ⅱ-016发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅱ-016发电机非驱动端轴承温度","yc_hs_0370","cur_33"]
[154,"b_右玉一期Ⅱ-016舱内温度","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅱ-016舱内温度","yc_hs_0370","cur_39"]
[155,"b_右玉一期Ⅱ-016舱外温度","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅱ-016舱外温度","yc_hs_0370","cur_41"]
[156,"b_右玉一期Ⅱ-021发电机转速","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅱ-021发电机转速","yc_hs_0373","cur_86"]
[157,"b_右玉一期Ⅱ-021发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅱ-021发电机驱动端轴承温度","yc_hs_0373","cur_87"]
[158,"b_右玉一期Ⅱ-021发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅱ-021发电机非驱动端轴承温度","yc_hs_0373","cur_88"]
[159,"b_右玉一期Ⅱ-021舱内温度","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅱ-021舱内温度","yc_hs_0373","cur_94"]
[160,"b_右玉一期Ⅱ-021舱外温度","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅱ-021舱外温度","yc_hs_0373","cur_96"]
[161,"b_右玉一期Ⅱ-021风向","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅱ-021风向","yc_hs_0373","cur_98"]
[162,"b_右玉一期Ⅱ-021风速","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅱ-021风速","yc_hs_0373","cur_99"]
[163,"b_右玉一期Ⅱ-021机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅱ-021机舱中轴线与风向夹角","yc_hs_0373","cur_100"]
[164,"b_右玉一期Ⅱ-021 1#桨叶片角度","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅱ-021 1#桨叶片角度","yc_hs_0374","cur_01"]
[165,"b_右玉一期Ⅱ-021 2#桨叶片角度","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅱ-021 2#桨叶片角度","yc_hs_0374","cur_03"]
[166,"b_右玉一期Ⅱ-021 3#桨叶片角度","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅱ-021 3#桨叶片角度","yc_hs_0374","cur_05"]
[167,"b_右玉一期Ⅲ-030机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅲ-030机舱侧向振动(已滤波)","yc_hs_0380","cur_72"]
[168,"b_右玉一期Ⅲ-030机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅲ-030机舱轴向振动(已滤波)","yc_hs_0380","cur_74"]
[169,"b_右玉一期Ⅲ-030机舱角度","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅲ-030机舱角度","yc_hs_0380","cur_75"]
[171,"b_右玉一期Ⅲ-031发电机有功功率","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅲ-031发电机有功功率","yc_hs_0380","cur_87"]
[172,"b_右玉一期Ⅲ-031发电机 绕组温度1","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅲ-031发电机 绕组温度1","yc_hs_0380","cur_90"]
[173,"b_右玉一期Ⅲ-031发电机 绕组温度2","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅲ-031发电机 绕组温度2","yc_hs_0380","cur_91"]
[174,"b_右玉一期Ⅲ-031发电机 绕组温度3","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅲ-031发电机 绕组温度3","yc_hs_0380","cur_92"]
[175,"b_右玉一期Ⅲ-031发电机转速","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅲ-031发电机转速","yc_hs_0380","cur_96"]
[176,"b_右玉一期Ⅲ-031发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅲ-031发电机驱动端轴承温度","yc_hs_0380","cur_97"]
[177,"b_右玉一期Ⅲ-031发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅲ-031发电机非驱动端轴承温度","yc_hs_0380","cur_98"]
[178,"b_右玉一期I-011发电机有功功率","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WGEN.GenActivePW","有功功率","active_power","b_右玉一期I-011发电机有功功率","yc_hs_0366","cur_67"]
[179,"b_右玉一期I-011发电机 绕组温度1","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期I-011发电机 绕组温度1","yc_hs_0366","cur_70"]
[180,"b_右玉一期I-011发电机 绕组温度2","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期I-011发电机 绕组温度2","yc_hs_0366","cur_71"]
[181,"b_右玉一期I-011发电机 绕组温度3","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期I-011发电机 绕组温度3","yc_hs_0366","cur_72"]
[182,"b_右玉一期I-011发电机转速","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期I-011发电机转速","yc_hs_0366","cur_76"]
[183,"b_右玉一期I-011发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期I-011发电机驱动端轴承温度","yc_hs_0366","cur_77"]
[184,"b_右玉一期I-011发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期I-011发电机非驱动端轴承温度","yc_hs_0366","cur_78"]
[185,"b_右玉一期I-011舱内温度","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期I-011舱内温度","yc_hs_0366","cur_84"]
[186,"b_右玉一期I-011舱外温度","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期I-011舱外温度","yc_hs_0366","cur_86"]
[187,"b_右玉一期I-011风向","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期I-011风向","yc_hs_0366","cur_88"]
[188,"b_右玉一期I-011风速","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期I-011风速","yc_hs_0366","cur_89"]
[189,"b_右玉一期I-011机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期I-011机舱中轴线与风向夹角","yc_hs_0366","cur_90"]
[190,"b_右玉一期I-011 1#桨叶片角度","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期I-011 1#桨叶片角度","yc_hs_0366","cur_91"]
[191,"b_右玉一期I-011 2#桨叶片角度","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期I-011 2#桨叶片角度","yc_hs_0366","cur_93"]
[192,"b_右玉一期I-011 3#桨叶片角度","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期I-011 3#桨叶片角度","yc_hs_0366","cur_95"]
[193,"b_右玉一期Ⅱ-016风向","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅱ-016风向","yc_hs_0370","cur_43"]
[194,"b_右玉一期Ⅱ-016风速","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅱ-016风速","yc_hs_0370","cur_44"]
[195,"b_右玉一期Ⅱ-016机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅱ-016机舱中轴线与风向夹角","yc_hs_0370","cur_45"]
[196,"b_右玉一期Ⅱ-016 1#桨叶片角度","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅱ-016 1#桨叶片角度","yc_hs_0370","cur_46"]
[197,"b_右玉一期Ⅱ-016 2#桨叶片角度","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅱ-016 2#桨叶片角度","yc_hs_0370","cur_48"]
[198,"b_右玉一期Ⅱ-016 3#桨叶片角度","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅱ-016 3#桨叶片角度","yc_hs_0370","cur_50"]
[199,"b_右玉一期Ⅱ-016机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅱ-016机舱侧向振动(已滤波)","yc_hs_0370","cur_78"]
[200,"b_右玉一期Ⅱ-021机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅱ-021机舱侧向振动(已滤波)","yc_hs_0374","cur_33"]
[201,"b_右玉一期Ⅱ-021机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅱ-021机舱轴向振动(已滤波)","yc_hs_0374","cur_35"]
[202,"b_右玉一期Ⅱ-021机舱角度","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅱ-021机舱角度","yc_hs_0374","cur_36"]
[204,"b_右玉一期Ⅱ-022发电机有功功率","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅱ-022发电机有功功率","yc_hs_0374","cur_48"]
[205,"b_右玉一期Ⅱ-022发电机 绕组温度1","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅱ-022发电机 绕组温度1","yc_hs_0374","cur_51"]
[206,"b_右玉一期Ⅱ-022发电机 绕组温度2","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅱ-022发电机 绕组温度2","yc_hs_0374","cur_52"]
[207,"b_右玉一期Ⅱ-022发电机 绕组温度3","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅱ-022发电机 绕组温度3","yc_hs_0374","cur_53"]
[208,"b_右玉一期Ⅱ-022发电机转速","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅱ-022发电机转速","yc_hs_0374","cur_57"]
[209,"b_右玉一期Ⅱ-022发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅱ-022发电机驱动端轴承温度","yc_hs_0374","cur_58"]
[210,"b_右玉一期Ⅲ-026机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅲ-026机舱侧向振动(已滤波)","yc_hs_0377","cur_88"]
[211,"b_右玉一期Ⅲ-026机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅲ-026机舱轴向振动(已滤波)","yc_hs_0377","cur_90"]
[212,"b_右玉一期Ⅲ-026机舱角度","右玉风光互补电站","WOF34900079",26,"SXYY.T1_L3.WTG026.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅲ-026机舱角度","yc_hs_0377","cur_91"]
[214,"b_右玉一期I-011机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期I-011机舱侧向振动(已滤波)","yc_hs_0367","cur_23"]
[215,"b_右玉一期I-011机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期I-011机舱轴向振动(已滤波)","yc_hs_0367","cur_25"]
[216,"b_右玉一期I-011机舱角度","右玉风光互补电站","WOF34900079",11,"SXYY.T1_L1.WTG011.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期I-011机舱角度","yc_hs_0367","cur_26"]
[218,"b_右玉一期Ⅱ-012发电机有功功率","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅱ-012发电机有功功率","yc_hs_0367","cur_38"]
[219,"b_右玉一期Ⅱ-016机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅱ-016机舱轴向振动(已滤波)","yc_hs_0370","cur_80"]
[220,"b_右玉一期Ⅱ-016机舱角度","右玉风光互补电站","WOF34900079",16,"SXYY.T1_L2.WTG016.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅱ-016机舱角度","yc_hs_0370","cur_81"]
[222,"b_右玉一期Ⅱ-017发电机有功功率","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅱ-017发电机有功功率","yc_hs_0370","cur_93"]
[223,"b_右玉一期Ⅱ-017发电机 绕组温度1","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅱ-017发电机 绕组温度1","yc_hs_0370","cur_96"]
[224,"b_右玉一期Ⅱ-017发电机 绕组温度2","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅱ-017发电机 绕组温度2","yc_hs_0370","cur_97"]
[225,"b_右玉一期Ⅱ-017发电机 绕组温度3","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅱ-017发电机 绕组温度3","yc_hs_0370","cur_98"]
[226,"b_右玉一期Ⅱ-017发电机转速","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅱ-017发电机转速","yc_hs_0371","cur_02"]
[227,"b_右玉一期Ⅱ-017发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅱ-017发电机驱动端轴承温度","yc_hs_0371","cur_03"]
[228,"b_右玉一期Ⅱ-017发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅱ-017发电机非驱动端轴承温度","yc_hs_0371","cur_04"]
[229,"b_右玉一期Ⅱ-017舱内温度","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅱ-017舱内温度","yc_hs_0371","cur_10"]
[230,"b_右玉一期Ⅱ-017舱外温度","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅱ-017舱外温度","yc_hs_0371","cur_12"]
[231,"b_右玉一期Ⅱ-017风向","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅱ-017风向","yc_hs_0371","cur_14"]
[232,"b_右玉一期Ⅱ-017风速","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅱ-017风速","yc_hs_0371","cur_15"]
[233,"b_右玉一期Ⅱ-017机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅱ-017机舱中轴线与风向夹角","yc_hs_0371","cur_16"]
[234,"b_右玉一期Ⅱ-017 1#桨叶片角度","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅱ-017 1#桨叶片角度","yc_hs_0371","cur_17"]
[235,"b_右玉一期Ⅱ-022发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅱ-022发电机非驱动端轴承温度","yc_hs_0374","cur_59"]
[236,"b_右玉一期Ⅱ-022舱内温度","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅱ-022舱内温度","yc_hs_0374","cur_65"]
[237,"b_右玉一期Ⅱ-022舱外温度","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅱ-022舱外温度","yc_hs_0374","cur_67"]
[238,"b_右玉一期Ⅱ-022风向","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅱ-022风向","yc_hs_0374","cur_69"]
[239,"b_右玉一期Ⅱ-022风速","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅱ-022风速","yc_hs_0374","cur_70"]
[240,"b_右玉一期Ⅱ-022机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅱ-022机舱中轴线与风向夹角","yc_hs_0374","cur_71"]
[241,"b_右玉一期Ⅱ-022 1#桨叶片角度","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅱ-022 1#桨叶片角度","yc_hs_0374","cur_72"]
[242,"b_右玉一期Ⅱ-022 2#桨叶片角度","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅱ-022 2#桨叶片角度","yc_hs_0374","cur_74"]
[243,"b_右玉一期Ⅱ-022 3#桨叶片角度","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅱ-022 3#桨叶片角度","yc_hs_0374","cur_76"]
[244,"b_右玉一期Ⅲ-028发电机 绕组温度1","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅲ-028发电机 绕组温度1","yc_hs_0378","cur_77"]
[245,"b_右玉一期Ⅲ-028发电机 绕组温度2","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅲ-028发电机 绕组温度2","yc_hs_0378","cur_78"]
[246,"b_右玉一期Ⅲ-028发电机 绕组温度3","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅲ-028发电机 绕组温度3","yc_hs_0378","cur_79"]
[247,"b_右玉一期Ⅲ-028发电机转速","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅲ-028发电机转速","yc_hs_0378","cur_83"]
[248,"b_右玉一期Ⅲ-028发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅲ-028发电机驱动端轴承温度","yc_hs_0378","cur_84"]
[249,"b_右玉一期Ⅲ-028发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅲ-028发电机非驱动端轴承温度","yc_hs_0378","cur_85"]
[250,"b_右玉一期Ⅲ-028舱内温度","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅲ-028舱内温度","yc_hs_0378","cur_91"]
[251,"b_右玉一期Ⅲ-028舱外温度","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅲ-028舱外温度","yc_hs_0378","cur_93"]
[252,"b_右玉一期Ⅲ-028风向","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅲ-028风向","yc_hs_0378","cur_95"]
[253,"b_右玉一期Ⅲ-028风速","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅲ-028风速","yc_hs_0378","cur_96"]
[254,"b_右玉一期Ⅲ-028机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅲ-028机舱中轴线与风向夹角","yc_hs_0378","cur_97"]
[255,"b_右玉一期Ⅲ-028 1#桨叶片角度","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅲ-028 1#桨叶片角度","yc_hs_0378","cur_98"]
[256,"b_右玉一期Ⅲ-028 2#桨叶片角度","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅲ-028 2#桨叶片角度","yc_hs_0378","cur_100"]
[257,"b_右玉一期Ⅲ-028 3#桨叶片角度","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅲ-028 3#桨叶片角度","yc_hs_0379","cur_02"]
[258,"b_右玉一期Ⅱ-012发电机 绕组温度1","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅱ-012发电机 绕组温度1","yc_hs_0367","cur_41"]
[259,"b_右玉一期Ⅱ-012发电机 绕组温度2","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅱ-012发电机 绕组温度2","yc_hs_0367","cur_42"]
[260,"b_右玉一期Ⅱ-012发电机 绕组温度3","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅱ-012发电机 绕组温度3","yc_hs_0367","cur_43"]
[261,"b_右玉一期Ⅱ-012发电机转速","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅱ-012发电机转速","yc_hs_0367","cur_47"]
[262,"b_右玉一期Ⅱ-012发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅱ-012发电机驱动端轴承温度","yc_hs_0367","cur_48"]
[263,"b_右玉一期Ⅱ-012发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅱ-012发电机非驱动端轴承温度","yc_hs_0367","cur_49"]
[264,"b_右玉一期Ⅱ-012舱内温度","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅱ-012舱内温度","yc_hs_0367","cur_55"]
[265,"b_右玉一期Ⅱ-012舱外温度","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅱ-012舱外温度","yc_hs_0367","cur_57"]
[266,"b_右玉一期Ⅱ-012风向","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅱ-012风向","yc_hs_0367","cur_59"]
[267,"b_右玉一期Ⅱ-012风速","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅱ-012风速","yc_hs_0367","cur_60"]
[268,"b_右玉一期Ⅱ-012机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅱ-012机舱中轴线与风向夹角","yc_hs_0367","cur_61"]
[269,"b_右玉一期Ⅱ-012 1#桨叶片角度","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅱ-012 1#桨叶片角度","yc_hs_0367","cur_62"]
[270,"b_右玉一期Ⅱ-012 2#桨叶片角度","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅱ-012 2#桨叶片角度","yc_hs_0367","cur_64"]
[271,"b_右玉一期Ⅱ-012 3#桨叶片角度","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅱ-012 3#桨叶片角度","yc_hs_0367","cur_66"]
[272,"b_右玉一期Ⅱ-017 2#桨叶片角度","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅱ-017 2#桨叶片角度","yc_hs_0371","cur_19"]
[273,"b_右玉一期Ⅱ-017 3#桨叶片角度","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅱ-017 3#桨叶片角度","yc_hs_0371","cur_21"]
[274,"b_右玉一期Ⅱ-017机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅱ-017机舱侧向振动(已滤波)","yc_hs_0371","cur_49"]
[275,"b_右玉一期Ⅱ-017机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅱ-017机舱轴向振动(已滤波)","yc_hs_0371","cur_51"]
[276,"b_右玉一期Ⅱ-017机舱角度","右玉风光互补电站","WOF34900079",17,"SXYY.T1_L2.WTG017.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅱ-017机舱角度","yc_hs_0371","cur_52"]
[278,"b_右玉一期Ⅱ-022机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅱ-022机舱侧向振动(已滤波)","yc_hs_0375","cur_04"]
[279,"b_右玉一期Ⅱ-022机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅱ-022机舱轴向振动(已滤波)","yc_hs_0375","cur_06"]
[280,"b_右玉一期Ⅱ-022机舱角度","右玉风光互补电站","WOF34900079",22,"SXYY.T1_L2.WTG022.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅱ-022机舱角度","yc_hs_0375","cur_07"]
[282,"b_右玉一期Ⅱ-023发电机有功功率","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅱ-023发电机有功功率","yc_hs_0375","cur_19"]
[283,"b_右玉一期Ⅱ-023发电机 绕组温度1","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅱ-023发电机 绕组温度1","yc_hs_0375","cur_22"]
[284,"b_右玉一期Ⅱ-023发电机 绕组温度2","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅱ-023发电机 绕组温度2","yc_hs_0375","cur_23"]
[285,"b_右玉一期Ⅱ-023发电机 绕组温度3","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅱ-023发电机 绕组温度3","yc_hs_0375","cur_24"]
[286,"b_右玉一期Ⅱ-023发电机转速","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅱ-023发电机转速","yc_hs_0375","cur_28"]
[287,"b_右玉一期Ⅱ-023发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅱ-023发电机驱动端轴承温度","yc_hs_0375","cur_29"]
[288,"b_右玉一期Ⅱ-023发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅱ-023发电机非驱动端轴承温度","yc_hs_0375","cur_30"]
[289,"b_右玉一期Ⅲ-028机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅲ-028机舱侧向振动(已滤波)","yc_hs_0379","cur_30"]
[290,"b_右玉一期Ⅲ-028机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅲ-028机舱轴向振动(已滤波)","yc_hs_0379","cur_32"]
[291,"b_右玉一期Ⅲ-028机舱角度","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅲ-028机舱角度","yc_hs_0379","cur_33"]
[293,"b_右玉一期Ⅲ-029发电机有功功率","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅲ-029发电机有功功率","yc_hs_0379","cur_45"]
[294,"b_右玉一期Ⅲ-029发电机 绕组温度1","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅲ-029发电机 绕组温度1","yc_hs_0379","cur_48"]
[295,"b_右玉一期Ⅲ-029发电机 绕组温度2","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅲ-029发电机 绕组温度2","yc_hs_0379","cur_49"]
[296,"b_右玉一期Ⅲ-029发电机 绕组温度3","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅲ-029发电机 绕组温度3","yc_hs_0379","cur_50"]
[297,"b_右玉一期Ⅱ-012机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅱ-012机舱侧向振动(已滤波)","yc_hs_0367","cur_94"]
[298,"b_右玉一期Ⅱ-012机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅱ-012机舱轴向振动(已滤波)","yc_hs_0367","cur_96"]
[299,"b_右玉一期Ⅱ-012机舱角度","右玉风光互补电站","WOF34900079",12,"SXYY.T1_L2.WTG012.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅱ-012机舱角度","yc_hs_0367","cur_97"]
[301,"b_右玉一期Ⅱ-013发电机有功功率","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅱ-013发电机有功功率","yc_hs_0368","cur_09"]
[302,"b_右玉一期Ⅱ-013发电机 绕组温度1","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅱ-013发电机 绕组温度1","yc_hs_0368","cur_12"]
[303,"b_右玉一期Ⅱ-013发电机 绕组温度2","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅱ-013发电机 绕组温度2","yc_hs_0368","cur_13"]
[304,"b_右玉一期Ⅱ-013发电机 绕组温度3","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅱ-013发电机 绕组温度3","yc_hs_0368","cur_14"]
[305,"b_右玉一期Ⅱ-018发电机有功功率","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅱ-018发电机有功功率","yc_hs_0371","cur_64"]
[306,"b_右玉一期Ⅱ-018发电机 绕组温度1","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅱ-018发电机 绕组温度1","yc_hs_0371","cur_67"]
[307,"b_右玉一期Ⅱ-018发电机 绕组温度2","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅱ-018发电机 绕组温度2","yc_hs_0371","cur_68"]
[308,"b_右玉一期Ⅱ-018发电机 绕组温度3","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅱ-018发电机 绕组温度3","yc_hs_0371","cur_69"]
[309,"b_右玉一期Ⅱ-018发电机转速","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅱ-018发电机转速","yc_hs_0371","cur_73"]
[310,"b_右玉一期Ⅱ-018发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅱ-018发电机驱动端轴承温度","yc_hs_0371","cur_74"]
[311,"b_右玉一期Ⅱ-018发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅱ-018发电机非驱动端轴承温度","yc_hs_0371","cur_75"]
[312,"b_右玉一期Ⅱ-018舱内温度","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅱ-018舱内温度","yc_hs_0371","cur_81"]
[313,"b_右玉一期Ⅱ-018舱外温度","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅱ-018舱外温度","yc_hs_0371","cur_83"]
[314,"b_右玉一期Ⅱ-018风向","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅱ-018风向","yc_hs_0371","cur_85"]
[315,"b_右玉一期Ⅱ-018风速","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅱ-018风速","yc_hs_0371","cur_86"]
[316,"b_右玉一期Ⅱ-018机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅱ-018机舱中轴线与风向夹角","yc_hs_0371","cur_87"]
[317,"b_右玉一期Ⅱ-018 1#桨叶片角度","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅱ-018 1#桨叶片角度","yc_hs_0371","cur_88"]
[318,"b_右玉一期Ⅱ-018 2#桨叶片角度","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅱ-018 2#桨叶片角度","yc_hs_0371","cur_90"]
[319,"b_右玉一期Ⅱ-018 3#桨叶片角度","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅱ-018 3#桨叶片角度","yc_hs_0371","cur_92"]
[320,"b_右玉一期Ⅱ-023舱内温度","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅱ-023舱内温度","yc_hs_0375","cur_36"]
[321,"b_右玉一期Ⅱ-023舱外温度","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅱ-023舱外温度","yc_hs_0375","cur_38"]
[322,"b_右玉一期Ⅱ-023风向","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅱ-023风向","yc_hs_0375","cur_40"]
[323,"b_右玉一期Ⅱ-023风速","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅱ-023风速","yc_hs_0375","cur_41"]
[324,"b_右玉一期Ⅱ-023机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅱ-023机舱中轴线与风向夹角","yc_hs_0375","cur_42"]
[325,"b_右玉一期Ⅱ-023 1#桨叶片角度","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅱ-023 1#桨叶片角度","yc_hs_0375","cur_43"]
[326,"b_右玉一期Ⅱ-023 2#桨叶片角度","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅱ-023 2#桨叶片角度","yc_hs_0375","cur_45"]
[327,"b_右玉一期Ⅱ-023 3#桨叶片角度","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅱ-023 3#桨叶片角度","yc_hs_0375","cur_47"]
[328,"b_右玉一期Ⅲ-027发电机有功功率","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅲ-027发电机有功功率","yc_hs_0378","cur_03"]
[329,"b_右玉一期Ⅲ-027发电机 绕组温度1","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅲ-027发电机 绕组温度1","yc_hs_0378","cur_06"]
[330,"b_右玉一期Ⅲ-027发电机 绕组温度2","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅲ-027发电机 绕组温度2","yc_hs_0378","cur_07"]
[331,"b_右玉一期Ⅲ-027发电机 绕组温度3","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅲ-027发电机 绕组温度3","yc_hs_0378","cur_08"]
[332,"b_右玉一期Ⅲ-027发电机转速","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅲ-027发电机转速","yc_hs_0378","cur_12"]
[333,"b_右玉一期Ⅲ-027发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅲ-027发电机驱动端轴承温度","yc_hs_0378","cur_13"]
[334,"b_右玉一期Ⅲ-027发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅲ-027发电机非驱动端轴承温度","yc_hs_0378","cur_14"]
[335,"b_右玉一期Ⅲ-027舱内温度","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅲ-027舱内温度","yc_hs_0378","cur_20"]
[336,"b_右玉一期Ⅲ-027舱外温度","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅲ-027舱外温度","yc_hs_0378","cur_22"]
[337,"b_右玉一期Ⅲ-027风向","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅲ-027风向","yc_hs_0378","cur_24"]
[338,"b_右玉一期Ⅲ-027风速","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅲ-027风速","yc_hs_0378","cur_25"]
[339,"b_右玉一期Ⅲ-027机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅲ-027机舱中轴线与风向夹角","yc_hs_0378","cur_26"]
[340,"b_右玉一期Ⅲ-027 1#桨叶片角度","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅲ-027 1#桨叶片角度","yc_hs_0378","cur_27"]
[341,"b_右玉一期Ⅲ-027 2#桨叶片角度","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅲ-027 2#桨叶片角度","yc_hs_0378","cur_29"]
[342,"b_右玉一期Ⅲ-027 3#桨叶片角度","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅲ-027 3#桨叶片角度","yc_hs_0378","cur_31"]
[343,"b_右玉一期Ⅱ-013发电机转速","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅱ-013发电机转速","yc_hs_0368","cur_18"]
[344,"b_右玉一期Ⅱ-013发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅱ-013发电机驱动端轴承温度","yc_hs_0368","cur_19"]
[345,"b_右玉一期Ⅱ-013发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅱ-013发电机非驱动端轴承温度","yc_hs_0368","cur_20"]
[346,"b_右玉一期Ⅱ-013舱内温度","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅱ-013舱内温度","yc_hs_0368","cur_26"]
[347,"b_右玉一期Ⅱ-013舱外温度","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅱ-013舱外温度","yc_hs_0368","cur_28"]
[348,"b_右玉一期Ⅱ-013风向","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅱ-013风向","yc_hs_0368","cur_30"]
[349,"b_右玉一期Ⅱ-013风速","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅱ-013风速","yc_hs_0368","cur_31"]
[350,"b_右玉一期Ⅱ-013机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅱ-013机舱中轴线与风向夹角","yc_hs_0368","cur_32"]
[351,"b_右玉一期Ⅱ-013 1#桨叶片角度","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅱ-013 1#桨叶片角度","yc_hs_0368","cur_33"]
[352,"b_右玉一期Ⅱ-013 2#桨叶片角度","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅱ-013 2#桨叶片角度","yc_hs_0368","cur_35"]
[353,"b_右玉一期Ⅱ-013 3#桨叶片角度","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅱ-013 3#桨叶片角度","yc_hs_0368","cur_37"]
[354,"b_右玉一期Ⅱ-018机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅱ-018机舱侧向振动(已滤波)","yc_hs_0372","cur_20"]
[355,"b_右玉一期Ⅱ-018机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅱ-018机舱轴向振动(已滤波)","yc_hs_0372","cur_22"]
[356,"b_右玉一期Ⅱ-018机舱角度","右玉风光互补电站","WOF34900079",18,"SXYY.T1_L2.WTG018.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅱ-018机舱角度","yc_hs_0372","cur_23"]
[358,"b_右玉一期Ⅱ-023机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅱ-023机舱侧向振动(已滤波)","yc_hs_0375","cur_75"]
[359,"b_右玉一期Ⅱ-023机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅱ-023机舱轴向振动(已滤波)","yc_hs_0375","cur_77"]
[360,"b_右玉一期Ⅱ-023机舱角度","右玉风光互补电站","WOF34900079",23,"SXYY.T1_L2.WTG023.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅱ-023机舱角度","yc_hs_0375","cur_78"]
[362,"b_右玉一期Ⅲ-024发电机有功功率","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅲ-024发电机有功功率","yc_hs_0375","cur_90"]
[363,"b_右玉一期Ⅲ-024发电机 绕组温度1","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅲ-024发电机 绕组温度1","yc_hs_0375","cur_93"]
[364,"b_右玉一期Ⅲ-024发电机 绕组温度2","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅲ-024发电机 绕组温度2","yc_hs_0375","cur_94"]
[365,"b_右玉一期Ⅲ-024发电机 绕组温度3","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅲ-024发电机 绕组温度3","yc_hs_0375","cur_95"]
[366,"b_右玉一期Ⅲ-024发电机转速","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅲ-024发电机转速","yc_hs_0375","cur_99"]
[367,"b_右玉一期Ⅲ-024发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅲ-024发电机驱动端轴承温度","yc_hs_0375","cur_100"]
[368,"b_右玉一期Ⅲ-024发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅲ-024发电机非驱动端轴承温度","yc_hs_0376","cur_01"]
[369,"b_右玉一期Ⅲ-024舱内温度","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅲ-024舱内温度","yc_hs_0376","cur_07"]
[370,"b_右玉一期Ⅲ-024舱外温度","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅲ-024舱外温度","yc_hs_0376","cur_09"]
[371,"b_右玉一期Ⅲ-029机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅲ-029机舱侧向振动(已滤波)","yc_hs_0380","cur_01"]
[372,"b_右玉一期Ⅲ-029机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅲ-029机舱轴向振动(已滤波)","yc_hs_0380","cur_03"]
[373,"b_右玉一期Ⅲ-029机舱角度","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅲ-029机舱角度","yc_hs_0380","cur_04"]
[375,"b_右玉一期Ⅲ-030发电机有功功率","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅲ-030发电机有功功率","yc_hs_0380","cur_16"]
[376,"b_右玉一期Ⅲ-030发电机 绕组温度1","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅲ-030发电机 绕组温度1","yc_hs_0380","cur_19"]
[377,"b_右玉一期Ⅲ-030发电机 绕组温度2","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅲ-030发电机 绕组温度2","yc_hs_0380","cur_20"]
[378,"b_右玉一期Ⅲ-030发电机 绕组温度3","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅲ-030发电机 绕组温度3","yc_hs_0380","cur_21"]
[379,"b_右玉一期Ⅲ-030发电机转速","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅲ-030发电机转速","yc_hs_0380","cur_25"]
[380,"b_右玉一期Ⅲ-030发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅲ-030发电机驱动端轴承温度","yc_hs_0380","cur_26"]
[381,"b_右玉一期Ⅱ-013机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅱ-013机舱侧向振动(已滤波)","yc_hs_0368","cur_65"]
[382,"b_右玉一期Ⅱ-013机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅱ-013机舱轴向振动(已滤波)","yc_hs_0368","cur_67"]
[383,"b_右玉一期Ⅱ-013机舱角度","右玉风光互补电站","WOF34900079",13,"SXYY.T1_L2.WTG013.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅱ-013机舱角度","yc_hs_0368","cur_68"]
[385,"b_右玉一期Ⅱ-014发电机有功功率","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅱ-014发电机有功功率","yc_hs_0368","cur_80"]
[386,"b_右玉一期Ⅱ-014发电机 绕组温度1","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅱ-014发电机 绕组温度1","yc_hs_0368","cur_83"]
[387,"b_右玉一期Ⅱ-014发电机 绕组温度2","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅱ-014发电机 绕组温度2","yc_hs_0368","cur_84"]
[388,"b_右玉一期Ⅱ-014发电机 绕组温度3","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅱ-014发电机 绕组温度3","yc_hs_0368","cur_85"]
[389,"b_右玉一期Ⅱ-014发电机转速","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅱ-014发电机转速","yc_hs_0368","cur_89"]
[390,"b_右玉一期Ⅱ-014发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅱ-014发电机驱动端轴承温度","yc_hs_0368","cur_90"]
[391,"b_右玉一期Ⅱ-019发电机有功功率","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅱ-019发电机有功功率","yc_hs_0372","cur_35"]
[392,"b_右玉一期Ⅱ-019发电机 绕组温度1","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅱ-019发电机 绕组温度1","yc_hs_0372","cur_38"]
[393,"b_右玉一期Ⅱ-019发电机 绕组温度2","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅱ-019发电机 绕组温度2","yc_hs_0372","cur_39"]
[394,"b_右玉一期Ⅱ-019发电机 绕组温度3","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅱ-019发电机 绕组温度3","yc_hs_0372","cur_40"]
[395,"b_右玉一期Ⅱ-019发电机转速","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅱ-019发电机转速","yc_hs_0372","cur_44"]
[396,"b_右玉一期Ⅱ-019发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅱ-019发电机驱动端轴承温度","yc_hs_0372","cur_45"]
[397,"b_右玉一期Ⅱ-019发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅱ-019发电机非驱动端轴承温度","yc_hs_0372","cur_46"]
[398,"b_右玉一期Ⅱ-019舱内温度","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅱ-019舱内温度","yc_hs_0372","cur_52"]
[399,"b_右玉一期Ⅱ-019舱外温度","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅱ-019舱外温度","yc_hs_0372","cur_54"]
[400,"b_右玉一期Ⅱ-019风向","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅱ-019风向","yc_hs_0372","cur_56"]
[401,"b_右玉一期Ⅱ-019风速","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅱ-019风速","yc_hs_0372","cur_57"]
[402,"b_右玉一期Ⅱ-019机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅱ-019机舱中轴线与风向夹角","yc_hs_0372","cur_58"]
[403,"b_右玉一期Ⅱ-019 1#桨叶片角度","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅱ-019 1#桨叶片角度","yc_hs_0372","cur_59"]
[404,"b_右玉一期Ⅱ-019 2#桨叶片角度","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅱ-019 2#桨叶片角度","yc_hs_0372","cur_61"]
[405,"b_右玉一期Ⅱ-019 3#桨叶片角度","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅱ-019 3#桨叶片角度","yc_hs_0372","cur_63"]
[406,"b_右玉一期Ⅲ-024风向","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅲ-024风向","yc_hs_0376","cur_11"]
[407,"b_右玉一期Ⅲ-024风速","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅲ-024风速","yc_hs_0376","cur_12"]
[408,"b_右玉一期Ⅲ-024机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅲ-024机舱中轴线与风向夹角","yc_hs_0376","cur_13"]
[409,"b_右玉一期Ⅲ-024 1#桨叶片角度","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅲ-024 1#桨叶片角度","yc_hs_0376","cur_14"]
[410,"b_右玉一期Ⅲ-024 2#桨叶片角度","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅲ-024 2#桨叶片角度","yc_hs_0376","cur_16"]
[411,"b_右玉一期Ⅲ-024 3#桨叶片角度","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅲ-024 3#桨叶片角度","yc_hs_0376","cur_18"]
[412,"b_右玉一期Ⅲ-024机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅲ-024机舱侧向振动(已滤波)","yc_hs_0376","cur_46"]
[413,"b_右玉一期Ⅲ-029发电机转速","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅲ-029发电机转速","yc_hs_0379","cur_54"]
[414,"b_右玉一期Ⅲ-029发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅲ-029发电机驱动端轴承温度","yc_hs_0379","cur_55"]
[415,"b_右玉一期Ⅲ-029发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅲ-029发电机非驱动端轴承温度","yc_hs_0379","cur_56"]
[416,"b_右玉一期Ⅲ-029舱内温度","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅲ-029舱内温度","yc_hs_0379","cur_62"]
[417,"b_右玉一期Ⅲ-029舱外温度","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅲ-029舱外温度","yc_hs_0379","cur_64"]
[418,"b_右玉一期Ⅲ-029风向","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅲ-029风向","yc_hs_0379","cur_66"]
[419,"b_右玉一期Ⅲ-029风速","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅲ-029风速","yc_hs_0379","cur_67"]
[420,"b_右玉一期Ⅲ-029机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅲ-029机舱中轴线与风向夹角","yc_hs_0379","cur_68"]
[421,"b_右玉一期Ⅲ-029 1#桨叶片角度","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅲ-029 1#桨叶片角度","yc_hs_0379","cur_69"]
[422,"b_右玉一期Ⅲ-029 2#桨叶片角度","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅲ-029 2#桨叶片角度","yc_hs_0379","cur_71"]
[423,"b_右玉一期Ⅲ-029 3#桨叶片角度","右玉风光互补电站","WOF34900079",29,"SXYY.T1_L3.WTG029.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅲ-029 3#桨叶片角度","yc_hs_0379","cur_73"]
[424,"b_右玉一期Ⅱ-014发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅱ-014发电机非驱动端轴承温度","yc_hs_0368","cur_91"]
[425,"b_右玉一期Ⅱ-014舱内温度","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅱ-014舱内温度","yc_hs_0368","cur_97"]
[426,"b_右玉一期Ⅱ-014舱外温度","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅱ-014舱外温度","yc_hs_0368","cur_99"]
[427,"b_右玉一期Ⅱ-014风向","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅱ-014风向","yc_hs_0369","cur_01"]
[428,"b_右玉一期Ⅱ-014风速","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅱ-014风速","yc_hs_0369","cur_02"]
[429,"b_右玉一期Ⅱ-014机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅱ-014机舱中轴线与风向夹角","yc_hs_0369","cur_03"]
[430,"b_右玉一期Ⅱ-014 1#桨叶片角度","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅱ-014 1#桨叶片角度","yc_hs_0369","cur_04"]
[431,"b_右玉一期Ⅱ-014 2#桨叶片角度","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅱ-014 2#桨叶片角度","yc_hs_0369","cur_06"]
[432,"b_右玉一期Ⅱ-014 3#桨叶片角度","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅱ-014 3#桨叶片角度","yc_hs_0369","cur_08"]
[433,"b_右玉一期Ⅱ-019机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅱ-019机舱侧向振动(已滤波)","yc_hs_0372","cur_91"]
[434,"b_右玉一期Ⅱ-019机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅱ-019机舱轴向振动(已滤波)","yc_hs_0372","cur_93"]
[435,"b_右玉一期Ⅱ-019机舱角度","右玉风光互补电站","WOF34900079",19,"SXYY.T1_L2.WTG019.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅱ-019机舱角度","yc_hs_0372","cur_94"]
[437,"b_右玉一期Ⅱ-020发电机有功功率","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅱ-020发电机有功功率","yc_hs_0373","cur_06"]
[438,"b_右玉一期Ⅲ-024机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅲ-024机舱轴向振动(已滤波)","yc_hs_0376","cur_48"]
[439,"b_右玉一期Ⅲ-024机舱角度","右玉风光互补电站","WOF34900079",24,"SXYY.T1_L3.WTG024.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅲ-024机舱角度","yc_hs_0376","cur_49"]
[441,"b_右玉一期Ⅲ-025发电机有功功率","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅲ-025发电机有功功率","yc_hs_0376","cur_61"]
[442,"b_右玉一期Ⅲ-025发电机 绕组温度1","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅲ-025发电机 绕组温度1","yc_hs_0376","cur_64"]
[443,"b_右玉一期Ⅲ-025发电机 绕组温度2","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅲ-025发电机 绕组温度2","yc_hs_0376","cur_65"]
[444,"b_右玉一期Ⅲ-025发电机 绕组温度3","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅲ-025发电机 绕组温度3","yc_hs_0376","cur_66"]
[445,"b_右玉一期Ⅲ-025发电机转速","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅲ-025发电机转速","yc_hs_0376","cur_70"]
[446,"b_右玉一期Ⅲ-025发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅲ-025发电机驱动端轴承温度","yc_hs_0376","cur_71"]
[447,"b_右玉一期Ⅲ-025发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅲ-025发电机非驱动端轴承温度","yc_hs_0376","cur_72"]
[448,"b_右玉一期Ⅲ-025舱内温度","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅲ-025舱内温度","yc_hs_0376","cur_78"]
[449,"b_右玉一期Ⅲ-025舱外温度","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅲ-025舱外温度","yc_hs_0376","cur_80"]
[450,"b_右玉一期Ⅲ-025风向","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅲ-025风向","yc_hs_0376","cur_82"]
[451,"b_右玉一期Ⅲ-025风速","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅲ-025风速","yc_hs_0376","cur_83"]
[452,"b_右玉一期Ⅲ-025机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅲ-025机舱中轴线与风向夹角","yc_hs_0376","cur_84"]
[453,"b_右玉一期Ⅲ-025 1#桨叶片角度","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅲ-025 1#桨叶片角度","yc_hs_0376","cur_85"]
[454,"b_右玉一期Ⅲ-027机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅲ-027机舱侧向振动(已滤波)","yc_hs_0378","cur_59"]
[455,"b_右玉一期Ⅲ-027机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅲ-027机舱轴向振动(已滤波)","yc_hs_0378","cur_61"]
[456,"b_右玉一期Ⅲ-027机舱角度","右玉风光互补电站","WOF34900079",27,"SXYY.T1_L3.WTG027.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅲ-027机舱角度","yc_hs_0378","cur_62"]
[458,"b_右玉一期Ⅲ-028发电机有功功率","右玉风光互补电站","WOF34900079",28,"SXYY.T1_L3.WTG028.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅲ-028发电机有功功率","yc_hs_0378","cur_74"]
[459,"b_右玉一期Ⅱ-014机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅱ-014机舱侧向振动(已滤波)","yc_hs_0369","cur_36"]
[460,"b_右玉一期Ⅱ-014机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅱ-014机舱轴向振动(已滤波)","yc_hs_0369","cur_38"]
[461,"b_右玉一期Ⅱ-014机舱角度","右玉风光互补电站","WOF34900079",14,"SXYY.T1_L2.WTG014.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅱ-014机舱角度","yc_hs_0369","cur_39"]
[463,"b_右玉一期Ⅱ-015发电机有功功率","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅱ-015发电机有功功率","yc_hs_0369","cur_51"]
[464,"b_右玉一期Ⅱ-015发电机 绕组温度1","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅱ-015发电机 绕组温度1","yc_hs_0369","cur_54"]
[465,"b_右玉一期Ⅱ-015发电机 绕组温度2","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅱ-015发电机 绕组温度2","yc_hs_0369","cur_55"]
[466,"b_右玉一期Ⅱ-015发电机 绕组温度3","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅱ-015发电机 绕组温度3","yc_hs_0369","cur_56"]
[467,"b_右玉一期Ⅱ-015发电机转速","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅱ-015发电机转速","yc_hs_0369","cur_60"]
[468,"b_右玉一期Ⅱ-015发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅱ-015发电机驱动端轴承温度","yc_hs_0369","cur_61"]
[469,"b_右玉一期Ⅱ-015发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅱ-015发电机非驱动端轴承温度","yc_hs_0369","cur_62"]
[470,"b_右玉一期Ⅱ-020发电机 绕组温度1","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅱ-020发电机 绕组温度1","yc_hs_0373","cur_09"]
[471,"b_右玉一期Ⅱ-020发电机 绕组温度2","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅱ-020发电机 绕组温度2","yc_hs_0373","cur_10"]
[472,"b_右玉一期Ⅱ-020发电机 绕组温度3","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅱ-020发电机 绕组温度3","yc_hs_0373","cur_11"]
[473,"b_右玉一期Ⅱ-020发电机转速","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅱ-020发电机转速","yc_hs_0373","cur_15"]
[474,"b_右玉一期Ⅱ-020发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅱ-020发电机驱动端轴承温度","yc_hs_0373","cur_16"]
[475,"b_右玉一期Ⅱ-020发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅱ-020发电机非驱动端轴承温度","yc_hs_0373","cur_17"]
[476,"b_右玉一期Ⅱ-020舱内温度","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅱ-020舱内温度","yc_hs_0373","cur_23"]
[477,"b_右玉一期Ⅱ-020舱外温度","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅱ-020舱外温度","yc_hs_0373","cur_25"]
[478,"b_右玉一期Ⅱ-020风向","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅱ-020风向","yc_hs_0373","cur_27"]
[479,"b_右玉一期Ⅱ-020风速","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅱ-020风速","yc_hs_0373","cur_28"]
[480,"b_右玉一期Ⅱ-020机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅱ-020机舱中轴线与风向夹角","yc_hs_0373","cur_29"]
[481,"b_右玉一期Ⅱ-020 1#桨叶片角度","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅱ-020 1#桨叶片角度","yc_hs_0373","cur_30"]
[482,"b_右玉一期Ⅱ-020 2#桨叶片角度","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅱ-020 2#桨叶片角度","yc_hs_0373","cur_32"]
[483,"b_右玉一期Ⅱ-020 3#桨叶片角度","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅱ-020 3#桨叶片角度","yc_hs_0373","cur_34"]
[484,"b_右玉一期Ⅲ-025 2#桨叶片角度","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅲ-025 2#桨叶片角度","yc_hs_0376","cur_87"]
[485,"b_右玉一期Ⅲ-025 3#桨叶片角度","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅲ-025 3#桨叶片角度","yc_hs_0376","cur_89"]
[486,"b_右玉一期Ⅲ-025机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅲ-025机舱侧向振动(已滤波)","yc_hs_0377","cur_17"]
[487,"b_右玉一期Ⅲ-025机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅲ-025机舱轴向振动(已滤波)","yc_hs_0377","cur_19"]
[488,"b_右玉一期Ⅲ-025机舱角度","右玉风光互补电站","WOF34900079",25,"SXYY.T1_L3.WTG025.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅲ-025机舱角度","yc_hs_0377","cur_20"]
[490,"b_右玉一期Ⅲ-030发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅲ-030发电机非驱动端轴承温度","yc_hs_0380","cur_27"]
[491,"b_右玉一期Ⅲ-030舱内温度","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅲ-030舱内温度","yc_hs_0380","cur_33"]
[492,"b_右玉一期Ⅲ-030舱外温度","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅲ-030舱外温度","yc_hs_0380","cur_35"]
[493,"b_右玉一期Ⅲ-030风向","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅲ-030风向","yc_hs_0380","cur_37"]
[494,"b_右玉一期Ⅲ-030风速","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅲ-030风速","yc_hs_0380","cur_38"]
[495,"b_右玉一期Ⅲ-030机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅲ-030机舱中轴线与风向夹角","yc_hs_0380","cur_39"]
[496,"b_右玉一期Ⅲ-030 1#桨叶片角度","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅲ-030 1#桨叶片角度","yc_hs_0380","cur_40"]
[497,"b_右玉一期Ⅲ-030 2#桨叶片角度","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅲ-030 2#桨叶片角度","yc_hs_0380","cur_42"]
[498,"b_右玉一期Ⅲ-030 3#桨叶片角度","右玉风光互补电站","WOF34900079",30,"SXYY.T1_L3.WTG030.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅲ-030 3#桨叶片角度","yc_hs_0380","cur_44"]
[499,"b_右玉一期Ⅱ-015舱内温度","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅱ-015舱内温度","yc_hs_0369","cur_68"]
[500,"b_右玉一期Ⅱ-015舱外温度","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅱ-015舱外温度","yc_hs_0369","cur_70"]
[501,"b_右玉一期Ⅱ-015风向","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅱ-015风向","yc_hs_0369","cur_72"]
[502,"b_右玉一期Ⅱ-015风速","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅱ-015风速","yc_hs_0369","cur_73"]
[503,"b_右玉一期Ⅱ-015机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅱ-015机舱中轴线与风向夹角","yc_hs_0369","cur_74"]
[504,"b_右玉一期Ⅱ-015 1#桨叶片角度","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅱ-015 1#桨叶片角度","yc_hs_0369","cur_75"]
[505,"b_右玉一期Ⅱ-015 2#桨叶片角度","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅱ-015 2#桨叶片角度","yc_hs_0369","cur_77"]
[506,"b_右玉一期Ⅱ-015 3#桨叶片角度","右玉风光互补电站","WOF34900079",15,"SXYY.T1_L2.WTG015.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅱ-015 3#桨叶片角度","yc_hs_0369","cur_79"]
[507,"b_右玉一期Ⅱ-020机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅱ-020机舱侧向振动(已滤波)","yc_hs_0373","cur_62"]
[508,"b_右玉一期Ⅱ-020机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅱ-020机舱轴向振动(已滤波)","yc_hs_0373","cur_64"]
[509,"b_右玉一期Ⅱ-020机舱角度","右玉风光互补电站","WOF34900079",20,"SXYY.T1_L2.WTG020.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅱ-020机舱角度","yc_hs_0373","cur_65"]
[511,"b_右玉一期Ⅱ-021发电机有功功率","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅱ-021发电机有功功率","yc_hs_0373","cur_77"]
[512,"b_右玉一期Ⅱ-021发电机 绕组温度1","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅱ-021发电机 绕组温度1","yc_hs_0373","cur_80"]
[513,"b_右玉一期Ⅱ-021发电机 绕组温度2","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅱ-021发电机 绕组温度2","yc_hs_0373","cur_81"]
[514,"b_右玉一期Ⅱ-021发电机 绕组温度3","右玉风光互补电站","WOF34900079",21,"SXYY.T1_L2.WTG021.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅱ-021发电机 绕组温度3","yc_hs_0373","cur_82"]
[515,"b_右玉一期I-002机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期I-002机舱侧向振动(已滤波)","yc_hs_0360","cur_82"]
[516,"b_右玉一期I-002机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期I-002机舱轴向振动(已滤波)","yc_hs_0360","cur_84"]
[517,"b_右玉一期I-002机舱角度","右玉风光互补电站","WOF34900079",2,"SXYY.T1_L1.WTG002.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期I-002机舱角度","yc_hs_0360","cur_85"]
[519,"b_右玉一期I-003发电机有功功率","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WGEN.GenActivePW","有功功率","active_power","b_右玉一期I-003发电机有功功率","yc_hs_0360","cur_97"]
[520,"b_右玉一期I-004发电机 绕组温度3","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期I-004发电机 绕组温度3","yc_hs_0361","cur_73"]
[521,"b_右玉一期I-004发电机转速","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期I-004发电机转速","yc_hs_0361","cur_77"]
[522,"b_右玉一期I-004发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期I-004发电机驱动端轴承温度","yc_hs_0361","cur_78"]
[523,"b_右玉一期I-004发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期I-004发电机非驱动端轴承温度","yc_hs_0361","cur_79"]
[524,"b_右玉一期I-004舱内温度","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期I-004舱内温度","yc_hs_0361","cur_85"]
[525,"b_右玉一期I-004舱外温度","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期I-004舱外温度","yc_hs_0361","cur_87"]
[526,"b_右玉一期I-004风向","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期I-004风向","yc_hs_0361","cur_89"]
[527,"b_右玉一期I-004风速","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期I-004风速","yc_hs_0361","cur_90"]
[528,"b_右玉一期I-004机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期I-004机舱中轴线与风向夹角","yc_hs_0361","cur_91"]
[529,"b_右玉一期I-004 1#桨叶片角度","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期I-004 1#桨叶片角度","yc_hs_0361","cur_92"]
[530,"b_右玉一期I-004 2#桨叶片角度","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期I-004 2#桨叶片角度","yc_hs_0361","cur_94"]
[531,"b_右玉一期I-004 3#桨叶片角度","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期I-004 3#桨叶片角度","yc_hs_0361","cur_96"]
[532,"b_右玉一期I-006舱内温度","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期I-006舱内温度","yc_hs_0363","cur_27"]
[533,"b_右玉一期I-006舱外温度","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期I-006舱外温度","yc_hs_0363","cur_29"]
[534,"b_右玉一期I-006风向","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期I-006风向","yc_hs_0363","cur_31"]
[535,"b_右玉一期I-006风速","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期I-006风速","yc_hs_0363","cur_32"]
[536,"b_右玉一期I-006机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期I-006机舱中轴线与风向夹角","yc_hs_0363","cur_33"]
[537,"b_右玉一期I-006 1#桨叶片角度","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期I-006 1#桨叶片角度","yc_hs_0363","cur_34"]
[538,"b_右玉一期I-006 2#桨叶片角度","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期I-006 2#桨叶片角度","yc_hs_0363","cur_36"]
[539,"b_右玉一期I-006 3#桨叶片角度","右玉风光互补电站","WOF34900079",6,"SXYY.T1_L1.WTG006.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期I-006 3#桨叶片角度","yc_hs_0363","cur_38"]
[540,"b_右玉一期I-001发电机有功功率","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WGEN.GenActivePW","有功功率","active_power","b_右玉一期I-001发电机有功功率","yc_hs_0359","cur_55"]
[541,"b_右玉一期I-001发电机 绕组温度1","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期I-001发电机 绕组温度1","yc_hs_0359","cur_58"]
[542,"b_右玉一期I-001发电机 绕组温度2","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期I-001发电机 绕组温度2","yc_hs_0359","cur_59"]
[543,"b_右玉一期I-001发电机 绕组温度3","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期I-001发电机 绕组温度3","yc_hs_0359","cur_60"]
[544,"b_右玉一期I-001发电机转速","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期I-001发电机转速","yc_hs_0359","cur_64"]
[545,"b_右玉一期I-001发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期I-001发电机驱动端轴承温度","yc_hs_0359","cur_65"]
[546,"b_右玉一期I-001发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期I-001发电机非驱动端轴承温度","yc_hs_0359","cur_66"]
[547,"b_右玉一期I-001舱内温度","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期I-001舱内温度","yc_hs_0359","cur_72"]
[548,"b_右玉一期I-001舱外温度","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期I-001舱外温度","yc_hs_0359","cur_74"]
[549,"b_右玉一期I-001风向","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期I-001风向","yc_hs_0359","cur_76"]
[550,"b_右玉一期I-001风速","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期I-001风速","yc_hs_0359","cur_77"]
[551,"b_右玉一期I-001机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期I-001机舱中轴线与风向夹角","yc_hs_0359","cur_78"]
[552,"b_右玉一期I-001 1#桨叶片角度","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期I-001 1#桨叶片角度","yc_hs_0359","cur_79"]
[553,"b_右玉一期I-001 2#桨叶片角度","右玉风光互补电站","WOF34900079",1,"SXYY.T1_L1.WTG001.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期I-001 2#桨叶片角度","yc_hs_0359","cur_81"]
[554,"b_右玉一期I-003发电机 绕组温度1","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期I-003发电机 绕组温度1","yc_hs_0360","cur_100"]
[555,"b_右玉一期I-003发电机 绕组温度2","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期I-003发电机 绕组温度2","yc_hs_0361","cur_01"]
[556,"b_右玉一期I-003发电机 绕组温度3","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期I-003发电机 绕组温度3","yc_hs_0361","cur_02"]
[557,"b_右玉一期I-003发电机转速","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期I-003发电机转速","yc_hs_0361","cur_06"]
[558,"b_右玉一期I-003发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期I-003发电机驱动端轴承温度","yc_hs_0361","cur_07"]
[559,"b_右玉一期I-003发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期I-003发电机非驱动端轴承温度","yc_hs_0361","cur_08"]
[560,"b_右玉一期I-003舱内温度","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期I-003舱内温度","yc_hs_0361","cur_14"]
[561,"b_右玉一期I-003舱外温度","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期I-003舱外温度","yc_hs_0361","cur_16"]
[562,"b_右玉一期I-003风向","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期I-003风向","yc_hs_0361","cur_18"]
[563,"b_右玉一期I-003风速","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期I-003风速","yc_hs_0361","cur_19"]
[564,"b_右玉一期I-003机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期I-003机舱中轴线与风向夹角","yc_hs_0361","cur_20"]
[565,"b_右玉一期I-003 1#桨叶片角度","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期I-003 1#桨叶片角度","yc_hs_0361","cur_21"]
[566,"b_右玉一期I-003 2#桨叶片角度","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期I-003 2#桨叶片角度","yc_hs_0361","cur_23"]
[567,"b_右玉一期I-003 3#桨叶片角度","右玉风光互补电站","WOF34900079",3,"SXYY.T1_L1.WTG003.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期I-003 3#桨叶片角度","yc_hs_0361","cur_25"]
[568,"b_右玉一期I-004机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期I-004机舱侧向振动(已滤波)","yc_hs_0362","cur_24"]
[569,"b_右玉一期I-004机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期I-004机舱轴向振动(已滤波)","yc_hs_0362","cur_26"]
[570,"b_右玉一期I-004机舱角度","右玉风光互补电站","WOF34900079",4,"SXYY.T1_L1.WTG004.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期I-004机舱角度","yc_hs_0362","cur_27"]
[572,"b_右玉一期I-005发电机有功功率","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WGEN.GenActivePW","有功功率","active_power","b_右玉一期I-005发电机有功功率","yc_hs_0362","cur_39"]
[573,"b_右玉一期I-005发电机 绕组温度1","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期I-005发电机 绕组温度1","yc_hs_0362","cur_42"]
[574,"b_右玉一期I-005发电机 绕组温度2","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期I-005发电机 绕组温度2","yc_hs_0362","cur_43"]
[575,"b_右玉一期I-005发电机 绕组温度3","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期I-005发电机 绕组温度3","yc_hs_0362","cur_44"]
[576,"b_右玉一期I-005发电机转速","右玉风光互补电站","WOF34900079",5,"SXYY.T1_L1.WTG005.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期I-005发电机转速","yc_hs_0362","cur_48"]
[577,"b_右玉一期Ⅲ-033 2#桨叶片角度","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅲ-033 2#桨叶片角度","yc_hs_0382","cur_55"]
[578,"b_右玉一期Ⅲ-033 3#桨叶片角度","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅲ-033 3#桨叶片角度","yc_hs_0382","cur_57"]
[579,"b_右玉一期Ⅲ-033机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅲ-033机舱侧向振动(已滤波)","yc_hs_0382","cur_85"]
[580,"b_右玉一期Ⅲ-033机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅲ-033机舱轴向振动(已滤波)","yc_hs_0382","cur_87"]
[581,"b_右玉一期Ⅲ-033机舱角度","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅲ-033机舱角度","yc_hs_0382","cur_88"]
[583,"b_右玉一期Ⅲ-031舱内温度","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅲ-031舱内温度","yc_hs_0381","cur_04"]
[584,"b_右玉一期Ⅲ-031舱外温度","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅲ-031舱外温度","yc_hs_0381","cur_06"]
[585,"b_右玉一期Ⅲ-031风向","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅲ-031风向","yc_hs_0381","cur_08"]
[586,"b_右玉一期Ⅲ-031风速","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅲ-031风速","yc_hs_0381","cur_09"]
[587,"b_右玉一期Ⅲ-031机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅲ-031机舱中轴线与风向夹角","yc_hs_0381","cur_10"]
[588,"b_右玉一期Ⅲ-031 1#桨叶片角度","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅲ-031 1#桨叶片角度","yc_hs_0381","cur_11"]
[589,"b_右玉一期Ⅲ-031 2#桨叶片角度","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅲ-031 2#桨叶片角度","yc_hs_0381","cur_13"]
[590,"b_右玉一期Ⅲ-031 3#桨叶片角度","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅲ-031 3#桨叶片角度","yc_hs_0381","cur_15"]
[591,"b_右玉一期Ⅲ-031机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅲ-031机舱侧向振动(已滤波)","yc_hs_0381","cur_43"]
[592,"b_右玉一期Ⅲ-031机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅲ-031机舱轴向振动(已滤波)","yc_hs_0381","cur_45"]
[593,"b_右玉一期Ⅲ-031机舱角度","右玉风光互补电站","WOF34900079",31,"SXYY.T1_L3.WTG031.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅲ-031机舱角度","yc_hs_0381","cur_46"]
[595,"b_右玉一期Ⅲ-032发电机有功功率","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅲ-032发电机有功功率","yc_hs_0381","cur_58"]
[596,"b_右玉一期Ⅲ-032发电机 绕组温度1","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅲ-032发电机 绕组温度1","yc_hs_0381","cur_61"]
[597,"b_右玉一期Ⅲ-032发电机 绕组温度2","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅲ-032发电机 绕组温度2","yc_hs_0381","cur_62"]
[598,"b_右玉一期Ⅲ-032发电机 绕组温度3","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅲ-032发电机 绕组温度3","yc_hs_0381","cur_63"]
[599,"b_右玉一期Ⅲ-032发电机转速","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅲ-032发电机转速","yc_hs_0381","cur_67"]
[600,"b_右玉一期Ⅲ-032发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅲ-032发电机驱动端轴承温度","yc_hs_0381","cur_68"]
[601,"b_右玉一期Ⅲ-032发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅲ-032发电机非驱动端轴承温度","yc_hs_0381","cur_69"]
[602,"b_右玉一期Ⅲ-032舱内温度","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅲ-032舱内温度","yc_hs_0381","cur_75"]
[603,"b_右玉一期Ⅲ-032舱外温度","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅲ-032舱外温度","yc_hs_0381","cur_77"]
[604,"b_右玉一期Ⅲ-032风向","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅲ-032风向","yc_hs_0381","cur_79"]
[605,"b_右玉一期Ⅲ-032风速","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅲ-032风速","yc_hs_0381","cur_80"]
[606,"b_右玉一期Ⅲ-032机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅲ-032机舱中轴线与风向夹角","yc_hs_0381","cur_81"]
[607,"b_右玉一期Ⅲ-032 1#桨叶片角度","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅲ-032 1#桨叶片角度","yc_hs_0381","cur_82"]
[608,"b_右玉一期Ⅲ-032 2#桨叶片角度","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉一期Ⅲ-032 2#桨叶片角度","yc_hs_0381","cur_84"]
[609,"b_右玉一期Ⅲ-032 3#桨叶片角度","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉一期Ⅲ-032 3#桨叶片角度","yc_hs_0381","cur_86"]
[610,"b_右玉一期Ⅲ-032机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉一期Ⅲ-032机舱侧向振动(已滤波)","yc_hs_0382","cur_14"]
[611,"b_右玉一期Ⅲ-032机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉一期Ⅲ-032机舱轴向振动(已滤波)","yc_hs_0382","cur_16"]
[612,"b_右玉一期Ⅲ-032机舱角度","右玉风光互补电站","WOF34900079",32,"SXYY.T1_L3.WTG032.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉一期Ⅲ-032机舱角度","yc_hs_0382","cur_17"]
[614,"b_右玉一期Ⅲ-033发电机有功功率","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WGEN.GenActivePW","有功功率","active_power","b_右玉一期Ⅲ-033发电机有功功率","yc_hs_0382","cur_29"]
[615,"b_右玉一期Ⅲ-033发电机 绕组温度1","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","b_右玉一期Ⅲ-033发电机 绕组温度1","yc_hs_0382","cur_32"]
[616,"b_右玉一期Ⅲ-033发电机 绕组温度2","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","b_右玉一期Ⅲ-033发电机 绕组温度2","yc_hs_0382","cur_33"]
[617,"b_右玉一期Ⅲ-033发电机 绕组温度3","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","b_右玉一期Ⅲ-033发电机 绕组温度3","yc_hs_0382","cur_34"]
[618,"b_右玉一期Ⅲ-033发电机转速","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WGEN.GenSpd","发电机转速","generator_speed","b_右玉一期Ⅲ-033发电机转速","yc_hs_0382","cur_38"]
[619,"b_右玉一期Ⅲ-033发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉一期Ⅲ-033发电机驱动端轴承温度","yc_hs_0382","cur_39"]
[620,"b_右玉一期Ⅲ-033发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉一期Ⅲ-033发电机非驱动端轴承温度","yc_hs_0382","cur_40"]
[621,"b_右玉一期Ⅲ-033舱内温度","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉一期Ⅲ-033舱内温度","yc_hs_0382","cur_46"]
[622,"b_右玉一期Ⅲ-033舱外温度","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉一期Ⅲ-033舱外温度","yc_hs_0382","cur_48"]
[623,"b_右玉一期Ⅲ-033风向","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉一期Ⅲ-033风向","yc_hs_0382","cur_50"]
[624,"b_右玉一期Ⅲ-033风速","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WNAC.WindSpeed","风速","wind_velocity","b_右玉一期Ⅲ-033风速","yc_hs_0382","cur_51"]
[625,"b_右玉一期Ⅲ-033机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉一期Ⅲ-033机舱中轴线与风向夹角","yc_hs_0382","cur_52"]
[626,"b_右玉一期Ⅲ-033 1#桨叶片角度","右玉风光互补电站","WOF34900079",33,"SXYY.T1_L3.WTG033.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉一期Ⅲ-033 1#桨叶片角度","yc_hs_0382","cur_53"]
[627,"i_平陆一期 II-13发电机非驱动端轴承温度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 II-13发电机非驱动端轴承温度","yc_hs_0005","cur_90"]
[628,"i_平陆一期 II-13发电机定子U相线圈温度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 II-13发电机定子U相线圈温度","yc_hs_0005","cur_91"]
[629,"i_平陆一期 II-13发电机定子V相线圈温度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 II-13发电机定子V相线圈温度","yc_hs_0121","cur_19"]
[630,"i_平陆一期 III-20发电机转速","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 III-20发电机转速","yc_hs_0008","cur_05"]
[631,"i_平陆一期 III-20发电机驱动端轴承温度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 III-20发电机驱动端轴承温度","yc_hs_0008","cur_06"]
[632,"i_平陆一期 III-20发电机非驱动端轴承温度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 III-20发电机非驱动端轴承温度","yc_hs_0008","cur_07"]
[633,"i_平陆一期 III-20发电机定子U相线圈温度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 III-20发电机定子U相线圈温度","yc_hs_0008","cur_08"]
[634,"i_平陆一期 III-20发电机定子V相线圈温度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 III-20发电机定子V相线圈温度","yc_hs_0125","cur_47"]
[635,"i_平陆一期 I-02 2#桨叶片角度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 I-02 2#桨叶片角度","yc_hs_0103","cur_92"]
[636,"i_平陆一期 III-24主轴承外圈温度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 III-24主轴承外圈温度","yc_hs_0009","cur_51"]
[637,"i_平陆一期 III-22发电机定子W相线圈温度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 III-22发电机定子W相线圈温度","yc_hs_0245","cur_24"]
[638,"i_平陆一期 I-02发电机有功功率","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 I-02发电机有功功率","yc_hs_0002","cur_45"]
[639,"i_平陆一期 I-02发电机转速","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 I-02发电机转速","yc_hs_0002","cur_47"]
[640,"i_平陆一期 I-01主轴转速","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 I-01主轴转速","yc_hs_0002","cur_33"]
[641,"i_平陆一期 I-01齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 I-01齿轮箱高速轴非驱动端轴承温度","yc_hs_0002","cur_36"]
[642,"i_平陆一期 I-01发电机转速","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 I-01发电机转速","yc_hs_0002","cur_17"]
[643,"i_平陆一期 I-01发电机有功功率","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 I-01发电机有功功率","yc_hs_0002","cur_15"]
[644,"i_平陆一期 I-01发电机定子U相线圈温度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 I-01发电机定子U相线圈温度","yc_hs_0002","cur_20"]
[645,"i_平陆一期 II-14 1#桨叶片角度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 II-14 1#桨叶片角度","yc_hs_0109","cur_33"]
[646,"i_平陆一期 II-13舱外温度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 II-13舱外温度","yc_hs_0005","cur_98"]
[647,"i_平陆一期 II-13发电机定子W相线圈温度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 II-13发电机定子W相线圈温度","yc_hs_0121","cur_20"]
[648,"i_平陆一期 II-10主轴承外圈温度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 II-10主轴承外圈温度","yc_hs_0005","cur_17"]
[649,"i_平陆一期 II-08舱内温度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 II-08舱内温度","yc_hs_0004","cur_41"]
[650,"i_平陆一期 III-17风向","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 III-17风向","yc_hs_0007","cur_23"]
[651,"i_平陆一期 II-09发电机定子V相线圈温度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 II-09发电机定子V相线圈温度","yc_hs_0118","cur_71"]
[652,"i_平陆一期 II-09发电机定子W相线圈温度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 II-09发电机定子W相线圈温度","yc_hs_0118","cur_72"]
[653,"i_平陆一期 II-09舱内温度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 II-09舱内温度","yc_hs_0004","cur_72"]
[654,"i_平陆一期 II-11齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 II-11齿轮箱高速轴非驱动端轴承温度","yc_hs_0005","cur_46"]
[655,"i_平陆一期 III-24齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 III-24齿轮箱高速轴非驱动端轴承温度","yc_hs_0009","cur_49"]
[656,"i_平陆一期 III-20机舱中轴线与风向夹角","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 III-20机舱中轴线与风向夹角","yc_hs_0125","cur_52"]
[657,"i_平陆一期 III-23齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 III-23齿轮箱高速轴非驱动端轴承温度","yc_hs_0009","cur_18"]
[658,"i_平陆一期 III-21发电机驱动端轴承温度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 III-21发电机驱动端轴承温度","yc_hs_0008","cur_37"]
[659,"i_平陆一期 III-20发电机定子W相线圈温度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 III-20发电机定子W相线圈温度","yc_hs_0125","cur_48"]
[660,"i_平陆一期 II-10机舱中轴线与风向夹角","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 II-10机舱中轴线与风向夹角","yc_hs_0119","cur_46"]
[661,"i_平陆一期 III-20舱内温度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 III-20舱内温度","yc_hs_0008","cur_13"]
[662,"i_平陆一期 II-11机舱角度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 II-11机舱角度","yc_hs_0005","cur_53"]
[663,"i_平陆一期 II-11扭缆角度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 II-11扭缆角度","yc_hs_0005","cur_54"]
[664,"i_平陆一期 III-22发电机有功功率","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 III-22发电机有功功率","yc_hs_0008","cur_65"]
[665,"i_平陆一期 III-22发电机转速","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 III-22发电机转速","yc_hs_0008","cur_67"]
[666,"i_平陆一期 III-22发电机驱动端轴承温度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 III-22发电机驱动端轴承温度","yc_hs_0008","cur_68"]
[667,"i_平陆一期 III-22发电机非驱动端轴承温度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 III-22发电机非驱动端轴承温度","yc_hs_0008","cur_69"]
[668,"i_平陆一期 III-22发电机定子U相线圈温度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 III-22发电机定子U相线圈温度","yc_hs_0008","cur_70"]
[669,"i_平陆一期 III-22发电机定子V相线圈温度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 III-22发电机定子V相线圈温度","yc_hs_0245","cur_23"]
[670,"i_平陆一期 I-06齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 I-06齿轮箱高速轴非驱动端轴承温度","yc_hs_0003","cur_91"]
[671,"i_平陆一期 I-04发电机有功功率","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 I-04发电机有功功率","yc_hs_0003","cur_07"]
[672,"i_平陆一期 II-13 3#桨叶片角度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 II-13 3#桨叶片角度","yc_hs_0108","cur_92"]
[673,"i_平陆一期 I-03机舱角度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 I-03机舱角度","yc_hs_0003","cur_05"]
[674,"i_平陆一期 I-03扭缆角度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 I-03扭缆角度","yc_hs_0003","cur_06"]
[675,"i_平陆一期 II-16 3#桨叶片角度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 II-16 3#桨叶片角度","yc_hs_0110","cur_27"]
[676,"i_平陆一期 II-15机舱中轴线与风向夹角","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 II-15机舱中轴线与风向夹角","yc_hs_0122","cur_50"]
[677,"i_平陆一期 II-15 1#桨叶片角度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 II-15 1#桨叶片角度","yc_hs_0109","cur_78"]
[678,"i_平陆一期 I-05 2#桨叶片角度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 I-05 2#桨叶片角度","yc_hs_0105","cur_27"]
[679,"i_平陆一期 I-05 3#桨叶片角度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 I-05 3#桨叶片角度","yc_hs_0105","cur_29"]
[680,"i_平陆一期 III-17发电机转速","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 III-17发电机转速","yc_hs_0007","cur_12"]
[681,"i_平陆一期 III-17发电机驱动端轴承温度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 III-17发电机驱动端轴承温度","yc_hs_0007","cur_13"]
[682,"i_平陆一期 III-17发电机非驱动端轴承温度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 III-17发电机非驱动端轴承温度","yc_hs_0007","cur_14"]
[683,"i_平陆一期 II-08发电机定子W相线圈温度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 II-08发电机定子W相线圈温度","yc_hs_0118","cur_12"]
[684,"i_平陆一期 III-20主轴承外圈温度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 III-20主轴承外圈温度","yc_hs_0008","cur_27"]
[685,"i_平陆一期 III-18机舱中轴线与风向夹角","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 III-18机舱中轴线与风向夹角","yc_hs_0124","cur_40"]
[686,"i_平陆一期 I-03发电机有功功率","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 I-03发电机有功功率","yc_hs_0002","cur_76"]
[687,"i_平陆一期 I-02机舱轴向振动(已滤波)","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 I-02机舱轴向振动(已滤波)","yc_hs_0002","cur_73"]
[688,"i_平陆一期 I-02机舱角度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 I-02机舱角度","yc_hs_0002","cur_74"]
[689,"i_平陆一期 I-02扭缆角度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 I-02扭缆角度","yc_hs_0002","cur_75"]
[690,"i_平陆一期 I-02发电机驱动端轴承温度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 I-02发电机驱动端轴承温度","yc_hs_0002","cur_48"]
[691,"i_平陆一期 I-02发电机非驱动端轴承温度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 I-02发电机非驱动端轴承温度","yc_hs_0002","cur_49"]
[692,"i_平陆一期 I-02发电机定子U相线圈温度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 I-02发电机定子U相线圈温度","yc_hs_0002","cur_50"]
[693,"i_平陆一期 III-20 1#桨叶片角度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 III-20 1#桨叶片角度","yc_hs_0112","cur_03"]
[694,"i_平陆一期 III-21风速","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 III-21风速","yc_hs_0008","cur_48"]
[695,"i_平陆一期 I-06机舱轴向振动(已滤波)","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 I-06机舱轴向振动(已滤波)","yc_hs_0003","cur_97"]
[696,"i_平陆一期 I-06主轴转速","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 I-06主轴转速","yc_hs_0003","cur_88"]
[697,"i_平陆一期 II-11主轴承外圈温度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 II-11主轴承外圈温度","yc_hs_0005","cur_48"]
[698,"i_平陆一期 II-11舱外温度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 II-11舱外温度","yc_hs_0005","cur_36"]
[699,"i_平陆一期 III-21主轴承外圈温度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 III-21主轴承外圈温度","yc_hs_0008","cur_58"]
[700,"i_平陆一期 III-21机舱侧向振动(已滤波)","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 III-21机舱侧向振动(已滤波)","yc_hs_0008","cur_61"]
[701,"i_平陆一期 III-21机舱轴向振动(已滤波)","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 III-21机舱轴向振动(已滤波)","yc_hs_0008","cur_62"]
[702,"i_平陆一期 III-21机舱角度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 III-21机舱角度","yc_hs_0008","cur_63"]
[703,"i_平陆一期 I-04主轴承外圈温度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 I-04主轴承外圈温度","yc_hs_0003","cur_31"]
[704,"i_平陆一期 I-04发电机转速","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 I-04发电机转速","yc_hs_0003","cur_09"]
[705,"i_平陆一期 I-04发电机驱动端轴承温度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 I-04发电机驱动端轴承温度","yc_hs_0003","cur_10"]
[706,"i_平陆一期 I-04发电机非驱动端轴承温度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 I-04发电机非驱动端轴承温度","yc_hs_0003","cur_11"]
[707,"i_平陆一期 I-04发电机定子U相线圈温度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 I-04发电机定子U相线圈温度","yc_hs_0003","cur_12"]
[708,"i_平陆一期 I-06扭缆角度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 I-06扭缆角度","yc_hs_0003","cur_99"]
[709,"i_平陆一期 III-19发电机定子W相线圈温度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 III-19发电机定子W相线圈温度","yc_hs_0124","cur_100"]
[710,"i_平陆一期 II-11机舱中轴线与风向夹角","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 II-11机舱中轴线与风向夹角","yc_hs_0120","cur_06"]
[711,"i_平陆一期 II-11 1#桨叶片角度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 II-11 1#桨叶片角度","yc_hs_0107","cur_98"]
[712,"i_平陆一期 II-09 3#桨叶片角度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 II-09 3#桨叶片角度","yc_hs_0107","cur_12"]
[713,"i_平陆一期 I-04舱内温度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 I-04舱内温度","yc_hs_0003","cur_17"]
[714,"i_平陆一期 III-20 2#桨叶片角度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 III-20 2#桨叶片角度","yc_hs_0112","cur_05"]
[715,"i_平陆一期 II-15主轴转速","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 II-15主轴转速","yc_hs_0006","cur_67"]
[716,"i_平陆一期 II-08 3#桨叶片角度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 II-08 3#桨叶片角度","yc_hs_0106","cur_67"]
[717,"i_平陆一期 II-12发电机有功功率","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 II-12发电机有功功率","yc_hs_0005","cur_55"]
[718,"i_平陆一期 II-12发电机转速","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 II-12发电机转速","yc_hs_0005","cur_57"]
[719,"i_平陆一期 II-08扭缆角度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 II-08扭缆角度","yc_hs_0004","cur_61"]
[720,"i_平陆一期 I-03舱外温度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 I-03舱外温度","yc_hs_0002","cur_88"]
[721,"i_平陆一期 I-03风向","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 I-03风向","yc_hs_0002","cur_89"]
[722,"i_平陆一期 II-09发电机驱动端轴承温度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 II-09发电机驱动端轴承温度","yc_hs_0004","cur_65"]
[723,"i_平陆一期 II-12 3#桨叶片角度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 II-12 3#桨叶片角度","yc_hs_0108","cur_47"]
[724,"i_平陆一期 III-22机舱轴向振动(已滤波)","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 III-22机舱轴向振动(已滤波)","yc_hs_0008","cur_93"]
[725,"i_平陆一期 III-22机舱角度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 III-22机舱角度","yc_hs_0008","cur_94"]
[726,"i_平陆一期 III-21机舱中轴线与风向夹角","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 III-21机舱中轴线与风向夹角","yc_hs_0125","cur_90"]
[727,"i_平陆一期 III-21 1#桨叶片角度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 III-21 1#桨叶片角度","yc_hs_0112","cur_48"]
[728,"i_平陆一期 III-21 2#桨叶片角度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 III-21 2#桨叶片角度","yc_hs_0112","cur_50"]
[729,"i_平陆一期 III-21 3#桨叶片角度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 III-21 3#桨叶片角度","yc_hs_0112","cur_52"]
[730,"i_平陆一期 III-21发电机有功功率","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 III-21发电机有功功率","yc_hs_0008","cur_34"]
[731,"i_平陆一期 III-21发电机转速","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 III-21发电机转速","yc_hs_0008","cur_36"]
[732,"i_平陆一期 I-01 1#桨叶片角度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 I-01 1#桨叶片角度","yc_hs_0103","cur_45"]
[733,"i_平陆一期 I-01 2#桨叶片角度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 I-01 2#桨叶片角度","yc_hs_0103","cur_47"]
[734,"i_平陆一期 I-01 3#桨叶片角度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 I-01 3#桨叶片角度","yc_hs_0103","cur_49"]
[735,"i_平陆一期 I-07发电机驱动端轴承温度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 I-07发电机驱动端轴承温度","yc_hs_0004","cur_03"]
[736,"i_平陆一期 I-07发电机非驱动端轴承温度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 I-07发电机非驱动端轴承温度","yc_hs_0004","cur_04"]
[737,"i_平陆一期 I-07发电机定子U相线圈温度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 I-07发电机定子U相线圈温度","yc_hs_0004","cur_05"]
[738,"i_平陆一期 III-24发电机驱动端轴承温度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 III-24发电机驱动端轴承温度","yc_hs_0009","cur_30"]
[739,"i_平陆一期 II-12机舱中轴线与风向夹角","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 II-12机舱中轴线与风向夹角","yc_hs_0120","cur_62"]
[740,"i_平陆一期 II-12 1#桨叶片角度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 II-12 1#桨叶片角度","yc_hs_0108","cur_43"]
[741,"i_平陆一期 II-12 2#桨叶片角度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 II-12 2#桨叶片角度","yc_hs_0108","cur_45"]
[742,"i_平陆一期 I-02发电机定子V相线圈温度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 I-02发电机定子V相线圈温度","yc_hs_0114","cur_09"]
[743,"i_平陆一期 I-02发电机定子W相线圈温度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 I-02发电机定子W相线圈温度","yc_hs_0114","cur_26"]
[744,"i_平陆一期 I-02舱内温度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 I-02舱内温度","yc_hs_0002","cur_55"]
[745,"i_平陆一期 I-02舱外温度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 I-02舱外温度","yc_hs_0002","cur_57"]
[746,"i_平陆一期 I-02风向","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 I-02风向","yc_hs_0002","cur_58"]
[747,"i_平陆一期 I-02风速","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 I-02风速","yc_hs_0002","cur_59"]
[748,"i_平陆一期 I-02机舱中轴线与风向夹角","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 I-02机舱中轴线与风向夹角","yc_hs_0114","cur_41"]
[749,"i_平陆一期 I-02 1#桨叶片角度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 I-02 1#桨叶片角度","yc_hs_0103","cur_90"]
[750,"i_平陆一期 III-19发电机定子U相线圈温度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 III-19发电机定子U相线圈温度","yc_hs_0007","cur_77"]
[751,"i_平陆一期 III-19发电机定子V相线圈温度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 III-19发电机定子V相线圈温度","yc_hs_0124","cur_99"]
[752,"i_平陆一期 III-21发电机定子U相线圈温度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 III-21发电机定子U相线圈温度","yc_hs_0008","cur_39"]
[753,"i_平陆一期 III-21发电机定子V相线圈温度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 III-21发电机定子V相线圈温度","yc_hs_0125","cur_85"]
[754,"i_平陆一期 III-21发电机定子W相线圈温度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 III-21发电机定子W相线圈温度","yc_hs_0125","cur_86"]
[755,"i_平陆一期 I-04 3#桨叶片角度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 I-04 3#桨叶片角度","yc_hs_0104","cur_84"]
[756,"i_平陆一期 I-06风速","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 I-06风速","yc_hs_0003","cur_83"]
[757,"i_平陆一期 I-06机舱中轴线与风向夹角","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 I-06机舱中轴线与风向夹角","yc_hs_0116","cur_87"]
[758,"i_平陆一期 I-06 1#桨叶片角度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 I-06 1#桨叶片角度","yc_hs_0105","cur_70"]
[759,"i_平陆一期 I-06 2#桨叶片角度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 I-06 2#桨叶片角度","yc_hs_0105","cur_72"]
[760,"i_平陆一期 III-24发电机定子U相线圈温度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 III-24发电机定子U相线圈温度","yc_hs_0009","cur_32"]
[761,"i_平陆一期 III-24发电机定子V相线圈温度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 III-24发电机定子V相线圈温度","yc_hs_0245","cur_99"]
[762,"i_平陆一期 III-24发电机定子W相线圈温度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 III-24发电机定子W相线圈温度","yc_hs_0245","cur_100"]
[763,"i_平陆一期 III-24舱内温度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 III-24舱内温度","yc_hs_0009","cur_37"]
[764,"i_平陆一期 II-15舱外温度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 II-15舱外温度","yc_hs_0006","cur_60"]
[765,"i_平陆一期 II-15风向","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 II-15风向","yc_hs_0006","cur_61"]
[766,"i_平陆一期 II-15风速","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 II-15风速","yc_hs_0006","cur_62"]
[767,"i_平陆一期 I-03发电机转速","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 I-03发电机转速","yc_hs_0002","cur_78"]
[768,"i_平陆一期 I-03发电机驱动端轴承温度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 I-03发电机驱动端轴承温度","yc_hs_0002","cur_79"]
[769,"i_平陆一期 I-03发电机非驱动端轴承温度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 I-03发电机非驱动端轴承温度","yc_hs_0002","cur_80"]
[770,"i_平陆一期 I-05发电机定子V相线圈温度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 I-05发电机定子V相线圈温度","yc_hs_0116","cur_14"]
[771,"i_平陆一期 II-08发电机有功功率","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 II-08发电机有功功率","yc_hs_0004","cur_31"]
[772,"i_平陆一期 II-11机舱轴向振动(已滤波)","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 II-11机舱轴向振动(已滤波)","yc_hs_0005","cur_52"]
[773,"i_平陆一期 I-03发电机定子W相线圈温度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 I-03发电机定子W相线圈温度","yc_hs_0114","cur_93"]
[774,"i_平陆一期 I-03舱内温度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 I-03舱内温度","yc_hs_0002","cur_86"]
[775,"i_平陆一期 II-15 3#桨叶片角度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 II-15 3#桨叶片角度","yc_hs_0109","cur_82"]
[776,"i_平陆一期 III-22扭缆角度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 III-22扭缆角度","yc_hs_0008","cur_95"]
[777,"i_平陆一期 III-19扭缆角度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 III-19扭缆角度","yc_hs_0008","cur_02"]
[778,"i_平陆一期 III-21扭缆角度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 III-21扭缆角度","yc_hs_0008","cur_64"]
[779,"i_平陆一期 I-07主轴转速","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 I-07主轴转速","yc_hs_0004","cur_19"]
[780,"i_平陆一期 I-06 3#桨叶片角度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 I-06 3#桨叶片角度","yc_hs_0105","cur_74"]
[781,"i_平陆一期 III-19发电机驱动端轴承温度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 III-19发电机驱动端轴承温度","yc_hs_0007","cur_75"]
[782,"i_平陆一期 III-19发电机非驱动端轴承温度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 III-19发电机非驱动端轴承温度","yc_hs_0007","cur_76"]
[783,"i_平陆一期 I-04 1#桨叶片角度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 I-04 1#桨叶片角度","yc_hs_0104","cur_80"]
[784,"i_平陆一期 I-04 2#桨叶片角度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 I-04 2#桨叶片角度","yc_hs_0104","cur_82"]
[785,"i_平陆一期 III-21发电机非驱动端轴承温度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 III-21发电机非驱动端轴承温度","yc_hs_0008","cur_38"]
[786,"i_平陆一期 III-22主轴转速","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 III-22主轴转速","yc_hs_0008","cur_84"]
[787,"i_平陆一期 I-04机舱侧向振动(已滤波)","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 I-04机舱侧向振动(已滤波)","yc_hs_0003","cur_34"]
[788,"i_平陆一期 III-20齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 III-20齿轮箱高速轴非驱动端轴承温度","yc_hs_0008","cur_25"]
[789,"i_平陆一期 II-10发电机转速","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 II-10发电机转速","yc_hs_0004","cur_95"]
[790,"i_平陆一期 III-20机舱轴向振动(已滤波)","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 III-20机舱轴向振动(已滤波)","yc_hs_0008","cur_31"]
[791,"i_平陆一期 II-15 2#桨叶片角度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 II-15 2#桨叶片角度","yc_hs_0109","cur_80"]
[792,"i_平陆一期 I-03齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 I-03齿轮箱高速轴非驱动端轴承温度","yc_hs_0002","cur_98"]
[793,"i_平陆一期 III-22齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 III-22齿轮箱高速轴非驱动端轴承温度","yc_hs_0008","cur_87"]
[794,"i_平陆一期 I-01风速","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 I-01风速","yc_hs_0002","cur_28"]
[795,"i_平陆一期 I-01机舱中轴线与风向夹角","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 I-01机舱中轴线与风向夹角","yc_hs_0113","cur_53"]
[796,"i_平陆一期 I-01舱外温度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 I-01舱外温度","yc_hs_0002","cur_27"]
[797,"i_平陆一期 II-15机舱侧向振动(已滤波)","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 II-15机舱侧向振动(已滤波)","yc_hs_0006","cur_75"]
[798,"i_平陆一期 II-15机舱轴向振动(已滤波)","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 II-15机舱轴向振动(已滤波)","yc_hs_0006","cur_76"]
[799,"i_平陆一期 II-15机舱角度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 II-15机舱角度","yc_hs_0006","cur_77"]
[800,"i_平陆一期 I-07机舱角度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 I-07机舱角度","yc_hs_0004","cur_29"]
[801,"i_平陆一期 I-07扭缆角度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 I-07扭缆角度","yc_hs_0004","cur_30"]
[802,"i_平陆一期 II-10机舱侧向振动(已滤波)","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 II-10机舱侧向振动(已滤波)","yc_hs_0005","cur_20"]
[803,"i_平陆一期 II-11机舱侧向振动(已滤波)","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 II-11机舱侧向振动(已滤波)","yc_hs_0005","cur_51"]
[804,"i_平陆一期 I-05发电机定子W相线圈温度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 I-05发电机定子W相线圈温度","yc_hs_0116","cur_15"]
[805,"i_平陆一期 I-05发电机转速","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 I-05发电机转速","yc_hs_0003","cur_40"]
[806,"i_平陆一期 I-07发电机有功功率","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 I-07发电机有功功率","yc_hs_0003","cur_100"]
[807,"i_平陆一期 I-07发电机转速","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 I-07发电机转速","yc_hs_0004","cur_02"]
[808,"i_平陆一期 I-07发电机定子V相线圈温度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 I-07发电机定子V相线圈温度","yc_hs_0117","cur_42"]
[809,"i_平陆一期 I-07发电机定子W相线圈温度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 I-07发电机定子W相线圈温度","yc_hs_0117","cur_44"]
[810,"i_平陆一期 I-01发电机定子V相线圈温度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 I-01发电机定子V相线圈温度","yc_hs_0113","cur_48"]
[811,"i_平陆一期 II-08舱外温度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 II-08舱外温度","yc_hs_0004","cur_43"]
[812,"i_平陆一期 II-08风向","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 II-08风向","yc_hs_0004","cur_44"]
[813,"i_平陆一期 II-13主轴转速","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 II-13主轴转速","yc_hs_0006","cur_05"]
[814,"i_平陆一期 III-17发电机定子U相线圈温度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 III-17发电机定子U相线圈温度","yc_hs_0007","cur_15"]
[815,"i_平陆一期 III-17发电机定子W相线圈温度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 III-17发电机定子W相线圈温度","yc_hs_0123","cur_74"]
[816,"i_平陆一期 III-18发电机驱动端轴承温度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 III-18发电机驱动端轴承温度","yc_hs_0007","cur_44"]
[817,"i_平陆一期 II-15齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 II-15齿轮箱高速轴非驱动端轴承温度","yc_hs_0006","cur_70"]
[818,"i_平陆一期 II-15主轴承外圈温度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 II-15主轴承外圈温度","yc_hs_0006","cur_72"]
[819,"i_平陆一期 I-04主轴转速","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 I-04主轴转速","yc_hs_0003","cur_26"]
[820,"i_平陆一期 III-19发电机转速","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 III-19发电机转速","yc_hs_0007","cur_74"]
[821,"i_平陆一期 I-01发电机定子W相线圈温度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 I-01发电机定子W相线圈温度","yc_hs_0113","cur_49"]
[822,"i_平陆一期 I-01机舱侧向振动(已滤波)","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 I-01机舱侧向振动(已滤波)","yc_hs_0002","cur_41"]
[823,"i_平陆一期 III-19主轴转速","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 III-19主轴转速","yc_hs_0007","cur_91"]
[824,"i_平陆一期 III-19齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 III-19齿轮箱高速轴非驱动端轴承温度","yc_hs_0007","cur_94"]
[825,"i_平陆一期 III-19主轴承外圈温度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 III-19主轴承外圈温度","yc_hs_0007","cur_96"]
[826,"i_平陆一期 III-19机舱侧向振动(已滤波)","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 III-19机舱侧向振动(已滤波)","yc_hs_0007","cur_99"]
[827,"i_平陆一期 II-14机舱侧向振动(已滤波)","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 II-14机舱侧向振动(已滤波)","yc_hs_0006","cur_44"]
[828,"i_平陆一期 I-07 2#桨叶片角度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 I-07 2#桨叶片角度","yc_hs_0106","cur_20"]
[829,"i_平陆一期 I-07 3#桨叶片角度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 I-07 3#桨叶片角度","yc_hs_0106","cur_22"]
[830,"i_平陆一期 III-18 3#桨叶片角度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 III-18 3#桨叶片角度","yc_hs_0111","cur_17"]
[831,"i_平陆一期 II-10 3#桨叶片角度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 II-10 3#桨叶片角度","yc_hs_0107","cur_57"]
[832,"i_平陆一期 III-17扭缆角度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 III-17扭缆角度","yc_hs_0007","cur_40"]
[833,"i_平陆一期 I-03主轴转速","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 I-03主轴转速","yc_hs_0002","cur_95"]
[834,"i_平陆一期 II-16齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 II-16齿轮箱高速轴非驱动端轴承温度","yc_hs_0007","cur_01"]
[835,"i_平陆一期 II-16主轴承外圈温度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 II-16主轴承外圈温度","yc_hs_0007","cur_03"]
[836,"i_平陆一期 II-15发电机有功功率","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 II-15发电机有功功率","yc_hs_0006","cur_48"]
[837,"i_平陆一期 II-15发电机转速","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 II-15发电机转速","yc_hs_0006","cur_50"]
[838,"i_平陆一期 I-05齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 I-05齿轮箱高速轴非驱动端轴承温度","yc_hs_0003","cur_60"]
[839,"i_平陆一期 III-20机舱角度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 III-20机舱角度","yc_hs_0008","cur_32"]
[840,"i_平陆一期 III-20扭缆角度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 III-20扭缆角度","yc_hs_0008","cur_33"]
[841,"i_平陆一期 I-06机舱角度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 I-06机舱角度","yc_hs_0003","cur_98"]
[842,"i_平陆一期 II-12机舱侧向振动(已滤波)","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 II-12机舱侧向振动(已滤波)","yc_hs_0005","cur_82"]
[843,"i_平陆一期 II-12机舱轴向振动(已滤波)","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 II-12机舱轴向振动(已滤波)","yc_hs_0005","cur_83"]
[844,"i_平陆一期 II-12机舱角度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 II-12机舱角度","yc_hs_0005","cur_84"]
[845,"i_平陆一期 II-12扭缆角度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 II-12扭缆角度","yc_hs_0005","cur_85"]
[846,"i_平陆一期 I-03风速","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 I-03风速","yc_hs_0002","cur_90"]
[847,"i_平陆一期 I-03机舱中轴线与风向夹角","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 I-03机舱中轴线与风向夹角","yc_hs_0115","cur_01"]
[848,"i_平陆一期 I-03 1#桨叶片角度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 I-03 1#桨叶片角度","yc_hs_0104","cur_35"]
[849,"i_平陆一期 I-05机舱侧向振动(已滤波)","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 I-05机舱侧向振动(已滤波)","yc_hs_0003","cur_65"]
[850,"i_平陆一期 I-05机舱轴向振动(已滤波)","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 I-05机舱轴向振动(已滤波)","yc_hs_0003","cur_66"]
[851,"i_平陆一期 I-05机舱角度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 I-05机舱角度","yc_hs_0003","cur_67"]
[852,"i_平陆一期 II-16机舱侧向振动(已滤波)","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 II-16机舱侧向振动(已滤波)","yc_hs_0007","cur_06"]
[853,"i_平陆一期 II-16机舱轴向振动(已滤波)","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 II-16机舱轴向振动(已滤波)","yc_hs_0007","cur_07"]
[854,"i_平陆一期 II-16机舱角度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 II-16机舱角度","yc_hs_0007","cur_08"]
[855,"i_平陆一期 II-16扭缆角度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 II-16扭缆角度","yc_hs_0007","cur_09"]
[856,"i_平陆一期 II-14发电机有功功率","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 II-14发电机有功功率","yc_hs_0006","cur_17"]
[857,"i_平陆一期 II-14发电机转速","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 II-14发电机转速","yc_hs_0006","cur_19"]
[858,"i_平陆一期 II-14发电机驱动端轴承温度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 II-14发电机驱动端轴承温度","yc_hs_0006","cur_20"]
[859,"i_平陆一期 II-14发电机非驱动端轴承温度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 II-14发电机非驱动端轴承温度","yc_hs_0006","cur_21"]
[860,"i_平陆一期 III-19机舱轴向振动(已滤波)","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 III-19机舱轴向振动(已滤波)","yc_hs_0007","cur_100"]
[861,"i_平陆一期 III-19机舱角度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 III-19机舱角度","yc_hs_0008","cur_01"]
[862,"i_平陆一期 I-05主轴承外圈温度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 I-05主轴承外圈温度","yc_hs_0003","cur_62"]
[863,"i_平陆一期 II-13主轴承外圈温度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 II-13主轴承外圈温度","yc_hs_0006","cur_10"]
[864,"i_平陆一期 II-15发电机驱动端轴承温度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 II-15发电机驱动端轴承温度","yc_hs_0006","cur_51"]
[865,"i_平陆一期 II-15发电机非驱动端轴承温度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 II-15发电机非驱动端轴承温度","yc_hs_0006","cur_52"]
[866,"i_平陆一期 II-10主轴转速","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 II-10主轴转速","yc_hs_0005","cur_12"]
[867,"i_平陆一期 II-13齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 II-13齿轮箱高速轴非驱动端轴承温度","yc_hs_0006","cur_08"]
[868,"i_平陆一期 III-17风速","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 III-17风速","yc_hs_0007","cur_24"]
[869,"i_平陆一期 III-17机舱中轴线与风向夹角","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 III-17机舱中轴线与风向夹角","yc_hs_0123","cur_78"]
[870,"i_平陆一期 III-17 1#桨叶片角度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 III-17 1#桨叶片角度","yc_hs_0110","cur_68"]
[871,"i_平陆一期 III-17 2#桨叶片角度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 III-17 2#桨叶片角度","yc_hs_0110","cur_70"]
[872,"i_平陆一期 III-17 3#桨叶片角度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 III-17 3#桨叶片角度","yc_hs_0110","cur_72"]
[873,"i_平陆一期 III-19发电机有功功率","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 III-19发电机有功功率","yc_hs_0007","cur_72"]
[874,"i_平陆一期 II-13机舱侧向振动(已滤波)","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 II-13机舱侧向振动(已滤波)","yc_hs_0006","cur_13"]
[875,"i_平陆一期 II-13机舱轴向振动(已滤波)","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 II-13机舱轴向振动(已滤波)","yc_hs_0006","cur_14"]
[876,"i_平陆一期 II-13机舱角度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 II-13机舱角度","yc_hs_0006","cur_15"]
[877,"i_平陆一期 II-13扭缆角度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 II-13扭缆角度","yc_hs_0006","cur_16"]
[878,"i_平陆一期 III-24发电机非驱动端轴承温度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 III-24发电机非驱动端轴承温度","yc_hs_0009","cur_31"]
[879,"i_平陆一期 II-14主轴转速","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 II-14主轴转速","yc_hs_0006","cur_36"]
[880,"i_平陆一期 II-14齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 II-14齿轮箱高速轴非驱动端轴承温度","yc_hs_0006","cur_39"]
[881,"i_平陆一期 III-20 3#桨叶片角度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 III-20 3#桨叶片角度","yc_hs_0112","cur_07"]
[882,"i_平陆一期 I-01机舱轴向振动(已滤波)","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 I-01机舱轴向振动(已滤波)","yc_hs_0002","cur_42"]
[883,"i_平陆一期 III-21舱内温度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 III-21舱内温度","yc_hs_0008","cur_44"]
[884,"i_平陆一期 III-21舱外温度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 III-21舱外温度","yc_hs_0008","cur_46"]
[885,"i_平陆一期 III-21风向","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 III-21风向","yc_hs_0008","cur_47"]
[886,"i_平陆一期 II-16发电机非驱动端轴承温度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 II-16发电机非驱动端轴承温度","yc_hs_0006","cur_83"]
[887,"i_平陆一期 II-16发电机定子U相线圈温度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 II-16发电机定子U相线圈温度","yc_hs_0006","cur_84"]
[888,"i_平陆一期 II-16发电机定子V相线圈温度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 II-16发电机定子V相线圈温度","yc_hs_0123","cur_05"]
[889,"i_平陆一期 II-16发电机定子W相线圈温度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 II-16发电机定子W相线圈温度","yc_hs_0123","cur_14"]
[890,"i_平陆一期 III-17发电机有功功率","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 III-17发电机有功功率","yc_hs_0007","cur_10"]
[891,"i_平陆一期 III-17机舱角度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 III-17机舱角度","yc_hs_0007","cur_39"]
[892,"i_平陆一期 III-24扭缆角度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 III-24扭缆角度","yc_hs_0009","cur_57"]
[893,"i_平陆一期 III-22机舱侧向振动(已滤波)","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 III-22机舱侧向振动(已滤波)","yc_hs_0008","cur_92"]
[894,"i_平陆一期 I-03 2#桨叶片角度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 I-03 2#桨叶片角度","yc_hs_0104","cur_37"]
[895,"i_平陆一期 I-03 3#桨叶片角度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 I-03 3#桨叶片角度","yc_hs_0104","cur_39"]
[896,"i_平陆一期 I-02 3#桨叶片角度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 I-02 3#桨叶片角度","yc_hs_0103","cur_94"]
[897,"i_平陆一期 II-14发电机定子U相线圈温度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 II-14发电机定子U相线圈温度","yc_hs_0006","cur_22"]
[898,"i_平陆一期 II-14发电机定子V相线圈温度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 II-14发电机定子V相线圈温度","yc_hs_0121","cur_83"]
[899,"i_平陆一期 II-14发电机定子W相线圈温度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 II-14发电机定子W相线圈温度","yc_hs_0121","cur_86"]
[900,"i_平陆一期 III-23主轴承外圈温度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 III-23主轴承外圈温度","yc_hs_0009","cur_20"]
[901,"i_平陆一期 III-24机舱侧向振动(已滤波)","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 III-24机舱侧向振动(已滤波)","yc_hs_0009","cur_54"]
[902,"i_平陆一期 III-24机舱轴向振动(已滤波)","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 III-24机舱轴向振动(已滤波)","yc_hs_0009","cur_55"]
[903,"i_平陆一期 III-24机舱角度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 III-24机舱角度","yc_hs_0009","cur_56"]
[904,"i_平陆一期 II-10 1#桨叶片角度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 II-10 1#桨叶片角度","yc_hs_0107","cur_53"]
[905,"i_平陆一期 II-10 2#桨叶片角度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 II-10 2#桨叶片角度","yc_hs_0107","cur_55"]
[906,"i_平陆一期 I-04机舱轴向振动(已滤波)","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 I-04机舱轴向振动(已滤波)","yc_hs_0003","cur_35"]
[907,"i_平陆一期 I-04机舱角度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 I-04机舱角度","yc_hs_0003","cur_36"]
[908,"i_平陆一期 I-04扭缆角度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 I-04扭缆角度","yc_hs_0003","cur_37"]
[909,"i_平陆一期 II-08发电机转速","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 II-08发电机转速","yc_hs_0004","cur_33"]
[910,"i_平陆一期 II-08发电机驱动端轴承温度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 II-08发电机驱动端轴承温度","yc_hs_0004","cur_34"]
[911,"i_平陆一期 II-08发电机非驱动端轴承温度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 II-08发电机非驱动端轴承温度","yc_hs_0004","cur_35"]
[912,"i_平陆一期 III-17主轴转速","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 III-17主轴转速","yc_hs_0007","cur_29"]
[913,"i_平陆一期 I-04舱外温度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 I-04舱外温度","yc_hs_0003","cur_19"]
[914,"i_平陆一期 I-04风向","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 I-04风向","yc_hs_0003","cur_20"]
[915,"i_平陆一期 I-04风速","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 I-04风速","yc_hs_0003","cur_21"]
[916,"i_平陆一期 I-04机舱中轴线与风向夹角","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 I-04机舱中轴线与风向夹角","yc_hs_0115","cur_58"]
[917,"i_平陆一期 III-19舱内温度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 III-19舱内温度","yc_hs_0007","cur_82"]
[918,"i_平陆一期 II-09舱外温度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 II-09舱外温度","yc_hs_0004","cur_74"]
[919,"i_平陆一期 II-09风向","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 II-09风向","yc_hs_0004","cur_75"]
[920,"i_平陆一期 II-09 2#桨叶片角度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 II-09 2#桨叶片角度","yc_hs_0107","cur_10"]
[921,"i_平陆一期 II-10发电机定子U相线圈温度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 II-10发电机定子U相线圈温度","yc_hs_0004","cur_98"]
[922,"i_平陆一期 II-10发电机定子V相线圈温度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 II-10发电机定子V相线圈温度","yc_hs_0119","cur_33"]
[923,"i_平陆一期 II-10发电机定子W相线圈温度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 II-10发电机定子W相线圈温度","yc_hs_0119","cur_34"]
[924,"i_平陆一期 I-07舱内温度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 I-07舱内温度","yc_hs_0004","cur_10"]
[925,"i_平陆一期 I-05发电机驱动端轴承温度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 I-05发电机驱动端轴承温度","yc_hs_0003","cur_41"]
[926,"i_平陆一期 I-05发电机非驱动端轴承温度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 I-05发电机非驱动端轴承温度","yc_hs_0003","cur_42"]
[927,"i_平陆一期 I-05发电机定子U相线圈温度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 I-05发电机定子U相线圈温度","yc_hs_0003","cur_43"]
[928,"i_平陆一期 II-09齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 II-09齿轮箱高速轴非驱动端轴承温度","yc_hs_0004","cur_84"]
[929,"i_平陆一期 II-09主轴承外圈温度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 II-09主轴承外圈温度","yc_hs_0004","cur_86"]
[930,"i_平陆一期 II-11 3#桨叶片角度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 II-11 3#桨叶片角度","yc_hs_0108","cur_02"]
[931,"i_平陆一期 III-20主轴转速","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 III-20主轴转速","yc_hs_0008","cur_22"]
[932,"i_平陆一期 III-23机舱中轴线与风向夹角","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 III-23机舱中轴线与风向夹角","yc_hs_0245","cur_66"]
[933,"i_平陆一期 III-23 1#桨叶片角度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 III-23 1#桨叶片角度","yc_hs_0113","cur_38"]
[934,"i_平陆一期 III-23 2#桨叶片角度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 III-23 2#桨叶片角度","yc_hs_0113","cur_40"]
[935,"i_平陆一期 II-14机舱轴向振动(已滤波)","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 II-14机舱轴向振动(已滤波)","yc_hs_0006","cur_45"]
[936,"i_平陆一期 II-14机舱角度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 II-14机舱角度","yc_hs_0006","cur_46"]
[937,"i_平陆一期 II-14扭缆角度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 II-14扭缆角度","yc_hs_0006","cur_47"]
[938,"i_平陆一期 II-09风速","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 II-09风速","yc_hs_0004","cur_76"]
[939,"i_平陆一期 II-09机舱中轴线与风向夹角","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 II-09机舱中轴线与风向夹角","yc_hs_0118","cur_76"]
[940,"i_平陆一期 I-05舱外温度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 I-05舱外温度","yc_hs_0003","cur_50"]
[941,"i_平陆一期 II-08 2#桨叶片角度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 II-08 2#桨叶片角度","yc_hs_0106","cur_65"]
[942,"i_平陆一期 II-10机舱轴向振动(已滤波)","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 II-10机舱轴向振动(已滤波)","yc_hs_0005","cur_21"]
[943,"i_平陆一期 II-10机舱角度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 II-10机舱角度","yc_hs_0005","cur_22"]
[944,"i_平陆一期 I-06机舱侧向振动(已滤波)","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 I-06机舱侧向振动(已滤波)","yc_hs_0003","cur_96"]
[945,"i_平陆一期 III-18发电机定子V相线圈温度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 III-18发电机定子V相线圈温度","yc_hs_0124","cur_29"]
[946,"i_平陆一期 III-18发电机定子W相线圈温度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 III-18发电机定子W相线圈温度","yc_hs_0124","cur_30"]
[947,"i_平陆一期 III-18舱内温度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 III-18舱内温度","yc_hs_0007","cur_51"]
[948,"i_平陆一期 III-18舱外温度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 III-18舱外温度","yc_hs_0007","cur_53"]
[949,"i_平陆一期 III-18风向","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 III-18风向","yc_hs_0007","cur_54"]
[950,"i_平陆一期 III-18风速","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 III-18风速","yc_hs_0007","cur_55"]
[951,"i_平陆一期 III-23机舱轴向振动(已滤波)","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 III-23机舱轴向振动(已滤波)","yc_hs_0009","cur_24"]
[952,"i_平陆一期 III-23机舱角度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 III-23机舱角度","yc_hs_0009","cur_25"]
[953,"i_平陆一期 I-03主轴承外圈温度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 I-03主轴承外圈温度","yc_hs_0002","cur_100"]
[954,"i_平陆一期 II-14舱内温度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 II-14舱内温度","yc_hs_0006","cur_27"]
[955,"i_平陆一期 II-14舱外温度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 II-14舱外温度","yc_hs_0006","cur_29"]
[956,"i_平陆一期 II-14风向","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 II-14风向","yc_hs_0006","cur_30"]
[957,"i_平陆一期 I-07舱外温度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 I-07舱外温度","yc_hs_0004","cur_12"]
[958,"i_平陆一期 I-07风向","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 I-07风向","yc_hs_0004","cur_13"]
[959,"i_平陆一期 I-07风速","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 I-07风速","yc_hs_0004","cur_14"]
[960,"i_平陆一期 I-07机舱中轴线与风向夹角","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 I-07机舱中轴线与风向夹角","yc_hs_0117","cur_52"]
[961,"i_平陆一期 I-07 1#桨叶片角度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 I-07 1#桨叶片角度","yc_hs_0106","cur_18"]
[962,"i_平陆一期 II-11主轴转速","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 II-11主轴转速","yc_hs_0005","cur_43"]
[963,"i_平陆一期 III-23扭缆角度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 III-23扭缆角度","yc_hs_0009","cur_26"]
[964,"i_平陆一期 III-23发电机转速","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 III-23发电机转速","yc_hs_0008","cur_98"]
[965,"i_平陆一期 III-23发电机驱动端轴承温度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 III-23发电机驱动端轴承温度","yc_hs_0008","cur_99"]
[966,"i_平陆一期 III-23发电机非驱动端轴承温度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 III-23发电机非驱动端轴承温度","yc_hs_0008","cur_100"]
[967,"i_平陆一期 III-23发电机定子U相线圈温度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 III-23发电机定子U相线圈温度","yc_hs_0009","cur_01"]
[968,"i_平陆一期 III-23发电机定子V相线圈温度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 III-23发电机定子V相线圈温度","yc_hs_0245","cur_61"]
[969,"i_平陆一期 I-06主轴承外圈温度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 I-06主轴承外圈温度","yc_hs_0003","cur_93"]
[970,"i_平陆一期 II-11舱内温度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 II-11舱内温度","yc_hs_0005","cur_34"]
[971,"i_平陆一期 III-17主轴承外圈温度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 III-17主轴承外圈温度","yc_hs_0007","cur_34"]
[972,"i_平陆一期 II-16舱内温度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 II-16舱内温度","yc_hs_0006","cur_89"]
[973,"i_平陆一期 II-16舱外温度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 II-16舱外温度","yc_hs_0006","cur_91"]
[974,"i_平陆一期 III-22 3#桨叶片角度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 III-22 3#桨叶片角度","yc_hs_0112","cur_97"]
[975,"i_平陆一期 I-06发电机有功功率","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 I-06发电机有功功率","yc_hs_0003","cur_69"]
[976,"i_平陆一期 I-06发电机转速","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 I-06发电机转速","yc_hs_0003","cur_71"]
[977,"i_平陆一期 I-06发电机驱动端轴承温度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 I-06发电机驱动端轴承温度","yc_hs_0003","cur_72"]
[978,"i_平陆一期 I-06发电机非驱动端轴承温度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 I-06发电机非驱动端轴承温度","yc_hs_0003","cur_73"]
[979,"i_平陆一期 I-06发电机定子U相线圈温度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 I-06发电机定子U相线圈温度","yc_hs_0003","cur_74"]
[980,"i_平陆一期 I-06发电机定子V相线圈温度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 I-06发电机定子V相线圈温度","yc_hs_0116","cur_80"]
[981,"i_平陆一期 I-06发电机定子W相线圈温度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 I-06发电机定子W相线圈温度","yc_hs_0116","cur_82"]
[982,"i_平陆一期 I-06舱内温度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 I-06舱内温度","yc_hs_0003","cur_79"]
[983,"i_平陆一期 I-06舱外温度","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 I-06舱外温度","yc_hs_0003","cur_81"]
[984,"i_平陆一期 I-06风向","平陆风电场","WOF35900004",6,"YCPL.T1_L1.WTG006.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 I-06风向","yc_hs_0003","cur_82"]
[985,"i_平陆一期 I-01舱内温度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 I-01舱内温度","yc_hs_0002","cur_25"]
[986,"i_平陆一期 I-01风向","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 I-01风向","yc_hs_0103","cur_44"]
[987,"i_平陆一期 III-24 1#桨叶片角度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 III-24 1#桨叶片角度","yc_hs_0113","cur_83"]
[988,"i_平陆一期 III-24 2#桨叶片角度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 III-24 2#桨叶片角度","yc_hs_0113","cur_85"]
[989,"i_平陆一期 III-24 3#桨叶片角度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 III-24 3#桨叶片角度","yc_hs_0113","cur_87"]
[990,"i_平陆一期 II-09 1#桨叶片角度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 II-09 1#桨叶片角度","yc_hs_0107","cur_08"]
[991,"i_平陆一期 I-07机舱侧向振动(已滤波)","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 I-07机舱侧向振动(已滤波)","yc_hs_0004","cur_27"]
[992,"i_平陆一期 I-07机舱轴向振动(已滤波)","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 I-07机舱轴向振动(已滤波)","yc_hs_0004","cur_28"]
[993,"i_平陆一期 II-15发电机定子U相线圈温度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 II-15发电机定子U相线圈温度","yc_hs_0006","cur_53"]
[994,"i_平陆一期 II-15发电机定子V相线圈温度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 II-15发电机定子V相线圈温度","yc_hs_0122","cur_43"]
[995,"i_平陆一期 II-15发电机定子W相线圈温度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 II-15发电机定子W相线圈温度","yc_hs_0122","cur_44"]
[996,"i_平陆一期 III-21主轴转速","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 III-21主轴转速","yc_hs_0008","cur_53"]
[997,"i_平陆一期 III-22 2#桨叶片角度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 III-22 2#桨叶片角度","yc_hs_0112","cur_95"]
[998,"i_平陆一期 II-11风向","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 II-11风向","yc_hs_0005","cur_37"]
[999,"i_平陆一期 II-11风速","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 II-11风速","yc_hs_0005","cur_38"]
[1000,"i_平陆一期 I-01发电机驱动端轴承温度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 I-01发电机驱动端轴承温度","yc_hs_0002","cur_18"]
[1001,"i_平陆一期 I-01发电机非驱动端轴承温度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 I-01发电机非驱动端轴承温度","yc_hs_0002","cur_19"]
[1002,"i_平陆一期 III-23舱内温度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 III-23舱内温度","yc_hs_0009","cur_06"]
[1003,"i_平陆一期 II-10发电机有功功率","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 II-10发电机有功功率","yc_hs_0004","cur_93"]
[1004,"i_平陆一期 II-14主轴承外圈温度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 II-14主轴承外圈温度","yc_hs_0006","cur_41"]
[1005,"i_平陆一期 II-10风向","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 II-10风向","yc_hs_0005","cur_06"]
[1006,"i_平陆一期 II-10风速","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 II-10风速","yc_hs_0005","cur_07"]
[1007,"i_平陆一期 I-03机舱轴向振动(已滤波)","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 I-03机舱轴向振动(已滤波)","yc_hs_0003","cur_04"]
[1008,"i_平陆一期 II-09发电机定子U相线圈温度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 II-09发电机定子U相线圈温度","yc_hs_0004","cur_67"]
[1009,"i_平陆一期 III-18 2#桨叶片角度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 III-18 2#桨叶片角度","yc_hs_0111","cur_15"]
[1010,"i_平陆一期 II-14风速","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 II-14风速","yc_hs_0006","cur_31"]
[1011,"i_平陆一期 II-14机舱中轴线与风向夹角","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 II-14机舱中轴线与风向夹角","yc_hs_0121","cur_92"]
[1012,"i_平陆一期 II-13风向","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 II-13风向","yc_hs_0005","cur_99"]
[1013,"i_平陆一期 II-13风速","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 II-13风速","yc_hs_0005","cur_100"]
[1014,"i_平陆一期 III-20发电机有功功率","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 III-20发电机有功功率","yc_hs_0008","cur_03"]
[1015,"i_平陆一期 III-23发电机有功功率","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 III-23发电机有功功率","yc_hs_0008","cur_96"]
[1016,"i_平陆一期 III-17发电机定子V相线圈温度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 III-17发电机定子V相线圈温度","yc_hs_0123","cur_72"]
[1017,"i_平陆一期 III-17舱内温度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 III-17舱内温度","yc_hs_0007","cur_20"]
[1018,"i_平陆一期 I-01机舱角度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 I-01机舱角度","yc_hs_0002","cur_43"]
[1019,"i_平陆一期 I-01扭缆角度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 I-01扭缆角度","yc_hs_0002","cur_44"]
[1020,"i_平陆一期 II-10齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 II-10齿轮箱高速轴非驱动端轴承温度","yc_hs_0005","cur_15"]
[1021,"i_平陆一期 II-14 3#桨叶片角度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 II-14 3#桨叶片角度","yc_hs_0109","cur_37"]
[1022,"i_平陆一期 I-05主轴转速","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 I-05主轴转速","yc_hs_0003","cur_57"]
[1023,"i_平陆一期 I-02机舱侧向振动(已滤波)","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 I-02机舱侧向振动(已滤波)","yc_hs_0002","cur_72"]
[1024,"i_平陆一期 III-20机舱侧向振动(已滤波)","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 III-20机舱侧向振动(已滤波)","yc_hs_0008","cur_30"]
[1025,"i_平陆一期 I-05风向","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 I-05风向","yc_hs_0003","cur_51"]
[1026,"i_平陆一期 III-18发电机转速","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 III-18发电机转速","yc_hs_0007","cur_43"]
[1027,"i_平陆一期 III-23 3#桨叶片角度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 III-23 3#桨叶片角度","yc_hs_0113","cur_42"]
[1028,"i_平陆一期 I-03机舱侧向振动(已滤波)","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 I-03机舱侧向振动(已滤波)","yc_hs_0003","cur_03"]
[1029,"i_平陆一期 II-16机舱中轴线与风向夹角","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 II-16机舱中轴线与风向夹角","yc_hs_0123","cur_18"]
[1030,"i_平陆一期 II-16 1#桨叶片角度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 II-16 1#桨叶片角度","yc_hs_0110","cur_23"]
[1031,"i_平陆一期 II-16 2#桨叶片角度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 II-16 2#桨叶片角度","yc_hs_0110","cur_25"]
[1032,"i_平陆一期 II-12主轴转速","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 II-12主轴转速","yc_hs_0005","cur_74"]
[1033,"i_平陆一期 II-12齿轮箱高速轴费非驱动端轴承温度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 II-12齿轮箱高速轴费非驱动端轴承温度","yc_hs_0005","cur_77"]
[1034,"i_平陆一期 II-12主轴承外圈温度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 II-12主轴承外圈温度","yc_hs_0005","cur_79"]
[1035,"i_平陆一期 III-18主轴承外圈温度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 III-18主轴承外圈温度","yc_hs_0007","cur_65"]
[1036,"i_平陆一期 III-18机舱侧向振动(已滤波)","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 III-18机舱侧向振动(已滤波)","yc_hs_0007","cur_68"]
[1037,"i_平陆一期 III-18发电机非驱动端轴承温度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 III-18发电机非驱动端轴承温度","yc_hs_0007","cur_45"]
[1038,"i_平陆一期 III-18发电机定子U相线圈温度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 III-18发电机定子U相线圈温度","yc_hs_0007","cur_46"]
[1039,"i_平陆一期 II-11发电机定子W相线圈温度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 II-11发电机定子W相线圈温度","yc_hs_0119","cur_98"]
[1040,"i_平陆一期 I-05扭缆角度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 I-05扭缆角度","yc_hs_0003","cur_68"]
[1041,"i_平陆一期 II-08主轴转速","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 II-08主轴转速","yc_hs_0004","cur_50"]
[1042,"i_平陆一期 II-13发电机有功功率","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 II-13发电机有功功率","yc_hs_0005","cur_86"]
[1043,"i_平陆一期 II-14 2#桨叶片角度","平陆风电场","WOF35900004",14,"YCPL.T1_L2.WTG014.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 II-14 2#桨叶片角度","yc_hs_0109","cur_35"]
[1044,"i_平陆一期 I-05舱内温度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 I-05舱内温度","yc_hs_0003","cur_48"]
[1045,"i_平陆一期 II-09发电机有功功率","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 II-09发电机有功功率","yc_hs_0004","cur_62"]
[1046,"i_平陆一期 II-09发电机转速","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 II-09发电机转速","yc_hs_0004","cur_64"]
[1047,"i_平陆一期 III-22主轴承外圈温度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 III-22主轴承外圈温度","yc_hs_0008","cur_89"]
[1048,"i_平陆一期 II-09机舱侧向振动(已滤波)","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 II-09机舱侧向振动(已滤波)","yc_hs_0004","cur_89"]
[1049,"i_平陆一期 II-09机舱轴向振动(已滤波)","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 II-09机舱轴向振动(已滤波)","yc_hs_0004","cur_90"]
[1050,"i_平陆一期 II-09机舱角度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 II-09机舱角度","yc_hs_0004","cur_91"]
[1051,"i_平陆一期 II-09扭缆角度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 II-09扭缆角度","yc_hs_0004","cur_92"]
[1052,"i_平陆一期 I-02主轴转速","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 I-02主轴转速","yc_hs_0002","cur_64"]
[1053,"i_平陆一期 I-02齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 I-02齿轮箱高速轴非驱动端轴承温度","yc_hs_0002","cur_67"]
[1054,"i_平陆一期 I-02主轴承外圈温度","平陆风电场","WOF35900004",2,"YCPL.T1_L1.WTG002.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 I-02主轴承外圈温度","yc_hs_0002","cur_69"]
[1055,"i_平陆一期 III-17舱外温度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 III-17舱外温度","yc_hs_0007","cur_22"]
[1056,"i_平陆一期 II-16发电机有功功率","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 II-16发电机有功功率","yc_hs_0006","cur_79"]
[1057,"i_平陆一期 II-16发电机转速","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 II-16发电机转速","yc_hs_0006","cur_81"]
[1058,"i_平陆一期 II-16发电机驱动端轴承温度","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 II-16发电机驱动端轴承温度","yc_hs_0006","cur_82"]
[1059,"i_平陆一期 III-18发电机有功功率","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 III-18发电机有功功率","yc_hs_0007","cur_41"]
[1060,"i_平陆一期 III-23机舱侧向振动(已滤波)","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 III-23机舱侧向振动(已滤波)","yc_hs_0009","cur_23"]
[1061,"i_平陆一期 I-07齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 I-07齿轮箱高速轴非驱动端轴承温度","yc_hs_0004","cur_22"]
[1062,"i_平陆一期 I-07主轴承外圈温度","平陆风电场","WOF35900004",7,"YCPL.T1_L1.WTG007.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 I-07主轴承外圈温度","yc_hs_0004","cur_24"]
[1063,"i_平陆一期 II-08齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 II-08齿轮箱高速轴非驱动端轴承温度","yc_hs_0004","cur_53"]
[1064,"i_平陆一期 III-24舱外温度","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 III-24舱外温度","yc_hs_0009","cur_39"]
[1065,"i_平陆一期 III-24风向","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 III-24风向","yc_hs_0009","cur_40"]
[1066,"i_平陆一期 II-16风向","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 II-16风向","yc_hs_0006","cur_92"]
[1067,"i_平陆一期 II-16风速","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 II-16风速","yc_hs_0006","cur_93"]
[1068,"i_平陆一期 III-21齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",21,"YCPL.T1_L3.WTG021.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 III-21齿轮箱高速轴非驱动端轴承温度","yc_hs_0008","cur_56"]
[1069,"i_平陆一期 III-22舱内温度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 III-22舱内温度","yc_hs_0008","cur_75"]
[1070,"i_平陆一期 III-22舱外温度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 III-22舱外温度","yc_hs_0008","cur_77"]
[1071,"i_平陆一期 III-22风向","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 III-22风向","yc_hs_0008","cur_78"]
[1072,"i_平陆一期 III-22风速","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 III-22风速","yc_hs_0008","cur_79"]
[1073,"i_平陆一期 III-22机舱中轴线与风向夹角","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 III-22机舱中轴线与风向夹角","yc_hs_0245","cur_28"]
[1074,"i_平陆一期 III-22 1#桨叶片角度","平陆风电场","WOF35900004",22,"YCPL.T1_L3.WTG022.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 III-22 1#桨叶片角度","yc_hs_0112","cur_93"]
[1075,"i_平陆一期 I-04齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 I-04齿轮箱高速轴非驱动端轴承温度","yc_hs_0003","cur_29"]
[1076,"i_平陆一期 II-13机舱中轴线与风向夹角","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 II-13机舱中轴线与风向夹角","yc_hs_0121","cur_32"]
[1077,"i_平陆一期 II-13 1#桨叶片角度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 II-13 1#桨叶片角度","yc_hs_0108","cur_88"]
[1078,"i_平陆一期 II-13 2#桨叶片角度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 II-13 2#桨叶片角度","yc_hs_0108","cur_90"]
[1079,"i_平陆一期 II-12发电机非驱动端轴承温度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 II-12发电机非驱动端轴承温度","yc_hs_0005","cur_59"]
[1080,"i_平陆一期 II-12发电机定子U相线圈温度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 II-12发电机定子U相线圈温度","yc_hs_0005","cur_60"]
[1081,"i_平陆一期 II-12发电机定子V相线圈温度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 II-12发电机定子V相线圈温度","yc_hs_0120","cur_57"]
[1082,"i_平陆一期 II-12发电机定子W相线圈温度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 II-12发电机定子W相线圈温度","yc_hs_0120","cur_58"]
[1083,"i_平陆一期 II-13发电机转速","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 II-13发电机转速","yc_hs_0005","cur_88"]
[1084,"i_平陆一期 II-13发电机驱动端轴承温度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 II-13发电机驱动端轴承温度","yc_hs_0005","cur_89"]
[1085,"i_平陆一期 III-23发电机定子W相线圈温度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 III-23发电机定子W相线圈温度","yc_hs_0245","cur_62"]
[1086,"i_平陆一期 II-09发电机非驱动端轴承温度","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 II-09发电机非驱动端轴承温度","yc_hs_0004","cur_66"]
[1087,"i_平陆一期 II-08发电机定子U相线圈温度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 II-08发电机定子U相线圈温度","yc_hs_0004","cur_36"]
[1088,"i_平陆一期 II-08发电机定子V相线圈温度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 II-08发电机定子V相线圈温度","yc_hs_0118","cur_11"]
[1089,"i_平陆一期 I-05风速","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 I-05风速","yc_hs_0003","cur_52"]
[1090,"i_平陆一期 I-05机舱中轴线与风向夹角","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 I-05机舱中轴线与风向夹角","yc_hs_0116","cur_27"]
[1091,"i_平陆一期 I-05 1#桨叶片角度","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 I-05 1#桨叶片角度","yc_hs_0105","cur_25"]
[1092,"i_平陆一期 III-24发电机有功功率","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 III-24发电机有功功率","yc_hs_0009","cur_27"]
[1093,"i_平陆一期 III-24发电机转速","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 III-24发电机转速","yc_hs_0009","cur_29"]
[1094,"i_平陆一期 III-17齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 III-17齿轮箱高速轴非驱动端轴承温度","yc_hs_0007","cur_32"]
[1095,"i_平陆一期 III-18主轴转速","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 III-18主轴转速","yc_hs_0007","cur_60"]
[1096,"i_平陆一期 III-18齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆一期 III-18齿轮箱高速轴非驱动端轴承温度","yc_hs_0007","cur_63"]
[1097,"i_平陆一期 III-18机舱轴向振动(已滤波)","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 III-18机舱轴向振动(已滤波)","yc_hs_0007","cur_69"]
[1098,"i_平陆一期 III-18机舱角度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 III-18机舱角度","yc_hs_0007","cur_70"]
[1099,"i_平陆一期 III-18扭缆角度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 III-18扭缆角度","yc_hs_0007","cur_71"]
[1100,"i_平陆一期 III-19舱外温度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 III-19舱外温度","yc_hs_0007","cur_84"]
[1101,"i_平陆一期 II-16主轴转速","平陆风电场","WOF35900004",16,"YCPL.T1_L2.WTG016.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 II-16主轴转速","yc_hs_0006","cur_98"]
[1102,"i_平陆一期 III-20舱外温度","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 III-20舱外温度","yc_hs_0008","cur_15"]
[1103,"i_平陆一期 III-20风向","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 III-20风向","yc_hs_0008","cur_16"]
[1104,"i_平陆一期 II-10发电机驱动端轴承温度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 II-10发电机驱动端轴承温度","yc_hs_0004","cur_96"]
[1105,"i_平陆一期 II-10发电机非驱动端轴承温度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 II-10发电机非驱动端轴承温度","yc_hs_0004","cur_97"]
[1106,"i_平陆一期 III-23舱外温度","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 III-23舱外温度","yc_hs_0009","cur_08"]
[1107,"i_平陆一期 III-23风向","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 III-23风向","yc_hs_0009","cur_09"]
[1108,"i_平陆一期 III-23风速","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 III-23风速","yc_hs_0009","cur_10"]
[1109,"i_平陆一期 II-11发电机有功功率","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 II-11发电机有功功率","yc_hs_0005","cur_24"]
[1110,"i_平陆一期 II-08风速","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 II-08风速","yc_hs_0004","cur_45"]
[1111,"i_平陆一期 II-08机舱中轴线与风向夹角","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 II-08机舱中轴线与风向夹角","yc_hs_0118","cur_18"]
[1112,"i_平陆一期 II-08 1#桨叶片角度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 II-08 1#桨叶片角度","yc_hs_0106","cur_63"]
[1113,"i_平陆一期 II-15舱内温度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 II-15舱内温度","yc_hs_0006","cur_58"]
[1114,"i_平陆一期 III-20风速","平陆风电场","WOF35900004",20,"YCPL.T1_L3.WTG020.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 III-20风速","yc_hs_0008","cur_17"]
[1115,"i_平陆一期 II-12发电机驱动端轴承温度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 II-12发电机驱动端轴承温度","yc_hs_0005","cur_58"]
[1116,"i_平陆一期 III-19风向","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 III-19风向","yc_hs_0007","cur_85"]
[1117,"i_平陆一期 III-19风速","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 III-19风速","yc_hs_0007","cur_86"]
[1118,"i_平陆一期 II-12舱内温度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 II-12舱内温度","yc_hs_0005","cur_65"]
[1119,"i_平陆一期 II-15扭缆角度","平陆风电场","WOF35900004",15,"YCPL.T1_L2.WTG015.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 II-15扭缆角度","yc_hs_0006","cur_78"]
[1120,"i_平陆一期 III-18 1#桨叶片角度","平陆风电场","WOF35900004",18,"YCPL.T1_L3.WTG018.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 III-18 1#桨叶片角度","yc_hs_0111","cur_13"]
[1121,"i_平陆一期 II-10舱内温度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 II-10舱内温度","yc_hs_0005","cur_03"]
[1122,"i_平陆一期 II-10舱外温度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 II-10舱外温度","yc_hs_0005","cur_05"]
[1123,"i_平陆一期 II-09主轴转速","平陆风电场","WOF35900004",9,"YCPL.T1_L2.WTG009.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 II-09主轴转速","yc_hs_0004","cur_81"]
[1124,"i_平陆一期 II-11 2#桨叶片角度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 II-11 2#桨叶片角度","yc_hs_0107","cur_100"]
[1125,"i_平陆一期 II-12舱外温度","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆一期 II-12舱外温度","yc_hs_0005","cur_67"]
[1126,"i_平陆一期 II-12风向","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆一期 II-12风向","yc_hs_0005","cur_68"]
[1127,"i_平陆一期 II-12风速","平陆风电场","WOF35900004",12,"YCPL.T1_L2.WTG012.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 II-12风速","yc_hs_0005","cur_69"]
[1128,"i_平陆一期 II-13舱内温度","平陆风电场","WOF35900004",13,"YCPL.T1_L2.WTG013.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆一期 II-13舱内温度","yc_hs_0005","cur_96"]
[1129,"i_平陆一期 I-01主轴承外圈温度","平陆风电场","WOF35900004",1,"YCPL.T1_L1.WTG001.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 I-01主轴承外圈温度","yc_hs_0002","cur_38"]
[1130,"i_平陆一期 III-17机舱侧向振动(已滤波)","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 III-17机舱侧向振动(已滤波)","yc_hs_0007","cur_37"]
[1131,"i_平陆一期 III-17机舱轴向振动(已滤波)","平陆风电场","WOF35900004",17,"YCPL.T1_L3.WTG017.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 III-17机舱轴向振动(已滤波)","yc_hs_0007","cur_38"]
[1132,"i_平陆一期 III-24主轴转速","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 III-24主轴转速","yc_hs_0009","cur_46"]
[1133,"i_平陆一期 III-24风速","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WNAC.WindSpeed","风速","wind_velocity","i_平陆一期 III-24风速","yc_hs_0009","cur_41"]
[1134,"i_平陆一期 III-24机舱中轴线与风向夹角","平陆风电场","WOF35900004",24,"YCPL.T1_L3.WTG024.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 III-24机舱中轴线与风向夹角","yc_hs_0246","cur_04"]
[1135,"i_平陆一期 I-03发电机定子U相线圈温度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 I-03发电机定子U相线圈温度","yc_hs_0002","cur_81"]
[1136,"i_平陆一期 I-03发电机定子V相线圈温度","平陆风电场","WOF35900004",3,"YCPL.T1_L1.WTG003.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 I-03发电机定子V相线圈温度","yc_hs_0114","cur_92"]
[1137,"i_平陆一期 II-08主轴承外圈温度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆一期 II-08主轴承外圈温度","yc_hs_0004","cur_55"]
[1138,"i_平陆一期 II-08机舱侧向振动(已滤波)","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆一期 II-08机舱侧向振动(已滤波)","yc_hs_0004","cur_58"]
[1139,"i_平陆一期 II-08机舱轴向振动(已滤波)","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆一期 II-08机舱轴向振动(已滤波)","yc_hs_0004","cur_59"]
[1140,"i_平陆一期 II-08机舱角度","平陆风电场","WOF35900004",8,"YCPL.T1_L2.WTG008.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆一期 II-08机舱角度","yc_hs_0004","cur_60"]
[1141,"i_平陆一期 I-05发电机有功功率","平陆风电场","WOF35900004",5,"YCPL.T1_L1.WTG005.WGEN.GenActivePW","有功功率","active_power","i_平陆一期 I-05发电机有功功率","yc_hs_0003","cur_38"]
[1142,"i_平陆一期 I-04发电机定子V相线圈温度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 I-04发电机定子V相线圈温度","yc_hs_0115","cur_52"]
[1143,"i_平陆一期 I-04发电机定子W相线圈温度","平陆风电场","WOF35900004",4,"YCPL.T1_L1.WTG004.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆一期 I-04发电机定子W相线圈温度","yc_hs_0115","cur_53"]
[1144,"i_平陆一期 III-19机舱中轴线与风向夹角","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆一期 III-19机舱中轴线与风向夹角","yc_hs_0125","cur_04"]
[1145,"i_平陆一期 III-19 1#桨叶片角度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆一期 III-19 1#桨叶片角度","yc_hs_0111","cur_58"]
[1146,"i_平陆一期 III-19 2#桨叶片角度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆一期 III-19 2#桨叶片角度","yc_hs_0111","cur_60"]
[1147,"i_平陆一期 III-19 3#桨叶片角度","平陆风电场","WOF35900004",19,"YCPL.T1_L3.WTG019.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆一期 III-19 3#桨叶片角度","yc_hs_0111","cur_62"]
[1148,"i_平陆一期 III-23主轴转速","平陆风电场","WOF35900004",23,"YCPL.T1_L3.WTG023.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆一期 III-23主轴转速","yc_hs_0009","cur_15"]
[1149,"i_平陆一期 II-11发电机转速","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WGEN.GenSpd","发电机转速","generator_speed","i_平陆一期 II-11发电机转速","yc_hs_0005","cur_26"]
[1150,"i_平陆一期 II-11发电机驱动端轴承温度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆一期 II-11发电机驱动端轴承温度","yc_hs_0005","cur_27"]
[1151,"i_平陆一期 II-11发电机非驱动端轴承温度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆一期 II-11发电机非驱动端轴承温度","yc_hs_0005","cur_28"]
[1152,"i_平陆一期 II-11发电机定子U相线圈温度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆一期 II-11发电机定子U相线圈温度","yc_hs_0005","cur_29"]
[1153,"i_平陆一期 II-11发电机定子V相线圈温度","平陆风电场","WOF35900004",11,"YCPL.T1_L2.WTG011.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆一期 II-11发电机定子V相线圈温度","yc_hs_0119","cur_97"]
[1154,"i_平陆一期 II-10扭缆角度","平陆风电场","WOF35900004",10,"YCPL.T1_L2.WTG010.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆一期 II-10扭缆角度","yc_hs_0005","cur_23"]
[1155,"i_平陆二期 V-41发电机有功功率","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 V-41发电机有功功率","yc_hs_0014","cur_38"]
[1156,"i_平陆二期 V-41发电机转速","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 V-41发电机转速","yc_hs_0014","cur_40"]
[1157,"i_平陆二期 V-41发电机驱动端轴承温度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 V-41发电机驱动端轴承温度","yc_hs_0014","cur_41"]
[1158,"i_平陆二期 V-41发电机非驱动端轴承温度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 V-41发电机非驱动端轴承温度","yc_hs_0014","cur_42"]
[1159,"i_平陆二期 V-41发电机定子U相线圈温度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 V-41发电机定子U相线圈温度","yc_hs_0014","cur_43"]
[1160,"i_平陆二期 V-41发电机定子V相线圈温度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 V-41发电机定子V相线圈温度","yc_hs_0252","cur_45"]
[1161,"i_平陆二期 V-41发电机定子W相线圈温度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 V-41发电机定子W相线圈温度","yc_hs_0252","cur_46"]
[1162,"i_平陆二期 V-41舱内温度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 V-41舱内温度","yc_hs_0014","cur_48"]
[1163,"i_平陆二期 V-41舱外温度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 V-41舱外温度","yc_hs_0014","cur_50"]
[1164,"i_平陆二期 V-41风向","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 V-41风向","yc_hs_0121","cur_84"]
[1165,"i_平陆二期 V-41风速","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 V-41风速","yc_hs_0014","cur_51"]
[1166,"i_平陆二期 V-41机舱中轴线与风向夹角","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 V-41机舱中轴线与风向夹角","yc_hs_0252","cur_50"]
[1167,"i_平陆二期 V-41 1#桨叶片角度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 V-41 1#桨叶片角度","yc_hs_0121","cur_85"]
[1168,"i_平陆二期 V-41 2#桨叶片角度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 V-41 2#桨叶片角度","yc_hs_0121","cur_87"]
[1169,"i_平陆二期 V-41 3#桨叶片角度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 V-41 3#桨叶片角度","yc_hs_0121","cur_89"]
[1170,"i_平陆二期 V-48 2#桨叶片角度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 V-48 2#桨叶片角度","yc_hs_0125","cur_09"]
[1171,"i_平陆二期 V-48 3#桨叶片角度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 V-48 3#桨叶片角度","yc_hs_0125","cur_11"]
[1172,"i_平陆二期 V-48主轴转速","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 V-48主轴转速","yc_hs_0016","cur_66"]
[1173,"i_平陆二期 V-48齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 V-48齿轮箱高速轴非驱动端轴承温度","yc_hs_0016","cur_69"]
[1174,"i_平陆二期 V-48主轴承外圈温度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 V-48主轴承外圈温度","yc_hs_0016","cur_71"]
[1175,"i_平陆二期 V-48机舱侧向振动(已滤波)","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 V-48机舱侧向振动(已滤波)","yc_hs_0016","cur_74"]
[1176,"i_平陆二期 IV-27发电机转速","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 IV-27发电机转速","yc_hs_0010","cur_20"]
[1177,"i_平陆二期 IV-27发电机驱动端轴承温度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 IV-27发电机驱动端轴承温度","yc_hs_0010","cur_21"]
[1178,"i_平陆二期 IV-27发电机非驱动端轴承温度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 IV-27发电机非驱动端轴承温度","yc_hs_0010","cur_22"]
[1179,"i_平陆二期 IV-27发电机定子U相线圈温度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 IV-27发电机定子U相线圈温度","yc_hs_0010","cur_23"]
[1180,"i_平陆二期 IV-27发电机定子V相线圈温度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 IV-27发电机定子V相线圈温度","yc_hs_0247","cur_13"]
[1181,"i_平陆二期 IV-27发电机定子W相线圈温度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 IV-27发电机定子W相线圈温度","yc_hs_0247","cur_14"]
[1182,"i_平陆二期 IV-27舱内温度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 IV-27舱内温度","yc_hs_0010","cur_28"]
[1183,"i_平陆二期 IV-27舱外温度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 IV-27舱外温度","yc_hs_0010","cur_30"]
[1184,"i_平陆二期 IV-27风向","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 IV-27风向","yc_hs_0115","cur_40"]
[1185,"i_平陆二期 IV-27风速","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 IV-27风速","yc_hs_0010","cur_31"]
[1186,"i_平陆二期 IV-27机舱中轴线与风向夹角","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 IV-27机舱中轴线与风向夹角","yc_hs_0247","cur_18"]
[1187,"i_平陆二期 IV-27 1#桨叶片角度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 IV-27 1#桨叶片角度","yc_hs_0115","cur_41"]
[1188,"i_平陆二期 IV-27 2#桨叶片角度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 IV-27 2#桨叶片角度","yc_hs_0115","cur_43"]
[1189,"i_平陆二期 IV-27 3#桨叶片角度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 IV-27 3#桨叶片角度","yc_hs_0115","cur_45"]
[1190,"i_平陆二期 IV-34发电机转速","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 IV-34发电机转速","yc_hs_0012","cur_30"]
[1191,"i_平陆二期 IV-34发电机驱动端轴承温度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 IV-34发电机驱动端轴承温度","yc_hs_0012","cur_31"]
[1192,"i_平陆二期 IV-34发电机非驱动端轴承温度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 IV-34发电机非驱动端轴承温度","yc_hs_0012","cur_32"]
[1193,"i_平陆二期 IV-34发电机定子U相线圈温度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 IV-34发电机定子U相线圈温度","yc_hs_0012","cur_33"]
[1194,"i_平陆二期 IV-34发电机定子V相线圈温度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 IV-34发电机定子V相线圈温度","yc_hs_0249","cur_79"]
[1195,"i_平陆二期 IV-34发电机定子W相线圈温度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 IV-34发电机定子W相线圈温度","yc_hs_0249","cur_80"]
[1196,"i_平陆二期 IV-34舱内温度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 IV-34舱内温度","yc_hs_0012","cur_38"]
[1197,"i_平陆二期 IV-34舱外温度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 IV-34舱外温度","yc_hs_0012","cur_40"]
[1198,"i_平陆二期 IV-34风向","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 IV-34风向","yc_hs_0118","cur_62"]
[1199,"i_平陆二期 IV-34风速","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 IV-34风速","yc_hs_0012","cur_41"]
[1200,"i_平陆二期 IV-34机舱中轴线与风向夹角","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 IV-34机舱中轴线与风向夹角","yc_hs_0249","cur_84"]
[1201,"i_平陆二期 IV-34 1#桨叶片角度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 IV-34 1#桨叶片角度","yc_hs_0118","cur_63"]
[1202,"i_平陆二期 IV-34 2#桨叶片角度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 IV-34 2#桨叶片角度","yc_hs_0118","cur_65"]
[1203,"i_平陆二期 IV-34 3#桨叶片角度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 IV-34 3#桨叶片角度","yc_hs_0118","cur_67"]
[1204,"i_平陆二期 V-41主轴转速","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 V-41主轴转速","yc_hs_0014","cur_56"]
[1205,"i_平陆二期 V-41齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 V-41齿轮箱高速轴非驱动端轴承温度","yc_hs_0014","cur_59"]
[1206,"i_平陆二期 V-41主轴承外圈温度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 V-41主轴承外圈温度","yc_hs_0014","cur_61"]
[1207,"i_平陆二期 V-41机舱侧向振动(已滤波)","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 V-41机舱侧向振动(已滤波)","yc_hs_0014","cur_64"]
[1208,"i_平陆二期 V-41机舱轴向振动(已滤波)","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 V-41机舱轴向振动(已滤波)","yc_hs_0014","cur_65"]
[1209,"i_平陆二期 V-41机舱角度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 V-41机舱角度","yc_hs_0014","cur_66"]
[1210,"i_平陆二期 V-41扭缆角度","平陆风电场","WOF35900004",41,"YCPL.T2_L2.WTG041.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 V-41扭缆角度","yc_hs_0014","cur_67"]
[1211,"i_平陆二期 V-48机舱轴向振动(已滤波)","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 V-48机舱轴向振动(已滤波)","yc_hs_0016","cur_75"]
[1212,"i_平陆二期 V-48机舱角度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 V-48机舱角度","yc_hs_0016","cur_76"]
[1213,"i_平陆二期 V-48扭缆角度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 V-48扭缆角度","yc_hs_0016","cur_77"]
[1214,"i_平陆二期 IV-27主轴转速","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 IV-27主轴转速","yc_hs_0010","cur_36"]
[1215,"i_平陆二期 IV-27齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 IV-27齿轮箱高速轴非驱动端轴承温度","yc_hs_0010","cur_39"]
[1216,"i_平陆二期 IV-27主轴承外圈温度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 IV-27主轴承外圈温度","yc_hs_0010","cur_41"]
[1217,"i_平陆二期 IV-27机舱侧向振动(已滤波)","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 IV-27机舱侧向振动(已滤波)","yc_hs_0010","cur_44"]
[1218,"i_平陆二期 IV-27机舱轴向振动(已滤波)","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 IV-27机舱轴向振动(已滤波)","yc_hs_0010","cur_45"]
[1219,"i_平陆二期 IV-27机舱角度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 IV-27机舱角度","yc_hs_0010","cur_46"]
[1220,"i_平陆二期 IV-27扭缆角度","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 IV-27扭缆角度","yc_hs_0010","cur_47"]
[1221,"i_平陆二期 IV-28发电机有功功率","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 IV-28发电机有功功率","yc_hs_0010","cur_48"]
[1222,"i_平陆二期 IV-34主轴转速","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 IV-34主轴转速","yc_hs_0012","cur_46"]
[1223,"i_平陆二期 IV-34齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 IV-34齿轮箱高速轴非驱动端轴承温度","yc_hs_0012","cur_49"]
[1224,"i_平陆二期 IV-34主轴承外圈温度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 IV-34主轴承外圈温度","yc_hs_0012","cur_51"]
[1225,"i_平陆二期 IV-34机舱侧向振动(已滤波)","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 IV-34机舱侧向振动(已滤波)","yc_hs_0012","cur_54"]
[1226,"i_平陆二期 IV-34机舱轴向振动(已滤波)","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 IV-34机舱轴向振动(已滤波)","yc_hs_0012","cur_55"]
[1227,"i_平陆二期 IV-34机舱角度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 IV-34机舱角度","yc_hs_0012","cur_56"]
[1228,"i_平陆二期 IV-34扭缆角度","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 IV-34扭缆角度","yc_hs_0012","cur_57"]
[1229,"i_平陆二期 IV-35发电机有功功率","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 IV-35发电机有功功率","yc_hs_0012","cur_58"]
[1230,"i_平陆二期 V-42发电机有功功率","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 V-42发电机有功功率","yc_hs_0014","cur_68"]
[1231,"i_平陆二期 V-42发电机转速","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 V-42发电机转速","yc_hs_0014","cur_70"]
[1232,"i_平陆二期 V-42发电机驱动端轴承温度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 V-42发电机驱动端轴承温度","yc_hs_0014","cur_71"]
[1233,"i_平陆二期 V-42发电机非驱动端轴承温度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 V-42发电机非驱动端轴承温度","yc_hs_0014","cur_72"]
[1234,"i_平陆二期 V-42发电机定子U相线圈温度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 V-42发电机定子U相线圈温度","yc_hs_0014","cur_73"]
[1235,"i_平陆二期 V-42发电机定子V相线圈温度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 V-42发电机定子V相线圈温度","yc_hs_0252","cur_83"]
[1236,"i_平陆二期 V-42发电机定子W相线圈温度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 V-42发电机定子W相线圈温度","yc_hs_0252","cur_84"]
[1237,"i_平陆二期 V-42舱内温度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 V-42舱内温度","yc_hs_0014","cur_78"]
[1238,"i_平陆二期 V-42舱外温度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 V-42舱外温度","yc_hs_0014","cur_80"]
[1239,"i_平陆二期 V-42风向","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 V-42风向","yc_hs_0122","cur_30"]
[1240,"i_平陆二期 V-42风速","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 V-42风速","yc_hs_0014","cur_81"]
[1241,"i_平陆二期 V-42机舱中轴线与风向夹角","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 V-42机舱中轴线与风向夹角","yc_hs_0252","cur_88"]
[1242,"i_平陆二期 V-42 1#桨叶片角度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 V-42 1#桨叶片角度","yc_hs_0122","cur_31"]
[1243,"i_平陆二期 V-42 2#桨叶片角度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 V-42 2#桨叶片角度","yc_hs_0122","cur_33"]
[1244,"i_平陆二期 V-42 3#桨叶片角度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 V-42 3#桨叶片角度","yc_hs_0122","cur_35"]
[1245,"i_平陆二期 IV-28发电机转速","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 IV-28发电机转速","yc_hs_0010","cur_50"]
[1246,"i_平陆二期 IV-28发电机驱动端轴承温度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 IV-28发电机驱动端轴承温度","yc_hs_0010","cur_51"]
[1247,"i_平陆二期 IV-28发电机非驱动端轴承温度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 IV-28发电机非驱动端轴承温度","yc_hs_0010","cur_52"]
[1248,"i_平陆二期 IV-28发电机定子U相线圈温度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 IV-28发电机定子U相线圈温度","yc_hs_0010","cur_53"]
[1249,"i_平陆二期 IV-28发电机定子V相线圈温度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 IV-28发电机定子V相线圈温度","yc_hs_0247","cur_51"]
[1250,"i_平陆二期 IV-28发电机定子W相线圈温度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 IV-28发电机定子W相线圈温度","yc_hs_0247","cur_52"]
[1251,"i_平陆二期 IV-28舱内温度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 IV-28舱内温度","yc_hs_0010","cur_58"]
[1252,"i_平陆二期 IV-28舱外温度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 IV-28舱外温度","yc_hs_0010","cur_60"]
[1253,"i_平陆二期 IV-28风向","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 IV-28风向","yc_hs_0115","cur_86"]
[1254,"i_平陆二期 IV-28风速","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 IV-28风速","yc_hs_0010","cur_61"]
[1255,"i_平陆二期 IV-28机舱中轴线与风向夹角","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 IV-28机舱中轴线与风向夹角","yc_hs_0247","cur_56"]
[1256,"i_平陆二期 IV-28 1#桨叶片角度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 IV-28 1#桨叶片角度","yc_hs_0115","cur_87"]
[1257,"i_平陆二期 IV-28 2#桨叶片角度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 IV-28 2#桨叶片角度","yc_hs_0115","cur_89"]
[1258,"i_平陆二期 IV-28 3#桨叶片角度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 IV-28 3#桨叶片角度","yc_hs_0115","cur_91"]
[1259,"i_平陆二期 IV-35发电机转速","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 IV-35发电机转速","yc_hs_0012","cur_60"]
[1260,"i_平陆二期 IV-35发电机驱动端轴承温度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 IV-35发电机驱动端轴承温度","yc_hs_0012","cur_61"]
[1261,"i_平陆二期 IV-35发电机非驱动端轴承温度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 IV-35发电机非驱动端轴承温度","yc_hs_0012","cur_62"]
[1262,"i_平陆二期 IV-35发电机定子U相线圈温度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 IV-35发电机定子U相线圈温度","yc_hs_0012","cur_63"]
[1263,"i_平陆二期 IV-35发电机定子V相线圈温度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 IV-35发电机定子V相线圈温度","yc_hs_0250","cur_17"]
[1264,"i_平陆二期 IV-35发电机定子W相线圈温度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 IV-35发电机定子W相线圈温度","yc_hs_0250","cur_18"]
[1265,"i_平陆二期 IV-35舱内温度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 IV-35舱内温度","yc_hs_0012","cur_68"]
[1266,"i_平陆二期 IV-35舱外温度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 IV-35舱外温度","yc_hs_0012","cur_70"]
[1267,"i_平陆二期 IV-35风向","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 IV-35风向","yc_hs_0119","cur_08"]
[1268,"i_平陆二期 IV-35风速","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 IV-35风速","yc_hs_0012","cur_71"]
[1269,"i_平陆二期 IV-35机舱中轴线与风向夹角","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 IV-35机舱中轴线与风向夹角","yc_hs_0250","cur_22"]
[1270,"i_平陆二期 IV-35 1#桨叶片角度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 IV-35 1#桨叶片角度","yc_hs_0119","cur_09"]
[1271,"i_平陆二期 IV-35 2#桨叶片角度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 IV-35 2#桨叶片角度","yc_hs_0119","cur_11"]
[1272,"i_平陆二期 IV-35 3#桨叶片角度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 IV-35 3#桨叶片角度","yc_hs_0119","cur_13"]
[1273,"i_平陆二期 V-42主轴转速","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 V-42主轴转速","yc_hs_0014","cur_86"]
[1274,"i_平陆二期 V-42齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 V-42齿轮箱高速轴非驱动端轴承温度","yc_hs_0014","cur_89"]
[1275,"i_平陆二期 V-42主轴承外圈温度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 V-42主轴承外圈温度","yc_hs_0014","cur_91"]
[1276,"i_平陆二期 V-42机舱侧向振动(已滤波)","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 V-42机舱侧向振动(已滤波)","yc_hs_0014","cur_94"]
[1277,"i_平陆二期 V-42机舱轴向振动(已滤波)","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 V-42机舱轴向振动(已滤波)","yc_hs_0014","cur_95"]
[1278,"i_平陆二期 V-42机舱角度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 V-42机舱角度","yc_hs_0014","cur_96"]
[1279,"i_平陆二期 V-42扭缆角度","平陆风电场","WOF35900004",42,"YCPL.T2_L2.WTG042.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 V-42扭缆角度","yc_hs_0014","cur_97"]
[1280,"i_平陆二期 IV-28主轴转速","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 IV-28主轴转速","yc_hs_0010","cur_66"]
[1281,"i_平陆二期 IV-28齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 IV-28齿轮箱高速轴非驱动端轴承温度","yc_hs_0010","cur_69"]
[1282,"i_平陆二期 IV-28主轴承外圈温度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 IV-28主轴承外圈温度","yc_hs_0010","cur_71"]
[1283,"i_平陆二期 IV-28机舱侧向振动(已滤波)","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 IV-28机舱侧向振动(已滤波)","yc_hs_0010","cur_74"]
[1284,"i_平陆二期 IV-28机舱轴向振动(已滤波)","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 IV-28机舱轴向振动(已滤波)","yc_hs_0010","cur_75"]
[1285,"i_平陆二期 IV-28机舱角度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 IV-28机舱角度","yc_hs_0010","cur_76"]
[1286,"i_平陆二期 IV-28扭缆角度","平陆风电场","WOF35900004",28,"YCPL.T2_L1.WTG028.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 IV-28扭缆角度","yc_hs_0010","cur_77"]
[1287,"i_平陆二期 IV-29发电机有功功率","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 IV-29发电机有功功率","yc_hs_0010","cur_78"]
[1288,"i_平陆二期 IV-35主轴转速","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 IV-35主轴转速","yc_hs_0012","cur_76"]
[1289,"i_平陆二期 IV-35齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 IV-35齿轮箱高速轴非驱动端轴承温度","yc_hs_0012","cur_79"]
[1290,"i_平陆二期 IV-35主轴承外圈温度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 IV-35主轴承外圈温度","yc_hs_0012","cur_81"]
[1291,"i_平陆二期 IV-35机舱侧向振动(已滤波)","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 IV-35机舱侧向振动(已滤波)","yc_hs_0012","cur_84"]
[1292,"i_平陆二期 IV-35机舱轴向振动(已滤波)","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 IV-35机舱轴向振动(已滤波)","yc_hs_0012","cur_85"]
[1293,"i_平陆二期 IV-35机舱角度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 IV-35机舱角度","yc_hs_0012","cur_86"]
[1294,"i_平陆二期 IV-35扭缆角度","平陆风电场","WOF35900004",35,"YCPL.T2_L1.WTG035.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 IV-35扭缆角度","yc_hs_0012","cur_87"]
[1295,"i_平陆二期 V-43发电机有功功率","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 V-43发电机有功功率","yc_hs_0014","cur_98"]
[1296,"i_平陆二期 V-43发电机转速","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 V-43发电机转速","yc_hs_0014","cur_100"]
[1297,"i_平陆二期 V-43发电机驱动端轴承温度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 V-43发电机驱动端轴承温度","yc_hs_0015","cur_01"]
[1298,"i_平陆二期 V-43发电机非驱动端轴承温度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 V-43发电机非驱动端轴承温度","yc_hs_0015","cur_02"]
[1299,"i_平陆二期 V-43发电机定子U相线圈温度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 V-43发电机定子U相线圈温度","yc_hs_0015","cur_03"]
[1300,"i_平陆二期 V-43发电机定子V相线圈温度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 V-43发电机定子V相线圈温度","yc_hs_0253","cur_21"]
[1301,"i_平陆二期 V-43发电机定子W相线圈温度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 V-43发电机定子W相线圈温度","yc_hs_0253","cur_22"]
[1302,"i_平陆二期 V-43舱内温度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 V-43舱内温度","yc_hs_0015","cur_08"]
[1303,"i_平陆二期 V-43舱外温度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 V-43舱外温度","yc_hs_0015","cur_10"]
[1304,"i_平陆二期 V-43风向","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 V-43风向","yc_hs_0122","cur_76"]
[1305,"i_平陆二期 V-43风速","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 V-43风速","yc_hs_0015","cur_11"]
[1306,"i_平陆二期 V-43机舱中轴线与风向夹角","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 V-43机舱中轴线与风向夹角","yc_hs_0253","cur_26"]
[1307,"i_平陆二期 V-43 1#桨叶片角度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 V-43 1#桨叶片角度","yc_hs_0122","cur_77"]
[1308,"i_平陆二期 V-43 2#桨叶片角度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 V-43 2#桨叶片角度","yc_hs_0122","cur_79"]
[1309,"i_平陆二期 V-43 3#桨叶片角度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 V-43 3#桨叶片角度","yc_hs_0122","cur_81"]
[1310,"i_平陆二期 IV-29发电机转速","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 IV-29发电机转速","yc_hs_0010","cur_80"]
[1311,"i_平陆二期 IV-29发电机驱动端轴承温度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 IV-29发电机驱动端轴承温度","yc_hs_0010","cur_81"]
[1312,"i_平陆二期 IV-29发电机非驱动端轴承温度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 IV-29发电机非驱动端轴承温度","yc_hs_0010","cur_82"]
[1313,"i_平陆二期 IV-29发电机定子U相线圈温度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 IV-29发电机定子U相线圈温度","yc_hs_0010","cur_83"]
[1314,"i_平陆二期 IV-29发电机定子V相线圈温度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 IV-29发电机定子V相线圈温度","yc_hs_0247","cur_89"]
[1315,"i_平陆二期 IV-29发电机定子W相线圈温度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 IV-29发电机定子W相线圈温度","yc_hs_0247","cur_90"]
[1316,"i_平陆二期 IV-29舱内温度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 IV-29舱内温度","yc_hs_0010","cur_88"]
[1317,"i_平陆二期 IV-29舱外温度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 IV-29舱外温度","yc_hs_0010","cur_90"]
[1318,"i_平陆二期 IV-29风向","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 IV-29风向","yc_hs_0116","cur_32"]
[1319,"i_平陆二期 IV-29风速","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 IV-29风速","yc_hs_0010","cur_91"]
[1320,"i_平陆二期 IV-29机舱中轴线与风向夹角","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 IV-29机舱中轴线与风向夹角","yc_hs_0247","cur_94"]
[1321,"i_平陆二期 IV-29 1#桨叶片角度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 IV-29 1#桨叶片角度","yc_hs_0116","cur_33"]
[1322,"i_平陆二期 IV-29 2#桨叶片角度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 IV-29 2#桨叶片角度","yc_hs_0116","cur_35"]
[1323,"i_平陆二期 IV-29 3#桨叶片角度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 IV-29 3#桨叶片角度","yc_hs_0116","cur_37"]
[1324,"i_平陆二期 IV-36发电机有功功率","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 IV-36发电机有功功率","yc_hs_0012","cur_88"]
[1325,"i_平陆二期 IV-36发电机转速","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 IV-36发电机转速","yc_hs_0012","cur_90"]
[1326,"i_平陆二期 IV-36发电机驱动端轴承温度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 IV-36发电机驱动端轴承温度","yc_hs_0012","cur_91"]
[1327,"i_平陆二期 IV-36发电机非驱动端轴承温度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 IV-36发电机非驱动端轴承温度","yc_hs_0012","cur_92"]
[1328,"i_平陆二期 IV-36发电机定子U相线圈温度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 IV-36发电机定子U相线圈温度","yc_hs_0012","cur_93"]
[1329,"i_平陆二期 IV-36发电机定子V相线圈温度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 IV-36发电机定子V相线圈温度","yc_hs_0250","cur_55"]
[1330,"i_平陆二期 IV-36发电机定子W相线圈温度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 IV-36发电机定子W相线圈温度","yc_hs_0250","cur_56"]
[1331,"i_平陆二期 IV-36舱内温度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 IV-36舱内温度","yc_hs_0012","cur_98"]
[1332,"i_平陆二期 IV-36舱外温度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 IV-36舱外温度","yc_hs_0012","cur_100"]
[1333,"i_平陆二期 IV-36风向","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 IV-36风向","yc_hs_0119","cur_54"]
[1334,"i_平陆二期 IV-36风速","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 IV-36风速","yc_hs_0013","cur_01"]
[1335,"i_平陆二期 IV-36机舱中轴线与风向夹角","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 IV-36机舱中轴线与风向夹角","yc_hs_0250","cur_60"]
[1336,"i_平陆二期 IV-36 1#桨叶片角度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 IV-36 1#桨叶片角度","yc_hs_0119","cur_55"]
[1337,"i_平陆二期 IV-36 2#桨叶片角度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 IV-36 2#桨叶片角度","yc_hs_0119","cur_57"]
[1338,"i_平陆二期 IV-36 3#桨叶片角度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 IV-36 3#桨叶片角度","yc_hs_0119","cur_59"]
[1339,"i_平陆二期 V-43主轴转速","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 V-43主轴转速","yc_hs_0015","cur_16"]
[1340,"i_平陆二期 V-43齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 V-43齿轮箱高速轴非驱动端轴承温度","yc_hs_0015","cur_19"]
[1341,"i_平陆二期 V-43主轴承外圈温度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 V-43主轴承外圈温度","yc_hs_0015","cur_21"]
[1342,"i_平陆二期 V-43机舱侧向振动(已滤波)","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 V-43机舱侧向振动(已滤波)","yc_hs_0015","cur_24"]
[1343,"i_平陆二期 V-43机舱轴向振动(已滤波)","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 V-43机舱轴向振动(已滤波)","yc_hs_0015","cur_25"]
[1344,"i_平陆二期 V-43机舱角度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 V-43机舱角度","yc_hs_0015","cur_26"]
[1345,"i_平陆二期 V-43扭缆角度","平陆风电场","WOF35900004",43,"YCPL.T2_L2.WTG043.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 V-43扭缆角度","yc_hs_0015","cur_27"]
[1346,"i_平陆二期 IV-29主轴转速","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 IV-29主轴转速","yc_hs_0010","cur_96"]
[1347,"i_平陆二期 IV-29齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 IV-29齿轮箱高速轴非驱动端轴承温度","yc_hs_0010","cur_99"]
[1348,"i_平陆二期 IV-29主轴承外圈温度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 IV-29主轴承外圈温度","yc_hs_0011","cur_01"]
[1349,"i_平陆二期 IV-29机舱侧向振动(已滤波)","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 IV-29机舱侧向振动(已滤波)","yc_hs_0011","cur_04"]
[1350,"i_平陆二期 IV-29机舱轴向振动(已滤波)","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 IV-29机舱轴向振动(已滤波)","yc_hs_0011","cur_05"]
[1351,"i_平陆二期 IV-29机舱角度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 IV-29机舱角度","yc_hs_0011","cur_06"]
[1352,"i_平陆二期 IV-29扭缆角度","平陆风电场","WOF35900004",29,"YCPL.T2_L1.WTG029.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 IV-29扭缆角度","yc_hs_0011","cur_07"]
[1353,"i_平陆二期 IV-30发电机有功功率","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 IV-30发电机有功功率","yc_hs_0011","cur_08"]
[1354,"i_平陆二期 IV-36主轴转速","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 IV-36主轴转速","yc_hs_0013","cur_06"]
[1355,"i_平陆二期 IV-36齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 IV-36齿轮箱高速轴非驱动端轴承温度","yc_hs_0013","cur_09"]
[1356,"i_平陆二期 IV-36主轴承外圈温度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 IV-36主轴承外圈温度","yc_hs_0013","cur_11"]
[1357,"i_平陆二期 IV-36机舱侧向振动(已滤波)","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 IV-36机舱侧向振动(已滤波)","yc_hs_0013","cur_14"]
[1358,"i_平陆二期 IV-36机舱轴向振动(已滤波)","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 IV-36机舱轴向振动(已滤波)","yc_hs_0013","cur_15"]
[1359,"i_平陆二期 IV-36机舱角度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 IV-36机舱角度","yc_hs_0013","cur_16"]
[1360,"i_平陆二期 IV-36扭缆角度","平陆风电场","WOF35900004",36,"YCPL.T2_L1.WTG036.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 IV-36扭缆角度","yc_hs_0013","cur_17"]
[1361,"i_平陆二期 V-44发电机有功功率","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 V-44发电机有功功率","yc_hs_0015","cur_28"]
[1362,"i_平陆二期 V-44发电机转速","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 V-44发电机转速","yc_hs_0015","cur_30"]
[1363,"i_平陆二期 V-44发电机驱动端轴承温度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 V-44发电机驱动端轴承温度","yc_hs_0015","cur_31"]
[1364,"i_平陆二期 V-44发电机非驱动端轴承温度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 V-44发电机非驱动端轴承温度","yc_hs_0015","cur_32"]
[1365,"i_平陆二期 V-44发电机定子U相线圈温度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 V-44发电机定子U相线圈温度","yc_hs_0015","cur_33"]
[1366,"i_平陆二期 V-44发电机定子V相线圈温度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 V-44发电机定子V相线圈温度","yc_hs_0253","cur_59"]
[1367,"i_平陆二期 V-44发电机定子W相线圈温度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 V-44发电机定子W相线圈温度","yc_hs_0253","cur_60"]
[1368,"i_平陆二期 V-44舱内温度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 V-44舱内温度","yc_hs_0015","cur_38"]
[1369,"i_平陆二期 V-44舱外温度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 V-44舱外温度","yc_hs_0015","cur_40"]
[1370,"i_平陆二期 V-44风向","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 V-44风向","yc_hs_0123","cur_22"]
[1371,"i_平陆二期 V-44风速","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 V-44风速","yc_hs_0015","cur_41"]
[1372,"i_平陆二期 V-44机舱中轴线与风向夹角","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 V-44机舱中轴线与风向夹角","yc_hs_0253","cur_64"]
[1373,"i_平陆二期 V-44 1#桨叶片角度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 V-44 1#桨叶片角度","yc_hs_0123","cur_23"]
[1374,"i_平陆二期 V-44 2#桨叶片角度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 V-44 2#桨叶片角度","yc_hs_0123","cur_25"]
[1375,"i_平陆二期 V-44 3#桨叶片角度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 V-44 3#桨叶片角度","yc_hs_0123","cur_27"]
[1376,"i_平陆二期 IV-30发电机转速","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 IV-30发电机转速","yc_hs_0011","cur_10"]
[1377,"i_平陆二期 IV-30发电机驱动端轴承温度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 IV-30发电机驱动端轴承温度","yc_hs_0011","cur_11"]
[1378,"i_平陆二期 IV-30发电机非驱动端轴承温度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 IV-30发电机非驱动端轴承温度","yc_hs_0011","cur_12"]
[1379,"i_平陆二期 IV-30发电机定子U相线圈温度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 IV-30发电机定子U相线圈温度","yc_hs_0011","cur_13"]
[1380,"i_平陆二期 IV-30发电机定子V相线圈温度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 IV-30发电机定子V相线圈温度","yc_hs_0248","cur_27"]
[1381,"i_平陆二期 IV-30发电机定子W相线圈温度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 IV-30发电机定子W相线圈温度","yc_hs_0248","cur_28"]
[1382,"i_平陆二期 IV-30舱内温度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 IV-30舱内温度","yc_hs_0011","cur_18"]
[1383,"i_平陆二期 IV-30舱外温度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 IV-30舱外温度","yc_hs_0011","cur_20"]
[1384,"i_平陆二期 IV-30风向","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 IV-30风向","yc_hs_0116","cur_78"]
[1385,"i_平陆二期 IV-30风速","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 IV-30风速","yc_hs_0011","cur_21"]
[1386,"i_平陆二期 IV-30机舱中轴线与风向夹角","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 IV-30机舱中轴线与风向夹角","yc_hs_0248","cur_32"]
[1387,"i_平陆二期 IV-30 1#桨叶片角度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 IV-30 1#桨叶片角度","yc_hs_0116","cur_79"]
[1388,"i_平陆二期 IV-30 2#桨叶片角度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 IV-30 2#桨叶片角度","yc_hs_0116","cur_81"]
[1389,"i_平陆二期 IV-30 3#桨叶片角度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 IV-30 3#桨叶片角度","yc_hs_0116","cur_83"]
[1390,"i_平陆二期 V-37发电机有功功率","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 V-37发电机有功功率","yc_hs_0013","cur_18"]
[1391,"i_平陆二期 V-37发电机转速","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 V-37发电机转速","yc_hs_0013","cur_20"]
[1392,"i_平陆二期 V-37发电机驱动端轴承温度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 V-37发电机驱动端轴承温度","yc_hs_0013","cur_21"]
[1393,"i_平陆二期 V-37发电机非驱动端轴承温度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 V-37发电机非驱动端轴承温度","yc_hs_0013","cur_22"]
[1394,"i_平陆二期 V-37发电机定子U相线圈温度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 V-37发电机定子U相线圈温度","yc_hs_0013","cur_23"]
[1395,"i_平陆二期 V-37发电机定子V相线圈温度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 V-37发电机定子V相线圈温度","yc_hs_0250","cur_93"]
[1396,"i_平陆二期 V-37发电机定子W相线圈温度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 V-37发电机定子W相线圈温度","yc_hs_0250","cur_94"]
[1397,"i_平陆二期 V-37舱内温度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 V-37舱内温度","yc_hs_0013","cur_28"]
[1398,"i_平陆二期 V-37舱外温度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 V-37舱外温度","yc_hs_0013","cur_30"]
[1399,"i_平陆二期 V-37风向","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 V-37风向","yc_hs_0119","cur_100"]
[1400,"i_平陆二期 V-37风速","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 V-37风速","yc_hs_0013","cur_31"]
[1401,"i_平陆二期 V-37机舱中轴线与风向夹角","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 V-37机舱中轴线与风向夹角","yc_hs_0250","cur_98"]
[1402,"i_平陆二期 V-37 1#桨叶片角度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 V-37 1#桨叶片角度","yc_hs_0120","cur_01"]
[1403,"i_平陆二期 V-37 2#桨叶片角度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 V-37 2#桨叶片角度","yc_hs_0120","cur_03"]
[1404,"i_平陆二期 V-37 3#桨叶片角度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 V-37 3#桨叶片角度","yc_hs_0120","cur_05"]
[1405,"i_平陆二期 V-44主轴转速","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 V-44主轴转速","yc_hs_0015","cur_46"]
[1406,"i_平陆二期 V-44齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 V-44齿轮箱高速轴非驱动端轴承温度","yc_hs_0015","cur_49"]
[1407,"i_平陆二期 V-44主轴承外圈温度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 V-44主轴承外圈温度","yc_hs_0015","cur_51"]
[1408,"i_平陆二期 V-44机舱侧向振动(已滤波)","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 V-44机舱侧向振动(已滤波)","yc_hs_0015","cur_54"]
[1409,"i_平陆二期 V-44机舱轴向振动(已滤波)","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 V-44机舱轴向振动(已滤波)","yc_hs_0015","cur_55"]
[1410,"i_平陆二期 V-44机舱角度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 V-44机舱角度","yc_hs_0015","cur_56"]
[1411,"i_平陆二期 V-44扭缆角度","平陆风电场","WOF35900004",44,"YCPL.T2_L2.WTG044.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 V-44扭缆角度","yc_hs_0015","cur_57"]
[1412,"i_平陆二期 IV-30主轴转速","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 IV-30主轴转速","yc_hs_0011","cur_26"]
[1413,"i_平陆二期 IV-30齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 IV-30齿轮箱高速轴非驱动端轴承温度","yc_hs_0011","cur_29"]
[1414,"i_平陆二期 IV-30主轴承外圈温度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 IV-30主轴承外圈温度","yc_hs_0011","cur_31"]
[1415,"i_平陆二期 IV-30机舱侧向振动(已滤波)","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 IV-30机舱侧向振动(已滤波)","yc_hs_0011","cur_34"]
[1416,"i_平陆二期 IV-30机舱轴向振动(已滤波)","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 IV-30机舱轴向振动(已滤波)","yc_hs_0011","cur_35"]
[1417,"i_平陆二期 IV-30机舱角度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 IV-30机舱角度","yc_hs_0011","cur_36"]
[1418,"i_平陆二期 IV-30扭缆角度","平陆风电场","WOF35900004",30,"YCPL.T2_L1.WTG030.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 IV-30扭缆角度","yc_hs_0011","cur_37"]
[1419,"i_平陆二期 IV-31发电机有功功率","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 IV-31发电机有功功率","yc_hs_0011","cur_38"]
[1420,"i_平陆二期 V-37主轴转速","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 V-37主轴转速","yc_hs_0013","cur_36"]
[1421,"i_平陆二期 V-37齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 V-37齿轮箱高速轴非驱动端轴承温度","yc_hs_0013","cur_39"]
[1422,"i_平陆二期 V-37主轴承外圈温度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 V-37主轴承外圈温度","yc_hs_0013","cur_41"]
[1423,"i_平陆二期 V-37机舱侧向振动(已滤波)","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 V-37机舱侧向振动(已滤波)","yc_hs_0013","cur_44"]
[1424,"i_平陆二期 V-37机舱轴向振动(已滤波)","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 V-37机舱轴向振动(已滤波)","yc_hs_0013","cur_45"]
[1425,"i_平陆二期 V-37机舱角度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 V-37机舱角度","yc_hs_0013","cur_46"]
[1426,"i_平陆二期 V-37扭缆角度","平陆风电场","WOF35900004",37,"YCPL.T2_L2.WTG037.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 V-37扭缆角度","yc_hs_0013","cur_47"]
[1427,"i_平陆二期 V-45发电机有功功率","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 V-45发电机有功功率","yc_hs_0015","cur_58"]
[1428,"i_平陆二期 V-45发电机转速","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 V-45发电机转速","yc_hs_0015","cur_60"]
[1429,"i_平陆二期 V-45发电机驱动端轴承温度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 V-45发电机驱动端轴承温度","yc_hs_0015","cur_61"]
[1430,"i_平陆二期 V-45发电机非驱动端轴承温度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 V-45发电机非驱动端轴承温度","yc_hs_0015","cur_62"]
[1431,"i_平陆二期 V-45发电机定子U相线圈温度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 V-45发电机定子U相线圈温度","yc_hs_0015","cur_63"]
[1432,"i_平陆二期 V-45发电机定子V相线圈温度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 V-45发电机定子V相线圈温度","yc_hs_0253","cur_97"]
[1433,"i_平陆二期 V-45发电机定子W相线圈温度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 V-45发电机定子W相线圈温度","yc_hs_0253","cur_98"]
[1434,"i_平陆二期 V-45舱内温度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 V-45舱内温度","yc_hs_0015","cur_68"]
[1435,"i_平陆二期 V-45舱外温度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 V-45舱外温度","yc_hs_0015","cur_70"]
[1436,"i_平陆二期 V-45风向","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 V-45风向","yc_hs_0123","cur_68"]
[1437,"i_平陆二期 V-45风速","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 V-45风速","yc_hs_0015","cur_71"]
[1438,"i_平陆二期 V-45机舱中轴线与风向夹角","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 V-45机舱中轴线与风向夹角","yc_hs_0254","cur_02"]
[1439,"i_平陆二期 V-45 1#桨叶片角度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 V-45 1#桨叶片角度","yc_hs_0123","cur_69"]
[1440,"i_平陆二期 V-45 2#桨叶片角度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 V-45 2#桨叶片角度","yc_hs_0123","cur_71"]
[1441,"i_平陆二期 IV-31发电机转速","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 IV-31发电机转速","yc_hs_0011","cur_40"]
[1442,"i_平陆二期 IV-31发电机驱动端轴承温度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 IV-31发电机驱动端轴承温度","yc_hs_0011","cur_41"]
[1443,"i_平陆二期 IV-31发电机非驱动端轴承温度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 IV-31发电机非驱动端轴承温度","yc_hs_0011","cur_42"]
[1444,"i_平陆二期 IV-31发电机定子U相线圈温度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 IV-31发电机定子U相线圈温度","yc_hs_0011","cur_43"]
[1445,"i_平陆二期 IV-31发电机定子V相线圈温度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 IV-31发电机定子V相线圈温度","yc_hs_0248","cur_65"]
[1446,"i_平陆二期 IV-31发电机定子W相线圈温度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 IV-31发电机定子W相线圈温度","yc_hs_0248","cur_66"]
[1447,"i_平陆二期 IV-31舱内温度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 IV-31舱内温度","yc_hs_0011","cur_48"]
[1448,"i_平陆二期 IV-31舱外温度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 IV-31舱外温度","yc_hs_0011","cur_50"]
[1449,"i_平陆二期 IV-31风向","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 IV-31风向","yc_hs_0117","cur_24"]
[1450,"i_平陆二期 IV-31风速","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 IV-31风速","yc_hs_0011","cur_51"]
[1451,"i_平陆二期 IV-31机舱中轴线与风向夹角","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 IV-31机舱中轴线与风向夹角","yc_hs_0248","cur_70"]
[1452,"i_平陆二期 IV-31 1#桨叶片角度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 IV-31 1#桨叶片角度","yc_hs_0117","cur_25"]
[1453,"i_平陆二期 IV-31 2#桨叶片角度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 IV-31 2#桨叶片角度","yc_hs_0117","cur_27"]
[1454,"i_平陆二期 IV-31 3#桨叶片角度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 IV-31 3#桨叶片角度","yc_hs_0117","cur_29"]
[1455,"i_平陆二期 V-38发电机有功功率","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 V-38发电机有功功率","yc_hs_0013","cur_48"]
[1456,"i_平陆二期 V-38发电机转速","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 V-38发电机转速","yc_hs_0013","cur_50"]
[1457,"i_平陆二期 V-38发电机驱动端轴承温度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 V-38发电机驱动端轴承温度","yc_hs_0013","cur_51"]
[1458,"i_平陆二期 V-38发电机非驱动端轴承温度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 V-38发电机非驱动端轴承温度","yc_hs_0013","cur_52"]
[1459,"i_平陆二期 V-38发电机定子U相线圈温度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 V-38发电机定子U相线圈温度","yc_hs_0013","cur_53"]
[1460,"i_平陆二期 V-38发电机定子V相线圈温度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 V-38发电机定子V相线圈温度","yc_hs_0251","cur_31"]
[1461,"i_平陆二期 V-38发电机定子W相线圈温度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 V-38发电机定子W相线圈温度","yc_hs_0251","cur_32"]
[1462,"i_平陆二期 V-38舱内温度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 V-38舱内温度","yc_hs_0013","cur_58"]
[1463,"i_平陆二期 V-38舱外温度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 V-38舱外温度","yc_hs_0013","cur_60"]
[1464,"i_平陆二期 V-38风向","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 V-38风向","yc_hs_0120","cur_46"]
[1465,"i_平陆二期 V-38风速","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 V-38风速","yc_hs_0013","cur_61"]
[1466,"i_平陆二期 V-38机舱中轴线与风向夹角","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 V-38机舱中轴线与风向夹角","yc_hs_0251","cur_36"]
[1467,"i_平陆二期 V-38 1#桨叶片角度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 V-38 1#桨叶片角度","yc_hs_0120","cur_47"]
[1468,"i_平陆二期 V-38 2#桨叶片角度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 V-38 2#桨叶片角度","yc_hs_0120","cur_49"]
[1469,"i_平陆二期 V-38 3#桨叶片角度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 V-38 3#桨叶片角度","yc_hs_0120","cur_51"]
[1470,"i_平陆二期 V-45 3#桨叶片角度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 V-45 3#桨叶片角度","yc_hs_0123","cur_73"]
[1471,"i_平陆二期 V-45主轴转速","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 V-45主轴转速","yc_hs_0015","cur_76"]
[1472,"i_平陆二期 V-45齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 V-45齿轮箱高速轴非驱动端轴承温度","yc_hs_0015","cur_79"]
[1473,"i_平陆二期 V-45主轴承外圈温度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 V-45主轴承外圈温度","yc_hs_0015","cur_81"]
[1474,"i_平陆二期 V-45机舱侧向振动(已滤波)","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 V-45机舱侧向振动(已滤波)","yc_hs_0015","cur_84"]
[1475,"i_平陆二期 V-45机舱轴向振动(已滤波)","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 V-45机舱轴向振动(已滤波)","yc_hs_0015","cur_85"]
[1476,"i_平陆二期 V-45机舱角度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 V-45机舱角度","yc_hs_0015","cur_86"]
[1477,"i_平陆二期 V-45扭缆角度","平陆风电场","WOF35900004",45,"YCPL.T2_L2.WTG045.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 V-45扭缆角度","yc_hs_0015","cur_87"]
[1478,"i_平陆二期 IV-31主轴转速","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 IV-31主轴转速","yc_hs_0011","cur_56"]
[1479,"i_平陆二期 IV-31齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 IV-31齿轮箱高速轴非驱动端轴承温度","yc_hs_0011","cur_59"]
[1480,"i_平陆二期 IV-31主轴承外圈温度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 IV-31主轴承外圈温度","yc_hs_0011","cur_61"]
[1481,"i_平陆二期 IV-31机舱侧向振动(已滤波)","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 IV-31机舱侧向振动(已滤波)","yc_hs_0011","cur_64"]
[1482,"i_平陆二期 IV-31机舱轴向振动(已滤波)","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 IV-31机舱轴向振动(已滤波)","yc_hs_0011","cur_65"]
[1483,"i_平陆二期 IV-31机舱角度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 IV-31机舱角度","yc_hs_0011","cur_66"]
[1484,"i_平陆二期 IV-31扭缆角度","平陆风电场","WOF35900004",31,"YCPL.T2_L1.WTG031.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 IV-31扭缆角度","yc_hs_0011","cur_67"]
[1485,"i_平陆二期 IV-32发电机有功功率","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 IV-32发电机有功功率","yc_hs_0011","cur_68"]
[1486,"i_平陆二期 V-38主轴转速","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 V-38主轴转速","yc_hs_0013","cur_66"]
[1487,"i_平陆二期 V-38齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 V-38齿轮箱高速轴非驱动端轴承温度","yc_hs_0013","cur_69"]
[1488,"i_平陆二期 V-38主轴承外圈温度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 V-38主轴承外圈温度","yc_hs_0013","cur_71"]
[1489,"i_平陆二期 V-38机舱侧向振动(已滤波)","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 V-38机舱侧向振动(已滤波)","yc_hs_0013","cur_74"]
[1490,"i_平陆二期 V-38机舱轴向振动(已滤波)","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 V-38机舱轴向振动(已滤波)","yc_hs_0013","cur_75"]
[1491,"i_平陆二期 V-38机舱角度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 V-38机舱角度","yc_hs_0013","cur_76"]
[1492,"i_平陆二期 V-38扭缆角度","平陆风电场","WOF35900004",38,"YCPL.T2_L2.WTG038.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 V-38扭缆角度","yc_hs_0013","cur_77"]
[1493,"i_平陆二期 V-46发电机有功功率","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 V-46发电机有功功率","yc_hs_0015","cur_88"]
[1494,"i_平陆二期 V-46发电机转速","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 V-46发电机转速","yc_hs_0015","cur_90"]
[1495,"i_平陆二期 V-46发电机驱动端轴承温度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 V-46发电机驱动端轴承温度","yc_hs_0015","cur_91"]
[1496,"i_平陆二期 V-46发电机非驱动端轴承温度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 V-46发电机非驱动端轴承温度","yc_hs_0015","cur_92"]
[1497,"i_平陆二期 V-46发电机定子U相线圈温度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 V-46发电机定子U相线圈温度","yc_hs_0015","cur_93"]
[1498,"i_平陆二期 V-46发电机定子V相线圈温度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 V-46发电机定子V相线圈温度","yc_hs_0254","cur_35"]
[1499,"i_平陆二期 V-46发电机定子W相线圈温度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 V-46发电机定子W相线圈温度","yc_hs_0254","cur_36"]
[1500,"i_平陆二期 V-46舱内温度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 V-46舱内温度","yc_hs_0015","cur_98"]
[1501,"i_平陆二期 V-46舱外温度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 V-46舱外温度","yc_hs_0015","cur_100"]
[1502,"i_平陆二期 V-46风向","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 V-46风向","yc_hs_0124","cur_14"]
[1503,"i_平陆二期 V-46风速","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 V-46风速","yc_hs_0016","cur_01"]
[1504,"i_平陆二期 V-46机舱中轴线与风向夹角","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 V-46机舱中轴线与风向夹角","yc_hs_0254","cur_40"]
[1505,"i_平陆二期 V-46 1#桨叶片角度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 V-46 1#桨叶片角度","yc_hs_0124","cur_15"]
[1506,"i_平陆二期 V-46 2#桨叶片角度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 V-46 2#桨叶片角度","yc_hs_0124","cur_17"]
[1507,"i_平陆二期 IV-25发电机有功功率","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 IV-25发电机有功功率","yc_hs_0009","cur_58"]
[1508,"i_平陆二期 IV-25发电机转速","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 IV-25发电机转速","yc_hs_0009","cur_60"]
[1509,"i_平陆二期 IV-25发电机驱动端轴承温度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 IV-25发电机驱动端轴承温度","yc_hs_0009","cur_61"]
[1510,"i_平陆二期 IV-32发电机转速","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 IV-32发电机转速","yc_hs_0011","cur_70"]
[1511,"i_平陆二期 IV-32发电机驱动端轴承温度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 IV-32发电机驱动端轴承温度","yc_hs_0011","cur_71"]
[1512,"i_平陆二期 IV-32发电机非驱动端轴承温度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 IV-32发电机非驱动端轴承温度","yc_hs_0011","cur_72"]
[1513,"i_平陆二期 IV-32发电机定子U相线圈温度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 IV-32发电机定子U相线圈温度","yc_hs_0011","cur_73"]
[1514,"i_平陆二期 IV-32发电机定子V相线圈温度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 IV-32发电机定子V相线圈温度","yc_hs_0249","cur_03"]
[1515,"i_平陆二期 IV-32发电机定子W相线圈温度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 IV-32发电机定子W相线圈温度","yc_hs_0249","cur_04"]
[1516,"i_平陆二期 IV-32舱内温度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 IV-32舱内温度","yc_hs_0011","cur_78"]
[1517,"i_平陆二期 IV-32舱外温度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 IV-32舱外温度","yc_hs_0011","cur_80"]
[1518,"i_平陆二期 IV-32风向","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 IV-32风向","yc_hs_0117","cur_70"]
[1519,"i_平陆二期 IV-32风速","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 IV-32风速","yc_hs_0011","cur_81"]
[1520,"i_平陆二期 IV-32机舱中轴线与风向夹角","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 IV-32机舱中轴线与风向夹角","yc_hs_0249","cur_08"]
[1521,"i_平陆二期 IV-32 1#桨叶片角度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 IV-32 1#桨叶片角度","yc_hs_0117","cur_71"]
[1522,"i_平陆二期 IV-32 2#桨叶片角度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 IV-32 2#桨叶片角度","yc_hs_0117","cur_73"]
[1523,"i_平陆二期 IV-32 3#桨叶片角度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 IV-32 3#桨叶片角度","yc_hs_0117","cur_75"]
[1524,"i_平陆二期 V-39发电机有功功率","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 V-39发电机有功功率","yc_hs_0013","cur_78"]
[1525,"i_平陆二期 V-39发电机转速","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 V-39发电机转速","yc_hs_0013","cur_80"]
[1526,"i_平陆二期 V-39发电机驱动端轴承温度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 V-39发电机驱动端轴承温度","yc_hs_0013","cur_81"]
[1527,"i_平陆二期 V-39发电机非驱动端轴承温度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 V-39发电机非驱动端轴承温度","yc_hs_0013","cur_82"]
[1528,"i_平陆二期 V-39发电机定子U相线圈温度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 V-39发电机定子U相线圈温度","yc_hs_0013","cur_83"]
[1529,"i_平陆二期 V-39发电机定子V相线圈温度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 V-39发电机定子V相线圈温度","yc_hs_0251","cur_69"]
[1530,"i_平陆二期 V-39发电机定子W相线圈温度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 V-39发电机定子W相线圈温度","yc_hs_0251","cur_70"]
[1531,"i_平陆二期 V-39舱内温度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 V-39舱内温度","yc_hs_0013","cur_88"]
[1532,"i_平陆二期 V-39舱外温度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 V-39舱外温度","yc_hs_0013","cur_90"]
[1533,"i_平陆二期 V-39风向","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 V-39风向","yc_hs_0120","cur_92"]
[1534,"i_平陆二期 V-39风速","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 V-39风速","yc_hs_0013","cur_91"]
[1535,"i_平陆二期 V-39机舱中轴线与风向夹角","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 V-39机舱中轴线与风向夹角","yc_hs_0251","cur_74"]
[1536,"i_平陆二期 V-39 1#桨叶片角度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 V-39 1#桨叶片角度","yc_hs_0120","cur_93"]
[1537,"i_平陆二期 V-39 2#桨叶片角度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 V-39 2#桨叶片角度","yc_hs_0120","cur_95"]
[1538,"i_平陆二期 V-39 3#桨叶片角度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 V-39 3#桨叶片角度","yc_hs_0120","cur_97"]
[1539,"i_平陆二期 V-46 3#桨叶片角度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 V-46 3#桨叶片角度","yc_hs_0124","cur_19"]
[1540,"i_平陆二期 V-46主轴转速","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 V-46主轴转速","yc_hs_0016","cur_06"]
[1541,"i_平陆二期 V-46齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 V-46齿轮箱高速轴非驱动端轴承温度","yc_hs_0016","cur_09"]
[1542,"i_平陆二期 V-46主轴承外圈温度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 V-46主轴承外圈温度","yc_hs_0016","cur_11"]
[1543,"i_平陆二期 V-46机舱侧向振动(已滤波)","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 V-46机舱侧向振动(已滤波)","yc_hs_0016","cur_14"]
[1544,"i_平陆二期 V-46机舱轴向振动(已滤波)","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 V-46机舱轴向振动(已滤波)","yc_hs_0016","cur_15"]
[1545,"i_平陆二期 V-46机舱角度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 V-46机舱角度","yc_hs_0016","cur_16"]
[1546,"i_平陆二期 IV-25发电机非驱动端轴承温度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 IV-25发电机非驱动端轴承温度","yc_hs_0009","cur_62"]
[1547,"i_平陆二期 IV-25发电机定子U相线圈温度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 IV-25发电机定子U相线圈温度","yc_hs_0009","cur_63"]
[1548,"i_平陆二期 IV-25发电机定子V相线圈温度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 IV-25发电机定子V相线圈温度","yc_hs_0246","cur_37"]
[1549,"i_平陆二期 IV-25发电机定子W相线圈温度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 IV-25发电机定子W相线圈温度","yc_hs_0246","cur_38"]
[1550,"i_平陆二期 IV-25舱内温度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 IV-25舱内温度","yc_hs_0009","cur_68"]
[1551,"i_平陆二期 IV-25舱外温度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 IV-25舱外温度","yc_hs_0009","cur_70"]
[1552,"i_平陆二期 IV-25风向","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 IV-25风向","yc_hs_0114","cur_48"]
[1553,"i_平陆二期 IV-25风速","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 IV-25风速","yc_hs_0009","cur_71"]
[1554,"i_平陆二期 IV-25机舱中轴线与风向夹角","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 IV-25机舱中轴线与风向夹角","yc_hs_0246","cur_42"]
[1555,"i_平陆二期 IV-25 1#桨叶片角度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 IV-25 1#桨叶片角度","yc_hs_0114","cur_49"]
[1556,"i_平陆二期 IV-25 2#桨叶片角度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 IV-25 2#桨叶片角度","yc_hs_0114","cur_51"]
[1557,"i_平陆二期 IV-25 3#桨叶片角度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 IV-25 3#桨叶片角度","yc_hs_0114","cur_53"]
[1558,"i_平陆二期 IV-32主轴转速","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 IV-32主轴转速","yc_hs_0011","cur_86"]
[1559,"i_平陆二期 IV-32齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 IV-32齿轮箱高速轴非驱动端轴承温度","yc_hs_0011","cur_89"]
[1560,"i_平陆二期 IV-32主轴承外圈温度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 IV-32主轴承外圈温度","yc_hs_0011","cur_91"]
[1561,"i_平陆二期 IV-32机舱侧向振动(已滤波)","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 IV-32机舱侧向振动(已滤波)","yc_hs_0011","cur_94"]
[1562,"i_平陆二期 IV-32机舱轴向振动(已滤波)","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 IV-32机舱轴向振动(已滤波)","yc_hs_0011","cur_95"]
[1563,"i_平陆二期 IV-32机舱角度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 IV-32机舱角度","yc_hs_0011","cur_96"]
[1564,"i_平陆二期 IV-32扭缆角度","平陆风电场","WOF35900004",32,"YCPL.T2_L1.WTG032.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 IV-32扭缆角度","yc_hs_0011","cur_97"]
[1565,"i_平陆二期 IV-33发电机有功功率","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 IV-33发电机有功功率","yc_hs_0011","cur_98"]
[1566,"i_平陆二期 V-39主轴转速","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 V-39主轴转速","yc_hs_0013","cur_96"]
[1567,"i_平陆二期 V-39齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 V-39齿轮箱高速轴非驱动端轴承温度","yc_hs_0013","cur_99"]
[1568,"i_平陆二期 V-39主轴承外圈温度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 V-39主轴承外圈温度","yc_hs_0014","cur_01"]
[1569,"i_平陆二期 V-39机舱侧向振动(已滤波)","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 V-39机舱侧向振动(已滤波)","yc_hs_0014","cur_04"]
[1570,"i_平陆二期 V-39机舱轴向振动(已滤波)","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 V-39机舱轴向振动(已滤波)","yc_hs_0014","cur_05"]
[1571,"i_平陆二期 V-39机舱角度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 V-39机舱角度","yc_hs_0014","cur_06"]
[1572,"i_平陆二期 V-39扭缆角度","平陆风电场","WOF35900004",39,"YCPL.T2_L2.WTG039.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 V-39扭缆角度","yc_hs_0014","cur_07"]
[1573,"i_平陆二期 V-46扭缆角度","平陆风电场","WOF35900004",46,"YCPL.T2_L2.WTG046.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 V-46扭缆角度","yc_hs_0016","cur_17"]
[1574,"i_平陆二期 V-47发电机有功功率","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 V-47发电机有功功率","yc_hs_0016","cur_18"]
[1575,"i_平陆二期 V-47发电机转速","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 V-47发电机转速","yc_hs_0016","cur_20"]
[1576,"i_平陆二期 V-47发电机驱动端轴承温度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 V-47发电机驱动端轴承温度","yc_hs_0016","cur_21"]
[1577,"i_平陆二期 V-47发电机非驱动端轴承温度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 V-47发电机非驱动端轴承温度","yc_hs_0016","cur_22"]
[1578,"i_平陆二期 V-47发电机定子U相线圈温度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 V-47发电机定子U相线圈温度","yc_hs_0016","cur_23"]
[1579,"i_平陆二期 V-47发电机定子V相线圈温度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 V-47发电机定子V相线圈温度","yc_hs_0254","cur_73"]
[1580,"i_平陆二期 V-47发电机定子W相线圈温度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 V-47发电机定子W相线圈温度","yc_hs_0254","cur_74"]
[1581,"i_平陆二期 V-47舱内温度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 V-47舱内温度","yc_hs_0016","cur_28"]
[1582,"i_平陆二期 V-47舱外温度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 V-47舱外温度","yc_hs_0016","cur_30"]
[1583,"i_平陆二期 V-47风向","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 V-47风向","yc_hs_0124","cur_60"]
[1584,"i_平陆二期 V-47风速","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 V-47风速","yc_hs_0016","cur_31"]
[1585,"i_平陆二期 V-47机舱中轴线与风向夹角","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 V-47机舱中轴线与风向夹角","yc_hs_0254","cur_78"]
[1586,"i_平陆二期 V-47 1#桨叶片角度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 V-47 1#桨叶片角度","yc_hs_0124","cur_61"]
[1587,"i_平陆二期 IV-25主轴转速","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 IV-25主轴转速","yc_hs_0009","cur_76"]
[1588,"i_平陆二期 IV-25齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 IV-25齿轮箱高速轴非驱动端轴承温度","yc_hs_0009","cur_79"]
[1589,"i_平陆二期 IV-25主轴承外圈温度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 IV-25主轴承外圈温度","yc_hs_0009","cur_81"]
[1590,"i_平陆二期 IV-25机舱侧向振动(已滤波)","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 IV-25机舱侧向振动(已滤波)","yc_hs_0009","cur_84"]
[1591,"i_平陆二期 IV-25机舱轴向振动(已滤波)","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 IV-25机舱轴向振动(已滤波)","yc_hs_0009","cur_85"]
[1592,"i_平陆二期 IV-25机舱角度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 IV-25机舱角度","yc_hs_0009","cur_86"]
[1593,"i_平陆二期 IV-25扭缆角度","平陆风电场","WOF35900004",25,"YCPL.T2_L1.WTG025.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 IV-25扭缆角度","yc_hs_0009","cur_87"]
[1594,"i_平陆二期 IV-26发电机有功功率","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 IV-26发电机有功功率","yc_hs_0009","cur_88"]
[1595,"i_平陆二期 IV-26发电机转速","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 IV-26发电机转速","yc_hs_0009","cur_90"]
[1596,"i_平陆二期 IV-33发电机转速","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 IV-33发电机转速","yc_hs_0011","cur_100"]
[1597,"i_平陆二期 IV-33发电机驱动端轴承温度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 IV-33发电机驱动端轴承温度","yc_hs_0012","cur_01"]
[1598,"i_平陆二期 IV-33发电机非驱动端轴承温度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 IV-33发电机非驱动端轴承温度","yc_hs_0012","cur_02"]
[1599,"i_平陆二期 IV-33发电机定子U相线圈温度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 IV-33发电机定子U相线圈温度","yc_hs_0012","cur_03"]
[1600,"i_平陆二期 IV-33发电机定子V相线圈温度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 IV-33发电机定子V相线圈温度","yc_hs_0249","cur_41"]
[1601,"i_平陆二期 IV-33发电机定子W相线圈温度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 IV-33发电机定子W相线圈温度","yc_hs_0249","cur_42"]
[1602,"i_平陆二期 IV-33舱内温度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 IV-33舱内温度","yc_hs_0012","cur_08"]
[1603,"i_平陆二期 IV-33舱外温度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 IV-33舱外温度","yc_hs_0012","cur_10"]
[1604,"i_平陆二期 IV-33风向","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 IV-33风向","yc_hs_0118","cur_16"]
[1605,"i_平陆二期 IV-33风速","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 IV-33风速","yc_hs_0012","cur_11"]
[1606,"i_平陆二期 IV-33机舱中轴线与风向夹角","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 IV-33机舱中轴线与风向夹角","yc_hs_0249","cur_46"]
[1607,"i_平陆二期 IV-33 1#桨叶片角度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 IV-33 1#桨叶片角度","yc_hs_0118","cur_17"]
[1608,"i_平陆二期 IV-33 2#桨叶片角度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 IV-33 2#桨叶片角度","yc_hs_0118","cur_19"]
[1609,"i_平陆二期 IV-33 3#桨叶片角度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 IV-33 3#桨叶片角度","yc_hs_0118","cur_21"]
[1610,"i_平陆二期 V-40发电机有功功率","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 V-40发电机有功功率","yc_hs_0014","cur_08"]
[1611,"i_平陆二期 V-40发电机转速","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 V-40发电机转速","yc_hs_0014","cur_10"]
[1612,"i_平陆二期 V-40发电机驱动端轴承温度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 V-40发电机驱动端轴承温度","yc_hs_0014","cur_11"]
[1613,"i_平陆二期 V-40发电机非驱动端轴承温度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 V-40发电机非驱动端轴承温度","yc_hs_0014","cur_12"]
[1614,"i_平陆二期 V-40发电机定子U相线圈温度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 V-40发电机定子U相线圈温度","yc_hs_0014","cur_13"]
[1615,"i_平陆二期 V-40发电机定子V相线圈温度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 V-40发电机定子V相线圈温度","yc_hs_0252","cur_07"]
[1616,"i_平陆二期 V-40发电机定子W相线圈温度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 V-40发电机定子W相线圈温度","yc_hs_0252","cur_08"]
[1617,"i_平陆二期 V-40舱内温度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 V-40舱内温度","yc_hs_0014","cur_18"]
[1618,"i_平陆二期 V-40舱外温度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 V-40舱外温度","yc_hs_0014","cur_20"]
[1619,"i_平陆二期 V-40风向","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 V-40风向","yc_hs_0121","cur_38"]
[1620,"i_平陆二期 V-40风速","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 V-40风速","yc_hs_0014","cur_21"]
[1621,"i_平陆二期 V-40机舱中轴线与风向夹角","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 V-40机舱中轴线与风向夹角","yc_hs_0252","cur_12"]
[1622,"i_平陆二期 V-40 1#桨叶片角度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 V-40 1#桨叶片角度","yc_hs_0121","cur_39"]
[1623,"i_平陆二期 V-40 2#桨叶片角度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 V-40 2#桨叶片角度","yc_hs_0121","cur_41"]
[1624,"i_平陆二期 V-40 3#桨叶片角度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 V-40 3#桨叶片角度","yc_hs_0121","cur_43"]
[1625,"i_平陆二期 V-47 2#桨叶片角度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 V-47 2#桨叶片角度","yc_hs_0124","cur_63"]
[1626,"i_平陆二期 V-47 3#桨叶片角度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 V-47 3#桨叶片角度","yc_hs_0124","cur_65"]
[1627,"i_平陆二期 V-47主轴转速","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 V-47主轴转速","yc_hs_0016","cur_36"]
[1628,"i_平陆二期 V-47齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 V-47齿轮箱高速轴非驱动端轴承温度","yc_hs_0016","cur_39"]
[1629,"i_平陆二期 V-47主轴承外圈温度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 V-47主轴承外圈温度","yc_hs_0016","cur_41"]
[1630,"i_平陆二期 V-47机舱侧向振动(已滤波)","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 V-47机舱侧向振动(已滤波)","yc_hs_0016","cur_44"]
[1631,"i_平陆二期 V-47机舱轴向振动(已滤波)","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 V-47机舱轴向振动(已滤波)","yc_hs_0016","cur_45"]
[1632,"i_平陆二期 IV-26发电机驱动端轴承温度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 IV-26发电机驱动端轴承温度","yc_hs_0009","cur_91"]
[1633,"i_平陆二期 IV-26发电机非驱动端轴承温度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 IV-26发电机非驱动端轴承温度","yc_hs_0009","cur_92"]
[1634,"i_平陆二期 IV-26发电机定子U相线圈温度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 IV-26发电机定子U相线圈温度","yc_hs_0009","cur_93"]
[1635,"i_平陆二期 IV-26发电机定子V相线圈温度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 IV-26发电机定子V相线圈温度","yc_hs_0246","cur_75"]
[1636,"i_平陆二期 IV-26发电机定子W相线圈温度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 IV-26发电机定子W相线圈温度","yc_hs_0246","cur_76"]
[1637,"i_平陆二期 IV-26舱内温度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 IV-26舱内温度","yc_hs_0009","cur_98"]
[1638,"i_平陆二期 IV-26舱外温度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 IV-26舱外温度","yc_hs_0009","cur_100"]
[1639,"i_平陆二期 IV-26风向","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 IV-26风向","yc_hs_0114","cur_94"]
[1640,"i_平陆二期 IV-26风速","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 IV-26风速","yc_hs_0010","cur_01"]
[1641,"i_平陆二期 IV-26机舱中轴线与风向夹角","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 IV-26机舱中轴线与风向夹角","yc_hs_0246","cur_80"]
[1642,"i_平陆二期 IV-26 1#桨叶片角度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 IV-26 1#桨叶片角度","yc_hs_0114","cur_95"]
[1643,"i_平陆二期 IV-26 2#桨叶片角度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆二期 IV-26 2#桨叶片角度","yc_hs_0114","cur_97"]
[1644,"i_平陆二期 IV-26 3#桨叶片角度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆二期 IV-26 3#桨叶片角度","yc_hs_0114","cur_99"]
[1645,"i_平陆二期 IV-33主轴转速","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 IV-33主轴转速","yc_hs_0012","cur_16"]
[1646,"i_平陆二期 IV-33齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 IV-33齿轮箱高速轴非驱动端轴承温度","yc_hs_0012","cur_19"]
[1647,"i_平陆二期 IV-33主轴承外圈温度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 IV-33主轴承外圈温度","yc_hs_0012","cur_21"]
[1648,"i_平陆二期 IV-33机舱侧向振动(已滤波)","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 IV-33机舱侧向振动(已滤波)","yc_hs_0012","cur_24"]
[1649,"i_平陆二期 IV-33机舱轴向振动(已滤波)","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 IV-33机舱轴向振动(已滤波)","yc_hs_0012","cur_25"]
[1650,"i_平陆二期 IV-33机舱角度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 IV-33机舱角度","yc_hs_0012","cur_26"]
[1651,"i_平陆二期 IV-33扭缆角度","平陆风电场","WOF35900004",33,"YCPL.T2_L1.WTG033.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 IV-33扭缆角度","yc_hs_0012","cur_27"]
[1652,"i_平陆二期 IV-34发电机有功功率","平陆风电场","WOF35900004",34,"YCPL.T2_L1.WTG034.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 IV-34发电机有功功率","yc_hs_0012","cur_28"]
[1653,"i_平陆二期 V-40主轴转速","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 V-40主轴转速","yc_hs_0014","cur_26"]
[1654,"i_平陆二期 V-40齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 V-40齿轮箱高速轴非驱动端轴承温度","yc_hs_0014","cur_29"]
[1655,"i_平陆二期 V-40主轴承外圈温度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 V-40主轴承外圈温度","yc_hs_0014","cur_31"]
[1656,"i_平陆二期 V-40机舱侧向振动(已滤波)","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 V-40机舱侧向振动(已滤波)","yc_hs_0014","cur_34"]
[1657,"i_平陆二期 V-40机舱轴向振动(已滤波)","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 V-40机舱轴向振动(已滤波)","yc_hs_0014","cur_35"]
[1658,"i_平陆二期 V-40机舱角度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 V-40机舱角度","yc_hs_0014","cur_36"]
[1659,"i_平陆二期 V-40扭缆角度","平陆风电场","WOF35900004",40,"YCPL.T2_L2.WTG040.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 V-40扭缆角度","yc_hs_0014","cur_37"]
[1660,"i_平陆二期 V-47机舱角度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 V-47机舱角度","yc_hs_0016","cur_46"]
[1661,"i_平陆二期 V-47扭缆角度","平陆风电场","WOF35900004",47,"YCPL.T2_L2.WTG047.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 V-47扭缆角度","yc_hs_0016","cur_47"]
[1662,"i_平陆二期 V-48发电机有功功率","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 V-48发电机有功功率","yc_hs_0016","cur_48"]
[1663,"i_平陆二期 V-48发电机转速","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WGEN.GenSpd","发电机转速","generator_speed","i_平陆二期 V-48发电机转速","yc_hs_0016","cur_50"]
[1664,"i_平陆二期 V-48发电机驱动端轴承温度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆二期 V-48发电机驱动端轴承温度","yc_hs_0016","cur_51"]
[1665,"i_平陆二期 V-48发电机非驱动端轴承温度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆二期 V-48发电机非驱动端轴承温度","yc_hs_0016","cur_52"]
[1666,"i_平陆二期 V-48发电机定子U相线圈温度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆二期 V-48发电机定子U相线圈温度","yc_hs_0016","cur_53"]
[1667,"i_平陆二期 V-48发电机定子V相线圈温度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆二期 V-48发电机定子V相线圈温度","yc_hs_0255","cur_11"]
[1668,"i_平陆二期 V-48发电机定子W相线圈温度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆二期 V-48发电机定子W相线圈温度","yc_hs_0255","cur_12"]
[1669,"i_平陆二期 V-48舱内温度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆二期 V-48舱内温度","yc_hs_0016","cur_58"]
[1670,"i_平陆二期 V-48舱外温度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆二期 V-48舱外温度","yc_hs_0016","cur_60"]
[1671,"i_平陆二期 V-48风向","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆二期 V-48风向","yc_hs_0125","cur_06"]
[1672,"i_平陆二期 V-48风速","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WNAC.WindSpeed","风速","wind_velocity","i_平陆二期 V-48风速","yc_hs_0016","cur_61"]
[1673,"i_平陆二期 V-48机舱中轴线与风向夹角","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆二期 V-48机舱中轴线与风向夹角","yc_hs_0255","cur_16"]
[1674,"i_平陆二期 V-48 1#桨叶片角度","平陆风电场","WOF35900004",48,"YCPL.T2_L2.WTG048.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆二期 V-48 1#桨叶片角度","yc_hs_0125","cur_07"]
[1675,"i_平陆二期 IV-26主轴转速","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆二期 IV-26主轴转速","yc_hs_0010","cur_06"]
[1676,"i_平陆二期 IV-26齿轮箱高速轴非驱动端轴承温度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆二期 IV-26齿轮箱高速轴非驱动端轴承温度","yc_hs_0010","cur_09"]
[1677,"i_平陆二期 IV-26主轴承外圈温度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆二期 IV-26主轴承外圈温度","yc_hs_0010","cur_11"]
[1678,"i_平陆二期 IV-26机舱侧向振动(已滤波)","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆二期 IV-26机舱侧向振动(已滤波)","yc_hs_0010","cur_14"]
[1679,"i_平陆二期 IV-26机舱轴向振动(已滤波)","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆二期 IV-26机舱轴向振动(已滤波)","yc_hs_0010","cur_15"]
[1680,"i_平陆二期 IV-26机舱角度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆二期 IV-26机舱角度","yc_hs_0010","cur_16"]
[1681,"i_平陆二期 IV-26扭缆角度","平陆风电场","WOF35900004",26,"YCPL.T2_L1.WTG026.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆二期 IV-26扭缆角度","yc_hs_0010","cur_17"]
[1682,"i_平陆二期 IV-27发电机有功功率","平陆风电场","WOF35900004",27,"YCPL.T2_L1.WTG027.WGEN.GenActivePW","有功功率","active_power","i_平陆二期 IV-27发电机有功功率","yc_hs_0010","cur_18"]
[1683,"j_芮城一期Ⅲ-001  1#桨叶片角度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅲ-001  1#桨叶片角度","yc_hs_0041","cur_84"]
[1684,"j_芮城一期Ⅲ-001  2#桨叶片角度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅲ-001  2#桨叶片角度","yc_hs_0041","cur_86"]
[1685,"j_芮城一期Ⅲ-001  3#桨叶片角度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅲ-001  3#桨叶片角度","yc_hs_0041","cur_88"]
[1686,"j_芮城一期Ⅲ-001 舱内温度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅲ-001 舱内温度","yc_hs_0041","cur_77"]
[1687,"j_芮城一期Ⅲ-001 舱外温度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅲ-001 舱外温度","yc_hs_0041","cur_79"]
[1688,"j_芮城一期Ⅲ-001 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅲ-001 齿轮箱高速轴非驱动端轴承温度","yc_hs_0042","cur_09"]
[1689,"j_芮城一期Ⅲ-001 齿轮箱油池温度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅲ-001 齿轮箱油池温度","yc_hs_0042","cur_10"]
[1690,"j_芮城一期Ⅲ-001 发电机定子U相线圈温度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅲ-001 发电机定子U相线圈温度","yc_hs_0041","cur_72"]
[1691,"j_芮城一期Ⅲ-001 发电机定子V相线圈温度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅲ-001 发电机定子V相线圈温度","yc_hs_0042","cur_49"]
[1692,"j_芮城一期Ⅲ-001 发电机定子W相线圈温度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅲ-001 发电机定子W相线圈温度","yc_hs_0042","cur_50"]
[1693,"j_芮城一期Ⅲ-001 发电机非驱动端轴承温度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅲ-001 发电机非驱动端轴承温度","yc_hs_0041","cur_71"]
[1694,"j_芮城一期Ⅲ-001 发电机驱动端轴承温度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅲ-001 发电机驱动端轴承温度","yc_hs_0041","cur_70"]
[1695,"j_芮城一期Ⅲ-001 发电机有功功率","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅲ-001 发电机有功功率","yc_hs_0041","cur_60"]
[1696,"j_芮城一期Ⅲ-001 发电机转速","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅲ-001 发电机转速","yc_hs_0041","cur_69"]
[1697,"j_芮城一期Ⅲ-001 风速","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅲ-001 风速","yc_hs_0041","cur_82"]
[1698,"j_芮城一期Ⅲ-001 风向","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅲ-001 风向","yc_hs_0041","cur_81"]
[1699,"j_芮城一期Ⅲ-001 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅲ-001 机舱侧向振动(已滤波)","yc_hs_0042","cur_18"]
[1700,"j_芮城一期Ⅲ-001 机舱角度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅲ-001 机舱角度","yc_hs_0043","cur_21"]
[1701,"j_芮城一期Ⅲ-001 机舱中轴线与风向夹角","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅲ-001 机舱中轴线与风向夹角","yc_hs_0041","cur_83"]
[1702,"j_芮城一期Ⅲ-001 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅲ-001 机舱轴向振动(已滤波)","yc_hs_0042","cur_20"]
[1703,"j_芮城一期Ⅲ-001 扭缆角度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅲ-001 扭缆角度","yc_hs_0042","cur_22"]
[1704,"j_芮城一期Ⅲ-001 主轴承外圈温度","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅲ-001 主轴承外圈温度","yc_hs_0042","cur_11"]
[1705,"j_芮城一期Ⅲ-001 主轴转速","芮城风电场","WOF35900078",1,"SXRC.T1_L1.WTG001.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅲ-001 主轴转速","yc_hs_0042","cur_06"]
[1706,"j_芮城一期Ⅲ-002  1#桨叶片角度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅲ-002  1#桨叶片角度","yc_hs_0042","cur_58"]
[1707,"j_芮城一期Ⅲ-002  2#桨叶片角度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅲ-002  2#桨叶片角度","yc_hs_0042","cur_60"]
[1708,"j_芮城一期Ⅲ-002  3#桨叶片角度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅲ-002  3#桨叶片角度","yc_hs_0042","cur_62"]
[1709,"j_芮城一期Ⅲ-002 舱内温度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅲ-002 舱内温度","yc_hs_0042","cur_51"]
[1710,"j_芮城一期Ⅲ-002 舱外温度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅲ-002 舱外温度","yc_hs_0042","cur_53"]
[1711,"j_芮城一期Ⅲ-002 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅲ-002 齿轮箱高速轴非驱动端轴承温度","yc_hs_0042","cur_83"]
[1712,"j_芮城一期Ⅲ-002 齿轮箱油池温度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅲ-002 齿轮箱油池温度","yc_hs_0042","cur_84"]
[1713,"j_芮城一期Ⅲ-002 发电机定子U相线圈温度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅲ-002 发电机定子U相线圈温度","yc_hs_0042","cur_46"]
[1714,"j_芮城一期Ⅲ-002 发电机定子V相线圈温度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅲ-002 发电机定子V相线圈温度","yc_hs_0043","cur_23"]
[1715,"j_芮城一期Ⅲ-002 发电机定子W相线圈温度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅲ-002 发电机定子W相线圈温度","yc_hs_0043","cur_24"]
[1716,"j_芮城一期Ⅲ-002 发电机非驱动端轴承温度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅲ-002 发电机非驱动端轴承温度","yc_hs_0042","cur_45"]
[1717,"j_芮城一期Ⅲ-002 发电机驱动端轴承温度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅲ-002 发电机驱动端轴承温度","yc_hs_0042","cur_44"]
[1718,"j_芮城一期Ⅲ-002 发电机有功功率","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅲ-002 发电机有功功率","yc_hs_0042","cur_34"]
[1719,"j_芮城一期Ⅲ-002 发电机转速","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅲ-002 发电机转速","yc_hs_0042","cur_43"]
[1720,"j_芮城一期Ⅲ-002 风速","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅲ-002 风速","yc_hs_0042","cur_56"]
[1721,"j_芮城一期Ⅲ-002 风向","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅲ-002 风向","yc_hs_0042","cur_55"]
[1722,"j_芮城一期Ⅲ-002 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅲ-002 机舱侧向振动(已滤波)","yc_hs_0042","cur_92"]
[1723,"j_芮城一期Ⅲ-002 机舱角度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅲ-002 机舱角度","yc_hs_0043","cur_95"]
[1724,"j_芮城一期Ⅲ-002 机舱中轴线与风向夹角","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅲ-002 机舱中轴线与风向夹角","yc_hs_0042","cur_57"]
[1725,"j_芮城一期Ⅲ-002 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅲ-002 机舱轴向振动(已滤波)","yc_hs_0042","cur_94"]
[1726,"j_芮城一期Ⅲ-002 扭缆角度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅲ-002 扭缆角度","yc_hs_0042","cur_96"]
[1727,"j_芮城一期Ⅲ-002 主轴承外圈温度","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅲ-002 主轴承外圈温度","yc_hs_0042","cur_85"]
[1728,"j_芮城一期Ⅲ-002 主轴转速","芮城风电场","WOF35900078",2,"SXRC.T1_L1.WTG002.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅲ-002 主轴转速","yc_hs_0042","cur_80"]
[1729,"j_芮城一期Ⅲ-003  1#桨叶片角度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅲ-003  1#桨叶片角度","yc_hs_0043","cur_32"]
[1730,"j_芮城一期Ⅲ-003  2#桨叶片角度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅲ-003  2#桨叶片角度","yc_hs_0043","cur_34"]
[1731,"j_芮城一期Ⅲ-003  3#桨叶片角度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅲ-003  3#桨叶片角度","yc_hs_0043","cur_36"]
[1732,"j_芮城一期Ⅲ-003 舱内温度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅲ-003 舱内温度","yc_hs_0043","cur_25"]
[1733,"j_芮城一期Ⅲ-003 舱外温度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅲ-003 舱外温度","yc_hs_0043","cur_27"]
[1734,"j_芮城一期Ⅲ-003 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅲ-003 齿轮箱高速轴非驱动端轴承温度","yc_hs_0043","cur_57"]
[1735,"j_芮城一期Ⅲ-003 齿轮箱油池温度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅲ-003 齿轮箱油池温度","yc_hs_0043","cur_58"]
[1736,"j_芮城一期Ⅲ-003 发电机定子U相线圈温度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅲ-003 发电机定子U相线圈温度","yc_hs_0043","cur_20"]
[1737,"j_芮城一期Ⅲ-003 发电机定子V相线圈温度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅲ-003 发电机定子V相线圈温度","yc_hs_0043","cur_97"]
[1738,"j_芮城一期Ⅲ-003 发电机定子W相线圈温度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅲ-003 发电机定子W相线圈温度","yc_hs_0043","cur_98"]
[1739,"j_芮城一期Ⅲ-003 发电机非驱动端轴承温度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅲ-003 发电机非驱动端轴承温度","yc_hs_0043","cur_19"]
[1740,"j_芮城一期Ⅲ-003 发电机驱动端轴承温度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅲ-003 发电机驱动端轴承温度","yc_hs_0043","cur_18"]
[1741,"j_芮城一期Ⅲ-003 发电机有功功率","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅲ-003 发电机有功功率","yc_hs_0043","cur_08"]
[1742,"j_芮城一期Ⅲ-003 发电机转速","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅲ-003 发电机转速","yc_hs_0043","cur_17"]
[1743,"j_芮城一期Ⅲ-003 风速","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅲ-003 风速","yc_hs_0043","cur_30"]
[1744,"j_芮城一期Ⅲ-003 风向","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅲ-003 风向","yc_hs_0043","cur_29"]
[1745,"j_芮城一期Ⅲ-003 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅲ-003 机舱侧向振动(已滤波)","yc_hs_0043","cur_66"]
[1746,"j_芮城一期Ⅲ-003 机舱角度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅲ-003 机舱角度","yc_hs_0044","cur_69"]
[1747,"j_芮城一期Ⅲ-003 机舱中轴线与风向夹角","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅲ-003 机舱中轴线与风向夹角","yc_hs_0043","cur_31"]
[1748,"j_芮城一期Ⅲ-003 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅲ-003 机舱轴向振动(已滤波)","yc_hs_0043","cur_68"]
[1749,"j_芮城一期Ⅲ-003 扭缆角度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅲ-003 扭缆角度","yc_hs_0043","cur_70"]
[1750,"j_芮城一期Ⅲ-003 主轴承外圈温度","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅲ-003 主轴承外圈温度","yc_hs_0043","cur_59"]
[1751,"j_芮城一期Ⅲ-003 主轴转速","芮城风电场","WOF35900078",3,"SXRC.T1_L1.WTG003.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅲ-003 主轴转速","yc_hs_0043","cur_54"]
[1752,"j_芮城一期Ⅲ-004  1#桨叶片角度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅲ-004  1#桨叶片角度","yc_hs_0044","cur_06"]
[1753,"j_芮城一期Ⅲ-004  2#桨叶片角度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅲ-004  2#桨叶片角度","yc_hs_0044","cur_08"]
[1754,"j_芮城一期Ⅲ-004  3#桨叶片角度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅲ-004  3#桨叶片角度","yc_hs_0044","cur_10"]
[1755,"j_芮城一期Ⅲ-004 舱内温度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅲ-004 舱内温度","yc_hs_0043","cur_99"]
[1756,"j_芮城一期Ⅲ-004 舱外温度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅲ-004 舱外温度","yc_hs_0044","cur_01"]
[1757,"j_芮城一期Ⅲ-004 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅲ-004 齿轮箱高速轴非驱动端轴承温度","yc_hs_0044","cur_31"]
[1758,"j_芮城一期Ⅲ-004 齿轮箱油池温度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅲ-004 齿轮箱油池温度","yc_hs_0044","cur_32"]
[1759,"j_芮城一期Ⅲ-004 发电机定子U相线圈温度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅲ-004 发电机定子U相线圈温度","yc_hs_0043","cur_94"]
[1760,"j_芮城一期Ⅲ-004 发电机定子V相线圈温度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅲ-004 发电机定子V相线圈温度","yc_hs_0044","cur_71"]
[1761,"j_芮城一期Ⅲ-004 发电机定子W相线圈温度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅲ-004 发电机定子W相线圈温度","yc_hs_0044","cur_72"]
[1762,"j_芮城一期Ⅲ-004 发电机非驱动端轴承温度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅲ-004 发电机非驱动端轴承温度","yc_hs_0043","cur_93"]
[1763,"j_芮城一期Ⅲ-004 发电机驱动端轴承温度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅲ-004 发电机驱动端轴承温度","yc_hs_0043","cur_92"]
[1764,"j_芮城一期Ⅲ-004 发电机有功功率","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅲ-004 发电机有功功率","yc_hs_0043","cur_82"]
[1765,"j_芮城一期Ⅲ-004 发电机转速","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅲ-004 发电机转速","yc_hs_0043","cur_91"]
[1766,"j_芮城一期Ⅲ-004 风速","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅲ-004 风速","yc_hs_0044","cur_04"]
[1767,"j_芮城一期Ⅲ-004 风向","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅲ-004 风向","yc_hs_0044","cur_03"]
[1768,"j_芮城一期Ⅲ-004 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅲ-004 机舱侧向振动(已滤波)","yc_hs_0044","cur_40"]
[1769,"j_芮城一期Ⅲ-004 机舱角度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅲ-004 机舱角度","yc_hs_0045","cur_43"]
[1770,"j_芮城一期Ⅲ-004 机舱中轴线与风向夹角","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅲ-004 机舱中轴线与风向夹角","yc_hs_0044","cur_05"]
[1771,"j_芮城一期Ⅲ-004 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅲ-004 机舱轴向振动(已滤波)","yc_hs_0044","cur_42"]
[1772,"j_芮城一期Ⅲ-004 扭缆角度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅲ-004 扭缆角度","yc_hs_0044","cur_44"]
[1773,"j_芮城一期Ⅲ-004 主轴承外圈温度","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅲ-004 主轴承外圈温度","yc_hs_0044","cur_33"]
[1774,"j_芮城一期Ⅲ-004 主轴转速","芮城风电场","WOF35900078",4,"SXRC.T1_L1.WTG004.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅲ-004 主轴转速","yc_hs_0044","cur_28"]
[1775,"j_芮城一期Ⅲ-005  1#桨叶片角度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅲ-005  1#桨叶片角度","yc_hs_0044","cur_80"]
[1776,"j_芮城一期Ⅲ-005  2#桨叶片角度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅲ-005  2#桨叶片角度","yc_hs_0044","cur_82"]
[1777,"j_芮城一期Ⅲ-005  3#桨叶片角度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅲ-005  3#桨叶片角度","yc_hs_0044","cur_84"]
[1778,"j_芮城一期Ⅲ-005 舱内温度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅲ-005 舱内温度","yc_hs_0044","cur_73"]
[1779,"j_芮城一期Ⅲ-005 舱外温度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅲ-005 舱外温度","yc_hs_0044","cur_75"]
[1780,"j_芮城一期Ⅲ-005 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅲ-005 齿轮箱高速轴非驱动端轴承温度","yc_hs_0045","cur_05"]
[1781,"j_芮城一期Ⅲ-005 齿轮箱油池温度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅲ-005 齿轮箱油池温度","yc_hs_0045","cur_06"]
[1782,"j_芮城一期Ⅲ-005 发电机定子U相线圈温度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅲ-005 发电机定子U相线圈温度","yc_hs_0044","cur_68"]
[1783,"j_芮城一期Ⅲ-005 发电机定子V相线圈温度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅲ-005 发电机定子V相线圈温度","yc_hs_0045","cur_45"]
[1784,"j_芮城一期Ⅲ-005 发电机定子W相线圈温度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅲ-005 发电机定子W相线圈温度","yc_hs_0045","cur_46"]
[1785,"j_芮城一期Ⅲ-005 发电机非驱动端轴承温度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅲ-005 发电机非驱动端轴承温度","yc_hs_0044","cur_67"]
[1786,"j_芮城一期Ⅲ-005 发电机驱动端轴承温度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅲ-005 发电机驱动端轴承温度","yc_hs_0044","cur_66"]
[1787,"j_芮城一期Ⅲ-005 发电机有功功率","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅲ-005 发电机有功功率","yc_hs_0044","cur_56"]
[1788,"j_芮城一期Ⅲ-005 发电机转速","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅲ-005 发电机转速","yc_hs_0044","cur_65"]
[1789,"j_芮城一期Ⅲ-005 风速","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅲ-005 风速","yc_hs_0044","cur_78"]
[1790,"j_芮城一期Ⅲ-005 风向","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅲ-005 风向","yc_hs_0044","cur_77"]
[1791,"j_芮城一期Ⅲ-005 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅲ-005 机舱侧向振动(已滤波)","yc_hs_0045","cur_14"]
[1792,"j_芮城一期Ⅲ-005 机舱角度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅲ-005 机舱角度","yc_hs_0046","cur_17"]
[1793,"j_芮城一期Ⅲ-005 机舱中轴线与风向夹角","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅲ-005 机舱中轴线与风向夹角","yc_hs_0044","cur_79"]
[1794,"j_芮城一期Ⅲ-005 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅲ-005 机舱轴向振动(已滤波)","yc_hs_0045","cur_16"]
[1795,"j_芮城一期Ⅲ-005 扭缆角度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅲ-005 扭缆角度","yc_hs_0045","cur_18"]
[1796,"j_芮城一期Ⅲ-005 主轴承外圈温度","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅲ-005 主轴承外圈温度","yc_hs_0045","cur_07"]
[1797,"j_芮城一期Ⅲ-005 主轴转速","芮城风电场","WOF35900078",5,"SXRC.T1_L1.WTG005.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅲ-005 主轴转速","yc_hs_0045","cur_02"]
[1798,"j_芮城一期Ⅲ-006  1#桨叶片角度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅲ-006  1#桨叶片角度","yc_hs_0045","cur_54"]
[1799,"j_芮城一期Ⅲ-006  2#桨叶片角度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅲ-006  2#桨叶片角度","yc_hs_0045","cur_56"]
[1800,"j_芮城一期Ⅲ-006  3#桨叶片角度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅲ-006  3#桨叶片角度","yc_hs_0045","cur_58"]
[1801,"j_芮城一期Ⅲ-006 舱内温度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅲ-006 舱内温度","yc_hs_0045","cur_47"]
[1802,"j_芮城一期Ⅲ-006 舱外温度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅲ-006 舱外温度","yc_hs_0045","cur_49"]
[1803,"j_芮城一期Ⅲ-006 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅲ-006 齿轮箱高速轴非驱动端轴承温度","yc_hs_0045","cur_79"]
[1804,"j_芮城一期Ⅲ-006 齿轮箱油池温度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅲ-006 齿轮箱油池温度","yc_hs_0045","cur_80"]
[1805,"j_芮城一期Ⅲ-006 发电机定子U相线圈温度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅲ-006 发电机定子U相线圈温度","yc_hs_0045","cur_42"]
[1806,"j_芮城一期Ⅲ-006 发电机定子V相线圈温度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅲ-006 发电机定子V相线圈温度","yc_hs_0046","cur_19"]
[1807,"j_芮城一期Ⅲ-006 发电机定子W相线圈温度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅲ-006 发电机定子W相线圈温度","yc_hs_0046","cur_20"]
[1808,"j_芮城一期Ⅲ-006 发电机非驱动端轴承温度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅲ-006 发电机非驱动端轴承温度","yc_hs_0045","cur_41"]
[1809,"j_芮城一期Ⅲ-006 发电机驱动端轴承温度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅲ-006 发电机驱动端轴承温度","yc_hs_0045","cur_40"]
[1810,"j_芮城一期Ⅲ-006 发电机有功功率","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅲ-006 发电机有功功率","yc_hs_0045","cur_30"]
[1811,"j_芮城一期Ⅲ-006 发电机转速","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅲ-006 发电机转速","yc_hs_0045","cur_39"]
[1812,"j_芮城一期Ⅲ-006 风速","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅲ-006 风速","yc_hs_0045","cur_52"]
[1813,"j_芮城一期Ⅲ-006 风向","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅲ-006 风向","yc_hs_0045","cur_51"]
[1814,"j_芮城一期Ⅲ-006 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅲ-006 机舱侧向振动(已滤波)","yc_hs_0045","cur_88"]
[1815,"j_芮城一期Ⅲ-006 机舱角度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅲ-006 机舱角度","yc_hs_0046","cur_91"]
[1816,"j_芮城一期Ⅲ-006 机舱中轴线与风向夹角","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅲ-006 机舱中轴线与风向夹角","yc_hs_0045","cur_53"]
[1817,"j_芮城一期Ⅲ-006 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅲ-006 机舱轴向振动(已滤波)","yc_hs_0045","cur_90"]
[1818,"j_芮城一期Ⅲ-006 扭缆角度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅲ-006 扭缆角度","yc_hs_0045","cur_92"]
[1819,"j_芮城一期Ⅲ-006 主轴承外圈温度","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅲ-006 主轴承外圈温度","yc_hs_0045","cur_81"]
[1820,"j_芮城一期Ⅲ-006 主轴转速","芮城风电场","WOF35900078",6,"SXRC.T1_L1.WTG006.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅲ-006 主轴转速","yc_hs_0045","cur_76"]
[1821,"j_芮城一期Ⅲ-007  1#桨叶片角度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅲ-007  1#桨叶片角度","yc_hs_0046","cur_28"]
[1822,"j_芮城一期Ⅲ-007  2#桨叶片角度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅲ-007  2#桨叶片角度","yc_hs_0046","cur_30"]
[1823,"j_芮城一期Ⅲ-007  3#桨叶片角度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅲ-007  3#桨叶片角度","yc_hs_0046","cur_32"]
[1824,"j_芮城一期Ⅲ-007 舱内温度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅲ-007 舱内温度","yc_hs_0046","cur_21"]
[1825,"j_芮城一期Ⅲ-007 舱外温度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅲ-007 舱外温度","yc_hs_0046","cur_23"]
[1826,"j_芮城一期Ⅲ-007 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅲ-007 齿轮箱高速轴非驱动端轴承温度","yc_hs_0046","cur_53"]
[1827,"j_芮城一期Ⅲ-007 齿轮箱油池温度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅲ-007 齿轮箱油池温度","yc_hs_0046","cur_54"]
[1828,"j_芮城一期Ⅲ-007 发电机定子U相线圈温度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅲ-007 发电机定子U相线圈温度","yc_hs_0046","cur_16"]
[1829,"j_芮城一期Ⅲ-007 发电机定子V相线圈温度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅲ-007 发电机定子V相线圈温度","yc_hs_0046","cur_93"]
[1830,"j_芮城一期Ⅲ-007 发电机定子W相线圈温度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅲ-007 发电机定子W相线圈温度","yc_hs_0046","cur_94"]
[1831,"j_芮城一期Ⅲ-007 发电机非驱动端轴承温度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅲ-007 发电机非驱动端轴承温度","yc_hs_0046","cur_15"]
[1832,"j_芮城一期Ⅲ-007 发电机驱动端轴承温度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅲ-007 发电机驱动端轴承温度","yc_hs_0046","cur_14"]
[1833,"j_芮城一期Ⅲ-007 发电机有功功率","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅲ-007 发电机有功功率","yc_hs_0046","cur_04"]
[1834,"j_芮城一期Ⅲ-007 发电机转速","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅲ-007 发电机转速","yc_hs_0046","cur_13"]
[1835,"j_芮城一期Ⅲ-007 风速","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅲ-007 风速","yc_hs_0046","cur_26"]
[1836,"j_芮城一期Ⅲ-007 风向","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅲ-007 风向","yc_hs_0046","cur_25"]
[1837,"j_芮城一期Ⅲ-007 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅲ-007 机舱侧向振动(已滤波)","yc_hs_0046","cur_62"]
[1838,"j_芮城一期Ⅲ-007 机舱角度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅲ-007 机舱角度","yc_hs_0047","cur_65"]
[1839,"j_芮城一期Ⅲ-007 机舱中轴线与风向夹角","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅲ-007 机舱中轴线与风向夹角","yc_hs_0046","cur_27"]
[1840,"j_芮城一期Ⅲ-007 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅲ-007 机舱轴向振动(已滤波)","yc_hs_0046","cur_64"]
[1841,"j_芮城一期Ⅲ-007 扭缆角度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅲ-007 扭缆角度","yc_hs_0046","cur_66"]
[1842,"j_芮城一期Ⅲ-007 主轴承外圈温度","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅲ-007 主轴承外圈温度","yc_hs_0046","cur_55"]
[1843,"j_芮城一期Ⅲ-007 主轴转速","芮城风电场","WOF35900078",7,"SXRC.T1_L1.WTG007.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅲ-007 主轴转速","yc_hs_0046","cur_50"]
[1844,"j_芮城一期Ⅲ-008  1#桨叶片角度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅲ-008  1#桨叶片角度","yc_hs_0047","cur_02"]
[1845,"j_芮城一期Ⅲ-008  2#桨叶片角度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅲ-008  2#桨叶片角度","yc_hs_0047","cur_04"]
[1846,"j_芮城一期Ⅲ-008  3#桨叶片角度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅲ-008  3#桨叶片角度","yc_hs_0047","cur_06"]
[1847,"j_芮城一期Ⅲ-008 舱内温度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅲ-008 舱内温度","yc_hs_0046","cur_95"]
[1848,"j_芮城一期Ⅲ-008 舱外温度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅲ-008 舱外温度","yc_hs_0046","cur_97"]
[1849,"j_芮城一期Ⅲ-008 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅲ-008 齿轮箱高速轴非驱动端轴承温度","yc_hs_0047","cur_27"]
[1850,"j_芮城一期Ⅲ-008 齿轮箱油池温度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅲ-008 齿轮箱油池温度","yc_hs_0047","cur_28"]
[1851,"j_芮城一期Ⅲ-008 发电机定子U相线圈温度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅲ-008 发电机定子U相线圈温度","yc_hs_0046","cur_90"]
[1852,"j_芮城一期Ⅲ-008 发电机定子V相线圈温度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅲ-008 发电机定子V相线圈温度","yc_hs_0047","cur_67"]
[1853,"j_芮城一期Ⅲ-008 发电机定子W相线圈温度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅲ-008 发电机定子W相线圈温度","yc_hs_0047","cur_68"]
[1854,"j_芮城一期Ⅲ-008 发电机非驱动端轴承温度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅲ-008 发电机非驱动端轴承温度","yc_hs_0046","cur_89"]
[1855,"j_芮城一期Ⅲ-008 发电机驱动端轴承温度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅲ-008 发电机驱动端轴承温度","yc_hs_0046","cur_88"]
[1856,"j_芮城一期Ⅲ-008 发电机有功功率","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅲ-008 发电机有功功率","yc_hs_0046","cur_78"]
[1857,"j_芮城一期Ⅲ-008 发电机转速","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅲ-008 发电机转速","yc_hs_0046","cur_87"]
[1858,"j_芮城一期Ⅲ-008 风速","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅲ-008 风速","yc_hs_0046","cur_100"]
[1859,"j_芮城一期Ⅲ-008 风向","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅲ-008 风向","yc_hs_0046","cur_99"]
[1860,"j_芮城一期Ⅲ-008 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅲ-008 机舱侧向振动(已滤波)","yc_hs_0047","cur_36"]
[1861,"j_芮城一期Ⅲ-008 机舱角度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅲ-008 机舱角度","yc_hs_0048","cur_39"]
[1862,"j_芮城一期Ⅲ-008 机舱中轴线与风向夹角","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅲ-008 机舱中轴线与风向夹角","yc_hs_0047","cur_01"]
[1863,"j_芮城一期Ⅲ-008 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅲ-008 机舱轴向振动(已滤波)","yc_hs_0047","cur_38"]
[1864,"j_芮城一期Ⅲ-008 扭缆角度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅲ-008 扭缆角度","yc_hs_0047","cur_40"]
[1865,"j_芮城一期Ⅲ-008 主轴承外圈温度","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅲ-008 主轴承外圈温度","yc_hs_0047","cur_29"]
[1866,"j_芮城一期Ⅲ-008 主轴转速","芮城风电场","WOF35900078",8,"SXRC.T1_L1.WTG008.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅲ-008 主轴转速","yc_hs_0047","cur_24"]
[1867,"j_芮城一期Ⅲ-010  1#桨叶片角度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅲ-010  1#桨叶片角度","yc_hs_0048","cur_50"]
[1868,"j_芮城一期Ⅲ-010  2#桨叶片角度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅲ-010  2#桨叶片角度","yc_hs_0048","cur_52"]
[1869,"j_芮城一期Ⅲ-010  3#桨叶片角度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅲ-010  3#桨叶片角度","yc_hs_0048","cur_54"]
[1870,"j_芮城一期Ⅲ-010 舱内温度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅲ-010 舱内温度","yc_hs_0048","cur_43"]
[1871,"j_芮城一期Ⅲ-010 舱外温度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅲ-010 舱外温度","yc_hs_0048","cur_45"]
[1872,"j_芮城一期Ⅲ-010 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅲ-010 齿轮箱高速轴非驱动端轴承温度","yc_hs_0048","cur_75"]
[1873,"j_芮城一期Ⅲ-010 齿轮箱油池温度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅲ-010 齿轮箱油池温度","yc_hs_0048","cur_76"]
[1874,"j_芮城一期Ⅲ-010 发电机定子U相线圈温度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅲ-010 发电机定子U相线圈温度","yc_hs_0048","cur_38"]
[1875,"j_芮城一期Ⅲ-010 发电机定子V相线圈温度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅲ-010 发电机定子V相线圈温度","yc_hs_0049","cur_15"]
[1876,"j_芮城一期Ⅲ-010 发电机定子W相线圈温度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅲ-010 发电机定子W相线圈温度","yc_hs_0049","cur_16"]
[1877,"j_芮城一期Ⅲ-010 发电机非驱动端轴承温度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅲ-010 发电机非驱动端轴承温度","yc_hs_0048","cur_37"]
[1878,"j_芮城一期Ⅲ-010 发电机驱动端轴承温度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅲ-010 发电机驱动端轴承温度","yc_hs_0048","cur_36"]
[1879,"j_芮城一期Ⅲ-010 发电机有功功率","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅲ-010 发电机有功功率","yc_hs_0048","cur_26"]
[1880,"j_芮城一期Ⅲ-010 发电机转速","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅲ-010 发电机转速","yc_hs_0048","cur_35"]
[1881,"j_芮城一期Ⅲ-010 风速","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅲ-010 风速","yc_hs_0048","cur_48"]
[1882,"j_芮城一期Ⅲ-010 风向","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅲ-010 风向","yc_hs_0048","cur_47"]
[1883,"j_芮城一期Ⅲ-010 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅲ-010 机舱侧向振动(已滤波)","yc_hs_0048","cur_84"]
[1884,"j_芮城一期Ⅲ-010 机舱角度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅲ-010 机舱角度","yc_hs_0049","cur_87"]
[1885,"j_芮城一期Ⅲ-010 机舱中轴线与风向夹角","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅲ-010 机舱中轴线与风向夹角","yc_hs_0048","cur_49"]
[1886,"j_芮城一期Ⅲ-010 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅲ-010 机舱轴向振动(已滤波)","yc_hs_0048","cur_86"]
[1887,"j_芮城一期Ⅲ-010 扭缆角度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅲ-010 扭缆角度","yc_hs_0048","cur_88"]
[1888,"j_芮城一期Ⅲ-010 主轴承外圈温度","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅲ-010 主轴承外圈温度","yc_hs_0048","cur_77"]
[1889,"j_芮城一期Ⅲ-010 主轴转速","芮城风电场","WOF35900078",10,"SXRC.T1_L1.WTG010.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅲ-010 主轴转速","yc_hs_0048","cur_72"]
[1890,"j_芮城一期Ⅲ-011  1#桨叶片角度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅲ-011  1#桨叶片角度","yc_hs_0049","cur_24"]
[1891,"j_芮城一期Ⅲ-011  2#桨叶片角度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅲ-011  2#桨叶片角度","yc_hs_0049","cur_26"]
[1892,"j_芮城一期Ⅲ-011  3#桨叶片角度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅲ-011  3#桨叶片角度","yc_hs_0049","cur_28"]
[1893,"j_芮城一期Ⅲ-011 舱内温度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅲ-011 舱内温度","yc_hs_0049","cur_17"]
[1894,"j_芮城一期Ⅲ-011 舱外温度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅲ-011 舱外温度","yc_hs_0049","cur_19"]
[1895,"j_芮城一期Ⅲ-011 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅲ-011 齿轮箱高速轴非驱动端轴承温度","yc_hs_0049","cur_49"]
[1896,"j_芮城一期Ⅲ-011 齿轮箱油池温度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅲ-011 齿轮箱油池温度","yc_hs_0049","cur_50"]
[1897,"j_芮城一期Ⅲ-011 发电机定子U相线圈温度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅲ-011 发电机定子U相线圈温度","yc_hs_0049","cur_12"]
[1898,"j_芮城一期Ⅲ-011 发电机定子V相线圈温度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅲ-011 发电机定子V相线圈温度","yc_hs_0049","cur_89"]
[1899,"j_芮城一期Ⅲ-011 发电机定子W相线圈温度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅲ-011 发电机定子W相线圈温度","yc_hs_0049","cur_90"]
[1900,"j_芮城一期Ⅲ-011 发电机非驱动端轴承温度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅲ-011 发电机非驱动端轴承温度","yc_hs_0049","cur_11"]
[1901,"j_芮城一期Ⅲ-011 发电机驱动端轴承温度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅲ-011 发电机驱动端轴承温度","yc_hs_0049","cur_10"]
[1902,"j_芮城一期Ⅲ-011 发电机有功功率","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅲ-011 发电机有功功率","yc_hs_0048","cur_100"]
[1903,"j_芮城一期Ⅲ-011 发电机转速","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅲ-011 发电机转速","yc_hs_0049","cur_09"]
[1904,"j_芮城一期Ⅲ-011 风速","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅲ-011 风速","yc_hs_0049","cur_22"]
[1905,"j_芮城一期Ⅲ-011 风向","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅲ-011 风向","yc_hs_0049","cur_21"]
[1906,"j_芮城一期Ⅲ-011 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅲ-011 机舱侧向振动(已滤波)","yc_hs_0049","cur_58"]
[1907,"j_芮城一期Ⅲ-011 机舱角度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅲ-011 机舱角度","yc_hs_0050","cur_61"]
[1908,"j_芮城一期Ⅲ-011 机舱中轴线与风向夹角","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅲ-011 机舱中轴线与风向夹角","yc_hs_0049","cur_23"]
[1909,"j_芮城一期Ⅲ-011 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅲ-011 机舱轴向振动(已滤波)","yc_hs_0049","cur_60"]
[1910,"j_芮城一期Ⅲ-011 扭缆角度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅲ-011 扭缆角度","yc_hs_0049","cur_62"]
[1911,"j_芮城一期Ⅲ-011 主轴承外圈温度","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅲ-011 主轴承外圈温度","yc_hs_0049","cur_51"]
[1912,"j_芮城一期Ⅲ-011 主轴转速","芮城风电场","WOF35900078",11,"SXRC.T1_L1.WTG011.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅲ-011 主轴转速","yc_hs_0049","cur_46"]
[1913,"j_芮城一期Ⅲ-012  1#桨叶片角度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅲ-012  1#桨叶片角度","yc_hs_0049","cur_98"]
[1914,"j_芮城一期Ⅲ-012  2#桨叶片角度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅲ-012  2#桨叶片角度","yc_hs_0049","cur_100"]
[1915,"j_芮城一期Ⅲ-012  3#桨叶片角度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅲ-012  3#桨叶片角度","yc_hs_0050","cur_02"]
[1916,"j_芮城一期Ⅲ-012 舱内温度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅲ-012 舱内温度","yc_hs_0049","cur_91"]
[1917,"j_芮城一期Ⅲ-012 舱外温度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅲ-012 舱外温度","yc_hs_0049","cur_93"]
[1918,"j_芮城一期Ⅲ-012 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅲ-012 齿轮箱高速轴非驱动端轴承温度","yc_hs_0050","cur_23"]
[1919,"j_芮城一期Ⅲ-012 齿轮箱油池温度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅲ-012 齿轮箱油池温度","yc_hs_0050","cur_24"]
[1920,"j_芮城一期Ⅲ-012 发电机定子U相线圈温度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅲ-012 发电机定子U相线圈温度","yc_hs_0049","cur_86"]
[1921,"j_芮城一期Ⅲ-012 发电机定子V相线圈温度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅲ-012 发电机定子V相线圈温度","yc_hs_0050","cur_63"]
[1922,"j_芮城一期Ⅲ-012 发电机定子W相线圈温度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅲ-012 发电机定子W相线圈温度","yc_hs_0050","cur_64"]
[1923,"j_芮城一期Ⅲ-012 发电机非驱动端轴承温度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅲ-012 发电机非驱动端轴承温度","yc_hs_0049","cur_85"]
[1924,"j_芮城一期Ⅲ-012 发电机驱动端轴承温度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅲ-012 发电机驱动端轴承温度","yc_hs_0049","cur_84"]
[1925,"j_芮城一期Ⅲ-012 发电机有功功率","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅲ-012 发电机有功功率","yc_hs_0049","cur_74"]
[1926,"j_芮城一期Ⅲ-012 发电机转速","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅲ-012 发电机转速","yc_hs_0049","cur_83"]
[1927,"j_芮城一期Ⅲ-012 风速","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅲ-012 风速","yc_hs_0049","cur_96"]
[1928,"j_芮城一期Ⅲ-012 风向","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅲ-012 风向","yc_hs_0049","cur_95"]
[1929,"j_芮城一期Ⅲ-012 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅲ-012 机舱侧向振动(已滤波)","yc_hs_0050","cur_32"]
[1930,"j_芮城一期Ⅲ-012 机舱角度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅲ-012 机舱角度","yc_hs_0051","cur_35"]
[1931,"j_芮城一期Ⅲ-012 机舱中轴线与风向夹角","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅲ-012 机舱中轴线与风向夹角","yc_hs_0049","cur_97"]
[1932,"j_芮城一期Ⅲ-012 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅲ-012 机舱轴向振动(已滤波)","yc_hs_0050","cur_34"]
[1933,"j_芮城一期Ⅲ-012 扭缆角度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅲ-012 扭缆角度","yc_hs_0050","cur_36"]
[1934,"j_芮城一期Ⅲ-012 主轴承外圈温度","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅲ-012 主轴承外圈温度","yc_hs_0050","cur_25"]
[1935,"j_芮城一期Ⅲ-012 主轴转速","芮城风电场","WOF35900078",12,"SXRC.T1_L1.WTG012.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅲ-012 主轴转速","yc_hs_0050","cur_20"]
[1936,"j_芮城一期Ⅱ-013  1#桨叶片角度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-013  1#桨叶片角度","yc_hs_0050","cur_72"]
[1937,"j_芮城一期Ⅱ-013  2#桨叶片角度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-013  2#桨叶片角度","yc_hs_0050","cur_74"]
[1938,"j_芮城一期Ⅱ-013  3#桨叶片角度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-013  3#桨叶片角度","yc_hs_0050","cur_76"]
[1939,"j_芮城一期Ⅱ-013 舱内温度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-013 舱内温度","yc_hs_0050","cur_65"]
[1940,"j_芮城一期Ⅱ-013 舱外温度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-013 舱外温度","yc_hs_0050","cur_67"]
[1941,"j_芮城一期Ⅱ-013 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-013 齿轮箱高速轴非驱动端轴承温度","yc_hs_0050","cur_97"]
[1942,"j_芮城一期Ⅱ-013 齿轮箱油池温度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-013 齿轮箱油池温度","yc_hs_0050","cur_98"]
[1943,"j_芮城一期Ⅱ-013 发电机定子U相线圈温度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-013 发电机定子U相线圈温度","yc_hs_0050","cur_60"]
[1944,"j_芮城一期Ⅱ-013 发电机定子V相线圈温度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-013 发电机定子V相线圈温度","yc_hs_0051","cur_37"]
[1945,"j_芮城一期Ⅱ-013 发电机定子W相线圈温度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-013 发电机定子W相线圈温度","yc_hs_0051","cur_38"]
[1946,"j_芮城一期Ⅱ-013 发电机非驱动端轴承温度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-013 发电机非驱动端轴承温度","yc_hs_0050","cur_59"]
[1947,"j_芮城一期Ⅱ-013 发电机驱动端轴承温度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-013 发电机驱动端轴承温度","yc_hs_0050","cur_58"]
[1948,"j_芮城一期Ⅱ-013 发电机有功功率","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-013 发电机有功功率","yc_hs_0050","cur_48"]
[1949,"j_芮城一期Ⅱ-013 发电机转速","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-013 发电机转速","yc_hs_0050","cur_57"]
[1950,"j_芮城一期Ⅱ-013 风速","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-013 风速","yc_hs_0050","cur_70"]
[1951,"j_芮城一期Ⅱ-013 风向","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-013 风向","yc_hs_0050","cur_69"]
[1952,"j_芮城一期Ⅱ-013 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-013 机舱侧向振动(已滤波)","yc_hs_0051","cur_06"]
[1953,"j_芮城一期Ⅱ-013 机舱角度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-013 机舱角度","yc_hs_0052","cur_09"]
[1954,"j_芮城一期Ⅱ-013 机舱中轴线与风向夹角","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-013 机舱中轴线与风向夹角","yc_hs_0050","cur_71"]
[1955,"j_芮城一期Ⅱ-013 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-013 机舱轴向振动(已滤波)","yc_hs_0051","cur_08"]
[1956,"j_芮城一期Ⅱ-013 扭缆角度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-013 扭缆角度","yc_hs_0051","cur_10"]
[1957,"j_芮城一期Ⅱ-013 主轴承外圈温度","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-013 主轴承外圈温度","yc_hs_0050","cur_99"]
[1958,"j_芮城一期Ⅱ-013 主轴转速","芮城风电场","WOF35900078",13,"SXRC.T1_L2.WTG013.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-013 主轴转速","yc_hs_0050","cur_94"]
[1959,"j_芮城一期Ⅱ-014  1#桨叶片角度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-014  1#桨叶片角度","yc_hs_0051","cur_46"]
[1960,"j_芮城一期Ⅱ-014  2#桨叶片角度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-014  2#桨叶片角度","yc_hs_0051","cur_48"]
[1961,"j_芮城一期Ⅱ-014  3#桨叶片角度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-014  3#桨叶片角度","yc_hs_0051","cur_50"]
[1962,"j_芮城一期Ⅱ-014 舱内温度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-014 舱内温度","yc_hs_0051","cur_39"]
[1963,"j_芮城一期Ⅱ-014 舱外温度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-014 舱外温度","yc_hs_0051","cur_41"]
[1964,"j_芮城一期Ⅱ-014 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-014 齿轮箱高速轴非驱动端轴承温度","yc_hs_0051","cur_71"]
[1965,"j_芮城一期Ⅱ-014 齿轮箱油池温度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-014 齿轮箱油池温度","yc_hs_0051","cur_72"]
[1966,"j_芮城一期Ⅱ-014 发电机定子U相线圈温度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-014 发电机定子U相线圈温度","yc_hs_0051","cur_34"]
[1967,"j_芮城一期Ⅱ-014 发电机定子V相线圈温度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-014 发电机定子V相线圈温度","yc_hs_0052","cur_11"]
[1968,"j_芮城一期Ⅱ-014 发电机定子W相线圈温度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-014 发电机定子W相线圈温度","yc_hs_0052","cur_12"]
[1969,"j_芮城一期Ⅱ-014 发电机非驱动端轴承温度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-014 发电机非驱动端轴承温度","yc_hs_0051","cur_33"]
[1970,"j_芮城一期Ⅱ-014 发电机驱动端轴承温度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-014 发电机驱动端轴承温度","yc_hs_0051","cur_32"]
[1971,"j_芮城一期Ⅱ-014 发电机有功功率","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-014 发电机有功功率","yc_hs_0051","cur_22"]
[1972,"j_芮城一期Ⅱ-014 发电机转速","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-014 发电机转速","yc_hs_0051","cur_31"]
[1973,"j_芮城一期Ⅱ-014 风速","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-014 风速","yc_hs_0051","cur_44"]
[1974,"j_芮城一期Ⅱ-014 风向","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-014 风向","yc_hs_0051","cur_43"]
[1975,"j_芮城一期Ⅱ-014 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-014 机舱侧向振动(已滤波)","yc_hs_0051","cur_80"]
[1976,"j_芮城一期Ⅱ-014 机舱角度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-014 机舱角度","yc_hs_0052","cur_83"]
[1977,"j_芮城一期Ⅱ-014 机舱中轴线与风向夹角","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-014 机舱中轴线与风向夹角","yc_hs_0051","cur_45"]
[1978,"j_芮城一期Ⅱ-014 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-014 机舱轴向振动(已滤波)","yc_hs_0051","cur_82"]
[1979,"j_芮城一期Ⅱ-014 扭缆角度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-014 扭缆角度","yc_hs_0051","cur_84"]
[1980,"j_芮城一期Ⅱ-014 主轴承外圈温度","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-014 主轴承外圈温度","yc_hs_0051","cur_73"]
[1981,"j_芮城一期Ⅱ-014 主轴转速","芮城风电场","WOF35900078",14,"SXRC.T1_L2.WTG014.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-014 主轴转速","yc_hs_0051","cur_68"]
[1982,"j_芮城一期Ⅱ-015  1#桨叶片角度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-015  1#桨叶片角度","yc_hs_0052","cur_20"]
[1983,"j_芮城一期Ⅱ-015  2#桨叶片角度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-015  2#桨叶片角度","yc_hs_0052","cur_22"]
[1984,"j_芮城一期Ⅱ-015  3#桨叶片角度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-015  3#桨叶片角度","yc_hs_0052","cur_24"]
[1985,"j_芮城一期Ⅱ-015 舱内温度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-015 舱内温度","yc_hs_0052","cur_13"]
[1986,"j_芮城一期Ⅱ-015 舱外温度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-015 舱外温度","yc_hs_0052","cur_15"]
[1987,"j_芮城一期Ⅱ-015 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-015 齿轮箱高速轴非驱动端轴承温度","yc_hs_0052","cur_45"]
[1988,"j_芮城一期Ⅱ-015 齿轮箱油池温度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-015 齿轮箱油池温度","yc_hs_0052","cur_46"]
[1989,"j_芮城一期Ⅱ-015 发电机定子U相线圈温度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-015 发电机定子U相线圈温度","yc_hs_0052","cur_08"]
[1990,"j_芮城一期Ⅱ-015 发电机定子V相线圈温度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-015 发电机定子V相线圈温度","yc_hs_0052","cur_85"]
[1991,"j_芮城一期Ⅱ-015 发电机定子W相线圈温度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-015 发电机定子W相线圈温度","yc_hs_0052","cur_86"]
[1992,"j_芮城一期Ⅱ-015 发电机非驱动端轴承温度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-015 发电机非驱动端轴承温度","yc_hs_0052","cur_07"]
[1993,"j_芮城一期Ⅱ-015 发电机驱动端轴承温度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-015 发电机驱动端轴承温度","yc_hs_0052","cur_06"]
[1994,"j_芮城一期Ⅱ-015 发电机有功功率","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-015 发电机有功功率","yc_hs_0051","cur_96"]
[1995,"j_芮城一期Ⅱ-015 发电机转速","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-015 发电机转速","yc_hs_0052","cur_05"]
[1996,"j_芮城一期Ⅱ-015 风速","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-015 风速","yc_hs_0052","cur_18"]
[1997,"j_芮城一期Ⅱ-015 风向","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-015 风向","yc_hs_0052","cur_17"]
[1998,"j_芮城一期Ⅱ-015 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-015 机舱侧向振动(已滤波)","yc_hs_0052","cur_54"]
[1999,"j_芮城一期Ⅱ-015 机舱角度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-015 机舱角度","yc_hs_0053","cur_57"]
[2000,"j_芮城一期Ⅱ-015 机舱中轴线与风向夹角","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-015 机舱中轴线与风向夹角","yc_hs_0052","cur_19"]
[2001,"j_芮城一期Ⅱ-015 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-015 机舱轴向振动(已滤波)","yc_hs_0052","cur_56"]
[2002,"j_芮城一期Ⅱ-015 扭缆角度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-015 扭缆角度","yc_hs_0052","cur_58"]
[2003,"j_芮城一期Ⅱ-015 主轴承外圈温度","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-015 主轴承外圈温度","yc_hs_0052","cur_47"]
[2004,"j_芮城一期Ⅱ-015 主轴转速","芮城风电场","WOF35900078",15,"SXRC.T1_L2.WTG015.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-015 主轴转速","yc_hs_0052","cur_42"]
[2005,"j_芮城一期Ⅱ-016  1#桨叶片角度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-016  1#桨叶片角度","yc_hs_0052","cur_94"]
[2006,"j_芮城一期Ⅱ-016  2#桨叶片角度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-016  2#桨叶片角度","yc_hs_0052","cur_96"]
[2007,"j_芮城一期Ⅱ-016  3#桨叶片角度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-016  3#桨叶片角度","yc_hs_0052","cur_98"]
[2008,"j_芮城一期Ⅱ-016 舱内温度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-016 舱内温度","yc_hs_0052","cur_87"]
[2009,"j_芮城一期Ⅱ-016 舱外温度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-016 舱外温度","yc_hs_0052","cur_89"]
[2010,"j_芮城一期Ⅱ-016 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-016 齿轮箱高速轴非驱动端轴承温度","yc_hs_0053","cur_19"]
[2011,"j_芮城一期Ⅱ-016 齿轮箱油池温度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-016 齿轮箱油池温度","yc_hs_0053","cur_20"]
[2012,"j_芮城一期Ⅱ-016 发电机定子U相线圈温度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-016 发电机定子U相线圈温度","yc_hs_0052","cur_82"]
[2013,"j_芮城一期Ⅱ-016 发电机定子V相线圈温度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-016 发电机定子V相线圈温度","yc_hs_0053","cur_59"]
[2014,"j_芮城一期Ⅱ-016 发电机定子W相线圈温度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-016 发电机定子W相线圈温度","yc_hs_0053","cur_60"]
[2015,"j_芮城一期Ⅱ-016 发电机非驱动端轴承温度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-016 发电机非驱动端轴承温度","yc_hs_0052","cur_81"]
[2016,"j_芮城一期Ⅱ-016 发电机驱动端轴承温度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-016 发电机驱动端轴承温度","yc_hs_0052","cur_80"]
[2017,"j_芮城一期Ⅱ-016 发电机有功功率","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-016 发电机有功功率","yc_hs_0052","cur_70"]
[2018,"j_芮城一期Ⅱ-016 发电机转速","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-016 发电机转速","yc_hs_0052","cur_79"]
[2019,"j_芮城一期Ⅱ-016 风速","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-016 风速","yc_hs_0052","cur_92"]
[2020,"j_芮城一期Ⅱ-016 风向","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-016 风向","yc_hs_0052","cur_91"]
[2021,"j_芮城一期Ⅱ-016 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-016 机舱侧向振动(已滤波)","yc_hs_0053","cur_28"]
[2022,"j_芮城一期Ⅱ-016 机舱角度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-016 机舱角度","yc_hs_0054","cur_31"]
[2023,"j_芮城一期Ⅱ-016 机舱中轴线与风向夹角","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-016 机舱中轴线与风向夹角","yc_hs_0052","cur_93"]
[2024,"j_芮城一期Ⅱ-016 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-016 机舱轴向振动(已滤波)","yc_hs_0053","cur_30"]
[2025,"j_芮城一期Ⅱ-016 扭缆角度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-016 扭缆角度","yc_hs_0053","cur_32"]
[2026,"j_芮城一期Ⅱ-016 主轴承外圈温度","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-016 主轴承外圈温度","yc_hs_0053","cur_21"]
[2027,"j_芮城一期Ⅱ-016 主轴转速","芮城风电场","WOF35900078",16,"SXRC.T1_L2.WTG016.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-016 主轴转速","yc_hs_0053","cur_16"]
[2028,"j_芮城一期Ⅱ-017  1#桨叶片角度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-017  1#桨叶片角度","yc_hs_0053","cur_68"]
[2029,"j_芮城一期Ⅱ-017  2#桨叶片角度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-017  2#桨叶片角度","yc_hs_0053","cur_70"]
[2030,"j_芮城一期Ⅱ-017  3#桨叶片角度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-017  3#桨叶片角度","yc_hs_0053","cur_72"]
[2031,"j_芮城一期Ⅱ-017 舱内温度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-017 舱内温度","yc_hs_0053","cur_61"]
[2032,"j_芮城一期Ⅱ-017 舱外温度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-017 舱外温度","yc_hs_0053","cur_63"]
[2033,"j_芮城一期Ⅱ-017 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-017 齿轮箱高速轴非驱动端轴承温度","yc_hs_0053","cur_93"]
[2034,"j_芮城一期Ⅱ-017 齿轮箱油池温度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-017 齿轮箱油池温度","yc_hs_0053","cur_94"]
[2035,"j_芮城一期Ⅱ-017 发电机定子U相线圈温度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-017 发电机定子U相线圈温度","yc_hs_0053","cur_56"]
[2036,"j_芮城一期Ⅱ-017 发电机定子V相线圈温度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-017 发电机定子V相线圈温度","yc_hs_0054","cur_33"]
[2037,"j_芮城一期Ⅱ-017 发电机定子W相线圈温度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-017 发电机定子W相线圈温度","yc_hs_0054","cur_34"]
[2038,"j_芮城一期Ⅱ-017 发电机非驱动端轴承温度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-017 发电机非驱动端轴承温度","yc_hs_0053","cur_55"]
[2039,"j_芮城一期Ⅱ-017 发电机驱动端轴承温度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-017 发电机驱动端轴承温度","yc_hs_0053","cur_54"]
[2040,"j_芮城一期Ⅱ-017 发电机有功功率","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-017 发电机有功功率","yc_hs_0053","cur_44"]
[2041,"j_芮城一期Ⅱ-017 发电机转速","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-017 发电机转速","yc_hs_0053","cur_53"]
[2042,"j_芮城一期Ⅱ-017 风速","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-017 风速","yc_hs_0053","cur_66"]
[2043,"j_芮城一期Ⅱ-017 风向","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-017 风向","yc_hs_0053","cur_65"]
[2044,"j_芮城一期Ⅱ-017 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-017 机舱侧向振动(已滤波)","yc_hs_0054","cur_02"]
[2045,"j_芮城一期Ⅱ-017 机舱角度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-017 机舱角度","yc_hs_0055","cur_05"]
[2046,"j_芮城一期Ⅱ-017 机舱中轴线与风向夹角","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-017 机舱中轴线与风向夹角","yc_hs_0053","cur_67"]
[2047,"j_芮城一期Ⅱ-017 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-017 机舱轴向振动(已滤波)","yc_hs_0054","cur_04"]
[2048,"j_芮城一期Ⅱ-017 扭缆角度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-017 扭缆角度","yc_hs_0054","cur_06"]
[2049,"j_芮城一期Ⅱ-017 主轴承外圈温度","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-017 主轴承外圈温度","yc_hs_0053","cur_95"]
[2050,"j_芮城一期Ⅱ-017 主轴转速","芮城风电场","WOF35900078",17,"SXRC.T1_L2.WTG017.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-017 主轴转速","yc_hs_0053","cur_90"]
[2051,"j_芮城一期Ⅱ-018  1#桨叶片角度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-018  1#桨叶片角度","yc_hs_0054","cur_42"]
[2052,"j_芮城一期Ⅱ-018  2#桨叶片角度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-018  2#桨叶片角度","yc_hs_0054","cur_44"]
[2053,"j_芮城一期Ⅱ-018  3#桨叶片角度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-018  3#桨叶片角度","yc_hs_0054","cur_46"]
[2054,"j_芮城一期Ⅱ-018 舱内温度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-018 舱内温度","yc_hs_0054","cur_35"]
[2055,"j_芮城一期Ⅱ-018 舱外温度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-018 舱外温度","yc_hs_0054","cur_37"]
[2056,"j_芮城一期Ⅱ-018 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-018 齿轮箱高速轴非驱动端轴承温度","yc_hs_0054","cur_67"]
[2057,"j_芮城一期Ⅱ-018 齿轮箱油池温度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-018 齿轮箱油池温度","yc_hs_0054","cur_68"]
[2058,"j_芮城一期Ⅱ-018 发电机定子U相线圈温度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-018 发电机定子U相线圈温度","yc_hs_0054","cur_30"]
[2059,"j_芮城一期Ⅱ-018 发电机定子V相线圈温度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-018 发电机定子V相线圈温度","yc_hs_0055","cur_07"]
[2060,"j_芮城一期Ⅱ-018 发电机定子W相线圈温度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-018 发电机定子W相线圈温度","yc_hs_0055","cur_08"]
[2061,"j_芮城一期Ⅱ-018 发电机非驱动端轴承温度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-018 发电机非驱动端轴承温度","yc_hs_0054","cur_29"]
[2062,"j_芮城一期Ⅱ-018 发电机驱动端轴承温度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-018 发电机驱动端轴承温度","yc_hs_0054","cur_28"]
[2063,"j_芮城一期Ⅱ-018 发电机有功功率","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-018 发电机有功功率","yc_hs_0054","cur_18"]
[2064,"j_芮城一期Ⅱ-018 发电机转速","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-018 发电机转速","yc_hs_0054","cur_27"]
[2065,"j_芮城一期Ⅱ-018 风速","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-018 风速","yc_hs_0054","cur_40"]
[2066,"j_芮城一期Ⅱ-018 风向","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-018 风向","yc_hs_0054","cur_39"]
[2067,"j_芮城一期Ⅱ-018 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-018 机舱侧向振动(已滤波)","yc_hs_0054","cur_76"]
[2068,"j_芮城一期Ⅱ-018 机舱角度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-018 机舱角度","yc_hs_0055","cur_79"]
[2069,"j_芮城一期Ⅱ-018 机舱中轴线与风向夹角","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-018 机舱中轴线与风向夹角","yc_hs_0054","cur_41"]
[2070,"j_芮城一期Ⅱ-018 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-018 机舱轴向振动(已滤波)","yc_hs_0054","cur_78"]
[2071,"j_芮城一期Ⅱ-018 扭缆角度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-018 扭缆角度","yc_hs_0054","cur_80"]
[2072,"j_芮城一期Ⅱ-018 主轴承外圈温度","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-018 主轴承外圈温度","yc_hs_0054","cur_69"]
[2073,"j_芮城一期Ⅱ-018 主轴转速","芮城风电场","WOF35900078",18,"SXRC.T1_L2.WTG018.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-018 主轴转速","yc_hs_0054","cur_64"]
[2074,"j_芮城一期Ⅱ-019  1#桨叶片角度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-019  1#桨叶片角度","yc_hs_0055","cur_16"]
[2075,"j_芮城一期Ⅱ-019  2#桨叶片角度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-019  2#桨叶片角度","yc_hs_0055","cur_18"]
[2076,"j_芮城一期Ⅱ-019  3#桨叶片角度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-019  3#桨叶片角度","yc_hs_0055","cur_20"]
[2077,"j_芮城一期Ⅱ-019 舱内温度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-019 舱内温度","yc_hs_0055","cur_09"]
[2078,"j_芮城一期Ⅱ-019 舱外温度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-019 舱外温度","yc_hs_0055","cur_11"]
[2079,"j_芮城一期Ⅱ-019 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-019 齿轮箱高速轴非驱动端轴承温度","yc_hs_0055","cur_41"]
[2080,"j_芮城一期Ⅱ-019 齿轮箱油池温度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-019 齿轮箱油池温度","yc_hs_0055","cur_42"]
[2081,"j_芮城一期Ⅱ-019 发电机定子U相线圈温度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-019 发电机定子U相线圈温度","yc_hs_0055","cur_04"]
[2082,"j_芮城一期Ⅱ-019 发电机定子V相线圈温度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-019 发电机定子V相线圈温度","yc_hs_0055","cur_81"]
[2083,"j_芮城一期Ⅱ-019 发电机定子W相线圈温度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-019 发电机定子W相线圈温度","yc_hs_0055","cur_82"]
[2084,"j_芮城一期Ⅱ-019 发电机非驱动端轴承温度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-019 发电机非驱动端轴承温度","yc_hs_0055","cur_03"]
[2085,"j_芮城一期Ⅱ-019 发电机驱动端轴承温度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-019 发电机驱动端轴承温度","yc_hs_0055","cur_02"]
[2086,"j_芮城一期Ⅱ-019 发电机有功功率","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-019 发电机有功功率","yc_hs_0054","cur_92"]
[2087,"j_芮城一期Ⅱ-019 发电机转速","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-019 发电机转速","yc_hs_0055","cur_01"]
[2088,"j_芮城一期Ⅱ-019 风速","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-019 风速","yc_hs_0055","cur_14"]
[2089,"j_芮城一期Ⅱ-019 风向","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-019 风向","yc_hs_0055","cur_13"]
[2090,"j_芮城一期Ⅱ-019 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-019 机舱侧向振动(已滤波)","yc_hs_0055","cur_50"]
[2091,"j_芮城一期Ⅱ-019 机舱角度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-019 机舱角度","yc_hs_0056","cur_53"]
[2092,"j_芮城一期Ⅱ-019 机舱中轴线与风向夹角","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-019 机舱中轴线与风向夹角","yc_hs_0055","cur_15"]
[2093,"j_芮城一期Ⅱ-019 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-019 机舱轴向振动(已滤波)","yc_hs_0055","cur_52"]
[2094,"j_芮城一期Ⅱ-019 扭缆角度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-019 扭缆角度","yc_hs_0055","cur_54"]
[2095,"j_芮城一期Ⅱ-019 主轴承外圈温度","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-019 主轴承外圈温度","yc_hs_0055","cur_43"]
[2096,"j_芮城一期Ⅱ-019 主轴转速","芮城风电场","WOF35900078",19,"SXRC.T1_L2.WTG019.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-019 主轴转速","yc_hs_0055","cur_38"]
[2097,"j_芮城一期Ⅱ-021  1#桨叶片角度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-021  1#桨叶片角度","yc_hs_0056","cur_64"]
[2098,"j_芮城一期Ⅱ-021  2#桨叶片角度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-021  2#桨叶片角度","yc_hs_0056","cur_66"]
[2099,"j_芮城一期Ⅱ-021  3#桨叶片角度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-021  3#桨叶片角度","yc_hs_0056","cur_68"]
[2100,"j_芮城一期Ⅱ-021 舱内温度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-021 舱内温度","yc_hs_0056","cur_57"]
[2101,"j_芮城一期Ⅱ-021 舱外温度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-021 舱外温度","yc_hs_0056","cur_59"]
[2102,"j_芮城一期Ⅱ-021 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-021 齿轮箱高速轴非驱动端轴承温度","yc_hs_0056","cur_89"]
[2103,"j_芮城一期Ⅱ-021 齿轮箱油池温度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-021 齿轮箱油池温度","yc_hs_0056","cur_90"]
[2104,"j_芮城一期Ⅱ-021 发电机定子U相线圈温度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-021 发电机定子U相线圈温度","yc_hs_0056","cur_52"]
[2105,"j_芮城一期Ⅱ-021 发电机定子V相线圈温度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-021 发电机定子V相线圈温度","yc_hs_0057","cur_29"]
[2106,"j_芮城一期Ⅱ-021 发电机定子W相线圈温度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-021 发电机定子W相线圈温度","yc_hs_0057","cur_30"]
[2107,"j_芮城一期Ⅱ-021 发电机非驱动端轴承温度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-021 发电机非驱动端轴承温度","yc_hs_0056","cur_51"]
[2108,"j_芮城一期Ⅱ-021 发电机驱动端轴承温度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-021 发电机驱动端轴承温度","yc_hs_0056","cur_50"]
[2109,"j_芮城一期Ⅱ-021 发电机有功功率","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-021 发电机有功功率","yc_hs_0056","cur_40"]
[2110,"j_芮城一期Ⅱ-021 发电机转速","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-021 发电机转速","yc_hs_0056","cur_49"]
[2111,"j_芮城一期Ⅱ-021 风速","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-021 风速","yc_hs_0056","cur_62"]
[2112,"j_芮城一期Ⅱ-021 风向","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-021 风向","yc_hs_0056","cur_61"]
[2113,"j_芮城一期Ⅱ-021 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-021 机舱侧向振动(已滤波)","yc_hs_0056","cur_98"]
[2114,"j_芮城一期Ⅱ-021 机舱角度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-021 机舱角度","yc_hs_0058","cur_01"]
[2115,"j_芮城一期Ⅱ-021 机舱中轴线与风向夹角","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-021 机舱中轴线与风向夹角","yc_hs_0056","cur_63"]
[2116,"j_芮城一期Ⅱ-021 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-021 机舱轴向振动(已滤波)","yc_hs_0056","cur_100"]
[2117,"j_芮城一期Ⅱ-021 扭缆角度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-021 扭缆角度","yc_hs_0057","cur_02"]
[2118,"j_芮城一期Ⅱ-021 主轴承外圈温度","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-021 主轴承外圈温度","yc_hs_0056","cur_91"]
[2119,"j_芮城一期Ⅱ-021 主轴转速","芮城风电场","WOF35900078",21,"SXRC.T1_L2.WTG021.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-021 主轴转速","yc_hs_0056","cur_86"]
[2120,"j_芮城一期Ⅱ-023  1#桨叶片角度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-023  1#桨叶片角度","yc_hs_0058","cur_12"]
[2121,"j_芮城一期Ⅱ-023  2#桨叶片角度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-023  2#桨叶片角度","yc_hs_0058","cur_14"]
[2122,"j_芮城一期Ⅱ-023  3#桨叶片角度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-023  3#桨叶片角度","yc_hs_0058","cur_16"]
[2123,"j_芮城一期Ⅱ-023 舱内温度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-023 舱内温度","yc_hs_0058","cur_05"]
[2124,"j_芮城一期Ⅱ-023 舱外温度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-023 舱外温度","yc_hs_0058","cur_07"]
[2125,"j_芮城一期Ⅱ-023 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-023 齿轮箱高速轴非驱动端轴承温度","yc_hs_0058","cur_37"]
[2126,"j_芮城一期Ⅱ-023 齿轮箱油池温度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-023 齿轮箱油池温度","yc_hs_0058","cur_38"]
[2127,"j_芮城一期Ⅱ-023 发电机定子U相线圈温度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-023 发电机定子U相线圈温度","yc_hs_0057","cur_100"]
[2128,"j_芮城一期Ⅱ-023 发电机定子V相线圈温度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-023 发电机定子V相线圈温度","yc_hs_0058","cur_77"]
[2129,"j_芮城一期Ⅱ-023 发电机定子W相线圈温度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-023 发电机定子W相线圈温度","yc_hs_0058","cur_78"]
[2130,"j_芮城一期Ⅱ-023 发电机非驱动端轴承温度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-023 发电机非驱动端轴承温度","yc_hs_0057","cur_99"]
[2131,"j_芮城一期Ⅱ-023 发电机驱动端轴承温度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-023 发电机驱动端轴承温度","yc_hs_0057","cur_98"]
[2132,"j_芮城一期Ⅱ-023 发电机有功功率","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-023 发电机有功功率","yc_hs_0057","cur_88"]
[2133,"j_芮城一期Ⅱ-023 发电机转速","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-023 发电机转速","yc_hs_0057","cur_97"]
[2134,"j_芮城一期Ⅱ-023 风速","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-023 风速","yc_hs_0058","cur_10"]
[2135,"j_芮城一期Ⅱ-023 风向","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-023 风向","yc_hs_0058","cur_09"]
[2136,"j_芮城一期Ⅱ-023 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-023 机舱侧向振动(已滤波)","yc_hs_0058","cur_46"]
[2137,"j_芮城一期Ⅱ-023 机舱角度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-023 机舱角度","yc_hs_0059","cur_49"]
[2138,"j_芮城一期Ⅱ-023 机舱中轴线与风向夹角","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-023 机舱中轴线与风向夹角","yc_hs_0058","cur_11"]
[2139,"j_芮城一期Ⅱ-023 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-023 机舱轴向振动(已滤波)","yc_hs_0058","cur_48"]
[2140,"j_芮城一期Ⅱ-023 扭缆角度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-023 扭缆角度","yc_hs_0058","cur_50"]
[2141,"j_芮城一期Ⅱ-023 主轴承外圈温度","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-023 主轴承外圈温度","yc_hs_0058","cur_39"]
[2142,"j_芮城一期Ⅱ-023 主轴转速","芮城风电场","WOF35900078",23,"SXRC.T1_L2.WTG023.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-023 主轴转速","yc_hs_0058","cur_34"]
[2143,"j_芮城一期Ⅱ-024  1#桨叶片角度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-024  1#桨叶片角度","yc_hs_0058","cur_86"]
[2144,"j_芮城一期Ⅱ-024  2#桨叶片角度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-024  2#桨叶片角度","yc_hs_0058","cur_88"]
[2145,"j_芮城一期Ⅱ-024  3#桨叶片角度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-024  3#桨叶片角度","yc_hs_0058","cur_90"]
[2146,"j_芮城一期Ⅱ-024 舱内温度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-024 舱内温度","yc_hs_0058","cur_79"]
[2147,"j_芮城一期Ⅱ-024 舱外温度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-024 舱外温度","yc_hs_0058","cur_81"]
[2148,"j_芮城一期Ⅱ-024 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-024 齿轮箱高速轴非驱动端轴承温度","yc_hs_0059","cur_11"]
[2149,"j_芮城一期Ⅱ-024 齿轮箱油池温度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-024 齿轮箱油池温度","yc_hs_0059","cur_12"]
[2150,"j_芮城一期Ⅱ-024 发电机定子U相线圈温度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-024 发电机定子U相线圈温度","yc_hs_0058","cur_74"]
[2151,"j_芮城一期Ⅱ-024 发电机定子V相线圈温度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-024 发电机定子V相线圈温度","yc_hs_0059","cur_51"]
[2152,"j_芮城一期Ⅱ-024 发电机定子W相线圈温度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-024 发电机定子W相线圈温度","yc_hs_0059","cur_52"]
[2153,"j_芮城一期Ⅱ-024 发电机非驱动端轴承温度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-024 发电机非驱动端轴承温度","yc_hs_0058","cur_73"]
[2154,"j_芮城一期Ⅱ-024 发电机驱动端轴承温度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-024 发电机驱动端轴承温度","yc_hs_0058","cur_72"]
[2155,"j_芮城一期Ⅱ-024 发电机有功功率","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-024 发电机有功功率","yc_hs_0058","cur_62"]
[2156,"j_芮城一期Ⅱ-024 发电机转速","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-024 发电机转速","yc_hs_0058","cur_71"]
[2157,"j_芮城一期Ⅱ-024 风速","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-024 风速","yc_hs_0058","cur_84"]
[2158,"j_芮城一期Ⅱ-024 风向","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-024 风向","yc_hs_0058","cur_83"]
[2159,"j_芮城一期Ⅱ-024 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-024 机舱侧向振动(已滤波)","yc_hs_0059","cur_20"]
[2160,"j_芮城一期Ⅱ-024 机舱角度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-024 机舱角度","yc_hs_0060","cur_23"]
[2161,"j_芮城一期Ⅱ-024 机舱中轴线与风向夹角","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-024 机舱中轴线与风向夹角","yc_hs_0058","cur_85"]
[2162,"j_芮城一期Ⅱ-024 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-024 机舱轴向振动(已滤波)","yc_hs_0059","cur_22"]
[2163,"j_芮城一期Ⅱ-024 扭缆角度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-024 扭缆角度","yc_hs_0059","cur_24"]
[2164,"j_芮城一期Ⅱ-024 主轴承外圈温度","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-024 主轴承外圈温度","yc_hs_0059","cur_13"]
[2165,"j_芮城一期Ⅱ-024 主轴转速","芮城风电场","WOF35900078",24,"SXRC.T1_L2.WTG024.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-024 主轴转速","yc_hs_0059","cur_08"]
[2166,"j_芮城一期Ⅱ-025  1#桨叶片角度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-025  1#桨叶片角度","yc_hs_0059","cur_60"]
[2167,"j_芮城一期Ⅱ-025  2#桨叶片角度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-025  2#桨叶片角度","yc_hs_0059","cur_62"]
[2168,"j_芮城一期Ⅱ-025  3#桨叶片角度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-025  3#桨叶片角度","yc_hs_0059","cur_64"]
[2169,"j_芮城一期Ⅱ-025 舱内温度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-025 舱内温度","yc_hs_0059","cur_53"]
[2170,"j_芮城一期Ⅱ-025 舱外温度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-025 舱外温度","yc_hs_0059","cur_55"]
[2171,"j_芮城一期Ⅱ-025 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-025 齿轮箱高速轴非驱动端轴承温度","yc_hs_0059","cur_85"]
[2172,"j_芮城一期Ⅱ-025 齿轮箱油池温度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-025 齿轮箱油池温度","yc_hs_0059","cur_86"]
[2173,"j_芮城一期Ⅱ-025 发电机定子U相线圈温度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-025 发电机定子U相线圈温度","yc_hs_0059","cur_48"]
[2174,"j_芮城一期Ⅱ-025 发电机定子V相线圈温度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-025 发电机定子V相线圈温度","yc_hs_0060","cur_25"]
[2175,"j_芮城一期Ⅱ-025 发电机定子W相线圈温度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-025 发电机定子W相线圈温度","yc_hs_0060","cur_26"]
[2176,"j_芮城一期Ⅱ-025 发电机非驱动端轴承温度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-025 发电机非驱动端轴承温度","yc_hs_0059","cur_47"]
[2177,"j_芮城一期Ⅱ-025 发电机驱动端轴承温度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-025 发电机驱动端轴承温度","yc_hs_0059","cur_46"]
[2178,"j_芮城一期Ⅱ-025 发电机有功功率","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-025 发电机有功功率","yc_hs_0059","cur_36"]
[2179,"j_芮城一期Ⅱ-025 发电机转速","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-025 发电机转速","yc_hs_0059","cur_45"]
[2180,"j_芮城一期Ⅱ-025 风速","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-025 风速","yc_hs_0059","cur_58"]
[2181,"j_芮城一期Ⅱ-025 风向","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-025 风向","yc_hs_0059","cur_57"]
[2182,"j_芮城一期Ⅱ-025 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-025 机舱侧向振动(已滤波)","yc_hs_0059","cur_94"]
[2183,"j_芮城一期Ⅱ-025 机舱角度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-025 机舱角度","yc_hs_0060","cur_97"]
[2184,"j_芮城一期Ⅱ-025 机舱中轴线与风向夹角","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-025 机舱中轴线与风向夹角","yc_hs_0059","cur_59"]
[2185,"j_芮城一期Ⅱ-025 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-025 机舱轴向振动(已滤波)","yc_hs_0059","cur_96"]
[2186,"j_芮城一期Ⅱ-025 扭缆角度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-025 扭缆角度","yc_hs_0059","cur_98"]
[2187,"j_芮城一期Ⅱ-025 主轴承外圈温度","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-025 主轴承外圈温度","yc_hs_0059","cur_87"]
[2188,"j_芮城一期Ⅱ-025 主轴转速","芮城风电场","WOF35900078",25,"SXRC.T1_L2.WTG025.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-025 主轴转速","yc_hs_0059","cur_82"]
[2189,"j_芮城一期Ⅱ-026  1#桨叶片角度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-026  1#桨叶片角度","yc_hs_0060","cur_34"]
[2190,"j_芮城一期Ⅱ-026  2#桨叶片角度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-026  2#桨叶片角度","yc_hs_0060","cur_36"]
[2191,"j_芮城一期Ⅱ-026  3#桨叶片角度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-026  3#桨叶片角度","yc_hs_0060","cur_38"]
[2192,"j_芮城一期Ⅱ-026 舱内温度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-026 舱内温度","yc_hs_0060","cur_27"]
[2193,"j_芮城一期Ⅱ-026 舱外温度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-026 舱外温度","yc_hs_0060","cur_29"]
[2194,"j_芮城一期Ⅱ-026 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-026 齿轮箱高速轴非驱动端轴承温度","yc_hs_0060","cur_59"]
[2195,"j_芮城一期Ⅱ-026 齿轮箱油池温度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-026 齿轮箱油池温度","yc_hs_0060","cur_60"]
[2196,"j_芮城一期Ⅱ-026 发电机定子U相线圈温度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-026 发电机定子U相线圈温度","yc_hs_0060","cur_22"]
[2197,"j_芮城一期Ⅱ-026 发电机定子V相线圈温度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-026 发电机定子V相线圈温度","yc_hs_0060","cur_99"]
[2198,"j_芮城一期Ⅱ-026 发电机定子W相线圈温度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-026 发电机定子W相线圈温度","yc_hs_0060","cur_100"]
[2199,"j_芮城一期Ⅱ-026 发电机非驱动端轴承温度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-026 发电机非驱动端轴承温度","yc_hs_0060","cur_21"]
[2200,"j_芮城一期Ⅱ-026 发电机驱动端轴承温度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-026 发电机驱动端轴承温度","yc_hs_0060","cur_20"]
[2201,"j_芮城一期Ⅱ-026 发电机有功功率","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-026 发电机有功功率","yc_hs_0060","cur_10"]
[2202,"j_芮城一期Ⅱ-026 发电机转速","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-026 发电机转速","yc_hs_0060","cur_19"]
[2203,"j_芮城一期Ⅱ-026 风速","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-026 风速","yc_hs_0060","cur_32"]
[2204,"j_芮城一期Ⅱ-026 风向","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-026 风向","yc_hs_0060","cur_31"]
[2205,"j_芮城一期Ⅱ-026 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-026 机舱侧向振动(已滤波)","yc_hs_0060","cur_68"]
[2206,"j_芮城一期Ⅱ-026 机舱角度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-026 机舱角度","yc_hs_0061","cur_71"]
[2207,"j_芮城一期Ⅱ-026 机舱中轴线与风向夹角","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-026 机舱中轴线与风向夹角","yc_hs_0060","cur_33"]
[2208,"j_芮城一期Ⅱ-026 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-026 机舱轴向振动(已滤波)","yc_hs_0060","cur_70"]
[2209,"j_芮城一期Ⅱ-026 扭缆角度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-026 扭缆角度","yc_hs_0060","cur_72"]
[2210,"j_芮城一期Ⅱ-026 主轴承外圈温度","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-026 主轴承外圈温度","yc_hs_0060","cur_61"]
[2211,"j_芮城一期Ⅱ-026 主轴转速","芮城风电场","WOF35900078",26,"SXRC.T1_L2.WTG026.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-026 主轴转速","yc_hs_0060","cur_56"]
[2212,"j_芮城一期Ⅱ-028  1#桨叶片角度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-028  1#桨叶片角度","yc_hs_0061","cur_82"]
[2213,"j_芮城一期Ⅱ-028  2#桨叶片角度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-028  2#桨叶片角度","yc_hs_0061","cur_84"]
[2214,"j_芮城一期Ⅱ-028  3#桨叶片角度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-028  3#桨叶片角度","yc_hs_0061","cur_86"]
[2215,"j_芮城一期Ⅱ-028 舱内温度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-028 舱内温度","yc_hs_0061","cur_75"]
[2216,"j_芮城一期Ⅱ-028 舱外温度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-028 舱外温度","yc_hs_0061","cur_77"]
[2217,"j_芮城一期Ⅱ-028 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-028 齿轮箱高速轴非驱动端轴承温度","yc_hs_0062","cur_07"]
[2218,"j_芮城一期Ⅱ-028 齿轮箱油池温度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-028 齿轮箱油池温度","yc_hs_0062","cur_08"]
[2219,"j_芮城一期Ⅱ-028 发电机定子U相线圈温度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-028 发电机定子U相线圈温度","yc_hs_0061","cur_70"]
[2220,"j_芮城一期Ⅱ-028 发电机定子V相线圈温度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-028 发电机定子V相线圈温度","yc_hs_0062","cur_47"]
[2221,"j_芮城一期Ⅱ-028 发电机定子W相线圈温度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-028 发电机定子W相线圈温度","yc_hs_0062","cur_48"]
[2222,"j_芮城一期Ⅱ-028 发电机非驱动端轴承温度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-028 发电机非驱动端轴承温度","yc_hs_0061","cur_69"]
[2223,"j_芮城一期Ⅱ-028 发电机驱动端轴承温度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-028 发电机驱动端轴承温度","yc_hs_0061","cur_68"]
[2224,"j_芮城一期Ⅱ-028 发电机有功功率","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-028 发电机有功功率","yc_hs_0061","cur_58"]
[2225,"j_芮城一期Ⅱ-028 发电机转速","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-028 发电机转速","yc_hs_0061","cur_67"]
[2226,"j_芮城一期Ⅱ-028 风速","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-028 风速","yc_hs_0061","cur_80"]
[2227,"j_芮城一期Ⅱ-028 风向","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-028 风向","yc_hs_0061","cur_79"]
[2228,"j_芮城一期Ⅱ-028 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-028 机舱侧向振动(已滤波)","yc_hs_0062","cur_16"]
[2229,"j_芮城一期Ⅱ-028 机舱角度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-028 机舱角度","yc_hs_0063","cur_19"]
[2230,"j_芮城一期Ⅱ-028 机舱中轴线与风向夹角","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-028 机舱中轴线与风向夹角","yc_hs_0061","cur_81"]
[2231,"j_芮城一期Ⅱ-028 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-028 机舱轴向振动(已滤波)","yc_hs_0062","cur_18"]
[2232,"j_芮城一期Ⅱ-028 扭缆角度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-028 扭缆角度","yc_hs_0062","cur_20"]
[2233,"j_芮城一期Ⅱ-028 主轴承外圈温度","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-028 主轴承外圈温度","yc_hs_0062","cur_09"]
[2234,"j_芮城一期Ⅱ-028 主轴转速","芮城风电场","WOF35900078",28,"SXRC.T1_L2.WTG028.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-028 主轴转速","yc_hs_0062","cur_04"]
[2235,"j_芮城一期Ⅱ-029  1#桨叶片角度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-029  1#桨叶片角度","yc_hs_0062","cur_56"]
[2236,"j_芮城一期Ⅱ-029  2#桨叶片角度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-029  2#桨叶片角度","yc_hs_0062","cur_58"]
[2237,"j_芮城一期Ⅱ-029  3#桨叶片角度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-029  3#桨叶片角度","yc_hs_0062","cur_60"]
[2238,"j_芮城一期Ⅱ-029 舱内温度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-029 舱内温度","yc_hs_0062","cur_49"]
[2239,"j_芮城一期Ⅱ-029 舱外温度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-029 舱外温度","yc_hs_0062","cur_51"]
[2240,"j_芮城一期Ⅱ-029 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-029 齿轮箱高速轴非驱动端轴承温度","yc_hs_0062","cur_81"]
[2241,"j_芮城一期Ⅱ-029 齿轮箱油池温度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-029 齿轮箱油池温度","yc_hs_0062","cur_82"]
[2242,"j_芮城一期Ⅱ-029 发电机定子U相线圈温度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-029 发电机定子U相线圈温度","yc_hs_0062","cur_44"]
[2243,"j_芮城一期Ⅱ-029 发电机定子V相线圈温度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-029 发电机定子V相线圈温度","yc_hs_0063","cur_21"]
[2244,"j_芮城一期Ⅱ-029 发电机定子W相线圈温度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-029 发电机定子W相线圈温度","yc_hs_0063","cur_22"]
[2245,"j_芮城一期Ⅱ-029 发电机非驱动端轴承温度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-029 发电机非驱动端轴承温度","yc_hs_0062","cur_43"]
[2246,"j_芮城一期Ⅱ-029 发电机驱动端轴承温度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-029 发电机驱动端轴承温度","yc_hs_0062","cur_42"]
[2247,"j_芮城一期Ⅱ-029 发电机有功功率","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-029 发电机有功功率","yc_hs_0062","cur_32"]
[2248,"j_芮城一期Ⅱ-029 发电机转速","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-029 发电机转速","yc_hs_0062","cur_41"]
[2249,"j_芮城一期Ⅱ-029 风速","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-029 风速","yc_hs_0062","cur_54"]
[2250,"j_芮城一期Ⅱ-029 风向","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-029 风向","yc_hs_0062","cur_53"]
[2251,"j_芮城一期Ⅱ-029 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-029 机舱侧向振动(已滤波)","yc_hs_0062","cur_90"]
[2252,"j_芮城一期Ⅱ-029 机舱角度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-029 机舱角度","yc_hs_0063","cur_93"]
[2253,"j_芮城一期Ⅱ-029 机舱中轴线与风向夹角","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-029 机舱中轴线与风向夹角","yc_hs_0062","cur_55"]
[2254,"j_芮城一期Ⅱ-029 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-029 机舱轴向振动(已滤波)","yc_hs_0062","cur_92"]
[2255,"j_芮城一期Ⅱ-029 扭缆角度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-029 扭缆角度","yc_hs_0062","cur_94"]
[2256,"j_芮城一期Ⅱ-029 主轴承外圈温度","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-029 主轴承外圈温度","yc_hs_0062","cur_83"]
[2257,"j_芮城一期Ⅱ-029 主轴转速","芮城风电场","WOF35900078",29,"SXRC.T1_L2.WTG029.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-029 主轴转速","yc_hs_0062","cur_78"]
[2258,"j_芮城一期Ⅱ-030  1#桨叶片角度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-030  1#桨叶片角度","yc_hs_0063","cur_30"]
[2259,"j_芮城一期Ⅱ-030  2#桨叶片角度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-030  2#桨叶片角度","yc_hs_0063","cur_32"]
[2260,"j_芮城一期Ⅱ-030  3#桨叶片角度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-030  3#桨叶片角度","yc_hs_0063","cur_34"]
[2261,"j_芮城一期Ⅱ-030 舱内温度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-030 舱内温度","yc_hs_0063","cur_23"]
[2262,"j_芮城一期Ⅱ-030 舱外温度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-030 舱外温度","yc_hs_0063","cur_25"]
[2263,"j_芮城一期Ⅱ-030 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-030 齿轮箱高速轴非驱动端轴承温度","yc_hs_0063","cur_55"]
[2264,"j_芮城一期Ⅱ-030 齿轮箱油池温度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-030 齿轮箱油池温度","yc_hs_0063","cur_56"]
[2265,"j_芮城一期Ⅱ-030 发电机定子U相线圈温度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-030 发电机定子U相线圈温度","yc_hs_0063","cur_18"]
[2266,"j_芮城一期Ⅱ-030 发电机定子V相线圈温度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-030 发电机定子V相线圈温度","yc_hs_0063","cur_95"]
[2267,"j_芮城一期Ⅱ-030 发电机定子W相线圈温度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-030 发电机定子W相线圈温度","yc_hs_0063","cur_96"]
[2268,"j_芮城一期Ⅱ-030 发电机非驱动端轴承温度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-030 发电机非驱动端轴承温度","yc_hs_0063","cur_17"]
[2269,"j_芮城一期Ⅱ-030 发电机驱动端轴承温度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-030 发电机驱动端轴承温度","yc_hs_0063","cur_16"]
[2270,"j_芮城一期Ⅱ-030 发电机有功功率","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-030 发电机有功功率","yc_hs_0063","cur_06"]
[2271,"j_芮城一期Ⅱ-030 发电机转速","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-030 发电机转速","yc_hs_0063","cur_15"]
[2272,"j_芮城一期Ⅱ-030 风速","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-030 风速","yc_hs_0063","cur_28"]
[2273,"j_芮城一期Ⅱ-030 风向","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-030 风向","yc_hs_0063","cur_27"]
[2274,"j_芮城一期Ⅱ-030 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-030 机舱侧向振动(已滤波)","yc_hs_0063","cur_64"]
[2275,"j_芮城一期Ⅱ-030 机舱角度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-030 机舱角度","yc_hs_0064","cur_67"]
[2276,"j_芮城一期Ⅱ-030 机舱中轴线与风向夹角","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-030 机舱中轴线与风向夹角","yc_hs_0063","cur_29"]
[2277,"j_芮城一期Ⅱ-030 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-030 机舱轴向振动(已滤波)","yc_hs_0063","cur_66"]
[2278,"j_芮城一期Ⅱ-030 扭缆角度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-030 扭缆角度","yc_hs_0063","cur_68"]
[2279,"j_芮城一期Ⅱ-030 主轴承外圈温度","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-030 主轴承外圈温度","yc_hs_0063","cur_57"]
[2280,"j_芮城一期Ⅱ-030 主轴转速","芮城风电场","WOF35900078",30,"SXRC.T1_L2.WTG030.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-030 主轴转速","yc_hs_0063","cur_52"]
[2281,"j_芮城一期Ⅱ-031  1#桨叶片角度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-031  1#桨叶片角度","yc_hs_0064","cur_04"]
[2282,"j_芮城一期Ⅱ-031  2#桨叶片角度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-031  2#桨叶片角度","yc_hs_0064","cur_06"]
[2283,"j_芮城一期Ⅱ-031  3#桨叶片角度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-031  3#桨叶片角度","yc_hs_0064","cur_08"]
[2284,"j_芮城一期Ⅱ-031 舱内温度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-031 舱内温度","yc_hs_0063","cur_97"]
[2285,"j_芮城一期Ⅱ-031 舱外温度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-031 舱外温度","yc_hs_0063","cur_99"]
[2286,"j_芮城一期Ⅱ-031 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-031 齿轮箱高速轴非驱动端轴承温度","yc_hs_0064","cur_29"]
[2287,"j_芮城一期Ⅱ-031 齿轮箱油池温度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-031 齿轮箱油池温度","yc_hs_0064","cur_30"]
[2288,"j_芮城一期Ⅱ-031 发电机定子U相线圈温度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-031 发电机定子U相线圈温度","yc_hs_0063","cur_92"]
[2289,"j_芮城一期Ⅱ-031 发电机定子V相线圈温度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-031 发电机定子V相线圈温度","yc_hs_0064","cur_69"]
[2290,"j_芮城一期Ⅱ-031 发电机定子W相线圈温度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-031 发电机定子W相线圈温度","yc_hs_0064","cur_70"]
[2291,"j_芮城一期Ⅱ-031 发电机非驱动端轴承温度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-031 发电机非驱动端轴承温度","yc_hs_0063","cur_91"]
[2292,"j_芮城一期Ⅱ-031 发电机驱动端轴承温度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-031 发电机驱动端轴承温度","yc_hs_0063","cur_90"]
[2293,"j_芮城一期Ⅱ-031 发电机有功功率","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-031 发电机有功功率","yc_hs_0063","cur_80"]
[2294,"j_芮城一期Ⅱ-031 发电机转速","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-031 发电机转速","yc_hs_0063","cur_89"]
[2295,"j_芮城一期Ⅱ-031 风速","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-031 风速","yc_hs_0064","cur_02"]
[2296,"j_芮城一期Ⅱ-031 风向","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-031 风向","yc_hs_0064","cur_01"]
[2297,"j_芮城一期Ⅱ-031 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-031 机舱侧向振动(已滤波)","yc_hs_0064","cur_38"]
[2298,"j_芮城一期Ⅱ-031 机舱角度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-031 机舱角度","yc_hs_0065","cur_41"]
[2299,"j_芮城一期Ⅱ-031 机舱中轴线与风向夹角","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-031 机舱中轴线与风向夹角","yc_hs_0064","cur_03"]
[2300,"j_芮城一期Ⅱ-031 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-031 机舱轴向振动(已滤波)","yc_hs_0064","cur_40"]
[2301,"j_芮城一期Ⅱ-031 扭缆角度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-031 扭缆角度","yc_hs_0064","cur_42"]
[2302,"j_芮城一期Ⅱ-031 主轴承外圈温度","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-031 主轴承外圈温度","yc_hs_0064","cur_31"]
[2303,"j_芮城一期Ⅱ-031 主轴转速","芮城风电场","WOF35900078",31,"SXRC.T1_L2.WTG031.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-031 主轴转速","yc_hs_0064","cur_26"]
[2304,"j_芮城一期Ⅱ-032  1#桨叶片角度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-032  1#桨叶片角度","yc_hs_0064","cur_78"]
[2305,"j_芮城一期Ⅱ-032  2#桨叶片角度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-032  2#桨叶片角度","yc_hs_0064","cur_80"]
[2306,"j_芮城一期Ⅱ-032  3#桨叶片角度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-032  3#桨叶片角度","yc_hs_0064","cur_82"]
[2307,"j_芮城一期Ⅱ-032 舱内温度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-032 舱内温度","yc_hs_0064","cur_71"]
[2308,"j_芮城一期Ⅱ-032 舱外温度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-032 舱外温度","yc_hs_0064","cur_73"]
[2309,"j_芮城一期Ⅱ-032 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-032 齿轮箱高速轴非驱动端轴承温度","yc_hs_0065","cur_03"]
[2310,"j_芮城一期Ⅱ-032 齿轮箱油池温度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-032 齿轮箱油池温度","yc_hs_0065","cur_04"]
[2311,"j_芮城一期Ⅱ-032 发电机定子U相线圈温度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-032 发电机定子U相线圈温度","yc_hs_0064","cur_66"]
[2312,"j_芮城一期Ⅱ-032 发电机定子V相线圈温度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-032 发电机定子V相线圈温度","yc_hs_0065","cur_43"]
[2313,"j_芮城一期Ⅱ-032 发电机定子W相线圈温度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-032 发电机定子W相线圈温度","yc_hs_0065","cur_44"]
[2314,"j_芮城一期Ⅱ-032 发电机非驱动端轴承温度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-032 发电机非驱动端轴承温度","yc_hs_0064","cur_65"]
[2315,"j_芮城一期Ⅱ-032 发电机驱动端轴承温度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-032 发电机驱动端轴承温度","yc_hs_0064","cur_64"]
[2316,"j_芮城一期Ⅱ-032 发电机有功功率","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-032 发电机有功功率","yc_hs_0064","cur_54"]
[2317,"j_芮城一期Ⅱ-032 发电机转速","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-032 发电机转速","yc_hs_0064","cur_63"]
[2318,"j_芮城一期Ⅱ-032 风速","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-032 风速","yc_hs_0064","cur_76"]
[2319,"j_芮城一期Ⅱ-032 风向","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-032 风向","yc_hs_0064","cur_75"]
[2320,"j_芮城一期Ⅱ-032 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-032 机舱侧向振动(已滤波)","yc_hs_0065","cur_12"]
[2321,"j_芮城一期Ⅱ-032 机舱角度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-032 机舱角度","yc_hs_0065","cur_93"]
[2322,"j_芮城一期Ⅱ-032 机舱中轴线与风向夹角","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-032 机舱中轴线与风向夹角","yc_hs_0064","cur_77"]
[2323,"j_芮城一期Ⅱ-032 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-032 机舱轴向振动(已滤波)","yc_hs_0065","cur_14"]
[2324,"j_芮城一期Ⅱ-032 扭缆角度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-032 扭缆角度","yc_hs_0065","cur_16"]
[2325,"j_芮城一期Ⅱ-032 主轴承外圈温度","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-032 主轴承外圈温度","yc_hs_0065","cur_05"]
[2326,"j_芮城一期Ⅱ-032 主轴转速","芮城风电场","WOF35900078",32,"SXRC.T1_L2.WTG032.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-032 主轴转速","yc_hs_0064","cur_100"]
[2327,"j_芮城一期Ⅱ-033  1#桨叶片角度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城一期Ⅱ-033  1#桨叶片角度","yc_hs_0065","cur_52"]
[2328,"j_芮城一期Ⅱ-033  2#桨叶片角度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城一期Ⅱ-033  2#桨叶片角度","yc_hs_0065","cur_54"]
[2329,"j_芮城一期Ⅱ-033  3#桨叶片角度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城一期Ⅱ-033  3#桨叶片角度","yc_hs_0065","cur_56"]
[2330,"j_芮城一期Ⅱ-033 舱内温度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城一期Ⅱ-033 舱内温度","yc_hs_0065","cur_45"]
[2331,"j_芮城一期Ⅱ-033 舱外温度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城一期Ⅱ-033 舱外温度","yc_hs_0065","cur_47"]
[2332,"j_芮城一期Ⅱ-033 齿轮箱高速轴非驱动端轴承温度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","j_芮城一期Ⅱ-033 齿轮箱高速轴非驱动端轴承温度","yc_hs_0065","cur_77"]
[2333,"j_芮城一期Ⅱ-033 齿轮箱油池温度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","j_芮城一期Ⅱ-033 齿轮箱油池温度","yc_hs_0065","cur_78"]
[2334,"j_芮城一期Ⅱ-033 发电机定子U相线圈温度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","j_芮城一期Ⅱ-033 发电机定子U相线圈温度","yc_hs_0065","cur_40"]
[2335,"j_芮城一期Ⅱ-033 发电机定子V相线圈温度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","j_芮城一期Ⅱ-033 发电机定子V相线圈温度","yc_hs_0065","cur_96"]
[2336,"j_芮城一期Ⅱ-033 发电机定子W相线圈温度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","j_芮城一期Ⅱ-033 发电机定子W相线圈温度","yc_hs_0065","cur_97"]
[2337,"j_芮城一期Ⅱ-033 发电机非驱动端轴承温度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","j_芮城一期Ⅱ-033 发电机非驱动端轴承温度","yc_hs_0065","cur_39"]
[2338,"j_芮城一期Ⅱ-033 发电机驱动端轴承温度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","j_芮城一期Ⅱ-033 发电机驱动端轴承温度","yc_hs_0065","cur_38"]
[2339,"j_芮城一期Ⅱ-033 发电机有功功率","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WGEN.GenActivePW","有功功率","active_power","j_芮城一期Ⅱ-033 发电机有功功率","yc_hs_0065","cur_28"]
[2340,"j_芮城一期Ⅱ-033 发电机转速","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WGEN.GenSpd","发电机转速","generator_speed","j_芮城一期Ⅱ-033 发电机转速","yc_hs_0065","cur_37"]
[2341,"j_芮城一期Ⅱ-033 风速","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WNAC.WindSpeed","风速","wind_velocity","j_芮城一期Ⅱ-033 风速","yc_hs_0065","cur_50"]
[2342,"j_芮城一期Ⅱ-033 风向","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城一期Ⅱ-033 风向","yc_hs_0065","cur_49"]
[2343,"j_芮城一期Ⅱ-033 机舱侧向振动(已滤波)","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","j_芮城一期Ⅱ-033 机舱侧向振动(已滤波)","yc_hs_0065","cur_86"]
[2344,"j_芮城一期Ⅱ-033 机舱角度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城一期Ⅱ-033 机舱角度","yc_hs_0322","cur_14"]
[2345,"j_芮城一期Ⅱ-033 机舱中轴线与风向夹角","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城一期Ⅱ-033 机舱中轴线与风向夹角","yc_hs_0065","cur_51"]
[2346,"j_芮城一期Ⅱ-033 机舱轴向振动(已滤波)","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","j_芮城一期Ⅱ-033 机舱轴向振动(已滤波)","yc_hs_0065","cur_88"]
[2347,"j_芮城一期Ⅱ-033 扭缆角度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","j_芮城一期Ⅱ-033 扭缆角度","yc_hs_0065","cur_90"]
[2348,"j_芮城一期Ⅱ-033 主轴承外圈温度","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","j_芮城一期Ⅱ-033 主轴承外圈温度","yc_hs_0065","cur_79"]
[2349,"j_芮城一期Ⅱ-033 主轴转速","芮城风电场","WOF35900078",33,"SXRC.T1_L2.WTG033.WTRM.RotorSpd","风轮转速","rotor_speed","j_芮城一期Ⅱ-033 主轴转速","yc_hs_0065","cur_74"]
[2350,"f_盂县一期Ⅱ-027发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-027发电机定子W相线圈温度","yc_hs_0093","cur_60"]
[2351,"f_盂县一期Ⅱ-027发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-027发电机非驱动端轴承温度","yc_hs_0093","cur_56"]
[2352,"f_盂县一期Ⅱ-032机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-032机舱侧向振动(已滤波)","yc_hs_0099","cur_53"]
[2353,"f_盂县一期Ⅱ-031风速","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-031风速","yc_hs_0097","cur_94"]
[2354,"f_盂县一期Ⅱ-031机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-031机舱中轴线与风向夹角","yc_hs_0097","cur_97"]
[2355,"f_盂县一期Ⅱ-031 1#桨叶片角度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-031 1#桨叶片角度","yc_hs_0098","cur_02"]
[2356,"f_盂县一期Ⅱ-031 2#桨叶片角度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-031 2#桨叶片角度","yc_hs_0098","cur_04"]
[2357,"f_盂县一期Ⅰ-007发电机有功功率","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-007发电机有功功率","yc_hs_0072","cur_49"]
[2358,"f_盂县一期Ⅰ-007发电机转速","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-007发电机转速","yc_hs_0072","cur_53"]
[2359,"f_盂县一期Ⅱ-032风向","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-032风向","yc_hs_0098","cur_97"]
[2360,"f_盂县一期Ⅱ-032风速","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-032风速","yc_hs_0098","cur_99"]
[2361,"f_盂县一期Ⅱ-032机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-032机舱中轴线与风向夹角","yc_hs_0099","cur_02"]
[2362,"f_盂县一期Ⅰ-004发电机有功功率","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-004发电机有功功率","yc_hs_0069","cur_34"]
[2363,"f_盂县一期Ⅰ-004发电机转速","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-004发电机转速","yc_hs_0069","cur_38"]
[2364,"f_盂县一期Ⅰ-004发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-004发电机驱动端轴承温度","yc_hs_0069","cur_40"]
[2365,"f_盂县一期Ⅰ-004发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-004发电机非驱动端轴承温度","yc_hs_0069","cur_41"]
[2366,"f_盂县一期Ⅱ-024机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-024机舱侧向振动(已滤波)","yc_hs_0091","cur_13"]
[2367,"f_盂县一期Ⅱ-024机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-024机舱轴向振动(已滤波)","yc_hs_0091","cur_15"]
[2368,"f_盂县一期Ⅱ-024机舱角度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-024机舱角度","yc_hs_0091","cur_16"]
[2369,"f_盂县一期Ⅱ-030扭揽角度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-030扭揽角度","yc_hs_0097","cur_48"]
[2370,"f_盂县一期Ⅰ-008发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-008发电机驱动端轴承温度","yc_hs_0073","cur_60"]
[2371,"f_盂县一期Ⅰ-008发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-008发电机非驱动端轴承温度","yc_hs_0073","cur_61"]
[2372,"f_盂县一期Ⅰ-008发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-008发电机定子U相线圈温度","yc_hs_0073","cur_63"]
[2373,"f_盂县一期Ⅰ-008发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-008发电机定子V相线圈温度","yc_hs_0073","cur_64"]
[2374,"f_盂县一期Ⅰ-008发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-008发电机定子W相线圈温度","yc_hs_0073","cur_65"]
[2375,"f_盂县一期Ⅰ-009主轴转速","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-009主轴转速","yc_hs_0075","cur_20"]
[2376,"f_盂县一期Ⅰ-016齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-016齿轮箱中速轴非驱动端轴承温度","yc_hs_0083","cur_21"]
[2377,"f_盂县一期Ⅱ-018发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-018发电机驱动端轴承温度","yc_hs_0084","cur_10"]
[2378,"f_盂县一期Ⅱ-018发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-018发电机非驱动端轴承温度","yc_hs_0084","cur_11"]
[2379,"f_盂县一期Ⅱ-018发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-018发电机定子U相线圈温度","yc_hs_0084","cur_13"]
[2380,"f_盂县一期Ⅱ-031齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-031齿轮箱高速轴非驱动端轴承温度","yc_hs_0098","cur_34"]
[2381,"f_盂县一期Ⅱ-031齿轮箱油池温度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-031齿轮箱油池温度","yc_hs_0098","cur_35"]
[2382,"f_盂县一期Ⅱ-031主轴承外圈温度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-031主轴承外圈温度","yc_hs_0098","cur_38"]
[2383,"f_盂县一期Ⅱ-031机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-031机舱侧向振动(已滤波)","yc_hs_0098","cur_48"]
[2384,"f_盂县一期Ⅱ-031机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-031机舱轴向振动(已滤波)","yc_hs_0098","cur_50"]
[2385,"f_盂县一期Ⅱ-031机舱角度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-031机舱角度","yc_hs_0098","cur_51"]
[2386,"f_盂县一期Ⅱ-031扭揽角度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-031扭揽角度","yc_hs_0098","cur_53"]
[2387,"f_盂县一期Ⅱ-033舱内温度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-033舱内温度","yc_hs_0099","cur_97"]
[2388,"f_盂县一期Ⅱ-033舱外温度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-033舱外温度","yc_hs_0099","cur_99"]
[2389,"f_盂县一期Ⅱ-033风向","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-033风向","yc_hs_0100","cur_02"]
[2390,"f_盂县一期Ⅱ-033风速","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-033风速","yc_hs_0100","cur_04"]
[2391,"f_盂县一期Ⅱ-033机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-033机舱中轴线与风向夹角","yc_hs_0100","cur_07"]
[2392,"f_盂县一期Ⅱ-033 1#桨叶片角度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-033 1#桨叶片角度","yc_hs_0100","cur_12"]
[2393,"f_盂县一期Ⅱ-028主轴转速","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-028主轴转速","yc_hs_0095","cur_15"]
[2394,"f_盂县一期Ⅱ-028齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-028齿轮箱高速轴非驱动端轴承温度","yc_hs_0095","cur_19"]
[2395,"f_盂县一期Ⅱ-028齿轮箱油池温度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-028齿轮箱油池温度","yc_hs_0095","cur_20"]
[2396,"f_盂县一期Ⅱ-018发电机有功功率","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-018发电机有功功率","yc_hs_0084","cur_04"]
[2397,"f_盂县一期Ⅱ-019风向","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-019风向","yc_hs_0085","cur_32"]
[2398,"f_盂县一期Ⅱ-019风速","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-019风速","yc_hs_0085","cur_34"]
[2399,"f_盂县一期Ⅰ-001发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-001发电机定子V相线圈温度","yc_hs_0066","cur_29"]
[2400,"f_盂县一期Ⅰ-001发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-001发电机定子W相线圈温度","yc_hs_0066","cur_30"]
[2401,"f_盂县一期Ⅰ-004发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-004发电机定子U相线圈温度","yc_hs_0069","cur_43"]
[2402,"f_盂县一期Ⅰ-004发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-004发电机定子V相线圈温度","yc_hs_0069","cur_44"]
[2403,"f_盂县一期Ⅰ-004发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-004发电机定子W相线圈温度","yc_hs_0069","cur_45"]
[2404,"f_盂县一期Ⅰ-001发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-001发电机定子U相线圈温度","yc_hs_0066","cur_28"]
[2405,"f_盂县一期Ⅰ-017发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-017发电机非驱动端轴承温度","yc_hs_0083","cur_06"]
[2406,"f_盂县一期Ⅱ-021发电机有功功率","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-021发电机有功功率","yc_hs_0087","cur_19"]
[2407,"f_盂县一期Ⅱ-021发电机转速","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-021发电机转速","yc_hs_0087","cur_23"]
[2408,"f_盂县一期Ⅱ-021发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-021发电机驱动端轴承温度","yc_hs_0087","cur_25"]
[2409,"f_盂县一期Ⅱ-021发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-021发电机非驱动端轴承温度","yc_hs_0087","cur_26"]
[2410,"f_盂县一期Ⅱ-021发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-021发电机定子U相线圈温度","yc_hs_0087","cur_28"]
[2411,"f_盂县一期Ⅱ-019主轴转速","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-019主轴转速","yc_hs_0085","cur_70"]
[2412,"f_盂县一期Ⅱ-019齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-019齿轮箱高速轴非驱动端轴承温度","yc_hs_0085","cur_74"]
[2413,"f_盂县一期Ⅱ-019齿轮箱油池温度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-019齿轮箱油池温度","yc_hs_0085","cur_75"]
[2414,"f_盂县一期Ⅱ-019主轴承外圈温度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-019主轴承外圈温度","yc_hs_0085","cur_78"]
[2415,"f_盂县一期Ⅰ-009发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-009发电机定子W相线圈温度","yc_hs_0074","cur_70"]
[2416,"f_盂县一期Ⅰ-009舱内温度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-009舱内温度","yc_hs_0074","cur_77"]
[2417,"f_盂县一期Ⅰ-009舱外温度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-009舱外温度","yc_hs_0074","cur_79"]
[2418,"f_盂县一期Ⅰ-009风向","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-009风向","yc_hs_0074","cur_82"]
[2419,"f_盂县一期Ⅰ-009风速","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-009风速","yc_hs_0074","cur_84"]
[2420,"f_盂县一期Ⅱ-030主轴转速","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-030主轴转速","yc_hs_0097","cur_25"]
[2421,"f_盂县一期Ⅱ-030齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-030齿轮箱高速轴非驱动端轴承温度","yc_hs_0097","cur_29"]
[2422,"f_盂县一期Ⅱ-030齿轮箱油池温度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-030齿轮箱油池温度","yc_hs_0097","cur_30"]
[2423,"f_盂县一期Ⅱ-030主轴承外圈温度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-030主轴承外圈温度","yc_hs_0097","cur_33"]
[2424,"f_盂县一期Ⅰ-013机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-013机舱中轴线与风向夹角","yc_hs_0079","cur_07"]
[2425,"f_盂县一期Ⅰ-013 1#桨叶片角度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-013 1#桨叶片角度","yc_hs_0079","cur_12"]
[2426,"f_盂县一期Ⅰ-017齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-017齿轮箱高速轴非驱动端轴承温度","yc_hs_0083","cur_64"]
[2427,"f_盂县一期Ⅰ-017齿轮箱油池温度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-017齿轮箱油池温度","yc_hs_0083","cur_65"]
[2428,"f_盂县一期Ⅰ-002机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-002机舱侧向振动(已滤波)","yc_hs_0068","cur_03"]
[2429,"f_盂县一期Ⅰ-001机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-001机舱侧向振动(已滤波)","yc_hs_0066","cur_98"]
[2430,"f_盂县一期Ⅰ-001机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-001机舱轴向振动(已滤波)","yc_hs_0066","cur_100"]
[2431,"f_盂县一期Ⅱ-031舱外温度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-031舱外温度","yc_hs_0097","cur_89"]
[2432,"f_盂县一期Ⅱ-031风向","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-031风向","yc_hs_0097","cur_92"]
[2433,"f_盂县一期Ⅰ-017机舱角度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-017机舱角度","yc_hs_0083","cur_81"]
[2434,"f_盂县一期Ⅱ-022扭揽角度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-022扭揽角度","yc_hs_0089","cur_08"]
[2435,"f_盂县一期Ⅱ-027机舱角度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-027机舱角度","yc_hs_0094","cur_31"]
[2436,"f_盂县一期Ⅱ-024发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-024发电机定子U相线圈温度","yc_hs_0090","cur_43"]
[2437,"f_盂县一期Ⅱ-024发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-024发电机定子V相线圈温度","yc_hs_0090","cur_44"]
[2438,"f_盂县一期Ⅱ-024发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-024发电机定子W相线圈温度","yc_hs_0090","cur_45"]
[2439,"f_盂县一期Ⅱ-023发电机转速","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-023发电机转速","yc_hs_0089","cur_33"]
[2440,"f_盂县一期Ⅱ-021主轴转速","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-021主轴转速","yc_hs_0087","cur_80"]
[2441,"f_盂县一期Ⅱ-021齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-021齿轮箱高速轴非驱动端轴承温度","yc_hs_0087","cur_84"]
[2442,"f_盂县一期Ⅰ-009机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-009机舱中轴线与风向夹角","yc_hs_0074","cur_87"]
[2443,"f_盂县一期Ⅰ-012发电机有功功率","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-012发电机有功功率","yc_hs_0077","cur_74"]
[2444,"f_盂县一期Ⅰ-012发电机转速","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-012发电机转速","yc_hs_0077","cur_78"]
[2445,"f_盂县一期Ⅰ-012发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-012发电机驱动端轴承温度","yc_hs_0077","cur_80"]
[2446,"f_盂县一期Ⅰ-012发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-012发电机非驱动端轴承温度","yc_hs_0077","cur_81"]
[2447,"f_盂县一期Ⅰ-012发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-012发电机定子U相线圈温度","yc_hs_0077","cur_83"]
[2448,"f_盂县一期Ⅰ-012发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-012发电机定子V相线圈温度","yc_hs_0077","cur_84"]
[2449,"f_盂县一期Ⅰ-012发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-012发电机定子W相线圈温度","yc_hs_0077","cur_85"]
[2450,"f_盂县一期Ⅰ-012舱内温度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-012舱内温度","yc_hs_0077","cur_92"]
[2451,"f_盂县一期Ⅰ-015扭揽角度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-015扭揽角度","yc_hs_0081","cur_73"]
[2452,"f_盂县一期Ⅱ-032 1#桨叶片角度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-032 1#桨叶片角度","yc_hs_0099","cur_07"]
[2453,"f_盂县一期Ⅱ-032 2#桨叶片角度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-032 2#桨叶片角度","yc_hs_0099","cur_09"]
[2454,"f_盂县一期Ⅱ-032 3#桨叶片角度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-032 3#桨叶片角度","yc_hs_0099","cur_11"]
[2455,"f_盂县一期Ⅰ-014发电机有功功率","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-014发电机有功功率","yc_hs_0079","cur_84"]
[2456,"f_盂县一期Ⅰ-014发电机转速","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-014发电机转速","yc_hs_0079","cur_88"]
[2457,"f_盂县一期Ⅰ-014发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-014发电机驱动端轴承温度","yc_hs_0079","cur_90"]
[2458,"f_盂县一期Ⅰ-014发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-014发电机非驱动端轴承温度","yc_hs_0079","cur_91"]
[2459,"f_盂县一期Ⅰ-014发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-014发电机定子U相线圈温度","yc_hs_0079","cur_93"]
[2460,"f_盂县一期Ⅰ-014发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-014发电机定子V相线圈温度","yc_hs_0079","cur_94"]
[2461,"f_盂县一期Ⅰ-014发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-014发电机定子W相线圈温度","yc_hs_0079","cur_95"]
[2462,"f_盂县一期Ⅰ-014舱内温度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-014舱内温度","yc_hs_0080","cur_02"]
[2463,"f_盂县一期Ⅰ-014舱外温度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-014舱外温度","yc_hs_0080","cur_04"]
[2464,"f_盂县一期Ⅰ-014风向","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-014风向","yc_hs_0080","cur_07"]
[2465,"f_盂县一期Ⅰ-014风速","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-014风速","yc_hs_0080","cur_09"]
[2466,"f_盂县一期Ⅰ-014机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-014机舱中轴线与风向夹角","yc_hs_0080","cur_12"]
[2467,"f_盂县一期Ⅰ-014 1#桨叶片角度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-014 1#桨叶片角度","yc_hs_0080","cur_17"]
[2468,"f_盂县一期Ⅱ-025风速","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-025风速","yc_hs_0091","cur_64"]
[2469,"f_盂县一期Ⅱ-025机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-025机舱中轴线与风向夹角","yc_hs_0091","cur_67"]
[2470,"f_盂县一期Ⅰ-008舱内温度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-008舱内温度","yc_hs_0073","cur_72"]
[2471,"f_盂县一期Ⅰ-008舱外温度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-008舱外温度","yc_hs_0073","cur_74"]
[2472,"f_盂县一期Ⅰ-008风向","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-008风向","yc_hs_0073","cur_77"]
[2473,"f_盂县一期Ⅰ-008风速","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-008风速","yc_hs_0073","cur_79"]
[2474,"f_盂县一期Ⅰ-008机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-008机舱中轴线与风向夹角","yc_hs_0073","cur_82"]
[2475,"f_盂县一期Ⅰ-008 1#桨叶片角度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-008 1#桨叶片角度","yc_hs_0073","cur_87"]
[2476,"f_盂县一期Ⅰ-008 2#桨叶片角度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-008 2#桨叶片角度","yc_hs_0073","cur_89"]
[2477,"f_盂县一期Ⅰ-008 3#桨叶片角度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-008 3#桨叶片角度","yc_hs_0073","cur_91"]
[2478,"f_盂县一期Ⅱ-028齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-028齿轮箱中速轴非驱动端轴承温度","yc_hs_0095","cur_81"]
[2479,"f_盂县一期Ⅱ-032齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-032齿轮箱中速轴非驱动端轴承温度","yc_hs_0100","cur_01"]
[2480,"f_盂县一期Ⅰ-009机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-009机舱侧向振动(已滤波)","yc_hs_0075","cur_38"]
[2481,"f_盂县一期Ⅰ-009机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-009机舱轴向振动(已滤波)","yc_hs_0075","cur_40"]
[2482,"f_盂县一期Ⅰ-009机舱角度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-009机舱角度","yc_hs_0075","cur_41"]
[2483,"f_盂县一期Ⅰ-009扭揽角度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-009扭揽角度","yc_hs_0075","cur_43"]
[2484,"f_盂县一期Ⅰ-002主轴转速","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-002主轴转速","yc_hs_0067","cur_85"]
[2485,"f_盂县一期Ⅰ-002齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-002齿轮箱高速轴非驱动端轴承温度","yc_hs_0067","cur_89"]
[2486,"f_盂县一期Ⅰ-002齿轮箱油池温度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-002齿轮箱油池温度","yc_hs_0067","cur_90"]
[2487,"f_盂县一期Ⅰ-002主轴承外圈温度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-002主轴承外圈温度","yc_hs_0067","cur_93"]
[2488,"f_盂县一期Ⅰ-012主轴转速","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-012主轴转速","yc_hs_0078","cur_35"]
[2489,"f_盂县一期Ⅰ-012齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-012齿轮箱高速轴非驱动端轴承温度","yc_hs_0078","cur_39"]
[2490,"f_盂县一期Ⅰ-012齿轮箱油池温度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-012齿轮箱油池温度","yc_hs_0078","cur_40"]
[2491,"f_盂县一期Ⅰ-012主轴承外圈温度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-012主轴承外圈温度","yc_hs_0078","cur_43"]
[2492,"f_盂县一期Ⅰ-012机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-012机舱侧向振动(已滤波)","yc_hs_0078","cur_53"]
[2493,"f_盂县一期Ⅱ-019机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-019机舱中轴线与风向夹角","yc_hs_0085","cur_37"]
[2494,"f_盂县一期Ⅱ-019 1#桨叶片角度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-019 1#桨叶片角度","yc_hs_0085","cur_42"]
[2495,"f_盂县一期Ⅱ-032主轴转速","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-032主轴转速","yc_hs_0099","cur_35"]
[2496,"f_盂县一期Ⅱ-032齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-032齿轮箱高速轴非驱动端轴承温度","yc_hs_0099","cur_39"]
[2497,"f_盂县一期Ⅱ-032齿轮箱油池温度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-032齿轮箱油池温度","yc_hs_0099","cur_40"]
[2498,"f_盂县一期Ⅱ-032主轴承外圈温度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-032主轴承外圈温度","yc_hs_0099","cur_43"]
[2499,"f_盂县一期Ⅰ-004舱内温度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-004舱内温度","yc_hs_0069","cur_52"]
[2500,"f_盂县一期Ⅰ-012 1#桨叶片角度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-012 1#桨叶片角度","yc_hs_0078","cur_07"]
[2501,"f_盂县一期Ⅰ-012 2#桨叶片角度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-012 2#桨叶片角度","yc_hs_0078","cur_09"]
[2502,"f_盂县一期Ⅰ-012 3#桨叶片角度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-012 3#桨叶片角度","yc_hs_0078","cur_11"]
[2503,"f_盂县一期Ⅱ-030发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-030发电机非驱动端轴承温度","yc_hs_0096","cur_71"]
[2504,"f_盂县一期Ⅱ-019机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-019机舱侧向振动(已滤波)","yc_hs_0085","cur_88"]
[2505,"f_盂县一期Ⅱ-019机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-019机舱轴向振动(已滤波)","yc_hs_0085","cur_90"]
[2506,"f_盂县一期Ⅱ-019机舱角度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-019机舱角度","yc_hs_0085","cur_91"]
[2507,"f_盂县一期Ⅱ-019扭揽角度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-019扭揽角度","yc_hs_0085","cur_93"]
[2508,"f_盂县一期Ⅱ-032机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-032机舱轴向振动(已滤波)","yc_hs_0099","cur_55"]
[2509,"f_盂县一期Ⅱ-020齿轮箱油池温度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-020齿轮箱油池温度","yc_hs_0086","cur_80"]
[2510,"f_盂县一期Ⅱ-020主轴承外圈温度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-020主轴承外圈温度","yc_hs_0086","cur_83"]
[2511,"f_盂县一期Ⅱ-023主轴转速","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-023主轴转速","yc_hs_0089","cur_90"]
[2512,"f_盂县一期Ⅱ-023齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-023齿轮箱高速轴非驱动端轴承温度","yc_hs_0089","cur_94"]
[2513,"f_盂县一期Ⅱ-023齿轮箱油池温度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-023齿轮箱油池温度","yc_hs_0089","cur_95"]
[2514,"f_盂县一期Ⅱ-023主轴承外圈温度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-023主轴承外圈温度","yc_hs_0089","cur_98"]
[2515,"f_盂县一期Ⅱ-020机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-020机舱中轴线与风向夹角","yc_hs_0086","cur_42"]
[2516,"f_盂县一期Ⅱ-020 1#桨叶片角度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-020 1#桨叶片角度","yc_hs_0086","cur_47"]
[2517,"f_盂县一期Ⅱ-031 3#桨叶片角度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-031 3#桨叶片角度","yc_hs_0098","cur_06"]
[2518,"f_盂县一期Ⅱ-025主轴转速","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-025主轴转速","yc_hs_0091","cur_100"]
[2519,"f_盂县一期Ⅱ-024发电机有功功率","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-024发电机有功功率","yc_hs_0090","cur_34"]
[2520,"f_盂县一期Ⅱ-024发电机转速","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-024发电机转速","yc_hs_0090","cur_38"]
[2521,"f_盂县一期Ⅱ-024发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-024发电机驱动端轴承温度","yc_hs_0090","cur_40"]
[2522,"f_盂县一期Ⅱ-024发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-024发电机非驱动端轴承温度","yc_hs_0090","cur_41"]
[2523,"f_盂县一期Ⅱ-030机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-030机舱侧向振动(已滤波)","yc_hs_0097","cur_43"]
[2524,"f_盂县一期Ⅰ-007舱外温度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-007舱外温度","yc_hs_0072","cur_69"]
[2525,"f_盂县一期Ⅰ-007风向","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-007风向","yc_hs_0072","cur_72"]
[2526,"f_盂县一期Ⅱ-019 2#桨叶片角度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-019 2#桨叶片角度","yc_hs_0085","cur_44"]
[2527,"f_盂县一期Ⅱ-019 3#桨叶片角度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-019 3#桨叶片角度","yc_hs_0085","cur_46"]
[2528,"f_盂县一期Ⅰ-013 3#桨叶片角度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-013 3#桨叶片角度","yc_hs_0079","cur_16"]
[2529,"f_盂县一期Ⅱ-019发电机有功功率","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-019发电机有功功率","yc_hs_0085","cur_09"]
[2530,"f_盂县一期Ⅱ-019发电机转速","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-019发电机转速","yc_hs_0085","cur_13"]
[2531,"f_盂县一期Ⅱ-019发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-019发电机驱动端轴承温度","yc_hs_0085","cur_15"]
[2532,"f_盂县一期Ⅱ-019发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-019发电机非驱动端轴承温度","yc_hs_0085","cur_16"]
[2533,"f_盂县一期Ⅱ-019发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-019发电机定子U相线圈温度","yc_hs_0085","cur_18"]
[2534,"f_盂县一期Ⅱ-019发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-019发电机定子V相线圈温度","yc_hs_0085","cur_19"]
[2535,"f_盂县一期Ⅱ-019发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-019发电机定子W相线圈温度","yc_hs_0085","cur_20"]
[2536,"f_盂县一期Ⅱ-018发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-018发电机定子V相线圈温度","yc_hs_0084","cur_14"]
[2537,"f_盂县一期Ⅱ-018发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-018发电机定子W相线圈温度","yc_hs_0084","cur_15"]
[2538,"f_盂县一期Ⅰ-005机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-005机舱侧向振动(已滤波)","yc_hs_0071","cur_18"]
[2539,"f_盂县一期Ⅰ-005机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-005机舱轴向振动(已滤波)","yc_hs_0071","cur_20"]
[2540,"f_盂县一期Ⅰ-005机舱角度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-005机舱角度","yc_hs_0071","cur_21"]
[2541,"f_盂县一期Ⅰ-005扭揽角度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-005扭揽角度","yc_hs_0071","cur_23"]
[2542,"f_盂县一期Ⅱ-021齿轮箱油池温度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-021齿轮箱油池温度","yc_hs_0087","cur_85"]
[2543,"f_盂县一期Ⅱ-021主轴承外圈温度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-021主轴承外圈温度","yc_hs_0087","cur_88"]
[2544,"f_盂县一期Ⅱ-024扭揽角度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-024扭揽角度","yc_hs_0091","cur_18"]
[2545,"f_盂县一期Ⅱ-027扭揽角度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-027扭揽角度","yc_hs_0094","cur_33"]
[2546,"f_盂县一期Ⅰ-003齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-003齿轮箱高速轴非驱动端轴承温度","yc_hs_0068","cur_94"]
[2547,"f_盂县一期Ⅰ-004主轴转速","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-004主轴转速","yc_hs_0069","cur_95"]
[2548,"f_盂县一期Ⅰ-004齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-004齿轮箱高速轴非驱动端轴承温度","yc_hs_0069","cur_99"]
[2549,"f_盂县一期Ⅰ-004舱外温度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-004舱外温度","yc_hs_0069","cur_54"]
[2550,"f_盂县一期Ⅰ-004风向","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-004风向","yc_hs_0069","cur_57"]
[2551,"f_盂县一期Ⅰ-004风速","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-004风速","yc_hs_0069","cur_59"]
[2552,"f_盂县一期Ⅰ-004机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-004机舱中轴线与风向夹角","yc_hs_0069","cur_62"]
[2553,"f_盂县一期Ⅱ-030发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-030发电机定子W相线圈温度","yc_hs_0096","cur_75"]
[2554,"f_盂县一期Ⅱ-030舱内温度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-030舱内温度","yc_hs_0096","cur_82"]
[2555,"f_盂县一期Ⅱ-030舱外温度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-030舱外温度","yc_hs_0096","cur_84"]
[2556,"f_盂县一期Ⅱ-030风向","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-030风向","yc_hs_0096","cur_87"]
[2557,"f_盂县一期Ⅱ-030风速","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-030风速","yc_hs_0096","cur_89"]
[2558,"f_盂县一期Ⅱ-026主轴转速","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-026主轴转速","yc_hs_0093","cur_05"]
[2559,"f_盂县一期Ⅱ-025 1#桨叶片角度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-025 1#桨叶片角度","yc_hs_0091","cur_72"]
[2560,"f_盂县一期Ⅱ-025 2#桨叶片角度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-025 2#桨叶片角度","yc_hs_0091","cur_74"]
[2561,"f_盂县一期Ⅱ-032机舱角度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-032机舱角度","yc_hs_0099","cur_56"]
[2562,"f_盂县一期Ⅱ-032扭揽角度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-032扭揽角度","yc_hs_0099","cur_58"]
[2563,"f_盂县一期Ⅱ-030机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-030机舱轴向振动(已滤波)","yc_hs_0097","cur_45"]
[2564,"f_盂县一期Ⅱ-028发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-028发电机定子V相线圈温度","yc_hs_0094","cur_64"]
[2565,"f_盂县一期Ⅰ-010发电机转速","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-010发电机转速","yc_hs_0075","cur_68"]
[2566,"f_盂县一期Ⅰ-010发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-010发电机驱动端轴承温度","yc_hs_0075","cur_70"]
[2567,"f_盂县一期Ⅰ-010发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-010发电机非驱动端轴承温度","yc_hs_0075","cur_71"]
[2568,"f_盂县一期Ⅰ-010发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-010发电机定子U相线圈温度","yc_hs_0075","cur_73"]
[2569,"f_盂县一期Ⅰ-012齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-012齿轮箱中速轴非驱动端轴承温度","yc_hs_0079","cur_01"]
[2570,"f_盂县一期Ⅱ-021机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-021机舱侧向振动(已滤波)","yc_hs_0087","cur_98"]
[2571,"f_盂县一期Ⅱ-021机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-021机舱轴向振动(已滤波)","yc_hs_0087","cur_100"]
[2572,"f_盂县一期Ⅱ-021机舱角度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-021机舱角度","yc_hs_0088","cur_01"]
[2573,"f_盂县一期Ⅱ-021扭揽角度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-021扭揽角度","yc_hs_0088","cur_03"]
[2574,"f_盂县一期Ⅱ-022发电机有功功率","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-022发电机有功功率","yc_hs_0088","cur_24"]
[2575,"f_盂县一期Ⅱ-022发电机转速","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-022发电机转速","yc_hs_0088","cur_28"]
[2576,"f_盂县一期Ⅰ-015 2#桨叶片角度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-015 2#桨叶片角度","yc_hs_0081","cur_24"]
[2577,"f_盂县一期Ⅰ-017发电机有功功率","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-017发电机有功功率","yc_hs_0082","cur_99"]
[2578,"f_盂县一期Ⅰ-011 3#桨叶片角度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-011 3#桨叶片角度","yc_hs_0077","cur_06"]
[2579,"f_盂县一期Ⅱ-020机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-020机舱侧向振动(已滤波)","yc_hs_0086","cur_93"]
[2580,"f_盂县一期Ⅱ-020机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-020机舱轴向振动(已滤波)","yc_hs_0086","cur_95"]
[2581,"f_盂县一期Ⅱ-020机舱角度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-020机舱角度","yc_hs_0086","cur_96"]
[2582,"f_盂县一期Ⅱ-020扭揽角度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-020扭揽角度","yc_hs_0086","cur_98"]
[2583,"f_盂县一期Ⅱ-025发电机有功功率","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-025发电机有功功率","yc_hs_0091","cur_39"]
[2584,"f_盂县一期Ⅱ-025发电机转速","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-025发电机转速","yc_hs_0091","cur_43"]
[2585,"f_盂县一期Ⅱ-025发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-025发电机驱动端轴承温度","yc_hs_0091","cur_45"]
[2586,"f_盂县一期Ⅱ-025发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-025发电机非驱动端轴承温度","yc_hs_0091","cur_46"]
[2587,"f_盂县一期Ⅱ-025发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-025发电机定子U相线圈温度","yc_hs_0091","cur_48"]
[2588,"f_盂县一期Ⅱ-025发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-025发电机定子V相线圈温度","yc_hs_0091","cur_49"]
[2589,"f_盂县一期Ⅱ-025发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-025发电机定子W相线圈温度","yc_hs_0091","cur_50"]
[2590,"f_盂县一期Ⅱ-025舱内温度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-025舱内温度","yc_hs_0091","cur_57"]
[2591,"f_盂县一期Ⅰ-005风速","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-005风速","yc_hs_0070","cur_64"]
[2592,"f_盂县一期Ⅰ-005机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-005机舱中轴线与风向夹角","yc_hs_0070","cur_67"]
[2593,"f_盂县一期Ⅰ-005 1#桨叶片角度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-005 1#桨叶片角度","yc_hs_0070","cur_72"]
[2594,"f_盂县一期Ⅱ-019舱内温度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-019舱内温度","yc_hs_0085","cur_27"]
[2595,"f_盂县一期Ⅱ-027发电机有功功率","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-027发电机有功功率","yc_hs_0093","cur_49"]
[2596,"f_盂县一期Ⅱ-025 3#桨叶片角度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-025 3#桨叶片角度","yc_hs_0091","cur_76"]
[2597,"f_盂县一期Ⅰ-010发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-010发电机定子V相线圈温度","yc_hs_0075","cur_74"]
[2598,"f_盂县一期Ⅰ-010发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-010发电机定子W相线圈温度","yc_hs_0075","cur_75"]
[2599,"f_盂县一期Ⅰ-010舱内温度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-010舱内温度","yc_hs_0075","cur_82"]
[2600,"f_盂县一期Ⅰ-010舱外温度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-010舱外温度","yc_hs_0075","cur_84"]
[2601,"f_盂县一期Ⅰ-010风向","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-010风向","yc_hs_0075","cur_87"]
[2602,"f_盂县一期Ⅰ-010风速","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-010风速","yc_hs_0075","cur_89"]
[2603,"f_盂县一期Ⅰ-010机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-010机舱中轴线与风向夹角","yc_hs_0075","cur_92"]
[2604,"f_盂县一期Ⅰ-010 1#桨叶片角度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-010 1#桨叶片角度","yc_hs_0075","cur_97"]
[2605,"f_盂县一期Ⅰ-010 2#桨叶片角度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-010 2#桨叶片角度","yc_hs_0075","cur_99"]
[2606,"f_盂县一期Ⅰ-010 3#桨叶片角度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-010 3#桨叶片角度","yc_hs_0076","cur_01"]
[2607,"f_盂县一期Ⅰ-017扭缆角度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-017扭缆角度","yc_hs_0083","cur_83"]
[2608,"f_盂县一期Ⅰ-015发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-015发电机驱动端轴承温度","yc_hs_0080","cur_95"]
[2609,"f_盂县一期Ⅰ-015发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-015发电机非驱动端轴承温度","yc_hs_0080","cur_96"]
[2610,"f_盂县一期Ⅱ-025齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-025齿轮箱高速轴非驱动端轴承温度","yc_hs_0092","cur_04"]
[2611,"f_盂县一期Ⅱ-025齿轮箱油池温度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-025齿轮箱油池温度","yc_hs_0092","cur_05"]
[2612,"f_盂县一期Ⅱ-025主轴承外圈温度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-025主轴承外圈温度","yc_hs_0092","cur_08"]
[2613,"f_盂县一期Ⅱ-025机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-025机舱侧向振动(已滤波)","yc_hs_0092","cur_18"]
[2614,"f_盂县一期Ⅱ-025机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-025机舱轴向振动(已滤波)","yc_hs_0092","cur_20"]
[2615,"f_盂县一期Ⅱ-025机舱角度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-025机舱角度","yc_hs_0092","cur_21"]
[2616,"f_盂县一期Ⅱ-025扭揽角度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-025扭揽角度","yc_hs_0092","cur_23"]
[2617,"f_盂县一期Ⅱ-027舱内温度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-027舱内温度","yc_hs_0093","cur_67"]
[2618,"f_盂县一期Ⅱ-027舱外温度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-027舱外温度","yc_hs_0093","cur_69"]
[2619,"f_盂县一期Ⅱ-027风向","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-027风向","yc_hs_0093","cur_72"]
[2620,"f_盂县一期Ⅱ-027风速","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-027风速","yc_hs_0093","cur_74"]
[2621,"f_盂县一期Ⅰ-001齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-001齿轮箱中速轴非驱动端轴承温度","yc_hs_0067","cur_46"]
[2622,"f_盂县一期Ⅰ-001主轴承外圈温度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-001主轴承外圈温度","yc_hs_0066","cur_88"]
[2623,"f_盂县一期Ⅰ-001主轴转速","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-001主轴转速","yc_hs_0066","cur_80"]
[2624,"f_盂县一期Ⅰ-001齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-001齿轮箱高速轴非驱动端轴承温度","yc_hs_0066","cur_84"]
[2625,"f_盂县一期Ⅰ-001齿轮箱油池温度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-001齿轮箱油池温度","yc_hs_0066","cur_85"]
[2626,"f_盂县一期Ⅰ-001发电机转速","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-001发电机转速","yc_hs_0066","cur_23"]
[2627,"f_盂县一期Ⅰ-001发电机有功功率","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-001发电机有功功率","yc_hs_0066","cur_19"]
[2628,"f_盂县一期Ⅱ-024齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-024齿轮箱高速轴非驱动端轴承温度","yc_hs_0090","cur_99"]
[2629,"f_盂县一期Ⅱ-024齿轮箱油池温度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-024齿轮箱油池温度","yc_hs_0090","cur_100"]
[2630,"f_盂县一期Ⅱ-024主轴承外圈温度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-024主轴承外圈温度","yc_hs_0091","cur_03"]
[2631,"f_盂县一期Ⅱ-026发电机有功功率","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-026发电机有功功率","yc_hs_0092","cur_44"]
[2632,"f_盂县一期Ⅱ-026发电机转速","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-026发电机转速","yc_hs_0092","cur_48"]
[2633,"f_盂县一期Ⅱ-026发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-026发电机驱动端轴承温度","yc_hs_0092","cur_50"]
[2634,"f_盂县一期Ⅱ-026发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-026发电机非驱动端轴承温度","yc_hs_0092","cur_51"]
[2635,"f_盂县一期Ⅱ-026发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-026发电机定子U相线圈温度","yc_hs_0092","cur_53"]
[2636,"f_盂县一期Ⅱ-026发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-026发电机定子V相线圈温度","yc_hs_0092","cur_54"]
[2637,"f_盂县一期Ⅱ-026发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-026发电机定子W相线圈温度","yc_hs_0092","cur_55"]
[2638,"f_盂县一期Ⅱ-026舱内温度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-026舱内温度","yc_hs_0092","cur_62"]
[2639,"f_盂县一期Ⅱ-026舱外温度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-026舱外温度","yc_hs_0092","cur_64"]
[2640,"f_盂县一期Ⅱ-026风向","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-026风向","yc_hs_0092","cur_67"]
[2641,"f_盂县一期Ⅱ-026风速","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-026风速","yc_hs_0092","cur_69"]
[2642,"f_盂县一期Ⅱ-026机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-026机舱中轴线与风向夹角","yc_hs_0092","cur_72"]
[2643,"f_盂县一期Ⅱ-026 1#桨叶片角度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-026 1#桨叶片角度","yc_hs_0092","cur_77"]
[2644,"f_盂县一期Ⅰ-008主轴转速","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-008主轴转速","yc_hs_0074","cur_15"]
[2645,"f_盂县一期Ⅱ-029舱外温度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-029舱外温度","yc_hs_0095","cur_79"]
[2646,"f_盂县一期Ⅱ-029风向","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-029风向","yc_hs_0095","cur_82"]
[2647,"f_盂县一期Ⅱ-029风速","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-029风速","yc_hs_0095","cur_84"]
[2648,"f_盂县一期Ⅱ-029机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-029机舱中轴线与风向夹角","yc_hs_0095","cur_87"]
[2649,"f_盂县一期Ⅱ-029 1#桨叶片角度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-029 1#桨叶片角度","yc_hs_0095","cur_92"]
[2650,"f_盂县一期Ⅱ-029 2#桨叶片角度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-029 2#桨叶片角度","yc_hs_0095","cur_94"]
[2651,"f_盂县一期Ⅱ-029 3#桨叶片角度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-029 3#桨叶片角度","yc_hs_0095","cur_96"]
[2652,"f_盂县一期Ⅱ-029主轴转速","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-029主轴转速","yc_hs_0096","cur_20"]
[2653,"f_盂县一期Ⅱ-029齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-029齿轮箱高速轴非驱动端轴承温度","yc_hs_0096","cur_24"]
[2654,"f_盂县一期Ⅱ-029齿轮箱油池温度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-029齿轮箱油池温度","yc_hs_0096","cur_25"]
[2655,"f_盂县一期Ⅱ-029主轴承外圈温度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-029主轴承外圈温度","yc_hs_0096","cur_28"]
[2656,"f_盂县一期Ⅰ-004齿轮箱油池温度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-004齿轮箱油池温度","yc_hs_0069","cur_100"]
[2657,"f_盂县一期Ⅰ-001机舱角度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-001机舱角度","yc_hs_0067","cur_01"]
[2658,"f_盂县一期Ⅰ-001扭揽角度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-001扭揽角度","yc_hs_0067","cur_03"]
[2659,"f_盂县一期Ⅱ-020舱外温度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-020舱外温度","yc_hs_0086","cur_34"]
[2660,"f_盂县一期Ⅱ-020风向","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-020风向","yc_hs_0086","cur_37"]
[2661,"f_盂县一期Ⅱ-027发电机转速","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-027发电机转速","yc_hs_0093","cur_53"]
[2662,"f_盂县一期Ⅱ-027机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-027机舱中轴线与风向夹角","yc_hs_0093","cur_77"]
[2663,"f_盂县一期Ⅱ-027 1#桨叶片角度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-027 1#桨叶片角度","yc_hs_0093","cur_82"]
[2664,"f_盂县一期Ⅱ-027 2#桨叶片角度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-027 2#桨叶片角度","yc_hs_0093","cur_84"]
[2665,"f_盂县一期Ⅱ-027 3#桨叶片角度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-027 3#桨叶片角度","yc_hs_0093","cur_86"]
[2666,"f_盂县一期Ⅱ-027机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-027机舱轴向振动(已滤波)","yc_hs_0094","cur_30"]
[2667,"f_盂县一期Ⅰ-003齿轮箱油池温度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-003齿轮箱油池温度","yc_hs_0068","cur_95"]
[2668,"f_盂县一期Ⅰ-003主轴承外圈温度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-003主轴承外圈温度","yc_hs_0068","cur_98"]
[2669,"f_盂县一期Ⅱ-031发电机有功功率","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-031发电机有功功率","yc_hs_0097","cur_69"]
[2670,"f_盂县一期Ⅱ-031发电机转速","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-031发电机转速","yc_hs_0097","cur_73"]
[2671,"f_盂县一期Ⅱ-031发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-031发电机驱动端轴承温度","yc_hs_0097","cur_75"]
[2672,"f_盂县一期Ⅱ-031发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-031发电机非驱动端轴承温度","yc_hs_0097","cur_76"]
[2673,"f_盂县一期Ⅱ-031发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-031发电机定子U相线圈温度","yc_hs_0097","cur_78"]
[2674,"f_盂县一期Ⅰ-003机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-003机舱轴向振动(已滤波)","yc_hs_0069","cur_10"]
[2675,"f_盂县一期Ⅰ-003机舱角度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-003机舱角度","yc_hs_0069","cur_11"]
[2676,"f_盂县一期Ⅰ-003扭揽角度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-003扭揽角度","yc_hs_0069","cur_13"]
[2677,"f_盂县一期Ⅰ-002发电机有功功率","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-002发电机有功功率","yc_hs_0067","cur_24"]
[2678,"f_盂县一期Ⅰ-002发电机转速","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-002发电机转速","yc_hs_0067","cur_28"]
[2679,"f_盂县一期Ⅰ-002发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-002发电机驱动端轴承温度","yc_hs_0067","cur_30"]
[2680,"f_盂县一期Ⅰ-002发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-002发电机非驱动端轴承温度","yc_hs_0067","cur_31"]
[2681,"f_盂县一期Ⅰ-002发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-002发电机定子U相线圈温度","yc_hs_0067","cur_33"]
[2682,"f_盂县一期Ⅰ-002发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-002发电机定子V相线圈温度","yc_hs_0067","cur_34"]
[2683,"f_盂县一期Ⅰ-002发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-002发电机定子W相线圈温度","yc_hs_0067","cur_35"]
[2684,"f_盂县一期Ⅰ-002舱内温度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-002舱内温度","yc_hs_0067","cur_42"]
[2685,"f_盂县一期Ⅰ-005齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-005齿轮箱中速轴非驱动端轴承温度","yc_hs_0071","cur_66"]
[2686,"f_盂县一期Ⅰ-008齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-008齿轮箱高速轴非驱动端轴承温度","yc_hs_0074","cur_19"]
[2687,"f_盂县一期Ⅱ-022舱外温度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-022舱外温度","yc_hs_0088","cur_44"]
[2688,"f_盂县一期Ⅱ-022风向","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-022风向","yc_hs_0088","cur_47"]
[2689,"f_盂县一期Ⅱ-022风速","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-022风速","yc_hs_0088","cur_49"]
[2690,"f_盂县一期Ⅱ-022机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-022机舱中轴线与风向夹角","yc_hs_0088","cur_52"]
[2691,"f_盂县一期Ⅱ-022 1#桨叶片角度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-022 1#桨叶片角度","yc_hs_0088","cur_57"]
[2692,"f_盂县一期Ⅰ-016发电机有功功率","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-016发电机有功功率","yc_hs_0081","cur_94"]
[2693,"f_盂县一期Ⅰ-011 2#桨叶片角度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-011 2#桨叶片角度","yc_hs_0077","cur_04"]
[2694,"f_盂县一期Ⅰ-012舱外温度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-012舱外温度","yc_hs_0077","cur_94"]
[2695,"f_盂县一期Ⅰ-012风向","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-012风向","yc_hs_0077","cur_97"]
[2696,"f_盂县一期Ⅰ-012风速","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-012风速","yc_hs_0077","cur_99"]
[2697,"f_盂县一期Ⅰ-006齿轮箱中间轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-006齿轮箱中间轴非驱动端轴承温度","yc_hs_0072","cur_09"]
[2698,"f_盂县一期Ⅰ-006齿轮箱油池温度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-006齿轮箱油池温度","yc_hs_0072","cur_10"]
[2699,"f_盂县一期Ⅰ-006主轴承外圈温度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-006主轴承外圈温度","yc_hs_0072","cur_13"]
[2700,"f_盂县一期Ⅰ-006机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-006机舱侧向振动(已滤波)","yc_hs_0072","cur_23"]
[2701,"f_盂县一期Ⅰ-006机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-006机舱轴向振动(已滤波)","yc_hs_0072","cur_25"]
[2702,"f_盂县一期Ⅰ-013主轴转速","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-013主轴转速","yc_hs_0079","cur_40"]
[2703,"f_盂县一期Ⅰ-017发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-017发电机定子U相线圈温度","yc_hs_0083","cur_08"]
[2704,"f_盂县一期Ⅰ-017发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-017发电机定子W相线圈温度","yc_hs_0083","cur_10"]
[2705,"f_盂县一期Ⅰ-017发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-017发电机定子V相线圈温度","yc_hs_0083","cur_09"]
[2706,"f_盂县一期Ⅰ-001 1#桨叶片角度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-001 1#桨叶片角度","yc_hs_0066","cur_52"]
[2707,"f_盂县一期Ⅰ-001 2#桨叶片角度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-001 2#桨叶片角度","yc_hs_0066","cur_54"]
[2708,"f_盂县一期Ⅰ-001 3#桨叶片角度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-001 3#桨叶片角度","yc_hs_0066","cur_56"]
[2709,"f_盂县一期Ⅰ-011发电机有功功率","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-011发电机有功功率","yc_hs_0076","cur_69"]
[2710,"f_盂县一期Ⅰ-011发电机转速","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-011发电机转速","yc_hs_0076","cur_73"]
[2711,"f_盂县一期Ⅰ-011发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-011发电机驱动端轴承温度","yc_hs_0076","cur_75"]
[2712,"f_盂县一期Ⅰ-011发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-011发电机非驱动端轴承温度","yc_hs_0076","cur_76"]
[2713,"f_盂县一期Ⅰ-011发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-011发电机定子U相线圈温度","yc_hs_0076","cur_78"]
[2714,"f_盂县一期Ⅰ-011发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-011发电机定子V相线圈温度","yc_hs_0076","cur_79"]
[2715,"f_盂县一期Ⅰ-011发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-011发电机定子W相线圈温度","yc_hs_0076","cur_80"]
[2716,"f_盂县一期Ⅰ-011舱内温度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-011舱内温度","yc_hs_0076","cur_87"]
[2717,"f_盂县一期Ⅱ-021发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-021发电机定子V相线圈温度","yc_hs_0087","cur_29"]
[2718,"f_盂县一期Ⅱ-027主轴转速","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-027主轴转速","yc_hs_0094","cur_10"]
[2719,"f_盂县一期Ⅱ-027齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-027齿轮箱高速轴非驱动端轴承温度","yc_hs_0094","cur_14"]
[2720,"f_盂县一期Ⅰ-002舱外温度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-002舱外温度","yc_hs_0067","cur_44"]
[2721,"f_盂县一期Ⅰ-002风向","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-002风向","yc_hs_0067","cur_47"]
[2722,"f_盂县一期Ⅰ-002风速","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-002风速","yc_hs_0067","cur_49"]
[2723,"f_盂县一期Ⅰ-002机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-002机舱中轴线与风向夹角","yc_hs_0067","cur_52"]
[2724,"f_盂县一期Ⅰ-002 1#桨叶片角度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-002 1#桨叶片角度","yc_hs_0067","cur_57"]
[2725,"f_盂县一期Ⅰ-002 2#桨叶片角度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-002 2#桨叶片角度","yc_hs_0067","cur_59"]
[2726,"f_盂县一期Ⅱ-018机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-018机舱中轴线与风向夹角","yc_hs_0084","cur_32"]
[2727,"f_盂县一期Ⅱ-018 1#桨叶片角度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-018 1#桨叶片角度","yc_hs_0084","cur_37"]
[2728,"f_盂县一期Ⅱ-018 2#桨叶片角度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-018 2#桨叶片角度","yc_hs_0084","cur_39"]
[2729,"f_盂县一期Ⅱ-029齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-029齿轮箱中速轴非驱动端轴承温度","yc_hs_0096","cur_86"]
[2730,"f_盂县一期Ⅰ-011主轴转速","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-011主轴转速","yc_hs_0077","cur_30"]
[2731,"f_盂县一期Ⅰ-011齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-011齿轮箱高速轴非驱动端轴承温度","yc_hs_0077","cur_34"]
[2732,"f_盂县一期Ⅰ-011齿轮箱油池温度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-011齿轮箱油池温度","yc_hs_0077","cur_35"]
[2733,"f_盂县一期Ⅰ-011主轴承外圈温度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-011主轴承外圈温度","yc_hs_0077","cur_38"]
[2734,"f_盂县一期Ⅱ-022发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-022发电机驱动端轴承温度","yc_hs_0088","cur_30"]
[2735,"f_盂县一期Ⅰ-013齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-013齿轮箱高速轴非驱动端轴承温度","yc_hs_0079","cur_44"]
[2736,"f_盂县一期Ⅰ-013齿轮箱油池温度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-013齿轮箱油池温度","yc_hs_0079","cur_45"]
[2737,"f_盂县一期Ⅰ-013主轴承外圈温度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-013主轴承外圈温度","yc_hs_0079","cur_48"]
[2738,"f_盂县一期Ⅰ-013机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-013机舱侧向振动(已滤波)","yc_hs_0079","cur_58"]
[2739,"f_盂县一期Ⅰ-013机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-013机舱轴向振动(已滤波)","yc_hs_0079","cur_60"]
[2740,"f_盂县一期Ⅰ-013机舱角度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-013机舱角度","yc_hs_0079","cur_61"]
[2741,"f_盂县一期Ⅰ-013扭揽角度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-013扭揽角度","yc_hs_0079","cur_63"]
[2742,"f_盂县一期Ⅰ-014 2#桨叶片角度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-014 2#桨叶片角度","yc_hs_0080","cur_19"]
[2743,"f_盂县一期Ⅰ-014 3#桨叶片角度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-014 3#桨叶片角度","yc_hs_0080","cur_21"]
[2744,"f_盂县一期Ⅱ-028发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-028发电机驱动端轴承温度","yc_hs_0094","cur_60"]
[2745,"f_盂县一期Ⅱ-028发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-028发电机非驱动端轴承温度","yc_hs_0094","cur_61"]
[2746,"f_盂县一期Ⅱ-028发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-028发电机定子U相线圈温度","yc_hs_0094","cur_63"]
[2747,"f_盂县一期Ⅰ-002 3#桨叶片角度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-002 3#桨叶片角度","yc_hs_0067","cur_61"]
[2748,"f_盂县一期Ⅰ-015齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-015齿轮箱高速轴非驱动端轴承温度","yc_hs_0081","cur_54"]
[2749,"f_盂县一期Ⅰ-015齿轮箱油池温度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-015齿轮箱油池温度","yc_hs_0081","cur_55"]
[2750,"f_盂县一期Ⅰ-015主轴承外圈温度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-015主轴承外圈温度","yc_hs_0081","cur_58"]
[2751,"f_盂县一期Ⅰ-013舱内温度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-013舱内温度","yc_hs_0078","cur_97"]
[2752,"f_盂县一期Ⅰ-013舱外温度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-013舱外温度","yc_hs_0078","cur_99"]
[2753,"f_盂县一期Ⅰ-013风向","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-013风向","yc_hs_0079","cur_02"]
[2754,"f_盂县一期Ⅰ-013风速","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-013风速","yc_hs_0079","cur_04"]
[2755,"f_盂县一期Ⅱ-033 2#桨叶片角度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-033 2#桨叶片角度","yc_hs_0100","cur_14"]
[2756,"f_盂县一期Ⅱ-033 3#桨叶片角度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-033 3#桨叶片角度","yc_hs_0100","cur_16"]
[2757,"f_盂县一期Ⅱ-033主轴转速","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-033主轴转速","yc_hs_0100","cur_40"]
[2758,"f_盂县一期Ⅱ-033齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-033齿轮箱高速轴非驱动端轴承温度","yc_hs_0100","cur_44"]
[2759,"f_盂县一期Ⅱ-033齿轮箱油池温度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-033齿轮箱油池温度","yc_hs_0100","cur_45"]
[2760,"f_盂县一期Ⅱ-033主轴承外圈温度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-033主轴承外圈温度","yc_hs_0100","cur_48"]
[2761,"f_盂县一期Ⅱ-033机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-033机舱侧向振动(已滤波)","yc_hs_0100","cur_58"]
[2762,"f_盂县一期Ⅱ-033机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-033机舱轴向振动(已滤波)","yc_hs_0100","cur_60"]
[2763,"f_盂县一期Ⅰ-006风向","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-006风向","yc_hs_0071","cur_67"]
[2764,"f_盂县一期Ⅰ-015发电机有功功率","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-015发电机有功功率","yc_hs_0080","cur_89"]
[2765,"f_盂县一期Ⅰ-015发电机转速","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-015发电机转速","yc_hs_0080","cur_93"]
[2766,"f_盂县一期Ⅰ-007发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-007发电机驱动端轴承温度","yc_hs_0072","cur_55"]
[2767,"f_盂县一期Ⅰ-007发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-007发电机非驱动端轴承温度","yc_hs_0072","cur_56"]
[2768,"f_盂县一期Ⅰ-007发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-007发电机定子U相线圈温度","yc_hs_0072","cur_58"]
[2769,"f_盂县一期Ⅰ-007发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-007发电机定子V相线圈温度","yc_hs_0072","cur_59"]
[2770,"f_盂县一期Ⅰ-007发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-007发电机定子W相线圈温度","yc_hs_0072","cur_60"]
[2771,"f_盂县一期Ⅱ-018 3#桨叶片角度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-018 3#桨叶片角度","yc_hs_0084","cur_41"]
[2772,"f_盂县一期Ⅱ-018主轴转速","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-018主轴转速","yc_hs_0084","cur_65"]
[2773,"f_盂县一期Ⅱ-018齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-018齿轮箱高速轴非驱动端轴承温度","yc_hs_0084","cur_69"]
[2774,"f_盂县一期Ⅱ-018齿轮箱油池温度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-018齿轮箱油池温度","yc_hs_0084","cur_70"]
[2775,"f_盂县一期Ⅱ-018主轴承外圈温度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-018主轴承外圈温度","yc_hs_0084","cur_73"]
[2776,"f_盂县一期Ⅱ-018机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-018机舱侧向振动(已滤波)","yc_hs_0084","cur_83"]
[2777,"f_盂县一期Ⅱ-018机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-018机舱轴向振动(已滤波)","yc_hs_0084","cur_85"]
[2778,"f_盂县一期Ⅱ-031发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-031发电机定子V相线圈温度","yc_hs_0097","cur_79"]
[2779,"f_盂县一期Ⅱ-031发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-031发电机定子W相线圈温度","yc_hs_0097","cur_80"]
[2780,"f_盂县一期Ⅱ-031舱内温度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-031舱内温度","yc_hs_0097","cur_87"]
[2781,"f_盂县一期Ⅱ-028舱内温度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-028舱内温度","yc_hs_0094","cur_72"]
[2782,"f_盂县一期Ⅱ-030发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-030发电机定子U相线圈温度","yc_hs_0096","cur_73"]
[2783,"f_盂县一期Ⅱ-030发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-030发电机定子V相线圈温度","yc_hs_0096","cur_74"]
[2784,"f_盂县一期Ⅱ-023发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-023发电机驱动端轴承温度","yc_hs_0089","cur_35"]
[2785,"f_盂县一期Ⅱ-023发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-023发电机非驱动端轴承温度","yc_hs_0089","cur_36"]
[2786,"f_盂县一期Ⅱ-023发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-023发电机定子U相线圈温度","yc_hs_0089","cur_38"]
[2787,"f_盂县一期Ⅱ-023发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-023发电机定子V相线圈温度","yc_hs_0089","cur_39"]
[2788,"f_盂县一期Ⅱ-023发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-023发电机定子W相线圈温度","yc_hs_0089","cur_40"]
[2789,"f_盂县一期Ⅱ-021齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-021齿轮箱中速轴非驱动端轴承温度","yc_hs_0088","cur_46"]
[2790,"f_盂县一期Ⅰ-015机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-015机舱侧向振动(已滤波)","yc_hs_0081","cur_68"]
[2791,"f_盂县一期Ⅰ-015机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-015机舱轴向振动(已滤波)","yc_hs_0081","cur_70"]
[2792,"f_盂县一期Ⅰ-015机舱角度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-015机舱角度","yc_hs_0081","cur_71"]
[2793,"f_盂县一期Ⅰ-007机舱角度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-007机舱角度","yc_hs_0073","cur_31"]
[2794,"f_盂县一期Ⅰ-007扭揽角度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-007扭揽角度","yc_hs_0073","cur_33"]
[2795,"f_盂县一期Ⅰ-010机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-010机舱侧向振动(已滤波)","yc_hs_0076","cur_43"]
[2796,"f_盂县一期Ⅰ-010机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-010机舱轴向振动(已滤波)","yc_hs_0076","cur_45"]
[2797,"f_盂县一期Ⅰ-010机舱角度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-010机舱角度","yc_hs_0076","cur_46"]
[2798,"f_盂县一期Ⅰ-010扭揽角度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-010扭揽角度","yc_hs_0076","cur_48"]
[2799,"f_盂县一期Ⅱ-022 2#桨叶片角度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-022 2#桨叶片角度","yc_hs_0088","cur_59"]
[2800,"f_盂县一期Ⅱ-032发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-032发电机定子U相线圈温度","yc_hs_0098","cur_83"]
[2801,"f_盂县一期Ⅱ-032发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-032发电机定子V相线圈温度","yc_hs_0098","cur_84"]
[2802,"f_盂县一期Ⅱ-032发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-032发电机定子W相线圈温度","yc_hs_0098","cur_85"]
[2803,"f_盂县一期Ⅱ-032舱内温度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-032舱内温度","yc_hs_0098","cur_92"]
[2804,"f_盂县一期Ⅱ-032舱外温度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-032舱外温度","yc_hs_0098","cur_94"]
[2805,"f_盂县一期Ⅰ-012机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-012机舱轴向振动(已滤波)","yc_hs_0078","cur_55"]
[2806,"f_盂县一期Ⅰ-012机舱角度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-012机舱角度","yc_hs_0078","cur_56"]
[2807,"f_盂县一期Ⅰ-017舱内温度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-017舱内温度","yc_hs_0083","cur_17"]
[2808,"f_盂县一期Ⅰ-017舱外温度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-017舱外温度","yc_hs_0083","cur_19"]
[2809,"f_盂县一期Ⅰ-017风向","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-017风向","yc_hs_0083","cur_22"]
[2810,"f_盂县一期Ⅰ-017风速","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-017风速","yc_hs_0083","cur_24"]
[2811,"f_盂县一期Ⅰ-007舱内温度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-007舱内温度","yc_hs_0072","cur_67"]
[2812,"f_盂县一期Ⅰ-010齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-010齿轮箱高速轴非驱动端轴承温度","yc_hs_0076","cur_29"]
[2813,"f_盂县一期Ⅰ-010齿轮箱油池温度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-010齿轮箱油池温度","yc_hs_0076","cur_30"]
[2814,"f_盂县一期Ⅱ-028主轴承外圈温度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-028主轴承外圈温度","yc_hs_0095","cur_23"]
[2815,"f_盂县一期Ⅱ-028机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-028机舱侧向振动(已滤波)","yc_hs_0095","cur_33"]
[2816,"f_盂县一期Ⅱ-028机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-028机舱轴向振动(已滤波)","yc_hs_0095","cur_35"]
[2817,"f_盂县一期Ⅱ-028机舱角度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-028机舱角度","yc_hs_0095","cur_36"]
[2818,"f_盂县一期Ⅰ-005发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-005发电机定子V相线圈温度","yc_hs_0070","cur_49"]
[2819,"f_盂县一期Ⅰ-008发电机有功功率","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-008发电机有功功率","yc_hs_0073","cur_54"]
[2820,"f_盂县一期Ⅰ-008发电机转速","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-008发电机转速","yc_hs_0073","cur_58"]
[2821,"f_盂县一期Ⅰ-014扭揽角度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-014扭揽角度","yc_hs_0080","cur_68"]
[2822,"f_盂县一期Ⅰ-005发电机有功功率","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-005发电机有功功率","yc_hs_0070","cur_39"]
[2823,"f_盂县一期Ⅰ-005发电机转速","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-005发电机转速","yc_hs_0070","cur_43"]
[2824,"f_盂县一期Ⅰ-005发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-005发电机驱动端轴承温度","yc_hs_0070","cur_45"]
[2825,"f_盂县一期Ⅰ-005发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-005发电机非驱动端轴承温度","yc_hs_0070","cur_46"]
[2826,"f_盂县一期Ⅰ-005发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-005发电机定子U相线圈温度","yc_hs_0070","cur_48"]
[2827,"f_盂县一期Ⅰ-009齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-009齿轮箱高速轴非驱动端轴承温度","yc_hs_0075","cur_24"]
[2828,"f_盂县一期Ⅱ-023舱内温度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-023舱内温度","yc_hs_0089","cur_47"]
[2829,"f_盂县一期Ⅱ-023舱外温度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-023舱外温度","yc_hs_0089","cur_49"]
[2830,"f_盂县一期Ⅱ-023风向","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-023风向","yc_hs_0089","cur_52"]
[2831,"f_盂县一期Ⅱ-023风速","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-023风速","yc_hs_0089","cur_54"]
[2832,"f_盂县一期Ⅱ-023机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-023机舱中轴线与风向夹角","yc_hs_0089","cur_57"]
[2833,"f_盂县一期Ⅱ-023 1#桨叶片角度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-023 1#桨叶片角度","yc_hs_0089","cur_62"]
[2834,"f_盂县一期Ⅱ-023 2#桨叶片角度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-023 2#桨叶片角度","yc_hs_0089","cur_64"]
[2835,"f_盂县一期Ⅱ-023 3#桨叶片角度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-023 3#桨叶片角度","yc_hs_0089","cur_66"]
[2836,"f_盂县一期Ⅱ-023机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-023机舱侧向振动(已滤波)","yc_hs_0090","cur_08"]
[2837,"f_盂县一期Ⅱ-023机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-023机舱轴向振动(已滤波)","yc_hs_0090","cur_10"]
[2838,"f_盂县一期Ⅱ-023机舱角度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-023机舱角度","yc_hs_0090","cur_11"]
[2839,"f_盂县一期Ⅱ-023扭揽角度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-023扭揽角度","yc_hs_0090","cur_13"]
[2840,"f_盂县一期Ⅱ-020风速","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-020风速","yc_hs_0086","cur_39"]
[2841,"f_盂县一期Ⅱ-032发电机有功功率","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-032发电机有功功率","yc_hs_0098","cur_74"]
[2842,"f_盂县一期Ⅱ-032发电机转速","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-032发电机转速","yc_hs_0098","cur_78"]
[2843,"f_盂县一期Ⅱ-032发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-032发电机驱动端轴承温度","yc_hs_0098","cur_80"]
[2844,"f_盂县一期Ⅱ-032发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",32,"SXYX.T1_L2.WTG032.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-032发电机非驱动端轴承温度","yc_hs_0098","cur_81"]
[2845,"f_盂县一期Ⅰ-011机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-011机舱侧向振动(已滤波)","yc_hs_0077","cur_48"]
[2846,"f_盂县一期Ⅰ-008齿轮箱油池温度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-008齿轮箱油池温度","yc_hs_0074","cur_20"]
[2847,"f_盂县一期Ⅰ-008主轴承外圈温度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-008主轴承外圈温度","yc_hs_0074","cur_23"]
[2848,"f_盂县一期Ⅰ-008机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-008机舱侧向振动(已滤波)","yc_hs_0074","cur_33"]
[2849,"f_盂县一期Ⅰ-008机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-008机舱轴向振动(已滤波)","yc_hs_0074","cur_35"]
[2850,"f_盂县一期Ⅰ-008机舱角度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-008机舱角度","yc_hs_0074","cur_36"]
[2851,"f_盂县一期Ⅰ-008扭揽角度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-008扭揽角度","yc_hs_0074","cur_38"]
[2852,"f_盂县一期Ⅰ-003舱外温度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-003舱外温度","yc_hs_0068","cur_49"]
[2853,"f_盂县一期Ⅰ-015 3#桨叶片角度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-015 3#桨叶片角度","yc_hs_0081","cur_26"]
[2854,"f_盂县一期Ⅱ-028扭揽角度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-028扭揽角度","yc_hs_0095","cur_38"]
[2855,"f_盂县一期Ⅱ-023发电机有功功率","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-023发电机有功功率","yc_hs_0089","cur_29"]
[2856,"f_盂县一期Ⅱ-021舱内温度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-021舱内温度","yc_hs_0087","cur_37"]
[2857,"f_盂县一期Ⅱ-021舱外温度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-021舱外温度","yc_hs_0087","cur_39"]
[2858,"f_盂县一期Ⅱ-021风向","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-021风向","yc_hs_0087","cur_42"]
[2859,"f_盂县一期Ⅱ-021风速","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-021风速","yc_hs_0087","cur_44"]
[2860,"f_盂县一期Ⅱ-021机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-021机舱中轴线与风向夹角","yc_hs_0087","cur_47"]
[2861,"f_盂县一期Ⅰ-003发电机有功功率","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-003发电机有功功率","yc_hs_0068","cur_29"]
[2862,"f_盂县一期Ⅰ-003发电机转速","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-003发电机转速","yc_hs_0068","cur_33"]
[2863,"f_盂县一期Ⅰ-003发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-003发电机驱动端轴承温度","yc_hs_0068","cur_35"]
[2864,"f_盂县一期Ⅰ-003发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-003发电机非驱动端轴承温度","yc_hs_0068","cur_36"]
[2865,"f_盂县一期Ⅰ-003发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-003发电机定子U相线圈温度","yc_hs_0068","cur_38"]
[2866,"f_盂县一期Ⅰ-017机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-017机舱中轴线与风向夹角","yc_hs_0083","cur_27"]
[2867,"f_盂县一期Ⅰ-017 1#桨叶片角度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-017 1#桨叶片角度","yc_hs_0083","cur_32"]
[2868,"f_盂县一期Ⅰ-017 2#桨叶片角度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-017 2#桨叶片角度","yc_hs_0083","cur_34"]
[2869,"f_盂县一期Ⅰ-017 3#桨叶片角度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-017 3#桨叶片角度","yc_hs_0083","cur_36"]
[2870,"f_盂县一期Ⅰ-017主轴转速","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-017主轴转速","yc_hs_0083","cur_60"]
[2871,"f_盂县一期Ⅰ-014齿轮箱油池温度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-014齿轮箱油池温度","yc_hs_0080","cur_50"]
[2872,"f_盂县一期Ⅰ-014主轴承外圈温度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-014主轴承外圈温度","yc_hs_0080","cur_53"]
[2873,"f_盂县一期Ⅱ-022 3#桨叶片角度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-022 3#桨叶片角度","yc_hs_0088","cur_61"]
[2874,"f_盂县一期Ⅱ-028 2#桨叶片角度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-028 2#桨叶片角度","yc_hs_0094","cur_89"]
[2875,"f_盂县一期Ⅱ-018舱内温度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-018舱内温度","yc_hs_0084","cur_22"]
[2876,"f_盂县一期Ⅱ-018舱外温度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-018舱外温度","yc_hs_0084","cur_24"]
[2877,"f_盂县一期Ⅱ-018风向","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-018风向","yc_hs_0084","cur_27"]
[2878,"f_盂县一期Ⅱ-018风速","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-018风速","yc_hs_0084","cur_29"]
[2879,"f_盂县一期Ⅱ-022发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-022发电机定子U相线圈温度","yc_hs_0088","cur_33"]
[2880,"f_盂县一期Ⅱ-022发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-022发电机定子V相线圈温度","yc_hs_0088","cur_34"]
[2881,"f_盂县一期Ⅰ-002机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-002机舱轴向振动(已滤波)","yc_hs_0068","cur_05"]
[2882,"f_盂县一期Ⅰ-002机舱角度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-002机舱角度","yc_hs_0068","cur_06"]
[2883,"f_盂县一期Ⅰ-002扭揽角度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-002扭揽角度","yc_hs_0068","cur_08"]
[2884,"f_盂县一期Ⅰ-009齿轮箱油池温度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-009齿轮箱油池温度","yc_hs_0075","cur_25"]
[2885,"f_盂县一期Ⅰ-009主轴承外圈温度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-009主轴承外圈温度","yc_hs_0075","cur_28"]
[2886,"f_盂县一期Ⅰ-016发电机转速","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-016发电机转速","yc_hs_0081","cur_98"]
[2887,"f_盂县一期Ⅰ-016发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-016发电机驱动端轴承温度","yc_hs_0081","cur_100"]
[2888,"f_盂县一期Ⅰ-016发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-016发电机非驱动端轴承温度","yc_hs_0082","cur_01"]
[2889,"f_盂县一期Ⅰ-016发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-016发电机定子U相线圈温度","yc_hs_0082","cur_03"]
[2890,"f_盂县一期Ⅰ-016发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-016发电机定子V相线圈温度","yc_hs_0082","cur_04"]
[2891,"f_盂县一期Ⅰ-016发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-016发电机定子W相线圈温度","yc_hs_0082","cur_05"]
[2892,"f_盂县一期Ⅰ-016舱内温度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-016舱内温度","yc_hs_0082","cur_12"]
[2893,"f_盂县一期Ⅰ-016舱外温度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-016舱外温度","yc_hs_0082","cur_14"]
[2894,"f_盂县一期Ⅰ-016风向","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-016风向","yc_hs_0082","cur_17"]
[2895,"f_盂县一期Ⅰ-016风速","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-016风速","yc_hs_0082","cur_19"]
[2896,"f_盂县一期Ⅱ-028 3#桨叶片角度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-028 3#桨叶片角度","yc_hs_0094","cur_91"]
[2897,"f_盂县一期Ⅰ-006风速","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-006风速","yc_hs_0071","cur_69"]
[2898,"f_盂县一期Ⅰ-006机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-006机舱中轴线与风向夹角","yc_hs_0071","cur_72"]
[2899,"f_盂县一期Ⅰ-006 1#桨叶片角度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-006 1#桨叶片角度","yc_hs_0071","cur_77"]
[2900,"f_盂县一期Ⅰ-006 2#桨叶片角度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-006 2#桨叶片角度","yc_hs_0071","cur_79"]
[2901,"f_盂县一期Ⅰ-005 3#桨叶片角度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-005 3#桨叶片角度","yc_hs_0070","cur_76"]
[2902,"f_盂县一期Ⅰ-017主轴承外圈温度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-017主轴承外圈温度","yc_hs_0083","cur_68"]
[2903,"f_盂县一期Ⅰ-017机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-017机舱侧向振动(已滤波)","yc_hs_0083","cur_78"]
[2904,"f_盂县一期Ⅰ-011机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-011机舱轴向振动(已滤波)","yc_hs_0077","cur_50"]
[2905,"f_盂县一期Ⅰ-011机舱角度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-011机舱角度","yc_hs_0077","cur_51"]
[2906,"f_盂县一期Ⅰ-011扭揽角度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-011扭揽角度","yc_hs_0077","cur_53"]
[2907,"f_盂县一期Ⅱ-030机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-030机舱中轴线与风向夹角","yc_hs_0096","cur_92"]
[2908,"f_盂县一期Ⅱ-030 1#桨叶片角度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-030 1#桨叶片角度","yc_hs_0096","cur_97"]
[2909,"f_盂县一期Ⅱ-030 2#桨叶片角度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-030 2#桨叶片角度","yc_hs_0096","cur_99"]
[2910,"f_盂县一期Ⅱ-030 3#桨叶片角度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-030 3#桨叶片角度","yc_hs_0097","cur_01"]
[2911,"f_盂县一期Ⅱ-018机舱角度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-018机舱角度","yc_hs_0084","cur_86"]
[2912,"f_盂县一期Ⅱ-018扭揽角度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-018扭揽角度","yc_hs_0084","cur_88"]
[2913,"f_盂县一期Ⅱ-019舱外温度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-019舱外温度","yc_hs_0085","cur_29"]
[2914,"f_盂县一期Ⅱ-028发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-028发电机定子W相线圈温度","yc_hs_0094","cur_65"]
[2915,"f_盂县一期Ⅱ-030机舱角度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-030机舱角度","yc_hs_0097","cur_46"]
[2916,"f_盂县一期Ⅰ-009 1#桨叶片角度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-009 1#桨叶片角度","yc_hs_0074","cur_92"]
[2917,"f_盂县一期Ⅰ-009 2#桨叶片角度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-009 2#桨叶片角度","yc_hs_0074","cur_94"]
[2918,"f_盂县一期Ⅰ-003主轴转速","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-003主轴转速","yc_hs_0068","cur_90"]
[2919,"f_盂县一期Ⅰ-013 2#桨叶片角度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-013 2#桨叶片角度","yc_hs_0079","cur_14"]
[2920,"f_盂县一期Ⅰ-014主轴转速","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-014主轴转速","yc_hs_0080","cur_45"]
[2921,"f_盂县一期Ⅰ-014齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-014齿轮箱高速轴非驱动端轴承温度","yc_hs_0080","cur_49"]
[2922,"f_盂县一期Ⅱ-021 1#桨叶片角度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-021 1#桨叶片角度","yc_hs_0087","cur_52"]
[2923,"f_盂县一期Ⅰ-006发电机有功功率","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-006发电机有功功率","yc_hs_0071","cur_44"]
[2924,"f_盂县一期Ⅰ-006发电机转速","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-006发电机转速","yc_hs_0071","cur_48"]
[2925,"f_盂县一期Ⅰ-006发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-006发电机驱动端轴承温度","yc_hs_0071","cur_50"]
[2926,"f_盂县一期Ⅰ-006发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-006发电机非驱动端轴承温度","yc_hs_0071","cur_51"]
[2927,"f_盂县一期Ⅰ-006发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-006发电机定子U相线圈温度","yc_hs_0071","cur_53"]
[2928,"f_盂县一期Ⅰ-006发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-006发电机定子V相线圈温度","yc_hs_0071","cur_54"]
[2929,"f_盂县一期Ⅰ-006发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-006发电机定子W相线圈温度","yc_hs_0071","cur_55"]
[2930,"f_盂县一期Ⅰ-006舱内温度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-006舱内温度","yc_hs_0071","cur_62"]
[2931,"f_盂县一期Ⅰ-006舱外温度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-006舱外温度","yc_hs_0071","cur_64"]
[2932,"f_盂县一期Ⅰ-001风速","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-001风速","yc_hs_0066","cur_44"]
[2933,"f_盂县一期Ⅰ-012扭揽角度","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-012扭揽角度","yc_hs_0078","cur_58"]
[2934,"f_盂县一期Ⅰ-016主轴转速","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-016主轴转速","yc_hs_0082","cur_55"]
[2935,"f_盂县一期Ⅰ-017机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-017机舱轴向振动(已滤波)","yc_hs_0083","cur_80"]
[2936,"f_盂县一期Ⅱ-022主轴转速","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-022主轴转速","yc_hs_0088","cur_85"]
[2937,"f_盂县一期Ⅱ-022齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-022齿轮箱高速轴非驱动端轴承温度","yc_hs_0088","cur_89"]
[2938,"f_盂县一期Ⅱ-022齿轮箱油池温度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-022齿轮箱油池温度","yc_hs_0088","cur_90"]
[2939,"f_盂县一期Ⅱ-022主轴承外圈温度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-022主轴承外圈温度","yc_hs_0088","cur_93"]
[2940,"f_盂县一期Ⅱ-022机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-022机舱侧向振动(已滤波)","yc_hs_0089","cur_03"]
[2941,"f_盂县一期Ⅱ-022机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-022机舱轴向振动(已滤波)","yc_hs_0089","cur_05"]
[2942,"f_盂县一期Ⅱ-022机舱角度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-022机舱角度","yc_hs_0089","cur_06"]
[2943,"f_盂县一期Ⅱ-025舱外温度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-025舱外温度","yc_hs_0091","cur_59"]
[2944,"f_盂县一期Ⅱ-025风向","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-025风向","yc_hs_0091","cur_62"]
[2945,"f_盂县一期Ⅰ-005 2#桨叶片角度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-005 2#桨叶片角度","yc_hs_0070","cur_74"]
[2946,"f_盂县一期Ⅰ-003风速","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-003风速","yc_hs_0068","cur_54"]
[2947,"f_盂县一期Ⅰ-003机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-003机舱中轴线与风向夹角","yc_hs_0068","cur_57"]
[2948,"f_盂县一期Ⅰ-003 1#桨叶片角度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-003 1#桨叶片角度","yc_hs_0068","cur_62"]
[2949,"f_盂县一期Ⅰ-003 2#桨叶片角度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-003 2#桨叶片角度","yc_hs_0068","cur_64"]
[2950,"f_盂县一期Ⅰ-003 3#桨叶片角度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-003 3#桨叶片角度","yc_hs_0068","cur_66"]
[2951,"f_盂县一期Ⅱ-029发电机有功功率","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-029发电机有功功率","yc_hs_0095","cur_59"]
[2952,"f_盂县一期Ⅱ-029发电机转速","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-029发电机转速","yc_hs_0095","cur_63"]
[2953,"f_盂县一期Ⅱ-029发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-029发电机驱动端轴承温度","yc_hs_0095","cur_65"]
[2954,"f_盂县一期Ⅱ-029发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-029发电机非驱动端轴承温度","yc_hs_0095","cur_66"]
[2955,"f_盂县一期Ⅱ-029发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-029发电机定子U相线圈温度","yc_hs_0095","cur_68"]
[2956,"f_盂县一期Ⅱ-029发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-029发电机定子V相线圈温度","yc_hs_0095","cur_69"]
[2957,"f_盂县一期Ⅱ-029发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-029发电机定子W相线圈温度","yc_hs_0095","cur_70"]
[2958,"f_盂县一期Ⅰ-017发电机转速","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-017发电机转速","yc_hs_0083","cur_03"]
[2959,"f_盂县一期Ⅰ-017发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-017发电机驱动端轴承温度","yc_hs_0083","cur_05"]
[2960,"f_盂县一期Ⅰ-010主轴承外圈温度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-010主轴承外圈温度","yc_hs_0076","cur_33"]
[2961,"f_盂县一期Ⅰ-005主轴转速","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-005主轴转速","yc_hs_0070","cur_100"]
[2962,"f_盂县一期Ⅰ-005齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-005齿轮箱高速轴非驱动端轴承温度","yc_hs_0071","cur_04"]
[2963,"f_盂县一期Ⅰ-005齿轮箱油池温度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-005齿轮箱油池温度","yc_hs_0071","cur_05"]
[2964,"f_盂县一期Ⅰ-005主轴承外圈温度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-005主轴承外圈温度","yc_hs_0071","cur_08"]
[2965,"f_盂县一期Ⅰ-016机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-016机舱轴向振动(已滤波)","yc_hs_0082","cur_75"]
[2966,"f_盂县一期Ⅰ-016机舱角度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-016机舱角度","yc_hs_0082","cur_76"]
[2967,"f_盂县一期Ⅰ-016扭揽角度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-016扭揽角度","yc_hs_0082","cur_78"]
[2968,"f_盂县一期Ⅰ-003发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-003发电机定子V相线圈温度","yc_hs_0068","cur_39"]
[2969,"f_盂县一期Ⅰ-003发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-003发电机定子W相线圈温度","yc_hs_0068","cur_40"]
[2970,"f_盂县一期Ⅰ-006 3#桨叶片角度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-006 3#桨叶片角度","yc_hs_0071","cur_81"]
[2971,"f_盂县一期Ⅰ-006主轴转速","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-006主轴转速","yc_hs_0072","cur_05"]
[2972,"f_盂县一期Ⅱ-020 2#桨叶片角度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-020 2#桨叶片角度","yc_hs_0086","cur_49"]
[2973,"f_盂县一期Ⅱ-020 3#桨叶片角度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-020 3#桨叶片角度","yc_hs_0086","cur_51"]
[2974,"f_盂县一期Ⅱ-020主轴转速","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-020主轴转速","yc_hs_0086","cur_75"]
[2975,"f_盂县一期Ⅱ-020齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-020齿轮箱高速轴非驱动端轴承温度","yc_hs_0086","cur_79"]
[2976,"f_盂县一期Ⅱ-030发电机有功功率","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-030发电机有功功率","yc_hs_0096","cur_64"]
[2977,"f_盂县一期Ⅱ-030发电机转速","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-030发电机转速","yc_hs_0096","cur_68"]
[2978,"f_盂县一期Ⅱ-030发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-030发电机驱动端轴承温度","yc_hs_0096","cur_70"]
[2979,"f_盂县一期Ⅱ-026 2#桨叶片角度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-026 2#桨叶片角度","yc_hs_0092","cur_79"]
[2980,"f_盂县一期Ⅱ-022发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-022发电机定子W相线圈温度","yc_hs_0088","cur_35"]
[2981,"f_盂县一期Ⅱ-022舱内温度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-022舱内温度","yc_hs_0088","cur_42"]
[2982,"f_盂县一期Ⅱ-027发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-027发电机驱动端轴承温度","yc_hs_0093","cur_55"]
[2983,"f_盂县一期Ⅱ-020发电机有功功率","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-020发电机有功功率","yc_hs_0086","cur_14"]
[2984,"f_盂县一期Ⅱ-020发电机转速","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-020发电机转速","yc_hs_0086","cur_18"]
[2985,"f_盂县一期Ⅱ-020发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-020发电机驱动端轴承温度","yc_hs_0086","cur_20"]
[2986,"f_盂县一期Ⅱ-020发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-020发电机非驱动端轴承温度","yc_hs_0086","cur_21"]
[2987,"f_盂县一期Ⅱ-020发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-020发电机定子U相线圈温度","yc_hs_0086","cur_23"]
[2988,"f_盂县一期Ⅱ-020发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-020发电机定子V相线圈温度","yc_hs_0086","cur_24"]
[2989,"f_盂县一期Ⅱ-020发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-020发电机定子W相线圈温度","yc_hs_0086","cur_25"]
[2990,"f_盂县一期Ⅱ-020舱内温度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-020舱内温度","yc_hs_0086","cur_32"]
[2991,"f_盂县一期Ⅰ-016主轴承外圈温度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-016主轴承外圈温度","yc_hs_0082","cur_63"]
[2992,"f_盂县一期Ⅰ-016机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-016机舱侧向振动(已滤波)","yc_hs_0082","cur_73"]
[2993,"f_盂县一期Ⅱ-029机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-029机舱侧向振动(已滤波)","yc_hs_0096","cur_38"]
[2994,"f_盂县一期Ⅱ-029机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-029机舱轴向振动(已滤波)","yc_hs_0096","cur_40"]
[2995,"f_盂县一期Ⅱ-029机舱角度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-029机舱角度","yc_hs_0096","cur_41"]
[2996,"f_盂县一期Ⅱ-029扭揽角度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-029扭揽角度","yc_hs_0096","cur_43"]
[2997,"f_盂县一期Ⅱ-031主轴转速","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-031主轴转速","yc_hs_0098","cur_30"]
[2998,"f_盂县一期Ⅱ-026齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅱ-026齿轮箱高速轴非驱动端轴承温度","yc_hs_0093","cur_09"]
[2999,"f_盂县一期Ⅱ-026齿轮箱油池温度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-026齿轮箱油池温度","yc_hs_0093","cur_10"]
[3000,"f_盂县一期Ⅱ-026主轴承外圈温度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-026主轴承外圈温度","yc_hs_0093","cur_13"]
[3001,"f_盂县一期Ⅱ-026机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-026机舱侧向振动(已滤波)","yc_hs_0093","cur_23"]
[3002,"f_盂县一期Ⅱ-026机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅱ-026机舱轴向振动(已滤波)","yc_hs_0093","cur_25"]
[3003,"f_盂县一期Ⅱ-026机舱角度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-026机舱角度","yc_hs_0093","cur_26"]
[3004,"f_盂县一期Ⅱ-026扭揽角度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-026扭揽角度","yc_hs_0093","cur_28"]
[3005,"f_盂县一期Ⅰ-003机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-003机舱侧向振动(已滤波)","yc_hs_0069","cur_08"]
[3006,"f_盂县一期Ⅰ-016机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-016机舱中轴线与风向夹角","yc_hs_0082","cur_22"]
[3007,"f_盂县一期Ⅰ-016 1#桨叶片角度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-016 1#桨叶片角度","yc_hs_0082","cur_27"]
[3008,"f_盂县一期Ⅰ-016 2#桨叶片角度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-016 2#桨叶片角度","yc_hs_0082","cur_29"]
[3009,"f_盂县一期Ⅰ-016 3#桨叶片角度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-016 3#桨叶片角度","yc_hs_0082","cur_31"]
[3010,"f_盂县一期Ⅰ-003舱内温度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-003舱内温度","yc_hs_0068","cur_47"]
[3011,"f_盂县一期Ⅰ-005发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-005发电机定子W相线圈温度","yc_hs_0070","cur_50"]
[3012,"f_盂县一期Ⅰ-005舱内温度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-005舱内温度","yc_hs_0070","cur_57"]
[3013,"f_盂县一期Ⅰ-005舱外温度","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-005舱外温度","yc_hs_0070","cur_59"]
[3014,"f_盂县一期Ⅰ-005风向","盂县风光互补电站","WOF35800082",5,"SXYX.T1_L1.WTG005.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-005风向","yc_hs_0070","cur_62"]
[3015,"f_盂县一期Ⅱ-018发电机转速","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-018发电机转速","yc_hs_0084","cur_08"]
[3016,"f_盂县一期Ⅰ-003风向","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-003风向","yc_hs_0068","cur_52"]
[3017,"f_盂县一期Ⅰ-014机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-014机舱侧向振动(已滤波)","yc_hs_0080","cur_63"]
[3018,"f_盂县一期Ⅰ-014机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-014机舱轴向振动(已滤波)","yc_hs_0080","cur_65"]
[3019,"f_盂县一期Ⅰ-014机舱角度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-014机舱角度","yc_hs_0080","cur_66"]
[3020,"f_盂县一期Ⅰ-001发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-001发电机驱动端轴承温度","yc_hs_0066","cur_25"]
[3021,"f_盂县一期Ⅰ-001发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-001发电机非驱动端轴承温度","yc_hs_0066","cur_26"]
[3022,"f_盂县一期Ⅱ-021 2#桨叶片角度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-021 2#桨叶片角度","yc_hs_0087","cur_54"]
[3023,"f_盂县一期Ⅱ-028舱外温度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-028舱外温度","yc_hs_0094","cur_74"]
[3024,"f_盂县一期Ⅱ-028风向","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-028风向","yc_hs_0094","cur_77"]
[3025,"f_盂县一期Ⅱ-028风速","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-028风速","yc_hs_0094","cur_79"]
[3026,"f_盂县一期Ⅱ-028机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-028机舱中轴线与风向夹角","yc_hs_0094","cur_82"]
[3027,"f_盂县一期Ⅱ-028 1#桨叶片角度","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-028 1#桨叶片角度","yc_hs_0094","cur_87"]
[3028,"f_盂县一期Ⅰ-004主轴承外圈温度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-004主轴承外圈温度","yc_hs_0070","cur_03"]
[3029,"f_盂县一期Ⅰ-004机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-004机舱侧向振动(已滤波)","yc_hs_0070","cur_13"]
[3030,"f_盂县一期Ⅰ-004机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-004机舱轴向振动(已滤波)","yc_hs_0070","cur_15"]
[3031,"f_盂县一期Ⅰ-004机舱角度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-004机舱角度","yc_hs_0070","cur_16"]
[3032,"f_盂县一期Ⅰ-004扭揽角度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-004扭揽角度","yc_hs_0070","cur_18"]
[3033,"f_盂县一期Ⅰ-004 1#桨叶片角度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-004 1#桨叶片角度","yc_hs_0069","cur_67"]
[3034,"f_盂县一期Ⅰ-004 2#桨叶片角度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-004 2#桨叶片角度","yc_hs_0069","cur_69"]
[3035,"f_盂县一期Ⅰ-004 3#桨叶片角度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-004 3#桨叶片角度","yc_hs_0069","cur_71"]
[3036,"f_盂县一期Ⅰ-006机舱角度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅰ-006机舱角度","yc_hs_0072","cur_26"]
[3037,"f_盂县一期Ⅰ-006扭揽角度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅰ-006扭揽角度","yc_hs_0072","cur_28"]
[3038,"f_盂县一期Ⅱ-033发电机有功功率","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-033发电机有功功率","yc_hs_0099","cur_79"]
[3039,"f_盂县一期Ⅱ-027齿轮箱油池温度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅱ-027齿轮箱油池温度","yc_hs_0094","cur_15"]
[3040,"f_盂县一期Ⅱ-027主轴承外圈温度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅱ-027主轴承外圈温度","yc_hs_0094","cur_18"]
[3041,"f_盂县一期Ⅱ-027机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅱ-027机舱侧向振动(已滤波)","yc_hs_0094","cur_28"]
[3042,"f_盂县一期Ⅰ-016齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-016齿轮箱高速轴非驱动端轴承温度","yc_hs_0082","cur_59"]
[3043,"f_盂县一期Ⅰ-016齿轮箱油池温度","盂县风光互补电站","WOF35800082",16,"SXYX.T1_L1.WTG016.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-016齿轮箱油池温度","yc_hs_0082","cur_60"]
[3044,"f_盂县一期Ⅰ-007 2#桨叶片角度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅰ-007 2#桨叶片角度","yc_hs_0072","cur_84"]
[3045,"f_盂县一期Ⅰ-007 3#桨叶片角度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-007 3#桨叶片角度","yc_hs_0072","cur_86"]
[3046,"f_盂县一期Ⅰ-010发电机有功功率","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-010发电机有功功率","yc_hs_0075","cur_64"]
[3047,"f_盂县一期Ⅰ-011舱外温度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-011舱外温度","yc_hs_0076","cur_89"]
[3048,"f_盂县一期Ⅰ-011风向","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-011风向","yc_hs_0076","cur_92"]
[3049,"f_盂县一期Ⅰ-011风速","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-011风速","yc_hs_0076","cur_94"]
[3050,"f_盂县一期Ⅰ-011机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-011机舱中轴线与风向夹角","yc_hs_0076","cur_97"]
[3051,"f_盂县一期Ⅰ-011 1#桨叶片角度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-011 1#桨叶片角度","yc_hs_0077","cur_02"]
[3052,"f_盂县一期Ⅰ-009 3#桨叶片角度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅰ-009 3#桨叶片角度","yc_hs_0074","cur_96"]
[3053,"f_盂县一期Ⅰ-001机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-001机舱中轴线与风向夹角","yc_hs_0066","cur_47"]
[3054,"f_盂县一期Ⅰ-001舱外温度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-001舱外温度","yc_hs_0066","cur_39"]
[3055,"f_盂县一期Ⅰ-001舱内温度","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-001舱内温度","yc_hs_0066","cur_37"]
[3056,"f_盂县一期Ⅰ-001风向","盂县风光互补电站","WOF35800082",1,"SXYX.T1_L1.WTG001.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-001风向","yc_hs_0066","cur_42"]
[3057,"f_盂县一期Ⅰ-007主轴转速","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-007主轴转速","yc_hs_0073","cur_10"]
[3058,"f_盂县一期Ⅱ-024舱内温度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-024舱内温度","yc_hs_0090","cur_52"]
[3059,"f_盂县一期Ⅱ-024舱外温度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅱ-024舱外温度","yc_hs_0090","cur_54"]
[3060,"f_盂县一期Ⅱ-024风向","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅱ-024风向","yc_hs_0090","cur_57"]
[3061,"f_盂县一期Ⅱ-024风速","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅱ-024风速","yc_hs_0090","cur_59"]
[3062,"f_盂县一期Ⅱ-024机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅱ-024机舱中轴线与风向夹角","yc_hs_0090","cur_62"]
[3063,"f_盂县一期Ⅱ-024 1#桨叶片角度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅱ-024 1#桨叶片角度","yc_hs_0090","cur_67"]
[3064,"f_盂县一期Ⅱ-024 2#桨叶片角度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县一期Ⅱ-024 2#桨叶片角度","yc_hs_0090","cur_69"]
[3065,"f_盂县一期Ⅱ-024 3#桨叶片角度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-024 3#桨叶片角度","yc_hs_0090","cur_71"]
[3066,"f_盂县一期Ⅰ-010齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-010齿轮箱中速轴非驱动端轴承温度","yc_hs_0076","cur_91"]
[3067,"f_盂县一期Ⅱ-021 3#桨叶片角度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-021 3#桨叶片角度","yc_hs_0087","cur_56"]
[3068,"f_盂县一期Ⅰ-013发电机有功功率","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-013发电机有功功率","yc_hs_0078","cur_79"]
[3069,"f_盂县一期Ⅰ-013发电机转速","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-013发电机转速","yc_hs_0078","cur_83"]
[3070,"f_盂县一期Ⅰ-013发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-013发电机驱动端轴承温度","yc_hs_0078","cur_85"]
[3071,"f_盂县一期Ⅰ-013发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-013发电机非驱动端轴承温度","yc_hs_0078","cur_86"]
[3072,"f_盂县一期Ⅰ-013发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-013发电机定子U相线圈温度","yc_hs_0078","cur_88"]
[3073,"f_盂县一期Ⅰ-013发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-013发电机定子V相线圈温度","yc_hs_0078","cur_89"]
[3074,"f_盂县一期Ⅰ-013发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-013发电机定子W相线圈温度","yc_hs_0078","cur_90"]
[3075,"f_盂县一期Ⅱ-029舱内温度","盂县风光互补电站","WOF35800082",29,"SXYX.T1_L2.WTG029.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅱ-029舱内温度","yc_hs_0095","cur_77"]
[3076,"f_盂县一期Ⅰ-012机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",12,"SXYX.T1_L1.WTG012.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-012机舱中轴线与风向夹角","yc_hs_0078","cur_02"]
[3077,"f_盂县一期Ⅰ-007风速","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-007风速","yc_hs_0072","cur_74"]
[3078,"f_盂县一期Ⅰ-007机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-007机舱中轴线与风向夹角","yc_hs_0072","cur_77"]
[3079,"f_盂县一期Ⅰ-007 1#桨叶片角度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-007 1#桨叶片角度","yc_hs_0072","cur_82"]
[3080,"f_盂县一期Ⅰ-015主轴转速","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-015主轴转速","yc_hs_0081","cur_50"]
[3081,"f_盂县一期Ⅱ-021发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",21,"SXYX.T1_L2.WTG021.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-021发电机定子W相线圈温度","yc_hs_0087","cur_30"]
[3082,"f_盂县一期Ⅱ-033发电机转速","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-033发电机转速","yc_hs_0099","cur_83"]
[3083,"f_盂县一期Ⅱ-033发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅱ-033发电机驱动端轴承温度","yc_hs_0099","cur_85"]
[3084,"f_盂县一期Ⅱ-033发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-033发电机非驱动端轴承温度","yc_hs_0099","cur_86"]
[3085,"f_盂县一期Ⅱ-033发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-033发电机定子U相线圈温度","yc_hs_0099","cur_88"]
[3086,"f_盂县一期Ⅱ-033发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-033发电机定子V相线圈温度","yc_hs_0099","cur_89"]
[3087,"f_盂县一期Ⅱ-033发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅱ-033发电机定子W相线圈温度","yc_hs_0099","cur_90"]
[3088,"f_盂县一期Ⅱ-028发电机有功功率","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅱ-028发电机有功功率","yc_hs_0094","cur_54"]
[3089,"f_盂县一期Ⅱ-028发电机转速","盂县风光互补电站","WOF35800082",28,"SXYX.T1_L2.WTG028.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅱ-028发电机转速","yc_hs_0094","cur_58"]
[3090,"f_盂县一期Ⅱ-022发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅱ-022发电机非驱动端轴承温度","yc_hs_0088","cur_31"]
[3091,"f_盂县一期Ⅰ-009发电机有功功率","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WGEN.GenActivePW","有功功率","active_power","f_盂县一期Ⅰ-009发电机有功功率","yc_hs_0074","cur_59"]
[3092,"f_盂县一期Ⅰ-009发电机转速","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WGEN.GenSpd","发电机转速","generator_speed","f_盂县一期Ⅰ-009发电机转速","yc_hs_0074","cur_63"]
[3093,"f_盂县一期Ⅰ-009发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县一期Ⅰ-009发电机驱动端轴承温度","yc_hs_0074","cur_65"]
[3094,"f_盂县一期Ⅰ-009发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县一期Ⅰ-009发电机非驱动端轴承温度","yc_hs_0074","cur_66"]
[3095,"f_盂县一期Ⅰ-009发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-009发电机定子U相线圈温度","yc_hs_0074","cur_68"]
[3096,"f_盂县一期Ⅰ-009发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-009发电机定子V相线圈温度","yc_hs_0074","cur_69"]
[3097,"f_盂县一期Ⅱ-026 3#桨叶片角度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县一期Ⅱ-026 3#桨叶片角度","yc_hs_0092","cur_81"]
[3098,"f_盂县一期Ⅱ-027发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅱ-027发电机定子U相线圈温度","yc_hs_0093","cur_58"]
[3099,"f_盂县一期Ⅱ-027发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅱ-027发电机定子V相线圈温度","yc_hs_0093","cur_59"]
[3100,"f_盂县一期Ⅰ-007齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县一期Ⅰ-007齿轮箱高速轴非驱动端轴承温度","yc_hs_0073","cur_14"]
[3101,"f_盂县一期Ⅰ-007齿轮箱油池温度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县一期Ⅰ-007齿轮箱油池温度","yc_hs_0073","cur_15"]
[3102,"f_盂县一期Ⅰ-007主轴承外圈温度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县一期Ⅰ-007主轴承外圈温度","yc_hs_0073","cur_18"]
[3103,"f_盂县一期Ⅰ-007机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县一期Ⅰ-007机舱侧向振动(已滤波)","yc_hs_0073","cur_28"]
[3104,"f_盂县一期Ⅰ-007机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县一期Ⅰ-007机舱轴向振动(已滤波)","yc_hs_0073","cur_30"]
[3105,"f_盂县一期Ⅰ-015发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县一期Ⅰ-015发电机定子U相线圈温度","yc_hs_0080","cur_98"]
[3106,"f_盂县一期Ⅰ-015发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县一期Ⅰ-015发电机定子V相线圈温度","yc_hs_0080","cur_99"]
[3107,"f_盂县一期Ⅰ-015发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县一期Ⅰ-015发电机定子W相线圈温度","yc_hs_0080","cur_100"]
[3108,"f_盂县一期Ⅰ-015舱内温度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县一期Ⅰ-015舱内温度","yc_hs_0081","cur_07"]
[3109,"f_盂县一期Ⅰ-015舱外温度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县一期Ⅰ-015舱外温度","yc_hs_0081","cur_09"]
[3110,"f_盂县一期Ⅰ-015风向","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县一期Ⅰ-015风向","yc_hs_0081","cur_12"]
[3111,"f_盂县一期Ⅰ-015风速","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WNAC.WindSpeed","风速","wind_velocity","f_盂县一期Ⅰ-015风速","yc_hs_0081","cur_14"]
[3112,"f_盂县一期Ⅰ-015机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县一期Ⅰ-015机舱中轴线与风向夹角","yc_hs_0081","cur_17"]
[3113,"f_盂县一期Ⅰ-015 1#桨叶片角度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县一期Ⅰ-015 1#桨叶片角度","yc_hs_0081","cur_22"]
[3114,"f_盂县一期Ⅱ-033机舱角度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县一期Ⅱ-033机舱角度","yc_hs_0100","cur_61"]
[3115,"f_盂县一期Ⅱ-033扭揽角度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县一期Ⅱ-033扭揽角度","yc_hs_0100","cur_63"]
[3116,"f_盂县一期Ⅱ-024主轴转速","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅱ-024主轴转速","yc_hs_0090","cur_95"]
[3117,"f_盂县一期Ⅰ-010主轴转速","盂县风光互补电站","WOF35800082",10,"SXYX.T1_L1.WTG010.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县一期Ⅰ-010主轴转速","yc_hs_0076","cur_25"]
[3118,"f_盂县一期Ⅱ-026齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",26,"SXYX.T1_L2.WTG026.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-026齿轮箱中速轴非驱动端轴承温度","yc_hs_0093","cur_71"]
[3119,"f_盂县一期Ⅰ-011齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",11,"SXYX.T1_L1.WTG011.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-011齿轮箱中速轴非驱动端轴承温度","yc_hs_0077","cur_96"]
[3120,"f_盂县一期Ⅱ-027齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",27,"SXYX.T1_L2.WTG027.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-027齿轮箱中速轴非驱动端轴承温度","yc_hs_0094","cur_76"]
[3121,"f_盂县一期Ⅱ-033齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",33,"SXYX.T1_L2.WTG033.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-033齿轮箱中速轴非驱动端轴承温度","yc_hs_0315","cur_54"]
[3122,"f_盂县一期Ⅰ-002齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",2,"SXYX.T1_L1.WTG002.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-002齿轮箱中速轴非驱动端轴承温度","yc_hs_0068","cur_51"]
[3123,"f_盂县一期Ⅰ-015齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",15,"SXYX.T1_L1.WTG015.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-015齿轮箱中速轴非驱动端轴承温度","yc_hs_0082","cur_16"]
[3124,"f_盂县一期Ⅱ-019齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",19,"SXYX.T1_L2.WTG019.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-019齿轮箱中速轴非驱动端轴承温度","yc_hs_0086","cur_36"]
[3125,"f_盂县一期Ⅱ-030齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",30,"SXYX.T1_L2.WTG030.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-030齿轮箱中速轴非驱动端轴承温度","yc_hs_0097","cur_91"]
[3126,"f_盂县一期Ⅱ-025齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",25,"SXYX.T1_L2.WTG025.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-025齿轮箱中速轴非驱动端轴承温度","yc_hs_0092","cur_66"]
[3127,"f_盂县一期Ⅰ-007齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",7,"SXYX.T1_L1.WTG007.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-007齿轮箱中速轴非驱动端轴承温度","yc_hs_0073","cur_76"]
[3128,"f_盂县一期Ⅱ-018齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",18,"SXYX.T1_L2.WTG018.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-018齿轮箱中速轴非驱动端轴承温度","yc_hs_0085","cur_31"]
[3129,"f_盂县一期Ⅰ-009齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",9,"SXYX.T1_L1.WTG009.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-009齿轮箱中速轴非驱动端轴承温度","yc_hs_0075","cur_86"]
[3130,"f_盂县一期Ⅰ-008齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",8,"SXYX.T1_L1.WTG008.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-008齿轮箱中速轴非驱动端轴承温度","yc_hs_0074","cur_81"]
[3131,"f_盂县一期Ⅱ-022齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",22,"SXYX.T1_L2.WTG022.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-022齿轮箱中速轴非驱动端轴承温度","yc_hs_0089","cur_51"]
[3132,"f_盂县一期Ⅰ-014齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",14,"SXYX.T1_L1.WTG014.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-014齿轮箱中速轴非驱动端轴承温度","yc_hs_0081","cur_11"]
[3133,"f_盂县一期Ⅰ-004齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",4,"SXYX.T1_L1.WTG004.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-004齿轮箱中速轴非驱动端轴承温度","yc_hs_0070","cur_61"]
[3134,"f_盂县一期Ⅱ-020齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",20,"SXYX.T1_L2.WTG020.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-020齿轮箱中速轴非驱动端轴承温度","yc_hs_0087","cur_41"]
[3135,"f_盂县一期Ⅰ-003齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",3,"SXYX.T1_L1.WTG003.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-003齿轮箱中速轴非驱动端轴承温度","yc_hs_0069","cur_56"]
[3136,"f_盂县一期Ⅰ-017齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",17,"SXYX.T1_L1.WTG017.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-017齿轮箱中速轴非驱动端轴承温度","yc_hs_0084","cur_26"]
[3137,"f_盂县一期Ⅱ-031齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",31,"SXYX.T1_L2.WTG031.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-031齿轮箱中速轴非驱动端轴承温度","yc_hs_0098","cur_96"]
[3138,"f_盂县一期Ⅱ-023齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",23,"SXYX.T1_L2.WTG023.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-023齿轮箱中速轴非驱动端轴承温度","yc_hs_0090","cur_56"]
[3139,"f_盂县一期Ⅱ-024齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",24,"SXYX.T1_L2.WTG024.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅱ-024齿轮箱中速轴非驱动端轴承温度","yc_hs_0091","cur_61"]
[3140,"f_盂县一期Ⅰ-013齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",13,"SXYX.T1_L1.WTG013.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-013齿轮箱中速轴非驱动端轴承温度","yc_hs_0080","cur_06"]
[3141,"f_盂县一期Ⅰ-006齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",6,"SXYX.T1_L1.WTG006.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县一期Ⅰ-006齿轮箱中速轴非驱动端轴承温度","yc_hs_0072","cur_71"]
[3142,"f_盂县二期Ⅲ-034 风速","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅲ-034 风速","yc_hs_0384","cur_02"]
[3143,"f_盂县二期Ⅲ-034 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅲ-034 机舱中轴线与风向夹角","yc_hs_0384","cur_03"]
[3144,"f_盂县二期Ⅲ-034 发电机有功功率","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅲ-034 发电机有功功率","yc_hs_0384","cur_04"]
[3145,"f_盂县二期Ⅲ-034 发电机转速","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅲ-034 发电机转速","yc_hs_0384","cur_05"]
[3146,"f_盂县二期Ⅲ-034 主轴转速","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅲ-034 主轴转速","yc_hs_0384","cur_15"]
[3147,"f_盂县二期Ⅲ-034 舱外温度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅲ-034 舱外温度","yc_hs_0384","cur_16"]
[3148,"f_盂县二期Ⅲ-034 舱内温度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅲ-034 舱内温度","yc_hs_0384","cur_17"]
[3149,"f_盂县二期Ⅲ-034 主轴承外圈温度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅲ-034 主轴承外圈温度","yc_hs_0384","cur_18"]
[3150,"f_盂县二期Ⅲ-034 齿轮箱油池温度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅲ-034 齿轮箱油池温度","yc_hs_0384","cur_19"]
[3151,"f_盂县二期Ⅲ-034 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅲ-034 发电机定子U相线圈温度","yc_hs_0384","cur_21"]
[3152,"f_盂县二期Ⅲ-034 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅲ-034 发电机定子V相线圈温度","yc_hs_0384","cur_22"]
[3153,"f_盂县二期Ⅲ-034 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅲ-034 发电机定子W相线圈温度","yc_hs_0384","cur_23"]
[3154,"f_盂县二期Ⅲ-034 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅲ-034 发电机驱动端轴承温度","yc_hs_0384","cur_24"]
[3155,"f_盂县二期Ⅲ-034 机舱角度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅲ-034 机舱角度","yc_hs_0384","cur_25"]
[3156,"f_盂县二期Ⅲ-034 1#桨叶片角度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅲ-034 1#桨叶片角度","yc_hs_0384","cur_26"]
[3157,"f_盂县二期Ⅲ-034 2#桨叶片角度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅲ-034 2#桨叶片角度","yc_hs_0384","cur_27"]
[3158,"f_盂县二期Ⅲ-034 3#桨叶片角度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅲ-034 3#桨叶片角度","yc_hs_0384","cur_28"]
[3159,"f_盂县二期Ⅲ-034 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅲ-034 齿轮箱高速轴非驱动端轴承温度","yc_hs_0384","cur_30"]
[3160,"f_盂县二期Ⅲ-034 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅲ-034 发电机非驱动端轴承温度","yc_hs_0384","cur_31"]
[3161,"f_盂县二期Ⅲ-034 扭揽角度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅲ-034 扭揽角度","yc_hs_0384","cur_38"]
[3162,"f_盂县二期Ⅲ-034 风向","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅲ-034 风向","yc_hs_0384","cur_43"]
[3163,"f_盂县二期Ⅲ-034 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅲ-034 机舱侧向振动(已滤波)","yc_hs_0384","cur_44"]
[3164,"f_盂县二期Ⅲ-034 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅲ-034 机舱轴向振动(已滤波)","yc_hs_0384","cur_45"]
[3165,"f_盂县二期Ⅲ-034 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",34,"SXYX.T2_L1.WTG034.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅲ-034 齿轮箱中速轴非驱动端轴承温度","yc_hs_0384","cur_68"]
[3166,"f_盂县二期Ⅲ-035 风速","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅲ-035 风速","yc_hs_0385","cur_06"]
[3167,"f_盂县二期Ⅲ-035 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅲ-035 机舱中轴线与风向夹角","yc_hs_0385","cur_07"]
[3168,"f_盂县二期Ⅲ-035 发电机有功功率","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅲ-035 发电机有功功率","yc_hs_0385","cur_08"]
[3169,"f_盂县二期Ⅲ-035 发电机转速","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅲ-035 发电机转速","yc_hs_0385","cur_09"]
[3170,"f_盂县二期Ⅲ-035 主轴转速","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅲ-035 主轴转速","yc_hs_0385","cur_19"]
[3171,"f_盂县二期Ⅲ-035 舱外温度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅲ-035 舱外温度","yc_hs_0385","cur_20"]
[3172,"f_盂县二期Ⅲ-035 舱内温度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅲ-035 舱内温度","yc_hs_0385","cur_21"]
[3173,"f_盂县二期Ⅲ-035 主轴承外圈温度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅲ-035 主轴承外圈温度","yc_hs_0385","cur_22"]
[3174,"f_盂县二期Ⅲ-035 齿轮箱油池温度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅲ-035 齿轮箱油池温度","yc_hs_0385","cur_23"]
[3175,"f_盂县二期Ⅲ-035 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅲ-035 发电机定子U相线圈温度","yc_hs_0385","cur_25"]
[3176,"f_盂县二期Ⅲ-035 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅲ-035 发电机定子V相线圈温度","yc_hs_0385","cur_26"]
[3177,"f_盂县二期Ⅲ-035 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅲ-035 发电机定子W相线圈温度","yc_hs_0385","cur_27"]
[3178,"f_盂县二期Ⅲ-035 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅲ-035 发电机驱动端轴承温度","yc_hs_0385","cur_28"]
[3179,"f_盂县二期Ⅲ-035 机舱角度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅲ-035 机舱角度","yc_hs_0385","cur_29"]
[3180,"f_盂县二期Ⅲ-035 1#桨叶片角度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅲ-035 1#桨叶片角度","yc_hs_0385","cur_30"]
[3181,"f_盂县二期Ⅲ-035 2#桨叶片角度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅲ-035 2#桨叶片角度","yc_hs_0385","cur_31"]
[3182,"f_盂县二期Ⅲ-035 3#桨叶片角度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅲ-035 3#桨叶片角度","yc_hs_0385","cur_32"]
[3183,"f_盂县二期Ⅲ-035 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅲ-035 齿轮箱高速轴非驱动端轴承温度","yc_hs_0385","cur_34"]
[3184,"f_盂县二期Ⅲ-035 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅲ-035 发电机非驱动端轴承温度","yc_hs_0385","cur_35"]
[3185,"f_盂县二期Ⅲ-035 扭揽角度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅲ-035 扭揽角度","yc_hs_0385","cur_42"]
[3186,"f_盂县二期Ⅲ-035 风向","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅲ-035 风向","yc_hs_0385","cur_47"]
[3187,"f_盂县二期Ⅲ-035 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅲ-035 机舱侧向振动(已滤波)","yc_hs_0385","cur_48"]
[3188,"f_盂县二期Ⅲ-035 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅲ-035 机舱轴向振动(已滤波)","yc_hs_0385","cur_49"]
[3189,"f_盂县二期Ⅲ-035 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",35,"SXYX.T2_L1.WTG035.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅲ-035 齿轮箱中速轴非驱动端轴承温度","yc_hs_0385","cur_72"]
[3190,"f_盂县二期Ⅲ-036 风速","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅲ-036 风速","yc_hs_0386","cur_10"]
[3191,"f_盂县二期Ⅲ-036 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅲ-036 机舱中轴线与风向夹角","yc_hs_0386","cur_11"]
[3192,"f_盂县二期Ⅲ-036 发电机有功功率","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅲ-036 发电机有功功率","yc_hs_0386","cur_12"]
[3193,"f_盂县二期Ⅲ-036 发电机转速","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅲ-036 发电机转速","yc_hs_0386","cur_13"]
[3194,"f_盂县二期Ⅲ-036 主轴转速","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅲ-036 主轴转速","yc_hs_0386","cur_23"]
[3195,"f_盂县二期Ⅲ-036 舱外温度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅲ-036 舱外温度","yc_hs_0386","cur_24"]
[3196,"f_盂县二期Ⅲ-036 舱内温度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅲ-036 舱内温度","yc_hs_0386","cur_25"]
[3197,"f_盂县二期Ⅲ-036 主轴承外圈温度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅲ-036 主轴承外圈温度","yc_hs_0386","cur_26"]
[3198,"f_盂县二期Ⅲ-036 齿轮箱油池温度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅲ-036 齿轮箱油池温度","yc_hs_0386","cur_27"]
[3199,"f_盂县二期Ⅲ-036 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅲ-036 发电机定子U相线圈温度","yc_hs_0386","cur_29"]
[3200,"f_盂县二期Ⅲ-036 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅲ-036 发电机定子V相线圈温度","yc_hs_0386","cur_30"]
[3201,"f_盂县二期Ⅲ-036 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅲ-036 发电机定子W相线圈温度","yc_hs_0386","cur_31"]
[3202,"f_盂县二期Ⅲ-036 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅲ-036 发电机驱动端轴承温度","yc_hs_0386","cur_32"]
[3203,"f_盂县二期Ⅲ-036 机舱角度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅲ-036 机舱角度","yc_hs_0386","cur_33"]
[3204,"f_盂县二期Ⅲ-036 1#桨叶片角度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅲ-036 1#桨叶片角度","yc_hs_0386","cur_34"]
[3205,"f_盂县二期Ⅲ-036 2#桨叶片角度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅲ-036 2#桨叶片角度","yc_hs_0386","cur_35"]
[3206,"f_盂县二期Ⅲ-036 3#桨叶片角度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅲ-036 3#桨叶片角度","yc_hs_0386","cur_36"]
[3207,"f_盂县二期Ⅲ-036 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅲ-036 齿轮箱高速轴非驱动端轴承温度","yc_hs_0386","cur_38"]
[3208,"f_盂县二期Ⅲ-036 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅲ-036 发电机非驱动端轴承温度","yc_hs_0386","cur_39"]
[3209,"f_盂县二期Ⅲ-036 扭揽角度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅲ-036 扭揽角度","yc_hs_0386","cur_46"]
[3210,"f_盂县二期Ⅲ-036 风向","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅲ-036 风向","yc_hs_0386","cur_51"]
[3211,"f_盂县二期Ⅲ-036 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅲ-036 机舱侧向振动(已滤波)","yc_hs_0386","cur_52"]
[3212,"f_盂县二期Ⅲ-036 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅲ-036 机舱轴向振动(已滤波)","yc_hs_0386","cur_53"]
[3213,"f_盂县二期Ⅲ-036 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",36,"SXYX.T2_L1.WTG036.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅲ-036 齿轮箱中速轴非驱动端轴承温度","yc_hs_0386","cur_76"]
[3214,"f_盂县二期Ⅲ-037 风速","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅲ-037 风速","yc_hs_0387","cur_14"]
[3215,"f_盂县二期Ⅲ-037 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅲ-037 机舱中轴线与风向夹角","yc_hs_0387","cur_15"]
[3216,"f_盂县二期Ⅲ-037 发电机有功功率","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅲ-037 发电机有功功率","yc_hs_0387","cur_16"]
[3217,"f_盂县二期Ⅲ-037 发电机转速","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅲ-037 发电机转速","yc_hs_0387","cur_17"]
[3218,"f_盂县二期Ⅲ-037 主轴转速","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅲ-037 主轴转速","yc_hs_0387","cur_27"]
[3219,"f_盂县二期Ⅲ-037 舱外温度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅲ-037 舱外温度","yc_hs_0387","cur_28"]
[3220,"f_盂县二期Ⅲ-037 舱内温度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅲ-037 舱内温度","yc_hs_0387","cur_29"]
[3221,"f_盂县二期Ⅲ-037 主轴承外圈温度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅲ-037 主轴承外圈温度","yc_hs_0387","cur_30"]
[3222,"f_盂县二期Ⅲ-037 齿轮箱油池温度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅲ-037 齿轮箱油池温度","yc_hs_0387","cur_31"]
[3223,"f_盂县二期Ⅲ-037 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅲ-037 发电机定子U相线圈温度","yc_hs_0387","cur_33"]
[3224,"f_盂县二期Ⅲ-037 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅲ-037 发电机定子V相线圈温度","yc_hs_0387","cur_34"]
[3225,"f_盂县二期Ⅲ-037 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅲ-037 发电机定子W相线圈温度","yc_hs_0387","cur_35"]
[3226,"f_盂县二期Ⅲ-037 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅲ-037 发电机驱动端轴承温度","yc_hs_0387","cur_36"]
[3227,"f_盂县二期Ⅲ-037 机舱角度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅲ-037 机舱角度","yc_hs_0387","cur_37"]
[3228,"f_盂县二期Ⅲ-037 1#桨叶片角度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅲ-037 1#桨叶片角度","yc_hs_0387","cur_38"]
[3229,"f_盂县二期Ⅲ-037 2#桨叶片角度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅲ-037 2#桨叶片角度","yc_hs_0387","cur_39"]
[3230,"f_盂县二期Ⅲ-037 3#桨叶片角度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅲ-037 3#桨叶片角度","yc_hs_0387","cur_40"]
[3231,"f_盂县二期Ⅲ-037 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅲ-037 齿轮箱高速轴非驱动端轴承温度","yc_hs_0387","cur_42"]
[3232,"f_盂县二期Ⅲ-037 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅲ-037 发电机非驱动端轴承温度","yc_hs_0387","cur_43"]
[3233,"f_盂县二期Ⅲ-037 扭揽角度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅲ-037 扭揽角度","yc_hs_0387","cur_50"]
[3234,"f_盂县二期Ⅲ-037 风向","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅲ-037 风向","yc_hs_0387","cur_55"]
[3235,"f_盂县二期Ⅲ-037 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅲ-037 机舱侧向振动(已滤波)","yc_hs_0387","cur_56"]
[3236,"f_盂县二期Ⅲ-037 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅲ-037 机舱轴向振动(已滤波)","yc_hs_0387","cur_57"]
[3237,"f_盂县二期Ⅲ-037 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",37,"SXYX.T2_L1.WTG037.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅲ-037 齿轮箱中速轴非驱动端轴承温度","yc_hs_0387","cur_80"]
[3238,"f_盂县二期Ⅲ-038 风速","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅲ-038 风速","yc_hs_0388","cur_18"]
[3239,"f_盂县二期Ⅲ-038 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅲ-038 机舱中轴线与风向夹角","yc_hs_0388","cur_19"]
[3240,"f_盂县二期Ⅲ-038 发电机有功功率","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅲ-038 发电机有功功率","yc_hs_0388","cur_20"]
[3241,"f_盂县二期Ⅲ-038 发电机转速","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅲ-038 发电机转速","yc_hs_0388","cur_21"]
[3242,"f_盂县二期Ⅲ-038 主轴转速","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅲ-038 主轴转速","yc_hs_0388","cur_31"]
[3243,"f_盂县二期Ⅲ-038 舱外温度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅲ-038 舱外温度","yc_hs_0388","cur_32"]
[3244,"f_盂县二期Ⅲ-038 舱内温度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅲ-038 舱内温度","yc_hs_0388","cur_33"]
[3245,"f_盂县二期Ⅲ-038 主轴承外圈温度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅲ-038 主轴承外圈温度","yc_hs_0388","cur_34"]
[3246,"f_盂县二期Ⅲ-038 齿轮箱油池温度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅲ-038 齿轮箱油池温度","yc_hs_0388","cur_35"]
[3247,"f_盂县二期Ⅲ-038 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅲ-038 发电机定子U相线圈温度","yc_hs_0388","cur_37"]
[3248,"f_盂县二期Ⅲ-038 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅲ-038 发电机定子V相线圈温度","yc_hs_0388","cur_38"]
[3249,"f_盂县二期Ⅲ-038 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅲ-038 发电机定子W相线圈温度","yc_hs_0388","cur_39"]
[3250,"f_盂县二期Ⅲ-038 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅲ-038 发电机驱动端轴承温度","yc_hs_0388","cur_40"]
[3251,"f_盂县二期Ⅲ-038 机舱角度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅲ-038 机舱角度","yc_hs_0388","cur_41"]
[3252,"f_盂县二期Ⅲ-038 1#桨叶片角度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅲ-038 1#桨叶片角度","yc_hs_0388","cur_42"]
[3253,"f_盂县二期Ⅲ-038 2#桨叶片角度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅲ-038 2#桨叶片角度","yc_hs_0388","cur_43"]
[3254,"f_盂县二期Ⅲ-038 3#桨叶片角度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅲ-038 3#桨叶片角度","yc_hs_0388","cur_44"]
[3255,"f_盂县二期Ⅲ-038 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅲ-038 齿轮箱高速轴非驱动端轴承温度","yc_hs_0388","cur_46"]
[3256,"f_盂县二期Ⅲ-038 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅲ-038 发电机非驱动端轴承温度","yc_hs_0388","cur_47"]
[3257,"f_盂县二期Ⅲ-038 扭揽角度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅲ-038 扭揽角度","yc_hs_0388","cur_54"]
[3258,"f_盂县二期Ⅲ-038 风向","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅲ-038 风向","yc_hs_0388","cur_59"]
[3259,"f_盂县二期Ⅲ-038 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅲ-038 机舱侧向振动(已滤波)","yc_hs_0388","cur_60"]
[3260,"f_盂县二期Ⅲ-038 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅲ-038 机舱轴向振动(已滤波)","yc_hs_0388","cur_61"]
[3261,"f_盂县二期Ⅲ-038 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",38,"SXYX.T2_L1.WTG038.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅲ-038 齿轮箱中速轴非驱动端轴承温度","yc_hs_0388","cur_84"]
[3262,"f_盂县二期Ⅲ-039 风速","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅲ-039 风速","yc_hs_0389","cur_22"]
[3263,"f_盂县二期Ⅲ-039 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅲ-039 机舱中轴线与风向夹角","yc_hs_0389","cur_23"]
[3264,"f_盂县二期Ⅲ-039 发电机有功功率","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅲ-039 发电机有功功率","yc_hs_0389","cur_24"]
[3265,"f_盂县二期Ⅲ-039 发电机转速","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅲ-039 发电机转速","yc_hs_0389","cur_25"]
[3266,"f_盂县二期Ⅲ-039 主轴转速","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅲ-039 主轴转速","yc_hs_0389","cur_35"]
[3267,"f_盂县二期Ⅲ-039 舱外温度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅲ-039 舱外温度","yc_hs_0389","cur_36"]
[3268,"f_盂县二期Ⅲ-039 舱内温度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅲ-039 舱内温度","yc_hs_0389","cur_37"]
[3269,"f_盂县二期Ⅲ-039 主轴承外圈温度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅲ-039 主轴承外圈温度","yc_hs_0389","cur_38"]
[3270,"f_盂县二期Ⅲ-039 齿轮箱油池温度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅲ-039 齿轮箱油池温度","yc_hs_0389","cur_39"]
[3271,"f_盂县二期Ⅲ-039 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅲ-039 发电机定子U相线圈温度","yc_hs_0389","cur_41"]
[3272,"f_盂县二期Ⅲ-039 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅲ-039 发电机定子V相线圈温度","yc_hs_0389","cur_42"]
[3273,"f_盂县二期Ⅲ-039 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅲ-039 发电机定子W相线圈温度","yc_hs_0389","cur_43"]
[3274,"f_盂县二期Ⅲ-039 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅲ-039 发电机驱动端轴承温度","yc_hs_0389","cur_44"]
[3275,"f_盂县二期Ⅲ-039 机舱角度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅲ-039 机舱角度","yc_hs_0389","cur_45"]
[3276,"f_盂县二期Ⅲ-039 1#桨叶片角度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅲ-039 1#桨叶片角度","yc_hs_0389","cur_46"]
[3277,"f_盂县二期Ⅲ-039 2#桨叶片角度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅲ-039 2#桨叶片角度","yc_hs_0389","cur_47"]
[3278,"f_盂县二期Ⅲ-039 3#桨叶片角度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅲ-039 3#桨叶片角度","yc_hs_0389","cur_48"]
[3279,"f_盂县二期Ⅲ-039 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅲ-039 齿轮箱高速轴非驱动端轴承温度","yc_hs_0389","cur_50"]
[3280,"f_盂县二期Ⅲ-039 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅲ-039 发电机非驱动端轴承温度","yc_hs_0389","cur_51"]
[3281,"f_盂县二期Ⅲ-039 扭揽角度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅲ-039 扭揽角度","yc_hs_0389","cur_58"]
[3282,"f_盂县二期Ⅲ-039 风向","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅲ-039 风向","yc_hs_0389","cur_63"]
[3283,"f_盂县二期Ⅲ-039 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅲ-039 机舱侧向振动(已滤波)","yc_hs_0389","cur_64"]
[3284,"f_盂县二期Ⅲ-039 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅲ-039 机舱轴向振动(已滤波)","yc_hs_0389","cur_65"]
[3285,"f_盂县二期Ⅲ-039 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",39,"SXYX.T2_L1.WTG039.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅲ-039 齿轮箱中速轴非驱动端轴承温度","yc_hs_0389","cur_88"]
[3286,"f_盂县二期Ⅲ-040 风速","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅲ-040 风速","yc_hs_0390","cur_26"]
[3287,"f_盂县二期Ⅲ-040 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅲ-040 机舱中轴线与风向夹角","yc_hs_0390","cur_27"]
[3288,"f_盂县二期Ⅲ-040 发电机有功功率","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅲ-040 发电机有功功率","yc_hs_0390","cur_28"]
[3289,"f_盂县二期Ⅲ-040 发电机转速","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅲ-040 发电机转速","yc_hs_0390","cur_29"]
[3290,"f_盂县二期Ⅲ-040 主轴转速","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅲ-040 主轴转速","yc_hs_0390","cur_39"]
[3291,"f_盂县二期Ⅲ-040 舱外温度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅲ-040 舱外温度","yc_hs_0390","cur_40"]
[3292,"f_盂县二期Ⅲ-040 舱内温度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅲ-040 舱内温度","yc_hs_0390","cur_41"]
[3293,"f_盂县二期Ⅲ-040 主轴承外圈温度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅲ-040 主轴承外圈温度","yc_hs_0390","cur_42"]
[3294,"f_盂县二期Ⅲ-040 齿轮箱油池温度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅲ-040 齿轮箱油池温度","yc_hs_0390","cur_43"]
[3295,"f_盂县二期Ⅲ-040 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅲ-040 发电机定子U相线圈温度","yc_hs_0390","cur_45"]
[3296,"f_盂县二期Ⅲ-040 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅲ-040 发电机定子V相线圈温度","yc_hs_0390","cur_46"]
[3297,"f_盂县二期Ⅲ-040 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅲ-040 发电机定子W相线圈温度","yc_hs_0390","cur_47"]
[3298,"f_盂县二期Ⅲ-040 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅲ-040 发电机驱动端轴承温度","yc_hs_0390","cur_48"]
[3299,"f_盂县二期Ⅲ-040 机舱角度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅲ-040 机舱角度","yc_hs_0390","cur_49"]
[3300,"f_盂县二期Ⅲ-040 1#桨叶片角度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅲ-040 1#桨叶片角度","yc_hs_0390","cur_50"]
[3301,"f_盂县二期Ⅲ-040 2#桨叶片角度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅲ-040 2#桨叶片角度","yc_hs_0390","cur_51"]
[3302,"f_盂县二期Ⅲ-040 3#桨叶片角度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅲ-040 3#桨叶片角度","yc_hs_0390","cur_52"]
[3303,"f_盂县二期Ⅲ-040 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅲ-040 齿轮箱高速轴非驱动端轴承温度","yc_hs_0390","cur_54"]
[3304,"f_盂县二期Ⅲ-040 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅲ-040 发电机非驱动端轴承温度","yc_hs_0390","cur_55"]
[3305,"f_盂县二期Ⅲ-040 扭揽角度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅲ-040 扭揽角度","yc_hs_0390","cur_62"]
[3306,"f_盂县二期Ⅲ-040 风向","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅲ-040 风向","yc_hs_0390","cur_67"]
[3307,"f_盂县二期Ⅲ-040 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅲ-040 机舱侧向振动(已滤波)","yc_hs_0390","cur_68"]
[3308,"f_盂县二期Ⅲ-040 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅲ-040 机舱轴向振动(已滤波)","yc_hs_0390","cur_69"]
[3309,"f_盂县二期Ⅲ-040 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",40,"SXYX.T2_L1.WTG040.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅲ-040 齿轮箱中速轴非驱动端轴承温度","yc_hs_0390","cur_92"]
[3310,"f_盂县二期Ⅲ-041 风速","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅲ-041 风速","yc_hs_0391","cur_30"]
[3311,"f_盂县二期Ⅲ-041 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅲ-041 机舱中轴线与风向夹角","yc_hs_0391","cur_31"]
[3312,"f_盂县二期Ⅲ-041 发电机有功功率","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅲ-041 发电机有功功率","yc_hs_0391","cur_32"]
[3313,"f_盂县二期Ⅲ-041 发电机转速","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅲ-041 发电机转速","yc_hs_0391","cur_33"]
[3314,"f_盂县二期Ⅲ-041 主轴转速","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅲ-041 主轴转速","yc_hs_0391","cur_43"]
[3315,"f_盂县二期Ⅲ-041 舱外温度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅲ-041 舱外温度","yc_hs_0391","cur_44"]
[3316,"f_盂县二期Ⅲ-041 舱内温度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅲ-041 舱内温度","yc_hs_0391","cur_45"]
[3317,"f_盂县二期Ⅲ-041 主轴承外圈温度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅲ-041 主轴承外圈温度","yc_hs_0391","cur_46"]
[3318,"f_盂县二期Ⅲ-041 齿轮箱油池温度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅲ-041 齿轮箱油池温度","yc_hs_0391","cur_47"]
[3319,"f_盂县二期Ⅲ-041 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅲ-041 发电机定子U相线圈温度","yc_hs_0391","cur_49"]
[3320,"f_盂县二期Ⅲ-041 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅲ-041 发电机定子V相线圈温度","yc_hs_0391","cur_50"]
[3321,"f_盂县二期Ⅲ-041 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅲ-041 发电机定子W相线圈温度","yc_hs_0391","cur_51"]
[3322,"f_盂县二期Ⅲ-041 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅲ-041 发电机驱动端轴承温度","yc_hs_0391","cur_52"]
[3323,"f_盂县二期Ⅲ-041 机舱角度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅲ-041 机舱角度","yc_hs_0391","cur_53"]
[3324,"f_盂县二期Ⅲ-041 1#桨叶片角度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅲ-041 1#桨叶片角度","yc_hs_0391","cur_54"]
[3325,"f_盂县二期Ⅲ-041 2#桨叶片角度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅲ-041 2#桨叶片角度","yc_hs_0391","cur_55"]
[3326,"f_盂县二期Ⅲ-041 3#桨叶片角度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅲ-041 3#桨叶片角度","yc_hs_0391","cur_56"]
[3327,"f_盂县二期Ⅲ-041 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅲ-041 齿轮箱高速轴非驱动端轴承温度","yc_hs_0391","cur_58"]
[3328,"f_盂县二期Ⅲ-041 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅲ-041 发电机非驱动端轴承温度","yc_hs_0391","cur_59"]
[3329,"f_盂县二期Ⅲ-041 扭揽角度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅲ-041 扭揽角度","yc_hs_0391","cur_66"]
[3330,"f_盂县二期Ⅲ-041 风向","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅲ-041 风向","yc_hs_0391","cur_71"]
[3331,"f_盂县二期Ⅲ-041 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅲ-041 机舱侧向振动(已滤波)","yc_hs_0391","cur_72"]
[3332,"f_盂县二期Ⅲ-041 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅲ-041 机舱轴向振动(已滤波)","yc_hs_0391","cur_73"]
[3333,"f_盂县二期Ⅲ-041 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",41,"SXYX.T2_L1.WTG041.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅲ-041 齿轮箱中速轴非驱动端轴承温度","yc_hs_0391","cur_96"]
[3334,"f_盂县二期Ⅲ-042 风速","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅲ-042 风速","yc_hs_0392","cur_34"]
[3335,"f_盂县二期Ⅲ-042 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅲ-042 机舱中轴线与风向夹角","yc_hs_0392","cur_35"]
[3336,"f_盂县二期Ⅲ-042 发电机有功功率","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅲ-042 发电机有功功率","yc_hs_0392","cur_36"]
[3337,"f_盂县二期Ⅲ-042 发电机转速","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅲ-042 发电机转速","yc_hs_0392","cur_37"]
[3338,"f_盂县二期Ⅲ-042 主轴转速","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅲ-042 主轴转速","yc_hs_0392","cur_47"]
[3339,"f_盂县二期Ⅲ-042 舱外温度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅲ-042 舱外温度","yc_hs_0392","cur_48"]
[3340,"f_盂县二期Ⅲ-042 舱内温度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅲ-042 舱内温度","yc_hs_0392","cur_49"]
[3341,"f_盂县二期Ⅲ-042 主轴承外圈温度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅲ-042 主轴承外圈温度","yc_hs_0392","cur_50"]
[3342,"f_盂县二期Ⅲ-042 齿轮箱油池温度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅲ-042 齿轮箱油池温度","yc_hs_0392","cur_51"]
[3343,"f_盂县二期Ⅲ-042 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅲ-042 发电机定子U相线圈温度","yc_hs_0392","cur_53"]
[3344,"f_盂县二期Ⅲ-042 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅲ-042 发电机定子V相线圈温度","yc_hs_0392","cur_54"]
[3345,"f_盂县二期Ⅲ-042 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅲ-042 发电机定子W相线圈温度","yc_hs_0392","cur_55"]
[3346,"f_盂县二期Ⅲ-042 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅲ-042 发电机驱动端轴承温度","yc_hs_0392","cur_56"]
[3347,"f_盂县二期Ⅲ-042 机舱角度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅲ-042 机舱角度","yc_hs_0392","cur_57"]
[3348,"f_盂县二期Ⅲ-042 1#桨叶片角度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅲ-042 1#桨叶片角度","yc_hs_0392","cur_58"]
[3349,"f_盂县二期Ⅲ-042 2#桨叶片角度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅲ-042 2#桨叶片角度","yc_hs_0392","cur_59"]
[3350,"f_盂县二期Ⅲ-042 3#桨叶片角度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅲ-042 3#桨叶片角度","yc_hs_0392","cur_60"]
[3351,"f_盂县二期Ⅲ-042 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅲ-042 齿轮箱高速轴非驱动端轴承温度","yc_hs_0392","cur_62"]
[3352,"f_盂县二期Ⅲ-042 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅲ-042 发电机非驱动端轴承温度","yc_hs_0392","cur_63"]
[3353,"f_盂县二期Ⅲ-042 扭揽角度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅲ-042 扭揽角度","yc_hs_0392","cur_70"]
[3354,"f_盂县二期Ⅲ-042 风向","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅲ-042 风向","yc_hs_0392","cur_75"]
[3355,"f_盂县二期Ⅲ-042 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅲ-042 机舱侧向振动(已滤波)","yc_hs_0392","cur_76"]
[3356,"f_盂县二期Ⅲ-042 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅲ-042 机舱轴向振动(已滤波)","yc_hs_0392","cur_77"]
[3357,"f_盂县二期Ⅲ-042 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",42,"SXYX.T2_L1.WTG042.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅲ-042 齿轮箱中速轴非驱动端轴承温度","yc_hs_0392","cur_100"]
[3358,"f_盂县二期Ⅲ-043 风速","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅲ-043 风速","yc_hs_0393","cur_38"]
[3359,"f_盂县二期Ⅲ-043 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅲ-043 机舱中轴线与风向夹角","yc_hs_0393","cur_39"]
[3360,"f_盂县二期Ⅲ-043 发电机有功功率","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅲ-043 发电机有功功率","yc_hs_0393","cur_40"]
[3361,"f_盂县二期Ⅲ-043 发电机转速","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅲ-043 发电机转速","yc_hs_0393","cur_41"]
[3362,"f_盂县二期Ⅲ-043 主轴转速","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅲ-043 主轴转速","yc_hs_0393","cur_51"]
[3363,"f_盂县二期Ⅲ-043 舱外温度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅲ-043 舱外温度","yc_hs_0393","cur_52"]
[3364,"f_盂县二期Ⅲ-043 舱内温度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅲ-043 舱内温度","yc_hs_0393","cur_53"]
[3365,"f_盂县二期Ⅲ-043 主轴承外圈温度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅲ-043 主轴承外圈温度","yc_hs_0393","cur_54"]
[3366,"f_盂县二期Ⅲ-043 齿轮箱油池温度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅲ-043 齿轮箱油池温度","yc_hs_0393","cur_55"]
[3367,"f_盂县二期Ⅲ-043 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅲ-043 发电机定子U相线圈温度","yc_hs_0393","cur_57"]
[3368,"f_盂县二期Ⅲ-043 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅲ-043 发电机定子V相线圈温度","yc_hs_0393","cur_58"]
[3369,"f_盂县二期Ⅲ-043 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅲ-043 发电机定子W相线圈温度","yc_hs_0393","cur_59"]
[3370,"f_盂县二期Ⅲ-043 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅲ-043 发电机驱动端轴承温度","yc_hs_0393","cur_60"]
[3371,"f_盂县二期Ⅲ-043 机舱角度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅲ-043 机舱角度","yc_hs_0393","cur_61"]
[3372,"f_盂县二期Ⅲ-043 1#桨叶片角度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅲ-043 1#桨叶片角度","yc_hs_0393","cur_62"]
[3373,"f_盂县二期Ⅲ-043 2#桨叶片角度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅲ-043 2#桨叶片角度","yc_hs_0393","cur_63"]
[3374,"f_盂县二期Ⅲ-043 3#桨叶片角度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅲ-043 3#桨叶片角度","yc_hs_0393","cur_64"]
[3375,"f_盂县二期Ⅲ-043 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅲ-043 齿轮箱高速轴非驱动端轴承温度","yc_hs_0393","cur_66"]
[3376,"f_盂县二期Ⅲ-043 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅲ-043 发电机非驱动端轴承温度","yc_hs_0393","cur_67"]
[3377,"f_盂县二期Ⅲ-043 扭揽角度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅲ-043 扭揽角度","yc_hs_0393","cur_74"]
[3378,"f_盂县二期Ⅲ-043 风向","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅲ-043 风向","yc_hs_0393","cur_79"]
[3379,"f_盂县二期Ⅲ-043 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅲ-043 机舱侧向振动(已滤波)","yc_hs_0393","cur_80"]
[3380,"f_盂县二期Ⅲ-043 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅲ-043 机舱轴向振动(已滤波)","yc_hs_0393","cur_81"]
[3381,"f_盂县二期Ⅲ-043 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",43,"SXYX.T2_L1.WTG043.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅲ-043 齿轮箱中速轴非驱动端轴承温度","yc_hs_0394","cur_04"]
[3382,"f_盂县二期Ⅳ-044 风速","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅳ-044 风速","yc_hs_0394","cur_42"]
[3383,"f_盂县二期Ⅳ-044 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅳ-044 机舱中轴线与风向夹角","yc_hs_0394","cur_43"]
[3384,"f_盂县二期Ⅳ-044 发电机有功功率","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅳ-044 发电机有功功率","yc_hs_0394","cur_44"]
[3385,"f_盂县二期Ⅳ-044 发电机转速","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅳ-044 发电机转速","yc_hs_0394","cur_45"]
[3386,"f_盂县二期Ⅳ-044 主轴转速","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅳ-044 主轴转速","yc_hs_0394","cur_55"]
[3387,"f_盂县二期Ⅳ-044 舱外温度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅳ-044 舱外温度","yc_hs_0394","cur_56"]
[3388,"f_盂县二期Ⅳ-044 舱内温度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅳ-044 舱内温度","yc_hs_0394","cur_57"]
[3389,"f_盂县二期Ⅳ-044 主轴承外圈温度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅳ-044 主轴承外圈温度","yc_hs_0394","cur_58"]
[3390,"f_盂县二期Ⅳ-044 齿轮箱油池温度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅳ-044 齿轮箱油池温度","yc_hs_0394","cur_59"]
[3391,"f_盂县二期Ⅳ-044 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅳ-044 发电机定子U相线圈温度","yc_hs_0394","cur_61"]
[3392,"f_盂县二期Ⅳ-044 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅳ-044 发电机定子V相线圈温度","yc_hs_0394","cur_62"]
[3393,"f_盂县二期Ⅳ-044 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅳ-044 发电机定子W相线圈温度","yc_hs_0394","cur_63"]
[3394,"f_盂县二期Ⅳ-044 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅳ-044 发电机驱动端轴承温度","yc_hs_0394","cur_64"]
[3395,"f_盂县二期Ⅳ-044 机舱角度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅳ-044 机舱角度","yc_hs_0394","cur_65"]
[3396,"f_盂县二期Ⅳ-044 1#桨叶片角度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅳ-044 1#桨叶片角度","yc_hs_0394","cur_66"]
[3397,"f_盂县二期Ⅳ-044 2#桨叶片角度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅳ-044 2#桨叶片角度","yc_hs_0394","cur_67"]
[3398,"f_盂县二期Ⅳ-044 3#桨叶片角度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅳ-044 3#桨叶片角度","yc_hs_0394","cur_68"]
[3399,"f_盂县二期Ⅳ-044 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅳ-044 齿轮箱高速轴非驱动端轴承温度","yc_hs_0394","cur_70"]
[3400,"f_盂县二期Ⅳ-044 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅳ-044 发电机非驱动端轴承温度","yc_hs_0394","cur_71"]
[3401,"f_盂县二期Ⅳ-044 扭揽角度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅳ-044 扭揽角度","yc_hs_0394","cur_78"]
[3402,"f_盂县二期Ⅳ-044 风向","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅳ-044 风向","yc_hs_0394","cur_83"]
[3403,"f_盂县二期Ⅳ-044 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅳ-044 机舱侧向振动(已滤波)","yc_hs_0394","cur_84"]
[3404,"f_盂县二期Ⅳ-044 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅳ-044 机舱轴向振动(已滤波)","yc_hs_0394","cur_85"]
[3405,"f_盂县二期Ⅳ-044 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",44,"SXYX.T2_L2.WTG044.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅳ-044 齿轮箱中速轴非驱动端轴承温度","yc_hs_0395","cur_08"]
[3406,"f_盂县二期Ⅳ-045 风速","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅳ-045 风速","yc_hs_0395","cur_46"]
[3407,"f_盂县二期Ⅳ-045 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅳ-045 机舱中轴线与风向夹角","yc_hs_0395","cur_47"]
[3408,"f_盂县二期Ⅳ-045 发电机有功功率","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅳ-045 发电机有功功率","yc_hs_0395","cur_48"]
[3409,"f_盂县二期Ⅳ-045 发电机转速","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅳ-045 发电机转速","yc_hs_0395","cur_49"]
[3410,"f_盂县二期Ⅳ-045 主轴转速","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅳ-045 主轴转速","yc_hs_0395","cur_59"]
[3411,"f_盂县二期Ⅳ-045 舱外温度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅳ-045 舱外温度","yc_hs_0395","cur_60"]
[3412,"f_盂县二期Ⅳ-045 舱内温度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅳ-045 舱内温度","yc_hs_0395","cur_61"]
[3413,"f_盂县二期Ⅳ-045 主轴承外圈温度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅳ-045 主轴承外圈温度","yc_hs_0395","cur_62"]
[3414,"f_盂县二期Ⅳ-045 齿轮箱油池温度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅳ-045 齿轮箱油池温度","yc_hs_0395","cur_63"]
[3415,"f_盂县二期Ⅳ-045 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅳ-045 发电机定子U相线圈温度","yc_hs_0395","cur_65"]
[3416,"f_盂县二期Ⅳ-045 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅳ-045 发电机定子V相线圈温度","yc_hs_0395","cur_66"]
[3417,"f_盂县二期Ⅳ-045 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅳ-045 发电机定子W相线圈温度","yc_hs_0395","cur_67"]
[3418,"f_盂县二期Ⅳ-045 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅳ-045 发电机驱动端轴承温度","yc_hs_0395","cur_68"]
[3419,"f_盂县二期Ⅳ-045 机舱角度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅳ-045 机舱角度","yc_hs_0395","cur_69"]
[3420,"f_盂县二期Ⅳ-045 1#桨叶片角度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅳ-045 1#桨叶片角度","yc_hs_0395","cur_70"]
[3421,"f_盂县二期Ⅳ-045 2#桨叶片角度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅳ-045 2#桨叶片角度","yc_hs_0395","cur_71"]
[3422,"f_盂县二期Ⅳ-045 3#桨叶片角度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅳ-045 3#桨叶片角度","yc_hs_0395","cur_72"]
[3423,"f_盂县二期Ⅳ-045 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅳ-045 齿轮箱高速轴非驱动端轴承温度","yc_hs_0395","cur_74"]
[3424,"f_盂县二期Ⅳ-045 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅳ-045 发电机非驱动端轴承温度","yc_hs_0395","cur_75"]
[3425,"f_盂县二期Ⅳ-045 扭揽角度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅳ-045 扭揽角度","yc_hs_0395","cur_82"]
[3426,"f_盂县二期Ⅳ-045 风向","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅳ-045 风向","yc_hs_0395","cur_87"]
[3427,"f_盂县二期Ⅳ-045 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅳ-045 机舱侧向振动(已滤波)","yc_hs_0395","cur_88"]
[3428,"f_盂县二期Ⅳ-045 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅳ-045 机舱轴向振动(已滤波)","yc_hs_0395","cur_89"]
[3429,"f_盂县二期Ⅳ-045 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",45,"SXYX.T2_L2.WTG045.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅳ-045 齿轮箱中速轴非驱动端轴承温度","yc_hs_0396","cur_12"]
[3430,"f_盂县二期Ⅳ-046 风速","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅳ-046 风速","yc_hs_0396","cur_50"]
[3431,"f_盂县二期Ⅳ-046 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅳ-046 机舱中轴线与风向夹角","yc_hs_0396","cur_51"]
[3432,"f_盂县二期Ⅳ-046 发电机有功功率","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅳ-046 发电机有功功率","yc_hs_0396","cur_52"]
[3433,"f_盂县二期Ⅳ-046 发电机转速","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅳ-046 发电机转速","yc_hs_0396","cur_53"]
[3434,"f_盂县二期Ⅳ-046 主轴转速","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅳ-046 主轴转速","yc_hs_0396","cur_63"]
[3435,"f_盂县二期Ⅳ-046 舱外温度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅳ-046 舱外温度","yc_hs_0396","cur_64"]
[3436,"f_盂县二期Ⅳ-046 舱内温度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅳ-046 舱内温度","yc_hs_0396","cur_65"]
[3437,"f_盂县二期Ⅳ-046 主轴承外圈温度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅳ-046 主轴承外圈温度","yc_hs_0396","cur_66"]
[3438,"f_盂县二期Ⅳ-046 齿轮箱油池温度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅳ-046 齿轮箱油池温度","yc_hs_0396","cur_67"]
[3439,"f_盂县二期Ⅳ-046 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅳ-046 发电机定子U相线圈温度","yc_hs_0396","cur_69"]
[3440,"f_盂县二期Ⅳ-046 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅳ-046 发电机定子V相线圈温度","yc_hs_0396","cur_70"]
[3441,"f_盂县二期Ⅳ-046 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅳ-046 发电机定子W相线圈温度","yc_hs_0396","cur_71"]
[3442,"f_盂县二期Ⅳ-046 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅳ-046 发电机驱动端轴承温度","yc_hs_0396","cur_72"]
[3443,"f_盂县二期Ⅳ-046 机舱角度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅳ-046 机舱角度","yc_hs_0396","cur_73"]
[3444,"f_盂县二期Ⅳ-046 1#桨叶片角度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅳ-046 1#桨叶片角度","yc_hs_0396","cur_74"]
[3445,"f_盂县二期Ⅳ-046 2#桨叶片角度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅳ-046 2#桨叶片角度","yc_hs_0396","cur_75"]
[3446,"f_盂县二期Ⅳ-046 3#桨叶片角度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅳ-046 3#桨叶片角度","yc_hs_0396","cur_76"]
[3447,"f_盂县二期Ⅳ-046 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅳ-046 齿轮箱高速轴非驱动端轴承温度","yc_hs_0396","cur_78"]
[3448,"f_盂县二期Ⅳ-046 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅳ-046 发电机非驱动端轴承温度","yc_hs_0396","cur_79"]
[3449,"f_盂县二期Ⅳ-046 扭揽角度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅳ-046 扭揽角度","yc_hs_0396","cur_86"]
[3450,"f_盂县二期Ⅳ-046 风向","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅳ-046 风向","yc_hs_0396","cur_91"]
[3451,"f_盂县二期Ⅳ-046 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅳ-046 机舱侧向振动(已滤波)","yc_hs_0396","cur_92"]
[3452,"f_盂县二期Ⅳ-046 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅳ-046 机舱轴向振动(已滤波)","yc_hs_0396","cur_93"]
[3453,"f_盂县二期Ⅳ-046 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",46,"SXYX.T2_L2.WTG046.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅳ-046 齿轮箱中速轴非驱动端轴承温度","yc_hs_0397","cur_16"]
[3454,"f_盂县二期Ⅳ-047 风速","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅳ-047 风速","yc_hs_0397","cur_54"]
[3455,"f_盂县二期Ⅳ-047 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅳ-047 机舱中轴线与风向夹角","yc_hs_0397","cur_55"]
[3456,"f_盂县二期Ⅳ-047 发电机有功功率","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅳ-047 发电机有功功率","yc_hs_0397","cur_56"]
[3457,"f_盂县二期Ⅳ-047 发电机转速","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅳ-047 发电机转速","yc_hs_0397","cur_57"]
[3458,"f_盂县二期Ⅳ-047 主轴转速","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅳ-047 主轴转速","yc_hs_0397","cur_67"]
[3459,"f_盂县二期Ⅳ-047 舱外温度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅳ-047 舱外温度","yc_hs_0397","cur_68"]
[3460,"f_盂县二期Ⅳ-047 舱内温度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅳ-047 舱内温度","yc_hs_0397","cur_69"]
[3461,"f_盂县二期Ⅳ-047 主轴承外圈温度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅳ-047 主轴承外圈温度","yc_hs_0397","cur_70"]
[3462,"f_盂县二期Ⅳ-047 齿轮箱油池温度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅳ-047 齿轮箱油池温度","yc_hs_0397","cur_71"]
[3463,"f_盂县二期Ⅳ-047 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅳ-047 发电机定子U相线圈温度","yc_hs_0397","cur_73"]
[3464,"f_盂县二期Ⅳ-047 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅳ-047 发电机定子V相线圈温度","yc_hs_0397","cur_74"]
[3465,"f_盂县二期Ⅳ-047 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅳ-047 发电机定子W相线圈温度","yc_hs_0397","cur_75"]
[3466,"f_盂县二期Ⅳ-047 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅳ-047 发电机驱动端轴承温度","yc_hs_0397","cur_76"]
[3467,"f_盂县二期Ⅳ-047 机舱角度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅳ-047 机舱角度","yc_hs_0397","cur_77"]
[3468,"f_盂县二期Ⅳ-047 1#桨叶片角度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅳ-047 1#桨叶片角度","yc_hs_0397","cur_78"]
[3469,"f_盂县二期Ⅳ-047 2#桨叶片角度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅳ-047 2#桨叶片角度","yc_hs_0397","cur_79"]
[3470,"f_盂县二期Ⅳ-047 3#桨叶片角度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅳ-047 3#桨叶片角度","yc_hs_0397","cur_80"]
[3471,"f_盂县二期Ⅳ-047 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅳ-047 齿轮箱高速轴非驱动端轴承温度","yc_hs_0397","cur_82"]
[3472,"f_盂县二期Ⅳ-047 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅳ-047 发电机非驱动端轴承温度","yc_hs_0397","cur_83"]
[3473,"f_盂县二期Ⅳ-047 扭揽角度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅳ-047 扭揽角度","yc_hs_0397","cur_90"]
[3474,"f_盂县二期Ⅳ-047 风向","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅳ-047 风向","yc_hs_0397","cur_95"]
[3475,"f_盂县二期Ⅳ-047 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅳ-047 机舱侧向振动(已滤波)","yc_hs_0397","cur_96"]
[3476,"f_盂县二期Ⅳ-047 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅳ-047 机舱轴向振动(已滤波)","yc_hs_0397","cur_97"]
[3477,"f_盂县二期Ⅳ-047 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",47,"SXYX.T2_L2.WTG047.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅳ-047 齿轮箱中速轴非驱动端轴承温度","yc_hs_0398","cur_20"]
[3478,"f_盂县二期Ⅳ-048 风速","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅳ-048 风速","yc_hs_0398","cur_58"]
[3479,"f_盂县二期Ⅳ-048 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅳ-048 机舱中轴线与风向夹角","yc_hs_0398","cur_59"]
[3480,"f_盂县二期Ⅳ-048 发电机有功功率","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅳ-048 发电机有功功率","yc_hs_0398","cur_60"]
[3481,"f_盂县二期Ⅳ-048 发电机转速","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅳ-048 发电机转速","yc_hs_0398","cur_61"]
[3482,"f_盂县二期Ⅳ-048 主轴转速","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅳ-048 主轴转速","yc_hs_0398","cur_71"]
[3483,"f_盂县二期Ⅳ-048 舱外温度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅳ-048 舱外温度","yc_hs_0398","cur_72"]
[3484,"f_盂县二期Ⅳ-048 舱内温度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅳ-048 舱内温度","yc_hs_0398","cur_73"]
[3485,"f_盂县二期Ⅳ-048 主轴承外圈温度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅳ-048 主轴承外圈温度","yc_hs_0398","cur_74"]
[3486,"f_盂县二期Ⅳ-048 齿轮箱油池温度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅳ-048 齿轮箱油池温度","yc_hs_0398","cur_75"]
[3487,"f_盂县二期Ⅳ-048 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅳ-048 发电机定子U相线圈温度","yc_hs_0398","cur_77"]
[3488,"f_盂县二期Ⅳ-048 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅳ-048 发电机定子V相线圈温度","yc_hs_0398","cur_78"]
[3489,"f_盂县二期Ⅳ-048 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅳ-048 发电机定子W相线圈温度","yc_hs_0398","cur_79"]
[3490,"f_盂县二期Ⅳ-048 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅳ-048 发电机驱动端轴承温度","yc_hs_0398","cur_80"]
[3491,"f_盂县二期Ⅳ-048 机舱角度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅳ-048 机舱角度","yc_hs_0398","cur_81"]
[3492,"f_盂县二期Ⅳ-048 1#桨叶片角度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅳ-048 1#桨叶片角度","yc_hs_0398","cur_82"]
[3493,"f_盂县二期Ⅳ-048 2#桨叶片角度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅳ-048 2#桨叶片角度","yc_hs_0398","cur_83"]
[3494,"f_盂县二期Ⅳ-048 3#桨叶片角度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅳ-048 3#桨叶片角度","yc_hs_0398","cur_84"]
[3495,"f_盂县二期Ⅳ-048 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅳ-048 齿轮箱高速轴非驱动端轴承温度","yc_hs_0398","cur_86"]
[3496,"f_盂县二期Ⅳ-048 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅳ-048 发电机非驱动端轴承温度","yc_hs_0398","cur_87"]
[3497,"f_盂县二期Ⅳ-048 扭揽角度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅳ-048 扭揽角度","yc_hs_0398","cur_94"]
[3498,"f_盂县二期Ⅳ-048 风向","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅳ-048 风向","yc_hs_0398","cur_99"]
[3499,"f_盂县二期Ⅳ-048 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅳ-048 机舱侧向振动(已滤波)","yc_hs_0398","cur_100"]
[3500,"f_盂县二期Ⅳ-048 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅳ-048 机舱轴向振动(已滤波)","yc_hs_0399","cur_01"]
[3501,"f_盂县二期Ⅳ-048 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",48,"SXYX.T2_L2.WTG048.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅳ-048 齿轮箱中速轴非驱动端轴承温度","yc_hs_0399","cur_24"]
[3502,"f_盂县二期Ⅳ-049 风速","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅳ-049 风速","yc_hs_0399","cur_62"]
[3503,"f_盂县二期Ⅳ-049 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅳ-049 机舱中轴线与风向夹角","yc_hs_0399","cur_63"]
[3504,"f_盂县二期Ⅳ-049 发电机有功功率","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅳ-049 发电机有功功率","yc_hs_0399","cur_64"]
[3505,"f_盂县二期Ⅳ-049 发电机转速","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅳ-049 发电机转速","yc_hs_0399","cur_65"]
[3506,"f_盂县二期Ⅳ-049 主轴转速","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅳ-049 主轴转速","yc_hs_0399","cur_75"]
[3507,"f_盂县二期Ⅳ-049 舱外温度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅳ-049 舱外温度","yc_hs_0399","cur_76"]
[3508,"f_盂县二期Ⅳ-049 舱内温度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅳ-049 舱内温度","yc_hs_0399","cur_77"]
[3509,"f_盂县二期Ⅳ-049 主轴承外圈温度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅳ-049 主轴承外圈温度","yc_hs_0399","cur_78"]
[3510,"f_盂县二期Ⅳ-049 齿轮箱油池温度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅳ-049 齿轮箱油池温度","yc_hs_0399","cur_79"]
[3511,"f_盂县二期Ⅳ-049 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅳ-049 发电机定子U相线圈温度","yc_hs_0399","cur_81"]
[3512,"f_盂县二期Ⅳ-049 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅳ-049 发电机定子V相线圈温度","yc_hs_0399","cur_82"]
[3513,"f_盂县二期Ⅳ-049 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅳ-049 发电机定子W相线圈温度","yc_hs_0399","cur_83"]
[3514,"f_盂县二期Ⅳ-049 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅳ-049 发电机驱动端轴承温度","yc_hs_0399","cur_84"]
[3515,"f_盂县二期Ⅳ-049 机舱角度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅳ-049 机舱角度","yc_hs_0399","cur_85"]
[3516,"f_盂县二期Ⅳ-049 1#桨叶片角度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅳ-049 1#桨叶片角度","yc_hs_0399","cur_86"]
[3517,"f_盂县二期Ⅳ-049 2#桨叶片角度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅳ-049 2#桨叶片角度","yc_hs_0399","cur_87"]
[3518,"f_盂县二期Ⅳ-049 3#桨叶片角度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅳ-049 3#桨叶片角度","yc_hs_0399","cur_88"]
[3519,"f_盂县二期Ⅳ-049 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅳ-049 齿轮箱高速轴非驱动端轴承温度","yc_hs_0399","cur_90"]
[3520,"f_盂县二期Ⅳ-049 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅳ-049 发电机非驱动端轴承温度","yc_hs_0399","cur_91"]
[3521,"f_盂县二期Ⅳ-049 扭揽角度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅳ-049 扭揽角度","yc_hs_0399","cur_98"]
[3522,"f_盂县二期Ⅳ-049 风向","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅳ-049 风向","yc_hs_0400","cur_03"]
[3523,"f_盂县二期Ⅳ-049 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅳ-049 机舱侧向振动(已滤波)","yc_hs_0400","cur_04"]
[3524,"f_盂县二期Ⅳ-049 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅳ-049 机舱轴向振动(已滤波)","yc_hs_0400","cur_05"]
[3525,"f_盂县二期Ⅳ-049 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",49,"SXYX.T2_L2.WTG049.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅳ-049 齿轮箱中速轴非驱动端轴承温度","yc_hs_0400","cur_28"]
[3526,"f_盂县二期Ⅳ-050 风速","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅳ-050 风速","yc_hs_0400","cur_66"]
[3527,"f_盂县二期Ⅳ-050 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅳ-050 机舱中轴线与风向夹角","yc_hs_0400","cur_67"]
[3528,"f_盂县二期Ⅳ-050 发电机有功功率","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅳ-050 发电机有功功率","yc_hs_0400","cur_68"]
[3529,"f_盂县二期Ⅳ-050 发电机转速","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅳ-050 发电机转速","yc_hs_0400","cur_69"]
[3530,"f_盂县二期Ⅳ-050 主轴转速","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅳ-050 主轴转速","yc_hs_0400","cur_79"]
[3531,"f_盂县二期Ⅳ-050 舱外温度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅳ-050 舱外温度","yc_hs_0400","cur_80"]
[3532,"f_盂县二期Ⅳ-050 舱内温度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅳ-050 舱内温度","yc_hs_0400","cur_81"]
[3533,"f_盂县二期Ⅳ-050 主轴承外圈温度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅳ-050 主轴承外圈温度","yc_hs_0400","cur_82"]
[3534,"f_盂县二期Ⅳ-050 齿轮箱油池温度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅳ-050 齿轮箱油池温度","yc_hs_0400","cur_83"]
[3535,"f_盂县二期Ⅳ-050 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅳ-050 发电机定子U相线圈温度","yc_hs_0400","cur_85"]
[3536,"f_盂县二期Ⅳ-050 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅳ-050 发电机定子V相线圈温度","yc_hs_0400","cur_86"]
[3537,"f_盂县二期Ⅳ-050 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅳ-050 发电机定子W相线圈温度","yc_hs_0400","cur_87"]
[3538,"f_盂县二期Ⅳ-050 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅳ-050 发电机驱动端轴承温度","yc_hs_0400","cur_88"]
[3539,"f_盂县二期Ⅳ-050 机舱角度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅳ-050 机舱角度","yc_hs_0400","cur_89"]
[3540,"f_盂县二期Ⅳ-050 1#桨叶片角度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅳ-050 1#桨叶片角度","yc_hs_0400","cur_90"]
[3541,"f_盂县二期Ⅳ-050 2#桨叶片角度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅳ-050 2#桨叶片角度","yc_hs_0400","cur_91"]
[3542,"f_盂县二期Ⅳ-050 3#桨叶片角度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅳ-050 3#桨叶片角度","yc_hs_0400","cur_92"]
[3543,"f_盂县二期Ⅳ-050 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅳ-050 齿轮箱高速轴非驱动端轴承温度","yc_hs_0400","cur_94"]
[3544,"f_盂县二期Ⅳ-050 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅳ-050 发电机非驱动端轴承温度","yc_hs_0400","cur_95"]
[3545,"f_盂县二期Ⅳ-050 扭揽角度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅳ-050 扭揽角度","yc_hs_0401","cur_02"]
[3546,"f_盂县二期Ⅳ-050 风向","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅳ-050 风向","yc_hs_0401","cur_07"]
[3547,"f_盂县二期Ⅳ-050 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅳ-050 机舱侧向振动(已滤波)","yc_hs_0401","cur_08"]
[3548,"f_盂县二期Ⅳ-050 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅳ-050 机舱轴向振动(已滤波)","yc_hs_0401","cur_09"]
[3549,"f_盂县二期Ⅳ-050 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",50,"SXYX.T2_L2.WTG050.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅳ-050 齿轮箱中速轴非驱动端轴承温度","yc_hs_0401","cur_32"]
[3550,"f_盂县二期Ⅳ-051 风速","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅳ-051 风速","yc_hs_0401","cur_70"]
[3551,"f_盂县二期Ⅳ-051 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅳ-051 机舱中轴线与风向夹角","yc_hs_0401","cur_71"]
[3552,"f_盂县二期Ⅳ-051 发电机有功功率","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅳ-051 发电机有功功率","yc_hs_0401","cur_72"]
[3553,"f_盂县二期Ⅳ-051 发电机转速","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅳ-051 发电机转速","yc_hs_0401","cur_73"]
[3554,"f_盂县二期Ⅳ-051 主轴转速","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅳ-051 主轴转速","yc_hs_0401","cur_83"]
[3555,"f_盂县二期Ⅳ-051 舱外温度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅳ-051 舱外温度","yc_hs_0401","cur_84"]
[3556,"f_盂县二期Ⅳ-051 舱内温度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅳ-051 舱内温度","yc_hs_0401","cur_85"]
[3557,"f_盂县二期Ⅳ-051 主轴承外圈温度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅳ-051 主轴承外圈温度","yc_hs_0401","cur_86"]
[3558,"f_盂县二期Ⅳ-051 齿轮箱油池温度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅳ-051 齿轮箱油池温度","yc_hs_0401","cur_87"]
[3559,"f_盂县二期Ⅳ-051 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅳ-051 发电机定子U相线圈温度","yc_hs_0401","cur_89"]
[3560,"f_盂县二期Ⅳ-051 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅳ-051 发电机定子V相线圈温度","yc_hs_0401","cur_90"]
[3561,"f_盂县二期Ⅳ-051 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅳ-051 发电机定子W相线圈温度","yc_hs_0401","cur_91"]
[3562,"f_盂县二期Ⅳ-051 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅳ-051 发电机驱动端轴承温度","yc_hs_0401","cur_92"]
[3563,"f_盂县二期Ⅳ-051 机舱角度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅳ-051 机舱角度","yc_hs_0401","cur_93"]
[3564,"f_盂县二期Ⅳ-051 1#桨叶片角度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅳ-051 1#桨叶片角度","yc_hs_0401","cur_94"]
[3565,"f_盂县二期Ⅳ-051 2#桨叶片角度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅳ-051 2#桨叶片角度","yc_hs_0401","cur_95"]
[3566,"f_盂县二期Ⅳ-051 3#桨叶片角度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅳ-051 3#桨叶片角度","yc_hs_0401","cur_96"]
[3567,"f_盂县二期Ⅳ-051 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅳ-051 齿轮箱高速轴非驱动端轴承温度","yc_hs_0401","cur_98"]
[3568,"f_盂县二期Ⅳ-051 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅳ-051 发电机非驱动端轴承温度","yc_hs_0401","cur_99"]
[3569,"f_盂县二期Ⅳ-051 扭揽角度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅳ-051 扭揽角度","yc_hs_0402","cur_06"]
[3570,"f_盂县二期Ⅳ-051 风向","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅳ-051 风向","yc_hs_0402","cur_11"]
[3571,"f_盂县二期Ⅳ-051 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅳ-051 机舱侧向振动(已滤波)","yc_hs_0402","cur_12"]
[3572,"f_盂县二期Ⅳ-051 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅳ-051 机舱轴向振动(已滤波)","yc_hs_0402","cur_13"]
[3573,"f_盂县二期Ⅳ-051 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",51,"SXYX.T2_L2.WTG051.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅳ-051 齿轮箱中速轴非驱动端轴承温度","yc_hs_0402","cur_36"]
[3574,"f_盂县二期Ⅳ-052 风速","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅳ-052 风速","yc_hs_0402","cur_74"]
[3575,"f_盂县二期Ⅳ-052 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅳ-052 机舱中轴线与风向夹角","yc_hs_0402","cur_75"]
[3576,"f_盂县二期Ⅳ-052 发电机有功功率","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅳ-052 发电机有功功率","yc_hs_0402","cur_76"]
[3577,"f_盂县二期Ⅳ-052 发电机转速","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅳ-052 发电机转速","yc_hs_0402","cur_77"]
[3578,"f_盂县二期Ⅳ-052 主轴转速","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅳ-052 主轴转速","yc_hs_0402","cur_87"]
[3579,"f_盂县二期Ⅳ-052 舱外温度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅳ-052 舱外温度","yc_hs_0402","cur_88"]
[3580,"f_盂县二期Ⅳ-052 舱内温度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅳ-052 舱内温度","yc_hs_0402","cur_89"]
[3581,"f_盂县二期Ⅳ-052 主轴承外圈温度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅳ-052 主轴承外圈温度","yc_hs_0402","cur_90"]
[3582,"f_盂县二期Ⅳ-052 齿轮箱油池温度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅳ-052 齿轮箱油池温度","yc_hs_0402","cur_91"]
[3583,"f_盂县二期Ⅳ-052 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅳ-052 发电机定子U相线圈温度","yc_hs_0402","cur_93"]
[3584,"f_盂县二期Ⅳ-052 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅳ-052 发电机定子V相线圈温度","yc_hs_0402","cur_94"]
[3585,"f_盂县二期Ⅳ-052 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅳ-052 发电机定子W相线圈温度","yc_hs_0402","cur_95"]
[3586,"f_盂县二期Ⅳ-052 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅳ-052 发电机驱动端轴承温度","yc_hs_0402","cur_96"]
[3587,"f_盂县二期Ⅳ-052 机舱角度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅳ-052 机舱角度","yc_hs_0402","cur_97"]
[3588,"f_盂县二期Ⅳ-052 1#桨叶片角度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅳ-052 1#桨叶片角度","yc_hs_0402","cur_98"]
[3589,"f_盂县二期Ⅳ-052 2#桨叶片角度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅳ-052 2#桨叶片角度","yc_hs_0402","cur_99"]
[3590,"f_盂县二期Ⅳ-052 3#桨叶片角度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅳ-052 3#桨叶片角度","yc_hs_0402","cur_100"]
[3591,"f_盂县二期Ⅳ-052 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅳ-052 齿轮箱高速轴非驱动端轴承温度","yc_hs_0403","cur_02"]
[3592,"f_盂县二期Ⅳ-052 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅳ-052 发电机非驱动端轴承温度","yc_hs_0403","cur_03"]
[3593,"f_盂县二期Ⅳ-052 扭揽角度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅳ-052 扭揽角度","yc_hs_0403","cur_10"]
[3594,"f_盂县二期Ⅳ-052 风向","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅳ-052 风向","yc_hs_0403","cur_15"]
[3595,"f_盂县二期Ⅳ-052 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅳ-052 机舱侧向振动(已滤波)","yc_hs_0403","cur_16"]
[3596,"f_盂县二期Ⅳ-052 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅳ-052 机舱轴向振动(已滤波)","yc_hs_0403","cur_17"]
[3597,"f_盂县二期Ⅳ-052 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",52,"SXYX.T2_L2.WTG052.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅳ-052 齿轮箱中速轴非驱动端轴承温度","yc_hs_0403","cur_40"]
[3598,"f_盂县二期Ⅳ-053 风速","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅳ-053 风速","yc_hs_0403","cur_78"]
[3599,"f_盂县二期Ⅳ-053 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅳ-053 机舱中轴线与风向夹角","yc_hs_0403","cur_79"]
[3600,"f_盂县二期Ⅳ-053 发电机有功功率","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅳ-053 发电机有功功率","yc_hs_0403","cur_80"]
[3601,"f_盂县二期Ⅳ-053 发电机转速","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅳ-053 发电机转速","yc_hs_0403","cur_81"]
[3602,"f_盂县二期Ⅳ-053 主轴转速","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅳ-053 主轴转速","yc_hs_0403","cur_91"]
[3603,"f_盂县二期Ⅳ-053 舱外温度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅳ-053 舱外温度","yc_hs_0403","cur_92"]
[3604,"f_盂县二期Ⅳ-053 舱内温度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅳ-053 舱内温度","yc_hs_0403","cur_93"]
[3605,"f_盂县二期Ⅳ-053 主轴承外圈温度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅳ-053 主轴承外圈温度","yc_hs_0403","cur_94"]
[3606,"f_盂县二期Ⅳ-053 齿轮箱油池温度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅳ-053 齿轮箱油池温度","yc_hs_0403","cur_95"]
[3607,"f_盂县二期Ⅳ-053 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅳ-053 发电机定子U相线圈温度","yc_hs_0403","cur_97"]
[3608,"f_盂县二期Ⅳ-053 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅳ-053 发电机定子V相线圈温度","yc_hs_0403","cur_98"]
[3609,"f_盂县二期Ⅳ-053 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅳ-053 发电机定子W相线圈温度","yc_hs_0403","cur_99"]
[3610,"f_盂县二期Ⅳ-053 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅳ-053 发电机驱动端轴承温度","yc_hs_0403","cur_100"]
[3611,"f_盂县二期Ⅳ-053 机舱角度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅳ-053 机舱角度","yc_hs_0404","cur_01"]
[3612,"f_盂县二期Ⅳ-053 1#桨叶片角度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅳ-053 1#桨叶片角度","yc_hs_0404","cur_02"]
[3613,"f_盂县二期Ⅳ-053 2#桨叶片角度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅳ-053 2#桨叶片角度","yc_hs_0404","cur_03"]
[3614,"f_盂县二期Ⅳ-053 3#桨叶片角度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅳ-053 3#桨叶片角度","yc_hs_0404","cur_04"]
[3615,"f_盂县二期Ⅳ-053 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅳ-053 齿轮箱高速轴非驱动端轴承温度","yc_hs_0404","cur_06"]
[3616,"f_盂县二期Ⅳ-053 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅳ-053 发电机非驱动端轴承温度","yc_hs_0404","cur_07"]
[3617,"f_盂县二期Ⅳ-053 扭揽角度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅳ-053 扭揽角度","yc_hs_0404","cur_14"]
[3618,"f_盂县二期Ⅳ-053 风向","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅳ-053 风向","yc_hs_0404","cur_19"]
[3619,"f_盂县二期Ⅳ-053 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅳ-053 机舱侧向振动(已滤波)","yc_hs_0404","cur_20"]
[3620,"f_盂县二期Ⅳ-053 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅳ-053 机舱轴向振动(已滤波)","yc_hs_0404","cur_21"]
[3621,"f_盂县二期Ⅳ-053 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",53,"SXYX.T2_L2.WTG053.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅳ-053 齿轮箱中速轴非驱动端轴承温度","yc_hs_0404","cur_44"]
[3622,"f_盂县二期Ⅳ-054 风速","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅳ-054 风速","yc_hs_0404","cur_82"]
[3623,"f_盂县二期Ⅳ-054 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅳ-054 机舱中轴线与风向夹角","yc_hs_0404","cur_83"]
[3624,"f_盂县二期Ⅳ-054 发电机有功功率","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅳ-054 发电机有功功率","yc_hs_0404","cur_84"]
[3625,"f_盂县二期Ⅳ-054 发电机转速","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅳ-054 发电机转速","yc_hs_0404","cur_85"]
[3626,"f_盂县二期Ⅳ-054 主轴转速","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅳ-054 主轴转速","yc_hs_0404","cur_95"]
[3627,"f_盂县二期Ⅳ-054 舱外温度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅳ-054 舱外温度","yc_hs_0404","cur_96"]
[3628,"f_盂县二期Ⅳ-054 舱内温度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅳ-054 舱内温度","yc_hs_0404","cur_97"]
[3629,"f_盂县二期Ⅳ-054 主轴承外圈温度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅳ-054 主轴承外圈温度","yc_hs_0404","cur_98"]
[3630,"f_盂县二期Ⅳ-054 齿轮箱油池温度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅳ-054 齿轮箱油池温度","yc_hs_0404","cur_99"]
[3631,"f_盂县二期Ⅳ-054 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅳ-054 发电机定子U相线圈温度","yc_hs_0405","cur_01"]
[3632,"f_盂县二期Ⅳ-054 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅳ-054 发电机定子V相线圈温度","yc_hs_0405","cur_02"]
[3633,"f_盂县二期Ⅳ-054 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅳ-054 发电机定子W相线圈温度","yc_hs_0405","cur_03"]
[3634,"f_盂县二期Ⅳ-054 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅳ-054 发电机驱动端轴承温度","yc_hs_0405","cur_04"]
[3635,"f_盂县二期Ⅳ-054 机舱角度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅳ-054 机舱角度","yc_hs_0405","cur_05"]
[3636,"f_盂县二期Ⅳ-054 1#桨叶片角度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅳ-054 1#桨叶片角度","yc_hs_0405","cur_06"]
[3637,"f_盂县二期Ⅳ-054 2#桨叶片角度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅳ-054 2#桨叶片角度","yc_hs_0405","cur_07"]
[3638,"f_盂县二期Ⅳ-054 3#桨叶片角度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅳ-054 3#桨叶片角度","yc_hs_0405","cur_08"]
[3639,"f_盂县二期Ⅳ-054 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅳ-054 齿轮箱高速轴非驱动端轴承温度","yc_hs_0405","cur_10"]
[3640,"f_盂县二期Ⅳ-054 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅳ-054 发电机非驱动端轴承温度","yc_hs_0405","cur_11"]
[3641,"f_盂县二期Ⅳ-054 扭揽角度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅳ-054 扭揽角度","yc_hs_0405","cur_18"]
[3642,"f_盂县二期Ⅳ-054 风向","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅳ-054 风向","yc_hs_0405","cur_23"]
[3643,"f_盂县二期Ⅳ-054 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅳ-054 机舱侧向振动(已滤波)","yc_hs_0405","cur_24"]
[3644,"f_盂县二期Ⅳ-054 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅳ-054 机舱轴向振动(已滤波)","yc_hs_0405","cur_25"]
[3645,"f_盂县二期Ⅳ-054 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",54,"SXYX.T2_L2.WTG054.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅳ-054 齿轮箱中速轴非驱动端轴承温度","yc_hs_0405","cur_48"]
[3646,"f_盂县二期Ⅳ-055 风速","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅳ-055 风速","yc_hs_0405","cur_86"]
[3647,"f_盂县二期Ⅳ-055 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅳ-055 机舱中轴线与风向夹角","yc_hs_0405","cur_87"]
[3648,"f_盂县二期Ⅳ-055 发电机有功功率","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅳ-055 发电机有功功率","yc_hs_0405","cur_88"]
[3649,"f_盂县二期Ⅳ-055 发电机转速","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅳ-055 发电机转速","yc_hs_0405","cur_89"]
[3650,"f_盂县二期Ⅳ-055 主轴转速","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅳ-055 主轴转速","yc_hs_0405","cur_99"]
[3651,"f_盂县二期Ⅳ-055 舱外温度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅳ-055 舱外温度","yc_hs_0405","cur_100"]
[3652,"f_盂县二期Ⅳ-055 舱内温度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅳ-055 舱内温度","yc_hs_0406","cur_01"]
[3653,"f_盂县二期Ⅳ-055 主轴承外圈温度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅳ-055 主轴承外圈温度","yc_hs_0406","cur_02"]
[3654,"f_盂县二期Ⅳ-055 齿轮箱油池温度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅳ-055 齿轮箱油池温度","yc_hs_0406","cur_03"]
[3655,"f_盂县二期Ⅳ-055 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅳ-055 发电机定子U相线圈温度","yc_hs_0406","cur_05"]
[3656,"f_盂县二期Ⅳ-055 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅳ-055 发电机定子V相线圈温度","yc_hs_0406","cur_06"]
[3657,"f_盂县二期Ⅳ-055 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅳ-055 发电机定子W相线圈温度","yc_hs_0406","cur_07"]
[3658,"f_盂县二期Ⅳ-055 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅳ-055 发电机驱动端轴承温度","yc_hs_0406","cur_08"]
[3659,"f_盂县二期Ⅳ-055 机舱角度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅳ-055 机舱角度","yc_hs_0406","cur_09"]
[3660,"f_盂县二期Ⅳ-055 1#桨叶片角度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅳ-055 1#桨叶片角度","yc_hs_0406","cur_10"]
[3661,"f_盂县二期Ⅳ-055 2#桨叶片角度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅳ-055 2#桨叶片角度","yc_hs_0406","cur_11"]
[3662,"f_盂县二期Ⅳ-055 3#桨叶片角度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅳ-055 3#桨叶片角度","yc_hs_0406","cur_12"]
[3663,"f_盂县二期Ⅳ-055 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅳ-055 齿轮箱高速轴非驱动端轴承温度","yc_hs_0406","cur_14"]
[3664,"f_盂县二期Ⅳ-055 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅳ-055 发电机非驱动端轴承温度","yc_hs_0406","cur_15"]
[3665,"f_盂县二期Ⅳ-055 扭揽角度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅳ-055 扭揽角度","yc_hs_0406","cur_22"]
[3666,"f_盂县二期Ⅳ-055 风向","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅳ-055 风向","yc_hs_0406","cur_27"]
[3667,"f_盂县二期Ⅳ-055 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅳ-055 机舱侧向振动(已滤波)","yc_hs_0406","cur_28"]
[3668,"f_盂县二期Ⅳ-055 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅳ-055 机舱轴向振动(已滤波)","yc_hs_0406","cur_29"]
[3669,"f_盂县二期Ⅳ-055 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",55,"SXYX.T2_L2.WTG055.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅳ-055 齿轮箱中速轴非驱动端轴承温度","yc_hs_0406","cur_52"]
[3670,"f_盂县二期Ⅳ-056 风速","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WNAC.WindSpeed","风速","wind_velocity","f_盂县二期Ⅳ-056 风速","yc_hs_0406","cur_90"]
[3671,"f_盂县二期Ⅳ-056 机舱中轴线与风向夹角","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WNAC.WindVaneDirection","对风角度","yaw_error1","f_盂县二期Ⅳ-056 机舱中轴线与风向夹角","yc_hs_0406","cur_91"]
[3672,"f_盂县二期Ⅳ-056 发电机有功功率","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WGEN.GenActivePW","有功功率","active_power","f_盂县二期Ⅳ-056 发电机有功功率","yc_hs_0406","cur_92"]
[3673,"f_盂县二期Ⅳ-056 发电机转速","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WGEN.GenSpd","发电机转速","generator_speed","f_盂县二期Ⅳ-056 发电机转速","yc_hs_0406","cur_93"]
[3674,"f_盂县二期Ⅳ-056 主轴转速","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县二期Ⅳ-056 主轴转速","yc_hs_0407","cur_03"]
[3675,"f_盂县二期Ⅳ-056 舱外温度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县二期Ⅳ-056 舱外温度","yc_hs_0407","cur_04"]
[3676,"f_盂县二期Ⅳ-056 舱内温度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县二期Ⅳ-056 舱内温度","yc_hs_0407","cur_05"]
[3677,"f_盂县二期Ⅳ-056 主轴承外圈温度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","f_盂县二期Ⅳ-056 主轴承外圈温度","yc_hs_0407","cur_06"]
[3678,"f_盂县二期Ⅳ-056 齿轮箱油池温度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县二期Ⅳ-056 齿轮箱油池温度","yc_hs_0407","cur_07"]
[3679,"f_盂县二期Ⅳ-056 发电机定子U相线圈温度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","f_盂县二期Ⅳ-056 发电机定子U相线圈温度","yc_hs_0407","cur_09"]
[3680,"f_盂县二期Ⅳ-056 发电机定子V相线圈温度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","f_盂县二期Ⅳ-056 发电机定子V相线圈温度","yc_hs_0407","cur_10"]
[3681,"f_盂县二期Ⅳ-056 发电机定子W相线圈温度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","f_盂县二期Ⅳ-056 发电机定子W相线圈温度","yc_hs_0407","cur_11"]
[3682,"f_盂县二期Ⅳ-056 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县二期Ⅳ-056 发电机驱动端轴承温度","yc_hs_0407","cur_12"]
[3683,"f_盂县二期Ⅳ-056 机舱角度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县二期Ⅳ-056 机舱角度","yc_hs_0407","cur_13"]
[3684,"f_盂县二期Ⅳ-056 1#桨叶片角度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县二期Ⅳ-056 1#桨叶片角度","yc_hs_0407","cur_14"]
[3685,"f_盂县二期Ⅳ-056 2#桨叶片角度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县二期Ⅳ-056 2#桨叶片角度","yc_hs_0407","cur_15"]
[3686,"f_盂县二期Ⅳ-056 3#桨叶片角度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县二期Ⅳ-056 3#桨叶片角度","yc_hs_0407","cur_16"]
[3687,"f_盂县二期Ⅳ-056 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县二期Ⅳ-056 齿轮箱高速轴非驱动端轴承温度","yc_hs_0407","cur_18"]
[3688,"f_盂县二期Ⅳ-056 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县二期Ⅳ-056 发电机非驱动端轴承温度","yc_hs_0407","cur_19"]
[3689,"f_盂县二期Ⅳ-056 扭揽角度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县二期Ⅳ-056 扭揽角度","yc_hs_0407","cur_26"]
[3690,"f_盂县二期Ⅳ-056 风向","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县二期Ⅳ-056 风向","yc_hs_0407","cur_31"]
[3691,"f_盂县二期Ⅳ-056 机舱侧向振动(已滤波)","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县二期Ⅳ-056 机舱侧向振动(已滤波)","yc_hs_0407","cur_32"]
[3692,"f_盂县二期Ⅳ-056 机舱轴向振动(已滤波)","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县二期Ⅳ-056 机舱轴向振动(已滤波)","yc_hs_0407","cur_33"]
[3693,"f_盂县二期Ⅳ-056 齿轮箱中速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",56,"SXYX.T2_L2.WTG056.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","f_盂县二期Ⅳ-056 齿轮箱中速轴非驱动端轴承温度","yc_hs_0407","cur_56"]
[3694,"b_右玉二期Ⅳ-034 发电机有功功率","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅳ-034 发电机有功功率","yc_hs_0409","cur_16"]
[3695,"b_右玉二期Ⅳ-034 发电机转速","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅳ-034 发电机转速","yc_hs_0409","cur_22"]
[3696,"b_右玉二期Ⅳ-034 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅳ-034 发电机驱动端轴承温度","yc_hs_0409","cur_26"]
[3697,"b_右玉二期Ⅳ-034 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅳ-034 发电机非驱动端轴承温度","yc_hs_0409","cur_27"]
[3698,"b_右玉二期Ⅳ-034 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅳ-034 发电机定子U相线圈温度","yc_hs_0409","cur_29"]
[3699,"b_右玉二期Ⅳ-034 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅳ-034 发电机定子V相线圈温度","yc_hs_0409","cur_30"]
[3700,"b_右玉二期Ⅳ-034 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅳ-034 发电机定子W相线圈温度","yc_hs_0409","cur_31"]
[3701,"b_右玉二期Ⅳ-034 舱内温度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅳ-034 舱内温度","yc_hs_0409","cur_38"]
[3702,"b_右玉二期Ⅳ-034 舱外温度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅳ-034 舱外温度","yc_hs_0409","cur_40"]
[3703,"b_右玉二期Ⅳ-034 风向","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅳ-034 风向","yc_hs_0409","cur_43"]
[3704,"b_右玉二期Ⅳ-034 风速","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅳ-034 风速","yc_hs_0409","cur_45"]
[3705,"b_右玉二期Ⅳ-034 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅳ-034 机舱中轴线与风向夹角","yc_hs_0409","cur_48"]
[3706,"b_右玉二期Ⅳ-034 1#桨叶片角度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅳ-034 1#桨叶片角度","yc_hs_0409","cur_53"]
[3707,"b_右玉二期Ⅳ-034 2#桨叶片角度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅳ-034 2#桨叶片角度","yc_hs_0409","cur_55"]
[3708,"b_右玉二期Ⅳ-034 3#桨叶片角度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅳ-034 3#桨叶片角度","yc_hs_0409","cur_57"]
[3709,"b_右玉二期Ⅳ-034 主轴转速","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅳ-034 主轴转速","yc_hs_0409","cur_81"]
[3710,"b_右玉二期Ⅳ-034 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅳ-034 齿轮箱高速轴非驱动端轴承温度","yc_hs_0409","cur_85"]
[3711,"b_右玉二期Ⅳ-034 齿轮箱油池温度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅳ-034 齿轮箱油池温度","yc_hs_0409","cur_86"]
[3712,"b_右玉二期Ⅳ-034 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅳ-034 齿轮箱中速轴非驱动端轴承温度","yc_hs_0409","cur_88"]
[3713,"b_右玉二期Ⅳ-034 主轴承外圈温度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅳ-034 主轴承外圈温度","yc_hs_0409","cur_89"]
[3714,"b_右玉二期Ⅳ-034 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅳ-034 机舱侧向振动(已滤波)","yc_hs_0409","cur_99"]
[3715,"b_右玉二期Ⅳ-034 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅳ-034 机舱轴向振动(已滤波)","yc_hs_0410","cur_01"]
[3716,"b_右玉二期Ⅳ-034 机舱角度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅳ-034 机舱角度","yc_hs_0410","cur_02"]
[3717,"b_右玉二期Ⅳ-034 扭缆角度","右玉风光互补电站","WOF34900079",34,"SXYY.T2_L1.WTG034.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅳ-034 扭缆角度","yc_hs_0410","cur_04"]
[3718,"b_右玉二期Ⅳ-035 发电机有功功率","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅳ-035 发电机有功功率","yc_hs_0410","cur_22"]
[3719,"b_右玉二期Ⅳ-035 发电机转速","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅳ-035 发电机转速","yc_hs_0410","cur_28"]
[3720,"b_右玉二期Ⅳ-035 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅳ-035 发电机驱动端轴承温度","yc_hs_0410","cur_32"]
[3721,"b_右玉二期Ⅳ-035 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅳ-035 发电机非驱动端轴承温度","yc_hs_0410","cur_33"]
[3722,"b_右玉二期Ⅳ-035 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅳ-035 发电机定子U相线圈温度","yc_hs_0410","cur_35"]
[3723,"b_右玉二期Ⅳ-035 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅳ-035 发电机定子V相线圈温度","yc_hs_0410","cur_36"]
[3724,"b_右玉二期Ⅳ-035 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅳ-035 发电机定子W相线圈温度","yc_hs_0410","cur_37"]
[3725,"b_右玉二期Ⅳ-035 舱内温度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅳ-035 舱内温度","yc_hs_0410","cur_44"]
[3726,"b_右玉二期Ⅳ-035 舱外温度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅳ-035 舱外温度","yc_hs_0410","cur_46"]
[3727,"b_右玉二期Ⅳ-035 风向","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅳ-035 风向","yc_hs_0410","cur_49"]
[3728,"b_右玉二期Ⅳ-035 风速","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅳ-035 风速","yc_hs_0410","cur_51"]
[3729,"b_右玉二期Ⅳ-035 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅳ-035 机舱中轴线与风向夹角","yc_hs_0410","cur_54"]
[3730,"b_右玉二期Ⅳ-035 1#桨叶片角度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅳ-035 1#桨叶片角度","yc_hs_0410","cur_59"]
[3731,"b_右玉二期Ⅳ-035 2#桨叶片角度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅳ-035 2#桨叶片角度","yc_hs_0410","cur_61"]
[3732,"b_右玉二期Ⅳ-035 3#桨叶片角度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅳ-035 3#桨叶片角度","yc_hs_0410","cur_63"]
[3733,"b_右玉二期Ⅳ-035 主轴转速","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅳ-035 主轴转速","yc_hs_0410","cur_87"]
[3734,"b_右玉二期Ⅳ-035 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅳ-035 齿轮箱高速轴非驱动端轴承温度","yc_hs_0410","cur_91"]
[3735,"b_右玉二期Ⅳ-035 齿轮箱油池温度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅳ-035 齿轮箱油池温度","yc_hs_0410","cur_92"]
[3736,"b_右玉二期Ⅳ-035 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅳ-035 齿轮箱中速轴非驱动端轴承温度","yc_hs_0410","cur_94"]
[3737,"b_右玉二期Ⅳ-035 主轴承外圈温度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅳ-035 主轴承外圈温度","yc_hs_0410","cur_95"]
[3738,"b_右玉二期Ⅳ-035 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅳ-035 机舱侧向振动(已滤波)","yc_hs_0411","cur_05"]
[3739,"b_右玉二期Ⅳ-035 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅳ-035 机舱轴向振动(已滤波)","yc_hs_0411","cur_07"]
[3740,"b_右玉二期Ⅳ-035 机舱角度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅳ-035 机舱角度","yc_hs_0411","cur_08"]
[3741,"b_右玉二期Ⅳ-035 扭缆角度","右玉风光互补电站","WOF34900079",35,"SXYY.T2_L1.WTG035.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅳ-035 扭缆角度","yc_hs_0411","cur_10"]
[3742,"b_右玉二期Ⅳ-036 发电机有功功率","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅳ-036 发电机有功功率","yc_hs_0411","cur_28"]
[3743,"b_右玉二期Ⅳ-036 发电机转速","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅳ-036 发电机转速","yc_hs_0411","cur_34"]
[3744,"b_右玉二期Ⅳ-036 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅳ-036 发电机驱动端轴承温度","yc_hs_0411","cur_38"]
[3745,"b_右玉二期Ⅳ-036 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅳ-036 发电机非驱动端轴承温度","yc_hs_0411","cur_39"]
[3746,"b_右玉二期Ⅳ-036 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅳ-036 发电机定子U相线圈温度","yc_hs_0411","cur_41"]
[3747,"b_右玉二期Ⅳ-036 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅳ-036 发电机定子V相线圈温度","yc_hs_0411","cur_42"]
[3748,"b_右玉二期Ⅳ-036 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅳ-036 发电机定子W相线圈温度","yc_hs_0411","cur_43"]
[3749,"b_右玉二期Ⅳ-036 舱内温度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅳ-036 舱内温度","yc_hs_0411","cur_50"]
[3750,"b_右玉二期Ⅳ-036 舱外温度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅳ-036 舱外温度","yc_hs_0411","cur_52"]
[3751,"b_右玉二期Ⅳ-036 风向","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅳ-036 风向","yc_hs_0411","cur_55"]
[3752,"b_右玉二期Ⅳ-036 风速","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅳ-036 风速","yc_hs_0411","cur_57"]
[3753,"b_右玉二期Ⅳ-036 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅳ-036 机舱中轴线与风向夹角","yc_hs_0411","cur_60"]
[3754,"b_右玉二期Ⅳ-036 1#桨叶片角度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅳ-036 1#桨叶片角度","yc_hs_0411","cur_65"]
[3755,"b_右玉二期Ⅳ-036 2#桨叶片角度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅳ-036 2#桨叶片角度","yc_hs_0411","cur_67"]
[3756,"b_右玉二期Ⅳ-036 3#桨叶片角度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅳ-036 3#桨叶片角度","yc_hs_0411","cur_69"]
[3757,"b_右玉二期Ⅳ-036 主轴转速","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅳ-036 主轴转速","yc_hs_0411","cur_93"]
[3758,"b_右玉二期Ⅳ-036 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅳ-036 齿轮箱高速轴非驱动端轴承温度","yc_hs_0411","cur_97"]
[3759,"b_右玉二期Ⅳ-036 齿轮箱油池温度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅳ-036 齿轮箱油池温度","yc_hs_0411","cur_98"]
[3760,"b_右玉二期Ⅳ-036 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅳ-036 齿轮箱中速轴非驱动端轴承温度","yc_hs_0411","cur_100"]
[3761,"b_右玉二期Ⅳ-036 主轴承外圈温度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅳ-036 主轴承外圈温度","yc_hs_0412","cur_01"]
[3762,"b_右玉二期Ⅳ-036 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅳ-036 机舱侧向振动(已滤波)","yc_hs_0412","cur_11"]
[3763,"b_右玉二期Ⅳ-036 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅳ-036 机舱轴向振动(已滤波)","yc_hs_0412","cur_13"]
[3764,"b_右玉二期Ⅳ-036 机舱角度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅳ-036 机舱角度","yc_hs_0412","cur_14"]
[3765,"b_右玉二期Ⅳ-036 扭缆角度","右玉风光互补电站","WOF34900079",36,"SXYY.T2_L1.WTG036.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅳ-036 扭缆角度","yc_hs_0412","cur_16"]
[3766,"b_右玉二期Ⅳ-037 发电机有功功率","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅳ-037 发电机有功功率","yc_hs_0412","cur_34"]
[3767,"b_右玉二期Ⅳ-037 发电机转速","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅳ-037 发电机转速","yc_hs_0412","cur_40"]
[3768,"b_右玉二期Ⅳ-037 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅳ-037 发电机驱动端轴承温度","yc_hs_0412","cur_44"]
[3769,"b_右玉二期Ⅳ-037 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅳ-037 发电机非驱动端轴承温度","yc_hs_0412","cur_45"]
[3770,"b_右玉二期Ⅳ-037 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅳ-037 发电机定子U相线圈温度","yc_hs_0412","cur_47"]
[3771,"b_右玉二期Ⅳ-037 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅳ-037 发电机定子V相线圈温度","yc_hs_0412","cur_48"]
[3772,"b_右玉二期Ⅳ-037 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅳ-037 发电机定子W相线圈温度","yc_hs_0412","cur_49"]
[3773,"b_右玉二期Ⅳ-037 舱内温度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅳ-037 舱内温度","yc_hs_0412","cur_56"]
[3774,"b_右玉二期Ⅳ-037 舱外温度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅳ-037 舱外温度","yc_hs_0412","cur_58"]
[3775,"b_右玉二期Ⅳ-037 风向","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅳ-037 风向","yc_hs_0412","cur_61"]
[3776,"b_右玉二期Ⅳ-037 风速","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅳ-037 风速","yc_hs_0412","cur_63"]
[3777,"b_右玉二期Ⅳ-037 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅳ-037 机舱中轴线与风向夹角","yc_hs_0412","cur_66"]
[3778,"b_右玉二期Ⅳ-037 1#桨叶片角度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅳ-037 1#桨叶片角度","yc_hs_0412","cur_71"]
[3779,"b_右玉二期Ⅳ-037 2#桨叶片角度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅳ-037 2#桨叶片角度","yc_hs_0412","cur_73"]
[3780,"b_右玉二期Ⅳ-037 3#桨叶片角度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅳ-037 3#桨叶片角度","yc_hs_0412","cur_75"]
[3781,"b_右玉二期Ⅳ-037 主轴转速","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅳ-037 主轴转速","yc_hs_0412","cur_99"]
[3782,"b_右玉二期Ⅳ-037 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅳ-037 齿轮箱高速轴非驱动端轴承温度","yc_hs_0413","cur_03"]
[3783,"b_右玉二期Ⅳ-037 齿轮箱油池温度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅳ-037 齿轮箱油池温度","yc_hs_0413","cur_04"]
[3784,"b_右玉二期Ⅳ-037 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅳ-037 齿轮箱中速轴非驱动端轴承温度","yc_hs_0413","cur_06"]
[3785,"b_右玉二期Ⅳ-037 主轴承外圈温度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅳ-037 主轴承外圈温度","yc_hs_0413","cur_07"]
[3786,"b_右玉二期Ⅳ-037 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅳ-037 机舱侧向振动(已滤波)","yc_hs_0413","cur_17"]
[3787,"b_右玉二期Ⅳ-037 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅳ-037 机舱轴向振动(已滤波)","yc_hs_0413","cur_19"]
[3788,"b_右玉二期Ⅳ-037 机舱角度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅳ-037 机舱角度","yc_hs_0413","cur_20"]
[3789,"b_右玉二期Ⅳ-037 扭缆角度","右玉风光互补电站","WOF34900079",37,"SXYY.T2_L1.WTG037.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅳ-037 扭缆角度","yc_hs_0413","cur_22"]
[3790,"b_右玉二期Ⅳ-038 发电机有功功率","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅳ-038 发电机有功功率","yc_hs_0413","cur_40"]
[3791,"b_右玉二期Ⅳ-038 发电机转速","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅳ-038 发电机转速","yc_hs_0413","cur_46"]
[3792,"b_右玉二期Ⅳ-038 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅳ-038 发电机驱动端轴承温度","yc_hs_0413","cur_50"]
[3793,"b_右玉二期Ⅳ-038 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅳ-038 发电机非驱动端轴承温度","yc_hs_0413","cur_51"]
[3794,"b_右玉二期Ⅳ-038 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅳ-038 发电机定子U相线圈温度","yc_hs_0413","cur_53"]
[3795,"b_右玉二期Ⅳ-038 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅳ-038 发电机定子V相线圈温度","yc_hs_0413","cur_54"]
[3796,"b_右玉二期Ⅳ-038 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅳ-038 发电机定子W相线圈温度","yc_hs_0413","cur_55"]
[3797,"b_右玉二期Ⅳ-038 舱内温度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅳ-038 舱内温度","yc_hs_0413","cur_62"]
[3798,"b_右玉二期Ⅳ-038 舱外温度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅳ-038 舱外温度","yc_hs_0413","cur_64"]
[3799,"b_右玉二期Ⅳ-038 风向","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅳ-038 风向","yc_hs_0413","cur_67"]
[3800,"b_右玉二期Ⅳ-038 风速","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅳ-038 风速","yc_hs_0413","cur_69"]
[3801,"b_右玉二期Ⅳ-038 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅳ-038 机舱中轴线与风向夹角","yc_hs_0413","cur_72"]
[3802,"b_右玉二期Ⅳ-038 1#桨叶片角度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅳ-038 1#桨叶片角度","yc_hs_0413","cur_77"]
[3803,"b_右玉二期Ⅳ-038 2#桨叶片角度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅳ-038 2#桨叶片角度","yc_hs_0413","cur_79"]
[3804,"b_右玉二期Ⅳ-038 3#桨叶片角度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅳ-038 3#桨叶片角度","yc_hs_0413","cur_81"]
[3805,"b_右玉二期Ⅳ-038 主轴转速","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅳ-038 主轴转速","yc_hs_0414","cur_05"]
[3806,"b_右玉二期Ⅳ-038 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅳ-038 齿轮箱高速轴非驱动端轴承温度","yc_hs_0414","cur_09"]
[3807,"b_右玉二期Ⅳ-038 齿轮箱油池温度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅳ-038 齿轮箱油池温度","yc_hs_0414","cur_10"]
[3808,"b_右玉二期Ⅳ-038 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅳ-038 齿轮箱中速轴非驱动端轴承温度","yc_hs_0414","cur_12"]
[3809,"b_右玉二期Ⅳ-038 主轴承外圈温度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅳ-038 主轴承外圈温度","yc_hs_0414","cur_13"]
[3810,"b_右玉二期Ⅳ-038 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅳ-038 机舱侧向振动(已滤波)","yc_hs_0414","cur_23"]
[3811,"b_右玉二期Ⅳ-038 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅳ-038 机舱轴向振动(已滤波)","yc_hs_0414","cur_25"]
[3812,"b_右玉二期Ⅳ-038 机舱角度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅳ-038 机舱角度","yc_hs_0414","cur_26"]
[3813,"b_右玉二期Ⅳ-038 扭缆角度","右玉风光互补电站","WOF34900079",38,"SXYY.T2_L1.WTG038.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅳ-038 扭缆角度","yc_hs_0414","cur_28"]
[3814,"b_右玉二期Ⅳ-039 发电机有功功率","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅳ-039 发电机有功功率","yc_hs_0414","cur_46"]
[3815,"b_右玉二期Ⅳ-039 发电机转速","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅳ-039 发电机转速","yc_hs_0414","cur_52"]
[3816,"b_右玉二期Ⅳ-039 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅳ-039 发电机驱动端轴承温度","yc_hs_0414","cur_56"]
[3817,"b_右玉二期Ⅳ-039 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅳ-039 发电机非驱动端轴承温度","yc_hs_0414","cur_57"]
[3818,"b_右玉二期Ⅳ-039 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅳ-039 发电机定子U相线圈温度","yc_hs_0414","cur_59"]
[3819,"b_右玉二期Ⅳ-039 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅳ-039 发电机定子V相线圈温度","yc_hs_0414","cur_60"]
[3820,"b_右玉二期Ⅳ-039 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅳ-039 发电机定子W相线圈温度","yc_hs_0414","cur_61"]
[3821,"b_右玉二期Ⅳ-039 舱内温度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅳ-039 舱内温度","yc_hs_0414","cur_68"]
[3822,"b_右玉二期Ⅳ-039 舱外温度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅳ-039 舱外温度","yc_hs_0414","cur_70"]
[3823,"b_右玉二期Ⅳ-039 风向","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅳ-039 风向","yc_hs_0414","cur_73"]
[3824,"b_右玉二期Ⅳ-039 风速","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅳ-039 风速","yc_hs_0414","cur_75"]
[3825,"b_右玉二期Ⅳ-039 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅳ-039 机舱中轴线与风向夹角","yc_hs_0414","cur_78"]
[3826,"b_右玉二期Ⅳ-039 1#桨叶片角度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅳ-039 1#桨叶片角度","yc_hs_0414","cur_83"]
[3827,"b_右玉二期Ⅳ-039 2#桨叶片角度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅳ-039 2#桨叶片角度","yc_hs_0414","cur_85"]
[3828,"b_右玉二期Ⅳ-039 3#桨叶片角度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅳ-039 3#桨叶片角度","yc_hs_0414","cur_87"]
[3829,"b_右玉二期Ⅳ-039 主轴转速","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅳ-039 主轴转速","yc_hs_0415","cur_11"]
[3830,"b_右玉二期Ⅳ-039 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅳ-039 齿轮箱高速轴非驱动端轴承温度","yc_hs_0415","cur_15"]
[3831,"b_右玉二期Ⅳ-039 齿轮箱油池温度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅳ-039 齿轮箱油池温度","yc_hs_0415","cur_16"]
[3832,"b_右玉二期Ⅳ-039 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅳ-039 齿轮箱中速轴非驱动端轴承温度","yc_hs_0415","cur_18"]
[3833,"b_右玉二期Ⅳ-039 主轴承外圈温度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅳ-039 主轴承外圈温度","yc_hs_0415","cur_19"]
[3834,"b_右玉二期Ⅳ-039 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅳ-039 机舱侧向振动(已滤波)","yc_hs_0415","cur_29"]
[3835,"b_右玉二期Ⅳ-039 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅳ-039 机舱轴向振动(已滤波)","yc_hs_0415","cur_31"]
[3836,"b_右玉二期Ⅳ-039 机舱角度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅳ-039 机舱角度","yc_hs_0415","cur_32"]
[3837,"b_右玉二期Ⅳ-039 扭缆角度","右玉风光互补电站","WOF34900079",39,"SXYY.T2_L1.WTG039.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅳ-039 扭缆角度","yc_hs_0415","cur_34"]
[3838,"b_右玉二期Ⅳ-040 发电机有功功率","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅳ-040 发电机有功功率","yc_hs_0415","cur_52"]
[3839,"b_右玉二期Ⅳ-040 发电机转速","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅳ-040 发电机转速","yc_hs_0415","cur_58"]
[3840,"b_右玉二期Ⅳ-040 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅳ-040 发电机驱动端轴承温度","yc_hs_0415","cur_62"]
[3841,"b_右玉二期Ⅳ-040 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅳ-040 发电机非驱动端轴承温度","yc_hs_0415","cur_63"]
[3842,"b_右玉二期Ⅳ-040 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅳ-040 发电机定子U相线圈温度","yc_hs_0415","cur_65"]
[3843,"b_右玉二期Ⅳ-040 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅳ-040 发电机定子V相线圈温度","yc_hs_0415","cur_66"]
[3844,"b_右玉二期Ⅳ-040 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅳ-040 发电机定子W相线圈温度","yc_hs_0415","cur_67"]
[3845,"b_右玉二期Ⅳ-040 舱内温度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅳ-040 舱内温度","yc_hs_0415","cur_74"]
[3846,"b_右玉二期Ⅳ-040 舱外温度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅳ-040 舱外温度","yc_hs_0415","cur_76"]
[3847,"b_右玉二期Ⅳ-040 风向","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅳ-040 风向","yc_hs_0415","cur_79"]
[3848,"b_右玉二期Ⅳ-040 风速","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅳ-040 风速","yc_hs_0415","cur_81"]
[3849,"b_右玉二期Ⅳ-040 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅳ-040 机舱中轴线与风向夹角","yc_hs_0415","cur_84"]
[3850,"b_右玉二期Ⅳ-040 1#桨叶片角度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅳ-040 1#桨叶片角度","yc_hs_0415","cur_89"]
[3851,"b_右玉二期Ⅳ-040 2#桨叶片角度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅳ-040 2#桨叶片角度","yc_hs_0415","cur_91"]
[3852,"b_右玉二期Ⅳ-040 3#桨叶片角度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅳ-040 3#桨叶片角度","yc_hs_0415","cur_93"]
[3853,"b_右玉二期Ⅳ-040 主轴转速","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅳ-040 主轴转速","yc_hs_0416","cur_17"]
[3854,"b_右玉二期Ⅳ-040 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅳ-040 齿轮箱高速轴非驱动端轴承温度","yc_hs_0416","cur_21"]
[3855,"b_右玉二期Ⅳ-040 齿轮箱油池温度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅳ-040 齿轮箱油池温度","yc_hs_0416","cur_22"]
[3856,"b_右玉二期Ⅳ-040 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅳ-040 齿轮箱中速轴非驱动端轴承温度","yc_hs_0416","cur_24"]
[3857,"b_右玉二期Ⅳ-040 主轴承外圈温度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅳ-040 主轴承外圈温度","yc_hs_0416","cur_25"]
[3858,"b_右玉二期Ⅳ-040 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅳ-040 机舱侧向振动(已滤波)","yc_hs_0416","cur_35"]
[3859,"b_右玉二期Ⅳ-040 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅳ-040 机舱轴向振动(已滤波)","yc_hs_0416","cur_37"]
[3860,"b_右玉二期Ⅳ-040 机舱角度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅳ-040 机舱角度","yc_hs_0416","cur_38"]
[3861,"b_右玉二期Ⅳ-040 扭缆角度","右玉风光互补电站","WOF34900079",40,"SXYY.T2_L1.WTG040.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅳ-040 扭缆角度","yc_hs_0416","cur_40"]
[3862,"b_右玉二期Ⅳ-041 发电机有功功率","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅳ-041 发电机有功功率","yc_hs_0416","cur_58"]
[3863,"b_右玉二期Ⅳ-041 发电机转速","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅳ-041 发电机转速","yc_hs_0416","cur_64"]
[3864,"b_右玉二期Ⅳ-041 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅳ-041 发电机驱动端轴承温度","yc_hs_0416","cur_68"]
[3865,"b_右玉二期Ⅳ-041 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅳ-041 发电机非驱动端轴承温度","yc_hs_0416","cur_69"]
[3866,"b_右玉二期Ⅳ-041 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅳ-041 发电机定子U相线圈温度","yc_hs_0416","cur_71"]
[3867,"b_右玉二期Ⅳ-041 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅳ-041 发电机定子V相线圈温度","yc_hs_0416","cur_72"]
[3868,"b_右玉二期Ⅳ-041 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅳ-041 发电机定子W相线圈温度","yc_hs_0416","cur_73"]
[3869,"b_右玉二期Ⅳ-041 舱内温度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅳ-041 舱内温度","yc_hs_0416","cur_80"]
[3870,"b_右玉二期Ⅳ-041 舱外温度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅳ-041 舱外温度","yc_hs_0416","cur_82"]
[3871,"b_右玉二期Ⅳ-041 风向","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅳ-041 风向","yc_hs_0416","cur_85"]
[3872,"b_右玉二期Ⅳ-041 风速","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅳ-041 风速","yc_hs_0416","cur_87"]
[3873,"b_右玉二期Ⅳ-041 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅳ-041 机舱中轴线与风向夹角","yc_hs_0416","cur_90"]
[3874,"b_右玉二期Ⅳ-041 1#桨叶片角度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅳ-041 1#桨叶片角度","yc_hs_0416","cur_95"]
[3875,"b_右玉二期Ⅳ-041 2#桨叶片角度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅳ-041 2#桨叶片角度","yc_hs_0416","cur_97"]
[3876,"b_右玉二期Ⅳ-041 3#桨叶片角度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅳ-041 3#桨叶片角度","yc_hs_0416","cur_99"]
[3877,"b_右玉二期Ⅳ-041 主轴转速","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅳ-041 主轴转速","yc_hs_0417","cur_23"]
[3878,"b_右玉二期Ⅳ-041 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅳ-041 齿轮箱高速轴非驱动端轴承温度","yc_hs_0417","cur_27"]
[3879,"b_右玉二期Ⅳ-041 齿轮箱油池温度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅳ-041 齿轮箱油池温度","yc_hs_0417","cur_28"]
[3880,"b_右玉二期Ⅳ-041 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅳ-041 齿轮箱中速轴非驱动端轴承温度","yc_hs_0417","cur_30"]
[3881,"b_右玉二期Ⅳ-041 主轴承外圈温度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅳ-041 主轴承外圈温度","yc_hs_0417","cur_31"]
[3882,"b_右玉二期Ⅳ-041 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅳ-041 机舱侧向振动(已滤波)","yc_hs_0417","cur_41"]
[3883,"b_右玉二期Ⅳ-041 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅳ-041 机舱轴向振动(已滤波)","yc_hs_0417","cur_43"]
[3884,"b_右玉二期Ⅳ-041 机舱角度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅳ-041 机舱角度","yc_hs_0417","cur_44"]
[3885,"b_右玉二期Ⅳ-041 扭缆角度","右玉风光互补电站","WOF34900079",41,"SXYY.T2_L1.WTG041.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅳ-041 扭缆角度","yc_hs_0417","cur_46"]
[3886,"b_右玉二期Ⅴ-042 发电机有功功率","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅴ-042 发电机有功功率","yc_hs_0417","cur_64"]
[3887,"b_右玉二期Ⅴ-042 发电机转速","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅴ-042 发电机转速","yc_hs_0417","cur_70"]
[3888,"b_右玉二期Ⅴ-042 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅴ-042 发电机驱动端轴承温度","yc_hs_0417","cur_74"]
[3889,"b_右玉二期Ⅴ-042 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅴ-042 发电机非驱动端轴承温度","yc_hs_0417","cur_75"]
[3890,"b_右玉二期Ⅴ-042 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅴ-042 发电机定子U相线圈温度","yc_hs_0417","cur_77"]
[3891,"b_右玉二期Ⅴ-042 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅴ-042 发电机定子V相线圈温度","yc_hs_0417","cur_78"]
[3892,"b_右玉二期Ⅴ-042 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅴ-042 发电机定子W相线圈温度","yc_hs_0417","cur_79"]
[3893,"b_右玉二期Ⅴ-042 舱内温度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅴ-042 舱内温度","yc_hs_0417","cur_86"]
[3894,"b_右玉二期Ⅴ-042 舱外温度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅴ-042 舱外温度","yc_hs_0417","cur_88"]
[3895,"b_右玉二期Ⅴ-042 风向","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅴ-042 风向","yc_hs_0417","cur_91"]
[3896,"b_右玉二期Ⅴ-042 风速","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅴ-042 风速","yc_hs_0417","cur_93"]
[3897,"b_右玉二期Ⅴ-042 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅴ-042 机舱中轴线与风向夹角","yc_hs_0417","cur_96"]
[3898,"b_右玉二期Ⅴ-042 1#桨叶片角度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅴ-042 1#桨叶片角度","yc_hs_0418","cur_01"]
[3899,"b_右玉二期Ⅴ-042 2#桨叶片角度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅴ-042 2#桨叶片角度","yc_hs_0418","cur_03"]
[3900,"b_右玉二期Ⅴ-042 3#桨叶片角度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅴ-042 3#桨叶片角度","yc_hs_0418","cur_05"]
[3901,"b_右玉二期Ⅴ-042 主轴转速","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅴ-042 主轴转速","yc_hs_0418","cur_29"]
[3902,"b_右玉二期Ⅴ-042 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅴ-042 齿轮箱高速轴非驱动端轴承温度","yc_hs_0418","cur_33"]
[3903,"b_右玉二期Ⅴ-042 齿轮箱油池温度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅴ-042 齿轮箱油池温度","yc_hs_0418","cur_34"]
[3904,"b_右玉二期Ⅴ-042 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅴ-042 齿轮箱中速轴非驱动端轴承温度","yc_hs_0418","cur_36"]
[3905,"b_右玉二期Ⅴ-042 主轴承外圈温度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅴ-042 主轴承外圈温度","yc_hs_0418","cur_37"]
[3906,"b_右玉二期Ⅴ-042 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅴ-042 机舱侧向振动(已滤波)","yc_hs_0418","cur_47"]
[3907,"b_右玉二期Ⅴ-042 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅴ-042 机舱轴向振动(已滤波)","yc_hs_0418","cur_49"]
[3908,"b_右玉二期Ⅴ-042 机舱角度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅴ-042 机舱角度","yc_hs_0418","cur_50"]
[3909,"b_右玉二期Ⅴ-042 扭缆角度","右玉风光互补电站","WOF34900079",42,"SXYY.T2_L2.WTG042.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅴ-042 扭缆角度","yc_hs_0418","cur_52"]
[3910,"b_右玉二期Ⅴ-043 发电机有功功率","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅴ-043 发电机有功功率","yc_hs_0418","cur_70"]
[3911,"b_右玉二期Ⅴ-043 发电机转速","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅴ-043 发电机转速","yc_hs_0418","cur_76"]
[3912,"b_右玉二期Ⅴ-043 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅴ-043 发电机驱动端轴承温度","yc_hs_0418","cur_80"]
[3913,"b_右玉二期Ⅴ-043 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅴ-043 发电机非驱动端轴承温度","yc_hs_0418","cur_81"]
[3914,"b_右玉二期Ⅴ-043 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅴ-043 发电机定子U相线圈温度","yc_hs_0418","cur_83"]
[3915,"b_右玉二期Ⅴ-043 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅴ-043 发电机定子V相线圈温度","yc_hs_0418","cur_84"]
[3916,"b_右玉二期Ⅴ-043 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅴ-043 发电机定子W相线圈温度","yc_hs_0418","cur_85"]
[3917,"b_右玉二期Ⅴ-043 舱内温度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅴ-043 舱内温度","yc_hs_0418","cur_92"]
[3918,"b_右玉二期Ⅴ-043 舱外温度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅴ-043 舱外温度","yc_hs_0418","cur_94"]
[3919,"b_右玉二期Ⅴ-043 风向","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅴ-043 风向","yc_hs_0418","cur_97"]
[3920,"b_右玉二期Ⅴ-043 风速","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅴ-043 风速","yc_hs_0418","cur_99"]
[3921,"b_右玉二期Ⅴ-043 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅴ-043 机舱中轴线与风向夹角","yc_hs_0419","cur_02"]
[3922,"b_右玉二期Ⅴ-043 1#桨叶片角度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅴ-043 1#桨叶片角度","yc_hs_0419","cur_07"]
[3923,"b_右玉二期Ⅴ-043 2#桨叶片角度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅴ-043 2#桨叶片角度","yc_hs_0419","cur_09"]
[3924,"b_右玉二期Ⅴ-043 3#桨叶片角度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅴ-043 3#桨叶片角度","yc_hs_0419","cur_11"]
[3925,"b_右玉二期Ⅴ-043 主轴转速","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅴ-043 主轴转速","yc_hs_0419","cur_35"]
[3926,"b_右玉二期Ⅴ-043 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅴ-043 齿轮箱高速轴非驱动端轴承温度","yc_hs_0419","cur_39"]
[3927,"b_右玉二期Ⅴ-043 齿轮箱油池温度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅴ-043 齿轮箱油池温度","yc_hs_0419","cur_40"]
[3928,"b_右玉二期Ⅴ-043 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅴ-043 齿轮箱中速轴非驱动端轴承温度","yc_hs_0419","cur_42"]
[3929,"b_右玉二期Ⅴ-043 主轴承外圈温度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅴ-043 主轴承外圈温度","yc_hs_0419","cur_43"]
[3930,"b_右玉二期Ⅴ-043 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅴ-043 机舱侧向振动(已滤波)","yc_hs_0419","cur_53"]
[3931,"b_右玉二期Ⅴ-043 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅴ-043 机舱轴向振动(已滤波)","yc_hs_0419","cur_55"]
[3932,"b_右玉二期Ⅴ-043 机舱角度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅴ-043 机舱角度","yc_hs_0419","cur_56"]
[3933,"b_右玉二期Ⅴ-043 扭缆角度","右玉风光互补电站","WOF34900079",43,"SXYY.T2_L2.WTG043.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅴ-043 扭缆角度","yc_hs_0419","cur_58"]
[3934,"b_右玉二期Ⅴ-044 发电机有功功率","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅴ-044 发电机有功功率","yc_hs_0419","cur_76"]
[3935,"b_右玉二期Ⅴ-044 发电机转速","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅴ-044 发电机转速","yc_hs_0419","cur_82"]
[3936,"b_右玉二期Ⅴ-044 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅴ-044 发电机驱动端轴承温度","yc_hs_0419","cur_86"]
[3937,"b_右玉二期Ⅴ-044 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅴ-044 发电机非驱动端轴承温度","yc_hs_0419","cur_87"]
[3938,"b_右玉二期Ⅴ-044 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅴ-044 发电机定子U相线圈温度","yc_hs_0419","cur_89"]
[3939,"b_右玉二期Ⅴ-044 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅴ-044 发电机定子V相线圈温度","yc_hs_0419","cur_90"]
[3940,"b_右玉二期Ⅴ-044 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅴ-044 发电机定子W相线圈温度","yc_hs_0419","cur_91"]
[3941,"b_右玉二期Ⅴ-044 舱内温度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅴ-044 舱内温度","yc_hs_0419","cur_98"]
[3942,"b_右玉二期Ⅴ-044 舱外温度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅴ-044 舱外温度","yc_hs_0419","cur_100"]
[3943,"b_右玉二期Ⅴ-044 风向","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅴ-044 风向","yc_hs_0420","cur_03"]
[3944,"b_右玉二期Ⅴ-044 风速","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅴ-044 风速","yc_hs_0420","cur_05"]
[3945,"b_右玉二期Ⅴ-044 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅴ-044 机舱中轴线与风向夹角","yc_hs_0420","cur_08"]
[3946,"b_右玉二期Ⅴ-044 1#桨叶片角度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅴ-044 1#桨叶片角度","yc_hs_0420","cur_13"]
[3947,"b_右玉二期Ⅴ-044 2#桨叶片角度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅴ-044 2#桨叶片角度","yc_hs_0420","cur_15"]
[3948,"b_右玉二期Ⅴ-044 3#桨叶片角度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅴ-044 3#桨叶片角度","yc_hs_0420","cur_17"]
[3949,"b_右玉二期Ⅴ-044 主轴转速","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅴ-044 主轴转速","yc_hs_0420","cur_41"]
[3950,"b_右玉二期Ⅴ-044 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅴ-044 齿轮箱高速轴非驱动端轴承温度","yc_hs_0420","cur_45"]
[3951,"b_右玉二期Ⅴ-044 齿轮箱油池温度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅴ-044 齿轮箱油池温度","yc_hs_0420","cur_46"]
[3952,"b_右玉二期Ⅴ-044 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅴ-044 齿轮箱中速轴非驱动端轴承温度","yc_hs_0420","cur_48"]
[3953,"b_右玉二期Ⅴ-044 主轴承外圈温度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅴ-044 主轴承外圈温度","yc_hs_0420","cur_49"]
[3954,"b_右玉二期Ⅴ-044 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅴ-044 机舱侧向振动(已滤波)","yc_hs_0420","cur_59"]
[3955,"b_右玉二期Ⅴ-044 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅴ-044 机舱轴向振动(已滤波)","yc_hs_0420","cur_61"]
[3956,"b_右玉二期Ⅴ-044 机舱角度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅴ-044 机舱角度","yc_hs_0420","cur_62"]
[3957,"b_右玉二期Ⅴ-044 扭缆角度","右玉风光互补电站","WOF34900079",44,"SXYY.T2_L2.WTG044.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅴ-044 扭缆角度","yc_hs_0420","cur_64"]
[3958,"b_右玉二期Ⅴ-045 发电机有功功率","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅴ-045 发电机有功功率","yc_hs_0420","cur_82"]
[3959,"b_右玉二期Ⅴ-045 发电机转速","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅴ-045 发电机转速","yc_hs_0420","cur_88"]
[3960,"b_右玉二期Ⅴ-045 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅴ-045 发电机驱动端轴承温度","yc_hs_0420","cur_92"]
[3961,"b_右玉二期Ⅴ-045 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅴ-045 发电机非驱动端轴承温度","yc_hs_0420","cur_93"]
[3962,"b_右玉二期Ⅴ-045 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅴ-045 发电机定子U相线圈温度","yc_hs_0420","cur_95"]
[3963,"b_右玉二期Ⅴ-045 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅴ-045 发电机定子V相线圈温度","yc_hs_0420","cur_96"]
[3964,"b_右玉二期Ⅴ-045 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅴ-045 发电机定子W相线圈温度","yc_hs_0420","cur_97"]
[3965,"b_右玉二期Ⅴ-045 舱内温度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅴ-045 舱内温度","yc_hs_0421","cur_04"]
[3966,"b_右玉二期Ⅴ-045 舱外温度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅴ-045 舱外温度","yc_hs_0421","cur_06"]
[3967,"b_右玉二期Ⅴ-045 风向","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅴ-045 风向","yc_hs_0421","cur_09"]
[3968,"b_右玉二期Ⅴ-045 风速","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅴ-045 风速","yc_hs_0421","cur_11"]
[3969,"b_右玉二期Ⅴ-045 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅴ-045 机舱中轴线与风向夹角","yc_hs_0421","cur_14"]
[3970,"b_右玉二期Ⅴ-045 1#桨叶片角度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅴ-045 1#桨叶片角度","yc_hs_0421","cur_19"]
[3971,"b_右玉二期Ⅴ-045 2#桨叶片角度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅴ-045 2#桨叶片角度","yc_hs_0421","cur_21"]
[3972,"b_右玉二期Ⅴ-045 3#桨叶片角度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅴ-045 3#桨叶片角度","yc_hs_0421","cur_23"]
[3973,"b_右玉二期Ⅴ-045 主轴转速","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅴ-045 主轴转速","yc_hs_0421","cur_47"]
[3974,"b_右玉二期Ⅴ-045 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅴ-045 齿轮箱高速轴非驱动端轴承温度","yc_hs_0421","cur_51"]
[3975,"b_右玉二期Ⅴ-045 齿轮箱油池温度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅴ-045 齿轮箱油池温度","yc_hs_0421","cur_52"]
[3976,"b_右玉二期Ⅴ-045 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅴ-045 齿轮箱中速轴非驱动端轴承温度","yc_hs_0421","cur_54"]
[3977,"b_右玉二期Ⅴ-045 主轴承外圈温度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅴ-045 主轴承外圈温度","yc_hs_0421","cur_55"]
[3978,"b_右玉二期Ⅴ-045 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅴ-045 机舱侧向振动(已滤波)","yc_hs_0421","cur_65"]
[3979,"b_右玉二期Ⅴ-045 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅴ-045 机舱轴向振动(已滤波)","yc_hs_0421","cur_67"]
[3980,"b_右玉二期Ⅴ-045 机舱角度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅴ-045 机舱角度","yc_hs_0421","cur_68"]
[3981,"b_右玉二期Ⅴ-045 扭缆角度","右玉风光互补电站","WOF34900079",45,"SXYY.T2_L2.WTG045.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅴ-045 扭缆角度","yc_hs_0421","cur_70"]
[3982,"b_右玉二期Ⅴ-046 发电机有功功率","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅴ-046 发电机有功功率","yc_hs_0421","cur_88"]
[3983,"b_右玉二期Ⅴ-046 发电机转速","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅴ-046 发电机转速","yc_hs_0421","cur_94"]
[3984,"b_右玉二期Ⅴ-046 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅴ-046 发电机驱动端轴承温度","yc_hs_0421","cur_98"]
[3985,"b_右玉二期Ⅴ-046 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅴ-046 发电机非驱动端轴承温度","yc_hs_0421","cur_99"]
[3986,"b_右玉二期Ⅴ-046 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅴ-046 发电机定子U相线圈温度","yc_hs_0422","cur_01"]
[3987,"b_右玉二期Ⅴ-046 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅴ-046 发电机定子V相线圈温度","yc_hs_0422","cur_02"]
[3988,"b_右玉二期Ⅴ-046 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅴ-046 发电机定子W相线圈温度","yc_hs_0422","cur_03"]
[3989,"b_右玉二期Ⅴ-046 舱内温度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅴ-046 舱内温度","yc_hs_0422","cur_10"]
[3990,"b_右玉二期Ⅴ-046 舱外温度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅴ-046 舱外温度","yc_hs_0422","cur_12"]
[3991,"b_右玉二期Ⅴ-046 风向","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅴ-046 风向","yc_hs_0422","cur_15"]
[3992,"b_右玉二期Ⅴ-046 风速","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅴ-046 风速","yc_hs_0422","cur_17"]
[3993,"b_右玉二期Ⅴ-046 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅴ-046 机舱中轴线与风向夹角","yc_hs_0422","cur_20"]
[3994,"b_右玉二期Ⅴ-046 1#桨叶片角度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅴ-046 1#桨叶片角度","yc_hs_0422","cur_25"]
[3995,"b_右玉二期Ⅴ-046 2#桨叶片角度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅴ-046 2#桨叶片角度","yc_hs_0422","cur_27"]
[3996,"b_右玉二期Ⅴ-046 3#桨叶片角度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅴ-046 3#桨叶片角度","yc_hs_0422","cur_29"]
[3997,"b_右玉二期Ⅴ-046 主轴转速","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅴ-046 主轴转速","yc_hs_0422","cur_53"]
[3998,"b_右玉二期Ⅴ-046 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅴ-046 齿轮箱高速轴非驱动端轴承温度","yc_hs_0422","cur_57"]
[3999,"b_右玉二期Ⅴ-046 齿轮箱油池温度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅴ-046 齿轮箱油池温度","yc_hs_0422","cur_58"]
[4000,"b_右玉二期Ⅴ-046 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅴ-046 齿轮箱中速轴非驱动端轴承温度","yc_hs_0422","cur_60"]
[4001,"b_右玉二期Ⅴ-046 主轴承外圈温度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅴ-046 主轴承外圈温度","yc_hs_0422","cur_61"]
[4002,"b_右玉二期Ⅴ-046 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅴ-046 机舱侧向振动(已滤波)","yc_hs_0422","cur_71"]
[4003,"b_右玉二期Ⅴ-046 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅴ-046 机舱轴向振动(已滤波)","yc_hs_0422","cur_73"]
[4004,"b_右玉二期Ⅴ-046 机舱角度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅴ-046 机舱角度","yc_hs_0422","cur_74"]
[4005,"b_右玉二期Ⅴ-046 扭缆角度","右玉风光互补电站","WOF34900079",46,"SXYY.T2_L2.WTG046.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅴ-046 扭缆角度","yc_hs_0422","cur_76"]
[4006,"b_右玉二期Ⅴ-047 发电机有功功率","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅴ-047 发电机有功功率","yc_hs_0422","cur_94"]
[4007,"b_右玉二期Ⅴ-047 发电机转速","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅴ-047 发电机转速","yc_hs_0422","cur_100"]
[4008,"b_右玉二期Ⅴ-047 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅴ-047 发电机驱动端轴承温度","yc_hs_0423","cur_04"]
[4009,"b_右玉二期Ⅴ-047 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅴ-047 发电机非驱动端轴承温度","yc_hs_0423","cur_05"]
[4010,"b_右玉二期Ⅴ-047 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅴ-047 发电机定子U相线圈温度","yc_hs_0423","cur_07"]
[4011,"b_右玉二期Ⅴ-047 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅴ-047 发电机定子V相线圈温度","yc_hs_0423","cur_08"]
[4012,"b_右玉二期Ⅴ-047 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅴ-047 发电机定子W相线圈温度","yc_hs_0423","cur_09"]
[4013,"b_右玉二期Ⅴ-047 舱内温度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅴ-047 舱内温度","yc_hs_0423","cur_16"]
[4014,"b_右玉二期Ⅴ-047 舱外温度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅴ-047 舱外温度","yc_hs_0423","cur_18"]
[4015,"b_右玉二期Ⅴ-047 风向","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅴ-047 风向","yc_hs_0423","cur_21"]
[4016,"b_右玉二期Ⅴ-047 风速","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅴ-047 风速","yc_hs_0423","cur_23"]
[4017,"b_右玉二期Ⅴ-047 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅴ-047 机舱中轴线与风向夹角","yc_hs_0423","cur_26"]
[4018,"b_右玉二期Ⅴ-047 1#桨叶片角度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅴ-047 1#桨叶片角度","yc_hs_0423","cur_31"]
[4019,"b_右玉二期Ⅴ-047 2#桨叶片角度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅴ-047 2#桨叶片角度","yc_hs_0423","cur_33"]
[4020,"b_右玉二期Ⅴ-047 3#桨叶片角度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅴ-047 3#桨叶片角度","yc_hs_0423","cur_35"]
[4021,"b_右玉二期Ⅴ-047 主轴转速","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅴ-047 主轴转速","yc_hs_0423","cur_59"]
[4022,"b_右玉二期Ⅴ-047 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅴ-047 齿轮箱高速轴非驱动端轴承温度","yc_hs_0423","cur_63"]
[4023,"b_右玉二期Ⅴ-047 齿轮箱油池温度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅴ-047 齿轮箱油池温度","yc_hs_0423","cur_64"]
[4024,"b_右玉二期Ⅴ-047 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅴ-047 齿轮箱中速轴非驱动端轴承温度","yc_hs_0423","cur_66"]
[4025,"b_右玉二期Ⅴ-047 主轴承外圈温度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅴ-047 主轴承外圈温度","yc_hs_0423","cur_67"]
[4026,"b_右玉二期Ⅴ-047 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅴ-047 机舱侧向振动(已滤波)","yc_hs_0423","cur_77"]
[4027,"b_右玉二期Ⅴ-047 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅴ-047 机舱轴向振动(已滤波)","yc_hs_0423","cur_79"]
[4028,"b_右玉二期Ⅴ-047 机舱角度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅴ-047 机舱角度","yc_hs_0423","cur_80"]
[4029,"b_右玉二期Ⅴ-047 扭缆角度","右玉风光互补电站","WOF34900079",47,"SXYY.T2_L2.WTG047.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅴ-047 扭缆角度","yc_hs_0423","cur_82"]
[4030,"b_右玉二期Ⅴ-048 发电机有功功率","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅴ-048 发电机有功功率","yc_hs_0423","cur_100"]
[4031,"b_右玉二期Ⅴ-048 发电机转速","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅴ-048 发电机转速","yc_hs_0424","cur_06"]
[4032,"b_右玉二期Ⅴ-048 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅴ-048 发电机驱动端轴承温度","yc_hs_0424","cur_10"]
[4033,"b_右玉二期Ⅴ-048 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅴ-048 发电机非驱动端轴承温度","yc_hs_0424","cur_11"]
[4034,"b_右玉二期Ⅴ-048 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅴ-048 发电机定子U相线圈温度","yc_hs_0424","cur_13"]
[4035,"b_右玉二期Ⅴ-048 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅴ-048 发电机定子V相线圈温度","yc_hs_0424","cur_14"]
[4036,"b_右玉二期Ⅴ-048 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅴ-048 发电机定子W相线圈温度","yc_hs_0424","cur_15"]
[4037,"b_右玉二期Ⅴ-048 舱内温度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅴ-048 舱内温度","yc_hs_0424","cur_22"]
[4038,"b_右玉二期Ⅴ-048 舱外温度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅴ-048 舱外温度","yc_hs_0424","cur_24"]
[4039,"b_右玉二期Ⅴ-048 风向","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅴ-048 风向","yc_hs_0424","cur_27"]
[4040,"b_右玉二期Ⅴ-048 风速","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅴ-048 风速","yc_hs_0424","cur_29"]
[4041,"b_右玉二期Ⅴ-048 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅴ-048 机舱中轴线与风向夹角","yc_hs_0424","cur_32"]
[4042,"b_右玉二期Ⅴ-048 1#桨叶片角度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅴ-048 1#桨叶片角度","yc_hs_0424","cur_37"]
[4043,"b_右玉二期Ⅴ-048 2#桨叶片角度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅴ-048 2#桨叶片角度","yc_hs_0424","cur_39"]
[4044,"b_右玉二期Ⅴ-048 3#桨叶片角度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅴ-048 3#桨叶片角度","yc_hs_0424","cur_41"]
[4045,"b_右玉二期Ⅴ-048 主轴转速","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅴ-048 主轴转速","yc_hs_0424","cur_65"]
[4046,"b_右玉二期Ⅴ-048 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅴ-048 齿轮箱高速轴非驱动端轴承温度","yc_hs_0424","cur_69"]
[4047,"b_右玉二期Ⅴ-048 齿轮箱油池温度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅴ-048 齿轮箱油池温度","yc_hs_0424","cur_70"]
[4048,"b_右玉二期Ⅴ-048 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅴ-048 齿轮箱中速轴非驱动端轴承温度","yc_hs_0424","cur_72"]
[4049,"b_右玉二期Ⅴ-048 主轴承外圈温度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅴ-048 主轴承外圈温度","yc_hs_0424","cur_73"]
[4050,"b_右玉二期Ⅴ-048 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅴ-048 机舱侧向振动(已滤波)","yc_hs_0424","cur_83"]
[4051,"b_右玉二期Ⅴ-048 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅴ-048 机舱轴向振动(已滤波)","yc_hs_0424","cur_85"]
[4052,"b_右玉二期Ⅴ-048 机舱角度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅴ-048 机舱角度","yc_hs_0424","cur_86"]
[4053,"b_右玉二期Ⅴ-048 扭缆角度","右玉风光互补电站","WOF34900079",48,"SXYY.T2_L2.WTG048.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅴ-048 扭缆角度","yc_hs_0424","cur_88"]
[4054,"b_右玉二期Ⅴ-049 发电机有功功率","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅴ-049 发电机有功功率","yc_hs_0425","cur_06"]
[4055,"b_右玉二期Ⅴ-049 发电机转速","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅴ-049 发电机转速","yc_hs_0425","cur_12"]
[4056,"b_右玉二期Ⅴ-049 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅴ-049 发电机驱动端轴承温度","yc_hs_0425","cur_16"]
[4057,"b_右玉二期Ⅴ-049 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅴ-049 发电机非驱动端轴承温度","yc_hs_0425","cur_17"]
[4058,"b_右玉二期Ⅴ-049 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅴ-049 发电机定子U相线圈温度","yc_hs_0425","cur_19"]
[4059,"b_右玉二期Ⅴ-049 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅴ-049 发电机定子V相线圈温度","yc_hs_0425","cur_20"]
[4060,"b_右玉二期Ⅴ-049 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅴ-049 发电机定子W相线圈温度","yc_hs_0425","cur_21"]
[4061,"b_右玉二期Ⅴ-049 舱内温度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅴ-049 舱内温度","yc_hs_0425","cur_28"]
[4062,"b_右玉二期Ⅴ-049 舱外温度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅴ-049 舱外温度","yc_hs_0425","cur_30"]
[4063,"b_右玉二期Ⅴ-049 风向","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅴ-049 风向","yc_hs_0425","cur_33"]
[4064,"b_右玉二期Ⅴ-049 风速","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅴ-049 风速","yc_hs_0425","cur_35"]
[4065,"b_右玉二期Ⅴ-049 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅴ-049 机舱中轴线与风向夹角","yc_hs_0425","cur_38"]
[4066,"b_右玉二期Ⅴ-049 1#桨叶片角度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅴ-049 1#桨叶片角度","yc_hs_0425","cur_43"]
[4067,"b_右玉二期Ⅴ-049 2#桨叶片角度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅴ-049 2#桨叶片角度","yc_hs_0425","cur_45"]
[4068,"b_右玉二期Ⅴ-049 3#桨叶片角度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅴ-049 3#桨叶片角度","yc_hs_0425","cur_47"]
[4069,"b_右玉二期Ⅴ-049 主轴转速","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅴ-049 主轴转速","yc_hs_0425","cur_71"]
[4070,"b_右玉二期Ⅴ-049 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅴ-049 齿轮箱高速轴非驱动端轴承温度","yc_hs_0425","cur_75"]
[4071,"b_右玉二期Ⅴ-049 齿轮箱油池温度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅴ-049 齿轮箱油池温度","yc_hs_0425","cur_76"]
[4072,"b_右玉二期Ⅴ-049 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅴ-049 齿轮箱中速轴非驱动端轴承温度","yc_hs_0425","cur_78"]
[4073,"b_右玉二期Ⅴ-049 主轴承外圈温度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅴ-049 主轴承外圈温度","yc_hs_0425","cur_79"]
[4074,"b_右玉二期Ⅴ-049 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅴ-049 机舱侧向振动(已滤波)","yc_hs_0425","cur_89"]
[4075,"b_右玉二期Ⅴ-049 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅴ-049 机舱轴向振动(已滤波)","yc_hs_0425","cur_91"]
[4076,"b_右玉二期Ⅴ-049 机舱角度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅴ-049 机舱角度","yc_hs_0425","cur_92"]
[4077,"b_右玉二期Ⅴ-049 扭缆角度","右玉风光互补电站","WOF34900079",49,"SXYY.T2_L2.WTG049.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅴ-049 扭缆角度","yc_hs_0425","cur_94"]
[4078,"b_右玉二期Ⅵ-050 发电机有功功率","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅵ-050 发电机有功功率","yc_hs_0426","cur_12"]
[4079,"b_右玉二期Ⅵ-050 发电机转速","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅵ-050 发电机转速","yc_hs_0426","cur_18"]
[4080,"b_右玉二期Ⅵ-050 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅵ-050 发电机驱动端轴承温度","yc_hs_0426","cur_22"]
[4081,"b_右玉二期Ⅵ-050 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅵ-050 发电机非驱动端轴承温度","yc_hs_0426","cur_23"]
[4082,"b_右玉二期Ⅵ-050 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅵ-050 发电机定子U相线圈温度","yc_hs_0426","cur_25"]
[4083,"b_右玉二期Ⅵ-050 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅵ-050 发电机定子V相线圈温度","yc_hs_0426","cur_26"]
[4084,"b_右玉二期Ⅵ-050 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅵ-050 发电机定子W相线圈温度","yc_hs_0426","cur_27"]
[4085,"b_右玉二期Ⅵ-050 舱内温度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅵ-050 舱内温度","yc_hs_0426","cur_34"]
[4086,"b_右玉二期Ⅵ-050 舱外温度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅵ-050 舱外温度","yc_hs_0426","cur_36"]
[4087,"b_右玉二期Ⅵ-050 风向","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅵ-050 风向","yc_hs_0426","cur_39"]
[4088,"b_右玉二期Ⅵ-050 风速","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅵ-050 风速","yc_hs_0426","cur_41"]
[4089,"b_右玉二期Ⅵ-050 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅵ-050 机舱中轴线与风向夹角","yc_hs_0426","cur_44"]
[4090,"b_右玉二期Ⅵ-050 1#桨叶片角度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅵ-050 1#桨叶片角度","yc_hs_0426","cur_49"]
[4091,"b_右玉二期Ⅵ-050 2#桨叶片角度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅵ-050 2#桨叶片角度","yc_hs_0426","cur_51"]
[4092,"b_右玉二期Ⅵ-050 3#桨叶片角度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅵ-050 3#桨叶片角度","yc_hs_0426","cur_53"]
[4093,"b_右玉二期Ⅵ-050 主轴转速","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅵ-050 主轴转速","yc_hs_0426","cur_77"]
[4094,"b_右玉二期Ⅵ-050 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅵ-050 齿轮箱高速轴非驱动端轴承温度","yc_hs_0426","cur_81"]
[4095,"b_右玉二期Ⅵ-050 齿轮箱油池温度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅵ-050 齿轮箱油池温度","yc_hs_0426","cur_82"]
[4096,"b_右玉二期Ⅵ-050 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅵ-050 齿轮箱中速轴非驱动端轴承温度","yc_hs_0426","cur_84"]
[4097,"b_右玉二期Ⅵ-050 主轴承外圈温度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅵ-050 主轴承外圈温度","yc_hs_0426","cur_85"]
[4098,"b_右玉二期Ⅵ-050 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅵ-050 机舱侧向振动(已滤波)","yc_hs_0426","cur_95"]
[4099,"b_右玉二期Ⅵ-050 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅵ-050 机舱轴向振动(已滤波)","yc_hs_0426","cur_97"]
[4100,"b_右玉二期Ⅵ-050 机舱角度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅵ-050 机舱角度","yc_hs_0426","cur_98"]
[4101,"b_右玉二期Ⅵ-050 扭缆角度","右玉风光互补电站","WOF34900079",50,"SXYY.T2_L3.WTG050.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅵ-050 扭缆角度","yc_hs_0426","cur_100"]
[4102,"b_右玉二期Ⅵ-051 发电机有功功率","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅵ-051 发电机有功功率","yc_hs_0427","cur_18"]
[4103,"b_右玉二期Ⅵ-051 发电机转速","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅵ-051 发电机转速","yc_hs_0427","cur_24"]
[4104,"b_右玉二期Ⅵ-051 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅵ-051 发电机驱动端轴承温度","yc_hs_0427","cur_28"]
[4105,"b_右玉二期Ⅵ-051 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅵ-051 发电机非驱动端轴承温度","yc_hs_0427","cur_29"]
[4106,"b_右玉二期Ⅵ-051 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅵ-051 发电机定子U相线圈温度","yc_hs_0427","cur_31"]
[4107,"b_右玉二期Ⅵ-051 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅵ-051 发电机定子V相线圈温度","yc_hs_0427","cur_32"]
[4108,"b_右玉二期Ⅵ-051 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅵ-051 发电机定子W相线圈温度","yc_hs_0427","cur_33"]
[4109,"b_右玉二期Ⅵ-051 舱内温度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅵ-051 舱内温度","yc_hs_0427","cur_40"]
[4110,"b_右玉二期Ⅵ-051 舱外温度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅵ-051 舱外温度","yc_hs_0427","cur_42"]
[4111,"b_右玉二期Ⅵ-051 风向","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅵ-051 风向","yc_hs_0427","cur_45"]
[4112,"b_右玉二期Ⅵ-051 风速","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅵ-051 风速","yc_hs_0427","cur_47"]
[4113,"b_右玉二期Ⅵ-051 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅵ-051 机舱中轴线与风向夹角","yc_hs_0427","cur_50"]
[4114,"b_右玉二期Ⅵ-051 1#桨叶片角度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅵ-051 1#桨叶片角度","yc_hs_0427","cur_55"]
[4115,"b_右玉二期Ⅵ-051 2#桨叶片角度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅵ-051 2#桨叶片角度","yc_hs_0427","cur_57"]
[4116,"b_右玉二期Ⅵ-051 3#桨叶片角度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅵ-051 3#桨叶片角度","yc_hs_0427","cur_59"]
[4117,"b_右玉二期Ⅵ-051 主轴转速","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅵ-051 主轴转速","yc_hs_0427","cur_83"]
[4118,"b_右玉二期Ⅵ-051 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅵ-051 齿轮箱高速轴非驱动端轴承温度","yc_hs_0427","cur_87"]
[4119,"b_右玉二期Ⅵ-051 齿轮箱油池温度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅵ-051 齿轮箱油池温度","yc_hs_0427","cur_88"]
[4120,"b_右玉二期Ⅵ-051 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅵ-051 齿轮箱中速轴非驱动端轴承温度","yc_hs_0427","cur_90"]
[4121,"b_右玉二期Ⅵ-051 主轴承外圈温度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅵ-051 主轴承外圈温度","yc_hs_0427","cur_91"]
[4122,"b_右玉二期Ⅵ-051 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅵ-051 机舱侧向振动(已滤波)","yc_hs_0428","cur_01"]
[4123,"b_右玉二期Ⅵ-051 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅵ-051 机舱轴向振动(已滤波)","yc_hs_0428","cur_03"]
[4124,"b_右玉二期Ⅵ-051 机舱角度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅵ-051 机舱角度","yc_hs_0428","cur_04"]
[4125,"b_右玉二期Ⅵ-051 扭缆角度","右玉风光互补电站","WOF34900079",51,"SXYY.T2_L3.WTG051.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅵ-051 扭缆角度","yc_hs_0428","cur_06"]
[4126,"b_右玉二期Ⅵ-052 发电机有功功率","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅵ-052 发电机有功功率","yc_hs_0428","cur_24"]
[4127,"b_右玉二期Ⅵ-052 发电机转速","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅵ-052 发电机转速","yc_hs_0428","cur_30"]
[4128,"b_右玉二期Ⅵ-052 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅵ-052 发电机驱动端轴承温度","yc_hs_0428","cur_34"]
[4129,"b_右玉二期Ⅵ-052 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅵ-052 发电机非驱动端轴承温度","yc_hs_0428","cur_35"]
[4130,"b_右玉二期Ⅵ-052 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅵ-052 发电机定子U相线圈温度","yc_hs_0428","cur_37"]
[4131,"b_右玉二期Ⅵ-052 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅵ-052 发电机定子V相线圈温度","yc_hs_0428","cur_38"]
[4132,"b_右玉二期Ⅵ-052 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅵ-052 发电机定子W相线圈温度","yc_hs_0428","cur_39"]
[4133,"b_右玉二期Ⅵ-052 舱内温度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅵ-052 舱内温度","yc_hs_0428","cur_46"]
[4134,"b_右玉二期Ⅵ-052 舱外温度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅵ-052 舱外温度","yc_hs_0428","cur_48"]
[4135,"b_右玉二期Ⅵ-052 风向","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅵ-052 风向","yc_hs_0428","cur_51"]
[4136,"b_右玉二期Ⅵ-052 风速","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅵ-052 风速","yc_hs_0428","cur_53"]
[4137,"b_右玉二期Ⅵ-052 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅵ-052 机舱中轴线与风向夹角","yc_hs_0428","cur_56"]
[4138,"b_右玉二期Ⅵ-052 1#桨叶片角度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅵ-052 1#桨叶片角度","yc_hs_0428","cur_61"]
[4139,"b_右玉二期Ⅵ-052 2#桨叶片角度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅵ-052 2#桨叶片角度","yc_hs_0428","cur_63"]
[4140,"b_右玉二期Ⅵ-052 3#桨叶片角度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅵ-052 3#桨叶片角度","yc_hs_0428","cur_65"]
[4141,"b_右玉二期Ⅵ-052 主轴转速","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅵ-052 主轴转速","yc_hs_0428","cur_89"]
[4142,"b_右玉二期Ⅵ-052 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅵ-052 齿轮箱高速轴非驱动端轴承温度","yc_hs_0428","cur_93"]
[4143,"b_右玉二期Ⅵ-052 齿轮箱油池温度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅵ-052 齿轮箱油池温度","yc_hs_0428","cur_94"]
[4144,"b_右玉二期Ⅵ-052 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅵ-052 齿轮箱中速轴非驱动端轴承温度","yc_hs_0428","cur_96"]
[4145,"b_右玉二期Ⅵ-052 主轴承外圈温度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅵ-052 主轴承外圈温度","yc_hs_0428","cur_97"]
[4146,"b_右玉二期Ⅵ-052 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅵ-052 机舱侧向振动(已滤波)","yc_hs_0429","cur_07"]
[4147,"b_右玉二期Ⅵ-052 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅵ-052 机舱轴向振动(已滤波)","yc_hs_0429","cur_09"]
[4148,"b_右玉二期Ⅵ-052 机舱角度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅵ-052 机舱角度","yc_hs_0429","cur_10"]
[4149,"b_右玉二期Ⅵ-052 扭缆角度","右玉风光互补电站","WOF34900079",52,"SXYY.T2_L3.WTG052.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅵ-052 扭缆角度","yc_hs_0429","cur_12"]
[4150,"b_右玉二期Ⅵ-053 发电机有功功率","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅵ-053 发电机有功功率","yc_hs_0429","cur_30"]
[4151,"b_右玉二期Ⅵ-053 发电机转速","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅵ-053 发电机转速","yc_hs_0429","cur_36"]
[4152,"b_右玉二期Ⅵ-053 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅵ-053 发电机驱动端轴承温度","yc_hs_0429","cur_40"]
[4153,"b_右玉二期Ⅵ-053 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅵ-053 发电机非驱动端轴承温度","yc_hs_0429","cur_41"]
[4154,"b_右玉二期Ⅵ-053 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅵ-053 发电机定子U相线圈温度","yc_hs_0429","cur_43"]
[4155,"b_右玉二期Ⅵ-053 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅵ-053 发电机定子V相线圈温度","yc_hs_0429","cur_44"]
[4156,"b_右玉二期Ⅵ-053 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅵ-053 发电机定子W相线圈温度","yc_hs_0429","cur_45"]
[4157,"b_右玉二期Ⅵ-053 舱内温度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅵ-053 舱内温度","yc_hs_0429","cur_52"]
[4158,"b_右玉二期Ⅵ-053 舱外温度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅵ-053 舱外温度","yc_hs_0429","cur_54"]
[4159,"b_右玉二期Ⅵ-053 风向","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅵ-053 风向","yc_hs_0429","cur_57"]
[4160,"b_右玉二期Ⅵ-053 风速","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅵ-053 风速","yc_hs_0429","cur_59"]
[4161,"b_右玉二期Ⅵ-053 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅵ-053 机舱中轴线与风向夹角","yc_hs_0429","cur_62"]
[4162,"b_右玉二期Ⅵ-053 1#桨叶片角度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅵ-053 1#桨叶片角度","yc_hs_0429","cur_67"]
[4163,"b_右玉二期Ⅵ-053 2#桨叶片角度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅵ-053 2#桨叶片角度","yc_hs_0429","cur_69"]
[4164,"b_右玉二期Ⅵ-053 3#桨叶片角度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅵ-053 3#桨叶片角度","yc_hs_0429","cur_71"]
[4165,"b_右玉二期Ⅵ-053 主轴转速","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅵ-053 主轴转速","yc_hs_0429","cur_95"]
[4166,"b_右玉二期Ⅵ-053 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅵ-053 齿轮箱高速轴非驱动端轴承温度","yc_hs_0429","cur_99"]
[4167,"b_右玉二期Ⅵ-053 齿轮箱油池温度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅵ-053 齿轮箱油池温度","yc_hs_0429","cur_100"]
[4168,"b_右玉二期Ⅵ-053 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅵ-053 齿轮箱中速轴非驱动端轴承温度","yc_hs_0430","cur_02"]
[4169,"b_右玉二期Ⅵ-053 主轴承外圈温度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅵ-053 主轴承外圈温度","yc_hs_0430","cur_03"]
[4170,"b_右玉二期Ⅵ-053 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅵ-053 机舱侧向振动(已滤波)","yc_hs_0430","cur_13"]
[4171,"b_右玉二期Ⅵ-053 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅵ-053 机舱轴向振动(已滤波)","yc_hs_0430","cur_15"]
[4172,"b_右玉二期Ⅵ-053 机舱角度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅵ-053 机舱角度","yc_hs_0430","cur_16"]
[4173,"b_右玉二期Ⅵ-053 扭缆角度","右玉风光互补电站","WOF34900079",53,"SXYY.T2_L3.WTG053.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅵ-053 扭缆角度","yc_hs_0430","cur_18"]
[4174,"b_右玉二期Ⅵ-054 发电机有功功率","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅵ-054 发电机有功功率","yc_hs_0430","cur_36"]
[4175,"b_右玉二期Ⅵ-054 发电机转速","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅵ-054 发电机转速","yc_hs_0430","cur_42"]
[4176,"b_右玉二期Ⅵ-054 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅵ-054 发电机驱动端轴承温度","yc_hs_0430","cur_46"]
[4177,"b_右玉二期Ⅵ-054 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅵ-054 发电机非驱动端轴承温度","yc_hs_0430","cur_47"]
[4178,"b_右玉二期Ⅵ-054 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅵ-054 发电机定子U相线圈温度","yc_hs_0430","cur_49"]
[4179,"b_右玉二期Ⅵ-054 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅵ-054 发电机定子V相线圈温度","yc_hs_0430","cur_50"]
[4180,"b_右玉二期Ⅵ-054 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅵ-054 发电机定子W相线圈温度","yc_hs_0430","cur_51"]
[4181,"b_右玉二期Ⅵ-054 舱内温度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅵ-054 舱内温度","yc_hs_0430","cur_58"]
[4182,"b_右玉二期Ⅵ-054 舱外温度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅵ-054 舱外温度","yc_hs_0430","cur_60"]
[4183,"b_右玉二期Ⅵ-054 风向","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅵ-054 风向","yc_hs_0430","cur_63"]
[4184,"b_右玉二期Ⅵ-054 风速","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅵ-054 风速","yc_hs_0430","cur_65"]
[4185,"b_右玉二期Ⅵ-054 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅵ-054 机舱中轴线与风向夹角","yc_hs_0430","cur_68"]
[4186,"b_右玉二期Ⅵ-054 1#桨叶片角度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅵ-054 1#桨叶片角度","yc_hs_0430","cur_73"]
[4187,"b_右玉二期Ⅵ-054 2#桨叶片角度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅵ-054 2#桨叶片角度","yc_hs_0430","cur_75"]
[4188,"b_右玉二期Ⅵ-054 3#桨叶片角度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅵ-054 3#桨叶片角度","yc_hs_0430","cur_77"]
[4189,"b_右玉二期Ⅵ-054 主轴转速","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅵ-054 主轴转速","yc_hs_0431","cur_01"]
[4190,"b_右玉二期Ⅵ-054 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅵ-054 齿轮箱高速轴非驱动端轴承温度","yc_hs_0431","cur_05"]
[4191,"b_右玉二期Ⅵ-054 齿轮箱油池温度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅵ-054 齿轮箱油池温度","yc_hs_0431","cur_06"]
[4192,"b_右玉二期Ⅵ-054 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅵ-054 齿轮箱中速轴非驱动端轴承温度","yc_hs_0431","cur_08"]
[4193,"b_右玉二期Ⅵ-054 主轴承外圈温度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅵ-054 主轴承外圈温度","yc_hs_0431","cur_09"]
[4194,"b_右玉二期Ⅵ-054 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅵ-054 机舱侧向振动(已滤波)","yc_hs_0431","cur_19"]
[4195,"b_右玉二期Ⅵ-054 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅵ-054 机舱轴向振动(已滤波)","yc_hs_0431","cur_21"]
[4196,"b_右玉二期Ⅵ-054 机舱角度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅵ-054 机舱角度","yc_hs_0431","cur_22"]
[4197,"b_右玉二期Ⅵ-054 扭缆角度","右玉风光互补电站","WOF34900079",54,"SXYY.T2_L3.WTG054.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅵ-054 扭缆角度","yc_hs_0431","cur_24"]
[4198,"b_右玉二期Ⅵ-055 发电机有功功率","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅵ-055 发电机有功功率","yc_hs_0431","cur_42"]
[4199,"b_右玉二期Ⅵ-055 发电机转速","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅵ-055 发电机转速","yc_hs_0431","cur_48"]
[4200,"b_右玉二期Ⅵ-055 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅵ-055 发电机驱动端轴承温度","yc_hs_0431","cur_52"]
[4201,"b_右玉二期Ⅵ-055 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅵ-055 发电机非驱动端轴承温度","yc_hs_0431","cur_53"]
[4202,"b_右玉二期Ⅵ-055 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅵ-055 发电机定子U相线圈温度","yc_hs_0431","cur_55"]
[4203,"b_右玉二期Ⅵ-055 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅵ-055 发电机定子V相线圈温度","yc_hs_0431","cur_56"]
[4204,"b_右玉二期Ⅵ-055 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅵ-055 发电机定子W相线圈温度","yc_hs_0431","cur_57"]
[4205,"b_右玉二期Ⅵ-055 舱内温度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅵ-055 舱内温度","yc_hs_0431","cur_64"]
[4206,"b_右玉二期Ⅵ-055 舱外温度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅵ-055 舱外温度","yc_hs_0431","cur_66"]
[4207,"b_右玉二期Ⅵ-055 风向","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅵ-055 风向","yc_hs_0431","cur_69"]
[4208,"b_右玉二期Ⅵ-055 风速","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅵ-055 风速","yc_hs_0431","cur_71"]
[4209,"b_右玉二期Ⅵ-055 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅵ-055 机舱中轴线与风向夹角","yc_hs_0431","cur_74"]
[4210,"b_右玉二期Ⅵ-055 1#桨叶片角度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅵ-055 1#桨叶片角度","yc_hs_0431","cur_79"]
[4211,"b_右玉二期Ⅵ-055 2#桨叶片角度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅵ-055 2#桨叶片角度","yc_hs_0431","cur_81"]
[4212,"b_右玉二期Ⅵ-055 3#桨叶片角度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅵ-055 3#桨叶片角度","yc_hs_0431","cur_83"]
[4213,"b_右玉二期Ⅵ-055 主轴转速","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅵ-055 主轴转速","yc_hs_0432","cur_07"]
[4214,"b_右玉二期Ⅵ-055 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅵ-055 齿轮箱高速轴非驱动端轴承温度","yc_hs_0432","cur_11"]
[4215,"b_右玉二期Ⅵ-055 齿轮箱油池温度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅵ-055 齿轮箱油池温度","yc_hs_0432","cur_12"]
[4216,"b_右玉二期Ⅵ-055 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅵ-055 齿轮箱中速轴非驱动端轴承温度","yc_hs_0432","cur_14"]
[4217,"b_右玉二期Ⅵ-055 主轴承外圈温度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅵ-055 主轴承外圈温度","yc_hs_0432","cur_15"]
[4218,"b_右玉二期Ⅵ-055 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅵ-055 机舱侧向振动(已滤波)","yc_hs_0432","cur_25"]
[4219,"b_右玉二期Ⅵ-055 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅵ-055 机舱轴向振动(已滤波)","yc_hs_0432","cur_27"]
[4220,"b_右玉二期Ⅵ-055 机舱角度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅵ-055 机舱角度","yc_hs_0432","cur_28"]
[4221,"b_右玉二期Ⅵ-055 扭缆角度","右玉风光互补电站","WOF34900079",55,"SXYY.T2_L3.WTG055.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅵ-055 扭缆角度","yc_hs_0432","cur_30"]
[4222,"b_右玉二期Ⅵ-056 发电机有功功率","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅵ-056 发电机有功功率","yc_hs_0432","cur_48"]
[4223,"b_右玉二期Ⅵ-056 发电机转速","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅵ-056 发电机转速","yc_hs_0432","cur_54"]
[4224,"b_右玉二期Ⅵ-056 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅵ-056 发电机驱动端轴承温度","yc_hs_0432","cur_58"]
[4225,"b_右玉二期Ⅵ-056 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅵ-056 发电机非驱动端轴承温度","yc_hs_0432","cur_59"]
[4226,"b_右玉二期Ⅵ-056 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅵ-056 发电机定子U相线圈温度","yc_hs_0432","cur_61"]
[4227,"b_右玉二期Ⅵ-056 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅵ-056 发电机定子V相线圈温度","yc_hs_0432","cur_62"]
[4228,"b_右玉二期Ⅵ-056 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅵ-056 发电机定子W相线圈温度","yc_hs_0432","cur_63"]
[4229,"b_右玉二期Ⅵ-056 舱内温度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅵ-056 舱内温度","yc_hs_0432","cur_70"]
[4230,"b_右玉二期Ⅵ-056 舱外温度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅵ-056 舱外温度","yc_hs_0432","cur_72"]
[4231,"b_右玉二期Ⅵ-056 风向","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅵ-056 风向","yc_hs_0432","cur_75"]
[4232,"b_右玉二期Ⅵ-056 风速","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅵ-056 风速","yc_hs_0432","cur_77"]
[4233,"b_右玉二期Ⅵ-056 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅵ-056 机舱中轴线与风向夹角","yc_hs_0432","cur_80"]
[4234,"b_右玉二期Ⅵ-056 1#桨叶片角度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅵ-056 1#桨叶片角度","yc_hs_0432","cur_85"]
[4235,"b_右玉二期Ⅵ-056 2#桨叶片角度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅵ-056 2#桨叶片角度","yc_hs_0432","cur_87"]
[4236,"b_右玉二期Ⅵ-056 3#桨叶片角度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅵ-056 3#桨叶片角度","yc_hs_0432","cur_89"]
[4237,"b_右玉二期Ⅵ-056 主轴转速","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅵ-056 主轴转速","yc_hs_0433","cur_13"]
[4238,"b_右玉二期Ⅵ-056 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅵ-056 齿轮箱高速轴非驱动端轴承温度","yc_hs_0433","cur_17"]
[4239,"b_右玉二期Ⅵ-056 齿轮箱油池温度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅵ-056 齿轮箱油池温度","yc_hs_0433","cur_18"]
[4240,"b_右玉二期Ⅵ-056 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅵ-056 齿轮箱中速轴非驱动端轴承温度","yc_hs_0433","cur_20"]
[4241,"b_右玉二期Ⅵ-056 主轴承外圈温度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅵ-056 主轴承外圈温度","yc_hs_0433","cur_21"]
[4242,"b_右玉二期Ⅵ-056 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅵ-056 机舱侧向振动(已滤波)","yc_hs_0433","cur_31"]
[4243,"b_右玉二期Ⅵ-056 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅵ-056 机舱轴向振动(已滤波)","yc_hs_0433","cur_33"]
[4244,"b_右玉二期Ⅵ-056 机舱角度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅵ-056 机舱角度","yc_hs_0433","cur_34"]
[4245,"b_右玉二期Ⅵ-056 扭缆角度","右玉风光互补电站","WOF34900079",56,"SXYY.T2_L3.WTG056.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅵ-056 扭缆角度","yc_hs_0433","cur_36"]
[4246,"b_右玉二期Ⅵ-057 发电机有功功率","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WGEN.GenActivePW","有功功率","active_power","b_右玉二期Ⅵ-057 发电机有功功率","yc_hs_0433","cur_54"]
[4247,"b_右玉二期Ⅵ-057 发电机转速","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WGEN.GenSpd","发电机转速","generator_speed","b_右玉二期Ⅵ-057 发电机转速","yc_hs_0433","cur_60"]
[4248,"b_右玉二期Ⅵ-057 发电机驱动端轴承温度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","b_右玉二期Ⅵ-057 发电机驱动端轴承温度","yc_hs_0433","cur_64"]
[4249,"b_右玉二期Ⅵ-057 发电机非驱动端轴承温度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","b_右玉二期Ⅵ-057 发电机非驱动端轴承温度","yc_hs_0433","cur_65"]
[4250,"b_右玉二期Ⅵ-057 发电机定子U相线圈温度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","b_右玉二期Ⅵ-057 发电机定子U相线圈温度","yc_hs_0433","cur_67"]
[4251,"b_右玉二期Ⅵ-057 发电机定子V相线圈温度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","b_右玉二期Ⅵ-057 发电机定子V相线圈温度","yc_hs_0433","cur_68"]
[4252,"b_右玉二期Ⅵ-057 发电机定子W相线圈温度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","b_右玉二期Ⅵ-057 发电机定子W相线圈温度","yc_hs_0433","cur_69"]
[4253,"b_右玉二期Ⅵ-057 舱内温度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WNAC.TemNacelle","机舱内温度","cabin_temperature","b_右玉二期Ⅵ-057 舱内温度","yc_hs_0433","cur_76"]
[4254,"b_右玉二期Ⅵ-057 舱外温度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WNAC.TemOut","环境温度","outside_cabin_temperature","b_右玉二期Ⅵ-057 舱外温度","yc_hs_0433","cur_78"]
[4255,"b_右玉二期Ⅵ-057 风向","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WNAC.WindDirection","绝对风向","true_wind_direction","b_右玉二期Ⅵ-057 风向","yc_hs_0433","cur_81"]
[4256,"b_右玉二期Ⅵ-057 风速","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WNAC.WindSpeed","风速","wind_velocity","b_右玉二期Ⅵ-057 风速","yc_hs_0433","cur_83"]
[4257,"b_右玉二期Ⅵ-057 机舱中轴线与风向夹角","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WNAC.WindVaneDirection","对风角度","yaw_error1","b_右玉二期Ⅵ-057 机舱中轴线与风向夹角","yc_hs_0433","cur_86"]
[4258,"b_右玉二期Ⅵ-057 1#桨叶片角度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","b_右玉二期Ⅵ-057 1#桨叶片角度","yc_hs_0433","cur_91"]
[4259,"b_右玉二期Ⅵ-057 2#桨叶片角度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","b_右玉二期Ⅵ-057 2#桨叶片角度","yc_hs_0433","cur_93"]
[4260,"b_右玉二期Ⅵ-057 3#桨叶片角度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","b_右玉二期Ⅵ-057 3#桨叶片角度","yc_hs_0433","cur_95"]
[4261,"b_右玉二期Ⅵ-057 主轴转速","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WTRM.RotorSpd","风轮转速","rotor_speed","b_右玉二期Ⅵ-057 主轴转速","yc_hs_0434","cur_19"]
[4262,"b_右玉二期Ⅵ-057 齿轮箱高速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","b_右玉二期Ⅵ-057 齿轮箱高速轴非驱动端轴承温度","yc_hs_0434","cur_23"]
[4263,"b_右玉二期Ⅵ-057 齿轮箱油池温度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","b_右玉二期Ⅵ-057 齿轮箱油池温度","yc_hs_0434","cur_24"]
[4264,"b_右玉二期Ⅵ-057 齿轮箱中速轴非驱动端轴承温度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","b_右玉二期Ⅵ-057 齿轮箱中速轴非驱动端轴承温度","yc_hs_0434","cur_26"]
[4265,"b_右玉二期Ⅵ-057 主轴承外圈温度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","b_右玉二期Ⅵ-057 主轴承外圈温度","yc_hs_0434","cur_27"]
[4266,"b_右玉二期Ⅵ-057 机舱侧向振动(已滤波)","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","b_右玉二期Ⅵ-057 机舱侧向振动(已滤波)","yc_hs_0434","cur_37"]
[4267,"b_右玉二期Ⅵ-057 机舱轴向振动(已滤波)","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","b_右玉二期Ⅵ-057 机舱轴向振动(已滤波)","yc_hs_0434","cur_39"]
[4268,"b_右玉二期Ⅵ-057 机舱角度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WYAW.NacellePosition","机舱位置","cabin_position","b_右玉二期Ⅵ-057 机舱角度","yc_hs_0434","cur_40"]
[4269,"b_右玉二期Ⅵ-057 扭缆角度","右玉风光互补电站","WOF34900079",57,"SXYY.T2_L3.WTG057.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","b_右玉二期Ⅵ-057 扭缆角度","yc_hs_0434","cur_42"]
[4270,"j_芮城二期Ⅰ-034 风速","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WNAC.WindSpeed","风速","wind_velocity","j_芮城二期Ⅰ-034 风速","yc_hs_0048","cur_80"]
[4271,"j_芮城二期Ⅰ-034 机舱与风向夹角","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城二期Ⅰ-034 机舱与风向夹角","yc_hs_0048","cur_83"]
[4272,"j_芮城二期Ⅰ-034 风向","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城二期Ⅰ-034 风向","yc_hs_0048","cur_73"]
[4273,"j_芮城二期Ⅰ-034 舱外温度","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城二期Ⅰ-034 舱外温度","yc_hs_0048","cur_68"]
[4274,"j_芮城二期Ⅰ-034 机舱角度（位置）","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城二期Ⅰ-034 机舱角度（位置）","yc_hs_0048","cur_63"]
[4275,"j_芮城二期Ⅰ-034 1#桨叶片角度(桨距角)","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城二期Ⅰ-034 1#桨叶片角度(桨距角)","yc_hs_0048","cur_85"]
[4276,"j_芮城二期Ⅰ-034 2#桨叶片角度(桨距角)","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城二期Ⅰ-034 2#桨叶片角度(桨距角)","yc_hs_0048","cur_87"]
[4277,"j_芮城二期Ⅰ-034 3#桨叶片角度(桨距角)","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城二期Ⅰ-034 3#桨叶片角度(桨距角)","yc_hs_0048","cur_96"]
[4278,"j_芮城二期Ⅰ-034 发电机转速","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WGEN.GenSpd","发电机转速","generator_speed","j_芮城二期Ⅰ-034 发电机转速","yc_hs_0048","cur_62"]
[4279,"j_芮城二期Ⅰ-034 发电机有功功率","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WGEN.GenActivePW","有功功率","active_power","j_芮城二期Ⅰ-034 发电机有功功率","yc_hs_0048","cur_12"]
[4280,"j_芮城二期Ⅰ-034 发电机绕组温度1","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","j_芮城二期Ⅰ-034 发电机绕组温度1","yc_hs_0048","cur_41"]
[4281,"j_芮城二期Ⅰ-034 发电机绕组温度2","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","j_芮城二期Ⅰ-034 发电机绕组温度2","yc_hs_0048","cur_42"]
[4282,"j_芮城二期Ⅰ-034 发电机绕组温度3","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","j_芮城二期Ⅰ-034 发电机绕组温度3","yc_hs_0048","cur_44"]
[4283,"j_芮城二期Ⅰ-034 舱内温度","芮城风电场","WOF35900078",34,"SXRC.T2_L3.WTG034.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城二期Ⅰ-034 舱内温度","yc_hs_0048","cur_64"]
[4284,"j_芮城二期Ⅰ-035 舱外温度","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城二期Ⅰ-035 舱外温度","yc_hs_0055","cur_97"]
[4285,"j_芮城二期Ⅰ-035 机舱角度（位置）","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城二期Ⅰ-035 机舱角度（位置）","yc_hs_0055","cur_94"]
[4286,"j_芮城二期Ⅰ-035 1#桨叶片角度(桨距角)","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城二期Ⅰ-035 1#桨叶片角度(桨距角)","yc_hs_0056","cur_06"]
[4287,"j_芮城二期Ⅰ-035 2#桨叶片角度(桨距角)","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城二期Ⅰ-035 2#桨叶片角度(桨距角)","yc_hs_0056","cur_07"]
[4288,"j_芮城二期Ⅰ-035 3#桨叶片角度(桨距角)","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城二期Ⅰ-035 3#桨叶片角度(桨距角)","yc_hs_0056","cur_11"]
[4289,"j_芮城二期Ⅰ-035 发电机转速","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WGEN.GenSpd","发电机转速","generator_speed","j_芮城二期Ⅰ-035 发电机转速","yc_hs_0055","cur_92"]
[4290,"j_芮城二期Ⅰ-035 发电机有功功率","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WGEN.GenActivePW","有功功率","active_power","j_芮城二期Ⅰ-035 发电机有功功率","yc_hs_0055","cur_77"]
[4291,"j_芮城二期Ⅰ-035 发电机绕组温度1","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","j_芮城二期Ⅰ-035 发电机绕组温度1","yc_hs_0055","cur_85"]
[4292,"j_芮城二期Ⅰ-035 发电机绕组温度2","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","j_芮城二期Ⅰ-035 发电机绕组温度2","yc_hs_0055","cur_86"]
[4293,"j_芮城二期Ⅰ-035 发电机绕组温度3","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","j_芮城二期Ⅰ-035 发电机绕组温度3","yc_hs_0055","cur_87"]
[4294,"j_芮城二期Ⅰ-035 舱内温度","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城二期Ⅰ-035 舱内温度","yc_hs_0055","cur_96"]
[4295,"j_芮城二期Ⅰ-035 风速","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WNAC.WindSpeed","风速","wind_velocity","j_芮城二期Ⅰ-035 风速","yc_hs_0056","cur_01"]
[4296,"j_芮城二期Ⅰ-035 机舱与风向夹角","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城二期Ⅰ-035 机舱与风向夹角","yc_hs_0056","cur_05"]
[4297,"j_芮城二期Ⅰ-035 风向","芮城风电场","WOF35900078",35,"SXRC.T2_L3.WTG035.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城二期Ⅰ-035 风向","yc_hs_0055","cur_100"]
[4298,"j_芮城二期Ⅰ-036 发电机绕组温度1","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","j_芮城二期Ⅰ-036 发电机绕组温度1","yc_hs_0056","cur_87"]
[4299,"j_芮城二期Ⅰ-036 发电机绕组温度2","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","j_芮城二期Ⅰ-036 发电机绕组温度2","yc_hs_0056","cur_94"]
[4300,"j_芮城二期Ⅰ-036 发电机绕组温度3","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","j_芮城二期Ⅰ-036 发电机绕组温度3","yc_hs_0056","cur_97"]
[4301,"j_芮城二期Ⅰ-036 舱内温度","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城二期Ⅰ-036 舱内温度","yc_hs_0057","cur_06"]
[4302,"j_芮城二期Ⅰ-036 风速","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WNAC.WindSpeed","风速","wind_velocity","j_芮城二期Ⅰ-036 风速","yc_hs_0057","cur_11"]
[4303,"j_芮城二期Ⅰ-036 机舱与风向夹角","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城二期Ⅰ-036 机舱与风向夹角","yc_hs_0057","cur_12"]
[4304,"j_芮城二期Ⅰ-036 风向","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城二期Ⅰ-036 风向","yc_hs_0057","cur_10"]
[4305,"j_芮城二期Ⅰ-036 舱外温度","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城二期Ⅰ-036 舱外温度","yc_hs_0057","cur_07"]
[4306,"j_芮城二期Ⅰ-036 机舱角度（位置）","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城二期Ⅰ-036 机舱角度（位置）","yc_hs_0057","cur_05"]
[4307,"j_芮城二期Ⅰ-036 1#桨叶片角度(桨距角)","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城二期Ⅰ-036 1#桨叶片角度(桨距角)","yc_hs_0057","cur_13"]
[4308,"j_芮城二期Ⅰ-036 2#桨叶片角度(桨距角)","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城二期Ⅰ-036 2#桨叶片角度(桨距角)","yc_hs_0057","cur_14"]
[4309,"j_芮城二期Ⅰ-036 3#桨叶片角度(桨距角)","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城二期Ⅰ-036 3#桨叶片角度(桨距角)","yc_hs_0057","cur_15"]
[4310,"j_芮城二期Ⅰ-036 发电机转速","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WGEN.GenSpd","发电机转速","generator_speed","j_芮城二期Ⅰ-036 发电机转速","yc_hs_0057","cur_04"]
[4311,"j_芮城二期Ⅰ-036 发电机有功功率","芮城风电场","WOF35900078",36,"SXRC.T2_L3.WTG036.WGEN.GenActivePW","有功功率","active_power","j_芮城二期Ⅰ-036 发电机有功功率","yc_hs_0056","cur_82"]
[4312,"j_芮城二期Ⅰ-037 风速","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WNAC.WindSpeed","风速","wind_velocity","j_芮城二期Ⅰ-037 风速","yc_hs_0057","cur_69"]
[4313,"j_芮城二期Ⅰ-037 机舱与风向夹角","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城二期Ⅰ-037 机舱与风向夹角","yc_hs_0057","cur_70"]
[4314,"j_芮城二期Ⅰ-037 风向","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城二期Ⅰ-037 风向","yc_hs_0057","cur_67"]
[4315,"j_芮城二期Ⅰ-037 舱外温度","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城二期Ⅰ-037 舱外温度","yc_hs_0057","cur_64"]
[4316,"j_芮城二期Ⅰ-037 机舱角度（位置）","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城二期Ⅰ-037 机舱角度（位置）","yc_hs_0057","cur_62"]
[4317,"j_芮城二期Ⅰ-037 1#桨叶片角度(桨距角)","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城二期Ⅰ-037 1#桨叶片角度(桨距角)","yc_hs_0057","cur_72"]
[4318,"j_芮城二期Ⅰ-037 2#桨叶片角度(桨距角)","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城二期Ⅰ-037 2#桨叶片角度(桨距角)","yc_hs_0057","cur_74"]
[4319,"j_芮城二期Ⅰ-037 3#桨叶片角度(桨距角)","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城二期Ⅰ-037 3#桨叶片角度(桨距角)","yc_hs_0057","cur_76"]
[4320,"j_芮城二期Ⅰ-037 发电机转速","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WGEN.GenSpd","发电机转速","generator_speed","j_芮城二期Ⅰ-037 发电机转速","yc_hs_0057","cur_60"]
[4321,"j_芮城二期Ⅰ-037 发电机有功功率","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WGEN.GenActivePW","有功功率","active_power","j_芮城二期Ⅰ-037 发电机有功功率","yc_hs_0057","cur_45"]
[4322,"j_芮城二期Ⅰ-037 发电机绕组温度1","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","j_芮城二期Ⅰ-037 发电机绕组温度1","yc_hs_0057","cur_48"]
[4323,"j_芮城二期Ⅰ-037 发电机绕组温度2","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","j_芮城二期Ⅰ-037 发电机绕组温度2","yc_hs_0057","cur_49"]
[4324,"j_芮城二期Ⅰ-037 发电机绕组温度3","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","j_芮城二期Ⅰ-037 发电机绕组温度3","yc_hs_0057","cur_53"]
[4325,"j_芮城二期Ⅰ-037 舱内温度","芮城风电场","WOF35900078",37,"SXRC.T2_L3.WTG037.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城二期Ⅰ-037 舱内温度","yc_hs_0057","cur_63"]
[4326,"j_芮城二期Ⅰ-038 风速","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WNAC.WindSpeed","风速","wind_velocity","j_芮城二期Ⅰ-038 风速","yc_hs_0060","cur_92"]
[4327,"j_芮城二期Ⅰ-038 机舱与风向夹角","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城二期Ⅰ-038 机舱与风向夹角","yc_hs_0060","cur_93"]
[4328,"j_芮城二期Ⅰ-038 风向","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城二期Ⅰ-038 风向","yc_hs_0060","cur_91"]
[4329,"j_芮城二期Ⅰ-038 舱外温度","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城二期Ⅰ-038 舱外温度","yc_hs_0060","cur_88"]
[4330,"j_芮城二期Ⅰ-038 机舱角度（位置）","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城二期Ⅰ-038 机舱角度（位置）","yc_hs_0060","cur_86"]
[4331,"j_芮城二期Ⅰ-038 1#桨叶片角度(桨距角)","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城二期Ⅰ-038 1#桨叶片角度(桨距角)","yc_hs_0060","cur_94"]
[4332,"j_芮城二期Ⅰ-038 2#桨叶片角度(桨距角)","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城二期Ⅰ-038 2#桨叶片角度(桨距角)","yc_hs_0060","cur_95"]
[4333,"j_芮城二期Ⅰ-038 3#桨叶片角度(桨距角)","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城二期Ⅰ-038 3#桨叶片角度(桨距角)","yc_hs_0060","cur_96"]
[4334,"j_芮城二期Ⅰ-038 发电机转速","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WGEN.GenSpd","发电机转速","generator_speed","j_芮城二期Ⅰ-038 发电机转速","yc_hs_0060","cur_85"]
[4335,"j_芮城二期Ⅰ-038 发电机有功功率","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WGEN.GenActivePW","有功功率","active_power","j_芮城二期Ⅰ-038 发电机有功功率","yc_hs_0060","cur_75"]
[4336,"j_芮城二期Ⅰ-038 发电机绕组温度1","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","j_芮城二期Ⅰ-038 发电机绕组温度1","yc_hs_0060","cur_78"]
[4337,"j_芮城二期Ⅰ-038 发电机绕组温度2","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","j_芮城二期Ⅰ-038 发电机绕组温度2","yc_hs_0060","cur_79"]
[4338,"j_芮城二期Ⅰ-038 发电机绕组温度3","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","j_芮城二期Ⅰ-038 发电机绕组温度3","yc_hs_0060","cur_81"]
[4339,"j_芮城二期Ⅰ-038 舱内温度","芮城风电场","WOF35900078",38,"SXRC.T2_L3.WTG038.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城二期Ⅰ-038 舱内温度","yc_hs_0060","cur_87"]
[4340,"j_芮城二期Ⅰ-039 风速","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WNAC.WindSpeed","风速","wind_velocity","j_芮城二期Ⅰ-039 风速","yc_hs_0061","cur_94"]
[4341,"j_芮城二期Ⅰ-039 机舱与风向夹角","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城二期Ⅰ-039 机舱与风向夹角","yc_hs_0061","cur_95"]
[4342,"j_芮城二期Ⅰ-039 风向","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城二期Ⅰ-039 风向","yc_hs_0061","cur_87"]
[4343,"j_芮城二期Ⅰ-039 舱外温度","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城二期Ⅰ-039 舱外温度","yc_hs_0061","cur_76"]
[4344,"j_芮城二期Ⅰ-039 机舱角度（位置）","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城二期Ⅰ-039 机舱角度（位置）","yc_hs_0061","cur_73"]
[4345,"j_芮城二期Ⅰ-039 1#桨叶片角度(桨距角)","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城二期Ⅰ-039 1#桨叶片角度(桨距角)","yc_hs_0061","cur_96"]
[4346,"j_芮城二期Ⅰ-039 2#桨叶片角度(桨距角)","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城二期Ⅰ-039 2#桨叶片角度(桨距角)","yc_hs_0061","cur_100"]
[4347,"j_芮城二期Ⅰ-039 3#桨叶片角度(桨距角)","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城二期Ⅰ-039 3#桨叶片角度(桨距角)","yc_hs_0062","cur_01"]
[4348,"j_芮城二期Ⅰ-039 发电机转速","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WGEN.GenSpd","发电机转速","generator_speed","j_芮城二期Ⅰ-039 发电机转速","yc_hs_0061","cur_72"]
[4349,"j_芮城二期Ⅰ-039 发电机有功功率","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WGEN.GenActivePW","有功功率","active_power","j_芮城二期Ⅰ-039 发电机有功功率","yc_hs_0061","cur_34"]
[4350,"j_芮城二期Ⅰ-039 发电机绕组温度1","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","j_芮城二期Ⅰ-039 发电机绕组温度1","yc_hs_0061","cur_37"]
[4351,"j_芮城二期Ⅰ-039 发电机绕组温度2","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","j_芮城二期Ⅰ-039 发电机绕组温度2","yc_hs_0061","cur_39"]
[4352,"j_芮城二期Ⅰ-039 发电机绕组温度3","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","j_芮城二期Ⅰ-039 发电机绕组温度3","yc_hs_0061","cur_40"]
[4353,"j_芮城二期Ⅰ-039 舱内温度","芮城风电场","WOF35900078",39,"SXRC.T2_L3.WTG039.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城二期Ⅰ-039 舱内温度","yc_hs_0061","cur_74"]
[4354,"j_芮城二期Ⅰ-040 发电机绕组温度3","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","j_芮城二期Ⅰ-040 发电机绕组温度3","yc_hs_0317","cur_24"]
[4355,"j_芮城二期Ⅰ-040 舱内温度","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城二期Ⅰ-040 舱内温度","yc_hs_0317","cur_30"]
[4356,"j_芮城二期Ⅰ-040 风速","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WNAC.WindSpeed","风速","wind_velocity","j_芮城二期Ⅰ-040 风速","yc_hs_0317","cur_35"]
[4357,"j_芮城二期Ⅰ-040 机舱与风向夹角","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城二期Ⅰ-040 机舱与风向夹角","yc_hs_0317","cur_36"]
[4358,"j_芮城二期Ⅰ-040 风向","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城二期Ⅰ-040 风向","yc_hs_0317","cur_34"]
[4359,"j_芮城二期Ⅰ-040 舱外温度","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城二期Ⅰ-040 舱外温度","yc_hs_0317","cur_31"]
[4360,"j_芮城二期Ⅰ-040 机舱角度（位置）","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城二期Ⅰ-040 机舱角度（位置）","yc_hs_0317","cur_29"]
[4361,"j_芮城二期Ⅰ-040 1#桨叶片角度(桨距角)","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城二期Ⅰ-040 1#桨叶片角度(桨距角)","yc_hs_0317","cur_37"]
[4362,"j_芮城二期Ⅰ-040 2#桨叶片角度(桨距角)","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城二期Ⅰ-040 2#桨叶片角度(桨距角)","yc_hs_0317","cur_38"]
[4363,"j_芮城二期Ⅰ-040 3#桨叶片角度(桨距角)","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城二期Ⅰ-040 3#桨叶片角度(桨距角)","yc_hs_0317","cur_39"]
[4364,"j_芮城二期Ⅰ-040 发电机转速","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WGEN.GenSpd","发电机转速","generator_speed","j_芮城二期Ⅰ-040 发电机转速","yc_hs_0317","cur_28"]
[4365,"j_芮城二期Ⅰ-040 发电机有功功率","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WGEN.GenActivePW","有功功率","active_power","j_芮城二期Ⅰ-040 发电机有功功率","yc_hs_0317","cur_19"]
[4366,"j_芮城二期Ⅰ-040 发电机绕组温度1","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","j_芮城二期Ⅰ-040 发电机绕组温度1","yc_hs_0317","cur_22"]
[4367,"j_芮城二期Ⅰ-040 发电机绕组温度2","芮城风电场","WOF35900078",40,"SXRC.T2_L3.WTG040.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","j_芮城二期Ⅰ-040 发电机绕组温度2","yc_hs_0317","cur_23"]
[4368,"j_芮城二期Ⅰ-041 风速","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WNAC.WindSpeed","风速","wind_velocity","j_芮城二期Ⅰ-041 风速","yc_hs_0317","cur_78"]
[4369,"j_芮城二期Ⅰ-041 机舱与风向夹角","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城二期Ⅰ-041 机舱与风向夹角","yc_hs_0317","cur_79"]
[4370,"j_芮城二期Ⅰ-041 风向","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城二期Ⅰ-041 风向","yc_hs_0317","cur_77"]
[4371,"j_芮城二期Ⅰ-041 舱外温度","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城二期Ⅰ-041 舱外温度","yc_hs_0317","cur_74"]
[4372,"j_芮城二期Ⅰ-041 机舱角度（位置）","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城二期Ⅰ-041 机舱角度（位置）","yc_hs_0317","cur_72"]
[4373,"j_芮城二期Ⅰ-041 1#桨叶片角度(桨距角)","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城二期Ⅰ-041 1#桨叶片角度(桨距角)","yc_hs_0317","cur_80"]
[4374,"j_芮城二期Ⅰ-041 2#桨叶片角度(桨距角)","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城二期Ⅰ-041 2#桨叶片角度(桨距角)","yc_hs_0317","cur_81"]
[4375,"j_芮城二期Ⅰ-041 3#桨叶片角度(桨距角)","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城二期Ⅰ-041 3#桨叶片角度(桨距角)","yc_hs_0317","cur_82"]
[4376,"j_芮城二期Ⅰ-041 发电机转速","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WGEN.GenSpd","发电机转速","generator_speed","j_芮城二期Ⅰ-041 发电机转速","yc_hs_0317","cur_71"]
[4377,"j_芮城二期Ⅰ-041 发电机有功功率","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WGEN.GenActivePW","有功功率","active_power","j_芮城二期Ⅰ-041 发电机有功功率","yc_hs_0317","cur_62"]
[4378,"j_芮城二期Ⅰ-041 发电机绕组温度1","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","j_芮城二期Ⅰ-041 发电机绕组温度1","yc_hs_0317","cur_65"]
[4379,"j_芮城二期Ⅰ-041 发电机绕组温度2","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","j_芮城二期Ⅰ-041 发电机绕组温度2","yc_hs_0317","cur_66"]
[4380,"j_芮城二期Ⅰ-041 发电机绕组温度3","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","j_芮城二期Ⅰ-041 发电机绕组温度3","yc_hs_0317","cur_67"]
[4381,"j_芮城二期Ⅰ-041 舱内温度","芮城风电场","WOF35900078",41,"SXRC.T2_L3.WTG041.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城二期Ⅰ-041 舱内温度","yc_hs_0317","cur_73"]
[4382,"j_芮城二期Ⅰ-042 风速","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WNAC.WindSpeed","风速","wind_velocity","j_芮城二期Ⅰ-042 风速","yc_hs_0322","cur_35"]
[4383,"j_芮城二期Ⅰ-042 机舱与风向夹角","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城二期Ⅰ-042 机舱与风向夹角","yc_hs_0322","cur_36"]
[4384,"j_芮城二期Ⅰ-042 风向","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城二期Ⅰ-042 风向","yc_hs_0322","cur_34"]
[4385,"j_芮城二期Ⅰ-042 舱外温度","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城二期Ⅰ-042 舱外温度","yc_hs_0322","cur_31"]
[4386,"j_芮城二期Ⅰ-042 机舱角度（位置）","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城二期Ⅰ-042 机舱角度（位置）","yc_hs_0322","cur_29"]
[4387,"j_芮城二期Ⅰ-042 1#桨叶片角度(桨距角)","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城二期Ⅰ-042 1#桨叶片角度(桨距角)","yc_hs_0322","cur_37"]
[4388,"j_芮城二期Ⅰ-042 2#桨叶片角度(桨距角)","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城二期Ⅰ-042 2#桨叶片角度(桨距角)","yc_hs_0322","cur_38"]
[4389,"j_芮城二期Ⅰ-042 3#桨叶片角度(桨距角)","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城二期Ⅰ-042 3#桨叶片角度(桨距角)","yc_hs_0322","cur_39"]
[4390,"j_芮城二期Ⅰ-042 发电机转速","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WGEN.GenSpd","发电机转速","generator_speed","j_芮城二期Ⅰ-042 发电机转速","yc_hs_0322","cur_28"]
[4391,"j_芮城二期Ⅰ-042 发电机有功功率","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WGEN.GenActivePW","有功功率","active_power","j_芮城二期Ⅰ-042 发电机有功功率","yc_hs_0322","cur_19"]
[4392,"j_芮城二期Ⅰ-042 发电机绕组温度1","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","j_芮城二期Ⅰ-042 发电机绕组温度1","yc_hs_0322","cur_22"]
[4393,"j_芮城二期Ⅰ-042 发电机绕组温度2","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","j_芮城二期Ⅰ-042 发电机绕组温度2","yc_hs_0322","cur_23"]
[4394,"j_芮城二期Ⅰ-042 发电机绕组温度3","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","j_芮城二期Ⅰ-042 发电机绕组温度3","yc_hs_0322","cur_24"]
[4395,"j_芮城二期Ⅰ-042 舱内温度","芮城风电场","WOF35900078",42,"SXRC.T2_L3.WTG042.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城二期Ⅰ-042 舱内温度","yc_hs_0322","cur_30"]
[4396,"j_芮城二期Ⅰ-043 风速","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WNAC.WindSpeed","风速","wind_velocity","j_芮城二期Ⅰ-043 风速","yc_hs_0322","cur_78"]
[4397,"j_芮城二期Ⅰ-043 机舱与风向夹角","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WNAC.WindVaneDirection","对风角度","yaw_error1","j_芮城二期Ⅰ-043 机舱与风向夹角","yc_hs_0322","cur_79"]
[4398,"j_芮城二期Ⅰ-043 风向","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WNAC.WindDirection","绝对风向","true_wind_direction","j_芮城二期Ⅰ-043 风向","yc_hs_0322","cur_77"]
[4399,"j_芮城二期Ⅰ-043 舱外温度","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WNAC.TemOut","环境温度","outside_cabin_temperature","j_芮城二期Ⅰ-043 舱外温度","yc_hs_0322","cur_74"]
[4400,"j_芮城二期Ⅰ-043 机舱角度（位置）","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WYAW.NacellePosition","机舱位置","cabin_position","j_芮城二期Ⅰ-043 机舱角度（位置）","yc_hs_0322","cur_72"]
[4401,"j_芮城二期Ⅰ-043 1#桨叶片角度(桨距角)","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","j_芮城二期Ⅰ-043 1#桨叶片角度(桨距角)","yc_hs_0322","cur_80"]
[4402,"j_芮城二期Ⅰ-043 2#桨叶片角度(桨距角)","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","j_芮城二期Ⅰ-043 2#桨叶片角度(桨距角)","yc_hs_0322","cur_81"]
[4403,"j_芮城二期Ⅰ-043 3#桨叶片角度(桨距角)","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","j_芮城二期Ⅰ-043 3#桨叶片角度(桨距角)","yc_hs_0322","cur_82"]
[4404,"j_芮城二期Ⅰ-043 发电机转速","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WGEN.GenSpd","发电机转速","generator_speed","j_芮城二期Ⅰ-043 发电机转速","yc_hs_0322","cur_71"]
[4405,"j_芮城二期Ⅰ-043 发电机有功功率","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WGEN.GenActivePW","有功功率","active_power","j_芮城二期Ⅰ-043 发电机有功功率","yc_hs_0322","cur_62"]
[4406,"j_芮城二期Ⅰ-043 发电机绕组温度1","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","j_芮城二期Ⅰ-043 发电机绕组温度1","yc_hs_0322","cur_65"]
[4407,"j_芮城二期Ⅰ-043 发电机绕组温度2","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","j_芮城二期Ⅰ-043 发电机绕组温度2","yc_hs_0322","cur_66"]
[4408,"j_芮城二期Ⅰ-043 发电机绕组温度3","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","j_芮城二期Ⅰ-043 发电机绕组温度3","yc_hs_0322","cur_67"]
[4409,"j_芮城二期Ⅰ-043 舱内温度","芮城风电场","WOF35900078",43,"SXRC.T2_L3.WTG043.WNAC.TemNacelle","机舱内温度","cabin_temperature","j_芮城二期Ⅰ-043 舱内温度","yc_hs_0322","cur_73"]
[4410,"f_盂县三期Ⅴ-057 发电机有功功率","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WGEN.GenActivePW","有功功率","active_power","f_盂县三期Ⅴ-057 发电机有功功率","yc_hs_0315","cur_98"]
[4411,"f_盂县三期Ⅴ-057 主轴(风轮)转速","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县三期Ⅴ-057 主轴(风轮)转速","yc_hs_0315","cur_100"]
[4412,"f_盂县三期Ⅴ-057 1#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县三期Ⅴ-057 1#桨叶片角度(桨距角)","yc_hs_0348","cur_02"]
[4413,"f_盂县三期Ⅴ-057 2#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县三期Ⅴ-057 2#桨叶片角度(桨距角)","yc_hs_0348","cur_03"]
[4414,"f_盂县三期Ⅴ-057 3#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县三期Ⅴ-057 3#桨叶片角度(桨距角)","yc_hs_0348","cur_04"]
[4415,"f_盂县三期Ⅴ-057 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县三期Ⅴ-057 齿轮箱高速轴非驱动端轴承温度","yc_hs_0348","cur_06"]
[4416,"f_盂县三期Ⅴ-057 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县三期Ⅴ-057 发电机驱动端轴承温度","yc_hs_0348","cur_07"]
[4417,"f_盂县三期Ⅴ-057 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县三期Ⅴ-057 发电机非驱动端轴承温度","yc_hs_0348","cur_08"]
[4418,"f_盂县三期Ⅴ-057 齿轮箱油池温度","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县三期Ⅴ-057 齿轮箱油池温度","yc_hs_0348","cur_09"]
[4419,"f_盂县三期Ⅴ-057 发电机转速","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WGEN.GenSpd","发电机转速","generator_speed","f_盂县三期Ⅴ-057 发电机转速","yc_hs_0348","cur_12"]
[4420,"f_盂县三期Ⅴ-057 发电机绕组温度1","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","f_盂县三期Ⅴ-057 发电机绕组温度1","yc_hs_0348","cur_13"]
[4421,"f_盂县三期Ⅴ-057 发电机绕组温度2","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","f_盂县三期Ⅴ-057 发电机绕组温度2","yc_hs_0348","cur_14"]
[4422,"f_盂县三期Ⅴ-057 发电机绕组温度3","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","f_盂县三期Ⅴ-057 发电机绕组温度3","yc_hs_0348","cur_15"]
[4423,"f_盂县三期Ⅴ-057 机舱角度（位置）","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县三期Ⅴ-057 机舱角度（位置）","yc_hs_0348","cur_30"]
[4424,"f_盂县三期Ⅴ-057 风速","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WNAC.WindSpeed","风速","wind_velocity","f_盂县三期Ⅴ-057 风速","yc_hs_0348","cur_31"]
[4425,"f_盂县三期Ⅴ-057 风向","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县三期Ⅴ-057 风向","yc_hs_0348","cur_32"]
[4426,"f_盂县三期Ⅴ-057 瞬时风向","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WNAC.WindDirectionInstant","对风角度","yaw_error1","f_盂县三期Ⅴ-057 瞬时风向","yc_hs_0348","cur_33"]
[4427,"f_盂县三期Ⅴ-057 舱外温度","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县三期Ⅴ-057 舱外温度","yc_hs_0348","cur_34"]
[4428,"f_盂县三期Ⅴ-057 舱内温度","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县三期Ⅴ-057 舱内温度","yc_hs_0348","cur_35"]
[4429,"f_盂县三期Ⅴ-057 机舱侧向振动值(已滤波)","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县三期Ⅴ-057 机舱侧向振动值(已滤波)","yc_hs_0348","cur_37"]
[4430,"f_盂县三期Ⅴ-057 机舱轴向振动值(已滤波)","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县三期Ⅴ-057 机舱轴向振动值(已滤波)","yc_hs_0348","cur_38"]
[4431,"f_盂县三期Ⅴ-057 扭揽角度","盂县风光互补电站","WOF35800082",57,"SXYX.T3_L5.WTG057.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县三期Ⅴ-057 扭揽角度","yc_hs_0348","cur_40"]
[4432,"f_盂县三期Ⅴ-058 发电机有功功率","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WGEN.GenActivePW","有功功率","active_power","f_盂县三期Ⅴ-058 发电机有功功率","yc_hs_0348","cur_54"]
[4433,"f_盂县三期Ⅴ-058 主轴(风轮)转速","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县三期Ⅴ-058 主轴(风轮)转速","yc_hs_0348","cur_56"]
[4434,"f_盂县三期Ⅴ-058 1#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县三期Ⅴ-058 1#桨叶片角度(桨距角)","yc_hs_0348","cur_58"]
[4435,"f_盂县三期Ⅴ-058 2#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县三期Ⅴ-058 2#桨叶片角度(桨距角)","yc_hs_0348","cur_59"]
[4436,"f_盂县三期Ⅴ-058 3#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县三期Ⅴ-058 3#桨叶片角度(桨距角)","yc_hs_0348","cur_60"]
[4437,"f_盂县三期Ⅴ-058 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县三期Ⅴ-058 齿轮箱高速轴非驱动端轴承温度","yc_hs_0348","cur_62"]
[4438,"f_盂县三期Ⅴ-058 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县三期Ⅴ-058 发电机驱动端轴承温度","yc_hs_0348","cur_63"]
[4439,"f_盂县三期Ⅴ-058 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县三期Ⅴ-058 发电机非驱动端轴承温度","yc_hs_0348","cur_64"]
[4440,"f_盂县三期Ⅴ-058 齿轮箱油池温度","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县三期Ⅴ-058 齿轮箱油池温度","yc_hs_0348","cur_65"]
[4441,"f_盂县三期Ⅴ-058 发电机转速","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WGEN.GenSpd","发电机转速","generator_speed","f_盂县三期Ⅴ-058 发电机转速","yc_hs_0348","cur_68"]
[4442,"f_盂县三期Ⅴ-058 发电机绕组温度1","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","f_盂县三期Ⅴ-058 发电机绕组温度1","yc_hs_0348","cur_69"]
[4443,"f_盂县三期Ⅴ-058 发电机绕组温度2","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","f_盂县三期Ⅴ-058 发电机绕组温度2","yc_hs_0348","cur_70"]
[4444,"f_盂县三期Ⅴ-058 发电机绕组温度3","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","f_盂县三期Ⅴ-058 发电机绕组温度3","yc_hs_0348","cur_71"]
[4445,"f_盂县三期Ⅴ-058 机舱角度（位置）","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县三期Ⅴ-058 机舱角度（位置）","yc_hs_0348","cur_86"]
[4446,"f_盂县三期Ⅴ-058 风速","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WNAC.WindSpeed","风速","wind_velocity","f_盂县三期Ⅴ-058 风速","yc_hs_0348","cur_87"]
[4447,"f_盂县三期Ⅴ-058 风向","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县三期Ⅴ-058 风向","yc_hs_0348","cur_88"]
[4448,"f_盂县三期Ⅴ-058 瞬时风向","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WNAC.WindDirectionInstant","对风角度","yaw_error1","f_盂县三期Ⅴ-058 瞬时风向","yc_hs_0348","cur_89"]
[4449,"f_盂县三期Ⅴ-058 舱外温度","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县三期Ⅴ-058 舱外温度","yc_hs_0348","cur_90"]
[4450,"f_盂县三期Ⅴ-058 舱内温度","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县三期Ⅴ-058 舱内温度","yc_hs_0348","cur_44"]
[4451,"f_盂县三期Ⅴ-058 机舱侧向振动值(已滤波)","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县三期Ⅴ-058 机舱侧向振动值(已滤波)","yc_hs_0348","cur_46"]
[4452,"f_盂县三期Ⅴ-058 机舱轴向振动值(已滤波)","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县三期Ⅴ-058 机舱轴向振动值(已滤波)","yc_hs_0348","cur_47"]
[4453,"f_盂县三期Ⅴ-058 扭揽角度","盂县风光互补电站","WOF35800082",58,"SXYX.T3_L5.WTG058.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县三期Ⅴ-058 扭揽角度","yc_hs_0348","cur_49"]
[4454,"f_盂县三期Ⅴ-059 发电机有功功率","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WGEN.GenActivePW","有功功率","active_power","f_盂县三期Ⅴ-059 发电机有功功率","yc_hs_0348","cur_92"]
[4455,"f_盂县三期Ⅴ-059 主轴(风轮)转速","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县三期Ⅴ-059 主轴(风轮)转速","yc_hs_0348","cur_94"]
[4456,"f_盂县三期Ⅴ-059 1#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县三期Ⅴ-059 1#桨叶片角度(桨距角)","yc_hs_0348","cur_96"]
[4457,"f_盂县三期Ⅴ-059 2#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县三期Ⅴ-059 2#桨叶片角度(桨距角)","yc_hs_0348","cur_97"]
[4458,"f_盂县三期Ⅴ-059 3#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县三期Ⅴ-059 3#桨叶片角度(桨距角)","yc_hs_0348","cur_98"]
[4459,"f_盂县三期Ⅴ-059 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县三期Ⅴ-059 齿轮箱高速轴非驱动端轴承温度","yc_hs_0348","cur_100"]
[4460,"f_盂县三期Ⅴ-059 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县三期Ⅴ-059 发电机驱动端轴承温度","yc_hs_0349","cur_01"]
[4461,"f_盂县三期Ⅴ-059 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县三期Ⅴ-059 发电机非驱动端轴承温度","yc_hs_0349","cur_02"]
[4462,"f_盂县三期Ⅴ-059 齿轮箱油池温度","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县三期Ⅴ-059 齿轮箱油池温度","yc_hs_0349","cur_03"]
[4463,"f_盂县三期Ⅴ-059 发电机转速","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WGEN.GenSpd","发电机转速","generator_speed","f_盂县三期Ⅴ-059 发电机转速","yc_hs_0349","cur_06"]
[4464,"f_盂县三期Ⅴ-059 发电机绕组温度1","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","f_盂县三期Ⅴ-059 发电机绕组温度1","yc_hs_0349","cur_07"]
[4465,"f_盂县三期Ⅴ-059 发电机绕组温度2","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","f_盂县三期Ⅴ-059 发电机绕组温度2","yc_hs_0349","cur_08"]
[4466,"f_盂县三期Ⅴ-059 发电机绕组温度3","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","f_盂县三期Ⅴ-059 发电机绕组温度3","yc_hs_0349","cur_09"]
[4467,"f_盂县三期Ⅴ-059 机舱角度（位置）","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县三期Ⅴ-059 机舱角度（位置）","yc_hs_0349","cur_24"]
[4468,"f_盂县三期Ⅴ-059 风速","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WNAC.WindSpeed","风速","wind_velocity","f_盂县三期Ⅴ-059 风速","yc_hs_0349","cur_25"]
[4469,"f_盂县三期Ⅴ-059 风向","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县三期Ⅴ-059 风向","yc_hs_0349","cur_26"]
[4470,"f_盂县三期Ⅴ-059 瞬时风向","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WNAC.WindDirectionInstant","对风角度","yaw_error1","f_盂县三期Ⅴ-059 瞬时风向","yc_hs_0349","cur_27"]
[4471,"f_盂县三期Ⅴ-059 舱外温度","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县三期Ⅴ-059 舱外温度","yc_hs_0349","cur_28"]
[4472,"f_盂县三期Ⅴ-059 舱内温度","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县三期Ⅴ-059 舱内温度","yc_hs_0349","cur_29"]
[4473,"f_盂县三期Ⅴ-059 机舱侧向振动值(已滤波)","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县三期Ⅴ-059 机舱侧向振动值(已滤波)","yc_hs_0349","cur_31"]
[4474,"f_盂县三期Ⅴ-059 机舱轴向振动值(已滤波)","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县三期Ⅴ-059 机舱轴向振动值(已滤波)","yc_hs_0349","cur_32"]
[4475,"f_盂县三期Ⅴ-059 扭揽角度","盂县风光互补电站","WOF35800082",59,"SXYX.T3_L5.WTG059.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县三期Ⅴ-059 扭揽角度","yc_hs_0349","cur_34"]
[4476,"f_盂县三期Ⅴ-060 发电机有功功率","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WGEN.GenActivePW","有功功率","active_power","f_盂县三期Ⅴ-060 发电机有功功率","yc_hs_0349","cur_39"]
[4477,"f_盂县三期Ⅴ-060 主轴(风轮)转速","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县三期Ⅴ-060 主轴(风轮)转速","yc_hs_0349","cur_41"]
[4478,"f_盂县三期Ⅴ-060 1#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县三期Ⅴ-060 1#桨叶片角度(桨距角)","yc_hs_0349","cur_43"]
[4479,"f_盂县三期Ⅴ-060 2#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县三期Ⅴ-060 2#桨叶片角度(桨距角)","yc_hs_0349","cur_44"]
[4480,"f_盂县三期Ⅴ-060 3#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县三期Ⅴ-060 3#桨叶片角度(桨距角)","yc_hs_0349","cur_45"]
[4481,"f_盂县三期Ⅴ-060 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县三期Ⅴ-060 齿轮箱高速轴非驱动端轴承温度","yc_hs_0349","cur_47"]
[4482,"f_盂县三期Ⅴ-060 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县三期Ⅴ-060 发电机驱动端轴承温度","yc_hs_0349","cur_48"]
[4483,"f_盂县三期Ⅴ-060 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县三期Ⅴ-060 发电机非驱动端轴承温度","yc_hs_0349","cur_49"]
[4484,"f_盂县三期Ⅴ-060 齿轮箱油池温度","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县三期Ⅴ-060 齿轮箱油池温度","yc_hs_0349","cur_50"]
[4485,"f_盂县三期Ⅴ-060 发电机转速","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WGEN.GenSpd","发电机转速","generator_speed","f_盂县三期Ⅴ-060 发电机转速","yc_hs_0349","cur_53"]
[4486,"f_盂县三期Ⅴ-060 发电机绕组温度1","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","f_盂县三期Ⅴ-060 发电机绕组温度1","yc_hs_0349","cur_54"]
[4487,"f_盂县三期Ⅴ-060 发电机绕组温度2","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","f_盂县三期Ⅴ-060 发电机绕组温度2","yc_hs_0349","cur_55"]
[4488,"f_盂县三期Ⅴ-060 发电机绕组温度3","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","f_盂县三期Ⅴ-060 发电机绕组温度3","yc_hs_0349","cur_56"]
[4489,"f_盂县三期Ⅴ-060 机舱角度（位置）","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县三期Ⅴ-060 机舱角度（位置）","yc_hs_0349","cur_71"]
[4490,"f_盂县三期Ⅴ-060 风速","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WNAC.WindSpeed","风速","wind_velocity","f_盂县三期Ⅴ-060 风速","yc_hs_0349","cur_72"]
[4491,"f_盂县三期Ⅴ-060 风向","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县三期Ⅴ-060 风向","yc_hs_0349","cur_73"]
[4492,"f_盂县三期Ⅴ-060 瞬时风向","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WNAC.WindDirectionInstant","对风角度","yaw_error1","f_盂县三期Ⅴ-060 瞬时风向","yc_hs_0349","cur_74"]
[4493,"f_盂县三期Ⅴ-060 舱外温度","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县三期Ⅴ-060 舱外温度","yc_hs_0349","cur_75"]
[4494,"f_盂县三期Ⅴ-060 舱内温度","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县三期Ⅴ-060 舱内温度","yc_hs_0349","cur_76"]
[4495,"f_盂县三期Ⅴ-060 机舱侧向振动值(已滤波)","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县三期Ⅴ-060 机舱侧向振动值(已滤波)","yc_hs_0349","cur_78"]
[4496,"f_盂县三期Ⅴ-060 机舱轴向振动值(已滤波)","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县三期Ⅴ-060 机舱轴向振动值(已滤波)","yc_hs_0349","cur_79"]
[4497,"f_盂县三期Ⅴ-060 扭揽角度","盂县风光互补电站","WOF35800082",60,"SXYX.T3_L5.WTG060.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县三期Ⅴ-060 扭揽角度","yc_hs_0349","cur_81"]
[4498,"f_盂县三期Ⅴ-061 发电机有功功率","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WGEN.GenActivePW","有功功率","active_power","f_盂县三期Ⅴ-061 发电机有功功率","yc_hs_0349","cur_86"]
[4499,"f_盂县三期Ⅴ-061 主轴(风轮)转速","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县三期Ⅴ-061 主轴(风轮)转速","yc_hs_0349","cur_88"]
[4500,"f_盂县三期Ⅴ-061 1#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县三期Ⅴ-061 1#桨叶片角度(桨距角)","yc_hs_0349","cur_90"]
[4501,"f_盂县三期Ⅴ-061 2#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县三期Ⅴ-061 2#桨叶片角度(桨距角)","yc_hs_0349","cur_91"]
[4502,"f_盂县三期Ⅴ-061 3#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县三期Ⅴ-061 3#桨叶片角度(桨距角)","yc_hs_0349","cur_92"]
[4503,"f_盂县三期Ⅴ-061 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县三期Ⅴ-061 齿轮箱高速轴非驱动端轴承温度","yc_hs_0349","cur_94"]
[4504,"f_盂县三期Ⅴ-061 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县三期Ⅴ-061 发电机驱动端轴承温度","yc_hs_0349","cur_95"]
[4505,"f_盂县三期Ⅴ-061 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县三期Ⅴ-061 发电机非驱动端轴承温度","yc_hs_0349","cur_96"]
[4506,"f_盂县三期Ⅴ-061 齿轮箱油池温度","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县三期Ⅴ-061 齿轮箱油池温度","yc_hs_0349","cur_97"]
[4507,"f_盂县三期Ⅴ-061 发电机转速","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WGEN.GenSpd","发电机转速","generator_speed","f_盂县三期Ⅴ-061 发电机转速","yc_hs_0349","cur_100"]
[4508,"f_盂县三期Ⅴ-061 发电机绕组温度1","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","f_盂县三期Ⅴ-061 发电机绕组温度1","yc_hs_0350","cur_01"]
[4509,"f_盂县三期Ⅴ-061 发电机绕组温度2","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","f_盂县三期Ⅴ-061 发电机绕组温度2","yc_hs_0350","cur_02"]
[4510,"f_盂县三期Ⅴ-061 发电机绕组温度3","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","f_盂县三期Ⅴ-061 发电机绕组温度3","yc_hs_0350","cur_03"]
[4511,"f_盂县三期Ⅴ-061 机舱角度（位置）","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县三期Ⅴ-061 机舱角度（位置）","yc_hs_0350","cur_18"]
[4512,"f_盂县三期Ⅴ-061 风速","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WNAC.WindSpeed","风速","wind_velocity","f_盂县三期Ⅴ-061 风速","yc_hs_0350","cur_19"]
[4513,"f_盂县三期Ⅴ-061 风向","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县三期Ⅴ-061 风向","yc_hs_0350","cur_20"]
[4514,"f_盂县三期Ⅴ-061 瞬时风向","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WNAC.WindDirectionInstant","对风角度","yaw_error1","f_盂县三期Ⅴ-061 瞬时风向","yc_hs_0350","cur_21"]
[4515,"f_盂县三期Ⅴ-061 舱外温度","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县三期Ⅴ-061 舱外温度","yc_hs_0350","cur_22"]
[4516,"f_盂县三期Ⅴ-061 舱内温度","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县三期Ⅴ-061 舱内温度","yc_hs_0350","cur_23"]
[4517,"f_盂县三期Ⅴ-061 机舱侧向振动值(已滤波)","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县三期Ⅴ-061 机舱侧向振动值(已滤波)","yc_hs_0350","cur_25"]
[4518,"f_盂县三期Ⅴ-061 机舱轴向振动值(已滤波)","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县三期Ⅴ-061 机舱轴向振动值(已滤波)","yc_hs_0350","cur_26"]
[4519,"f_盂县三期Ⅴ-061 扭揽角度","盂县风光互补电站","WOF35800082",61,"SXYX.T3_L5.WTG061.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县三期Ⅴ-061 扭揽角度","yc_hs_0350","cur_28"]
[4520,"f_盂县三期Ⅴ-062 发电机有功功率","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WGEN.GenActivePW","有功功率","active_power","f_盂县三期Ⅴ-062 发电机有功功率","yc_hs_0350","cur_33"]
[4521,"f_盂县三期Ⅴ-062 主轴(风轮)转速","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县三期Ⅴ-062 主轴(风轮)转速","yc_hs_0350","cur_35"]
[4522,"f_盂县三期Ⅴ-062 1#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县三期Ⅴ-062 1#桨叶片角度(桨距角)","yc_hs_0350","cur_37"]
[4523,"f_盂县三期Ⅴ-062 2#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县三期Ⅴ-062 2#桨叶片角度(桨距角)","yc_hs_0350","cur_38"]
[4524,"f_盂县三期Ⅴ-062 3#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县三期Ⅴ-062 3#桨叶片角度(桨距角)","yc_hs_0350","cur_39"]
[4525,"f_盂县三期Ⅴ-062 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县三期Ⅴ-062 齿轮箱高速轴非驱动端轴承温度","yc_hs_0350","cur_41"]
[4526,"f_盂县三期Ⅴ-062 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县三期Ⅴ-062 发电机驱动端轴承温度","yc_hs_0350","cur_42"]
[4527,"f_盂县三期Ⅴ-062 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县三期Ⅴ-062 发电机非驱动端轴承温度","yc_hs_0350","cur_43"]
[4528,"f_盂县三期Ⅴ-062 齿轮箱油池温度","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县三期Ⅴ-062 齿轮箱油池温度","yc_hs_0350","cur_44"]
[4529,"f_盂县三期Ⅴ-062 发电机转速","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WGEN.GenSpd","发电机转速","generator_speed","f_盂县三期Ⅴ-062 发电机转速","yc_hs_0350","cur_47"]
[4530,"f_盂县三期Ⅴ-062 发电机绕组温度1","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","f_盂县三期Ⅴ-062 发电机绕组温度1","yc_hs_0350","cur_48"]
[4531,"f_盂县三期Ⅴ-062 发电机绕组温度2","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","f_盂县三期Ⅴ-062 发电机绕组温度2","yc_hs_0350","cur_49"]
[4532,"f_盂县三期Ⅴ-062 发电机绕组温度3","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","f_盂县三期Ⅴ-062 发电机绕组温度3","yc_hs_0350","cur_50"]
[4533,"f_盂县三期Ⅴ-062 机舱角度（位置）","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县三期Ⅴ-062 机舱角度（位置）","yc_hs_0350","cur_65"]
[4534,"f_盂县三期Ⅴ-062 风速","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WNAC.WindSpeed","风速","wind_velocity","f_盂县三期Ⅴ-062 风速","yc_hs_0350","cur_66"]
[4535,"f_盂县三期Ⅴ-062 风向","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县三期Ⅴ-062 风向","yc_hs_0350","cur_67"]
[4536,"f_盂县三期Ⅴ-062 瞬时风向","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WNAC.WindDirectionInstant","对风角度","yaw_error1","f_盂县三期Ⅴ-062 瞬时风向","yc_hs_0350","cur_68"]
[4537,"f_盂县三期Ⅴ-062 舱外温度","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县三期Ⅴ-062 舱外温度","yc_hs_0350","cur_69"]
[4538,"f_盂县三期Ⅴ-062 舱内温度","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县三期Ⅴ-062 舱内温度","yc_hs_0350","cur_70"]
[4539,"f_盂县三期Ⅴ-062 机舱侧向振动值(已滤波)","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县三期Ⅴ-062 机舱侧向振动值(已滤波)","yc_hs_0350","cur_72"]
[4540,"f_盂县三期Ⅴ-062 机舱轴向振动值(已滤波)","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县三期Ⅴ-062 机舱轴向振动值(已滤波)","yc_hs_0350","cur_73"]
[4541,"f_盂县三期Ⅴ-062 扭揽角度","盂县风光互补电站","WOF35800082",62,"SXYX.T3_L5.WTG062.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县三期Ⅴ-062 扭揽角度","yc_hs_0350","cur_75"]
[4542,"f_盂县三期Ⅴ-063 发电机有功功率","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WGEN.GenActivePW","有功功率","active_power","f_盂县三期Ⅴ-063 发电机有功功率","yc_hs_0351","cur_16"]
[4543,"f_盂县三期Ⅴ-063 主轴(风轮)转速","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县三期Ⅴ-063 主轴(风轮)转速","yc_hs_0351","cur_18"]
[4544,"f_盂县三期Ⅴ-063 1#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县三期Ⅴ-063 1#桨叶片角度(桨距角)","yc_hs_0351","cur_20"]
[4545,"f_盂县三期Ⅴ-063 2#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县三期Ⅴ-063 2#桨叶片角度(桨距角)","yc_hs_0351","cur_21"]
[4546,"f_盂县三期Ⅴ-063 3#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县三期Ⅴ-063 3#桨叶片角度(桨距角)","yc_hs_0351","cur_22"]
[4547,"f_盂县三期Ⅴ-063 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县三期Ⅴ-063 齿轮箱高速轴非驱动端轴承温度","yc_hs_0351","cur_24"]
[4548,"f_盂县三期Ⅴ-063 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县三期Ⅴ-063 发电机驱动端轴承温度","yc_hs_0351","cur_25"]
[4549,"f_盂县三期Ⅴ-063 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县三期Ⅴ-063 发电机非驱动端轴承温度","yc_hs_0350","cur_79"]
[4550,"f_盂县三期Ⅴ-063 齿轮箱油池温度","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县三期Ⅴ-063 齿轮箱油池温度","yc_hs_0350","cur_80"]
[4551,"f_盂县三期Ⅴ-063 发电机转速","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WGEN.GenSpd","发电机转速","generator_speed","f_盂县三期Ⅴ-063 发电机转速","yc_hs_0350","cur_83"]
[4552,"f_盂县三期Ⅴ-063 发电机绕组温度1","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","f_盂县三期Ⅴ-063 发电机绕组温度1","yc_hs_0350","cur_84"]
[4553,"f_盂县三期Ⅴ-063 发电机绕组温度2","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","f_盂县三期Ⅴ-063 发电机绕组温度2","yc_hs_0350","cur_85"]
[4554,"f_盂县三期Ⅴ-063 发电机绕组温度3","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","f_盂县三期Ⅴ-063 发电机绕组温度3","yc_hs_0350","cur_86"]
[4555,"f_盂县三期Ⅴ-063 机舱角度（位置）","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县三期Ⅴ-063 机舱角度（位置）","yc_hs_0351","cur_01"]
[4556,"f_盂县三期Ⅴ-063 风速","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WNAC.WindSpeed","风速","wind_velocity","f_盂县三期Ⅴ-063 风速","yc_hs_0351","cur_02"]
[4557,"f_盂县三期Ⅴ-063 风向","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县三期Ⅴ-063 风向","yc_hs_0351","cur_03"]
[4558,"f_盂县三期Ⅴ-063 瞬时风向","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WNAC.WindDirectionInstant","对风角度","yaw_error1","f_盂县三期Ⅴ-063 瞬时风向","yc_hs_0351","cur_04"]
[4559,"f_盂县三期Ⅴ-063 舱外温度","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县三期Ⅴ-063 舱外温度","yc_hs_0351","cur_05"]
[4560,"f_盂县三期Ⅴ-063 舱内温度","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县三期Ⅴ-063 舱内温度","yc_hs_0351","cur_06"]
[4561,"f_盂县三期Ⅴ-063 机舱侧向振动值(已滤波)","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县三期Ⅴ-063 机舱侧向振动值(已滤波)","yc_hs_0351","cur_08"]
[4562,"f_盂县三期Ⅴ-063 机舱轴向振动值(已滤波)","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县三期Ⅴ-063 机舱轴向振动值(已滤波)","yc_hs_0351","cur_09"]
[4563,"f_盂县三期Ⅴ-063 扭揽角度","盂县风光互补电站","WOF35800082",63,"SXYX.T3_L5.WTG063.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县三期Ⅴ-063 扭揽角度","yc_hs_0351","cur_11"]
[4564,"f_盂县三期Ⅴ-064 发电机有功功率","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WGEN.GenActivePW","有功功率","active_power","f_盂县三期Ⅴ-064 发电机有功功率","yc_hs_0351","cur_41"]
[4565,"f_盂县三期Ⅴ-064 主轴(风轮)转速","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县三期Ⅴ-064 主轴(风轮)转速","yc_hs_0351","cur_43"]
[4566,"f_盂县三期Ⅴ-064 1#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县三期Ⅴ-064 1#桨叶片角度(桨距角)","yc_hs_0351","cur_45"]
[4567,"f_盂县三期Ⅴ-064 2#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县三期Ⅴ-064 2#桨叶片角度(桨距角)","yc_hs_0351","cur_46"]
[4568,"f_盂县三期Ⅴ-064 3#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县三期Ⅴ-064 3#桨叶片角度(桨距角)","yc_hs_0351","cur_47"]
[4569,"f_盂县三期Ⅴ-064 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县三期Ⅴ-064 齿轮箱高速轴非驱动端轴承温度","yc_hs_0351","cur_49"]
[4570,"f_盂县三期Ⅴ-064 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县三期Ⅴ-064 发电机驱动端轴承温度","yc_hs_0351","cur_50"]
[4571,"f_盂县三期Ⅴ-064 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县三期Ⅴ-064 发电机非驱动端轴承温度","yc_hs_0351","cur_51"]
[4572,"f_盂县三期Ⅴ-064 齿轮箱油池温度","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县三期Ⅴ-064 齿轮箱油池温度","yc_hs_0351","cur_52"]
[4573,"f_盂县三期Ⅴ-064 发电机转速","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WGEN.GenSpd","发电机转速","generator_speed","f_盂县三期Ⅴ-064 发电机转速","yc_hs_0351","cur_55"]
[4574,"f_盂县三期Ⅴ-064 发电机绕组温度1","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","f_盂县三期Ⅴ-064 发电机绕组温度1","yc_hs_0351","cur_56"]
[4575,"f_盂县三期Ⅴ-064 发电机绕组温度2","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","f_盂县三期Ⅴ-064 发电机绕组温度2","yc_hs_0351","cur_57"]
[4576,"f_盂县三期Ⅴ-064 发电机绕组温度3","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","f_盂县三期Ⅴ-064 发电机绕组温度3","yc_hs_0351","cur_58"]
[4577,"f_盂县三期Ⅴ-064 机舱角度（位置）","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县三期Ⅴ-064 机舱角度（位置）","yc_hs_0351","cur_26"]
[4578,"f_盂县三期Ⅴ-064 风速","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WNAC.WindSpeed","风速","wind_velocity","f_盂县三期Ⅴ-064 风速","yc_hs_0351","cur_27"]
[4579,"f_盂县三期Ⅴ-064 风向","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县三期Ⅴ-064 风向","yc_hs_0351","cur_28"]
[4580,"f_盂县三期Ⅴ-064 瞬时风向","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WNAC.WindDirectionInstant","对风角度","yaw_error1","f_盂县三期Ⅴ-064 瞬时风向","yc_hs_0351","cur_29"]
[4581,"f_盂县三期Ⅴ-064 舱外温度","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县三期Ⅴ-064 舱外温度","yc_hs_0351","cur_30"]
[4582,"f_盂县三期Ⅴ-064 舱内温度","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县三期Ⅴ-064 舱内温度","yc_hs_0351","cur_31"]
[4583,"f_盂县三期Ⅴ-064 机舱侧向振动值(已滤波)","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县三期Ⅴ-064 机舱侧向振动值(已滤波)","yc_hs_0351","cur_33"]
[4584,"f_盂县三期Ⅴ-064 机舱轴向振动值(已滤波)","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县三期Ⅴ-064 机舱轴向振动值(已滤波)","yc_hs_0351","cur_34"]
[4585,"f_盂县三期Ⅴ-064 扭揽角度","盂县风光互补电站","WOF35800082",64,"SXYX.T3_L5.WTG064.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县三期Ⅴ-064 扭揽角度","yc_hs_0351","cur_36"]
[4586,"f_盂县三期Ⅴ-065 发电机有功功率","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WGEN.GenActivePW","有功功率","active_power","f_盂县三期Ⅴ-065 发电机有功功率","yc_hs_0351","cur_74"]
[4587,"f_盂县三期Ⅴ-065 主轴(风轮)转速","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县三期Ⅴ-065 主轴(风轮)转速","yc_hs_0351","cur_76"]
[4588,"f_盂县三期Ⅴ-065 1#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县三期Ⅴ-065 1#桨叶片角度(桨距角)","yc_hs_0351","cur_78"]
[4589,"f_盂县三期Ⅴ-065 2#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县三期Ⅴ-065 2#桨叶片角度(桨距角)","yc_hs_0351","cur_79"]
[4590,"f_盂县三期Ⅴ-065 3#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县三期Ⅴ-065 3#桨叶片角度(桨距角)","yc_hs_0351","cur_80"]
[4591,"f_盂县三期Ⅴ-065 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县三期Ⅴ-065 齿轮箱高速轴非驱动端轴承温度","yc_hs_0351","cur_82"]
[4592,"f_盂县三期Ⅴ-065 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县三期Ⅴ-065 发电机驱动端轴承温度","yc_hs_0351","cur_83"]
[4593,"f_盂县三期Ⅴ-065 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县三期Ⅴ-065 发电机非驱动端轴承温度","yc_hs_0351","cur_84"]
[4594,"f_盂县三期Ⅴ-065 齿轮箱油池温度","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县三期Ⅴ-065 齿轮箱油池温度","yc_hs_0351","cur_85"]
[4595,"f_盂县三期Ⅴ-065 发电机转速","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WGEN.GenSpd","发电机转速","generator_speed","f_盂县三期Ⅴ-065 发电机转速","yc_hs_0351","cur_88"]
[4596,"f_盂县三期Ⅴ-065 发电机绕组温度1","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","f_盂县三期Ⅴ-065 发电机绕组温度1","yc_hs_0351","cur_89"]
[4597,"f_盂县三期Ⅴ-065 发电机绕组温度2","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","f_盂县三期Ⅴ-065 发电机绕组温度2","yc_hs_0351","cur_90"]
[4598,"f_盂县三期Ⅴ-065 发电机绕组温度3","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","f_盂县三期Ⅴ-065 发电机绕组温度3","yc_hs_0351","cur_91"]
[4599,"f_盂县三期Ⅴ-065 机舱角度（位置）","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县三期Ⅴ-065 机舱角度（位置）","yc_hs_0352","cur_06"]
[4600,"f_盂县三期Ⅴ-065 风速","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WNAC.WindSpeed","风速","wind_velocity","f_盂县三期Ⅴ-065 风速","yc_hs_0352","cur_07"]
[4601,"f_盂县三期Ⅴ-065 风向","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县三期Ⅴ-065 风向","yc_hs_0352","cur_08"]
[4602,"f_盂县三期Ⅴ-065 瞬时风向","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WNAC.WindDirectionInstant","对风角度","yaw_error1","f_盂县三期Ⅴ-065 瞬时风向","yc_hs_0352","cur_09"]
[4603,"f_盂县三期Ⅴ-065 舱外温度","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县三期Ⅴ-065 舱外温度","yc_hs_0352","cur_10"]
[4604,"f_盂县三期Ⅴ-065 舱内温度","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县三期Ⅴ-065 舱内温度","yc_hs_0352","cur_11"]
[4605,"f_盂县三期Ⅴ-065 机舱侧向振动值(已滤波)","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县三期Ⅴ-065 机舱侧向振动值(已滤波)","yc_hs_0352","cur_13"]
[4606,"f_盂县三期Ⅴ-065 机舱轴向振动值(已滤波)","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县三期Ⅴ-065 机舱轴向振动值(已滤波)","yc_hs_0352","cur_14"]
[4607,"f_盂县三期Ⅴ-065 扭揽角度","盂县风光互补电站","WOF35800082",65,"SXYX.T3_L5.WTG065.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县三期Ⅴ-065 扭揽角度","yc_hs_0352","cur_16"]
[4608,"f_盂县三期Ⅴ-066 机舱轴向振动值(已滤波)","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","f_盂县三期Ⅴ-066 机舱轴向振动值(已滤波)","yc_hs_0352","cur_43"]
[4609,"f_盂县三期Ⅴ-066 扭揽角度","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","f_盂县三期Ⅴ-066 扭揽角度","yc_hs_0352","cur_45"]
[4610,"f_盂县三期Ⅴ-066 发电机有功功率","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WGEN.GenActivePW","有功功率","active_power","f_盂县三期Ⅴ-066 发电机有功功率","yc_hs_0352","cur_50"]
[4611,"f_盂县三期Ⅴ-066 主轴(风轮)转速","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WTRM.RotorSpd","风轮转速","rotor_speed","f_盂县三期Ⅴ-066 主轴(风轮)转速","yc_hs_0352","cur_52"]
[4612,"f_盂县三期Ⅴ-066 1#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","f_盂县三期Ⅴ-066 1#桨叶片角度(桨距角)","yc_hs_0352","cur_54"]
[4613,"f_盂县三期Ⅴ-066 2#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","f_盂县三期Ⅴ-066 2#桨叶片角度(桨距角)","yc_hs_0352","cur_55"]
[4614,"f_盂县三期Ⅴ-066 3#桨叶片角度(桨距角)","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","f_盂县三期Ⅴ-066 3#桨叶片角度(桨距角)","yc_hs_0352","cur_56"]
[4615,"f_盂县三期Ⅴ-066 齿轮箱高速轴非驱动端轴承温度","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","f_盂县三期Ⅴ-066 齿轮箱高速轴非驱动端轴承温度","yc_hs_0352","cur_58"]
[4616,"f_盂县三期Ⅴ-066 发电机驱动端轴承温度","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","f_盂县三期Ⅴ-066 发电机驱动端轴承温度","yc_hs_0352","cur_59"]
[4617,"f_盂县三期Ⅴ-066 发电机非驱动端轴承温度","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","f_盂县三期Ⅴ-066 发电机非驱动端轴承温度","yc_hs_0352","cur_60"]
[4618,"f_盂县三期Ⅴ-066 齿轮箱油池温度","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","f_盂县三期Ⅴ-066 齿轮箱油池温度","yc_hs_0352","cur_61"]
[4619,"f_盂县三期Ⅴ-066 发电机转速","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WGEN.GenSpd","发电机转速","generator_speed","f_盂县三期Ⅴ-066 发电机转速","yc_hs_0352","cur_64"]
[4620,"f_盂县三期Ⅴ-066 发电机绕组温度1","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","f_盂县三期Ⅴ-066 发电机绕组温度1","yc_hs_0352","cur_65"]
[4621,"f_盂县三期Ⅴ-066 发电机绕组温度2","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","f_盂县三期Ⅴ-066 发电机绕组温度2","yc_hs_0352","cur_66"]
[4622,"f_盂县三期Ⅴ-066 发电机绕组温度3","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","f_盂县三期Ⅴ-066 发电机绕组温度3","yc_hs_0352","cur_20"]
[4623,"f_盂县三期Ⅴ-066 机舱角度（位置）","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WYAW.NacellePosition","机舱位置","cabin_position","f_盂县三期Ⅴ-066 机舱角度（位置）","yc_hs_0352","cur_35"]
[4624,"f_盂县三期Ⅴ-066 风速","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WNAC.WindSpeed","风速","wind_velocity","f_盂县三期Ⅴ-066 风速","yc_hs_0352","cur_36"]
[4625,"f_盂县三期Ⅴ-066 风向","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WNAC.WindDirection","绝对风向","true_wind_direction","f_盂县三期Ⅴ-066 风向","yc_hs_0352","cur_37"]
[4626,"f_盂县三期Ⅴ-066 瞬时风向","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WNAC.WindDirectionInstant","对风角度","yaw_error1","f_盂县三期Ⅴ-066 瞬时风向","yc_hs_0352","cur_38"]
[4627,"f_盂县三期Ⅴ-066 舱外温度","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WNAC.TemOut","环境温度","outside_cabin_temperature","f_盂县三期Ⅴ-066 舱外温度","yc_hs_0352","cur_39"]
[4628,"f_盂县三期Ⅴ-066 舱内温度","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WNAC.TemNacelle","机舱内温度","cabin_temperature","f_盂县三期Ⅴ-066 舱内温度","yc_hs_0352","cur_40"]
[4629,"f_盂县三期Ⅴ-066 机舱侧向振动值(已滤波)","盂县风光互补电站","WOF35800082",66,"SXYX.T3_L5.WTG066.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","f_盂县三期Ⅴ-066 机舱侧向振动值(已滤波)","yc_hs_0352","cur_42"]
[4630,"d_古交一期Ⅰ-006 机舱与风向夹角","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅰ-006 机舱与风向夹角","yc_hs_0358","cur_05"]
[4631,"d_古交一期Ⅰ-006 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅰ-006 1#桨叶片角度(桨距角)","yc_hs_0358","cur_06"]
[4632,"d_古交一期Ⅰ-006 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅰ-006 2#桨叶片角度(桨距角)","yc_hs_0358","cur_07"]
[4633,"d_古交一期Ⅰ-006 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅰ-006 3#桨叶片角度(桨距角)","yc_hs_0358","cur_08"]
[4634,"d_古交一期Ⅰ-006 主轴转速","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅰ-006 主轴转速","yc_hs_0358","cur_15"]
[4635,"d_古交一期Ⅰ-006 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅰ-006 齿轮箱高速轴非驱动端轴承温度","yc_hs_0358","cur_17"]
[4636,"d_古交一期Ⅰ-006 齿轮箱油池温度","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅰ-006 齿轮箱油池温度","yc_hs_0358","cur_18"]
[4637,"d_古交一期Ⅰ-006 主轴承外圈温度","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅰ-006 主轴承外圈温度","yc_hs_0358","cur_19"]
[4638,"d_古交一期Ⅱ-012 发电机转速","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅱ-012 发电机转速","yc_hs_0358","cur_23"]
[4639,"d_古交一期Ⅱ-012 发电机驱动端轴承温度","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅱ-012 发电机驱动端轴承温度","yc_hs_0358","cur_24"]
[4640,"d_古交一期Ⅱ-012 发电机非驱动端轴承温度","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅱ-012 发电机非驱动端轴承温度","yc_hs_0358","cur_25"]
[4641,"d_古交一期Ⅱ-012 发电机定子U相线圈温度","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅱ-012 发电机定子U相线圈温度","yc_hs_0358","cur_26"]
[4642,"d_古交一期Ⅱ-012 发电机定子V相线圈温度","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅱ-012 发电机定子V相线圈温度","yc_hs_0358","cur_27"]
[4643,"d_古交一期Ⅱ-012 发电机定子W相线圈温度","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅱ-012 发电机定子W相线圈温度","yc_hs_0358","cur_28"]
[4644,"d_古交一期Ⅱ-012 舱内温度","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅱ-012 舱内温度","yc_hs_0358","cur_40"]
[4645,"d_古交一期Ⅱ-012 舱外温度","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅱ-012 舱外温度","yc_hs_0358","cur_41"]
[4646,"d_古交一期Ⅱ-012 风向","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅱ-012 风向","yc_hs_0358","cur_42"]
[4647,"d_古交一期Ⅱ-012 机舱角度（位置）","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅱ-012 机舱角度（位置）","yc_hs_0358","cur_44"]
[4648,"d_古交一期Ⅱ-012 偏航角度(扭缆角度）","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅱ-012 偏航角度(扭缆角度）","yc_hs_0358","cur_45"]
[4649,"d_古交一期Ⅱ-012 机舱与风向夹角","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅱ-012 机舱与风向夹角","yc_hs_0358","cur_46"]
[4650,"d_古交一期Ⅱ-012 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅱ-012 1#桨叶片角度(桨距角)","yc_hs_0358","cur_47"]
[4651,"d_古交一期Ⅱ-010 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅱ-010 机舱侧向振动值(已滤波)","yc_hs_0479","cur_75"]
[4652,"d_古交一期Ⅱ-010 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅱ-010 机舱轴向振动值(已滤波)","yc_hs_0479","cur_77"]
[4653,"d_古交一期Ⅱ-010 风速","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅱ-010 风速","yc_hs_0479","cur_78"]
[4654,"d_古交一期Ⅱ-010 发电机有功功率","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅱ-010 发电机有功功率","yc_hs_0479","cur_79"]
[4655,"d_古交一期Ⅱ-010 发电机转速","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅱ-010 发电机转速","yc_hs_0479","cur_81"]
[4656,"d_古交一期Ⅱ-010 发电机驱动端轴承温度","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅱ-010 发电机驱动端轴承温度","yc_hs_0479","cur_82"]
[4657,"d_古交一期Ⅱ-010 发电机非驱动端轴承温度","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅱ-010 发电机非驱动端轴承温度","yc_hs_0479","cur_83"]
[4658,"d_古交一期Ⅱ-010 发电机定子U相线圈温度","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅱ-010 发电机定子U相线圈温度","yc_hs_0479","cur_84"]
[4659,"d_古交一期Ⅱ-010 发电机定子V相线圈温度","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅱ-010 发电机定子V相线圈温度","yc_hs_0479","cur_85"]
[4660,"d_古交一期Ⅱ-010 发电机定子W相线圈温度","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅱ-010 发电机定子W相线圈温度","yc_hs_0479","cur_86"]
[4661,"d_古交一期Ⅱ-015 主轴转速","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅱ-015 主轴转速","yc_hs_0479","cur_89"]
[4662,"d_古交一期Ⅱ-015 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅱ-015 齿轮箱高速轴非驱动端轴承温度","yc_hs_0480","cur_75"]
[4663,"d_古交一期Ⅱ-015 齿轮箱油池温度","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅱ-015 齿轮箱油池温度","yc_hs_0480","cur_76"]
[4664,"d_古交一期Ⅱ-015 主轴承外圈温度","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅱ-015 主轴承外圈温度","yc_hs_0480","cur_77"]
[4665,"d_古交一期Ⅲ-021 舱内温度","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅲ-021 舱内温度","yc_hs_0480","cur_84"]
[4666,"d_古交一期Ⅲ-021 舱外温度","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅲ-021 舱外温度","yc_hs_0480","cur_85"]
[4667,"d_古交一期Ⅲ-021 风向","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅲ-021 风向","yc_hs_0480","cur_86"]
[4668,"d_古交一期Ⅲ-021 机舱角度（位置）","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅲ-021 机舱角度（位置）","yc_hs_0480","cur_88"]
[4669,"d_古交一期Ⅲ-021 偏航角度(扭缆角度）","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅲ-021 偏航角度(扭缆角度）","yc_hs_0480","cur_89"]
[4670,"d_古交一期Ⅲ-021 机舱与风向夹角","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅲ-021 机舱与风向夹角","yc_hs_0480","cur_90"]
[4671,"d_古交一期Ⅲ-021 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅲ-021 1#桨叶片角度(桨距角)","yc_hs_0480","cur_91"]
[4672,"d_古交一期Ⅲ-021 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅲ-021 2#桨叶片角度(桨距角)","yc_hs_0480","cur_92"]
[4673,"d_古交一期Ⅲ-021 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅲ-021 3#桨叶片角度(桨距角)","yc_hs_0480","cur_93"]
[4674,"d_古交一期Ⅲ-021 主轴转速","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅲ-021 主轴转速","yc_hs_0480","cur_100"]
[4675,"d_古交一期Ⅲ-021 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅲ-021 齿轮箱高速轴非驱动端轴承温度","yc_hs_0481","cur_02"]
[4676,"d_古交一期Ⅲ-021 齿轮箱油池温度","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅲ-021 齿轮箱油池温度","yc_hs_0481","cur_03"]
[4677,"d_古交一期Ⅲ-021 主轴承外圈温度","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅲ-021 主轴承外圈温度","yc_hs_0481","cur_04"]
[4678,"d_古交一期Ⅱ-012 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅱ-012 2#桨叶片角度(桨距角)","yc_hs_0482","cur_03"]
[4679,"d_古交一期Ⅱ-012 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅱ-012 3#桨叶片角度(桨距角)","yc_hs_0482","cur_04"]
[4680,"d_古交一期Ⅲ-018 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅲ-018 机舱侧向振动值(已滤波)","yc_hs_0482","cur_14"]
[4681,"d_古交一期Ⅲ-018 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅲ-018 机舱轴向振动值(已滤波)","yc_hs_0482","cur_16"]
[4682,"d_古交一期Ⅲ-018 风速","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅲ-018 风速","yc_hs_0482","cur_17"]
[4683,"d_古交一期Ⅲ-018 发电机有功功率","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅲ-018 发电机有功功率","yc_hs_0482","cur_18"]
[4684,"d_古交一期Ⅲ-018 发电机转速","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅲ-018 发电机转速","yc_hs_0482","cur_20"]
[4685,"d_古交一期Ⅲ-018 发电机驱动端轴承温度","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅲ-018 发电机驱动端轴承温度","yc_hs_0482","cur_21"]
[4686,"d_古交一期Ⅲ-018 发电机非驱动端轴承温度","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅲ-018 发电机非驱动端轴承温度","yc_hs_0482","cur_22"]
[4687,"d_古交一期Ⅲ-018 发电机定子U相线圈温度","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅲ-018 发电机定子U相线圈温度","yc_hs_0482","cur_23"]
[4688,"d_古交一期Ⅲ-018 发电机定子V相线圈温度","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅲ-018 发电机定子V相线圈温度","yc_hs_0482","cur_24"]
[4689,"d_古交一期Ⅲ-018 发电机定子W相线圈温度","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅲ-018 发电机定子W相线圈温度","yc_hs_0482","cur_25"]
[4690,"d_古交一期Ⅲ-018 舱内温度","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅲ-018 舱内温度","yc_hs_0482","cur_37"]
[4691,"d_古交一期Ⅲ-018 舱外温度","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅲ-018 舱外温度","yc_hs_0482","cur_38"]
[4692,"d_古交一期Ⅲ-018 风向","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅲ-018 风向","yc_hs_0482","cur_39"]
[4693,"d_古交一期Ⅲ-018 机舱角度（位置）","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅲ-018 机舱角度（位置）","yc_hs_0482","cur_41"]
[4694,"d_古交一期Ⅲ-018 偏航角度(扭缆角度）","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅲ-018 偏航角度(扭缆角度）","yc_hs_0482","cur_42"]
[4695,"d_古交一期Ⅲ-018 机舱与风向夹角","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅲ-018 机舱与风向夹角","yc_hs_0482","cur_43"]
[4696,"d_古交一期Ⅲ-018 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅲ-018 1#桨叶片角度(桨距角)","yc_hs_0482","cur_44"]
[4697,"d_古交一期Ⅲ-024 主轴承外圈温度","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅲ-024 主轴承外圈温度","yc_hs_0482","cur_45"]
[4698,"d_古交一期Ⅱ-010 舱内温度","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅱ-010 舱内温度","yc_hs_0483","cur_33"]
[4699,"d_古交一期Ⅱ-010 舱外温度","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅱ-010 舱外温度","yc_hs_0483","cur_34"]
[4700,"d_古交一期Ⅱ-010 风向","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅱ-010 风向","yc_hs_0483","cur_35"]
[4701,"d_古交一期Ⅱ-010 机舱角度（位置）","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅱ-010 机舱角度（位置）","yc_hs_0483","cur_37"]
[4702,"d_古交一期Ⅱ-010 偏航角度(扭缆角度）","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅱ-010 偏航角度(扭缆角度）","yc_hs_0483","cur_38"]
[4703,"d_古交一期Ⅱ-010 机舱与风向夹角","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅱ-010 机舱与风向夹角","yc_hs_0483","cur_39"]
[4704,"d_古交一期Ⅱ-010 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅱ-010 1#桨叶片角度(桨距角)","yc_hs_0483","cur_40"]
[4705,"d_古交一期Ⅱ-010 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅱ-010 2#桨叶片角度(桨距角)","yc_hs_0483","cur_41"]
[4706,"d_古交一期Ⅱ-010 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅱ-010 3#桨叶片角度(桨距角)","yc_hs_0483","cur_42"]
[4707,"d_古交一期Ⅱ-010 主轴转速","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅱ-010 主轴转速","yc_hs_0483","cur_49"]
[4708,"d_古交一期Ⅱ-010 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅱ-010 齿轮箱高速轴非驱动端轴承温度","yc_hs_0483","cur_51"]
[4709,"d_古交一期Ⅱ-010 齿轮箱油池温度","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅱ-010 齿轮箱油池温度","yc_hs_0483","cur_52"]
[4710,"d_古交一期Ⅲ-016 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅲ-016 机舱侧向振动值(已滤波)","yc_hs_0483","cur_55"]
[4711,"d_古交一期Ⅲ-016 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅲ-016 机舱轴向振动值(已滤波)","yc_hs_0483","cur_57"]
[4712,"d_古交一期Ⅲ-016 风速","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅲ-016 风速","yc_hs_0483","cur_58"]
[4713,"d_古交一期Ⅲ-016 发电机有功功率","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅲ-016 发电机有功功率","yc_hs_0483","cur_59"]
[4714,"d_古交一期Ⅲ-016 发电机转速","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅲ-016 发电机转速","yc_hs_0483","cur_61"]
[4715,"d_古交一期Ⅲ-016 发电机驱动端轴承温度","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅲ-016 发电机驱动端轴承温度","yc_hs_0483","cur_62"]
[4716,"d_古交一期Ⅲ-016 发电机非驱动端轴承温度","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅲ-016 发电机非驱动端轴承温度","yc_hs_0483","cur_63"]
[4717,"d_古交一期Ⅲ-016 发电机定子U相线圈温度","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅲ-016 发电机定子U相线圈温度","yc_hs_0483","cur_64"]
[4718,"d_古交一期Ⅲ-016 发电机定子V相线圈温度","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅲ-016 发电机定子V相线圈温度","yc_hs_0483","cur_65"]
[4719,"d_古交一期Ⅲ-016 发电机定子W相线圈温度","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅲ-016 发电机定子W相线圈温度","yc_hs_0483","cur_66"]
[4720,"d_古交一期Ⅰ-002 舱内温度","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅰ-002 舱内温度","yc_hs_0485","cur_77"]
[4721,"d_古交一期Ⅰ-002 舱外温度","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅰ-002 舱外温度","yc_hs_0485","cur_78"]
[4722,"d_古交一期Ⅰ-002 风向","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅰ-002 风向","yc_hs_0485","cur_79"]
[4723,"d_古交一期Ⅰ-002 机舱角度（位置）","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅰ-002 机舱角度（位置）","yc_hs_0485","cur_81"]
[4724,"d_古交一期Ⅰ-002 偏航角度(扭缆角度）","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅰ-002 偏航角度(扭缆角度）","yc_hs_0485","cur_82"]
[4725,"d_古交一期Ⅰ-002 机舱与风向夹角","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅰ-002 机舱与风向夹角","yc_hs_0485","cur_83"]
[4726,"d_古交一期Ⅰ-002 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅰ-002 1#桨叶片角度(桨距角)","yc_hs_0485","cur_84"]
[4727,"d_古交一期Ⅰ-002 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅰ-002 2#桨叶片角度(桨距角)","yc_hs_0485","cur_85"]
[4728,"d_古交一期Ⅰ-002 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅰ-002 3#桨叶片角度(桨距角)","yc_hs_0485","cur_86"]
[4729,"d_古交一期Ⅰ-002 主轴转速","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅰ-002 主轴转速","yc_hs_0485","cur_93"]
[4730,"d_古交一期Ⅰ-002 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅰ-002 齿轮箱高速轴非驱动端轴承温度","yc_hs_0485","cur_95"]
[4731,"d_古交一期Ⅰ-003 主轴转速","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅰ-003 主轴转速","yc_hs_0486","cur_01"]
[4732,"d_古交一期Ⅰ-003 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅰ-003 齿轮箱高速轴非驱动端轴承温度","yc_hs_0486","cur_03"]
[4733,"d_古交一期Ⅰ-003 齿轮箱油池温度","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅰ-003 齿轮箱油池温度","yc_hs_0486","cur_04"]
[4734,"d_古交一期Ⅰ-003 主轴承外圈温度","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅰ-003 主轴承外圈温度","yc_hs_0486","cur_05"]
[4735,"d_古交一期Ⅰ-001 发电机定子W相线圈温度","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅰ-001 发电机定子W相线圈温度","yc_hs_0486","cur_09"]
[4736,"d_古交一期Ⅲ-016 舱内温度","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅲ-016 舱内温度","yc_hs_0488","cur_47"]
[4737,"d_古交一期Ⅲ-016 舱外温度","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅲ-016 舱外温度","yc_hs_0488","cur_48"]
[4738,"d_古交一期Ⅲ-016 风向","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅲ-016 风向","yc_hs_0488","cur_49"]
[4739,"d_古交一期Ⅲ-016 机舱角度（位置）","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅲ-016 机舱角度（位置）","yc_hs_0488","cur_51"]
[4740,"d_古交一期Ⅲ-016 偏航角度(扭缆角度）","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅲ-016 偏航角度(扭缆角度）","yc_hs_0488","cur_52"]
[4741,"d_古交一期Ⅲ-016 机舱与风向夹角","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅲ-016 机舱与风向夹角","yc_hs_0488","cur_53"]
[4742,"d_古交一期Ⅲ-016 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅲ-016 1#桨叶片角度(桨距角)","yc_hs_0488","cur_54"]
[4743,"d_古交一期Ⅲ-016 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅲ-016 2#桨叶片角度(桨距角)","yc_hs_0488","cur_55"]
[4744,"d_古交一期Ⅲ-016 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅲ-016 3#桨叶片角度(桨距角)","yc_hs_0488","cur_56"]
[4745,"d_古交一期Ⅲ-022 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅲ-022 机舱侧向振动值(已滤波)","yc_hs_0488","cur_67"]
[4746,"d_古交一期Ⅲ-022 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅲ-022 机舱轴向振动值(已滤波)","yc_hs_0488","cur_69"]
[4747,"d_古交一期Ⅲ-022 风速","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅲ-022 风速","yc_hs_0488","cur_70"]
[4748,"d_古交一期Ⅲ-022 发电机有功功率","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅲ-022 发电机有功功率","yc_hs_0488","cur_71"]
[4749,"d_古交一期Ⅲ-022 发电机转速","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅲ-022 发电机转速","yc_hs_0488","cur_73"]
[4750,"d_古交一期Ⅲ-022 发电机驱动端轴承温度","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅲ-022 发电机驱动端轴承温度","yc_hs_0488","cur_74"]
[4751,"d_古交一期Ⅲ-022 发电机非驱动端轴承温度","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅲ-022 发电机非驱动端轴承温度","yc_hs_0488","cur_75"]
[4752,"d_古交一期Ⅲ-022 发电机定子U相线圈温度","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅲ-022 发电机定子U相线圈温度","yc_hs_0488","cur_76"]
[4753,"d_古交一期Ⅲ-022 发电机定子V相线圈温度","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅲ-022 发电机定子V相线圈温度","yc_hs_0488","cur_77"]
[4754,"d_古交一期Ⅲ-022 发电机定子W相线圈温度","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅲ-022 发电机定子W相线圈温度","yc_hs_0488","cur_78"]
[4755,"d_古交一期Ⅰ-007 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅰ-007 机舱侧向振动值(已滤波)","yc_hs_0488","cur_92"]
[4756,"d_古交一期Ⅰ-007 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅰ-007 机舱轴向振动值(已滤波)","yc_hs_0488","cur_94"]
[4757,"d_古交一期Ⅰ-007 风速","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅰ-007 风速","yc_hs_0488","cur_95"]
[4758,"d_古交一期Ⅰ-007 发电机有功功率","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅰ-007 发电机有功功率","yc_hs_0488","cur_96"]
[4759,"d_古交一期Ⅰ-007 发电机转速","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅰ-007 发电机转速","yc_hs_0488","cur_98"]
[4760,"d_古交一期Ⅰ-007 发电机驱动端轴承温度","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅰ-007 发电机驱动端轴承温度","yc_hs_0488","cur_99"]
[4761,"d_古交一期Ⅰ-007 发电机非驱动端轴承温度","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅰ-007 发电机非驱动端轴承温度","yc_hs_0488","cur_100"]
[4762,"d_古交一期Ⅰ-007 发电机定子U相线圈温度","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅰ-007 发电机定子U相线圈温度","yc_hs_0489","cur_01"]
[4763,"d_古交一期Ⅰ-007 发电机定子V相线圈温度","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅰ-007 发电机定子V相线圈温度","yc_hs_0489","cur_02"]
[4764,"d_古交一期Ⅰ-007 发电机定子W相线圈温度","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅰ-007 发电机定子W相线圈温度","yc_hs_0489","cur_03"]
[4765,"d_古交一期Ⅱ-012 主轴转速","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅱ-012 主轴转速","yc_hs_0489","cur_15"]
[4766,"d_古交一期Ⅱ-012 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅱ-012 齿轮箱高速轴非驱动端轴承温度","yc_hs_0489","cur_17"]
[4767,"d_古交一期Ⅱ-012 齿轮箱油池温度","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅱ-012 齿轮箱油池温度","yc_hs_0489","cur_18"]
[4768,"d_古交一期Ⅱ-012 主轴承外圈温度","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅱ-012 主轴承外圈温度","yc_hs_0489","cur_19"]
[4769,"d_古交一期Ⅱ-013 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅱ-013 机舱侧向振动值(已滤波)","yc_hs_0489","cur_27"]
[4770,"d_古交一期Ⅱ-013 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅱ-013 机舱轴向振动值(已滤波)","yc_hs_0489","cur_29"]
[4771,"d_古交一期Ⅲ-018 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅲ-018 2#桨叶片角度(桨距角)","yc_hs_0489","cur_30"]
[4772,"d_古交一期Ⅰ-001 舱内温度","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅰ-001 舱内温度","yc_hs_0489","cur_33"]
[4773,"d_古交一期Ⅰ-001 舱外温度","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅰ-001 舱外温度","yc_hs_0489","cur_34"]
[4774,"d_古交一期Ⅰ-001 风向","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅰ-001 风向","yc_hs_0489","cur_35"]
[4775,"d_古交一期Ⅰ-001 机舱角度（位置）","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅰ-001 机舱角度（位置）","yc_hs_0489","cur_37"]
[4776,"d_古交一期Ⅰ-001 偏航角度(扭缆角度）","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅰ-001 偏航角度(扭缆角度）","yc_hs_0489","cur_38"]
[4777,"d_古交一期Ⅰ-001 机舱与风向夹角","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅰ-001 机舱与风向夹角","yc_hs_0489","cur_39"]
[4778,"d_古交一期Ⅰ-001 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅰ-001 1#桨叶片角度(桨距角)","yc_hs_0489","cur_40"]
[4779,"d_古交一期Ⅰ-001 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅰ-001 2#桨叶片角度(桨距角)","yc_hs_0489","cur_41"]
[4780,"d_古交一期Ⅰ-001 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅰ-001 3#桨叶片角度(桨距角)","yc_hs_0489","cur_42"]
[4781,"d_古交一期Ⅰ-001 主轴转速","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅰ-001 主轴转速","yc_hs_0489","cur_49"]
[4782,"d_古交一期Ⅰ-001 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅰ-001 齿轮箱高速轴非驱动端轴承温度","yc_hs_0489","cur_51"]
[4783,"d_古交一期Ⅰ-001 齿轮箱油池温度","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅰ-001 齿轮箱油池温度","yc_hs_0356","cur_01"]
[4784,"d_古交一期Ⅲ-024 舱内温度","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅲ-024 舱内温度","yc_hs_0356","cur_31"]
[4785,"d_古交一期Ⅲ-024 舱外温度","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅲ-024 舱外温度","yc_hs_0356","cur_32"]
[4786,"d_古交一期Ⅲ-024 风向","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅲ-024 风向","yc_hs_0356","cur_33"]
[4787,"d_古交一期Ⅲ-024 机舱角度（位置）","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅲ-024 机舱角度（位置）","yc_hs_0356","cur_35"]
[4788,"d_古交一期Ⅲ-024 偏航角度(扭缆角度）","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅲ-024 偏航角度(扭缆角度）","yc_hs_0356","cur_36"]
[4789,"d_古交一期Ⅲ-024 机舱与风向夹角","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅲ-024 机舱与风向夹角","yc_hs_0356","cur_37"]
[4790,"d_古交一期Ⅲ-024 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅲ-024 1#桨叶片角度(桨距角)","yc_hs_0356","cur_38"]
[4791,"d_古交一期Ⅲ-024 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅲ-024 2#桨叶片角度(桨距角)","yc_hs_0356","cur_39"]
[4792,"d_古交一期Ⅲ-024 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅲ-024 3#桨叶片角度(桨距角)","yc_hs_0356","cur_40"]
[4793,"d_古交一期Ⅲ-024 主轴转速","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅲ-024 主轴转速","yc_hs_0358","cur_66"]
[4794,"d_古交一期Ⅲ-024 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅲ-024 齿轮箱高速轴非驱动端轴承温度","yc_hs_0358","cur_68"]
[4795,"d_古交一期Ⅲ-024 齿轮箱油池温度","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅲ-024 齿轮箱油池温度","yc_hs_0358","cur_69"]
[4796,"d_古交一期Ⅱ-010 主轴承外圈温度","古交风电场","WOF35100073",10,"SXGJ.T1_L2.WTG010.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅱ-010 主轴承外圈温度","yc_hs_0358","cur_70"]
[4797,"d_古交一期Ⅱ-011 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅱ-011 机舱侧向振动值(已滤波)","yc_hs_0358","cur_78"]
[4798,"d_古交一期Ⅱ-011 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅱ-011 机舱轴向振动值(已滤波)","yc_hs_0358","cur_80"]
[4799,"d_古交一期Ⅱ-011 风速","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅱ-011 风速","yc_hs_0358","cur_81"]
[4800,"d_古交一期Ⅱ-011 发电机有功功率","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅱ-011 发电机有功功率","yc_hs_0358","cur_82"]
[4801,"d_古交一期Ⅲ-018 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅲ-018 3#桨叶片角度(桨距角)","yc_hs_0358","cur_84"]
[4802,"d_古交一期Ⅲ-018 主轴转速","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅲ-018 主轴转速","yc_hs_0358","cur_91"]
[4803,"d_古交一期Ⅲ-018 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅲ-018 齿轮箱高速轴非驱动端轴承温度","yc_hs_0358","cur_93"]
[4804,"d_古交一期Ⅲ-018 齿轮箱油池温度","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅲ-018 齿轮箱油池温度","yc_hs_0358","cur_94"]
[4805,"d_古交一期Ⅲ-018 主轴承外圈温度","古交风电场","WOF35100073",18,"SXGJ.T1_L3.WTG018.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅲ-018 主轴承外圈温度","yc_hs_0358","cur_95"]
[4806,"d_古交一期Ⅰ-007 舱内温度","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅰ-007 舱内温度","yc_hs_0358","cur_100"]
[4807,"d_古交一期Ⅰ-007 舱外温度","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅰ-007 舱外温度","yc_hs_0479","cur_01"]
[4808,"d_古交一期Ⅰ-007 风向","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅰ-007 风向","yc_hs_0479","cur_02"]
[4809,"d_古交一期Ⅰ-007 机舱角度（位置）","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅰ-007 机舱角度（位置）","yc_hs_0479","cur_04"]
[4810,"d_古交一期Ⅰ-007 偏航角度(扭缆角度）","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅰ-007 偏航角度(扭缆角度）","yc_hs_0479","cur_90"]
[4811,"d_古交一期Ⅰ-007 机舱与风向夹角","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅰ-007 机舱与风向夹角","yc_hs_0479","cur_91"]
[4812,"d_古交一期Ⅰ-007 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅰ-007 1#桨叶片角度(桨距角)","yc_hs_0479","cur_92"]
[4813,"d_古交一期Ⅰ-007 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅰ-007 2#桨叶片角度(桨距角)","yc_hs_0479","cur_93"]
[4814,"d_古交一期Ⅰ-007 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅰ-007 3#桨叶片角度(桨距角)","yc_hs_0479","cur_94"]
[4815,"d_古交一期Ⅰ-007 主轴转速","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅰ-007 主轴转速","yc_hs_0480","cur_01"]
[4816,"d_古交一期Ⅰ-007 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅰ-007 齿轮箱高速轴非驱动端轴承温度","yc_hs_0480","cur_03"]
[4817,"d_古交一期Ⅰ-007 齿轮箱油池温度","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅰ-007 齿轮箱油池温度","yc_hs_0480","cur_04"]
[4818,"d_古交一期Ⅰ-007 主轴承外圈温度","古交风电场","WOF35100073",7,"SXGJ.T1_L1.WTG007.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅰ-007 主轴承外圈温度","yc_hs_0480","cur_05"]
[4819,"d_古交一期Ⅱ-013 风速","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅱ-013 风速","yc_hs_0480","cur_08"]
[4820,"d_古交一期Ⅱ-013 发电机有功功率","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅱ-013 发电机有功功率","yc_hs_0480","cur_09"]
[4821,"d_古交一期Ⅱ-013 发电机转速","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅱ-013 发电机转速","yc_hs_0480","cur_11"]
[4822,"d_古交一期Ⅱ-011 发电机转速","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅱ-011 发电机转速","yc_hs_0481","cur_27"]
[4823,"d_古交一期Ⅱ-011 发电机驱动端轴承温度","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅱ-011 发电机驱动端轴承温度","yc_hs_0481","cur_28"]
[4824,"d_古交一期Ⅱ-011 发电机非驱动端轴承温度","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅱ-011 发电机非驱动端轴承温度","yc_hs_0481","cur_29"]
[4825,"d_古交一期Ⅲ-016 主轴转速","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅲ-016 主轴转速","yc_hs_0481","cur_32"]
[4826,"d_古交一期Ⅲ-016 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅲ-016 齿轮箱高速轴非驱动端轴承温度","yc_hs_0481","cur_34"]
[4827,"d_古交一期Ⅲ-016 齿轮箱油池温度","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅲ-016 齿轮箱油池温度","yc_hs_0481","cur_35"]
[4828,"d_古交一期Ⅲ-016 主轴承外圈温度","古交风电场","WOF35100073",16,"SXGJ.T1_L3.WTG016.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅲ-016 主轴承外圈温度","yc_hs_0481","cur_36"]
[4829,"d_古交一期Ⅰ-001 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅰ-001 机舱侧向振动值(已滤波)","yc_hs_0481","cur_46"]
[4830,"d_古交一期Ⅰ-001 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅰ-001 机舱轴向振动值(已滤波)","yc_hs_0481","cur_48"]
[4831,"d_古交一期Ⅰ-001 风速","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅰ-001 风速","yc_hs_0481","cur_49"]
[4832,"d_古交一期Ⅰ-001 发电机有功功率","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅰ-001 发电机有功功率","yc_hs_0481","cur_50"]
[4833,"d_古交一期Ⅰ-001 发电机转速","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅰ-001 发电机转速","yc_hs_0481","cur_52"]
[4834,"d_古交一期Ⅰ-001 发电机驱动端轴承温度","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅰ-001 发电机驱动端轴承温度","yc_hs_0481","cur_53"]
[4835,"d_古交一期Ⅰ-001 发电机非驱动端轴承温度","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅰ-001 发电机非驱动端轴承温度","yc_hs_0481","cur_54"]
[4836,"d_古交一期Ⅰ-001 发电机定子U相线圈温度","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅰ-001 发电机定子U相线圈温度","yc_hs_0481","cur_55"]
[4837,"d_古交一期Ⅰ-001 发电机定子V相线圈温度","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅰ-001 发电机定子V相线圈温度","yc_hs_0481","cur_56"]
[4838,"d_古交一期Ⅰ-002 发电机定子U相线圈温度","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅰ-002 发电机定子U相线圈温度","yc_hs_0481","cur_57"]
[4839,"d_古交一期Ⅰ-002 发电机定子V相线圈温度","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅰ-002 发电机定子V相线圈温度","yc_hs_0481","cur_58"]
[4840,"d_古交一期Ⅰ-002 发电机定子W相线圈温度","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅰ-002 发电机定子W相线圈温度","yc_hs_0482","cur_46"]
[4841,"d_古交一期Ⅱ-013 发电机驱动端轴承温度","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅱ-013 发电机驱动端轴承温度","yc_hs_0482","cur_57"]
[4842,"d_古交一期Ⅱ-013 发电机非驱动端轴承温度","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅱ-013 发电机非驱动端轴承温度","yc_hs_0482","cur_58"]
[4843,"d_古交一期Ⅱ-013 发电机定子U相线圈温度","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅱ-013 发电机定子U相线圈温度","yc_hs_0482","cur_59"]
[4844,"d_古交一期Ⅱ-013 发电机定子V相线圈温度","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅱ-013 发电机定子V相线圈温度","yc_hs_0482","cur_60"]
[4845,"d_古交一期Ⅱ-013 发电机定子W相线圈温度","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅱ-013 发电机定子W相线圈温度","yc_hs_0482","cur_61"]
[4846,"d_古交一期Ⅱ-013 舱内温度","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅱ-013 舱内温度","yc_hs_0482","cur_73"]
[4847,"d_古交一期Ⅱ-013 舱外温度","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅱ-013 舱外温度","yc_hs_0482","cur_74"]
[4848,"d_古交一期Ⅱ-013 风向","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅱ-013 风向","yc_hs_0482","cur_75"]
[4849,"d_古交一期Ⅱ-013 机舱角度（位置）","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅱ-013 机舱角度（位置）","yc_hs_0482","cur_77"]
[4850,"d_古交一期Ⅱ-013 偏航角度(扭缆角度）","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅱ-013 偏航角度(扭缆角度）","yc_hs_0482","cur_78"]
[4851,"d_古交一期Ⅱ-013 机舱与风向夹角","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅱ-013 机舱与风向夹角","yc_hs_0482","cur_79"]
[4852,"d_古交一期Ⅱ-013 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅱ-013 1#桨叶片角度(桨距角)","yc_hs_0482","cur_80"]
[4853,"d_古交一期Ⅱ-013 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅱ-013 2#桨叶片角度(桨距角)","yc_hs_0482","cur_81"]
[4854,"d_古交一期Ⅱ-013 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅱ-013 3#桨叶片角度(桨距角)","yc_hs_0482","cur_82"]
[4855,"d_古交一期Ⅲ-019 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅲ-019 机舱侧向振动值(已滤波)","yc_hs_0483","cur_77"]
[4856,"d_古交一期Ⅲ-019 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅲ-019 机舱轴向振动值(已滤波)","yc_hs_0483","cur_79"]
[4857,"d_古交一期Ⅲ-019 风速","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅲ-019 风速","yc_hs_0483","cur_80"]
[4858,"d_古交一期Ⅲ-019 发电机有功功率","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅲ-019 发电机有功功率","yc_hs_0483","cur_81"]
[4859,"d_古交一期Ⅲ-019 发电机转速","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅲ-019 发电机转速","yc_hs_0483","cur_83"]
[4860,"d_古交一期Ⅲ-019 发电机驱动端轴承温度","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅲ-019 发电机驱动端轴承温度","yc_hs_0483","cur_84"]
[4861,"d_古交一期Ⅲ-019 发电机非驱动端轴承温度","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅲ-019 发电机非驱动端轴承温度","yc_hs_0483","cur_85"]
[4862,"d_古交一期Ⅲ-019 发电机定子U相线圈温度","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅲ-019 发电机定子U相线圈温度","yc_hs_0483","cur_86"]
[4863,"d_古交一期Ⅲ-019 发电机定子V相线圈温度","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅲ-019 发电机定子V相线圈温度","yc_hs_0483","cur_87"]
[4864,"d_古交一期Ⅲ-019 发电机定子W相线圈温度","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅲ-019 发电机定子W相线圈温度","yc_hs_0483","cur_88"]
[4865,"d_古交一期Ⅲ-019 舱内温度","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅲ-019 舱内温度","yc_hs_0483","cur_100"]
[4866,"d_古交一期Ⅲ-019 舱外温度","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅲ-019 舱外温度","yc_hs_0484","cur_01"]
[4867,"d_古交一期Ⅲ-019 风向","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅲ-019 风向","yc_hs_0484","cur_02"]
[4868,"d_古交一期Ⅲ-019 机舱角度（位置）","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅲ-019 机舱角度（位置）","yc_hs_0484","cur_04"]
[4869,"d_古交一期Ⅲ-023 舱内温度","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅲ-023 舱内温度","yc_hs_0484","cur_13"]
[4870,"d_古交一期Ⅲ-023 舱外温度","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅲ-023 舱外温度","yc_hs_0484","cur_14"]
[4871,"d_古交一期Ⅲ-023 风向","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅲ-023 风向","yc_hs_0484","cur_15"]
[4872,"d_古交一期Ⅲ-023 机舱角度（位置）","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅲ-023 机舱角度（位置）","yc_hs_0484","cur_17"]
[4873,"d_古交一期Ⅲ-023 偏航角度(扭缆角度）","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅲ-023 偏航角度(扭缆角度）","yc_hs_0484","cur_18"]
[4874,"d_古交一期Ⅲ-023 机舱与风向夹角","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅲ-023 机舱与风向夹角","yc_hs_0484","cur_89"]
[4875,"d_古交一期Ⅲ-023 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅲ-023 1#桨叶片角度(桨距角)","yc_hs_0484","cur_90"]
[4876,"d_古交一期Ⅲ-023 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅲ-023 2#桨叶片角度(桨距角)","yc_hs_0484","cur_91"]
[4877,"d_古交一期Ⅲ-023 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅲ-023 3#桨叶片角度(桨距角)","yc_hs_0484","cur_92"]
[4878,"d_古交一期Ⅲ-023 主轴转速","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅲ-023 主轴转速","yc_hs_0484","cur_99"]
[4879,"d_古交一期Ⅲ-023 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅲ-023 齿轮箱高速轴非驱动端轴承温度","yc_hs_0485","cur_01"]
[4880,"d_古交一期Ⅲ-023 齿轮箱油池温度","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅲ-023 齿轮箱油池温度","yc_hs_0485","cur_02"]
[4881,"d_古交一期Ⅲ-023 主轴承外圈温度","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅲ-023 主轴承外圈温度","yc_hs_0485","cur_03"]
[4882,"d_古交一期Ⅱ-008 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅱ-008 机舱侧向振动值(已滤波)","yc_hs_0485","cur_11"]
[4883,"d_古交一期Ⅱ-008 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅱ-008 机舱轴向振动值(已滤波)","yc_hs_0485","cur_13"]
[4884,"d_古交一期Ⅱ-008 风速","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅱ-008 风速","yc_hs_0485","cur_14"]
[4885,"d_古交一期Ⅱ-008 发电机有功功率","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅱ-008 发电机有功功率","yc_hs_0485","cur_15"]
[4886,"d_古交一期Ⅱ-008 发电机转速","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅱ-008 发电机转速","yc_hs_0485","cur_17"]
[4887,"d_古交一期Ⅱ-008 发电机驱动端轴承温度","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅱ-008 发电机驱动端轴承温度","yc_hs_0485","cur_18"]
[4888,"d_古交一期Ⅱ-008 发电机非驱动端轴承温度","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅱ-008 发电机非驱动端轴承温度","yc_hs_0485","cur_19"]
[4889,"d_古交一期Ⅱ-008 发电机定子U相线圈温度","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅱ-008 发电机定子U相线圈温度","yc_hs_0485","cur_20"]
[4890,"d_古交一期Ⅱ-008 发电机定子V相线圈温度","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅱ-008 发电机定子V相线圈温度","yc_hs_0485","cur_21"]
[4891,"d_古交一期Ⅱ-008 发电机定子W相线圈温度","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅱ-008 发电机定子W相线圈温度","yc_hs_0485","cur_22"]
[4892,"d_古交一期Ⅱ-013 主轴转速","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅱ-013 主轴转速","yc_hs_0486","cur_18"]
[4893,"d_古交一期Ⅱ-013 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅱ-013 齿轮箱高速轴非驱动端轴承温度","yc_hs_0486","cur_20"]
[4894,"d_古交一期Ⅱ-013 齿轮箱油池温度","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅱ-013 齿轮箱油池温度","yc_hs_0486","cur_21"]
[4895,"d_古交一期Ⅱ-013 主轴承外圈温度","古交风电场","WOF35100073",13,"SXGJ.T1_L2.WTG013.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅱ-013 主轴承外圈温度","yc_hs_0486","cur_22"]
[4896,"d_古交一期Ⅱ-014 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅱ-014 机舱侧向振动值(已滤波)","yc_hs_0486","cur_30"]
[4897,"d_古交一期Ⅲ-019 偏航角度(扭缆角度）","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅲ-019 偏航角度(扭缆角度）","yc_hs_0486","cur_31"]
[4898,"d_古交一期Ⅲ-019 机舱与风向夹角","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅲ-019 机舱与风向夹角","yc_hs_0486","cur_32"]
[4899,"d_古交一期Ⅲ-019 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅲ-019 1#桨叶片角度(桨距角)","yc_hs_0486","cur_33"]
[4900,"d_古交一期Ⅲ-019 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅲ-019 2#桨叶片角度(桨距角)","yc_hs_0486","cur_34"]
[4901,"d_古交一期Ⅲ-019 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅲ-019 3#桨叶片角度(桨距角)","yc_hs_0486","cur_35"]
[4902,"d_古交一期Ⅲ-019 主轴转速","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅲ-019 主轴转速","yc_hs_0486","cur_42"]
[4903,"d_古交一期Ⅲ-019 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅲ-019 齿轮箱高速轴非驱动端轴承温度","yc_hs_0486","cur_44"]
[4904,"d_古交一期Ⅲ-019 齿轮箱油池温度","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅲ-019 齿轮箱油池温度","yc_hs_0486","cur_45"]
[4905,"d_古交一期Ⅲ-019 主轴承外圈温度","古交风电场","WOF35100073",19,"SXGJ.T1_L3.WTG019.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅲ-019 主轴承外圈温度","yc_hs_0486","cur_46"]
[4906,"d_古交一期Ⅰ-001 主轴承外圈温度","古交风电场","WOF35100073",1,"SXGJ.T1_L1.WTG001.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅰ-001 主轴承外圈温度","yc_hs_0486","cur_91"]
[4907,"d_古交一期Ⅰ-002 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅰ-002 机舱侧向振动值(已滤波)","yc_hs_0486","cur_99"]
[4908,"d_古交一期Ⅰ-002 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅰ-002 机舱轴向振动值(已滤波)","yc_hs_0487","cur_01"]
[4909,"d_古交一期Ⅰ-002 风速","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅰ-002 风速","yc_hs_0487","cur_02"]
[4910,"d_古交一期Ⅰ-002 发电机有功功率","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅰ-002 发电机有功功率","yc_hs_0487","cur_03"]
[4911,"d_古交一期Ⅰ-002 发电机转速","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅰ-002 发电机转速","yc_hs_0487","cur_05"]
[4912,"d_古交一期Ⅰ-002 发电机驱动端轴承温度","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅰ-002 发电机驱动端轴承温度","yc_hs_0487","cur_06"]
[4913,"d_古交一期Ⅰ-002 齿轮箱油池温度","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅰ-002 齿轮箱油池温度","yc_hs_0487","cur_07"]
[4914,"d_古交一期Ⅰ-002 主轴承外圈温度","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅰ-002 主轴承外圈温度","yc_hs_0487","cur_08"]
[4915,"d_古交一期Ⅰ-003 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅰ-003 机舱侧向振动值(已滤波)","yc_hs_0487","cur_16"]
[4916,"d_古交一期Ⅰ-003 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅰ-003 机舱轴向振动值(已滤波)","yc_hs_0487","cur_18"]
[4917,"d_古交一期Ⅰ-003 风速","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅰ-003 风速","yc_hs_0487","cur_19"]
[4918,"d_古交一期Ⅰ-003 发电机有功功率","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅰ-003 发电机有功功率","yc_hs_0487","cur_20"]
[4919,"d_古交一期Ⅰ-003 发电机驱动端轴承温度","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅰ-003 发电机驱动端轴承温度","yc_hs_0487","cur_22"]
[4920,"d_古交一期Ⅰ-003 发电机非驱动端轴承温度","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅰ-003 发电机非驱动端轴承温度","yc_hs_0487","cur_23"]
[4921,"d_古交一期Ⅰ-003 发电机定子U相线圈温度","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅰ-003 发电机定子U相线圈温度","yc_hs_0487","cur_68"]
[4922,"d_古交一期Ⅰ-003 发电机定子V相线圈温度","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅰ-003 发电机定子V相线圈温度","yc_hs_0487","cur_69"]
[4923,"d_古交一期Ⅰ-003 发电机定子W相线圈温度","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅰ-003 发电机定子W相线圈温度","yc_hs_0487","cur_70"]
[4924,"d_古交一期Ⅱ-008 舱内温度","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅱ-008 舱内温度","yc_hs_0487","cur_89"]
[4925,"d_古交一期Ⅱ-008 舱外温度","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅱ-008 舱外温度","yc_hs_0487","cur_90"]
[4926,"d_古交一期Ⅱ-008 风向","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅱ-008 风向","yc_hs_0487","cur_91"]
[4927,"d_古交一期Ⅱ-008 机舱角度（位置）","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅱ-008 机舱角度（位置）","yc_hs_0487","cur_93"]
[4928,"d_古交一期Ⅱ-008 偏航角度(扭缆角度）","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅱ-008 偏航角度(扭缆角度）","yc_hs_0487","cur_94"]
[4929,"d_古交一期Ⅱ-008 机舱与风向夹角","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅱ-008 机舱与风向夹角","yc_hs_0487","cur_95"]
[4930,"d_古交一期Ⅱ-008 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅱ-008 1#桨叶片角度(桨距角)","yc_hs_0487","cur_96"]
[4931,"d_古交一期Ⅱ-008 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅱ-008 2#桨叶片角度(桨距角)","yc_hs_0487","cur_97"]
[4932,"d_古交一期Ⅱ-008 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅱ-008 3#桨叶片角度(桨距角)","yc_hs_0487","cur_98"]
[4933,"d_古交一期Ⅱ-008 主轴转速","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅱ-008 主轴转速","yc_hs_0356","cur_47"]
[4934,"d_古交一期Ⅰ-003 舱内温度","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅰ-003 舱内温度","yc_hs_0356","cur_56"]
[4935,"d_古交一期Ⅰ-003 舱外温度","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅰ-003 舱外温度","yc_hs_0356","cur_57"]
[4936,"d_古交一期Ⅰ-003 风向","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅰ-003 风向","yc_hs_0356","cur_58"]
[4937,"d_古交一期Ⅰ-003 机舱角度（位置）","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅰ-003 机舱角度（位置）","yc_hs_0356","cur_60"]
[4938,"d_古交一期Ⅰ-003 偏航角度(扭缆角度）","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅰ-003 偏航角度(扭缆角度）","yc_hs_0356","cur_61"]
[4939,"d_古交一期Ⅰ-003 机舱与风向夹角","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅰ-003 机舱与风向夹角","yc_hs_0356","cur_62"]
[4940,"d_古交一期Ⅰ-003 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅰ-003 1#桨叶片角度(桨距角)","yc_hs_0356","cur_63"]
[4941,"d_古交一期Ⅰ-003 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅰ-003 2#桨叶片角度(桨距角)","yc_hs_0356","cur_64"]
[4942,"d_古交一期Ⅰ-003 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅰ-003 3#桨叶片角度(桨距角)","yc_hs_0356","cur_65"]
[4943,"d_古交一期Ⅰ-004 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅰ-004 机舱侧向振动值(已滤波)","yc_hs_0356","cur_70"]
[4944,"d_古交一期Ⅰ-004 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅰ-004 机舱轴向振动值(已滤波)","yc_hs_0356","cur_72"]
[4945,"d_古交一期Ⅰ-004 风速","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅰ-004 风速","yc_hs_0356","cur_73"]
[4946,"d_古交一期Ⅰ-004 发电机有功功率","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅰ-004 发电机有功功率","yc_hs_0356","cur_74"]
[4947,"d_古交一期Ⅰ-004 发电机转速","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅰ-004 发电机转速","yc_hs_0356","cur_76"]
[4948,"d_古交一期Ⅰ-004 发电机驱动端轴承温度","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅰ-004 发电机驱动端轴承温度","yc_hs_0356","cur_77"]
[4949,"d_古交一期Ⅰ-004 发电机非驱动端轴承温度","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅰ-004 发电机非驱动端轴承温度","yc_hs_0356","cur_78"]
[4950,"d_古交一期Ⅰ-004 发电机定子U相线圈温度","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅰ-004 发电机定子U相线圈温度","yc_hs_0356","cur_79"]
[4951,"d_古交一期Ⅰ-004 发电机定子V相线圈温度","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅰ-004 发电机定子V相线圈温度","yc_hs_0356","cur_80"]
[4952,"d_古交一期Ⅰ-004 发电机定子W相线圈温度","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅰ-004 发电机定子W相线圈温度","yc_hs_0356","cur_81"]
[4953,"d_古交一期Ⅱ-008 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅱ-008 齿轮箱高速轴非驱动端轴承温度","yc_hs_0357","cur_68"]
[4954,"d_古交一期Ⅱ-008 齿轮箱油池温度","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅱ-008 齿轮箱油池温度","yc_hs_0357","cur_69"]
[4955,"d_古交一期Ⅱ-008 主轴承外圈温度","古交风电场","WOF35100073",8,"SXGJ.T1_L2.WTG008.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅱ-008 主轴承外圈温度","yc_hs_0357","cur_70"]
[4956,"d_古交一期Ⅱ-014 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅱ-014 机舱轴向振动值(已滤波)","yc_hs_0357","cur_74"]
[4957,"d_古交一期Ⅱ-014 风速","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅱ-014 风速","yc_hs_0357","cur_75"]
[4958,"d_古交一期Ⅱ-014 发电机有功功率","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅱ-014 发电机有功功率","yc_hs_0357","cur_76"]
[4959,"d_古交一期Ⅱ-014 发电机转速","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅱ-014 发电机转速","yc_hs_0357","cur_78"]
[4960,"d_古交一期Ⅱ-014 发电机驱动端轴承温度","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅱ-014 发电机驱动端轴承温度","yc_hs_0357","cur_79"]
[4961,"d_古交一期Ⅱ-014 发电机非驱动端轴承温度","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅱ-014 发电机非驱动端轴承温度","yc_hs_0357","cur_80"]
[4962,"d_古交一期Ⅱ-014 发电机定子U相线圈温度","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅱ-014 发电机定子U相线圈温度","yc_hs_0357","cur_81"]
[4963,"d_古交一期Ⅱ-014 发电机定子V相线圈温度","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅱ-014 发电机定子V相线圈温度","yc_hs_0357","cur_82"]
[4964,"d_古交一期Ⅱ-014 发电机定子W相线圈温度","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅱ-014 发电机定子W相线圈温度","yc_hs_0357","cur_83"]
[4965,"d_古交一期Ⅱ-014 舱内温度","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅱ-014 舱内温度","yc_hs_0357","cur_95"]
[4966,"d_古交一期Ⅱ-014 舱外温度","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅱ-014 舱外温度","yc_hs_0357","cur_96"]
[4967,"d_古交一期Ⅱ-014 风向","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅱ-014 风向","yc_hs_0357","cur_97"]
[4968,"d_古交一期Ⅱ-014 机舱角度（位置）","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅱ-014 机舱角度（位置）","yc_hs_0357","cur_99"]
[4969,"d_古交一期Ⅱ-014 偏航角度(扭缆角度）","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅱ-014 偏航角度(扭缆角度）","yc_hs_0357","cur_100"]
[4970,"d_古交一期Ⅱ-014 机舱与风向夹角","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅱ-014 机舱与风向夹角","yc_hs_0358","cur_01"]
[4971,"d_古交一期Ⅱ-014 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅱ-014 1#桨叶片角度(桨距角)","yc_hs_0358","cur_02"]
[4972,"d_古交一期Ⅱ-014 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅱ-014 2#桨叶片角度(桨距角)","yc_hs_0358","cur_03"]
[4973,"d_古交一期Ⅱ-014 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅱ-014 3#桨叶片角度(桨距角)","yc_hs_0358","cur_04"]
[4974,"d_古交一期Ⅰ-004 舱内温度","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅰ-004 舱内温度","yc_hs_0479","cur_12"]
[4975,"d_古交一期Ⅰ-004 舱外温度","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅰ-004 舱外温度","yc_hs_0479","cur_13"]
[4976,"d_古交一期Ⅰ-004 风向","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅰ-004 风向","yc_hs_0479","cur_14"]
[4977,"d_古交一期Ⅰ-004 机舱角度（位置）","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅰ-004 机舱角度（位置）","yc_hs_0479","cur_16"]
[4978,"d_古交一期Ⅰ-004 偏航角度(扭缆角度）","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅰ-004 偏航角度(扭缆角度）","yc_hs_0479","cur_17"]
[4979,"d_古交一期Ⅰ-004 机舱与风向夹角","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅰ-004 机舱与风向夹角","yc_hs_0479","cur_18"]
[4980,"d_古交一期Ⅰ-004 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅰ-004 1#桨叶片角度(桨距角)","yc_hs_0479","cur_19"]
[4981,"d_古交一期Ⅰ-002 发电机非驱动端轴承温度","古交风电场","WOF35100073",2,"SXGJ.T1_L1.WTG002.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅰ-002 发电机非驱动端轴承温度","yc_hs_0479","cur_20"]
[4982,"d_古交一期Ⅰ-004 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅰ-004 3#桨叶片角度(桨距角)","yc_hs_0479","cur_21"]
[4983,"d_古交一期Ⅰ-004 主轴转速","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅰ-004 主轴转速","yc_hs_0479","cur_28"]
[4984,"d_古交一期Ⅰ-004 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅰ-004 齿轮箱高速轴非驱动端轴承温度","yc_hs_0479","cur_30"]
[4985,"d_古交一期Ⅰ-004 齿轮箱油池温度","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅰ-004 齿轮箱油池温度","yc_hs_0479","cur_31"]
[4986,"d_古交一期Ⅰ-004 主轴承外圈温度","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅰ-004 主轴承外圈温度","yc_hs_0479","cur_32"]
[4987,"d_古交一期Ⅰ-003 发电机转速","古交风电场","WOF35100073",3,"SXGJ.T1_L1.WTG003.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅰ-003 发电机转速","yc_hs_0479","cur_36"]
[4988,"d_古交一期Ⅰ-005 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅰ-005 机舱侧向振动值(已滤波)","yc_hs_0479","cur_41"]
[4989,"d_古交一期Ⅰ-005 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅰ-005 机舱轴向振动值(已滤波)","yc_hs_0479","cur_43"]
[4990,"d_古交一期Ⅰ-005 风速","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅰ-005 风速","yc_hs_0479","cur_44"]
[4991,"d_古交一期Ⅰ-005 发电机有功功率","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅰ-005 发电机有功功率","yc_hs_0479","cur_45"]
[4992,"d_古交一期Ⅰ-005 发电机转速","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅰ-005 发电机转速","yc_hs_0479","cur_47"]
[4993,"d_古交一期Ⅰ-005 发电机驱动端轴承温度","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅰ-005 发电机驱动端轴承温度","yc_hs_0480","cur_31"]
[4994,"d_古交一期Ⅰ-005 发电机非驱动端轴承温度","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅰ-005 发电机非驱动端轴承温度","yc_hs_0480","cur_32"]
[4995,"d_古交一期Ⅰ-005 发电机定子U相线圈温度","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅰ-005 发电机定子U相线圈温度","yc_hs_0480","cur_33"]
[4996,"d_古交一期Ⅰ-005 发电机定子V相线圈温度","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅰ-005 发电机定子V相线圈温度","yc_hs_0480","cur_34"]
[4997,"d_古交一期Ⅰ-005 发电机定子W相线圈温度","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅰ-005 发电机定子W相线圈温度","yc_hs_0480","cur_35"]
[4998,"d_古交一期Ⅲ-020 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅲ-020 机舱侧向振动值(已滤波)","yc_hs_0480","cur_40"]
[4999,"d_古交一期Ⅲ-020 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅲ-020 机舱轴向振动值(已滤波)","yc_hs_0480","cur_42"]
[5000,"d_古交一期Ⅲ-020 风速","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅲ-020 风速","yc_hs_0480","cur_43"]
[5001,"d_古交一期Ⅲ-020 发电机有功功率","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅲ-020 发电机有功功率","yc_hs_0480","cur_44"]
[5002,"d_古交一期Ⅲ-020 发电机转速","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅲ-020 发电机转速","yc_hs_0480","cur_46"]
[5003,"d_古交一期Ⅲ-020 发电机驱动端轴承温度","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅲ-020 发电机驱动端轴承温度","yc_hs_0480","cur_47"]
[5004,"d_古交一期Ⅲ-020 发电机非驱动端轴承温度","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅲ-020 发电机非驱动端轴承温度","yc_hs_0480","cur_48"]
[5005,"d_古交一期Ⅲ-020 发电机定子U相线圈温度","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅲ-020 发电机定子U相线圈温度","yc_hs_0480","cur_49"]
[5006,"d_古交一期Ⅲ-020 发电机定子V相线圈温度","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅲ-020 发电机定子V相线圈温度","yc_hs_0480","cur_50"]
[5007,"d_古交一期Ⅲ-020 发电机定子W相线圈温度","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅲ-020 发电机定子W相线圈温度","yc_hs_0480","cur_51"]
[5008,"d_古交一期Ⅲ-020 舱内温度","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅲ-020 舱内温度","yc_hs_0480","cur_63"]
[5009,"d_古交一期Ⅲ-020 舱外温度","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅲ-020 舱外温度","yc_hs_0480","cur_64"]
[5010,"d_古交一期Ⅱ-009 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅱ-009 机舱侧向振动值(已滤波)","yc_hs_0480","cur_70"]
[5011,"d_古交一期Ⅱ-009 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅱ-009 机舱轴向振动值(已滤波)","yc_hs_0480","cur_72"]
[5012,"d_古交一期Ⅱ-009 风速","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅱ-009 风速","yc_hs_0480","cur_73"]
[5013,"d_古交一期Ⅱ-009 发电机有功功率","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅱ-009 发电机有功功率","yc_hs_0481","cur_59"]
[5014,"d_古交一期Ⅱ-009 发电机转速","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅱ-009 发电机转速","yc_hs_0481","cur_61"]
[5015,"d_古交一期Ⅱ-009 发电机驱动端轴承温度","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅱ-009 发电机驱动端轴承温度","yc_hs_0481","cur_62"]
[5016,"d_古交一期Ⅱ-009 发电机非驱动端轴承温度","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅱ-009 发电机非驱动端轴承温度","yc_hs_0481","cur_63"]
[5017,"d_古交一期Ⅰ-005 舱内温度","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅰ-005 舱内温度","yc_hs_0481","cur_75"]
[5018,"d_古交一期Ⅰ-005 舱外温度","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅰ-005 舱外温度","yc_hs_0481","cur_76"]
[5019,"d_古交一期Ⅰ-005 风向","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅰ-005 风向","yc_hs_0481","cur_77"]
[5020,"d_古交一期Ⅰ-005 机舱角度（位置）","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅰ-005 机舱角度（位置）","yc_hs_0481","cur_79"]
[5021,"d_古交一期Ⅲ-022 舱内温度","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅲ-022 舱内温度","yc_hs_0481","cur_85"]
[5022,"d_古交一期Ⅲ-022 舱外温度","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅲ-022 舱外温度","yc_hs_0481","cur_86"]
[5023,"d_古交一期Ⅲ-022 风向","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅲ-022 风向","yc_hs_0481","cur_87"]
[5024,"d_古交一期Ⅲ-022 机舱角度（位置）","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅲ-022 机舱角度（位置）","yc_hs_0481","cur_89"]
[5025,"d_古交一期Ⅲ-022 偏航角度(扭缆角度）","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅲ-022 偏航角度(扭缆角度）","yc_hs_0481","cur_90"]
[5026,"d_古交一期Ⅲ-022 机舱与风向夹角","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅲ-022 机舱与风向夹角","yc_hs_0481","cur_91"]
[5027,"d_古交一期Ⅲ-022 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅲ-022 1#桨叶片角度(桨距角)","yc_hs_0481","cur_92"]
[5028,"d_古交一期Ⅲ-022 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅲ-022 2#桨叶片角度(桨距角)","yc_hs_0481","cur_93"]
[5029,"d_古交一期Ⅲ-022 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅲ-022 3#桨叶片角度(桨距角)","yc_hs_0481","cur_94"]
[5030,"d_古交一期Ⅲ-022 主轴转速","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅲ-022 主轴转速","yc_hs_0482","cur_01"]
[5031,"d_古交一期Ⅲ-022 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅲ-022 齿轮箱高速轴非驱动端轴承温度","yc_hs_0482","cur_89"]
[5032,"d_古交一期Ⅲ-022 齿轮箱油池温度","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅲ-022 齿轮箱油池温度","yc_hs_0482","cur_90"]
[5033,"d_古交一期Ⅲ-022 主轴承外圈温度","古交风电场","WOF35100073",22,"SXGJ.T1_L3.WTG022.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅲ-022 主轴承外圈温度","yc_hs_0482","cur_91"]
[5034,"d_古交一期Ⅱ-009 发电机定子U相线圈温度","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅱ-009 发电机定子U相线圈温度","yc_hs_0482","cur_93"]
[5035,"d_古交一期Ⅱ-009 发电机定子V相线圈温度","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅱ-009 发电机定子V相线圈温度","yc_hs_0482","cur_94"]
[5036,"d_古交一期Ⅱ-009 发电机定子W相线圈温度","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅱ-009 发电机定子W相线圈温度","yc_hs_0482","cur_95"]
[5037,"d_古交一期Ⅱ-014 主轴转速","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅱ-014 主轴转速","yc_hs_0483","cur_01"]
[5038,"d_古交一期Ⅱ-014 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅱ-014 齿轮箱高速轴非驱动端轴承温度","yc_hs_0483","cur_03"]
[5039,"d_古交一期Ⅱ-014 齿轮箱油池温度","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅱ-014 齿轮箱油池温度","yc_hs_0483","cur_04"]
[5040,"d_古交一期Ⅱ-014 主轴承外圈温度","古交风电场","WOF35100073",14,"SXGJ.T1_L2.WTG014.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅱ-014 主轴承外圈温度","yc_hs_0483","cur_05"]
[5041,"d_古交一期Ⅲ-020 风向","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅲ-020 风向","yc_hs_0483","cur_12"]
[5042,"d_古交一期Ⅲ-020 机舱角度（位置）","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅲ-020 机舱角度（位置）","yc_hs_0483","cur_14"]
[5043,"d_古交一期Ⅲ-020 偏航角度(扭缆角度）","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅲ-020 偏航角度(扭缆角度）","yc_hs_0483","cur_15"]
[5044,"d_古交一期Ⅲ-020 机舱与风向夹角","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅲ-020 机舱与风向夹角","yc_hs_0483","cur_16"]
[5045,"d_古交一期Ⅲ-020 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅲ-020 1#桨叶片角度(桨距角)","yc_hs_0483","cur_17"]
[5046,"d_古交一期Ⅲ-020 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅲ-020 2#桨叶片角度(桨距角)","yc_hs_0483","cur_18"]
[5047,"d_古交一期Ⅲ-020 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅲ-020 3#桨叶片角度(桨距角)","yc_hs_0483","cur_19"]
[5048,"d_古交一期Ⅲ-020 主轴转速","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅲ-020 主轴转速","yc_hs_0483","cur_26"]
[5049,"d_古交一期Ⅲ-020 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅲ-020 齿轮箱高速轴非驱动端轴承温度","yc_hs_0483","cur_28"]
[5050,"d_古交一期Ⅲ-020 齿轮箱油池温度","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅲ-020 齿轮箱油池温度","yc_hs_0483","cur_29"]
[5051,"d_古交一期Ⅲ-020 主轴承外圈温度","古交风电场","WOF35100073",20,"SXGJ.T1_L3.WTG020.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅲ-020 主轴承外圈温度","yc_hs_0483","cur_30"]
[5052,"d_古交一期Ⅰ-004 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",4,"SXGJ.T1_L1.WTG004.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅰ-004 2#桨叶片角度(桨距角)","yc_hs_0484","cur_23"]
[5053,"d_古交一期Ⅰ-005 机舱与风向夹角","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅰ-005 机舱与风向夹角","yc_hs_0484","cur_24"]
[5054,"d_古交一期Ⅰ-005 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅰ-005 1#桨叶片角度(桨距角)","yc_hs_0484","cur_25"]
[5055,"d_古交一期Ⅰ-005 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅰ-005 2#桨叶片角度(桨距角)","yc_hs_0484","cur_26"]
[5056,"d_古交一期Ⅰ-005 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅰ-005 3#桨叶片角度(桨距角)","yc_hs_0484","cur_27"]
[5057,"d_古交一期Ⅰ-005 主轴转速","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅰ-005 主轴转速","yc_hs_0484","cur_34"]
[5058,"d_古交一期Ⅰ-005 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅰ-005 齿轮箱高速轴非驱动端轴承温度","yc_hs_0484","cur_36"]
[5059,"d_古交一期Ⅰ-005 齿轮箱油池温度","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅰ-005 齿轮箱油池温度","yc_hs_0484","cur_37"]
[5060,"d_古交一期Ⅰ-005 主轴承外圈温度","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅰ-005 主轴承外圈温度","yc_hs_0484","cur_38"]
[5061,"d_古交一期Ⅱ-011 发电机定子U相线圈温度","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅱ-011 发电机定子U相线圈温度","yc_hs_0484","cur_41"]
[5062,"d_古交一期Ⅱ-011 发电机定子V相线圈温度","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅱ-011 发电机定子V相线圈温度","yc_hs_0484","cur_42"]
[5063,"d_古交一期Ⅱ-011 发电机定子W相线圈温度","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅱ-011 发电机定子W相线圈温度","yc_hs_0484","cur_43"]
[5064,"d_古交一期Ⅱ-011 舱内温度","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅱ-011 舱内温度","yc_hs_0484","cur_55"]
[5065,"d_古交一期Ⅱ-011 舱外温度","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅱ-011 舱外温度","yc_hs_0484","cur_56"]
[5066,"d_古交一期Ⅱ-011 风向","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅱ-011 风向","yc_hs_0484","cur_57"]
[5067,"d_古交一期Ⅱ-011 机舱角度（位置）","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅱ-011 机舱角度（位置）","yc_hs_0484","cur_59"]
[5068,"d_古交一期Ⅱ-011 偏航角度(扭缆角度）","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅱ-011 偏航角度(扭缆角度）","yc_hs_0484","cur_60"]
[5069,"d_古交一期Ⅱ-011 机舱与风向夹角","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅱ-011 机舱与风向夹角","yc_hs_0484","cur_61"]
[5070,"d_古交一期Ⅱ-011 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅱ-011 1#桨叶片角度(桨距角)","yc_hs_0485","cur_32"]
[5071,"d_古交一期Ⅱ-011 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅱ-011 2#桨叶片角度(桨距角)","yc_hs_0485","cur_33"]
[5072,"d_古交一期Ⅱ-011 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅱ-011 3#桨叶片角度(桨距角)","yc_hs_0485","cur_34"]
[5073,"d_古交一期Ⅲ-024 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅲ-024 机舱侧向振动值(已滤波)","yc_hs_0485","cur_38"]
[5074,"d_古交一期Ⅲ-024 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅲ-024 机舱轴向振动值(已滤波)","yc_hs_0485","cur_40"]
[5075,"d_古交一期Ⅲ-024 风速","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅲ-024 风速","yc_hs_0485","cur_41"]
[5076,"d_古交一期Ⅲ-024 发电机有功功率","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅲ-024 发电机有功功率","yc_hs_0485","cur_42"]
[5077,"d_古交一期Ⅲ-024 发电机转速","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅲ-024 发电机转速","yc_hs_0485","cur_44"]
[5078,"d_古交一期Ⅲ-024 发电机驱动端轴承温度","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅲ-024 发电机驱动端轴承温度","yc_hs_0485","cur_45"]
[5079,"d_古交一期Ⅲ-024 发电机非驱动端轴承温度","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅲ-024 发电机非驱动端轴承温度","yc_hs_0485","cur_46"]
[5080,"d_古交一期Ⅲ-024 发电机定子U相线圈温度","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅲ-024 发电机定子U相线圈温度","yc_hs_0485","cur_47"]
[5081,"d_古交一期Ⅲ-024 发电机定子V相线圈温度","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅲ-024 发电机定子V相线圈温度","yc_hs_0485","cur_48"]
[5082,"d_古交一期Ⅲ-024 发电机定子W相线圈温度","古交风电场","WOF35100073",24,"SXGJ.T1_L3.WTG024.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅲ-024 发电机定子W相线圈温度","yc_hs_0485","cur_49"]
[5083,"d_古交一期Ⅱ-009 舱内温度","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅱ-009 舱内温度","yc_hs_0485","cur_58"]
[5084,"d_古交一期Ⅱ-009 舱外温度","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅱ-009 舱外温度","yc_hs_0485","cur_59"]
[5085,"d_古交一期Ⅱ-009 风向","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅱ-009 风向","yc_hs_0485","cur_60"]
[5086,"d_古交一期Ⅱ-009 机舱角度（位置）","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅱ-009 机舱角度（位置）","yc_hs_0485","cur_62"]
[5087,"d_古交一期Ⅱ-009 偏航角度(扭缆角度）","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅱ-009 偏航角度(扭缆角度）","yc_hs_0485","cur_63"]
[5088,"d_古交一期Ⅱ-009 机舱与风向夹角","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅱ-009 机舱与风向夹角","yc_hs_0485","cur_64"]
[5089,"d_古交一期Ⅱ-009 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅱ-009 1#桨叶片角度(桨距角)","yc_hs_0485","cur_65"]
[5090,"d_古交一期Ⅱ-009 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅱ-009 2#桨叶片角度(桨距角)","yc_hs_0485","cur_66"]
[5091,"d_古交一期Ⅱ-009 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅱ-009 3#桨叶片角度(桨距角)","yc_hs_0485","cur_67"]
[5092,"d_古交一期Ⅱ-009 主轴转速","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅱ-009 主轴转速","yc_hs_0485","cur_74"]
[5093,"d_古交一期Ⅱ-009 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅱ-009 齿轮箱高速轴非驱动端轴承温度","yc_hs_0486","cur_53"]
[5094,"d_古交一期Ⅱ-009 齿轮箱油池温度","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅱ-009 齿轮箱油池温度","yc_hs_0486","cur_54"]
[5095,"d_古交一期Ⅱ-011 主轴转速","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅱ-011 主轴转速","yc_hs_0486","cur_61"]
[5096,"d_古交一期Ⅰ-005 偏航角度(扭缆角度）","古交风电场","WOF35100073",5,"SXGJ.T1_L1.WTG005.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅰ-005 偏航角度(扭缆角度）","yc_hs_0486","cur_63"]
[5097,"d_古交一期Ⅲ-017 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅲ-017 机舱侧向振动值(已滤波)","yc_hs_0486","cur_68"]
[5098,"d_古交一期Ⅲ-017 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅲ-017 机舱轴向振动值(已滤波)","yc_hs_0486","cur_70"]
[5099,"d_古交一期Ⅲ-017 风速","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅲ-017 风速","yc_hs_0486","cur_71"]
[5100,"d_古交一期Ⅲ-017 发电机有功功率","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅲ-017 发电机有功功率","yc_hs_0486","cur_72"]
[5101,"d_古交一期Ⅲ-017 发电机转速","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅲ-017 发电机转速","yc_hs_0486","cur_74"]
[5102,"d_古交一期Ⅲ-017 发电机驱动端轴承温度","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅲ-017 发电机驱动端轴承温度","yc_hs_0486","cur_75"]
[5103,"d_古交一期Ⅲ-017 发电机非驱动端轴承温度","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅲ-017 发电机非驱动端轴承温度","yc_hs_0486","cur_76"]
[5104,"d_古交一期Ⅲ-017 发电机定子U相线圈温度","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅲ-017 发电机定子U相线圈温度","yc_hs_0486","cur_77"]
[5105,"d_古交一期Ⅲ-017 发电机定子V相线圈温度","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅲ-017 发电机定子V相线圈温度","yc_hs_0486","cur_78"]
[5106,"d_古交一期Ⅲ-017 发电机定子W相线圈温度","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅲ-017 发电机定子W相线圈温度","yc_hs_0486","cur_79"]
[5107,"d_古交一期Ⅲ-017 舱内温度","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅲ-017 舱内温度","yc_hs_0487","cur_33"]
[5108,"d_古交一期Ⅲ-017 舱外温度","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅲ-017 舱外温度","yc_hs_0487","cur_34"]
[5109,"d_古交一期Ⅲ-017 风向","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅲ-017 风向","yc_hs_0487","cur_35"]
[5110,"d_古交一期Ⅲ-017 机舱角度（位置）","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅲ-017 机舱角度（位置）","yc_hs_0487","cur_37"]
[5111,"d_古交一期Ⅲ-017 偏航角度(扭缆角度）","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅲ-017 偏航角度(扭缆角度）","yc_hs_0487","cur_38"]
[5112,"d_古交一期Ⅲ-017 机舱与风向夹角","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅲ-017 机舱与风向夹角","yc_hs_0487","cur_39"]
[5113,"d_古交一期Ⅱ-009 主轴承外圈温度","古交风电场","WOF35100073",9,"SXGJ.T1_L2.WTG009.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅱ-009 主轴承外圈温度","yc_hs_0487","cur_40"]
[5114,"d_古交一期Ⅱ-015 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅱ-015 机舱侧向振动值(已滤波)","yc_hs_0487","cur_44"]
[5115,"d_古交一期Ⅱ-015 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅱ-015 机舱轴向振动值(已滤波)","yc_hs_0487","cur_46"]
[5116,"d_古交一期Ⅱ-015 风速","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅱ-015 风速","yc_hs_0487","cur_47"]
[5117,"d_古交一期Ⅱ-015 发电机有功功率","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅱ-015 发电机有功功率","yc_hs_0487","cur_48"]
[5118,"d_古交一期Ⅱ-015 发电机转速","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅱ-015 发电机转速","yc_hs_0487","cur_50"]
[5119,"d_古交一期Ⅱ-015 发电机驱动端轴承温度","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅱ-015 发电机驱动端轴承温度","yc_hs_0487","cur_51"]
[5120,"d_古交一期Ⅱ-015 发电机非驱动端轴承温度","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅱ-015 发电机非驱动端轴承温度","yc_hs_0487","cur_52"]
[5121,"d_古交一期Ⅱ-015 发电机定子U相线圈温度","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅱ-015 发电机定子U相线圈温度","yc_hs_0487","cur_53"]
[5122,"d_古交一期Ⅱ-015 发电机定子V相线圈温度","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅱ-015 发电机定子V相线圈温度","yc_hs_0487","cur_54"]
[5123,"d_古交一期Ⅱ-015 发电机定子W相线圈温度","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅱ-015 发电机定子W相线圈温度","yc_hs_0487","cur_55"]
[5124,"d_古交一期Ⅱ-015 舱内温度","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅱ-015 舱内温度","yc_hs_0487","cur_67"]
[5125,"d_古交一期Ⅱ-015 舱外温度","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅱ-015 舱外温度","yc_hs_0487","cur_100"]
[5126,"d_古交一期Ⅱ-015 风向","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅱ-015 风向","yc_hs_0488","cur_01"]
[5127,"d_古交一期Ⅱ-015 机舱角度（位置）","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅱ-015 机舱角度（位置）","yc_hs_0488","cur_03"]
[5128,"d_古交一期Ⅱ-015 偏航角度(扭缆角度）","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅱ-015 偏航角度(扭缆角度）","yc_hs_0488","cur_04"]
[5129,"d_古交一期Ⅱ-015 机舱与风向夹角","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WNAC.WindVaneDirection","对风角度","yaw_error1","d_古交一期Ⅱ-015 机舱与风向夹角","yc_hs_0488","cur_05"]
[5130,"d_古交一期Ⅱ-015 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅱ-015 1#桨叶片角度(桨距角)","yc_hs_0488","cur_06"]
[5131,"d_古交一期Ⅱ-015 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅱ-015 2#桨叶片角度(桨距角)","yc_hs_0488","cur_07"]
[5132,"d_古交一期Ⅱ-015 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",15,"SXGJ.T1_L2.WTG015.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅱ-015 3#桨叶片角度(桨距角)","yc_hs_0488","cur_08"]
[5133,"d_古交一期Ⅲ-017 1#桨叶片角度(桨距角)","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","d_古交一期Ⅲ-017 1#桨叶片角度(桨距角)","yc_hs_0488","cur_15"]
[5134,"d_古交一期Ⅲ-017 2#桨叶片角度(桨距角)","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","d_古交一期Ⅲ-017 2#桨叶片角度(桨距角)","yc_hs_0488","cur_16"]
[5135,"d_古交一期Ⅲ-017 3#桨叶片角度(桨距角)","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","d_古交一期Ⅲ-017 3#桨叶片角度(桨距角)","yc_hs_0488","cur_17"]
[5136,"d_古交一期Ⅲ-023 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅲ-023 机舱侧向振动值(已滤波)","yc_hs_0488","cur_24"]
[5137,"d_古交一期Ⅲ-023 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅲ-023 机舱轴向振动值(已滤波)","yc_hs_0488","cur_26"]
[5138,"d_古交一期Ⅲ-023 风速","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅲ-023 风速","yc_hs_0488","cur_27"]
[5139,"d_古交一期Ⅲ-023 发电机有功功率","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅲ-023 发电机有功功率","yc_hs_0488","cur_28"]
[5140,"d_古交一期Ⅲ-023 发电机转速","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅲ-023 发电机转速","yc_hs_0488","cur_30"]
[5141,"d_古交一期Ⅲ-023 发电机驱动端轴承温度","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅲ-023 发电机驱动端轴承温度","yc_hs_0488","cur_31"]
[5142,"d_古交一期Ⅲ-023 发电机非驱动端轴承温度","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅲ-023 发电机非驱动端轴承温度","yc_hs_0488","cur_32"]
[5143,"d_古交一期Ⅲ-023 发电机定子U相线圈温度","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅲ-023 发电机定子U相线圈温度","yc_hs_0488","cur_33"]
[5144,"d_古交一期Ⅲ-023 发电机定子V相线圈温度","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅲ-023 发电机定子V相线圈温度","yc_hs_0488","cur_34"]
[5145,"d_古交一期Ⅲ-023 发电机定子W相线圈温度","古交风电场","WOF35100073",23,"SXGJ.T1_L3.WTG023.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅲ-023 发电机定子W相线圈温度","yc_hs_0488","cur_35"]
[5146,"d_古交一期Ⅰ-006 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅰ-006 机舱侧向振动值(已滤波)","yc_hs_0356","cur_86"]
[5147,"d_古交一期Ⅰ-006 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅰ-006 机舱轴向振动值(已滤波)","yc_hs_0356","cur_88"]
[5148,"d_古交一期Ⅰ-006 风速","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅰ-006 风速","yc_hs_0356","cur_89"]
[5149,"d_古交一期Ⅰ-006 发电机有功功率","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅰ-006 发电机有功功率","yc_hs_0356","cur_90"]
[5150,"d_古交一期Ⅰ-006 发电机转速","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅰ-006 发电机转速","yc_hs_0356","cur_92"]
[5151,"d_古交一期Ⅰ-006 发电机驱动端轴承温度","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅰ-006 发电机驱动端轴承温度","yc_hs_0356","cur_93"]
[5152,"d_古交一期Ⅰ-006 发电机非驱动端轴承温度","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅰ-006 发电机非驱动端轴承温度","yc_hs_0356","cur_94"]
[5153,"d_古交一期Ⅰ-006 发电机定子U相线圈温度","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅰ-006 发电机定子U相线圈温度","yc_hs_0356","cur_95"]
[5154,"d_古交一期Ⅰ-006 发电机定子V相线圈温度","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅰ-006 发电机定子V相线圈温度","yc_hs_0356","cur_96"]
[5155,"d_古交一期Ⅰ-006 发电机定子W相线圈温度","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅰ-006 发电机定子W相线圈温度","yc_hs_0356","cur_97"]
[5156,"d_古交一期Ⅲ-021 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅲ-021 机舱侧向振动值(已滤波)","yc_hs_0357","cur_04"]
[5157,"d_古交一期Ⅲ-021 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅲ-021 机舱轴向振动值(已滤波)","yc_hs_0357","cur_06"]
[5158,"d_古交一期Ⅲ-021 风速","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅲ-021 风速","yc_hs_0357","cur_07"]
[5159,"d_古交一期Ⅲ-021 发电机有功功率","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅲ-021 发电机有功功率","yc_hs_0357","cur_08"]
[5160,"d_古交一期Ⅲ-021 发电机转速","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WGEN.GenSpd","发电机转速","generator_speed","d_古交一期Ⅲ-021 发电机转速","yc_hs_0357","cur_10"]
[5161,"d_古交一期Ⅲ-021 发电机驱动端轴承温度","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","d_古交一期Ⅲ-021 发电机驱动端轴承温度","yc_hs_0357","cur_11"]
[5162,"d_古交一期Ⅲ-021 发电机非驱动端轴承温度","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","d_古交一期Ⅲ-021 发电机非驱动端轴承温度","yc_hs_0357","cur_12"]
[5163,"d_古交一期Ⅲ-021 发电机定子U相线圈温度","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","d_古交一期Ⅲ-021 发电机定子U相线圈温度","yc_hs_0357","cur_13"]
[5164,"d_古交一期Ⅲ-021 发电机定子V相线圈温度","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","d_古交一期Ⅲ-021 发电机定子V相线圈温度","yc_hs_0357","cur_14"]
[5165,"d_古交一期Ⅲ-021 发电机定子W相线圈温度","古交风电场","WOF35100073",21,"SXGJ.T1_L3.WTG021.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","d_古交一期Ⅲ-021 发电机定子W相线圈温度","yc_hs_0357","cur_15"]
[5166,"d_古交一期Ⅰ-006 舱内温度","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WNAC.TemNacelle","机舱内温度","cabin_temperature","d_古交一期Ⅰ-006 舱内温度","yc_hs_0357","cur_41"]
[5167,"d_古交一期Ⅰ-006 舱外温度","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WNAC.TemOut","环境温度","outside_cabin_temperature","d_古交一期Ⅰ-006 舱外温度","yc_hs_0357","cur_42"]
[5168,"d_古交一期Ⅱ-011 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅱ-011 齿轮箱高速轴非驱动端轴承温度","yc_hs_0357","cur_43"]
[5169,"d_古交一期Ⅱ-011 齿轮箱油池温度","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅱ-011 齿轮箱油池温度","yc_hs_0357","cur_44"]
[5170,"d_古交一期Ⅱ-011 主轴承外圈温度","古交风电场","WOF35100073",11,"SXGJ.T1_L2.WTG011.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅱ-011 主轴承外圈温度","yc_hs_0357","cur_45"]
[5171,"d_古交一期Ⅱ-012 机舱侧向振动值(已滤波)","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","d_古交一期Ⅱ-012 机舱侧向振动值(已滤波)","yc_hs_0357","cur_53"]
[5172,"d_古交一期Ⅱ-012 机舱轴向振动值(已滤波)","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","d_古交一期Ⅱ-012 机舱轴向振动值(已滤波)","yc_hs_0357","cur_55"]
[5173,"d_古交一期Ⅱ-012 风速","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WNAC.WindSpeed","风速","wind_velocity","d_古交一期Ⅱ-012 风速","yc_hs_0357","cur_56"]
[5174,"d_古交一期Ⅱ-012 发电机有功功率","古交风电场","WOF35100073",12,"SXGJ.T1_L2.WTG012.WGEN.GenActivePW","有功功率","active_power","d_古交一期Ⅱ-012 发电机有功功率","yc_hs_0357","cur_57"]
[5175,"d_古交一期Ⅲ-017 主轴转速","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WTRM.RotorSpd","风轮转速","rotor_speed","d_古交一期Ⅲ-017 主轴转速","yc_hs_0358","cur_49"]
[5176,"d_古交一期Ⅲ-017 齿轮箱高速轴非驱动端轴承温度","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","d_古交一期Ⅲ-017 齿轮箱高速轴非驱动端轴承温度","yc_hs_0358","cur_51"]
[5177,"d_古交一期Ⅲ-017 齿轮箱油池温度","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","d_古交一期Ⅲ-017 齿轮箱油池温度","yc_hs_0358","cur_52"]
[5178,"d_古交一期Ⅲ-017 主轴承外圈温度","古交风电场","WOF35100073",17,"SXGJ.T1_L3.WTG017.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","d_古交一期Ⅲ-017 主轴承外圈温度","yc_hs_0358","cur_53"]
[5179,"d_古交一期Ⅰ-006 风向","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WNAC.WindDirection","绝对风向","true_wind_direction","d_古交一期Ⅰ-006 风向","yc_hs_0358","cur_58"]
[5180,"d_古交一期Ⅰ-006 机舱角度（位置）","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WYAW.NacellePosition","机舱位置","cabin_position","d_古交一期Ⅰ-006 机舱角度（位置）","yc_hs_0358","cur_60"]
[5181,"d_古交一期Ⅰ-006 偏航角度(扭缆角度）","古交风电场","WOF35100073",6,"SXGJ.T1_L1.WTG006.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","d_古交一期Ⅰ-006 偏航角度(扭缆角度）","yc_hs_0358","cur_61"]
[5182,"e_石楼一期Ⅰ-003 舱内温度","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅰ-003 舱内温度","yc_hs_0490","cur_01"]
[5183,"e_石楼一期Ⅰ-003 舱外温度","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅰ-003 舱外温度","yc_hs_0490","cur_04"]
[5184,"e_石楼一期Ⅰ-003 偏航角度(扭缆角度）","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅰ-003 偏航角度(扭缆角度）","yc_hs_0490","cur_05"]
[5185,"e_石楼一期Ⅰ-003 风向","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅰ-003 风向","yc_hs_0232","cur_84"]
[5186,"e_石楼一期Ⅰ-003 风速","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅰ-003 风速","yc_hs_0490","cur_06"]
[5187,"e_石楼一期Ⅰ-003 机舱中轴线与风向夹角","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅰ-003 机舱中轴线与风向夹角","yc_hs_0490","cur_07"]
[5188,"e_石楼一期Ⅰ-003 1#桨叶片角度","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅰ-003 1#桨叶片角度","yc_hs_0232","cur_85"]
[5189,"e_石楼一期Ⅰ-003 2#桨叶片角度","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅰ-003 2#桨叶片角度","yc_hs_0232","cur_86"]
[5190,"e_石楼一期Ⅰ-003 3#桨叶片角度","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅰ-003 3#桨叶片角度","yc_hs_0232","cur_87"]
[5191,"e_石楼一期Ⅰ-003 主轴转速","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅰ-003 主轴转速","yc_hs_0490","cur_08"]
[5192,"e_石楼一期Ⅰ-003 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅰ-003 机舱轴向振动(已滤波)","yc_hs_0490","cur_10"]
[5193,"e_石楼一期Ⅰ-004 发电机有功功率","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅰ-004 发电机有功功率","yc_hs_0490","cur_12"]
[5194,"e_石楼一期Ⅰ-004 发电机 绕组温度1","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅰ-004 发电机 绕组温度1","yc_hs_0233","cur_12"]
[5195,"e_石楼一期Ⅰ-004 发电机 绕组温度2","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅰ-004 发电机 绕组温度2","yc_hs_0233","cur_13"]
[5196,"e_石楼一期Ⅰ-004 发电机 绕组温度3","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅰ-004 发电机 绕组温度3","yc_hs_0233","cur_14"]
[5197,"e_石楼一期Ⅰ-001 发电机有功功率","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅰ-001 发电机有功功率","yc_hs_0490","cur_68"]
[5198,"e_石楼一期Ⅰ-001 发电机 绕组温度1","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅰ-001 发电机 绕组温度1","yc_hs_0232","cur_10"]
[5199,"e_石楼一期Ⅰ-001 发电机 绕组温度2","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅰ-001 发电机 绕组温度2","yc_hs_0232","cur_11"]
[5200,"e_石楼一期Ⅰ-001 发电机 绕组温度3","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅰ-001 发电机 绕组温度3","yc_hs_0232","cur_12"]
[5201,"e_石楼一期Ⅰ-001 发电机转速","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅰ-001 发电机转速","yc_hs_0491","cur_33"]
[5202,"e_石楼一期Ⅰ-001 舱内温度","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅰ-001 舱内温度","yc_hs_0491","cur_34"]
[5203,"e_石楼一期Ⅰ-001 舱外温度","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅰ-001 舱外温度","yc_hs_0491","cur_37"]
[5204,"e_石楼一期Ⅰ-001 偏航角度(扭缆角度）","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅰ-001 偏航角度(扭缆角度）","yc_hs_0491","cur_38"]
[5205,"e_石楼一期Ⅰ-001 风向","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅰ-001 风向","yc_hs_0232","cur_16"]
[5206,"e_石楼一期Ⅰ-001 风速","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅰ-001 风速","yc_hs_0491","cur_39"]
[5207,"e_石楼一期Ⅰ-001 机舱中轴线与风向夹角","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅰ-001 机舱中轴线与风向夹角","yc_hs_0491","cur_40"]
[5208,"e_石楼一期Ⅰ-001 1#桨叶片角度","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅰ-001 1#桨叶片角度","yc_hs_0232","cur_17"]
[5209,"e_石楼一期Ⅰ-001 2#桨叶片角度","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅰ-001 2#桨叶片角度","yc_hs_0232","cur_18"]
[5210,"e_石楼一期Ⅰ-001 3#桨叶片角度","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅰ-001 3#桨叶片角度","yc_hs_0232","cur_19"]
[5211,"e_石楼一期Ⅰ-001 主轴转速","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅰ-001 主轴转速","yc_hs_0491","cur_41"]
[5212,"e_石楼一期Ⅰ-001 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",1,"SLRY.T1_L1.WTG001.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅰ-001 机舱轴向振动(已滤波)","yc_hs_0491","cur_43"]
[5213,"e_石楼一期Ⅰ-002 发电机有功功率","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅰ-002 发电机有功功率","yc_hs_0491","cur_44"]
[5214,"e_石楼一期Ⅰ-002 发电机 绕组温度1","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅰ-002 发电机 绕组温度1","yc_hs_0232","cur_44"]
[5215,"e_石楼一期Ⅰ-002 发电机 绕组温度2","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅰ-002 发电机 绕组温度2","yc_hs_0232","cur_45"]
[5216,"e_石楼一期Ⅰ-002 发电机 绕组温度3","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅰ-002 发电机 绕组温度3","yc_hs_0232","cur_46"]
[5217,"e_石楼一期Ⅰ-002 发电机转速","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅰ-002 发电机转速","yc_hs_0490","cur_70"]
[5218,"e_石楼一期Ⅰ-002 舱内温度","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅰ-002 舱内温度","yc_hs_0490","cur_71"]
[5219,"e_石楼一期Ⅰ-002 舱外温度","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅰ-002 舱外温度","yc_hs_0490","cur_74"]
[5220,"e_石楼一期Ⅰ-002 偏航角度(扭缆角度）","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅰ-002 偏航角度(扭缆角度）","yc_hs_0490","cur_75"]
[5221,"e_石楼一期Ⅰ-002 风向","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅰ-002 风向","yc_hs_0232","cur_50"]
[5222,"e_石楼一期Ⅰ-002 风速","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅰ-002 风速","yc_hs_0490","cur_76"]
[5223,"e_石楼一期Ⅰ-002 机舱中轴线与风向夹角","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅰ-002 机舱中轴线与风向夹角","yc_hs_0490","cur_77"]
[5224,"e_石楼一期Ⅰ-002 1#桨叶片角度","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅰ-002 1#桨叶片角度","yc_hs_0232","cur_51"]
[5225,"e_石楼一期Ⅰ-002 2#桨叶片角度","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅰ-002 2#桨叶片角度","yc_hs_0232","cur_52"]
[5226,"e_石楼一期Ⅰ-002 3#桨叶片角度","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅰ-002 3#桨叶片角度","yc_hs_0232","cur_53"]
[5227,"e_石楼一期Ⅰ-002 主轴转速","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅰ-002 主轴转速","yc_hs_0490","cur_78"]
[5228,"e_石楼一期Ⅰ-002 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",2,"SLRY.T1_L1.WTG002.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅰ-002 机舱轴向振动(已滤波)","yc_hs_0490","cur_80"]
[5229,"e_石楼一期Ⅰ-003 发电机有功功率","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅰ-003 发电机有功功率","yc_hs_0490","cur_81"]
[5230,"e_石楼一期Ⅰ-003 发电机 绕组温度1","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅰ-003 发电机 绕组温度1","yc_hs_0232","cur_78"]
[5231,"e_石楼一期Ⅰ-003 发电机 绕组温度2","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅰ-003 发电机 绕组温度2","yc_hs_0232","cur_79"]
[5232,"e_石楼一期Ⅰ-003 发电机 绕组温度3","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅰ-003 发电机 绕组温度3","yc_hs_0232","cur_80"]
[5233,"e_石楼一期Ⅰ-003 发电机转速","石楼风电场","WOF35800081",3,"SLRY.T1_L1.WTG003.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅰ-003 发电机转速","yc_hs_0490","cur_94"]
[5234,"e_石楼一期Ⅱ-020 发电机 绕组温度3","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅱ-020 发电机 绕组温度3","yc_hs_0238","cur_58"]
[5235,"e_石楼一期Ⅱ-020 发电机转速","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅱ-020 发电机转速","yc_hs_0490","cur_95"]
[5236,"e_石楼一期Ⅱ-020 舱内温度","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅱ-020 舱内温度","yc_hs_0490","cur_96"]
[5237,"e_石楼一期Ⅱ-020 舱外温度","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅱ-020 舱外温度","yc_hs_0490","cur_99"]
[5238,"e_石楼一期Ⅱ-020 偏航角度(扭缆角度）","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅱ-020 偏航角度(扭缆角度）","yc_hs_0490","cur_100"]
[5239,"e_石楼一期Ⅱ-020 风向","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅱ-020 风向","yc_hs_0238","cur_62"]
[5240,"e_石楼一期Ⅱ-020 风速","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅱ-020 风速","yc_hs_0491","cur_01"]
[5241,"e_石楼一期Ⅱ-020 机舱中轴线与风向夹角","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅱ-020 机舱中轴线与风向夹角","yc_hs_0491","cur_02"]
[5242,"e_石楼一期Ⅱ-020 1#桨叶片角度","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅱ-020 1#桨叶片角度","yc_hs_0238","cur_63"]
[5243,"e_石楼一期Ⅱ-020 2#桨叶片角度","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅱ-020 2#桨叶片角度","yc_hs_0238","cur_64"]
[5244,"e_石楼一期Ⅱ-020 3#桨叶片角度","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅱ-020 3#桨叶片角度","yc_hs_0238","cur_65"]
[5245,"e_石楼一期Ⅱ-020 主轴转速","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅱ-020 主轴转速","yc_hs_0491","cur_03"]
[5246,"e_石楼一期Ⅱ-020 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅱ-020 机舱轴向振动(已滤波)","yc_hs_0491","cur_05"]
[5247,"e_石楼一期Ⅱ-021 发电机有功功率","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅱ-021 发电机有功功率","yc_hs_0491","cur_06"]
[5248,"e_石楼一期Ⅰ-005 发电机 绕组温度3","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅰ-005 发电机 绕组温度3","yc_hs_0233","cur_48"]
[5249,"e_石楼一期Ⅰ-005 发电机转速","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅰ-005 发电机转速","yc_hs_0491","cur_08"]
[5250,"e_石楼一期Ⅰ-005 舱内温度","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅰ-005 舱内温度","yc_hs_0491","cur_09"]
[5251,"e_石楼一期Ⅰ-005 舱外温度","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅰ-005 舱外温度","yc_hs_0491","cur_12"]
[5252,"e_石楼一期Ⅰ-005 偏航角度(扭缆角度）","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅰ-005 偏航角度(扭缆角度）","yc_hs_0491","cur_13"]
[5253,"e_石楼一期Ⅰ-005 风向","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅰ-005 风向","yc_hs_0233","cur_52"]
[5254,"e_石楼一期Ⅰ-005 风速","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅰ-005 风速","yc_hs_0491","cur_14"]
[5255,"e_石楼一期Ⅰ-005 机舱中轴线与风向夹角","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅰ-005 机舱中轴线与风向夹角","yc_hs_0491","cur_15"]
[5256,"e_石楼一期Ⅰ-005 1#桨叶片角度","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅰ-005 1#桨叶片角度","yc_hs_0233","cur_53"]
[5257,"e_石楼一期Ⅰ-005 2#桨叶片角度","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅰ-005 2#桨叶片角度","yc_hs_0233","cur_54"]
[5258,"e_石楼一期Ⅰ-005 3#桨叶片角度","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅰ-005 3#桨叶片角度","yc_hs_0233","cur_55"]
[5259,"e_石楼一期Ⅰ-005 主轴转速","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅰ-005 主轴转速","yc_hs_0491","cur_16"]
[5260,"e_石楼一期Ⅰ-005 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅰ-005 机舱轴向振动(已滤波)","yc_hs_0491","cur_18"]
[5261,"e_石楼一期Ⅰ-006 发电机有功功率","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅰ-006 发电机有功功率","yc_hs_0491","cur_46"]
[5262,"e_石楼一期Ⅱ-021 发电机 绕组温度1","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅱ-021 发电机 绕组温度1","yc_hs_0238","cur_90"]
[5263,"e_石楼一期Ⅱ-021 发电机 绕组温度2","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅱ-021 发电机 绕组温度2","yc_hs_0238","cur_91"]
[5264,"e_石楼一期Ⅱ-021 发电机 绕组温度3","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅱ-021 发电机 绕组温度3","yc_hs_0238","cur_92"]
[5265,"e_石楼一期Ⅱ-021 发电机转速","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅱ-021 发电机转速","yc_hs_0491","cur_48"]
[5266,"e_石楼一期Ⅱ-021 舱内温度","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅱ-021 舱内温度","yc_hs_0491","cur_49"]
[5267,"e_石楼一期Ⅱ-021 舱外温度","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅱ-021 舱外温度","yc_hs_0491","cur_52"]
[5268,"e_石楼一期Ⅱ-021 偏航角度(扭缆角度）","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅱ-021 偏航角度(扭缆角度）","yc_hs_0491","cur_53"]
[5269,"e_石楼一期Ⅱ-021 风向","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅱ-021 风向","yc_hs_0238","cur_96"]
[5270,"e_石楼一期Ⅱ-021 风速","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅱ-021 风速","yc_hs_0491","cur_54"]
[5271,"e_石楼一期Ⅱ-021 机舱中轴线与风向夹角","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅱ-021 机舱中轴线与风向夹角","yc_hs_0491","cur_55"]
[5272,"e_石楼一期Ⅱ-021 1#桨叶片角度","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅱ-021 1#桨叶片角度","yc_hs_0238","cur_97"]
[5273,"e_石楼一期Ⅱ-021 2#桨叶片角度","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅱ-021 2#桨叶片角度","yc_hs_0238","cur_98"]
[5274,"e_石楼一期Ⅱ-021 3#桨叶片角度","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅱ-021 3#桨叶片角度","yc_hs_0238","cur_99"]
[5275,"e_石楼一期Ⅱ-021 主轴转速","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅱ-021 主轴转速","yc_hs_0491","cur_56"]
[5276,"e_石楼一期Ⅱ-021 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",21,"SLRY.T1_L2.WTG021.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅱ-021 机舱轴向振动(已滤波)","yc_hs_0491","cur_58"]
[5277,"e_石楼一期Ⅰ-006 发电机 绕组温度1","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅰ-006 发电机 绕组温度1","yc_hs_0233","cur_80"]
[5278,"e_石楼一期Ⅰ-006 发电机 绕组温度2","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅰ-006 发电机 绕组温度2","yc_hs_0233","cur_81"]
[5279,"e_石楼一期Ⅰ-006 发电机 绕组温度3","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅰ-006 发电机 绕组温度3","yc_hs_0233","cur_82"]
[5280,"e_石楼一期Ⅰ-006 发电机转速","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅰ-006 发电机转速","yc_hs_0490","cur_83"]
[5281,"e_石楼一期Ⅰ-006 舱内温度","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅰ-006 舱内温度","yc_hs_0490","cur_84"]
[5282,"e_石楼一期Ⅰ-006 舱外温度","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅰ-006 舱外温度","yc_hs_0490","cur_87"]
[5283,"e_石楼一期Ⅰ-006 偏航角度(扭缆角度）","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅰ-006 偏航角度(扭缆角度）","yc_hs_0490","cur_88"]
[5284,"e_石楼一期Ⅰ-006 风向","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅰ-006 风向","yc_hs_0233","cur_86"]
[5285,"e_石楼一期Ⅰ-006 风速","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅰ-006 风速","yc_hs_0490","cur_89"]
[5286,"e_石楼一期Ⅰ-006 机舱中轴线与风向夹角","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅰ-006 机舱中轴线与风向夹角","yc_hs_0490","cur_90"]
[5287,"e_石楼一期Ⅰ-006 1#桨叶片角度","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅰ-006 1#桨叶片角度","yc_hs_0233","cur_87"]
[5288,"e_石楼一期Ⅰ-006 2#桨叶片角度","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅰ-006 2#桨叶片角度","yc_hs_0233","cur_88"]
[5289,"e_石楼一期Ⅰ-006 3#桨叶片角度","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅰ-006 3#桨叶片角度","yc_hs_0233","cur_89"]
[5290,"e_石楼一期Ⅰ-006 主轴转速","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅰ-006 主轴转速","yc_hs_0490","cur_91"]
[5291,"e_石楼一期Ⅰ-006 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",6,"SLRY.T1_L1.WTG006.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅰ-006 机舱轴向振动(已滤波)","yc_hs_0490","cur_93"]
[5292,"e_石楼一期Ⅰ-010 发电机有功功率","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅰ-010 发电机有功功率","yc_hs_0491","cur_19"]
[5293,"e_石楼一期Ⅱ-022 发电机有功功率","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅱ-022 发电机有功功率","yc_hs_0491","cur_20"]
[5294,"e_石楼一期Ⅱ-022 发电机 绕组温度1","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅱ-022 发电机 绕组温度1","yc_hs_0239","cur_24"]
[5295,"e_石楼一期Ⅱ-022 发电机 绕组温度2","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅱ-022 发电机 绕组温度2","yc_hs_0239","cur_25"]
[5296,"e_石楼一期Ⅱ-022 发电机 绕组温度3","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅱ-022 发电机 绕组温度3","yc_hs_0239","cur_26"]
[5297,"e_石楼一期Ⅱ-022 发电机转速","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅱ-022 发电机转速","yc_hs_0491","cur_22"]
[5298,"e_石楼一期Ⅱ-022 舱内温度","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅱ-022 舱内温度","yc_hs_0491","cur_23"]
[5299,"e_石楼一期Ⅱ-022 舱外温度","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅱ-022 舱外温度","yc_hs_0491","cur_26"]
[5300,"e_石楼一期Ⅱ-022 偏航角度(扭缆角度）","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅱ-022 偏航角度(扭缆角度）","yc_hs_0491","cur_27"]
[5301,"e_石楼一期Ⅱ-022 风向","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅱ-022 风向","yc_hs_0239","cur_30"]
[5302,"e_石楼一期Ⅱ-022 风速","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅱ-022 风速","yc_hs_0491","cur_28"]
[5303,"e_石楼一期Ⅱ-022 机舱中轴线与风向夹角","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅱ-022 机舱中轴线与风向夹角","yc_hs_0491","cur_29"]
[5304,"e_石楼一期Ⅱ-022 1#桨叶片角度","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅱ-022 1#桨叶片角度","yc_hs_0239","cur_31"]
[5305,"e_石楼一期Ⅱ-022 2#桨叶片角度","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅱ-022 2#桨叶片角度","yc_hs_0239","cur_32"]
[5306,"e_石楼一期Ⅱ-022 3#桨叶片角度","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅱ-022 3#桨叶片角度","yc_hs_0239","cur_33"]
[5307,"e_石楼一期Ⅱ-022 主轴转速","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅱ-022 主轴转速","yc_hs_0491","cur_30"]
[5308,"e_石楼一期Ⅱ-022 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",22,"SLRY.T1_L2.WTG022.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅱ-022 机舱轴向振动(已滤波)","yc_hs_0491","cur_32"]
[5309,"e_石楼一期Ⅰ-010 发电机 绕组温度1","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅰ-010 发电机 绕组温度1","yc_hs_0234","cur_14"]
[5310,"e_石楼一期Ⅰ-010 发电机 绕组温度2","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅰ-010 发电机 绕组温度2","yc_hs_0234","cur_15"]
[5311,"e_石楼一期Ⅰ-010 发电机 绕组温度3","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅰ-010 发电机 绕组温度3","yc_hs_0234","cur_16"]
[5312,"e_石楼一期Ⅰ-010 发电机转速","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅰ-010 发电机转速","yc_hs_0493","cur_56"]
[5313,"e_石楼一期Ⅰ-010 舱内温度","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅰ-010 舱内温度","yc_hs_0493","cur_57"]
[5314,"e_石楼一期Ⅰ-010 舱外温度","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅰ-010 舱外温度","yc_hs_0493","cur_60"]
[5315,"e_石楼一期Ⅰ-010 偏航角度(扭缆角度）","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅰ-010 偏航角度(扭缆角度）","yc_hs_0493","cur_61"]
[5316,"e_石楼一期Ⅰ-010 风向","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅰ-010 风向","yc_hs_0234","cur_20"]
[5317,"e_石楼一期Ⅰ-010 风速","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅰ-010 风速","yc_hs_0493","cur_62"]
[5318,"e_石楼一期Ⅰ-010 机舱中轴线与风向夹角","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅰ-010 机舱中轴线与风向夹角","yc_hs_0493","cur_63"]
[5319,"e_石楼一期Ⅰ-010 1#桨叶片角度","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅰ-010 1#桨叶片角度","yc_hs_0234","cur_21"]
[5320,"e_石楼一期Ⅰ-010 2#桨叶片角度","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅰ-010 2#桨叶片角度","yc_hs_0234","cur_22"]
[5321,"e_石楼一期Ⅰ-010 3#桨叶片角度","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅰ-010 3#桨叶片角度","yc_hs_0234","cur_23"]
[5322,"e_石楼一期Ⅰ-010 主轴转速","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅰ-010 主轴转速","yc_hs_0493","cur_64"]
[5323,"e_石楼一期Ⅰ-010 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",10,"SLRY.T1_L1.WTG010.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅰ-010 机舱轴向振动(已滤波)","yc_hs_0493","cur_66"]
[5324,"e_石楼一期Ⅱ-023 发电机有功功率","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅱ-023 发电机有功功率","yc_hs_0491","cur_65"]
[5325,"e_石楼一期Ⅱ-023 发电机 绕组温度1","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅱ-023 发电机 绕组温度1","yc_hs_0239","cur_58"]
[5326,"e_石楼一期Ⅱ-023 发电机 绕组温度2","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅱ-023 发电机 绕组温度2","yc_hs_0239","cur_59"]
[5327,"e_石楼一期Ⅱ-023 发电机 绕组温度3","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅱ-023 发电机 绕组温度3","yc_hs_0239","cur_60"]
[5328,"e_石楼一期Ⅱ-023 发电机转速","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅱ-023 发电机转速","yc_hs_0491","cur_67"]
[5329,"e_石楼一期Ⅱ-023 舱内温度","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅱ-023 舱内温度","yc_hs_0491","cur_68"]
[5330,"e_石楼一期Ⅱ-023 舱外温度","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅱ-023 舱外温度","yc_hs_0491","cur_71"]
[5331,"e_石楼一期Ⅱ-023 偏航角度(扭缆角度）","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅱ-023 偏航角度(扭缆角度）","yc_hs_0491","cur_72"]
[5332,"e_石楼一期Ⅱ-023 风向","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅱ-023 风向","yc_hs_0239","cur_64"]
[5333,"e_石楼一期Ⅱ-023 风速","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅱ-023 风速","yc_hs_0491","cur_73"]
[5334,"e_石楼一期Ⅱ-023 机舱中轴线与风向夹角","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅱ-023 机舱中轴线与风向夹角","yc_hs_0491","cur_74"]
[5335,"e_石楼一期Ⅱ-023 1#桨叶片角度","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅱ-023 1#桨叶片角度","yc_hs_0239","cur_65"]
[5336,"e_石楼一期Ⅱ-023 2#桨叶片角度","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅱ-023 2#桨叶片角度","yc_hs_0239","cur_66"]
[5337,"e_石楼一期Ⅱ-023 3#桨叶片角度","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅱ-023 3#桨叶片角度","yc_hs_0239","cur_67"]
[5338,"e_石楼一期Ⅱ-023 主轴转速","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅱ-023 主轴转速","yc_hs_0491","cur_75"]
[5339,"e_石楼一期Ⅱ-023 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",23,"SLRY.T1_L2.WTG023.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅱ-023 机舱轴向振动(已滤波)","yc_hs_0491","cur_77"]
[5340,"e_石楼一期Ⅰ-011 发电机有功功率","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅰ-011 发电机有功功率","yc_hs_0491","cur_78"]
[5341,"e_石楼一期Ⅰ-011 发电机 绕组温度1","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅰ-011 发电机 绕组温度1","yc_hs_0234","cur_48"]
[5342,"e_石楼一期Ⅰ-011 发电机 绕组温度2","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅰ-011 发电机 绕组温度2","yc_hs_0234","cur_49"]
[5343,"e_石楼一期Ⅰ-011 发电机 绕组温度3","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅰ-011 发电机 绕组温度3","yc_hs_0234","cur_50"]
[5344,"e_石楼一期Ⅰ-011 发电机转速","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅰ-011 发电机转速","yc_hs_0491","cur_80"]
[5345,"e_石楼一期Ⅰ-011 舱内温度","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅰ-011 舱内温度","yc_hs_0491","cur_81"]
[5346,"e_石楼一期Ⅰ-011 舱外温度","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅰ-011 舱外温度","yc_hs_0491","cur_84"]
[5347,"e_石楼一期Ⅰ-011 偏航角度(扭缆角度）","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅰ-011 偏航角度(扭缆角度）","yc_hs_0491","cur_85"]
[5348,"e_石楼一期Ⅰ-011 风向","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅰ-011 风向","yc_hs_0234","cur_54"]
[5349,"e_石楼一期Ⅰ-011 风速","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅰ-011 风速","yc_hs_0491","cur_86"]
[5350,"e_石楼一期Ⅰ-011 机舱中轴线与风向夹角","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅰ-011 机舱中轴线与风向夹角","yc_hs_0491","cur_87"]
[5351,"e_石楼一期Ⅰ-011 1#桨叶片角度","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅰ-011 1#桨叶片角度","yc_hs_0234","cur_55"]
[5352,"e_石楼一期Ⅰ-011 2#桨叶片角度","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅰ-011 2#桨叶片角度","yc_hs_0234","cur_56"]
[5353,"e_石楼一期Ⅰ-011 3#桨叶片角度","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅰ-011 3#桨叶片角度","yc_hs_0234","cur_57"]
[5354,"e_石楼一期Ⅰ-011 主轴转速","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅰ-011 主轴转速","yc_hs_0491","cur_88"]
[5355,"e_石楼一期Ⅰ-011 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",11,"SLRY.T1_L1.WTG011.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅰ-011 机舱轴向振动(已滤波)","yc_hs_0491","cur_90"]
[5356,"e_石楼一期Ⅱ-024 发电机有功功率","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅱ-024 发电机有功功率","yc_hs_0491","cur_91"]
[5357,"e_石楼一期Ⅱ-024 发电机 绕组温度1","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅱ-024 发电机 绕组温度1","yc_hs_0239","cur_92"]
[5358,"e_石楼一期Ⅱ-024 发电机 绕组温度2","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅱ-024 发电机 绕组温度2","yc_hs_0239","cur_93"]
[5359,"e_石楼一期Ⅱ-024 发电机 绕组温度3","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅱ-024 发电机 绕组温度3","yc_hs_0239","cur_94"]
[5360,"e_石楼一期Ⅱ-024 发电机转速","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅱ-024 发电机转速","yc_hs_0491","cur_93"]
[5361,"e_石楼一期Ⅱ-024 舱内温度","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅱ-024 舱内温度","yc_hs_0491","cur_94"]
[5362,"e_石楼一期Ⅱ-024 舱外温度","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅱ-024 舱外温度","yc_hs_0491","cur_97"]
[5363,"e_石楼一期Ⅱ-024 偏航角度(扭缆角度）","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅱ-024 偏航角度(扭缆角度）","yc_hs_0491","cur_98"]
[5364,"e_石楼一期Ⅱ-024 风向","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅱ-024 风向","yc_hs_0239","cur_98"]
[5365,"e_石楼一期Ⅱ-024 风速","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅱ-024 风速","yc_hs_0491","cur_99"]
[5366,"e_石楼一期Ⅱ-024 机舱中轴线与风向夹角","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅱ-024 机舱中轴线与风向夹角","yc_hs_0491","cur_100"]
[5367,"e_石楼一期Ⅱ-024 1#桨叶片角度","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅱ-024 1#桨叶片角度","yc_hs_0239","cur_99"]
[5368,"e_石楼一期Ⅱ-024 2#桨叶片角度","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅱ-024 2#桨叶片角度","yc_hs_0239","cur_100"]
[5369,"e_石楼一期Ⅱ-024 3#桨叶片角度","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅱ-024 3#桨叶片角度","yc_hs_0240","cur_01"]
[5370,"e_石楼一期Ⅱ-024 主轴转速","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅱ-024 主轴转速","yc_hs_0492","cur_01"]
[5371,"e_石楼一期Ⅰ-012 发电机有功功率","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅰ-012 发电机有功功率","yc_hs_0492","cur_03"]
[5372,"e_石楼一期Ⅰ-012 发电机 绕组温度1","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅰ-012 发电机 绕组温度1","yc_hs_0234","cur_82"]
[5373,"e_石楼一期Ⅰ-012 发电机 绕组温度2","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅰ-012 发电机 绕组温度2","yc_hs_0234","cur_83"]
[5374,"e_石楼一期Ⅰ-012 发电机 绕组温度3","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅰ-012 发电机 绕组温度3","yc_hs_0234","cur_84"]
[5375,"e_石楼一期Ⅰ-012 发电机转速","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅰ-012 发电机转速","yc_hs_0492","cur_05"]
[5376,"e_石楼一期Ⅰ-012 舱内温度","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅰ-012 舱内温度","yc_hs_0492","cur_06"]
[5377,"e_石楼一期Ⅰ-012 舱外温度","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅰ-012 舱外温度","yc_hs_0492","cur_09"]
[5378,"e_石楼一期Ⅰ-012 偏航角度(扭缆角度）","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅰ-012 偏航角度(扭缆角度）","yc_hs_0492","cur_10"]
[5379,"e_石楼一期Ⅰ-012 风向","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅰ-012 风向","yc_hs_0234","cur_88"]
[5380,"e_石楼一期Ⅰ-012 风速","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅰ-012 风速","yc_hs_0492","cur_11"]
[5381,"e_石楼一期Ⅰ-012 机舱中轴线与风向夹角","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅰ-012 机舱中轴线与风向夹角","yc_hs_0492","cur_12"]
[5382,"e_石楼一期Ⅰ-012 1#桨叶片角度","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅰ-012 1#桨叶片角度","yc_hs_0234","cur_89"]
[5383,"e_石楼一期Ⅰ-012 2#桨叶片角度","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅰ-012 2#桨叶片角度","yc_hs_0234","cur_90"]
[5384,"e_石楼一期Ⅰ-012 3#桨叶片角度","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅰ-012 3#桨叶片角度","yc_hs_0234","cur_91"]
[5385,"e_石楼一期Ⅰ-012 主轴转速","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅰ-012 主轴转速","yc_hs_0492","cur_13"]
[5386,"e_石楼一期Ⅰ-012 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",12,"SLRY.T1_L1.WTG012.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅰ-012 机舱轴向振动(已滤波)","yc_hs_0492","cur_15"]
[5387,"e_石楼一期Ⅱ-024 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",24,"SLRY.T1_L2.WTG024.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅱ-024 机舱轴向振动(已滤波)","yc_hs_0492","cur_16"]
[5388,"e_石楼一期Ⅱ-025 发电机有功功率","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅱ-025 发电机有功功率","yc_hs_0492","cur_17"]
[5389,"e_石楼一期Ⅱ-025 发电机 绕组温度1","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅱ-025 发电机 绕组温度1","yc_hs_0240","cur_26"]
[5390,"e_石楼一期Ⅱ-025 发电机 绕组温度2","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅱ-025 发电机 绕组温度2","yc_hs_0240","cur_27"]
[5391,"e_石楼一期Ⅱ-025 发电机 绕组温度3","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅱ-025 发电机 绕组温度3","yc_hs_0240","cur_28"]
[5392,"e_石楼一期Ⅱ-025 发电机转速","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅱ-025 发电机转速","yc_hs_0492","cur_19"]
[5393,"e_石楼一期Ⅱ-025 舱内温度","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅱ-025 舱内温度","yc_hs_0492","cur_20"]
[5394,"e_石楼一期Ⅱ-025 舱外温度","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅱ-025 舱外温度","yc_hs_0492","cur_23"]
[5395,"e_石楼一期Ⅱ-025 偏航角度(扭缆角度）","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅱ-025 偏航角度(扭缆角度）","yc_hs_0492","cur_24"]
[5396,"e_石楼一期Ⅱ-025 风向","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅱ-025 风向","yc_hs_0240","cur_32"]
[5397,"e_石楼一期Ⅱ-025 风速","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅱ-025 风速","yc_hs_0492","cur_25"]
[5398,"e_石楼一期Ⅱ-025 机舱中轴线与风向夹角","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅱ-025 机舱中轴线与风向夹角","yc_hs_0492","cur_26"]
[5399,"e_石楼一期Ⅱ-025 1#桨叶片角度","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅱ-025 1#桨叶片角度","yc_hs_0240","cur_33"]
[5400,"e_石楼一期Ⅱ-025 2#桨叶片角度","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅱ-025 2#桨叶片角度","yc_hs_0240","cur_34"]
[5401,"e_石楼一期Ⅱ-025 3#桨叶片角度","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅱ-025 3#桨叶片角度","yc_hs_0240","cur_35"]
[5402,"e_石楼一期Ⅱ-025 主轴转速","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅱ-025 主轴转速","yc_hs_0492","cur_27"]
[5403,"e_石楼一期Ⅰ-013 发电机有功功率","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅰ-013 发电机有功功率","yc_hs_0492","cur_28"]
[5404,"e_石楼一期Ⅰ-013 发电机 绕组温度1","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅰ-013 发电机 绕组温度1","yc_hs_0235","cur_16"]
[5405,"e_石楼一期Ⅰ-013 发电机 绕组温度2","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅰ-013 发电机 绕组温度2","yc_hs_0235","cur_17"]
[5406,"e_石楼一期Ⅰ-013 发电机 绕组温度3","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅰ-013 发电机 绕组温度3","yc_hs_0235","cur_18"]
[5407,"e_石楼一期Ⅰ-013 发电机转速","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅰ-013 发电机转速","yc_hs_0492","cur_30"]
[5408,"e_石楼一期Ⅰ-013 舱内温度","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅰ-013 舱内温度","yc_hs_0492","cur_31"]
[5409,"e_石楼一期Ⅰ-013 舱外温度","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅰ-013 舱外温度","yc_hs_0492","cur_34"]
[5410,"e_石楼一期Ⅰ-013 偏航角度(扭缆角度）","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅰ-013 偏航角度(扭缆角度）","yc_hs_0492","cur_35"]
[5411,"e_石楼一期Ⅰ-013 风向","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅰ-013 风向","yc_hs_0235","cur_22"]
[5412,"e_石楼一期Ⅰ-013 风速","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅰ-013 风速","yc_hs_0492","cur_36"]
[5413,"e_石楼一期Ⅰ-013 机舱中轴线与风向夹角","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅰ-013 机舱中轴线与风向夹角","yc_hs_0492","cur_37"]
[5414,"e_石楼一期Ⅰ-013 1#桨叶片角度","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅰ-013 1#桨叶片角度","yc_hs_0235","cur_23"]
[5415,"e_石楼一期Ⅰ-013 2#桨叶片角度","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅰ-013 2#桨叶片角度","yc_hs_0235","cur_24"]
[5416,"e_石楼一期Ⅰ-013 3#桨叶片角度","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅰ-013 3#桨叶片角度","yc_hs_0235","cur_25"]
[5417,"e_石楼一期Ⅰ-013 主轴转速","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅰ-013 主轴转速","yc_hs_0492","cur_38"]
[5418,"e_石楼一期Ⅱ-025 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",25,"SLRY.T1_L2.WTG025.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅱ-025 机舱轴向振动(已滤波)","yc_hs_0492","cur_40"]
[5419,"e_石楼一期Ⅰ-013 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",13,"SLRY.T1_L1.WTG013.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅰ-013 机舱轴向振动(已滤波)","yc_hs_0492","cur_42"]
[5420,"e_石楼一期Ⅰ-014 发电机有功功率","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅰ-014 发电机有功功率","yc_hs_0492","cur_43"]
[5421,"e_石楼一期Ⅰ-014 发电机 绕组温度1","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅰ-014 发电机 绕组温度1","yc_hs_0235","cur_50"]
[5422,"e_石楼一期Ⅰ-014 发电机 绕组温度2","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅰ-014 发电机 绕组温度2","yc_hs_0235","cur_51"]
[5423,"e_石楼一期Ⅰ-014 发电机 绕组温度3","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅰ-014 发电机 绕组温度3","yc_hs_0235","cur_52"]
[5424,"e_石楼一期Ⅰ-014 发电机转速","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅰ-014 发电机转速","yc_hs_0492","cur_45"]
[5425,"e_石楼一期Ⅰ-014 舱内温度","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅰ-014 舱内温度","yc_hs_0492","cur_46"]
[5426,"e_石楼一期Ⅰ-014 舱外温度","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅰ-014 舱外温度","yc_hs_0492","cur_49"]
[5427,"e_石楼一期Ⅰ-014 偏航角度(扭缆角度）","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅰ-014 偏航角度(扭缆角度）","yc_hs_0492","cur_50"]
[5428,"e_石楼一期Ⅰ-014 风向","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅰ-014 风向","yc_hs_0235","cur_56"]
[5429,"e_石楼一期Ⅰ-014 风速","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅰ-014 风速","yc_hs_0492","cur_51"]
[5430,"e_石楼一期Ⅰ-014 机舱中轴线与风向夹角","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅰ-014 机舱中轴线与风向夹角","yc_hs_0492","cur_52"]
[5431,"e_石楼一期Ⅰ-014 1#桨叶片角度","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅰ-014 1#桨叶片角度","yc_hs_0235","cur_57"]
[5432,"e_石楼一期Ⅰ-014 2#桨叶片角度","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅰ-014 2#桨叶片角度","yc_hs_0235","cur_58"]
[5433,"e_石楼一期Ⅰ-014 3#桨叶片角度","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅰ-014 3#桨叶片角度","yc_hs_0235","cur_59"]
[5434,"e_石楼一期Ⅰ-014 主轴转速","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅰ-014 主轴转速","yc_hs_0492","cur_53"]
[5435,"e_石楼一期Ⅰ-014 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",14,"SLRY.T1_L1.WTG014.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅰ-014 机舱轴向振动(已滤波)","yc_hs_0492","cur_55"]
[5436,"e_石楼一期Ⅰ-015 发电机有功功率","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅰ-015 发电机有功功率","yc_hs_0492","cur_56"]
[5437,"e_石楼一期Ⅰ-015 发电机 绕组温度1","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅰ-015 发电机 绕组温度1","yc_hs_0235","cur_84"]
[5438,"e_石楼一期Ⅰ-015 发电机 绕组温度2","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅰ-015 发电机 绕组温度2","yc_hs_0235","cur_85"]
[5439,"e_石楼一期Ⅰ-015 发电机 绕组温度3","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅰ-015 发电机 绕组温度3","yc_hs_0235","cur_86"]
[5440,"e_石楼一期Ⅰ-015 发电机转速","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅰ-015 发电机转速","yc_hs_0492","cur_58"]
[5441,"e_石楼一期Ⅰ-015 舱内温度","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅰ-015 舱内温度","yc_hs_0492","cur_59"]
[5442,"e_石楼一期Ⅰ-015 舱外温度","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅰ-015 舱外温度","yc_hs_0492","cur_62"]
[5443,"e_石楼一期Ⅰ-015 偏航角度(扭缆角度）","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅰ-015 偏航角度(扭缆角度）","yc_hs_0492","cur_63"]
[5444,"e_石楼一期Ⅰ-015 风向","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅰ-015 风向","yc_hs_0235","cur_90"]
[5445,"e_石楼一期Ⅰ-015 风速","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅰ-015 风速","yc_hs_0492","cur_64"]
[5446,"e_石楼一期Ⅰ-015 机舱中轴线与风向夹角","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅰ-015 机舱中轴线与风向夹角","yc_hs_0492","cur_65"]
[5447,"e_石楼一期Ⅰ-015 1#桨叶片角度","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅰ-015 1#桨叶片角度","yc_hs_0235","cur_91"]
[5448,"e_石楼一期Ⅰ-015 2#桨叶片角度","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅰ-015 2#桨叶片角度","yc_hs_0235","cur_92"]
[5449,"e_石楼一期Ⅰ-015 3#桨叶片角度","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅰ-015 3#桨叶片角度","yc_hs_0235","cur_93"]
[5450,"e_石楼一期Ⅰ-015 主轴转速","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅰ-015 主轴转速","yc_hs_0492","cur_66"]
[5451,"e_石楼一期Ⅰ-015 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",15,"SLRY.T1_L1.WTG015.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅰ-015 机舱轴向振动(已滤波)","yc_hs_0492","cur_68"]
[5452,"e_石楼一期Ⅰ-016 发电机有功功率","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅰ-016 发电机有功功率","yc_hs_0492","cur_69"]
[5453,"e_石楼一期Ⅰ-016 发电机 绕组温度1","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅰ-016 发电机 绕组温度1","yc_hs_0236","cur_18"]
[5454,"e_石楼一期Ⅰ-016 发电机 绕组温度2","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅰ-016 发电机 绕组温度2","yc_hs_0236","cur_19"]
[5455,"e_石楼一期Ⅰ-016 发电机 绕组温度3","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅰ-016 发电机 绕组温度3","yc_hs_0236","cur_20"]
[5456,"e_石楼一期Ⅰ-016 发电机转速","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅰ-016 发电机转速","yc_hs_0492","cur_71"]
[5457,"e_石楼一期Ⅰ-016 舱内温度","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅰ-016 舱内温度","yc_hs_0492","cur_72"]
[5458,"e_石楼一期Ⅰ-016 舱外温度","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅰ-016 舱外温度","yc_hs_0492","cur_75"]
[5459,"e_石楼一期Ⅰ-016 偏航角度(扭缆角度）","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅰ-016 偏航角度(扭缆角度）","yc_hs_0492","cur_76"]
[5460,"e_石楼一期Ⅰ-016 风向","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅰ-016 风向","yc_hs_0236","cur_24"]
[5461,"e_石楼一期Ⅰ-016 风速","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅰ-016 风速","yc_hs_0492","cur_77"]
[5462,"e_石楼一期Ⅰ-016 机舱中轴线与风向夹角","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅰ-016 机舱中轴线与风向夹角","yc_hs_0492","cur_78"]
[5463,"e_石楼一期Ⅰ-016 1#桨叶片角度","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅰ-016 1#桨叶片角度","yc_hs_0236","cur_25"]
[5464,"e_石楼一期Ⅰ-016 2#桨叶片角度","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅰ-016 2#桨叶片角度","yc_hs_0236","cur_26"]
[5465,"e_石楼一期Ⅰ-016 3#桨叶片角度","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅰ-016 3#桨叶片角度","yc_hs_0236","cur_27"]
[5466,"e_石楼一期Ⅰ-016 主轴转速","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅰ-016 主轴转速","yc_hs_0492","cur_79"]
[5467,"e_石楼一期Ⅰ-016 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",16,"SLRY.T1_L1.WTG016.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅰ-016 机舱轴向振动(已滤波)","yc_hs_0492","cur_81"]
[5468,"e_石楼一期Ⅱ-007 发电机有功功率","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅱ-007 发电机有功功率","yc_hs_0492","cur_82"]
[5469,"e_石楼一期Ⅱ-007 发电机 绕组温度1","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅱ-007 发电机 绕组温度1","yc_hs_0236","cur_52"]
[5470,"e_石楼一期Ⅱ-007 发电机 绕组温度2","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅱ-007 发电机 绕组温度2","yc_hs_0236","cur_53"]
[5471,"e_石楼一期Ⅱ-007 发电机 绕组温度3","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅱ-007 发电机 绕组温度3","yc_hs_0236","cur_54"]
[5472,"e_石楼一期Ⅱ-007 发电机转速","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅱ-007 发电机转速","yc_hs_0492","cur_84"]
[5473,"e_石楼一期Ⅱ-007 舱内温度","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅱ-007 舱内温度","yc_hs_0492","cur_85"]
[5474,"e_石楼一期Ⅱ-007 舱外温度","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅱ-007 舱外温度","yc_hs_0492","cur_88"]
[5475,"e_石楼一期Ⅱ-007 偏航角度(扭缆角度）","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅱ-007 偏航角度(扭缆角度）","yc_hs_0492","cur_89"]
[5476,"e_石楼一期Ⅱ-007 风向","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅱ-007 风向","yc_hs_0236","cur_58"]
[5477,"e_石楼一期Ⅱ-007 风速","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅱ-007 风速","yc_hs_0492","cur_90"]
[5478,"e_石楼一期Ⅱ-007 机舱中轴线与风向夹角","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅱ-007 机舱中轴线与风向夹角","yc_hs_0492","cur_91"]
[5479,"e_石楼一期Ⅱ-007 1#桨叶片角度","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅱ-007 1#桨叶片角度","yc_hs_0236","cur_59"]
[5480,"e_石楼一期Ⅱ-007 2#桨叶片角度","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅱ-007 2#桨叶片角度","yc_hs_0236","cur_60"]
[5481,"e_石楼一期Ⅱ-007 3#桨叶片角度","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅱ-007 3#桨叶片角度","yc_hs_0236","cur_61"]
[5482,"e_石楼一期Ⅱ-007 主轴转速","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅱ-007 主轴转速","yc_hs_0492","cur_92"]
[5483,"e_石楼一期Ⅱ-007 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",7,"SLRY.T1_L2.WTG007.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅱ-007 机舱轴向振动(已滤波)","yc_hs_0492","cur_94"]
[5484,"e_石楼一期Ⅱ-008 发电机有功功率","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅱ-008 发电机有功功率","yc_hs_0492","cur_95"]
[5485,"e_石楼一期Ⅱ-008 发电机 绕组温度1","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅱ-008 发电机 绕组温度1","yc_hs_0236","cur_86"]
[5486,"e_石楼一期Ⅱ-008 发电机 绕组温度2","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅱ-008 发电机 绕组温度2","yc_hs_0236","cur_87"]
[5487,"e_石楼一期Ⅱ-008 发电机 绕组温度3","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅱ-008 发电机 绕组温度3","yc_hs_0236","cur_88"]
[5488,"e_石楼一期Ⅱ-008 发电机转速","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅱ-008 发电机转速","yc_hs_0492","cur_97"]
[5489,"e_石楼一期Ⅱ-008 舱内温度","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅱ-008 舱内温度","yc_hs_0492","cur_98"]
[5490,"e_石楼一期Ⅱ-008 舱外温度","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅱ-008 舱外温度","yc_hs_0493","cur_01"]
[5491,"e_石楼一期Ⅱ-008 偏航角度(扭缆角度）","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅱ-008 偏航角度(扭缆角度）","yc_hs_0493","cur_02"]
[5492,"e_石楼一期Ⅱ-008 风向","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅱ-008 风向","yc_hs_0236","cur_92"]
[5493,"e_石楼一期Ⅱ-008 风速","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅱ-008 风速","yc_hs_0493","cur_03"]
[5494,"e_石楼一期Ⅱ-008 机舱中轴线与风向夹角","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅱ-008 机舱中轴线与风向夹角","yc_hs_0493","cur_04"]
[5495,"e_石楼一期Ⅱ-008 1#桨叶片角度","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅱ-008 1#桨叶片角度","yc_hs_0236","cur_93"]
[5496,"e_石楼一期Ⅱ-008 2#桨叶片角度","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅱ-008 2#桨叶片角度","yc_hs_0236","cur_94"]
[5497,"e_石楼一期Ⅱ-008 3#桨叶片角度","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅱ-008 3#桨叶片角度","yc_hs_0236","cur_95"]
[5498,"e_石楼一期Ⅱ-008 主轴转速","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅱ-008 主轴转速","yc_hs_0493","cur_05"]
[5499,"e_石楼一期Ⅱ-008 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",8,"SLRY.T1_L2.WTG008.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅱ-008 机舱轴向振动(已滤波)","yc_hs_0493","cur_07"]
[5500,"e_石楼一期Ⅱ-009 发电机有功功率","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅱ-009 发电机有功功率","yc_hs_0493","cur_08"]
[5501,"e_石楼一期Ⅱ-009 发电机 绕组温度1","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅱ-009 发电机 绕组温度1","yc_hs_0237","cur_20"]
[5502,"e_石楼一期Ⅱ-009 发电机 绕组温度2","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅱ-009 发电机 绕组温度2","yc_hs_0237","cur_21"]
[5503,"e_石楼一期Ⅱ-009 发电机 绕组温度3","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅱ-009 发电机 绕组温度3","yc_hs_0237","cur_22"]
[5504,"e_石楼一期Ⅱ-009 发电机转速","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅱ-009 发电机转速","yc_hs_0493","cur_10"]
[5505,"e_石楼一期Ⅱ-009 舱内温度","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅱ-009 舱内温度","yc_hs_0493","cur_11"]
[5506,"e_石楼一期Ⅱ-009 舱外温度","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅱ-009 舱外温度","yc_hs_0493","cur_14"]
[5507,"e_石楼一期Ⅱ-009 偏航角度(扭缆角度）","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅱ-009 偏航角度(扭缆角度）","yc_hs_0493","cur_15"]
[5508,"e_石楼一期Ⅱ-009 风向","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅱ-009 风向","yc_hs_0237","cur_26"]
[5509,"e_石楼一期Ⅱ-009 风速","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅱ-009 风速","yc_hs_0493","cur_16"]
[5510,"e_石楼一期Ⅱ-009 机舱中轴线与风向夹角","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅱ-009 机舱中轴线与风向夹角","yc_hs_0493","cur_17"]
[5511,"e_石楼一期Ⅱ-009 1#桨叶片角度","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅱ-009 1#桨叶片角度","yc_hs_0237","cur_27"]
[5512,"e_石楼一期Ⅱ-009 2#桨叶片角度","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅱ-009 2#桨叶片角度","yc_hs_0237","cur_28"]
[5513,"e_石楼一期Ⅱ-009 3#桨叶片角度","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅱ-009 3#桨叶片角度","yc_hs_0237","cur_29"]
[5514,"e_石楼一期Ⅱ-009 主轴转速","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅱ-009 主轴转速","yc_hs_0493","cur_18"]
[5515,"e_石楼一期Ⅱ-009 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",9,"SLRY.T1_L2.WTG009.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅱ-009 机舱轴向振动(已滤波)","yc_hs_0493","cur_20"]
[5516,"e_石楼一期Ⅱ-017 发电机有功功率","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅱ-017 发电机有功功率","yc_hs_0493","cur_21"]
[5517,"e_石楼一期Ⅱ-017 发电机 绕组温度1","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅱ-017 发电机 绕组温度1","yc_hs_0237","cur_54"]
[5518,"e_石楼一期Ⅱ-017 发电机 绕组温度2","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅱ-017 发电机 绕组温度2","yc_hs_0237","cur_55"]
[5519,"e_石楼一期Ⅱ-017 发电机 绕组温度3","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅱ-017 发电机 绕组温度3","yc_hs_0237","cur_56"]
[5520,"e_石楼一期Ⅱ-017 发电机转速","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅱ-017 发电机转速","yc_hs_0493","cur_23"]
[5521,"e_石楼一期Ⅱ-017 舱内温度","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅱ-017 舱内温度","yc_hs_0493","cur_24"]
[5522,"e_石楼一期Ⅱ-017 舱外温度","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅱ-017 舱外温度","yc_hs_0493","cur_27"]
[5523,"e_石楼一期Ⅱ-017 偏航角度(扭缆角度）","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅱ-017 偏航角度(扭缆角度）","yc_hs_0493","cur_28"]
[5524,"e_石楼一期Ⅱ-017 风向","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅱ-017 风向","yc_hs_0237","cur_60"]
[5525,"e_石楼一期Ⅱ-017 风速","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅱ-017 风速","yc_hs_0493","cur_29"]
[5526,"e_石楼一期Ⅱ-017 机舱中轴线与风向夹角","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅱ-017 机舱中轴线与风向夹角","yc_hs_0493","cur_30"]
[5527,"e_石楼一期Ⅱ-017 1#桨叶片角度","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅱ-017 1#桨叶片角度","yc_hs_0237","cur_61"]
[5528,"e_石楼一期Ⅱ-017 2#桨叶片角度","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅱ-017 2#桨叶片角度","yc_hs_0237","cur_62"]
[5529,"e_石楼一期Ⅱ-017 3#桨叶片角度","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅱ-017 3#桨叶片角度","yc_hs_0237","cur_63"]
[5530,"e_石楼一期Ⅱ-017 主轴转速","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅱ-017 主轴转速","yc_hs_0493","cur_31"]
[5531,"e_石楼一期Ⅱ-017 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",17,"SLRY.T1_L2.WTG017.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅱ-017 机舱轴向振动(已滤波)","yc_hs_0493","cur_33"]
[5532,"e_石楼一期Ⅱ-018 发电机有功功率","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅱ-018 发电机有功功率","yc_hs_0493","cur_34"]
[5533,"e_石楼一期Ⅱ-018 发电机 绕组温度1","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅱ-018 发电机 绕组温度1","yc_hs_0237","cur_88"]
[5534,"e_石楼一期Ⅱ-018 发电机 绕组温度2","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅱ-018 发电机 绕组温度2","yc_hs_0237","cur_89"]
[5535,"e_石楼一期Ⅱ-018 发电机 绕组温度3","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅱ-018 发电机 绕组温度3","yc_hs_0237","cur_90"]
[5536,"e_石楼一期Ⅱ-018 发电机转速","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅱ-018 发电机转速","yc_hs_0493","cur_36"]
[5537,"e_石楼一期Ⅱ-018 舱内温度","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅱ-018 舱内温度","yc_hs_0493","cur_37"]
[5538,"e_石楼一期Ⅱ-018 舱外温度","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅱ-018 舱外温度","yc_hs_0493","cur_40"]
[5539,"e_石楼一期Ⅱ-018 偏航角度(扭缆角度）","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅱ-018 偏航角度(扭缆角度）","yc_hs_0493","cur_41"]
[5540,"e_石楼一期Ⅱ-018 风向","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅱ-018 风向","yc_hs_0237","cur_94"]
[5541,"e_石楼一期Ⅱ-018 风速","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅱ-018 风速","yc_hs_0493","cur_42"]
[5542,"e_石楼一期Ⅱ-018 机舱中轴线与风向夹角","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅱ-018 机舱中轴线与风向夹角","yc_hs_0493","cur_43"]
[5543,"e_石楼一期Ⅱ-018 1#桨叶片角度","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅱ-018 1#桨叶片角度","yc_hs_0237","cur_95"]
[5544,"e_石楼一期Ⅱ-018 2#桨叶片角度","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅱ-018 2#桨叶片角度","yc_hs_0237","cur_96"]
[5545,"e_石楼一期Ⅱ-018 3#桨叶片角度","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅱ-018 3#桨叶片角度","yc_hs_0237","cur_97"]
[5546,"e_石楼一期Ⅱ-018 主轴转速","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅱ-018 主轴转速","yc_hs_0493","cur_44"]
[5547,"e_石楼一期Ⅱ-018 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",18,"SLRY.T1_L2.WTG018.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅱ-018 机舱轴向振动(已滤波)","yc_hs_0493","cur_46"]
[5548,"e_石楼一期Ⅱ-019 发电机有功功率","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅱ-019 发电机有功功率","yc_hs_0493","cur_47"]
[5549,"e_石楼一期Ⅱ-019 发电机 绕组温度1","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅱ-019 发电机 绕组温度1","yc_hs_0238","cur_22"]
[5550,"e_石楼一期Ⅱ-019 发电机 绕组温度2","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅱ-019 发电机 绕组温度2","yc_hs_0238","cur_23"]
[5551,"e_石楼一期Ⅱ-019 发电机 绕组温度3","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WGEN.GenSenTmp3","发电机绕组3温度","generator_winding3_temperature","e_石楼一期Ⅱ-019 发电机 绕组温度3","yc_hs_0238","cur_24"]
[5552,"e_石楼一期Ⅰ-004 发电机转速","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅰ-004 发电机转速","yc_hs_0493","cur_49"]
[5553,"e_石楼一期Ⅰ-004 舱内温度","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅰ-004 舱内温度","yc_hs_0493","cur_50"]
[5554,"e_石楼一期Ⅰ-004 舱外温度","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅰ-004 舱外温度","yc_hs_0493","cur_53"]
[5555,"e_石楼一期Ⅰ-004 偏航角度(扭缆角度）","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅰ-004 偏航角度(扭缆角度）","yc_hs_0493","cur_54"]
[5556,"e_石楼一期Ⅰ-004 风向","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅰ-004 风向","yc_hs_0233","cur_18"]
[5557,"e_石楼一期Ⅰ-004 风速","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅰ-004 风速","yc_hs_0493","cur_55"]
[5558,"e_石楼一期Ⅰ-004 机舱中轴线与风向夹角","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅰ-004 机舱中轴线与风向夹角","yc_hs_0493","cur_67"]
[5559,"e_石楼一期Ⅰ-004 1#桨叶片角度","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅰ-004 1#桨叶片角度","yc_hs_0233","cur_19"]
[5560,"e_石楼一期Ⅰ-004 2#桨叶片角度","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅰ-004 2#桨叶片角度","yc_hs_0233","cur_20"]
[5561,"e_石楼一期Ⅰ-004 3#桨叶片角度","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅰ-004 3#桨叶片角度","yc_hs_0233","cur_21"]
[5562,"e_石楼一期Ⅰ-004 主轴转速","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅰ-004 主轴转速","yc_hs_0493","cur_68"]
[5563,"e_石楼一期Ⅰ-004 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",4,"SLRY.T1_L1.WTG004.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅰ-004 机舱轴向振动(已滤波)","yc_hs_0493","cur_70"]
[5564,"e_石楼一期Ⅰ-005 发电机有功功率","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅰ-005 发电机有功功率","yc_hs_0493","cur_71"]
[5565,"e_石楼一期Ⅰ-005 发电机 绕组温度1","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅰ-005 发电机 绕组温度1","yc_hs_0233","cur_46"]
[5566,"e_石楼一期Ⅰ-005 发电机 绕组温度2","石楼风电场","WOF35800081",5,"SLRY.T1_L1.WTG005.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅰ-005 发电机 绕组温度2","yc_hs_0233","cur_47"]
[5567,"e_石楼一期Ⅱ-019 发电机转速","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WGEN.GenSpd","发电机转速","generator_speed","e_石楼一期Ⅱ-019 发电机转速","yc_hs_0493","cur_73"]
[5568,"e_石楼一期Ⅱ-019 舱内温度","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼一期Ⅱ-019 舱内温度","yc_hs_0493","cur_74"]
[5569,"e_石楼一期Ⅱ-019 舱外温度","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼一期Ⅱ-019 舱外温度","yc_hs_0493","cur_77"]
[5570,"e_石楼一期Ⅱ-019 偏航角度(扭缆角度）","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WNAC.TemOut2","扭缆角度","twisted_cable_angle","e_石楼一期Ⅱ-019 偏航角度(扭缆角度）","yc_hs_0493","cur_78"]
[5571,"e_石楼一期Ⅱ-019 风向","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼一期Ⅱ-019 风向","yc_hs_0238","cur_28"]
[5572,"e_石楼一期Ⅱ-019 风速","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WNAC.WindSpeed","风速","wind_velocity","e_石楼一期Ⅱ-019 风速","yc_hs_0493","cur_79"]
[5573,"e_石楼一期Ⅱ-019 机舱中轴线与风向夹角","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼一期Ⅱ-019 机舱中轴线与风向夹角","yc_hs_0493","cur_80"]
[5574,"e_石楼一期Ⅱ-019 1#桨叶片角度","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼一期Ⅱ-019 1#桨叶片角度","yc_hs_0238","cur_29"]
[5575,"e_石楼一期Ⅱ-019 2#桨叶片角度","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼一期Ⅱ-019 2#桨叶片角度","yc_hs_0238","cur_30"]
[5576,"e_石楼一期Ⅱ-019 3#桨叶片角度","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼一期Ⅱ-019 3#桨叶片角度","yc_hs_0238","cur_31"]
[5577,"e_石楼一期Ⅱ-019 主轴转速","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WTRM.RotorSpd","风轮转速","rotor_speed","e_石楼一期Ⅱ-019 主轴转速","yc_hs_0491","cur_59"]
[5578,"e_石楼一期Ⅱ-019 机舱轴向振动(已滤波)","石楼风电场","WOF35800081",19,"SLRY.T1_L2.WTG019.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼一期Ⅱ-019 机舱轴向振动(已滤波)","yc_hs_0491","cur_61"]
[5579,"e_石楼一期Ⅱ-020 发电机有功功率","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WGEN.GenActivePW","有功功率","active_power","e_石楼一期Ⅱ-020 发电机有功功率","yc_hs_0491","cur_62"]
[5580,"e_石楼一期Ⅱ-020 发电机 绕组温度1","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WGEN.GenSenTmp1","发电机绕组1温度","generator_winding1_temperature","e_石楼一期Ⅱ-020 发电机 绕组温度1","yc_hs_0238","cur_56"]
[5581,"e_石楼一期Ⅱ-020 发电机 绕组温度2","石楼风电场","WOF35800081",20,"SLRY.T1_L2.WTG020.WGEN.GenSenTmp2","发电机绕组2温度","generator_winding2_temperature","e_石楼一期Ⅱ-020 发电机 绕组温度2","yc_hs_0238","cur_57"]
[5582,"e_石楼二期Ⅲ-026 风速","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅲ-026 风速","yc_hs_0538","cur_09"]
[5583,"e_石楼二期Ⅲ-026 发电机有功功率","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅲ-026 发电机有功功率","yc_hs_0538","cur_10"]
[5584,"e_石楼二期Ⅲ-026 发电机转速","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅲ-026 发电机转速","yc_hs_0538","cur_20"]
[5585,"e_石楼二期Ⅲ-026 主轴转速","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅲ-026 主轴转速","yc_hs_0538","cur_21"]
[5586,"e_石楼二期Ⅲ-026 机舱与风向夹角","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅲ-026 机舱与风向夹角","yc_hs_0538","cur_22"]
[5587,"e_石楼二期Ⅲ-026 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅲ-026 1#桨叶片角度(桨距角)","yc_hs_0538","cur_23"]
[5588,"e_石楼二期Ⅲ-026 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅲ-026 2#桨叶片角度(桨距角)","yc_hs_0538","cur_24"]
[5589,"e_石楼二期Ⅲ-026 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅲ-026 3#桨叶片角度(桨距角)","yc_hs_0538","cur_25"]
[5590,"e_石楼二期Ⅲ-026 舱外温度","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅲ-026 舱外温度","yc_hs_0538","cur_26"]
[5591,"e_石楼二期Ⅲ-026 舱内温度","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅲ-026 舱内温度","yc_hs_0538","cur_27"]
[5592,"e_石楼二期Ⅲ-026 齿轮箱油池温度","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅲ-026 齿轮箱油池温度","yc_hs_0538","cur_28"]
[5593,"e_石楼二期Ⅲ-026 主轴后轴承温度","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅲ-026 主轴后轴承温度","yc_hs_0538","cur_30"]
[5594,"e_石楼二期Ⅲ-026 发电机驱动端轴承温度","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅲ-026 发电机驱动端轴承温度","yc_hs_0538","cur_31"]
[5595,"e_石楼二期Ⅲ-026 发电机非驱动端轴承温度","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅲ-026 发电机非驱动端轴承温度","yc_hs_0538","cur_32"]
[5596,"e_石楼二期Ⅲ-026 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅲ-026 齿轮箱高速轴非驱动端轴承温度","yc_hs_0538","cur_34"]
[5597,"e_石楼二期Ⅲ-026 发电机定子U相线圈温度","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅲ-026 发电机定子U相线圈温度","yc_hs_0538","cur_35"]
[5598,"e_石楼二期Ⅲ-026 发电机定子V相线圈温度","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅲ-026 发电机定子V相线圈温度","yc_hs_0538","cur_36"]
[5599,"e_石楼二期Ⅲ-026 发电机定子W相线圈温度","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅲ-026 发电机定子W相线圈温度","yc_hs_0538","cur_37"]
[5600,"e_石楼二期Ⅲ-026 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅲ-026 机舱侧向振动值(已滤波)","yc_hs_0538","cur_40"]
[5601,"e_石楼二期Ⅲ-026 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅲ-026 机舱轴向振动值(已滤波)","yc_hs_0538","cur_41"]
[5602,"e_石楼二期Ⅲ-026 风向","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅲ-026 风向","yc_hs_0538","cur_58"]
[5603,"e_石楼二期Ⅲ-026 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅲ-026 齿轮箱中速轴非驱动端轴承温度","yc_hs_0538","cur_74"]
[5604,"e_石楼二期Ⅲ-026 机舱角度（位置）","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅲ-026 机舱角度（位置）","yc_hs_0538","cur_75"]
[5605,"e_石楼二期Ⅲ-026 偏航角度(扭缆角度）","石楼风电场","WOF35800081",26,"SLRY.T2_L3.WTG026.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅲ-026 偏航角度(扭缆角度）","yc_hs_0538","cur_76"]
[5606,"e_石楼二期Ⅲ-027 舱外温度","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅲ-027 舱外温度","yc_hs_0538","cur_78"]
[5607,"e_石楼二期Ⅲ-027 舱内温度","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅲ-027 舱内温度","yc_hs_0538","cur_79"]
[5608,"e_石楼二期Ⅲ-027 齿轮箱油池温度","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅲ-027 齿轮箱油池温度","yc_hs_0538","cur_80"]
[5609,"e_石楼二期Ⅲ-027 主轴后轴承温度","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅲ-027 主轴后轴承温度","yc_hs_0538","cur_82"]
[5610,"e_石楼二期Ⅲ-027 发电机驱动端轴承温度","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅲ-027 发电机驱动端轴承温度","yc_hs_0538","cur_83"]
[5611,"e_石楼二期Ⅲ-027 发电机非驱动端轴承温度","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅲ-027 发电机非驱动端轴承温度","yc_hs_0538","cur_84"]
[5612,"e_石楼二期Ⅲ-027 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅲ-027 齿轮箱高速轴非驱动端轴承温度","yc_hs_0538","cur_86"]
[5613,"e_石楼二期Ⅲ-027 发电机定子U相线圈温度","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅲ-027 发电机定子U相线圈温度","yc_hs_0538","cur_87"]
[5614,"e_石楼二期Ⅲ-027 发电机定子V相线圈温度","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅲ-027 发电机定子V相线圈温度","yc_hs_0538","cur_88"]
[5615,"e_石楼二期Ⅲ-027 发电机定子W相线圈温度","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅲ-027 发电机定子W相线圈温度","yc_hs_0538","cur_89"]
[5616,"e_石楼二期Ⅲ-027 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅲ-027 机舱侧向振动值(已滤波)","yc_hs_0538","cur_92"]
[5617,"e_石楼二期Ⅲ-027 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅲ-027 机舱轴向振动值(已滤波)","yc_hs_0538","cur_93"]
[5618,"e_石楼二期Ⅲ-027 风向","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅲ-027 风向","yc_hs_0539","cur_10"]
[5619,"e_石楼二期Ⅲ-027 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅲ-027 齿轮箱中速轴非驱动端轴承温度","yc_hs_0539","cur_26"]
[5620,"e_石楼二期Ⅲ-027 机舱角度（位置）","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅲ-027 机舱角度（位置）","yc_hs_0539","cur_27"]
[5621,"e_石楼二期Ⅲ-027 偏航角度(扭缆角度）","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅲ-027 偏航角度(扭缆角度）","yc_hs_0539","cur_28"]
[5622,"e_石楼二期Ⅲ-027 风速","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅲ-027 风速","yc_hs_0539","cur_31"]
[5623,"e_石楼二期Ⅲ-027 发电机有功功率","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅲ-027 发电机有功功率","yc_hs_0539","cur_32"]
[5624,"e_石楼二期Ⅲ-027 发电机转速","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅲ-027 发电机转速","yc_hs_0539","cur_42"]
[5625,"e_石楼二期Ⅲ-027 主轴转速","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅲ-027 主轴转速","yc_hs_0539","cur_43"]
[5626,"e_石楼二期Ⅲ-027 机舱与风向夹角","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅲ-027 机舱与风向夹角","yc_hs_0539","cur_44"]
[5627,"e_石楼二期Ⅲ-027 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅲ-027 1#桨叶片角度(桨距角)","yc_hs_0539","cur_45"]
[5628,"e_石楼二期Ⅲ-027 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅲ-027 2#桨叶片角度(桨距角)","yc_hs_0539","cur_46"]
[5629,"e_石楼二期Ⅲ-027 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",27,"SLRY.T2_L3.WTG027.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅲ-027 3#桨叶片角度(桨距角)","yc_hs_0539","cur_47"]
[5630,"e_石楼二期Ⅲ-028 风速","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅲ-028 风速","yc_hs_0539","cur_49"]
[5631,"e_石楼二期Ⅲ-028 发电机有功功率","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅲ-028 发电机有功功率","yc_hs_0539","cur_50"]
[5632,"e_石楼二期Ⅲ-028 发电机转速","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅲ-028 发电机转速","yc_hs_0539","cur_60"]
[5633,"e_石楼二期Ⅲ-028 主轴转速","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅲ-028 主轴转速","yc_hs_0539","cur_61"]
[5634,"e_石楼二期Ⅲ-028 机舱与风向夹角","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅲ-028 机舱与风向夹角","yc_hs_0539","cur_62"]
[5635,"e_石楼二期Ⅲ-028 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅲ-028 1#桨叶片角度(桨距角)","yc_hs_0539","cur_63"]
[5636,"e_石楼二期Ⅲ-028 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅲ-028 2#桨叶片角度(桨距角)","yc_hs_0539","cur_64"]
[5637,"e_石楼二期Ⅲ-028 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅲ-028 3#桨叶片角度(桨距角)","yc_hs_0539","cur_65"]
[5638,"e_石楼二期Ⅲ-028 舱外温度","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅲ-028 舱外温度","yc_hs_0539","cur_66"]
[5639,"e_石楼二期Ⅲ-028 舱内温度","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅲ-028 舱内温度","yc_hs_0539","cur_67"]
[5640,"e_石楼二期Ⅲ-028 齿轮箱油池温度","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅲ-028 齿轮箱油池温度","yc_hs_0539","cur_68"]
[5641,"e_石楼二期Ⅲ-028 主轴后轴承温度","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅲ-028 主轴后轴承温度","yc_hs_0539","cur_70"]
[5642,"e_石楼二期Ⅲ-028 发电机驱动端轴承温度","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅲ-028 发电机驱动端轴承温度","yc_hs_0539","cur_71"]
[5643,"e_石楼二期Ⅲ-028 发电机非驱动端轴承温度","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅲ-028 发电机非驱动端轴承温度","yc_hs_0539","cur_72"]
[5644,"e_石楼二期Ⅲ-028 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅲ-028 齿轮箱高速轴非驱动端轴承温度","yc_hs_0539","cur_74"]
[5645,"e_石楼二期Ⅲ-028 发电机定子U相线圈温度","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅲ-028 发电机定子U相线圈温度","yc_hs_0539","cur_75"]
[5646,"e_石楼二期Ⅲ-028 发电机定子V相线圈温度","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅲ-028 发电机定子V相线圈温度","yc_hs_0539","cur_76"]
[5647,"e_石楼二期Ⅲ-028 发电机定子W相线圈温度","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅲ-028 发电机定子W相线圈温度","yc_hs_0539","cur_77"]
[5648,"e_石楼二期Ⅲ-028 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅲ-028 机舱侧向振动值(已滤波)","yc_hs_0539","cur_80"]
[5649,"e_石楼二期Ⅲ-028 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅲ-028 机舱轴向振动值(已滤波)","yc_hs_0539","cur_81"]
[5650,"e_石楼二期Ⅲ-028 风向","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅲ-028 风向","yc_hs_0539","cur_98"]
[5651,"e_石楼二期Ⅲ-028 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅲ-028 齿轮箱中速轴非驱动端轴承温度","yc_hs_0540","cur_14"]
[5652,"e_石楼二期Ⅲ-028 机舱角度（位置）","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅲ-028 机舱角度（位置）","yc_hs_0540","cur_15"]
[5653,"e_石楼二期Ⅲ-028 偏航角度(扭缆角度）","石楼风电场","WOF35800081",28,"SLRY.T2_L3.WTG028.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅲ-028 偏航角度(扭缆角度）","yc_hs_0540","cur_16"]
[5654,"e_石楼二期Ⅲ-029 风向","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅲ-029 风向","yc_hs_0540","cur_55"]
[5655,"e_石楼二期Ⅲ-029 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅲ-029 齿轮箱中速轴非驱动端轴承温度","yc_hs_0540","cur_71"]
[5656,"e_石楼二期Ⅲ-029 机舱角度（位置）","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅲ-029 机舱角度（位置）","yc_hs_0540","cur_72"]
[5657,"e_石楼二期Ⅲ-029 偏航角度(扭缆角度）","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅲ-029 偏航角度(扭缆角度）","yc_hs_0540","cur_73"]
[5658,"e_石楼二期Ⅲ-029 风速","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅲ-029 风速","yc_hs_0540","cur_76"]
[5659,"e_石楼二期Ⅲ-029 发电机有功功率","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅲ-029 发电机有功功率","yc_hs_0540","cur_77"]
[5660,"e_石楼二期Ⅲ-029 发电机转速","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅲ-029 发电机转速","yc_hs_0540","cur_87"]
[5661,"e_石楼二期Ⅲ-029 主轴转速","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅲ-029 主轴转速","yc_hs_0540","cur_18"]
[5662,"e_石楼二期Ⅲ-029 机舱与风向夹角","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅲ-029 机舱与风向夹角","yc_hs_0540","cur_19"]
[5663,"e_石楼二期Ⅲ-029 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅲ-029 1#桨叶片角度(桨距角)","yc_hs_0540","cur_20"]
[5664,"e_石楼二期Ⅲ-029 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅲ-029 2#桨叶片角度(桨距角)","yc_hs_0540","cur_21"]
[5665,"e_石楼二期Ⅲ-029 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅲ-029 3#桨叶片角度(桨距角)","yc_hs_0540","cur_22"]
[5666,"e_石楼二期Ⅲ-029 舱外温度","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅲ-029 舱外温度","yc_hs_0540","cur_23"]
[5667,"e_石楼二期Ⅲ-029 舱内温度","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅲ-029 舱内温度","yc_hs_0540","cur_24"]
[5668,"e_石楼二期Ⅲ-029 齿轮箱油池温度","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅲ-029 齿轮箱油池温度","yc_hs_0540","cur_25"]
[5669,"e_石楼二期Ⅲ-029 主轴后轴承温度","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅲ-029 主轴后轴承温度","yc_hs_0540","cur_27"]
[5670,"e_石楼二期Ⅲ-029 发电机驱动端轴承温度","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅲ-029 发电机驱动端轴承温度","yc_hs_0540","cur_28"]
[5671,"e_石楼二期Ⅲ-029 发电机非驱动端轴承温度","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅲ-029 发电机非驱动端轴承温度","yc_hs_0540","cur_29"]
[5672,"e_石楼二期Ⅲ-029 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅲ-029 齿轮箱高速轴非驱动端轴承温度","yc_hs_0540","cur_31"]
[5673,"e_石楼二期Ⅲ-029 发电机定子U相线圈温度","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅲ-029 发电机定子U相线圈温度","yc_hs_0540","cur_32"]
[5674,"e_石楼二期Ⅲ-029 发电机定子V相线圈温度","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅲ-029 发电机定子V相线圈温度","yc_hs_0540","cur_33"]
[5675,"e_石楼二期Ⅲ-029 发电机定子W相线圈温度","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅲ-029 发电机定子W相线圈温度","yc_hs_0540","cur_34"]
[5676,"e_石楼二期Ⅲ-029 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅲ-029 机舱侧向振动值(已滤波)","yc_hs_0540","cur_37"]
[5677,"e_石楼二期Ⅲ-029 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",29,"SLRY.T2_L3.WTG029.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅲ-029 机舱轴向振动值(已滤波)","yc_hs_0540","cur_38"]
[5678,"e_石楼二期Ⅲ-030 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅲ-030 齿轮箱中速轴非驱动端轴承温度","yc_hs_0540","cur_93"]
[5679,"e_石楼二期Ⅲ-030 机舱角度（位置）","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅲ-030 机舱角度（位置）","yc_hs_0540","cur_94"]
[5680,"e_石楼二期Ⅲ-030 偏航角度(扭缆角度）","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅲ-030 偏航角度(扭缆角度）","yc_hs_0540","cur_95"]
[5681,"e_石楼二期Ⅲ-030 风速","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅲ-030 风速","yc_hs_0540","cur_98"]
[5682,"e_石楼二期Ⅲ-030 发电机有功功率","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅲ-030 发电机有功功率","yc_hs_0540","cur_99"]
[5683,"e_石楼二期Ⅲ-030 发电机转速","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅲ-030 发电机转速","yc_hs_0541","cur_09"]
[5684,"e_石楼二期Ⅲ-030 主轴转速","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅲ-030 主轴转速","yc_hs_0541","cur_10"]
[5685,"e_石楼二期Ⅲ-030 机舱与风向夹角","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅲ-030 机舱与风向夹角","yc_hs_0541","cur_11"]
[5686,"e_石楼二期Ⅲ-030 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅲ-030 1#桨叶片角度(桨距角)","yc_hs_0541","cur_12"]
[5687,"e_石楼二期Ⅲ-030 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅲ-030 2#桨叶片角度(桨距角)","yc_hs_0541","cur_13"]
[5688,"e_石楼二期Ⅲ-030 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅲ-030 3#桨叶片角度(桨距角)","yc_hs_0541","cur_14"]
[5689,"e_石楼二期Ⅲ-030 舱外温度","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅲ-030 舱外温度","yc_hs_0541","cur_15"]
[5690,"e_石楼二期Ⅲ-030 舱内温度","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅲ-030 舱内温度","yc_hs_0541","cur_16"]
[5691,"e_石楼二期Ⅲ-030 齿轮箱油池温度","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅲ-030 齿轮箱油池温度","yc_hs_0541","cur_17"]
[5692,"e_石楼二期Ⅲ-030 主轴后轴承温度","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅲ-030 主轴后轴承温度","yc_hs_0541","cur_19"]
[5693,"e_石楼二期Ⅲ-030 发电机驱动端轴承温度","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅲ-030 发电机驱动端轴承温度","yc_hs_0541","cur_20"]
[5694,"e_石楼二期Ⅲ-030 发电机非驱动端轴承温度","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅲ-030 发电机非驱动端轴承温度","yc_hs_0541","cur_21"]
[5695,"e_石楼二期Ⅲ-030 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅲ-030 齿轮箱高速轴非驱动端轴承温度","yc_hs_0541","cur_23"]
[5696,"e_石楼二期Ⅲ-030 发电机定子U相线圈温度","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅲ-030 发电机定子U相线圈温度","yc_hs_0541","cur_24"]
[5697,"e_石楼二期Ⅲ-030 发电机定子V相线圈温度","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅲ-030 发电机定子V相线圈温度","yc_hs_0541","cur_25"]
[5698,"e_石楼二期Ⅲ-030 发电机定子W相线圈温度","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅲ-030 发电机定子W相线圈温度","yc_hs_0541","cur_26"]
[5699,"e_石楼二期Ⅲ-030 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅲ-030 机舱侧向振动值(已滤波)","yc_hs_0541","cur_29"]
[5700,"e_石楼二期Ⅲ-030 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅲ-030 机舱轴向振动值(已滤波)","yc_hs_0541","cur_30"]
[5701,"e_石楼二期Ⅲ-030 风向","石楼风电场","WOF35800081",30,"SLRY.T2_L3.WTG030.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅲ-030 风向","yc_hs_0541","cur_47"]
[5702,"e_石楼二期Ⅲ-031 风速","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅲ-031 风速","yc_hs_0541","cur_59"]
[5703,"e_石楼二期Ⅲ-031 发电机有功功率","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅲ-031 发电机有功功率","yc_hs_0541","cur_60"]
[5704,"e_石楼二期Ⅲ-031 发电机转速","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅲ-031 发电机转速","yc_hs_0541","cur_70"]
[5705,"e_石楼二期Ⅲ-031 主轴转速","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅲ-031 主轴转速","yc_hs_0541","cur_71"]
[5706,"e_石楼二期Ⅲ-031 机舱与风向夹角","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅲ-031 机舱与风向夹角","yc_hs_0541","cur_72"]
[5707,"e_石楼二期Ⅲ-031 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅲ-031 1#桨叶片角度(桨距角)","yc_hs_0541","cur_73"]
[5708,"e_石楼二期Ⅲ-031 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅲ-031 2#桨叶片角度(桨距角)","yc_hs_0541","cur_74"]
[5709,"e_石楼二期Ⅲ-031 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅲ-031 3#桨叶片角度(桨距角)","yc_hs_0541","cur_75"]
[5710,"e_石楼二期Ⅲ-031 舱外温度","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅲ-031 舱外温度","yc_hs_0541","cur_76"]
[5711,"e_石楼二期Ⅲ-031 舱内温度","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅲ-031 舱内温度","yc_hs_0541","cur_77"]
[5712,"e_石楼二期Ⅲ-031 齿轮箱油池温度","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅲ-031 齿轮箱油池温度","yc_hs_0541","cur_78"]
[5713,"e_石楼二期Ⅲ-031 主轴后轴承温度","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅲ-031 主轴后轴承温度","yc_hs_0541","cur_80"]
[5714,"e_石楼二期Ⅲ-031 发电机驱动端轴承温度","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅲ-031 发电机驱动端轴承温度","yc_hs_0541","cur_81"]
[5715,"e_石楼二期Ⅲ-031 发电机非驱动端轴承温度","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅲ-031 发电机非驱动端轴承温度","yc_hs_0541","cur_82"]
[5716,"e_石楼二期Ⅲ-031 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅲ-031 齿轮箱高速轴非驱动端轴承温度","yc_hs_0541","cur_84"]
[5717,"e_石楼二期Ⅲ-031 发电机定子U相线圈温度","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅲ-031 发电机定子U相线圈温度","yc_hs_0541","cur_85"]
[5718,"e_石楼二期Ⅲ-031 发电机定子V相线圈温度","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅲ-031 发电机定子V相线圈温度","yc_hs_0541","cur_86"]
[5719,"e_石楼二期Ⅲ-031 发电机定子W相线圈温度","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅲ-031 发电机定子W相线圈温度","yc_hs_0541","cur_87"]
[5720,"e_石楼二期Ⅲ-031 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅲ-031 机舱侧向振动值(已滤波)","yc_hs_0541","cur_90"]
[5721,"e_石楼二期Ⅲ-031 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅲ-031 机舱轴向振动值(已滤波)","yc_hs_0541","cur_91"]
[5722,"e_石楼二期Ⅲ-031 风向","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅲ-031 风向","yc_hs_0542","cur_08"]
[5723,"e_石楼二期Ⅲ-031 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅲ-031 齿轮箱中速轴非驱动端轴承温度","yc_hs_0542","cur_24"]
[5724,"e_石楼二期Ⅲ-031 机舱角度（位置）","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅲ-031 机舱角度（位置）","yc_hs_0542","cur_25"]
[5725,"e_石楼二期Ⅲ-031 偏航角度(扭缆角度）","石楼风电场","WOF35800081",31,"SLRY.T2_L3.WTG031.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅲ-031 偏航角度(扭缆角度）","yc_hs_0542","cur_26"]
[5726,"e_石楼二期Ⅲ-032 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅲ-032 齿轮箱中速轴非驱动端轴承温度","yc_hs_0542","cur_43"]
[5727,"e_石楼二期Ⅲ-032 机舱角度（位置）","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅲ-032 机舱角度（位置）","yc_hs_0542","cur_44"]
[5728,"e_石楼二期Ⅲ-032 偏航角度(扭缆角度）","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅲ-032 偏航角度(扭缆角度）","yc_hs_0542","cur_45"]
[5729,"e_石楼二期Ⅲ-032 发电机转速","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅲ-032 发电机转速","yc_hs_0542","cur_51"]
[5730,"e_石楼二期Ⅲ-032 主轴转速","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅲ-032 主轴转速","yc_hs_0542","cur_52"]
[5731,"e_石楼二期Ⅲ-032 机舱与风向夹角","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅲ-032 机舱与风向夹角","yc_hs_0542","cur_53"]
[5732,"e_石楼二期Ⅲ-032 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅲ-032 1#桨叶片角度(桨距角)","yc_hs_0542","cur_54"]
[5733,"e_石楼二期Ⅲ-032 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅲ-032 2#桨叶片角度(桨距角)","yc_hs_0542","cur_55"]
[5734,"e_石楼二期Ⅲ-032 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅲ-032 3#桨叶片角度(桨距角)","yc_hs_0542","cur_56"]
[5735,"e_石楼二期Ⅲ-032 舱外温度","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅲ-032 舱外温度","yc_hs_0542","cur_57"]
[5736,"e_石楼二期Ⅲ-032 舱内温度","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅲ-032 舱内温度","yc_hs_0542","cur_58"]
[5737,"e_石楼二期Ⅲ-032 齿轮箱油池温度","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅲ-032 齿轮箱油池温度","yc_hs_0542","cur_59"]
[5738,"e_石楼二期Ⅲ-032 主轴后轴承温度","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅲ-032 主轴后轴承温度","yc_hs_0542","cur_61"]
[5739,"e_石楼二期Ⅲ-032 发电机驱动端轴承温度","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅲ-032 发电机驱动端轴承温度","yc_hs_0542","cur_62"]
[5740,"e_石楼二期Ⅲ-032 发电机非驱动端轴承温度","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅲ-032 发电机非驱动端轴承温度","yc_hs_0542","cur_63"]
[5741,"e_石楼二期Ⅲ-032 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅲ-032 齿轮箱高速轴非驱动端轴承温度","yc_hs_0542","cur_65"]
[5742,"e_石楼二期Ⅲ-032 发电机定子U相线圈温度","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅲ-032 发电机定子U相线圈温度","yc_hs_0542","cur_66"]
[5743,"e_石楼二期Ⅲ-032 发电机定子V相线圈温度","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅲ-032 发电机定子V相线圈温度","yc_hs_0542","cur_67"]
[5744,"e_石楼二期Ⅲ-032 发电机定子W相线圈温度","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅲ-032 发电机定子W相线圈温度","yc_hs_0542","cur_68"]
[5745,"e_石楼二期Ⅲ-032 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅲ-032 机舱侧向振动值(已滤波)","yc_hs_0542","cur_71"]
[5746,"e_石楼二期Ⅲ-032 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅲ-032 机舱轴向振动值(已滤波)","yc_hs_0542","cur_72"]
[5747,"e_石楼二期Ⅲ-032 风向","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅲ-032 风向","yc_hs_0542","cur_89"]
[5748,"e_石楼二期Ⅲ-032 风速","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅲ-032 风速","yc_hs_0542","cur_91"]
[5749,"e_石楼二期Ⅲ-032 发电机有功功率","石楼风电场","WOF35800081",32,"SLRY.T2_L3.WTG032.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅲ-032 发电机有功功率","yc_hs_0542","cur_92"]
[5750,"e_石楼二期Ⅲ-033 主轴后轴承温度","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅲ-033 主轴后轴承温度","yc_hs_0542","cur_98"]
[5751,"e_石楼二期Ⅲ-033 发电机驱动端轴承温度","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅲ-033 发电机驱动端轴承温度","yc_hs_0542","cur_99"]
[5752,"e_石楼二期Ⅲ-033 发电机非驱动端轴承温度","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅲ-033 发电机非驱动端轴承温度","yc_hs_0542","cur_100"]
[5753,"e_石楼二期Ⅲ-033 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅲ-033 齿轮箱高速轴非驱动端轴承温度","yc_hs_0543","cur_02"]
[5754,"e_石楼二期Ⅲ-033 发电机定子U相线圈温度","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅲ-033 发电机定子U相线圈温度","yc_hs_0543","cur_03"]
[5755,"e_石楼二期Ⅲ-033 发电机定子V相线圈温度","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅲ-033 发电机定子V相线圈温度","yc_hs_0543","cur_04"]
[5756,"e_石楼二期Ⅲ-033 发电机定子W相线圈温度","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅲ-033 发电机定子W相线圈温度","yc_hs_0543","cur_05"]
[5757,"e_石楼二期Ⅲ-033 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅲ-033 机舱侧向振动值(已滤波)","yc_hs_0543","cur_08"]
[5758,"e_石楼二期Ⅲ-033 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅲ-033 机舱轴向振动值(已滤波)","yc_hs_0543","cur_09"]
[5759,"e_石楼二期Ⅲ-033 齿轮箱油池温度","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅲ-033 齿轮箱油池温度","yc_hs_0543","cur_20"]
[5760,"e_石楼二期Ⅲ-033 风向","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅲ-033 风向","yc_hs_0543","cur_28"]
[5761,"e_石楼二期Ⅲ-033 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅲ-033 齿轮箱中速轴非驱动端轴承温度","yc_hs_0543","cur_44"]
[5762,"e_石楼二期Ⅲ-033 机舱角度（位置）","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅲ-033 机舱角度（位置）","yc_hs_0543","cur_45"]
[5763,"e_石楼二期Ⅲ-033 偏航角度(扭缆角度）","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅲ-033 偏航角度(扭缆角度）","yc_hs_0543","cur_46"]
[5764,"e_石楼二期Ⅲ-033 风速","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅲ-033 风速","yc_hs_0543","cur_49"]
[5765,"e_石楼二期Ⅲ-033 发电机有功功率","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅲ-033 发电机有功功率","yc_hs_0543","cur_50"]
[5766,"e_石楼二期Ⅲ-033 发电机转速","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅲ-033 发电机转速","yc_hs_0543","cur_60"]
[5767,"e_石楼二期Ⅲ-033 主轴转速","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅲ-033 主轴转速","yc_hs_0543","cur_61"]
[5768,"e_石楼二期Ⅲ-033 机舱与风向夹角","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅲ-033 机舱与风向夹角","yc_hs_0543","cur_62"]
[5769,"e_石楼二期Ⅲ-033 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅲ-033 1#桨叶片角度(桨距角)","yc_hs_0543","cur_63"]
[5770,"e_石楼二期Ⅲ-033 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅲ-033 2#桨叶片角度(桨距角)","yc_hs_0543","cur_64"]
[5771,"e_石楼二期Ⅲ-033 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅲ-033 3#桨叶片角度(桨距角)","yc_hs_0543","cur_65"]
[5772,"e_石楼二期Ⅲ-033 舱外温度","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅲ-033 舱外温度","yc_hs_0543","cur_66"]
[5773,"e_石楼二期Ⅲ-033 舱内温度","石楼风电场","WOF35800081",33,"SLRY.T2_L3.WTG033.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅲ-033 舱内温度","yc_hs_0543","cur_67"]
[5774,"e_石楼二期Ⅲ-034 风速","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅲ-034 风速","yc_hs_0544","cur_05"]
[5775,"e_石楼二期Ⅲ-034 发电机有功功率","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅲ-034 发电机有功功率","yc_hs_0544","cur_06"]
[5776,"e_石楼二期Ⅲ-034 发电机转速","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅲ-034 发电机转速","yc_hs_0544","cur_16"]
[5777,"e_石楼二期Ⅲ-034 主轴转速","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅲ-034 主轴转速","yc_hs_0544","cur_17"]
[5778,"e_石楼二期Ⅲ-034 机舱与风向夹角","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅲ-034 机舱与风向夹角","yc_hs_0544","cur_18"]
[5779,"e_石楼二期Ⅲ-034 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅲ-034 1#桨叶片角度(桨距角)","yc_hs_0544","cur_19"]
[5780,"e_石楼二期Ⅲ-034 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅲ-034 2#桨叶片角度(桨距角)","yc_hs_0544","cur_20"]
[5781,"e_石楼二期Ⅲ-034 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅲ-034 3#桨叶片角度(桨距角)","yc_hs_0544","cur_21"]
[5782,"e_石楼二期Ⅲ-034 舱外温度","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅲ-034 舱外温度","yc_hs_0544","cur_22"]
[5783,"e_石楼二期Ⅲ-034 舱内温度","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅲ-034 舱内温度","yc_hs_0544","cur_23"]
[5784,"e_石楼二期Ⅲ-034 齿轮箱油池温度","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅲ-034 齿轮箱油池温度","yc_hs_0544","cur_24"]
[5785,"e_石楼二期Ⅲ-034 主轴后轴承温度","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅲ-034 主轴后轴承温度","yc_hs_0544","cur_26"]
[5786,"e_石楼二期Ⅲ-034 发电机驱动端轴承温度","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅲ-034 发电机驱动端轴承温度","yc_hs_0544","cur_27"]
[5787,"e_石楼二期Ⅲ-034 发电机非驱动端轴承温度","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅲ-034 发电机非驱动端轴承温度","yc_hs_0544","cur_28"]
[5788,"e_石楼二期Ⅲ-034 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅲ-034 齿轮箱高速轴非驱动端轴承温度","yc_hs_0544","cur_30"]
[5789,"e_石楼二期Ⅲ-034 发电机定子U相线圈温度","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅲ-034 发电机定子U相线圈温度","yc_hs_0544","cur_31"]
[5790,"e_石楼二期Ⅲ-034 发电机定子V相线圈温度","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅲ-034 发电机定子V相线圈温度","yc_hs_0544","cur_32"]
[5791,"e_石楼二期Ⅲ-034 发电机定子W相线圈温度","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅲ-034 发电机定子W相线圈温度","yc_hs_0544","cur_33"]
[5792,"e_石楼二期Ⅲ-034 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅲ-034 机舱侧向振动值(已滤波)","yc_hs_0544","cur_36"]
[5793,"e_石楼二期Ⅲ-034 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅲ-034 机舱轴向振动值(已滤波)","yc_hs_0544","cur_37"]
[5794,"e_石楼二期Ⅲ-034 风向","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅲ-034 风向","yc_hs_0543","cur_84"]
[5795,"e_石楼二期Ⅲ-034 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅲ-034 齿轮箱中速轴非驱动端轴承温度","yc_hs_0543","cur_100"]
[5796,"e_石楼二期Ⅲ-034 机舱角度（位置）","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅲ-034 机舱角度（位置）","yc_hs_0544","cur_01"]
[5797,"e_石楼二期Ⅲ-034 偏航角度(扭缆角度）","石楼风电场","WOF35800081",34,"SLRY.T2_L3.WTG034.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅲ-034 偏航角度(扭缆角度）","yc_hs_0544","cur_02"]
[5798,"e_石楼二期Ⅳ-035 风速","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅳ-035 风速","yc_hs_0544","cur_39"]
[5799,"e_石楼二期Ⅳ-035 发电机有功功率","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅳ-035 发电机有功功率","yc_hs_0544","cur_40"]
[5800,"e_石楼二期Ⅳ-035 发电机转速","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅳ-035 发电机转速","yc_hs_0544","cur_50"]
[5801,"e_石楼二期Ⅳ-035 主轴转速","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅳ-035 主轴转速","yc_hs_0544","cur_51"]
[5802,"e_石楼二期Ⅳ-035 机舱与风向夹角","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅳ-035 机舱与风向夹角","yc_hs_0544","cur_52"]
[5803,"e_石楼二期Ⅳ-035 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅳ-035 1#桨叶片角度(桨距角)","yc_hs_0544","cur_53"]
[5804,"e_石楼二期Ⅳ-035 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅳ-035 2#桨叶片角度(桨距角)","yc_hs_0544","cur_54"]
[5805,"e_石楼二期Ⅳ-035 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅳ-035 3#桨叶片角度(桨距角)","yc_hs_0544","cur_55"]
[5806,"e_石楼二期Ⅳ-035 舱外温度","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅳ-035 舱外温度","yc_hs_0544","cur_56"]
[5807,"e_石楼二期Ⅳ-035 舱内温度","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅳ-035 舱内温度","yc_hs_0544","cur_57"]
[5808,"e_石楼二期Ⅳ-035 齿轮箱油池温度","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅳ-035 齿轮箱油池温度","yc_hs_0544","cur_58"]
[5809,"e_石楼二期Ⅳ-035 主轴后轴承温度","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅳ-035 主轴后轴承温度","yc_hs_0544","cur_60"]
[5810,"e_石楼二期Ⅳ-035 发电机驱动端轴承温度","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅳ-035 发电机驱动端轴承温度","yc_hs_0544","cur_61"]
[5811,"e_石楼二期Ⅳ-035 发电机非驱动端轴承温度","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅳ-035 发电机非驱动端轴承温度","yc_hs_0544","cur_62"]
[5812,"e_石楼二期Ⅳ-035 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅳ-035 齿轮箱高速轴非驱动端轴承温度","yc_hs_0544","cur_64"]
[5813,"e_石楼二期Ⅳ-035 发电机定子U相线圈温度","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅳ-035 发电机定子U相线圈温度","yc_hs_0544","cur_65"]
[5814,"e_石楼二期Ⅳ-035 发电机定子V相线圈温度","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅳ-035 发电机定子V相线圈温度","yc_hs_0544","cur_66"]
[5815,"e_石楼二期Ⅳ-035 发电机定子W相线圈温度","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅳ-035 发电机定子W相线圈温度","yc_hs_0544","cur_67"]
[5816,"e_石楼二期Ⅳ-035 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅳ-035 机舱侧向振动值(已滤波)","yc_hs_0544","cur_70"]
[5817,"e_石楼二期Ⅳ-035 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅳ-035 机舱轴向振动值(已滤波)","yc_hs_0544","cur_71"]
[5818,"e_石楼二期Ⅳ-035 风向","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅳ-035 风向","yc_hs_0544","cur_88"]
[5819,"e_石楼二期Ⅳ-035 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅳ-035 齿轮箱中速轴非驱动端轴承温度","yc_hs_0545","cur_04"]
[5820,"e_石楼二期Ⅳ-035 机舱角度（位置）","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅳ-035 机舱角度（位置）","yc_hs_0545","cur_05"]
[5821,"e_石楼二期Ⅳ-035 偏航角度(扭缆角度）","石楼风电场","WOF35800081",35,"SLRY.T2_L4.WTG035.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅳ-035 偏航角度(扭缆角度）","yc_hs_0545","cur_06"]
[5822,"e_石楼二期Ⅳ-036 风速","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅳ-036 风速","yc_hs_0545","cur_09"]
[5823,"e_石楼二期Ⅳ-036 发电机有功功率","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅳ-036 发电机有功功率","yc_hs_0545","cur_10"]
[5824,"e_石楼二期Ⅳ-036 发电机转速","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅳ-036 发电机转速","yc_hs_0545","cur_20"]
[5825,"e_石楼二期Ⅳ-036 主轴转速","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅳ-036 主轴转速","yc_hs_0545","cur_21"]
[5826,"e_石楼二期Ⅳ-036 机舱与风向夹角","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅳ-036 机舱与风向夹角","yc_hs_0545","cur_22"]
[5827,"e_石楼二期Ⅳ-036 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅳ-036 1#桨叶片角度(桨距角)","yc_hs_0545","cur_23"]
[5828,"e_石楼二期Ⅳ-036 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅳ-036 2#桨叶片角度(桨距角)","yc_hs_0545","cur_24"]
[5829,"e_石楼二期Ⅳ-036 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅳ-036 3#桨叶片角度(桨距角)","yc_hs_0545","cur_25"]
[5830,"e_石楼二期Ⅳ-036 舱外温度","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅳ-036 舱外温度","yc_hs_0545","cur_26"]
[5831,"e_石楼二期Ⅳ-036 舱内温度","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅳ-036 舱内温度","yc_hs_0545","cur_27"]
[5832,"e_石楼二期Ⅳ-036 齿轮箱油池温度","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅳ-036 齿轮箱油池温度","yc_hs_0545","cur_28"]
[5833,"e_石楼二期Ⅳ-036 主轴后轴承温度","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅳ-036 主轴后轴承温度","yc_hs_0545","cur_30"]
[5834,"e_石楼二期Ⅳ-036 发电机驱动端轴承温度","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅳ-036 发电机驱动端轴承温度","yc_hs_0545","cur_31"]
[5835,"e_石楼二期Ⅳ-036 发电机非驱动端轴承温度","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅳ-036 发电机非驱动端轴承温度","yc_hs_0545","cur_32"]
[5836,"e_石楼二期Ⅳ-036 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅳ-036 齿轮箱高速轴非驱动端轴承温度","yc_hs_0545","cur_34"]
[5837,"e_石楼二期Ⅳ-036 发电机定子U相线圈温度","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅳ-036 发电机定子U相线圈温度","yc_hs_0545","cur_35"]
[5838,"e_石楼二期Ⅳ-036 发电机定子V相线圈温度","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅳ-036 发电机定子V相线圈温度","yc_hs_0545","cur_36"]
[5839,"e_石楼二期Ⅳ-036 发电机定子W相线圈温度","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅳ-036 发电机定子W相线圈温度","yc_hs_0545","cur_37"]
[5840,"e_石楼二期Ⅳ-036 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅳ-036 机舱侧向振动值(已滤波)","yc_hs_0545","cur_40"]
[5841,"e_石楼二期Ⅳ-036 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅳ-036 机舱轴向振动值(已滤波)","yc_hs_0545","cur_41"]
[5842,"e_石楼二期Ⅳ-036 风向","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅳ-036 风向","yc_hs_0545","cur_58"]
[5843,"e_石楼二期Ⅳ-036 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅳ-036 齿轮箱中速轴非驱动端轴承温度","yc_hs_0545","cur_74"]
[5844,"e_石楼二期Ⅳ-036 机舱角度（位置）","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅳ-036 机舱角度（位置）","yc_hs_0545","cur_75"]
[5845,"e_石楼二期Ⅳ-036 偏航角度(扭缆角度）","石楼风电场","WOF35800081",36,"SLRY.T2_L4.WTG036.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅳ-036 偏航角度(扭缆角度）","yc_hs_0545","cur_76"]
[5846,"e_石楼二期Ⅳ-037 风向","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅳ-037 风向","yc_hs_0545","cur_79"]
[5847,"e_石楼二期Ⅳ-037 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅳ-037 齿轮箱中速轴非驱动端轴承温度","yc_hs_0545","cur_95"]
[5848,"e_石楼二期Ⅳ-037 机舱角度（位置）","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅳ-037 机舱角度（位置）","yc_hs_0545","cur_96"]
[5849,"e_石楼二期Ⅳ-037 偏航角度(扭缆角度）","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅳ-037 偏航角度(扭缆角度）","yc_hs_0545","cur_97"]
[5850,"e_石楼二期Ⅳ-037 风速","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅳ-037 风速","yc_hs_0545","cur_100"]
[5851,"e_石楼二期Ⅳ-037 发电机有功功率","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅳ-037 发电机有功功率","yc_hs_0546","cur_01"]
[5852,"e_石楼二期Ⅳ-037 发电机转速","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅳ-037 发电机转速","yc_hs_0546","cur_11"]
[5853,"e_石楼二期Ⅳ-037 主轴转速","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅳ-037 主轴转速","yc_hs_0546","cur_12"]
[5854,"e_石楼二期Ⅳ-037 机舱与风向夹角","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅳ-037 机舱与风向夹角","yc_hs_0546","cur_13"]
[5855,"e_石楼二期Ⅳ-037 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅳ-037 1#桨叶片角度(桨距角)","yc_hs_0546","cur_14"]
[5856,"e_石楼二期Ⅳ-037 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅳ-037 2#桨叶片角度(桨距角)","yc_hs_0546","cur_15"]
[5857,"e_石楼二期Ⅳ-037 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅳ-037 3#桨叶片角度(桨距角)","yc_hs_0546","cur_16"]
[5858,"e_石楼二期Ⅳ-037 舱外温度","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅳ-037 舱外温度","yc_hs_0546","cur_17"]
[5859,"e_石楼二期Ⅳ-037 舱内温度","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅳ-037 舱内温度","yc_hs_0546","cur_18"]
[5860,"e_石楼二期Ⅳ-037 齿轮箱油池温度","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅳ-037 齿轮箱油池温度","yc_hs_0546","cur_19"]
[5861,"e_石楼二期Ⅳ-037 主轴后轴承温度","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅳ-037 主轴后轴承温度","yc_hs_0546","cur_21"]
[5862,"e_石楼二期Ⅳ-037 发电机驱动端轴承温度","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅳ-037 发电机驱动端轴承温度","yc_hs_0546","cur_22"]
[5863,"e_石楼二期Ⅳ-037 发电机非驱动端轴承温度","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅳ-037 发电机非驱动端轴承温度","yc_hs_0546","cur_23"]
[5864,"e_石楼二期Ⅳ-037 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅳ-037 齿轮箱高速轴非驱动端轴承温度","yc_hs_0546","cur_25"]
[5865,"e_石楼二期Ⅳ-037 发电机定子U相线圈温度","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅳ-037 发电机定子U相线圈温度","yc_hs_0546","cur_26"]
[5866,"e_石楼二期Ⅳ-037 发电机定子V相线圈温度","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅳ-037 发电机定子V相线圈温度","yc_hs_0546","cur_27"]
[5867,"e_石楼二期Ⅳ-037 发电机定子W相线圈温度","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅳ-037 发电机定子W相线圈温度","yc_hs_0546","cur_28"]
[5868,"e_石楼二期Ⅳ-037 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅳ-037 机舱侧向振动值(已滤波)","yc_hs_0546","cur_31"]
[5869,"e_石楼二期Ⅳ-037 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",37,"SLRY.T2_L4.WTG037.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅳ-037 机舱轴向振动值(已滤波)","yc_hs_0546","cur_32"]
[5870,"e_石楼二期Ⅳ-038 风速","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅳ-038 风速","yc_hs_0546","cur_49"]
[5871,"e_石楼二期Ⅳ-038 发电机有功功率","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅳ-038 发电机有功功率","yc_hs_0546","cur_50"]
[5872,"e_石楼二期Ⅳ-038 发电机转速","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅳ-038 发电机转速","yc_hs_0546","cur_60"]
[5873,"e_石楼二期Ⅳ-038 主轴转速","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅳ-038 主轴转速","yc_hs_0546","cur_61"]
[5874,"e_石楼二期Ⅳ-038 机舱与风向夹角","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅳ-038 机舱与风向夹角","yc_hs_0546","cur_62"]
[5875,"e_石楼二期Ⅳ-038 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅳ-038 1#桨叶片角度(桨距角)","yc_hs_0546","cur_63"]
[5876,"e_石楼二期Ⅳ-038 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅳ-038 2#桨叶片角度(桨距角)","yc_hs_0546","cur_64"]
[5877,"e_石楼二期Ⅳ-038 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅳ-038 3#桨叶片角度(桨距角)","yc_hs_0546","cur_65"]
[5878,"e_石楼二期Ⅳ-038 舱外温度","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅳ-038 舱外温度","yc_hs_0546","cur_66"]
[5879,"e_石楼二期Ⅳ-038 舱内温度","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅳ-038 舱内温度","yc_hs_0546","cur_67"]
[5880,"e_石楼二期Ⅳ-038 齿轮箱油池温度","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅳ-038 齿轮箱油池温度","yc_hs_0546","cur_68"]
[5881,"e_石楼二期Ⅳ-038 主轴后轴承温度","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅳ-038 主轴后轴承温度","yc_hs_0546","cur_70"]
[5882,"e_石楼二期Ⅳ-038 发电机驱动端轴承温度","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅳ-038 发电机驱动端轴承温度","yc_hs_0546","cur_71"]
[5883,"e_石楼二期Ⅳ-038 发电机非驱动端轴承温度","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅳ-038 发电机非驱动端轴承温度","yc_hs_0546","cur_72"]
[5884,"e_石楼二期Ⅳ-038 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅳ-038 齿轮箱高速轴非驱动端轴承温度","yc_hs_0546","cur_74"]
[5885,"e_石楼二期Ⅳ-038 发电机定子U相线圈温度","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅳ-038 发电机定子U相线圈温度","yc_hs_0546","cur_75"]
[5886,"e_石楼二期Ⅳ-038 发电机定子V相线圈温度","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅳ-038 发电机定子V相线圈温度","yc_hs_0546","cur_76"]
[5887,"e_石楼二期Ⅳ-038 发电机定子W相线圈温度","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅳ-038 发电机定子W相线圈温度","yc_hs_0546","cur_77"]
[5888,"e_石楼二期Ⅳ-038 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅳ-038 机舱侧向振动值(已滤波)","yc_hs_0546","cur_80"]
[5889,"e_石楼二期Ⅳ-038 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅳ-038 机舱轴向振动值(已滤波)","yc_hs_0546","cur_81"]
[5890,"e_石楼二期Ⅳ-038 风向","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅳ-038 风向","yc_hs_0546","cur_98"]
[5891,"e_石楼二期Ⅳ-038 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅳ-038 齿轮箱中速轴非驱动端轴承温度","yc_hs_0547","cur_14"]
[5892,"e_石楼二期Ⅳ-038 机舱角度（位置）","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅳ-038 机舱角度（位置）","yc_hs_0547","cur_15"]
[5893,"e_石楼二期Ⅳ-038 偏航角度(扭缆角度）","石楼风电场","WOF35800081",38,"SLRY.T2_L4.WTG038.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅳ-038 偏航角度(扭缆角度）","yc_hs_0547","cur_16"]
[5894,"e_石楼二期Ⅳ-039 风速","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅳ-039 风速","yc_hs_0547","cur_19"]
[5895,"e_石楼二期Ⅳ-039 发电机有功功率","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅳ-039 发电机有功功率","yc_hs_0547","cur_20"]
[5896,"e_石楼二期Ⅳ-039 发电机转速","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅳ-039 发电机转速","yc_hs_0547","cur_30"]
[5897,"e_石楼二期Ⅳ-039 主轴转速","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅳ-039 主轴转速","yc_hs_0547","cur_31"]
[5898,"e_石楼二期Ⅳ-039 机舱与风向夹角","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅳ-039 机舱与风向夹角","yc_hs_0547","cur_32"]
[5899,"e_石楼二期Ⅳ-039 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅳ-039 1#桨叶片角度(桨距角)","yc_hs_0547","cur_33"]
[5900,"e_石楼二期Ⅳ-039 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅳ-039 2#桨叶片角度(桨距角)","yc_hs_0547","cur_34"]
[5901,"e_石楼二期Ⅳ-039 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅳ-039 3#桨叶片角度(桨距角)","yc_hs_0547","cur_35"]
[5902,"e_石楼二期Ⅳ-039 舱外温度","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅳ-039 舱外温度","yc_hs_0547","cur_36"]
[5903,"e_石楼二期Ⅳ-039 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅳ-039 齿轮箱中速轴非驱动端轴承温度","yc_hs_0547","cur_40"]
[5904,"e_石楼二期Ⅳ-039 机舱角度（位置）","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅳ-039 机舱角度（位置）","yc_hs_0547","cur_41"]
[5905,"e_石楼二期Ⅳ-039 舱内温度","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅳ-039 舱内温度","yc_hs_0547","cur_42"]
[5906,"e_石楼二期Ⅳ-039 齿轮箱油池温度","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅳ-039 齿轮箱油池温度","yc_hs_0547","cur_43"]
[5907,"e_石楼二期Ⅳ-039 主轴后轴承温度","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅳ-039 主轴后轴承温度","yc_hs_0547","cur_45"]
[5908,"e_石楼二期Ⅳ-039 发电机驱动端轴承温度","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅳ-039 发电机驱动端轴承温度","yc_hs_0547","cur_46"]
[5909,"e_石楼二期Ⅳ-039 发电机非驱动端轴承温度","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅳ-039 发电机非驱动端轴承温度","yc_hs_0547","cur_47"]
[5910,"e_石楼二期Ⅳ-039 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅳ-039 齿轮箱高速轴非驱动端轴承温度","yc_hs_0547","cur_49"]
[5911,"e_石楼二期Ⅳ-039 发电机定子U相线圈温度","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅳ-039 发电机定子U相线圈温度","yc_hs_0547","cur_50"]
[5912,"e_石楼二期Ⅳ-039 发电机定子V相线圈温度","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅳ-039 发电机定子V相线圈温度","yc_hs_0547","cur_51"]
[5913,"e_石楼二期Ⅳ-039 发电机定子W相线圈温度","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅳ-039 发电机定子W相线圈温度","yc_hs_0547","cur_52"]
[5914,"e_石楼二期Ⅳ-039 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅳ-039 机舱侧向振动值(已滤波)","yc_hs_0547","cur_55"]
[5915,"e_石楼二期Ⅳ-039 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅳ-039 机舱轴向振动值(已滤波)","yc_hs_0547","cur_56"]
[5916,"e_石楼二期Ⅳ-039 风向","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅳ-039 风向","yc_hs_0547","cur_73"]
[5917,"e_石楼二期Ⅳ-039 偏航角度(扭缆角度）","石楼风电场","WOF35800081",39,"SLRY.T2_L4.WTG039.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅳ-039 偏航角度(扭缆角度）","yc_hs_0547","cur_86"]
[5918,"e_石楼二期Ⅳ-040 风速","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅳ-040 风速","yc_hs_0547","cur_89"]
[5919,"e_石楼二期Ⅳ-040 发电机有功功率","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅳ-040 发电机有功功率","yc_hs_0547","cur_90"]
[5920,"e_石楼二期Ⅳ-040 发电机转速","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅳ-040 发电机转速","yc_hs_0547","cur_100"]
[5921,"e_石楼二期Ⅳ-040 主轴转速","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅳ-040 主轴转速","yc_hs_0548","cur_01"]
[5922,"e_石楼二期Ⅳ-040 机舱与风向夹角","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅳ-040 机舱与风向夹角","yc_hs_0548","cur_02"]
[5923,"e_石楼二期Ⅳ-040 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅳ-040 1#桨叶片角度(桨距角)","yc_hs_0548","cur_03"]
[5924,"e_石楼二期Ⅳ-040 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅳ-040 2#桨叶片角度(桨距角)","yc_hs_0548","cur_04"]
[5925,"e_石楼二期Ⅳ-040 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅳ-040 3#桨叶片角度(桨距角)","yc_hs_0548","cur_05"]
[5926,"e_石楼二期Ⅳ-040 舱外温度","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅳ-040 舱外温度","yc_hs_0548","cur_06"]
[5927,"e_石楼二期Ⅳ-040 舱内温度","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅳ-040 舱内温度","yc_hs_0548","cur_07"]
[5928,"e_石楼二期Ⅳ-040 齿轮箱油池温度","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅳ-040 齿轮箱油池温度","yc_hs_0548","cur_08"]
[5929,"e_石楼二期Ⅳ-040 主轴后轴承温度","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅳ-040 主轴后轴承温度","yc_hs_0548","cur_10"]
[5930,"e_石楼二期Ⅳ-040 发电机驱动端轴承温度","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅳ-040 发电机驱动端轴承温度","yc_hs_0548","cur_11"]
[5931,"e_石楼二期Ⅳ-040 发电机非驱动端轴承温度","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅳ-040 发电机非驱动端轴承温度","yc_hs_0548","cur_12"]
[5932,"e_石楼二期Ⅳ-040 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅳ-040 齿轮箱高速轴非驱动端轴承温度","yc_hs_0548","cur_14"]
[5933,"e_石楼二期Ⅳ-040 发电机定子U相线圈温度","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅳ-040 发电机定子U相线圈温度","yc_hs_0548","cur_15"]
[5934,"e_石楼二期Ⅳ-040 发电机定子V相线圈温度","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅳ-040 发电机定子V相线圈温度","yc_hs_0548","cur_16"]
[5935,"e_石楼二期Ⅳ-040 发电机定子W相线圈温度","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅳ-040 发电机定子W相线圈温度","yc_hs_0548","cur_17"]
[5936,"e_石楼二期Ⅳ-040 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅳ-040 机舱侧向振动值(已滤波)","yc_hs_0548","cur_20"]
[5937,"e_石楼二期Ⅳ-040 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅳ-040 机舱轴向振动值(已滤波)","yc_hs_0548","cur_21"]
[5938,"e_石楼二期Ⅳ-040 风向","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅳ-040 风向","yc_hs_0548","cur_38"]
[5939,"e_石楼二期Ⅳ-040 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅳ-040 齿轮箱中速轴非驱动端轴承温度","yc_hs_0548","cur_54"]
[5940,"e_石楼二期Ⅳ-040 机舱角度（位置）","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅳ-040 机舱角度（位置）","yc_hs_0548","cur_55"]
[5941,"e_石楼二期Ⅳ-040 偏航角度(扭缆角度）","石楼风电场","WOF35800081",40,"SLRY.T2_L4.WTG040.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅳ-040 偏航角度(扭缆角度）","yc_hs_0548","cur_56"]
[5942,"e_石楼二期Ⅳ-041 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅳ-041 齿轮箱中速轴非驱动端轴承温度","yc_hs_0548","cur_62"]
[5943,"e_石楼二期Ⅳ-041 机舱角度（位置）","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅳ-041 机舱角度（位置）","yc_hs_0548","cur_63"]
[5944,"e_石楼二期Ⅳ-041 偏航角度(扭缆角度）","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅳ-041 偏航角度(扭缆角度）","yc_hs_0548","cur_64"]
[5945,"e_石楼二期Ⅳ-041 风速","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅳ-041 风速","yc_hs_0548","cur_67"]
[5946,"e_石楼二期Ⅳ-041 发电机有功功率","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅳ-041 发电机有功功率","yc_hs_0548","cur_68"]
[5947,"e_石楼二期Ⅳ-041 发电机转速","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅳ-041 发电机转速","yc_hs_0548","cur_78"]
[5948,"e_石楼二期Ⅳ-041 主轴转速","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅳ-041 主轴转速","yc_hs_0548","cur_79"]
[5949,"e_石楼二期Ⅳ-041 机舱与风向夹角","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅳ-041 机舱与风向夹角","yc_hs_0548","cur_80"]
[5950,"e_石楼二期Ⅳ-041 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅳ-041 1#桨叶片角度(桨距角)","yc_hs_0548","cur_81"]
[5951,"e_石楼二期Ⅳ-041 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅳ-041 2#桨叶片角度(桨距角)","yc_hs_0548","cur_82"]
[5952,"e_石楼二期Ⅳ-041 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅳ-041 3#桨叶片角度(桨距角)","yc_hs_0548","cur_83"]
[5953,"e_石楼二期Ⅳ-041 舱外温度","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅳ-041 舱外温度","yc_hs_0548","cur_84"]
[5954,"e_石楼二期Ⅳ-041 舱内温度","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅳ-041 舱内温度","yc_hs_0548","cur_85"]
[5955,"e_石楼二期Ⅳ-041 齿轮箱油池温度","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅳ-041 齿轮箱油池温度","yc_hs_0548","cur_86"]
[5956,"e_石楼二期Ⅳ-041 主轴后轴承温度","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅳ-041 主轴后轴承温度","yc_hs_0548","cur_88"]
[5957,"e_石楼二期Ⅳ-041 发电机驱动端轴承温度","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅳ-041 发电机驱动端轴承温度","yc_hs_0548","cur_89"]
[5958,"e_石楼二期Ⅳ-041 发电机非驱动端轴承温度","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅳ-041 发电机非驱动端轴承温度","yc_hs_0548","cur_90"]
[5959,"e_石楼二期Ⅳ-041 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅳ-041 齿轮箱高速轴非驱动端轴承温度","yc_hs_0548","cur_92"]
[5960,"e_石楼二期Ⅳ-041 发电机定子U相线圈温度","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅳ-041 发电机定子U相线圈温度","yc_hs_0548","cur_93"]
[5961,"e_石楼二期Ⅳ-041 发电机定子V相线圈温度","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅳ-041 发电机定子V相线圈温度","yc_hs_0548","cur_94"]
[5962,"e_石楼二期Ⅳ-041 发电机定子W相线圈温度","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅳ-041 发电机定子W相线圈温度","yc_hs_0548","cur_95"]
[5963,"e_石楼二期Ⅳ-041 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅳ-041 机舱侧向振动值(已滤波)","yc_hs_0548","cur_98"]
[5964,"e_石楼二期Ⅳ-041 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅳ-041 机舱轴向振动值(已滤波)","yc_hs_0548","cur_99"]
[5965,"e_石楼二期Ⅳ-041 风向","石楼风电场","WOF35800081",41,"SLRY.T2_L4.WTG041.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅳ-041 风向","yc_hs_0549","cur_16"]
[5966,"e_石楼二期Ⅳ-042 发电机转速","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅳ-042 发电机转速","yc_hs_0549","cur_47"]
[5967,"e_石楼二期Ⅳ-042 主轴转速","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅳ-042 主轴转速","yc_hs_0549","cur_48"]
[5968,"e_石楼二期Ⅳ-042 机舱与风向夹角","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅳ-042 机舱与风向夹角","yc_hs_0549","cur_49"]
[5969,"e_石楼二期Ⅳ-042 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅳ-042 1#桨叶片角度(桨距角)","yc_hs_0549","cur_50"]
[5970,"e_石楼二期Ⅳ-042 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅳ-042 2#桨叶片角度(桨距角)","yc_hs_0549","cur_51"]
[5971,"e_石楼二期Ⅳ-042 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅳ-042 3#桨叶片角度(桨距角)","yc_hs_0549","cur_52"]
[5972,"e_石楼二期Ⅳ-042 舱外温度","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅳ-042 舱外温度","yc_hs_0549","cur_53"]
[5973,"e_石楼二期Ⅳ-042 舱内温度","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅳ-042 舱内温度","yc_hs_0549","cur_54"]
[5974,"e_石楼二期Ⅳ-042 齿轮箱油池温度","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅳ-042 齿轮箱油池温度","yc_hs_0549","cur_55"]
[5975,"e_石楼二期Ⅳ-042 主轴后轴承温度","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅳ-042 主轴后轴承温度","yc_hs_0549","cur_57"]
[5976,"e_石楼二期Ⅳ-042 发电机驱动端轴承温度","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅳ-042 发电机驱动端轴承温度","yc_hs_0549","cur_58"]
[5977,"e_石楼二期Ⅳ-042 发电机非驱动端轴承温度","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅳ-042 发电机非驱动端轴承温度","yc_hs_0549","cur_59"]
[5978,"e_石楼二期Ⅳ-042 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅳ-042 齿轮箱高速轴非驱动端轴承温度","yc_hs_0549","cur_61"]
[5979,"e_石楼二期Ⅳ-042 发电机定子U相线圈温度","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅳ-042 发电机定子U相线圈温度","yc_hs_0549","cur_62"]
[5980,"e_石楼二期Ⅳ-042 发电机定子V相线圈温度","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅳ-042 发电机定子V相线圈温度","yc_hs_0549","cur_63"]
[5981,"e_石楼二期Ⅳ-042 发电机定子W相线圈温度","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅳ-042 发电机定子W相线圈温度","yc_hs_0549","cur_64"]
[5982,"e_石楼二期Ⅳ-042 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅳ-042 机舱侧向振动值(已滤波)","yc_hs_0549","cur_67"]
[5983,"e_石楼二期Ⅳ-042 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅳ-042 机舱轴向振动值(已滤波)","yc_hs_0549","cur_68"]
[5984,"e_石楼二期Ⅳ-042 风速","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅳ-042 风速","yc_hs_0549","cur_83"]
[5985,"e_石楼二期Ⅳ-042 发电机有功功率","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅳ-042 发电机有功功率","yc_hs_0549","cur_84"]
[5986,"e_石楼二期Ⅳ-042 风向","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅳ-042 风向","yc_hs_0549","cur_89"]
[5987,"e_石楼二期Ⅳ-042 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅳ-042 齿轮箱中速轴非驱动端轴承温度","yc_hs_0549","cur_35"]
[5988,"e_石楼二期Ⅳ-042 机舱角度（位置）","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅳ-042 机舱角度（位置）","yc_hs_0549","cur_36"]
[5989,"e_石楼二期Ⅳ-042 偏航角度(扭缆角度）","石楼风电场","WOF35800081",42,"SLRY.T2_L4.WTG042.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅳ-042 偏航角度(扭缆角度）","yc_hs_0549","cur_37"]
[5990,"e_石楼二期Ⅳ-043 风向","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅳ-043 风向","yc_hs_0549","cur_98"]
[5991,"e_石楼二期Ⅳ-043 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅳ-043 齿轮箱中速轴非驱动端轴承温度","yc_hs_0550","cur_14"]
[5992,"e_石楼二期Ⅳ-043 机舱角度（位置）","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅳ-043 机舱角度（位置）","yc_hs_0550","cur_15"]
[5993,"e_石楼二期Ⅳ-043 偏航角度(扭缆角度）","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅳ-043 偏航角度(扭缆角度）","yc_hs_0550","cur_16"]
[5994,"e_石楼二期Ⅳ-043 风速","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅳ-043 风速","yc_hs_0550","cur_19"]
[5995,"e_石楼二期Ⅳ-043 发电机有功功率","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅳ-043 发电机有功功率","yc_hs_0550","cur_20"]
[5996,"e_石楼二期Ⅳ-043 发电机转速","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅳ-043 发电机转速","yc_hs_0550","cur_30"]
[5997,"e_石楼二期Ⅳ-043 主轴转速","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅳ-043 主轴转速","yc_hs_0550","cur_31"]
[5998,"e_石楼二期Ⅳ-043 机舱与风向夹角","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅳ-043 机舱与风向夹角","yc_hs_0550","cur_32"]
[5999,"e_石楼二期Ⅳ-043 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅳ-043 1#桨叶片角度(桨距角)","yc_hs_0550","cur_33"]
[6000,"e_石楼二期Ⅳ-043 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅳ-043 2#桨叶片角度(桨距角)","yc_hs_0550","cur_34"]
[6001,"e_石楼二期Ⅳ-043 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅳ-043 3#桨叶片角度(桨距角)","yc_hs_0550","cur_35"]
[6002,"e_石楼二期Ⅳ-043 舱外温度","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅳ-043 舱外温度","yc_hs_0550","cur_36"]
[6003,"e_石楼二期Ⅳ-043 舱内温度","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅳ-043 舱内温度","yc_hs_0550","cur_37"]
[6004,"e_石楼二期Ⅳ-043 齿轮箱油池温度","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅳ-043 齿轮箱油池温度","yc_hs_0550","cur_38"]
[6005,"e_石楼二期Ⅳ-043 主轴后轴承温度","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅳ-043 主轴后轴承温度","yc_hs_0550","cur_40"]
[6006,"e_石楼二期Ⅳ-043 发电机驱动端轴承温度","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅳ-043 发电机驱动端轴承温度","yc_hs_0550","cur_41"]
[6007,"e_石楼二期Ⅳ-043 发电机非驱动端轴承温度","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅳ-043 发电机非驱动端轴承温度","yc_hs_0550","cur_42"]
[6008,"e_石楼二期Ⅳ-043 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅳ-043 齿轮箱高速轴非驱动端轴承温度","yc_hs_0550","cur_44"]
[6009,"e_石楼二期Ⅳ-043 发电机定子U相线圈温度","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅳ-043 发电机定子U相线圈温度","yc_hs_0550","cur_45"]
[6010,"e_石楼二期Ⅳ-043 发电机定子V相线圈温度","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅳ-043 发电机定子V相线圈温度","yc_hs_0550","cur_46"]
[6011,"e_石楼二期Ⅳ-043 发电机定子W相线圈温度","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅳ-043 发电机定子W相线圈温度","yc_hs_0550","cur_47"]
[6012,"e_石楼二期Ⅳ-043 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅳ-043 机舱侧向振动值(已滤波)","yc_hs_0550","cur_50"]
[6013,"e_石楼二期Ⅳ-043 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",43,"SLRY.T2_L4.WTG043.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅳ-043 机舱轴向振动值(已滤波)","yc_hs_0550","cur_51"]
[6014,"e_石楼二期Ⅳ-044 风速","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WNAC.WindSpeed","风速","wind_velocity","e_石楼二期Ⅳ-044 风速","yc_hs_0550","cur_69"]
[6015,"e_石楼二期Ⅳ-044 发电机有功功率","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WGEN.GenActivePW","有功功率","active_power","e_石楼二期Ⅳ-044 发电机有功功率","yc_hs_0550","cur_70"]
[6016,"e_石楼二期Ⅳ-044 发电机转速","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WGEN.GenSpd","发电机转速","generator_speed","e_石楼二期Ⅳ-044 发电机转速","yc_hs_0550","cur_80"]
[6017,"e_石楼二期Ⅳ-044 主轴转速","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WTRM.RotorSpdPrcs","风轮转速","rotor_speed","e_石楼二期Ⅳ-044 主轴转速","yc_hs_0550","cur_81"]
[6018,"e_石楼二期Ⅳ-044 机舱与风向夹角","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WNAC.WindVaneDirection","对风角度","yaw_error1","e_石楼二期Ⅳ-044 机舱与风向夹角","yc_hs_0550","cur_82"]
[6019,"e_石楼二期Ⅳ-044 1#桨叶片角度(桨距角)","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","e_石楼二期Ⅳ-044 1#桨叶片角度(桨距角)","yc_hs_0550","cur_83"]
[6020,"e_石楼二期Ⅳ-044 2#桨叶片角度(桨距角)","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","e_石楼二期Ⅳ-044 2#桨叶片角度(桨距角)","yc_hs_0550","cur_84"]
[6021,"e_石楼二期Ⅳ-044 3#桨叶片角度(桨距角)","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","e_石楼二期Ⅳ-044 3#桨叶片角度(桨距角)","yc_hs_0550","cur_85"]
[6022,"e_石楼二期Ⅳ-044 舱外温度","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WNAC.TemOut","环境温度","outside_cabin_temperature","e_石楼二期Ⅳ-044 舱外温度","yc_hs_0550","cur_86"]
[6023,"e_石楼二期Ⅳ-044 舱内温度","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WNAC.TemNacelle","机舱内温度","cabin_temperature","e_石楼二期Ⅳ-044 舱内温度","yc_hs_0550","cur_87"]
[6024,"e_石楼二期Ⅳ-044 齿轮箱油池温度","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WTRM.TemGeaOil","齿轮箱油温","gearbox_oil_temperature","e_石楼二期Ⅳ-044 齿轮箱油池温度","yc_hs_0550","cur_88"]
[6025,"e_石楼二期Ⅳ-044 主轴后轴承温度","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","e_石楼二期Ⅳ-044 主轴后轴承温度","yc_hs_0550","cur_90"]
[6026,"e_石楼二期Ⅳ-044 发电机驱动端轴承温度","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","e_石楼二期Ⅳ-044 发电机驱动端轴承温度","yc_hs_0550","cur_91"]
[6027,"e_石楼二期Ⅳ-044 发电机非驱动端轴承温度","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","e_石楼二期Ⅳ-044 发电机非驱动端轴承温度","yc_hs_0550","cur_92"]
[6028,"e_石楼二期Ⅳ-044 齿轮箱高速轴非驱动端轴承温度","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WTRM.TemGeaMSND","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","e_石楼二期Ⅳ-044 齿轮箱高速轴非驱动端轴承温度","yc_hs_0550","cur_94"]
[6029,"e_石楼二期Ⅳ-044 发电机定子U相线圈温度","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","e_石楼二期Ⅳ-044 发电机定子U相线圈温度","yc_hs_0550","cur_95"]
[6030,"e_石楼二期Ⅳ-044 发电机定子V相线圈温度","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","e_石楼二期Ⅳ-044 发电机定子V相线圈温度","yc_hs_0550","cur_96"]
[6031,"e_石楼二期Ⅳ-044 发电机定子W相线圈温度","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","e_石楼二期Ⅳ-044 发电机定子W相线圈温度","yc_hs_0550","cur_97"]
[6032,"e_石楼二期Ⅳ-044 机舱侧向振动值(已滤波)","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","e_石楼二期Ⅳ-044 机舱侧向振动值(已滤波)","yc_hs_0550","cur_100"]
[6033,"e_石楼二期Ⅳ-044 机舱轴向振动值(已滤波)","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","e_石楼二期Ⅳ-044 机舱轴向振动值(已滤波)","yc_hs_0551","cur_01"]
[6034,"e_石楼二期Ⅳ-044 风向","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WNAC.WindDirection","绝对风向","true_wind_direction","e_石楼二期Ⅳ-044 风向","yc_hs_0551","cur_18"]
[6035,"e_石楼二期Ⅳ-044 齿轮箱中速轴非驱动端轴承温度","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WTRM.TemGeaZSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","e_石楼二期Ⅳ-044 齿轮箱中速轴非驱动端轴承温度","yc_hs_0551","cur_34"]
[6036,"e_石楼二期Ⅳ-044 机舱角度（位置）","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WYAW.NacellePosition","机舱位置","cabin_position","e_石楼二期Ⅳ-044 机舱角度（位置）","yc_hs_0551","cur_35"]
[6037,"e_石楼二期Ⅳ-044 偏航角度(扭缆角度）","石楼风电场","WOF35800081",44,"SLRY.T2_L4.WTG044.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","e_石楼二期Ⅳ-044 偏航角度(扭缆角度）","yc_hs_0551","cur_36"]
[6038,"i_平陆三期 VI-49 机舱角度（位置）","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VI-49 机舱角度（位置）","yc_hs_0002","cur_96"]
[6039,"i_平陆三期 VI-49 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VI-49 机舱侧向振动值(已滤波)","yc_hs_0003","cur_13"]
[6040,"i_平陆三期 VI-49 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VI-49 机舱轴向振动值(已滤波)","yc_hs_0003","cur_14"]
[6041,"i_平陆三期 VI-49 风速","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VI-49 风速","yc_hs_0003","cur_15"]
[6042,"i_平陆三期 VI-49 舱外温度","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VI-49 舱外温度","yc_hs_0003","cur_16"]
[6043,"i_平陆三期 VI-49 舱内温度","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VI-49 舱内温度","yc_hs_0003","cur_22"]
[6044,"i_平陆三期 VI-49 机舱与风向夹角","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VI-49 机舱与风向夹角","yc_hs_0003","cur_23"]
[6045,"i_平陆三期 VI-49 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VI-49 1#桨叶片角度(桨距角)","yc_hs_0003","cur_25"]
[6046,"i_平陆三期 VI-49 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VI-49 2#桨叶片角度(桨距角)","yc_hs_0003","cur_27"]
[6047,"i_平陆三期 VI-49 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VI-49 3#桨叶片角度(桨距角)","yc_hs_0003","cur_44"]
[6048,"i_平陆三期 VI-49 发电机定子U相线圈温度","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VI-49 发电机定子U相线圈温度","yc_hs_0003","cur_45"]
[6049,"i_平陆三期 VI-49 发电机定子V相线圈温度","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VI-49 发电机定子V相线圈温度","yc_hs_0003","cur_46"]
[6050,"i_平陆三期 VI-49 发电机定子W相线圈温度","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VI-49 发电机定子W相线圈温度","yc_hs_0003","cur_47"]
[6051,"i_平陆三期 VI-49 发电机转速","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VI-49 发电机转速","yc_hs_0003","cur_56"]
[6052,"i_平陆三期 VI-49 发电机有功功率","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VI-49 发电机有功功率","yc_hs_0003","cur_58"]
[6053,"i_平陆三期 VI-49 发电机驱动端轴承温度","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VI-49 发电机驱动端轴承温度","yc_hs_0003","cur_76"]
[6054,"i_平陆三期 VI-49 发电机非驱动端轴承温度","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VI-49 发电机非驱动端轴承温度","yc_hs_0003","cur_77"]
[6055,"i_平陆三期 VI-49 风轮（主轴）转速","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VI-49 风轮（主轴）转速","yc_hs_0004","cur_08"]
[6056,"i_平陆三期 VI-49 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VI-49 齿轮箱高速轴驱动端轴承温度","yc_hs_0004","cur_09"]
[6057,"i_平陆三期 VI-49 风向","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VI-49 风向","yc_hs_0004","cur_37"]
[6058,"i_平陆三期 VI-49 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VI-49 齿轮箱中间轴非驱动端轴承温度","yc_hs_0004","cur_49"]
[6059,"i_平陆三期 VI-49 主轴承外圈温度","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VI-49 主轴承外圈温度","yc_hs_0004","cur_51"]
[6060,"i_平陆三期 VI-49 扭缆角度","平陆风电场","WOF35900004",49,"YCPL.T3_L1.WTG049.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VI-49 扭缆角度","yc_hs_0004","cur_69"]
[6061,"i_平陆三期 VI-50 风向","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VI-50 风向","yc_hs_0004","cur_77"]
[6062,"i_平陆三期 VI-50 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VI-50 齿轮箱中间轴非驱动端轴承温度","yc_hs_0005","cur_01"]
[6063,"i_平陆三期 VI-50 主轴承外圈温度","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VI-50 主轴承外圈温度","yc_hs_0005","cur_02"]
[6064,"i_平陆三期 VI-50 扭缆角度","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VI-50 扭缆角度","yc_hs_0005","cur_09"]
[6065,"i_平陆三期 VI-50 风速","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VI-50 风速","yc_hs_0005","cur_10"]
[6066,"i_平陆三期 VI-50 舱外温度","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VI-50 舱外温度","yc_hs_0005","cur_11"]
[6067,"i_平陆三期 VI-50 舱内温度","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VI-50 舱内温度","yc_hs_0005","cur_13"]
[6068,"i_平陆三期 VI-50 机舱与风向夹角","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VI-50 机舱与风向夹角","yc_hs_0005","cur_30"]
[6069,"i_平陆三期 VI-50 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VI-50 1#桨叶片角度(桨距角)","yc_hs_0005","cur_32"]
[6070,"i_平陆三期 VI-50 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VI-50 2#桨叶片角度(桨距角)","yc_hs_0005","cur_33"]
[6071,"i_平陆三期 VI-50 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VI-50 3#桨叶片角度(桨距角)","yc_hs_0005","cur_39"]
[6072,"i_平陆三期 VI-50 发电机定子U相线圈温度","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VI-50 发电机定子U相线圈温度","yc_hs_0005","cur_40"]
[6073,"i_平陆三期 VI-50 发电机定子V相线圈温度","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VI-50 发电机定子V相线圈温度","yc_hs_0005","cur_41"]
[6074,"i_平陆三期 VI-50 发电机定子W相线圈温度","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VI-50 发电机定子W相线圈温度","yc_hs_0005","cur_42"]
[6075,"i_平陆三期 VI-50 发电机转速","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VI-50 发电机转速","yc_hs_0005","cur_63"]
[6076,"i_平陆三期 VI-50 发电机有功功率","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VI-50 发电机有功功率","yc_hs_0005","cur_64"]
[6077,"i_平陆三期 VI-50 发电机驱动端轴承温度","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VI-50 发电机驱动端轴承温度","yc_hs_0005","cur_71"]
[6078,"i_平陆三期 VI-50 发电机非驱动端轴承温度","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VI-50 发电机非驱动端轴承温度","yc_hs_0005","cur_72"]
[6079,"i_平陆三期 VI-50 风轮（主轴）转速","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VI-50 风轮（主轴）转速","yc_hs_0006","cur_03"]
[6080,"i_平陆三期 VI-50 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VI-50 齿轮箱高速轴驱动端轴承温度","yc_hs_0006","cur_04"]
[6081,"i_平陆三期 VI-50 机舱角度（位置）","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VI-50 机舱角度（位置）","yc_hs_0006","cur_26"]
[6082,"i_平陆三期 VI-50 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VI-50 机舱侧向振动值(已滤波)","yc_hs_0006","cur_32"]
[6083,"i_平陆三期 VI-50 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",50,"YCPL.T3_L1.WTG050.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VI-50 机舱轴向振动值(已滤波)","yc_hs_0006","cur_33"]
[6084,"i_平陆三期 VI-51 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VI-51 齿轮箱中间轴非驱动端轴承温度","yc_hs_0006","cur_37"]
[6085,"i_平陆三期 VI-51 主轴承外圈温度","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VI-51 主轴承外圈温度","yc_hs_0006","cur_54"]
[6086,"i_平陆三期 VI-51 扭缆角度","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VI-51 扭缆角度","yc_hs_0006","cur_56"]
[6087,"i_平陆三期 VI-51 风速","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VI-51 风速","yc_hs_0006","cur_57"]
[6088,"i_平陆三期 VI-51 舱外温度","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VI-51 舱外温度","yc_hs_0006","cur_63"]
[6089,"i_平陆三期 VI-51 舱内温度","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VI-51 舱内温度","yc_hs_0006","cur_64"]
[6090,"i_平陆三期 VI-51 机舱与风向夹角","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VI-51 机舱与风向夹角","yc_hs_0006","cur_65"]
[6091,"i_平陆三期 VI-51 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VI-51 1#桨叶片角度(桨距角)","yc_hs_0006","cur_68"]
[6092,"i_平陆三期 VI-51 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VI-51 2#桨叶片角度(桨距角)","yc_hs_0006","cur_85"]
[6093,"i_平陆三期 VI-51 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VI-51 3#桨叶片角度(桨距角)","yc_hs_0006","cur_86"]
[6094,"i_平陆三期 VI-51 发电机定子U相线圈温度","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VI-51 发电机定子U相线圈温度","yc_hs_0006","cur_87"]
[6095,"i_平陆三期 VI-51 发电机定子V相线圈温度","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VI-51 发电机定子V相线圈温度","yc_hs_0006","cur_88"]
[6096,"i_平陆三期 VI-51 发电机定子W相线圈温度","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VI-51 发电机定子W相线圈温度","yc_hs_0006","cur_94"]
[6097,"i_平陆三期 VI-51 发电机转速","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VI-51 发电机转速","yc_hs_0006","cur_99"]
[6098,"i_平陆三期 VI-51 发电机有功功率","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VI-51 发电机有功功率","yc_hs_0007","cur_16"]
[6099,"i_平陆三期 VI-51 发电机驱动端轴承温度","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VI-51 发电机驱动端轴承温度","yc_hs_0007","cur_18"]
[6100,"i_平陆三期 VI-51 发电机非驱动端轴承温度","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VI-51 发电机非驱动端轴承温度","yc_hs_0007","cur_19"]
[6101,"i_平陆三期 VI-51 风轮（主轴）转速","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VI-51 风轮（主轴）转速","yc_hs_0007","cur_50"]
[6102,"i_平陆三期 VI-51 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VI-51 齿轮箱高速轴驱动端轴承温度","yc_hs_0007","cur_56"]
[6103,"i_平陆三期 VI-51 机舱角度（位置）","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VI-51 机舱角度（位置）","yc_hs_0007","cur_78"]
[6104,"i_平陆三期 VI-51 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VI-51 机舱侧向振动值(已滤波)","yc_hs_0007","cur_79"]
[6105,"i_平陆三期 VI-51 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VI-51 机舱轴向振动值(已滤波)","yc_hs_0007","cur_80"]
[6106,"i_平陆三期 VI-51 风向","平陆风电场","WOF35900004",51,"YCPL.T3_L1.WTG051.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VI-51 风向","yc_hs_0007","cur_89"]
[6107,"i_平陆三期 VI-52 风速","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VI-52 风速","yc_hs_0008","cur_12"]
[6108,"i_平陆三期 VI-52 舱外温度","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VI-52 舱外温度","yc_hs_0008","cur_18"]
[6109,"i_平陆三期 VI-52 舱内温度","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VI-52 舱内温度","yc_hs_0008","cur_19"]
[6110,"i_平陆三期 VI-52 机舱与风向夹角","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VI-52 机舱与风向夹角","yc_hs_0008","cur_20"]
[6111,"i_平陆三期 VI-52 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VI-52 1#桨叶片角度(桨距角)","yc_hs_0008","cur_23"]
[6112,"i_平陆三期 VI-52 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VI-52 2#桨叶片角度(桨距角)","yc_hs_0008","cur_40"]
[6113,"i_平陆三期 VI-52 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VI-52 3#桨叶片角度(桨距角)","yc_hs_0008","cur_41"]
[6114,"i_平陆三期 VI-52 发电机定子U相线圈温度","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VI-52 发电机定子U相线圈温度","yc_hs_0008","cur_42"]
[6115,"i_平陆三期 VI-52 发电机定子V相线圈温度","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VI-52 发电机定子V相线圈温度","yc_hs_0008","cur_43"]
[6116,"i_平陆三期 VI-52 发电机定子W相线圈温度","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VI-52 发电机定子W相线圈温度","yc_hs_0008","cur_49"]
[6117,"i_平陆三期 VI-52 发电机转速","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VI-52 发电机转速","yc_hs_0008","cur_54"]
[6118,"i_平陆三期 VI-52 发电机有功功率","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VI-52 发电机有功功率","yc_hs_0008","cur_71"]
[6119,"i_平陆三期 VI-52 发电机驱动端轴承温度","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VI-52 发电机驱动端轴承温度","yc_hs_0008","cur_73"]
[6120,"i_平陆三期 VI-52 发电机非驱动端轴承温度","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VI-52 发电机非驱动端轴承温度","yc_hs_0008","cur_74"]
[6121,"i_平陆三期 VI-52 风轮（主轴）转速","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VI-52 风轮（主轴）转速","yc_hs_0009","cur_05"]
[6122,"i_平陆三期 VI-52 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VI-52 齿轮箱高速轴驱动端轴承温度","yc_hs_0009","cur_11"]
[6123,"i_平陆三期 VI-52 机舱角度（位置）","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VI-52 机舱角度（位置）","yc_hs_0009","cur_33"]
[6124,"i_平陆三期 VI-52 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VI-52 机舱侧向振动值(已滤波)","yc_hs_0009","cur_34"]
[6125,"i_平陆三期 VI-52 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VI-52 机舱轴向振动值(已滤波)","yc_hs_0009","cur_35"]
[6126,"i_平陆三期 VI-52 风向","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VI-52 风向","yc_hs_0009","cur_44"]
[6127,"i_平陆三期 VI-52 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VI-52 齿轮箱中间轴非驱动端轴承温度","yc_hs_0009","cur_72"]
[6128,"i_平陆三期 VI-52 主轴承外圈温度","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VI-52 主轴承外圈温度","yc_hs_0009","cur_73"]
[6129,"i_平陆三期 VI-52 扭缆角度","平陆风电场","WOF35900004",52,"YCPL.T3_L1.WTG052.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VI-52 扭缆角度","yc_hs_0009","cur_75"]
[6130,"i_平陆三期 VI-53 发电机驱动端轴承温度","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VI-53 发电机驱动端轴承温度","yc_hs_0010","cur_05"]
[6131,"i_平陆三期 VI-53 发电机非驱动端轴承温度","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VI-53 发电机非驱动端轴承温度","yc_hs_0010","cur_07"]
[6132,"i_平陆三期 VI-53 风轮（主轴）转速","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VI-53 风轮（主轴）转速","yc_hs_0010","cur_37"]
[6133,"i_平陆三期 VI-53 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VI-53 齿轮箱高速轴驱动端轴承温度","yc_hs_0010","cur_54"]
[6134,"i_平陆三期 VI-53 机舱角度（位置）","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VI-53 机舱角度（位置）","yc_hs_0010","cur_63"]
[6135,"i_平陆三期 VI-53 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VI-53 机舱侧向振动值(已滤波)","yc_hs_0010","cur_64"]
[6136,"i_平陆三期 VI-53 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VI-53 机舱轴向振动值(已滤波)","yc_hs_0010","cur_65"]
[6137,"i_平陆三期 VI-53 风向","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VI-53 风向","yc_hs_0010","cur_86"]
[6138,"i_平陆三期 VI-53 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VI-53 齿轮箱中间轴非驱动端轴承温度","yc_hs_0011","cur_14"]
[6139,"i_平陆三期 VI-53 主轴承外圈温度","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VI-53 主轴承外圈温度","yc_hs_0011","cur_15"]
[6140,"i_平陆三期 VI-53 扭缆角度","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VI-53 扭缆角度","yc_hs_0011","cur_22"]
[6141,"i_平陆三期 VI-53 风速","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VI-53 风速","yc_hs_0011","cur_23"]
[6142,"i_平陆三期 VI-53 舱外温度","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VI-53 舱外温度","yc_hs_0011","cur_24"]
[6143,"i_平陆三期 VI-53 舱内温度","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VI-53 舱内温度","yc_hs_0011","cur_25"]
[6144,"i_平陆三期 VI-53 机舱与风向夹角","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VI-53 机舱与风向夹角","yc_hs_0011","cur_27"]
[6145,"i_平陆三期 VI-53 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VI-53 1#桨叶片角度(桨距角)","yc_hs_0011","cur_45"]
[6146,"i_平陆三期 VI-53 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VI-53 2#桨叶片角度(桨距角)","yc_hs_0011","cur_46"]
[6147,"i_平陆三期 VI-53 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VI-53 3#桨叶片角度(桨距角)","yc_hs_0011","cur_47"]
[6148,"i_平陆三期 VI-53 发电机定子U相线圈温度","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VI-53 发电机定子U相线圈温度","yc_hs_0009","cur_77"]
[6149,"i_平陆三期 VI-53 发电机定子V相线圈温度","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VI-53 发电机定子V相线圈温度","yc_hs_0009","cur_94"]
[6150,"i_平陆三期 VI-53 发电机定子W相线圈温度","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VI-53 发电机定子W相线圈温度","yc_hs_0009","cur_95"]
[6151,"i_平陆三期 VI-53 发电机转速","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VI-53 发电机转速","yc_hs_0010","cur_03"]
[6152,"i_平陆三期 VI-53 发电机有功功率","平陆风电场","WOF35900004",53,"YCPL.T3_L1.WTG053.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VI-53 发电机有功功率","yc_hs_0010","cur_04"]
[6153,"i_平陆三期 VI-54 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VI-54 齿轮箱中间轴非驱动端轴承温度","yc_hs_0011","cur_57"]
[6154,"i_平陆三期 VI-54 主轴承外圈温度","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VI-54 主轴承外圈温度","yc_hs_0011","cur_74"]
[6155,"i_平陆三期 VI-54 扭缆角度","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VI-54 扭缆角度","yc_hs_0011","cur_76"]
[6156,"i_平陆三期 VI-54 风轮（主轴）转速","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VI-54 风轮（主轴）转速","yc_hs_0012","cur_04"]
[6157,"i_平陆三期 VI-54 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VI-54 齿轮箱高速轴驱动端轴承温度","yc_hs_0012","cur_05"]
[6158,"i_平陆三期 VI-54 机舱角度（位置）","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VI-54 机舱角度（位置）","yc_hs_0012","cur_14"]
[6159,"i_平陆三期 VI-54 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VI-54 机舱侧向振动值(已滤波)","yc_hs_0012","cur_15"]
[6160,"i_平陆三期 VI-54 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VI-54 机舱轴向振动值(已滤波)","yc_hs_0012","cur_17"]
[6161,"i_平陆三期 VI-54 风向","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VI-54 风向","yc_hs_0012","cur_37"]
[6162,"i_平陆三期 VI-54 风速","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VI-54 风速","yc_hs_0012","cur_44"]
[6163,"i_平陆三期 VI-54 舱外温度","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VI-54 舱外温度","yc_hs_0012","cur_45"]
[6164,"i_平陆三期 VI-54 舱内温度","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VI-54 舱内温度","yc_hs_0012","cur_47"]
[6165,"i_平陆三期 VI-54 机舱与风向夹角","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VI-54 机舱与风向夹角","yc_hs_0012","cur_64"]
[6166,"i_平陆三期 VI-54 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VI-54 1#桨叶片角度(桨距角)","yc_hs_0012","cur_66"]
[6167,"i_平陆三期 VI-54 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VI-54 2#桨叶片角度(桨距角)","yc_hs_0012","cur_67"]
[6168,"i_平陆三期 VI-54 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VI-54 3#桨叶片角度(桨距角)","yc_hs_0012","cur_72"]
[6169,"i_平陆三期 VI-54 发电机定子U相线圈温度","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VI-54 发电机定子U相线圈温度","yc_hs_0012","cur_73"]
[6170,"i_平陆三期 VI-54 发电机定子V相线圈温度","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VI-54 发电机定子V相线圈温度","yc_hs_0012","cur_74"]
[6171,"i_平陆三期 VI-54 发电机定子W相线圈温度","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VI-54 发电机定子W相线圈温度","yc_hs_0012","cur_75"]
[6172,"i_平陆三期 VI-54 发电机转速","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VI-54 发电机转速","yc_hs_0012","cur_96"]
[6173,"i_平陆三期 VI-54 发电机有功功率","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VI-54 发电机有功功率","yc_hs_0012","cur_97"]
[6174,"i_平陆三期 VI-54 发电机驱动端轴承温度","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VI-54 发电机驱动端轴承温度","yc_hs_0013","cur_03"]
[6175,"i_平陆三期 VI-54 发电机非驱动端轴承温度","平陆风电场","WOF35900004",54,"YCPL.T3_L1.WTG054.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VI-54 发电机非驱动端轴承温度","yc_hs_0013","cur_04"]
[6176,"i_平陆三期 VI-55 风轮（主轴）转速","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VI-55 风轮（主轴）转速","yc_hs_0013","cur_54"]
[6177,"i_平陆三期 VI-55 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VI-55 齿轮箱高速轴驱动端轴承温度","yc_hs_0013","cur_55"]
[6178,"i_平陆三期 VI-55 机舱角度（位置）","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VI-55 机舱角度（位置）","yc_hs_0013","cur_64"]
[6179,"i_平陆三期 VI-55 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VI-55 机舱侧向振动值(已滤波)","yc_hs_0013","cur_65"]
[6180,"i_平陆三期 VI-55 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VI-55 机舱轴向振动值(已滤波)","yc_hs_0013","cur_67"]
[6181,"i_平陆三期 VI-55 风向","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VI-55 风向","yc_hs_0013","cur_87"]
[6182,"i_平陆三期 VI-55 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VI-55 齿轮箱中间轴非驱动端轴承温度","yc_hs_0014","cur_15"]
[6183,"i_平陆三期 VI-55 主轴承外圈温度","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VI-55 主轴承外圈温度","yc_hs_0014","cur_16"]
[6184,"i_平陆三期 VI-55 扭缆角度","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VI-55 扭缆角度","yc_hs_0014","cur_22"]
[6185,"i_平陆三期 VI-55 风速","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VI-55 风速","yc_hs_0014","cur_23"]
[6186,"i_平陆三期 VI-55 舱外温度","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VI-55 舱外温度","yc_hs_0014","cur_24"]
[6187,"i_平陆三期 VI-55 舱内温度","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VI-55 舱内温度","yc_hs_0014","cur_25"]
[6188,"i_平陆三期 VI-55 机舱与风向夹角","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VI-55 机舱与风向夹角","yc_hs_0014","cur_27"]
[6189,"i_平陆三期 VI-55 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VI-55 1#桨叶片角度(桨距角)","yc_hs_0014","cur_45"]
[6190,"i_平陆三期 VI-55 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VI-55 2#桨叶片角度(桨距角)","yc_hs_0014","cur_46"]
[6191,"i_平陆三期 VI-55 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VI-55 3#桨叶片角度(桨距角)","yc_hs_0014","cur_47"]
[6192,"i_平陆三期 VI-55 发电机定子U相线圈温度","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VI-55 发电机定子U相线圈温度","yc_hs_0014","cur_52"]
[6193,"i_平陆三期 VI-55 发电机定子V相线圈温度","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VI-55 发电机定子V相线圈温度","yc_hs_0014","cur_53"]
[6194,"i_平陆三期 VI-55 发电机定子W相线圈温度","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VI-55 发电机定子W相线圈温度","yc_hs_0014","cur_54"]
[6195,"i_平陆三期 VI-55 发电机转速","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VI-55 发电机转速","yc_hs_0014","cur_75"]
[6196,"i_平陆三期 VI-55 发电机有功功率","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VI-55 发电机有功功率","yc_hs_0014","cur_76"]
[6197,"i_平陆三期 VI-55 发电机驱动端轴承温度","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VI-55 发电机驱动端轴承温度","yc_hs_0014","cur_82"]
[6198,"i_平陆三期 VI-55 发电机非驱动端轴承温度","平陆风电场","WOF35900004",55,"YCPL.T3_L1.WTG055.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VI-55 发电机非驱动端轴承温度","yc_hs_0013","cur_24"]
[6199,"i_平陆三期 VI-56 风速","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VI-56 风速","yc_hs_0014","cur_83"]
[6200,"i_平陆三期 VI-56 舱外温度","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VI-56 舱外温度","yc_hs_0014","cur_84"]
[6201,"i_平陆三期 VI-56 舱内温度","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VI-56 舱内温度","yc_hs_0014","cur_85"]
[6202,"i_平陆三期 VI-56 机舱与风向夹角","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VI-56 机舱与风向夹角","yc_hs_0014","cur_87"]
[6203,"i_平陆三期 VI-56 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VI-56 1#桨叶片角度(桨距角)","yc_hs_0015","cur_05"]
[6204,"i_平陆三期 VI-56 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VI-56 2#桨叶片角度(桨距角)","yc_hs_0015","cur_06"]
[6205,"i_平陆三期 VI-56 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VI-56 3#桨叶片角度(桨距角)","yc_hs_0015","cur_07"]
[6206,"i_平陆三期 VI-56 发电机定子U相线圈温度","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VI-56 发电机定子U相线圈温度","yc_hs_0015","cur_12"]
[6207,"i_平陆三期 VI-56 发电机定子V相线圈温度","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VI-56 发电机定子V相线圈温度","yc_hs_0015","cur_13"]
[6208,"i_平陆三期 VI-56 发电机定子W相线圈温度","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VI-56 发电机定子W相线圈温度","yc_hs_0015","cur_14"]
[6209,"i_平陆三期 VI-56 发电机转速","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VI-56 发电机转速","yc_hs_0015","cur_35"]
[6210,"i_平陆三期 VI-56 发电机有功功率","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VI-56 发电机有功功率","yc_hs_0015","cur_36"]
[6211,"i_平陆三期 VI-56 发电机驱动端轴承温度","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VI-56 发电机驱动端轴承温度","yc_hs_0015","cur_42"]
[6212,"i_平陆三期 VI-56 发电机非驱动端轴承温度","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VI-56 发电机非驱动端轴承温度","yc_hs_0015","cur_43"]
[6213,"i_平陆三期 VI-56 风轮（主轴）转速","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VI-56 风轮（主轴）转速","yc_hs_0015","cur_73"]
[6214,"i_平陆三期 VI-56 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VI-56 齿轮箱高速轴驱动端轴承温度","yc_hs_0015","cur_74"]
[6215,"i_平陆三期 VI-56 机舱角度（位置）","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VI-56 机舱角度（位置）","yc_hs_0015","cur_96"]
[6216,"i_平陆三期 VI-56 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VI-56 机舱侧向振动值(已滤波)","yc_hs_0015","cur_97"]
[6217,"i_平陆三期 VI-56 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VI-56 机舱轴向振动值(已滤波)","yc_hs_0016","cur_02"]
[6218,"i_平陆三期 VI-56 风向","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VI-56 风向","yc_hs_0016","cur_07"]
[6219,"i_平陆三期 VI-56 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VI-56 齿轮箱中间轴非驱动端轴承温度","yc_hs_0016","cur_34"]
[6220,"i_平陆三期 VI-56 主轴承外圈温度","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VI-56 主轴承外圈温度","yc_hs_0016","cur_35"]
[6221,"i_平陆三期 VI-56 扭缆角度","平陆风电场","WOF35900004",56,"YCPL.T3_L1.WTG056.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VI-56 扭缆角度","yc_hs_0016","cur_54"]
[6222,"i_平陆三期 VI-57 风速","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VI-57 风速","yc_hs_0016","cur_55"]
[6223,"i_平陆三期 VI-57 舱外温度","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VI-57 舱外温度","yc_hs_0016","cur_56"]
[6224,"i_平陆三期 VI-57 舱内温度","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VI-57 舱内温度","yc_hs_0016","cur_57"]
[6225,"i_平陆三期 VI-57 机舱与风向夹角","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VI-57 机舱与风向夹角","yc_hs_0016","cur_62"]
[6226,"i_平陆三期 VI-57 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VI-57 1#桨叶片角度(桨距角)","yc_hs_0016","cur_64"]
[6227,"i_平陆三期 VI-57 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VI-57 2#桨叶片角度(桨距角)","yc_hs_0016","cur_65"]
[6228,"i_平陆三期 VI-57 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VI-57 3#桨叶片角度(桨距角)","yc_hs_0016","cur_67"]
[6229,"i_平陆三期 VI-57 发电机定子U相线圈温度","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VI-57 发电机定子U相线圈温度","yc_hs_0016","cur_92"]
[6230,"i_平陆三期 VI-57 发电机定子V相线圈温度","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VI-57 发电机定子V相线圈温度","yc_hs_0016","cur_94"]
[6231,"i_平陆三期 VI-57 发电机定子W相线圈温度","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VI-57 发电机定子W相线圈温度","yc_hs_0016","cur_96"]
[6232,"i_平陆三期 VI-57 发电机转速","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VI-57 发电机转速","yc_hs_0103","cur_01"]
[6233,"i_平陆三期 VI-57 发电机有功功率","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VI-57 发电机有功功率","yc_hs_0103","cur_02"]
[6234,"i_平陆三期 VI-57 发电机驱动端轴承温度","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VI-57 发电机驱动端轴承温度","yc_hs_0103","cur_04"]
[6235,"i_平陆三期 VI-57 发电机非驱动端轴承温度","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VI-57 发电机非驱动端轴承温度","yc_hs_0103","cur_22"]
[6236,"i_平陆三期 VI-57 风轮（主轴）转速","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VI-57 风轮（主轴）转速","yc_hs_0103","cur_42"]
[6237,"i_平陆三期 VI-57 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VI-57 齿轮箱高速轴驱动端轴承温度","yc_hs_0103","cur_43"]
[6238,"i_平陆三期 VI-57 机舱角度（位置）","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VI-57 机舱角度（位置）","yc_hs_0103","cur_52"]
[6239,"i_平陆三期 VI-57 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VI-57 机舱侧向振动值(已滤波)","yc_hs_0103","cur_53"]
[6240,"i_平陆三期 VI-57 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VI-57 机舱轴向振动值(已滤波)","yc_hs_0103","cur_54"]
[6241,"i_平陆三期 VI-57 风向","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VI-57 风向","yc_hs_0103","cur_58"]
[6242,"i_平陆三期 VI-57 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VI-57 齿轮箱中间轴非驱动端轴承温度","yc_hs_0103","cur_71"]
[6243,"i_平陆三期 VI-57 主轴承外圈温度","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VI-57 主轴承外圈温度","yc_hs_0103","cur_72"]
[6244,"i_平陆三期 VI-57 扭缆角度","平陆风电场","WOF35900004",57,"YCPL.T3_L1.WTG057.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VI-57 扭缆角度","yc_hs_0103","cur_82"]
[6245,"i_平陆三期 VI-58 发电机定子U相线圈温度","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VI-58 发电机定子U相线圈温度","yc_hs_0103","cur_83"]
[6246,"i_平陆三期 VI-58 发电机定子V相线圈温度","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VI-58 发电机定子V相线圈温度","yc_hs_0103","cur_84"]
[6247,"i_平陆三期 VI-58 发电机定子W相线圈温度","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VI-58 发电机定子W相线圈温度","yc_hs_0103","cur_85"]
[6248,"i_平陆三期 VI-58 发电机转速","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VI-58 发电机转速","yc_hs_0103","cur_89"]
[6249,"i_平陆三期 VI-58 发电机有功功率","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VI-58 发电机有功功率","yc_hs_0103","cur_91"]
[6250,"i_平陆三期 VI-58 发电机驱动端轴承温度","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VI-58 发电机驱动端轴承温度","yc_hs_0103","cur_95"]
[6251,"i_平陆三期 VI-58 发电机非驱动端轴承温度","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VI-58 发电机非驱动端轴承温度","yc_hs_0103","cur_96"]
[6252,"i_平陆三期 VI-58 风轮（主轴）转速","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VI-58 风轮（主轴）转速","yc_hs_0104","cur_05"]
[6253,"i_平陆三期 VI-58 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VI-58 齿轮箱高速轴驱动端轴承温度","yc_hs_0104","cur_07"]
[6254,"i_平陆三期 VI-58 机舱角度（位置）","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VI-58 机舱角度（位置）","yc_hs_0104","cur_17"]
[6255,"i_平陆三期 VI-58 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VI-58 机舱侧向振动值(已滤波)","yc_hs_0104","cur_18"]
[6256,"i_平陆三期 VI-58 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VI-58 机舱轴向振动值(已滤波)","yc_hs_0104","cur_27"]
[6257,"i_平陆三期 VI-58 风向","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VI-58 风向","yc_hs_0104","cur_31"]
[6258,"i_平陆三期 VI-58 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VI-58 齿轮箱中间轴非驱动端轴承温度","yc_hs_0104","cur_41"]
[6259,"i_平陆三期 VI-58 主轴承外圈温度","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VI-58 主轴承外圈温度","yc_hs_0104","cur_42"]
[6260,"i_平陆三期 VI-58 扭缆角度","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VI-58 扭缆角度","yc_hs_0104","cur_44"]
[6261,"i_平陆三期 VI-58 风速","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VI-58 风速","yc_hs_0104","cur_45"]
[6262,"i_平陆三期 VI-58 舱外温度","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VI-58 舱外温度","yc_hs_0104","cur_46"]
[6263,"i_平陆三期 VI-58 舱内温度","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VI-58 舱内温度","yc_hs_0104","cur_47"]
[6264,"i_平陆三期 VI-58 机舱与风向夹角","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VI-58 机舱与风向夹角","yc_hs_0104","cur_48"]
[6265,"i_平陆三期 VI-58 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VI-58 1#桨叶片角度(桨距角)","yc_hs_0104","cur_50"]
[6266,"i_平陆三期 VI-58 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VI-58 2#桨叶片角度(桨距角)","yc_hs_0104","cur_52"]
[6267,"i_平陆三期 VI-58 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",58,"YCPL.T3_L1.WTG058.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VI-58 3#桨叶片角度(桨距角)","yc_hs_0104","cur_54"]
[6268,"i_平陆三期 VI-59 风速","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VI-59 风速","yc_hs_0104","cur_97"]
[6269,"i_平陆三期 VI-59 舱外温度","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VI-59 舱外温度","yc_hs_0104","cur_99"]
[6270,"i_平陆三期 VI-59 舱内温度","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VI-59 舱内温度","yc_hs_0105","cur_04"]
[6271,"i_平陆三期 VI-59 机舱与风向夹角","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VI-59 机舱与风向夹角","yc_hs_0105","cur_05"]
[6272,"i_平陆三期 VI-59 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VI-59 1#桨叶片角度(桨距角)","yc_hs_0105","cur_07"]
[6273,"i_平陆三期 VI-59 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VI-59 2#桨叶片角度(桨距角)","yc_hs_0105","cur_08"]
[6274,"i_平陆三期 VI-59 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VI-59 3#桨叶片角度(桨距角)","yc_hs_0105","cur_17"]
[6275,"i_平陆三期 VI-59 发电机定子U相线圈温度","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VI-59 发电机定子U相线圈温度","yc_hs_0105","cur_18"]
[6276,"i_平陆三期 VI-59 发电机定子V相线圈温度","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VI-59 发电机定子V相线圈温度","yc_hs_0105","cur_19"]
[6277,"i_平陆三期 VI-59 发电机定子W相线圈温度","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VI-59 发电机定子W相线圈温度","yc_hs_0105","cur_20"]
[6278,"i_平陆三期 VI-59 发电机转速","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VI-59 发电机转速","yc_hs_0105","cur_24"]
[6279,"i_平陆三期 VI-59 发电机有功功率","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VI-59 发电机有功功率","yc_hs_0105","cur_26"]
[6280,"i_平陆三期 VI-59 发电机驱动端轴承温度","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VI-59 发电机驱动端轴承温度","yc_hs_0105","cur_30"]
[6281,"i_平陆三期 VI-59 发电机非驱动端轴承温度","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VI-59 发电机非驱动端轴承温度","yc_hs_0105","cur_31"]
[6282,"i_平陆三期 VI-59 风轮（主轴）转速","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VI-59 风轮（主轴）转速","yc_hs_0104","cur_62"]
[6283,"i_平陆三期 VI-59 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VI-59 齿轮箱高速轴驱动端轴承温度","yc_hs_0104","cur_63"]
[6284,"i_平陆三期 VI-59 机舱角度（位置）","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VI-59 机舱角度（位置）","yc_hs_0104","cur_76"]
[6285,"i_平陆三期 VI-59 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VI-59 机舱侧向振动值(已滤波)","yc_hs_0104","cur_77"]
[6286,"i_平陆三期 VI-59 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VI-59 机舱轴向振动值(已滤波)","yc_hs_0104","cur_78"]
[6287,"i_平陆三期 VI-59 风向","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VI-59 风向","yc_hs_0104","cur_85"]
[6288,"i_平陆三期 VI-59 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VI-59 齿轮箱中间轴非驱动端轴承温度","yc_hs_0104","cur_92"]
[6289,"i_平陆三期 VI-59 主轴承外圈温度","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VI-59 主轴承外圈温度","yc_hs_0104","cur_93"]
[6290,"i_平陆三期 VI-59 扭缆角度","平陆风电场","WOF35900004",59,"YCPL.T3_L1.WTG059.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VI-59 扭缆角度","yc_hs_0104","cur_95"]
[6291,"i_平陆三期 VI-60 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VI-60 齿轮箱中间轴非驱动端轴承温度","yc_hs_0105","cur_81"]
[6292,"i_平陆三期 VI-60 主轴承外圈温度","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VI-60 主轴承外圈温度","yc_hs_0105","cur_82"]
[6293,"i_平陆三期 VI-60 扭缆角度","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VI-60 扭缆角度","yc_hs_0105","cur_84"]
[6294,"i_平陆三期 VI-60 风速","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VI-60 风速","yc_hs_0105","cur_85"]
[6295,"i_平陆三期 VI-60 舱外温度","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VI-60 舱外温度","yc_hs_0105","cur_87"]
[6296,"i_平陆三期 VI-60 舱内温度","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VI-60 舱内温度","yc_hs_0105","cur_89"]
[6297,"i_平陆三期 VI-60 机舱与风向夹角","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VI-60 机舱与风向夹角","yc_hs_0105","cur_94"]
[6298,"i_平陆三期 VI-60 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VI-60 1#桨叶片角度(桨距角)","yc_hs_0105","cur_96"]
[6299,"i_平陆三期 VI-60 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VI-60 2#桨叶片角度(桨距角)","yc_hs_0105","cur_97"]
[6300,"i_平陆三期 VI-60 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VI-60 3#桨叶片角度(桨距角)","yc_hs_0105","cur_98"]
[6301,"i_平陆三期 VI-60 发电机定子U相线圈温度","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VI-60 发电机定子U相线圈温度","yc_hs_0105","cur_99"]
[6302,"i_平陆三期 VI-60 发电机定子V相线圈温度","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VI-60 发电机定子V相线圈温度","yc_hs_0105","cur_100"]
[6303,"i_平陆三期 VI-60 发电机定子W相线圈温度","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VI-60 发电机定子W相线圈温度","yc_hs_0106","cur_01"]
[6304,"i_平陆三期 VI-60 发电机转速","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VI-60 发电机转速","yc_hs_0106","cur_13"]
[6305,"i_平陆三期 VI-60 发电机有功功率","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VI-60 发电机有功功率","yc_hs_0106","cur_14"]
[6306,"i_平陆三期 VI-60 发电机驱动端轴承温度","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VI-60 发电机驱动端轴承温度","yc_hs_0106","cur_16"]
[6307,"i_平陆三期 VI-60 发电机非驱动端轴承温度","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VI-60 发电机非驱动端轴承温度","yc_hs_0106","cur_17"]
[6308,"i_平陆三期 VI-60 风轮（主轴）转速","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VI-60 风轮（主轴）转速","yc_hs_0105","cur_51"]
[6309,"i_平陆三期 VI-60 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VI-60 齿轮箱高速轴驱动端轴承温度","yc_hs_0105","cur_52"]
[6310,"i_平陆三期 VI-60 机舱角度（位置）","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VI-60 机舱角度（位置）","yc_hs_0105","cur_65"]
[6311,"i_平陆三期 VI-60 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VI-60 机舱侧向振动值(已滤波)","yc_hs_0105","cur_66"]
[6312,"i_平陆三期 VI-60 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VI-60 机舱轴向振动值(已滤波)","yc_hs_0105","cur_67"]
[6313,"i_平陆三期 VI-60 风向","平陆风电场","WOF35900004",60,"YCPL.T3_L1.WTG060.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VI-60 风向","yc_hs_0105","cur_73"]
[6314,"i_平陆三期 VII-62 风速","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VII-62 风速","yc_hs_0106","cur_19"]
[6315,"i_平陆三期 VII-62 舱外温度","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VII-62 舱外温度","yc_hs_0106","cur_21"]
[6316,"i_平陆三期 VII-62 舱内温度","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VII-62 舱内温度","yc_hs_0106","cur_23"]
[6317,"i_平陆三期 VII-62 机舱与风向夹角","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VII-62 机舱与风向夹角","yc_hs_0106","cur_24"]
[6318,"i_平陆三期 VII-62 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VII-62 1#桨叶片角度(桨距角)","yc_hs_0106","cur_26"]
[6319,"i_平陆三期 VII-62 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VII-62 2#桨叶片角度(桨距角)","yc_hs_0106","cur_27"]
[6320,"i_平陆三期 VII-62 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VII-62 3#桨叶片角度(桨距角)","yc_hs_0106","cur_28"]
[6321,"i_平陆三期 VII-62 发电机定子U相线圈温度","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VII-62 发电机定子U相线圈温度","yc_hs_0106","cur_29"]
[6322,"i_平陆三期 VII-62 发电机定子V相线圈温度","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VII-62 发电机定子V相线圈温度","yc_hs_0106","cur_30"]
[6323,"i_平陆三期 VII-62 发电机定子W相线圈温度","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VII-62 发电机定子W相线圈温度","yc_hs_0106","cur_31"]
[6324,"i_平陆三期 VII-62 发电机转速","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VII-62 发电机转速","yc_hs_0106","cur_37"]
[6325,"i_平陆三期 VII-62 发电机有功功率","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VII-62 发电机有功功率","yc_hs_0106","cur_42"]
[6326,"i_平陆三期 VII-62 发电机驱动端轴承温度","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VII-62 发电机驱动端轴承温度","yc_hs_0106","cur_44"]
[6327,"i_平陆三期 VII-62 发电机非驱动端轴承温度","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VII-62 发电机非驱动端轴承温度","yc_hs_0106","cur_45"]
[6328,"i_平陆三期 VII-62 风轮（主轴）转速","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VII-62 风轮（主轴）转速","yc_hs_0106","cur_62"]
[6329,"i_平陆三期 VII-62 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VII-62 齿轮箱高速轴驱动端轴承温度","yc_hs_0106","cur_64"]
[6330,"i_平陆三期 VII-62 机舱角度（位置）","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VII-62 机舱角度（位置）","yc_hs_0106","cur_71"]
[6331,"i_平陆三期 VII-62 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VII-62 机舱侧向振动值(已滤波)","yc_hs_0106","cur_72"]
[6332,"i_平陆三期 VII-62 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VII-62 机舱轴向振动值(已滤波)","yc_hs_0106","cur_73"]
[6333,"i_平陆三期 VII-62 风向","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VII-62 风向","yc_hs_0106","cur_77"]
[6334,"i_平陆三期 VII-62 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VII-62 齿轮箱中间轴非驱动端轴承温度","yc_hs_0106","cur_90"]
[6335,"i_平陆三期 VII-62 主轴承外圈温度","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VII-62 主轴承外圈温度","yc_hs_0106","cur_91"]
[6336,"i_平陆三期 VII-62 扭缆角度","平陆风电场","WOF35900004",62,"YCPL.T3_L2.WTG062.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VII-62 扭缆角度","yc_hs_0107","cur_01"]
[6337,"i_平陆三期 VII-63 风速","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VII-63 风速","yc_hs_0107","cur_02"]
[6338,"i_平陆三期 VII-63 舱外温度","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VII-63 舱外温度","yc_hs_0107","cur_03"]
[6339,"i_平陆三期 VII-63 舱内温度","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VII-63 舱内温度","yc_hs_0107","cur_04"]
[6340,"i_平陆三期 VII-63 机舱与风向夹角","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VII-63 机舱与风向夹角","yc_hs_0107","cur_05"]
[6341,"i_平陆三期 VII-63 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VII-63 1#桨叶片角度(桨距角)","yc_hs_0107","cur_07"]
[6342,"i_平陆三期 VII-63 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VII-63 2#桨叶片角度(桨距角)","yc_hs_0107","cur_09"]
[6343,"i_平陆三期 VII-63 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VII-63 3#桨叶片角度(桨距角)","yc_hs_0107","cur_11"]
[6344,"i_平陆三期 VII-63 发电机定子U相线圈温度","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VII-63 发电机定子U相线圈温度","yc_hs_0107","cur_13"]
[6345,"i_平陆三期 VII-63 发电机定子V相线圈温度","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VII-63 发电机定子V相线圈温度","yc_hs_0107","cur_14"]
[6346,"i_平陆三期 VII-63 发电机定子W相线圈温度","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VII-63 发电机定子W相线圈温度","yc_hs_0107","cur_15"]
[6347,"i_平陆三期 VII-63 发电机转速","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VII-63 发电机转速","yc_hs_0107","cur_19"]
[6348,"i_平陆三期 VII-63 发电机有功功率","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VII-63 发电机有功功率","yc_hs_0107","cur_20"]
[6349,"i_平陆三期 VII-63 发电机驱动端轴承温度","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VII-63 发电机驱动端轴承温度","yc_hs_0107","cur_22"]
[6350,"i_平陆三期 VII-63 发电机非驱动端轴承温度","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VII-63 发电机非驱动端轴承温度","yc_hs_0107","cur_23"]
[6351,"i_平陆三期 VII-63 风轮（主轴）转速","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VII-63 风轮（主轴）转速","yc_hs_0107","cur_46"]
[6352,"i_平陆三期 VII-63 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VII-63 齿轮箱高速轴驱动端轴承温度","yc_hs_0107","cur_47"]
[6353,"i_平陆三期 VII-63 机舱角度（位置）","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VII-63 机舱角度（位置）","yc_hs_0107","cur_52"]
[6354,"i_平陆三期 VII-63 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VII-63 机舱侧向振动值(已滤波)","yc_hs_0107","cur_54"]
[6355,"i_平陆三期 VII-63 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VII-63 机舱轴向振动值(已滤波)","yc_hs_0107","cur_56"]
[6356,"i_平陆三期 VII-63 风向","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VII-63 风向","yc_hs_0107","cur_61"]
[6357,"i_平陆三期 VII-63 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VII-63 齿轮箱中间轴非驱动端轴承温度","yc_hs_0107","cur_68"]
[6358,"i_平陆三期 VII-63 主轴承外圈温度","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VII-63 主轴承外圈温度","yc_hs_0107","cur_70"]
[6359,"i_平陆三期 VII-63 扭缆角度","平陆风电场","WOF35900004",63,"YCPL.T3_L2.WTG063.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VII-63 扭缆角度","yc_hs_0107","cur_77"]
[6360,"i_平陆三期 VII-64 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VII-64 齿轮箱中间轴非驱动端轴承温度","yc_hs_0107","cur_80"]
[6361,"i_平陆三期 VII-64 主轴承外圈温度","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VII-64 主轴承外圈温度","yc_hs_0107","cur_81"]
[6362,"i_平陆三期 VII-64 扭缆角度","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VII-64 扭缆角度","yc_hs_0107","cur_91"]
[6363,"i_平陆三期 VII-64 风速","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VII-64 风速","yc_hs_0107","cur_92"]
[6364,"i_平陆三期 VII-64 舱外温度","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VII-64 舱外温度","yc_hs_0107","cur_93"]
[6365,"i_平陆三期 VII-64 舱内温度","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VII-64 舱内温度","yc_hs_0107","cur_94"]
[6366,"i_平陆三期 VII-64 机舱与风向夹角","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VII-64 机舱与风向夹角","yc_hs_0107","cur_95"]
[6367,"i_平陆三期 VII-64 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VII-64 1#桨叶片角度(桨距角)","yc_hs_0107","cur_97"]
[6368,"i_平陆三期 VII-64 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VII-64 2#桨叶片角度(桨距角)","yc_hs_0107","cur_99"]
[6369,"i_平陆三期 VII-64 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VII-64 3#桨叶片角度(桨距角)","yc_hs_0108","cur_01"]
[6370,"i_平陆三期 VII-64 发电机定子U相线圈温度","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VII-64 发电机定子U相线圈温度","yc_hs_0108","cur_03"]
[6371,"i_平陆三期 VII-64 发电机定子V相线圈温度","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VII-64 发电机定子V相线圈温度","yc_hs_0108","cur_04"]
[6372,"i_平陆三期 VII-64 发电机定子W相线圈温度","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VII-64 发电机定子W相线圈温度","yc_hs_0108","cur_05"]
[6373,"i_平陆三期 VII-64 发电机转速","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VII-64 发电机转速","yc_hs_0108","cur_09"]
[6374,"i_平陆三期 VII-64 发电机有功功率","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VII-64 发电机有功功率","yc_hs_0108","cur_10"]
[6375,"i_平陆三期 VII-64 发电机驱动端轴承温度","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VII-64 发电机驱动端轴承温度","yc_hs_0108","cur_12"]
[6376,"i_平陆三期 VII-64 发电机非驱动端轴承温度","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VII-64 发电机非驱动端轴承温度","yc_hs_0108","cur_13"]
[6377,"i_平陆三期 VII-64 风轮（主轴）转速","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VII-64 风轮（主轴）转速","yc_hs_0108","cur_36"]
[6378,"i_平陆三期 VII-64 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VII-64 齿轮箱高速轴驱动端轴承温度","yc_hs_0108","cur_37"]
[6379,"i_平陆三期 VII-64 机舱角度（位置）","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VII-64 机舱角度（位置）","yc_hs_0108","cur_42"]
[6380,"i_平陆三期 VII-64 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VII-64 机舱侧向振动值(已滤波)","yc_hs_0108","cur_44"]
[6381,"i_平陆三期 VII-64 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VII-64 机舱轴向振动值(已滤波)","yc_hs_0108","cur_46"]
[6382,"i_平陆三期 VII-64 风向","平陆风电场","WOF35900004",64,"YCPL.T3_L2.WTG064.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VII-64 风向","yc_hs_0108","cur_51"]
[6383,"i_平陆三期 VII-65 风速","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VII-65 风速","yc_hs_0108","cur_56"]
[6384,"i_平陆三期 VII-65 舱外温度","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VII-65 舱外温度","yc_hs_0108","cur_57"]
[6385,"i_平陆三期 VII-65 舱内温度","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VII-65 舱内温度","yc_hs_0108","cur_58"]
[6386,"i_平陆三期 VII-65 机舱与风向夹角","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VII-65 机舱与风向夹角","yc_hs_0108","cur_60"]
[6387,"i_平陆三期 VII-65 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VII-65 1#桨叶片角度(桨距角)","yc_hs_0108","cur_67"]
[6388,"i_平陆三期 VII-65 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VII-65 2#桨叶片角度(桨距角)","yc_hs_0108","cur_68"]
[6389,"i_平陆三期 VII-65 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VII-65 3#桨叶片角度(桨距角)","yc_hs_0108","cur_69"]
[6390,"i_平陆三期 VII-65 发电机定子U相线圈温度","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VII-65 发电机定子U相线圈温度","yc_hs_0108","cur_70"]
[6391,"i_平陆三期 VII-65 发电机定子V相线圈温度","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VII-65 发电机定子V相线圈温度","yc_hs_0108","cur_71"]
[6392,"i_平陆三期 VII-65 发电机定子W相线圈温度","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VII-65 发电机定子W相线圈温度","yc_hs_0108","cur_80"]
[6393,"i_平陆三期 VII-65 发电机转速","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VII-65 发电机转速","yc_hs_0108","cur_84"]
[6394,"i_平陆三期 VII-65 发电机有功功率","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VII-65 发电机有功功率","yc_hs_0108","cur_85"]
[6395,"i_平陆三期 VII-65 发电机驱动端轴承温度","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VII-65 发电机驱动端轴承温度","yc_hs_0108","cur_87"]
[6396,"i_平陆三期 VII-65 发电机非驱动端轴承温度","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VII-65 发电机非驱动端轴承温度","yc_hs_0108","cur_89"]
[6397,"i_平陆三期 VII-65 风轮（主轴）转速","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VII-65 风轮（主轴）转速","yc_hs_0108","cur_100"]
[6398,"i_平陆三期 VII-65 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VII-65 齿轮箱高速轴驱动端轴承温度","yc_hs_0109","cur_01"]
[6399,"i_平陆三期 VII-65 机舱角度（位置）","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VII-65 机舱角度（位置）","yc_hs_0109","cur_12"]
[6400,"i_平陆三期 VII-65 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VII-65 机舱侧向振动值(已滤波)","yc_hs_0109","cur_13"]
[6401,"i_平陆三期 VII-65 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VII-65 机舱轴向振动值(已滤波)","yc_hs_0109","cur_14"]
[6402,"i_平陆三期 VII-65 风向","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VII-65 风向","yc_hs_0109","cur_26"]
[6403,"i_平陆三期 VII-65 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VII-65 齿轮箱中间轴非驱动端轴承温度","yc_hs_0109","cur_34"]
[6404,"i_平陆三期 VII-65 主轴承外圈温度","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VII-65 主轴承外圈温度","yc_hs_0109","cur_36"]
[6405,"i_平陆三期 VII-65 扭缆角度","平陆风电场","WOF35900004",65,"YCPL.T3_L2.WTG065.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VII-65 扭缆角度","yc_hs_0109","cur_39"]
[6406,"i_平陆三期 VII-66 风速","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VII-66 风速","yc_hs_0109","cur_40"]
[6407,"i_平陆三期 VII-66 舱外温度","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VII-66 舱外温度","yc_hs_0109","cur_41"]
[6408,"i_平陆三期 VII-66 舱内温度","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VII-66 舱内温度","yc_hs_0109","cur_42"]
[6409,"i_平陆三期 VII-66 机舱与风向夹角","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VII-66 机舱与风向夹角","yc_hs_0109","cur_43"]
[6410,"i_平陆三期 VII-66 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VII-66 1#桨叶片角度(桨距角)","yc_hs_0109","cur_45"]
[6411,"i_平陆三期 VII-66 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VII-66 2#桨叶片角度(桨距角)","yc_hs_0109","cur_46"]
[6412,"i_平陆三期 VII-66 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VII-66 3#桨叶片角度(桨距角)","yc_hs_0109","cur_47"]
[6413,"i_平陆三期 VII-66 发电机定子U相线圈温度","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VII-66 发电机定子U相线圈温度","yc_hs_0109","cur_48"]
[6414,"i_平陆三期 VII-66 发电机定子V相线圈温度","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VII-66 发电机定子V相线圈温度","yc_hs_0109","cur_50"]
[6415,"i_平陆三期 VII-66 发电机定子W相线圈温度","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VII-66 发电机定子W相线圈温度","yc_hs_0109","cur_52"]
[6416,"i_平陆三期 VII-66 发电机转速","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VII-66 发电机转速","yc_hs_0109","cur_60"]
[6417,"i_平陆三期 VII-66 发电机有功功率","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VII-66 发电机有功功率","yc_hs_0109","cur_61"]
[6418,"i_平陆三期 VII-66 发电机驱动端轴承温度","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VII-66 发电机驱动端轴承温度","yc_hs_0109","cur_71"]
[6419,"i_平陆三期 VII-66 发电机非驱动端轴承温度","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VII-66 发电机非驱动端轴承温度","yc_hs_0109","cur_72"]
[6420,"i_平陆三期 VII-66 风轮（主轴）转速","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VII-66 风轮（主轴）转速","yc_hs_0109","cur_84"]
[6421,"i_平陆三期 VII-66 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VII-66 齿轮箱高速轴驱动端轴承温度","yc_hs_0109","cur_85"]
[6422,"i_平陆三期 VII-66 机舱角度（位置）","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VII-66 机舱角度（位置）","yc_hs_0109","cur_90"]
[6423,"i_平陆三期 VII-66 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VII-66 机舱侧向振动值(已滤波)","yc_hs_0109","cur_91"]
[6424,"i_平陆三期 VII-66 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VII-66 机舱轴向振动值(已滤波)","yc_hs_0109","cur_92"]
[6425,"i_平陆三期 VII-66 风向","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VII-66 风向","yc_hs_0110","cur_02"]
[6426,"i_平陆三期 VII-66 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VII-66 齿轮箱中间轴非驱动端轴承温度","yc_hs_0110","cur_17"]
[6427,"i_平陆三期 VII-66 主轴承外圈温度","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VII-66 主轴承外圈温度","yc_hs_0110","cur_18"]
[6428,"i_平陆三期 VII-66 扭缆角度","平陆风电场","WOF35900004",66,"YCPL.T3_L2.WTG066.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VII-66 扭缆角度","yc_hs_0110","cur_20"]
[6429,"i_平陆三期 VII-67 风速","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VII-67 风速","yc_hs_0110","cur_69"]
[6430,"i_平陆三期 VII-67 舱外温度","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VII-67 舱外温度","yc_hs_0110","cur_71"]
[6431,"i_平陆三期 VII-67 舱内温度","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VII-67 舱内温度","yc_hs_0110","cur_73"]
[6432,"i_平陆三期 VII-67 机舱与风向夹角","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VII-67 机舱与风向夹角","yc_hs_0110","cur_74"]
[6433,"i_平陆三期 VII-67 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VII-67 1#桨叶片角度(桨距角)","yc_hs_0110","cur_76"]
[6434,"i_平陆三期 VII-67 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VII-67 2#桨叶片角度(桨距角)","yc_hs_0110","cur_77"]
[6435,"i_平陆三期 VII-67 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VII-67 3#桨叶片角度(桨距角)","yc_hs_0110","cur_78"]
[6436,"i_平陆三期 VII-67 发电机定子U相线圈温度","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VII-67 发电机定子U相线圈温度","yc_hs_0110","cur_79"]
[6437,"i_平陆三期 VII-67 发电机定子V相线圈温度","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VII-67 发电机定子V相线圈温度","yc_hs_0110","cur_80"]
[6438,"i_平陆三期 VII-67 发电机定子W相线圈温度","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VII-67 发电机定子W相线圈温度","yc_hs_0111","cur_07"]
[6439,"i_平陆三期 VII-67 发电机转速","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VII-67 发电机转速","yc_hs_0111","cur_11"]
[6440,"i_平陆三期 VII-67 发电机有功功率","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VII-67 发电机有功功率","yc_hs_0111","cur_12"]
[6441,"i_平陆三期 VII-67 发电机驱动端轴承温度","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VII-67 发电机驱动端轴承温度","yc_hs_0111","cur_16"]
[6442,"i_平陆三期 VII-67 发电机非驱动端轴承温度","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VII-67 发电机非驱动端轴承温度","yc_hs_0111","cur_18"]
[6443,"i_平陆三期 VII-67 风轮（主轴）转速","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VII-67 风轮（主轴）转速","yc_hs_0110","cur_31"]
[6444,"i_平陆三期 VII-67 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VII-67 齿轮箱高速轴驱动端轴承温度","yc_hs_0110","cur_32"]
[6445,"i_平陆三期 VII-67 机舱角度（位置）","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VII-67 机舱角度（位置）","yc_hs_0110","cur_37"]
[6446,"i_平陆三期 VII-67 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VII-67 机舱侧向振动值(已滤波)","yc_hs_0110","cur_38"]
[6447,"i_平陆三期 VII-67 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VII-67 机舱轴向振动值(已滤波)","yc_hs_0110","cur_40"]
[6448,"i_平陆三期 VII-67 风向","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VII-67 风向","yc_hs_0110","cur_49"]
[6449,"i_平陆三期 VII-67 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VII-67 齿轮箱中间轴非驱动端轴承温度","yc_hs_0110","cur_64"]
[6450,"i_平陆三期 VII-67 主轴承外圈温度","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VII-67 主轴承外圈温度","yc_hs_0110","cur_65"]
[6451,"i_平陆三期 VII-67 扭缆角度","平陆风电场","WOF35900004",67,"YCPL.T3_L2.WTG067.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VII-67 扭缆角度","yc_hs_0110","cur_67"]
[6452,"i_平陆三期 VII-68 风速","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VII-68 风速","yc_hs_0111","cur_20"]
[6453,"i_平陆三期 VII-68 舱外温度","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VII-68 舱外温度","yc_hs_0111","cur_21"]
[6454,"i_平陆三期 VII-68 舱内温度","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VII-68 舱内温度","yc_hs_0111","cur_22"]
[6455,"i_平陆三期 VII-68 机舱与风向夹角","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VII-68 机舱与风向夹角","yc_hs_0111","cur_23"]
[6456,"i_平陆三期 VII-68 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VII-68 1#桨叶片角度(桨距角)","yc_hs_0111","cur_25"]
[6457,"i_平陆三期 VII-68 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VII-68 2#桨叶片角度(桨距角)","yc_hs_0111","cur_26"]
[6458,"i_平陆三期 VII-68 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VII-68 3#桨叶片角度(桨距角)","yc_hs_0111","cur_27"]
[6459,"i_平陆三期 VII-68 发电机定子U相线圈温度","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VII-68 发电机定子U相线圈温度","yc_hs_0111","cur_28"]
[6460,"i_平陆三期 VII-68 发电机定子V相线圈温度","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VII-68 发电机定子V相线圈温度","yc_hs_0111","cur_30"]
[6461,"i_平陆三期 VII-68 发电机定子W相线圈温度","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VII-68 发电机定子W相线圈温度","yc_hs_0111","cur_32"]
[6462,"i_平陆三期 VII-68 发电机转速","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VII-68 发电机转速","yc_hs_0111","cur_40"]
[6463,"i_平陆三期 VII-68 发电机有功功率","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VII-68 发电机有功功率","yc_hs_0111","cur_41"]
[6464,"i_平陆三期 VII-68 发电机驱动端轴承温度","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VII-68 发电机驱动端轴承温度","yc_hs_0111","cur_51"]
[6465,"i_平陆三期 VII-68 发电机非驱动端轴承温度","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VII-68 发电机非驱动端轴承温度","yc_hs_0111","cur_52"]
[6466,"i_平陆三期 VII-68 风轮（主轴）转速","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VII-68 风轮（主轴）转速","yc_hs_0111","cur_64"]
[6467,"i_平陆三期 VII-68 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VII-68 齿轮箱高速轴驱动端轴承温度","yc_hs_0111","cur_65"]
[6468,"i_平陆三期 VII-68 机舱角度（位置）","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VII-68 机舱角度（位置）","yc_hs_0111","cur_70"]
[6469,"i_平陆三期 VII-68 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VII-68 机舱侧向振动值(已滤波)","yc_hs_0111","cur_71"]
[6470,"i_平陆三期 VII-68 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VII-68 机舱轴向振动值(已滤波)","yc_hs_0111","cur_72"]
[6471,"i_平陆三期 VII-68 风向","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VII-68 风向","yc_hs_0111","cur_82"]
[6472,"i_平陆三期 VII-68 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VII-68 齿轮箱中间轴非驱动端轴承温度","yc_hs_0111","cur_97"]
[6473,"i_平陆三期 VII-68 主轴承外圈温度","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VII-68 主轴承外圈温度","yc_hs_0111","cur_98"]
[6474,"i_平陆三期 VII-68 扭缆角度","平陆风电场","WOF35900004",68,"YCPL.T3_L2.WTG068.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VII-68 扭缆角度","yc_hs_0111","cur_100"]
[6475,"i_平陆三期 VII-69 1#桨叶片角度(桨距角)","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WROT.Blade1Position","桨距角1","pitch_angle_blade_1","i_平陆三期 VII-69 1#桨叶片角度(桨距角)","yc_hs_0112","cur_02"]
[6476,"i_平陆三期 VII-69 2#桨叶片角度(桨距角)","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WROT.Blade2Position","桨距角2","pitch_angle_blade_2","i_平陆三期 VII-69 2#桨叶片角度(桨距角)","yc_hs_0112","cur_04"]
[6477,"i_平陆三期 VII-69 3#桨叶片角度(桨距角)","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WROT.Blade3Position","桨距角3","pitch_angle_blade_3","i_平陆三期 VII-69 3#桨叶片角度(桨距角)","yc_hs_0112","cur_06"]
[6478,"i_平陆三期 VII-69 发电机定子U相线圈温度","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WGEN.TemGenStaU","发电机绕组1温度","generator_winding1_temperature","i_平陆三期 VII-69 发电机定子U相线圈温度","yc_hs_0112","cur_08"]
[6479,"i_平陆三期 VII-69 发电机定子V相线圈温度","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WGEN.TemGenStaV","发电机绕组2温度","generator_winding2_temperature","i_平陆三期 VII-69 发电机定子V相线圈温度","yc_hs_0112","cur_09"]
[6480,"i_平陆三期 VII-69 发电机定子W相线圈温度","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WGEN.TemGenStaW","发电机绕组3温度","generator_winding3_temperature","i_平陆三期 VII-69 发电机定子W相线圈温度","yc_hs_0112","cur_10"]
[6481,"i_平陆三期 VII-69 发电机转速","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WGEN.GenSpd","发电机转速","generator_speed","i_平陆三期 VII-69 发电机转速","yc_hs_0112","cur_14"]
[6482,"i_平陆三期 VII-69 发电机有功功率","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WGEN.GenActivePW","有功功率","active_power","i_平陆三期 VII-69 发电机有功功率","yc_hs_0112","cur_15"]
[6483,"i_平陆三期 VII-69 发电机驱动端轴承温度","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WGEN.TemGenDriEnd","发电机驱动端轴承温度","generatordrive_end_bearing_temperature","i_平陆三期 VII-69 发电机驱动端轴承温度","yc_hs_0112","cur_17"]
[6484,"i_平陆三期 VII-69 发电机非驱动端轴承温度","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WGEN.TemGenNonDE","发电机非驱动端轴承温度","generatornon_drive_end_bearing_temperature","i_平陆三期 VII-69 发电机非驱动端轴承温度","yc_hs_0112","cur_18"]
[6485,"i_平陆三期 VII-69 风轮（主轴）转速","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WTRM.RotorSpd","风轮转速","rotor_speed","i_平陆三期 VII-69 风轮（主轴）转速","yc_hs_0112","cur_41"]
[6486,"i_平陆三期 VII-69 齿轮箱高速轴驱动端轴承温度","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WTRM.TemGeaMSDE","齿轮箱高速轴轴承温度","gearbox_high_speed_shaft_bearing_temperature","i_平陆三期 VII-69 齿轮箱高速轴驱动端轴承温度","yc_hs_0112","cur_42"]
[6487,"i_平陆三期 VII-69 机舱角度（位置）","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WYAW.NacellePosition","机舱位置","cabin_position","i_平陆三期 VII-69 机舱角度（位置）","yc_hs_0112","cur_47"]
[6488,"i_平陆三期 VII-69 机舱侧向振动值(已滤波)","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WVIB.VibrationLFil","机舱左右振动","side_to_side_vibration_of_the_cabin","i_平陆三期 VII-69 机舱侧向振动值(已滤波)","yc_hs_0112","cur_49"]
[6489,"i_平陆三期 VII-69 机舱轴向振动值(已滤波)","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WVIB.VibrationVFil","机舱前后振动","front_back_vibration_of_the_cabin","i_平陆三期 VII-69 机舱轴向振动值(已滤波)","yc_hs_0112","cur_51"]
[6490,"i_平陆三期 VII-69 风向","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WNAC.WindDirection","绝对风向","true_wind_direction","i_平陆三期 VII-69 风向","yc_hs_0112","cur_56"]
[6491,"i_平陆三期 VII-69 齿轮箱中间轴非驱动端轴承温度","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WTRM.TemGeaMSND","齿轮箱中速轴轴承温度","gearboxmedium_speed_shaftbearing_temperature","i_平陆三期 VII-69 齿轮箱中间轴非驱动端轴承温度","yc_hs_0112","cur_63"]
[6492,"i_平陆三期 VII-69 主轴承外圈温度","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WTRM.TemMainBearing","主轴承轴承温度","main_bearing_temperature","i_平陆三期 VII-69 主轴承外圈温度","yc_hs_0112","cur_65"]
[6493,"i_平陆三期 VII-69 扭缆角度","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WYAW.TotalTwist","扭缆角度","twisted_cable_angle","i_平陆三期 VII-69 扭缆角度","yc_hs_0112","cur_72"]
[6494,"i_平陆三期 VII-69 风速","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WNAC.WindSpeed","风速","wind_velocity","i_平陆三期 VII-69 风速","yc_hs_0112","cur_73"]
[6495,"i_平陆三期 VII-69 舱外温度","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WNAC.TemOut","环境温度","outside_cabin_temperature","i_平陆三期 VII-69 舱外温度","yc_hs_0112","cur_74"]
[6496,"i_平陆三期 VII-69 舱内温度","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WNAC.TemNacelle","机舱内温度","cabin_temperature","i_平陆三期 VII-69 舱内温度","yc_hs_0112","cur_75"]
[6497,"i_平陆三期 VII-69 机舱与风向夹角","平陆风电场","WOF35900004",69,"YCPL.T3_L2.WTG069.WNAC.WindVaneDirection","对风角度","yaw_error1","i_平陆三期 VII-69 机舱与风向夹角","yc_hs_0112","cur_76"]