{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":38485,"n_cols":4,"rows_kept":4500,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["主控ID","状态编码","SC中文描述","告警等级"]
["SD03-1 ",-5,"通讯恢复","提示信息 "]
["SD03-1 ",-4,"通讯中断","告警信息 "]
["SD03-1 ",-3,"恢复连接","提示信息 "]
["SD03-1 ",-2,"无连接","告警信息 "]
["SD03-1 ",-1,"初始化","提示信息 "]
["SD03-1 ",0,"系统正常","提示信息 "]
["SD03-1 ",10001,"机舱振动有效值超限","故障 "]
["SD03-1 ",10002,"机舱振动瞬时值超限","故障 "]
["SD03-1 ",10011,"机舱振动报警","告警信息 "]
["SD03-1 ",10012,"备留","提示信息 "]
["SD03-1 ",10021,"备留","提示信息 "]
["SD03-1 ",10022,"备留","提示信息 "]
["SD03-1 ",10031,"备留","提示信息 "]
["SD03-1 ",10032,"备留","提示信息 "]
["SD03-1 ",10041,"备留","提示信息 "]
["SD03-1 ",10042,"备留","提示信息 "]
["SD03-1 ",10051,"备留","提示信息 "]
["SD03-1 ",10052,"备留","提示信息 "]
["SD03-1 ",10061,"备留","提示信息 "]
["SD03-1 ",10062,"备留","提示信息 "]
["SD03-1 ",10071,"备留","提示信息 "]
["SD03-1 ",20001,"自检程序1液压站系统压力故障","故障 "]
["SD03-1 ",20005,"自检程序2变桨位置故障1","故障 "]
["SD03-1 ",20006,"自检程序2变桨位置故障2","故障 "]
["SD03-1 ",20008,"自检程序3转速传感器故障","故障 "]
["SD03-1 ",20011,"切入故障","故障 "]
["SD03-1 ",20021,"备留","提示信息 "]
["SD03-1 ",20022,"备留","提示信息 "]
["SD03-1 ",20025,"备留","提示信息 "]
["SD03-1 ",20026,"备留","提示信息 "]
["SD03-1 ",20031,"备留","提示信息 "]
["SD03-1 ",20032,"备留","提示信息 "]
["SD03-1 ",20033,"备留","提示信息 "]
["SD03-1 ",20034,"备留","提示信息 "]
["SD03-1 ",20035,"备留","提示信息 "]
["SD03-1 ",20036,"备留","提示信息 "]
["SD03-1 ",20037,"备留","提示信息 "]
["SD03-1 ",20038,"备留","提示信息 "]
["SD03-1 ",20039,"备留","提示信息 "]
["SD03-1 ",20040,"备留","提示信息 "]
["SD03-1 ",20041,"备留","提示信息 "]
["SD03-1 ",30001,"变流器测得的发电机超速","故障 "]
["SD03-1 ",30002,"变流器ups报警","告警信息 "]
["SD03-1 ",30003,"变流器crowbar动作","故障 "]
["SD03-1 ",30004,"变流器CSC状态","故障 "]
["SD03-1 ",30005,"变流器加热","告警信息 "]
["SD03-1 ",30006,"变流器并网故障","故障 "]
["SD03-1 ",30011,"变流器准备好并网信号超时","故障 "]
["SD03-1 ",30062,"变流器与主控Profibus通讯中断","故障 "]
["SD03-1 ",30071,"变频器RS232通讯中断","故障 "]
["SD03-1 ",30100,"变流器内部通讯故障","故障 "]
["SD03-1 ",30101,"变流器控制板A/D故障","故障 "]
["SD03-1 ",30102,"变流器测得编码器故障","故障 "]
["SD03-1 ",30103,"变流器测得编码器信号丢失","故障 "]
["SD03-1 ",30104,"变流器直流侧chopper故障","故障 "]
["SD03-1 ",30105,"变流器转子侧Crowbar故障","故障 "]
["SD03-1 ",30106,"变流器低电压穿越超时","故障 "]
["SD03-1 ",30107,"变流器预充电直流侧电压低","故障 "]
["SD03-1 ",30110,"变流器直流侧电压高","故障 "]
["SD03-1 ",30111,"变流器直流侧电压低","故障 "]
["SD03-1 ",30112,"变流器测得电网电压相序出错","故障 "]
["SD03-1 ",30113,"变流器测得电网电压A相丢失","故障 "]
["SD03-1 ",30114,"变流器测得电网电压B相丢失","故障 "]
["SD03-1 ",30115,"变流器测得电网电压C相丢失","故障 "]
["SD03-1 ",30116,"变流器测得电网电压高","提示信息 "]
["SD03-1 ",30117,"变流器测得电网电压低","提示信息 "]
["SD03-1 ",30120,"变流器测得定子电压高","故障 "]
["SD03-1 ",30121,"变流器测得定子电压低","故障 "]
["SD03-1 ",30122,"变流器网侧A相IPM故障","故障 "]
["SD03-1 ",30123,"变流器网侧B相IPM故障","故障 "]
["SD03-1 ",30124,"变流器网侧C相IPM故障","故障 "]
["SD03-1 ",30125,"变流器转子侧A相IPM故障","故障 "]
["SD03-1 ",30126,"变流器转子侧B相IPM故障","故障 "]
["SD03-1 ",30127,"变流器转子侧C相IPM故障","故障 "]
["SD03-1 ",30130,"变流器网侧A相电流高","故障 "]
["SD03-1 ",30131,"变流器网侧B相电流高","故障 "]
["SD03-1 ",30132,"变流器网侧C相电流高","故障 "]
["SD03-1 ",30133,"变流器转子侧A相电流高","故障 "]
["SD03-1 ",30134,"变流器转子侧B相电流高","故障 "]
["SD03-1 ",30135,"变流器转子侧C相电流高","故障 "]
["SD03-1 ",30136,"变流器测得定子A相电流高","故障 "]
["SD03-1 ",30137,"变流器测得定子B相电流高","故障 "]
["SD03-1 ",30140,"变流器测得定子C相电流高","故障 "]
["SD03-1 ",30141,"变流器测得发电机转速低","故障 "]
["SD03-1 ",30142,"变流器测得发电机速度高","故障 "]
["SD03-1 ",30143,"变流器测得发电机并网转速低","故障 "]
["SD03-1 ",30144,"变流器测得发电机并网速度高","故障 "]
["SD03-1 ",30150,"变流器散热器过温报警","故障 "]
["SD03-1 ",30151,"chopper.crobar过温","告警信息 "]
["SD03-1 ",30152,"变流器定子断路器故障（电网熔断器故障）","故障 "]
["SD03-1 ",30153,"熔断器电压检测开关故障","故障 "]
["SD03-1 ",30154,"防雷及浪涌电气故障","故障 "]
["SD03-1 ",30155,"冷却水泵及空调故障","故障 "]
["SD03-1 ",30156,"变压器及电抗器故障","故障 "]
["SD03-1 ",30157,"变流器冷却水压力低","故障 "]
["SD03-1 ",30160,"变流器紧停","故障 "]
["SD03-1 ",30161,"变流器安全链紧停","故障 "]
["SD03-1 ",30170,"变流器网侧IPM过载报警","告警信息 "]
["SD03-1 ",30171,"变流器转子侧IPM过载报警","告警信息 "]
["SD03-1 ",30172,"变流器测得发电机过速报警","告警信息 "]
["SD03-1 ",30173,"变流器测得发电机速度低报警","告警信息 "]
["SD03-1 ",30174,"变流器测得定子电压高报警","告警信息 "]
["SD03-1 ",30175,"变流器测得定子电压低报警","告警信息 "]
["SD03-1 ",30176,"变流器冷却水温高报警","告警信息 "]
["SD03-1 ",30201,"变流器未插入SD卡","故障 "]
["SD03-1 ",30202,"变流器SD卡写保护","故障 "]
["SD03-1 ",30203,"变流器非指令脱网","故障 "]
["SD03-1 ",30204,"变流器未开机","故障 "]
["SD03-1 ",30205,"变流器系统故障数据记录中","故障 "]
["SD03-1 ",30206,"变流器冷却水温超限","故障 "]
["SD03-1 ",30207,"变流器主断路器内部跳闸","告警信息 "]
["SD03-1 ",30301,"转子侧变流器故障","告警信息 "]
["SD03-1 ",30302,"转子侧变流器电压故障","告警信息 "]
["SD03-1 ",30303,"转子侧变流器电流故障","告警信息 "]
["SD03-1 ",30401,"转子侧变流器温度故障","告警信息 "]
["SD03-1 ",30402,"其他转子侧变流器故障","告警信息 "]
["SD03-1 ",30403,"网侧变流器故障","告警信息 "]
["SD03-1 ",30501,"网侧变流器电压故障","告警信息 "]
["SD03-1 ",30502,"网侧变流器电流故障","告警信息 "]
["SD03-1 ",30503,"网侧变流器温度故障","告警信息 "]
["SD03-1 ",30504,"其他网侧变流器故障","告警信息 "]
["SD03-1 ",30601,"备留","提示信息 "]
["SD03-1 ",30602,"备留","提示信息 "]
["SD03-1 ",30603,"备留","提示信息 "]
["SD03-1 ",30604,"备留","提示信息 "]
["SD03-1 ",30605,"备留","提示信息 "]
["SD03-1 ",30606,"备留","提示信息 "]
["SD03-1 ",30607,"备留","提示信息 "]
["SD03-1 ",30608,"备留","提示信息 "]
["SD03-1 ",30609,"备留","提示信息 "]
["SD03-1 ",30610,"备留","提示信息 "]
["SD03-1 ",30701,"备留","提示信息 "]
["SD03-1 ",30702,"备留","提示信息 "]
["SD03-1 ",30703,"备留","提示信息 "]
["SD03-1 ",30704,"备留","提示信息 "]
["SD03-1 ",30705,"备留","提示信息 "]
["SD03-1 ",30706,"备留","提示信息 "]
["SD03-1 ",30707,"备留","提示信息 "]
["SD03-1 ",30708,"备留","提示信息 "]
["SD03-1 ",30709,"备留","提示信息 "]
["SD03-1 ",30710,"备留","提示信息 "]
["SD03-1 ",30801,"备留","提示信息 "]
["SD03-1 ",30802,"备留","提示信息 "]
["SD03-1 ",30803,"备留","提示信息 "]
["SD03-1 ",30804,"备留","提示信息 "]
["SD03-1 ",30805,"备留","提示信息 "]
["SD03-1 ",30806,"备留","提示信息 "]
["SD03-1 ",30807,"备留","提示信息 "]
["SD03-1 ",30808,"备留","提示信息 "]
["SD03-1 ",30809,"备留","提示信息 "]
["SD03-1 ",30810,"备留","提示信息 "]
["SD03-1 ",30901,"备留","提示信息 "]
["SD03-1 ",30902,"备留","提示信息 "]
["SD03-1 ",30903,"备留","提示信息 "]
["SD03-1 ",30904,"备留","提示信息 "]
["SD03-1 ",30905,"备留","提示信息 "]
["SD03-1 ",30906,"备留","提示信息 "]
["SD03-1 ",30907,"备留","提示信息 "]
["SD03-1 ",30908,"备留","提示信息 "]
["SD03-1 ",30909,"备留","提示信息 "]
["SD03-1 ",30910,"备留","提示信息 "]
["SD03-1 ",31001,"备留","提示信息 "]
["SD03-1 ",31002,"备留","提示信息 "]
["SD03-1 ",31003,"备留","提示信息 "]
["SD03-1 ",31004,"备留","提示信息 "]
["SD03-1 ",31005,"备留","提示信息 "]
["SD03-1 ",31006,"备留","提示信息 "]
["SD03-1 ",31007,"备留","提示信息 "]
["SD03-1 ",31008,"备留","提示信息 "]
["SD03-1 ",31009,"备留","提示信息 "]
["SD03-1 ",31010,"备留","提示信息 "]
["SD03-1 ",31101,"备留","提示信息 "]
["SD03-1 ",31102,"备留","提示信息 "]
["SD03-1 ",31103,"备留","提示信息 "]
["SD03-1 ",31104,"备留","提示信息 "]
["SD03-1 ",31105,"备留","提示信息 "]
["SD03-1 ",40010,"风轮制动垫故障","故障 "]
["SD03-1 ",40030,"风轮制动垫报警","告警信息 "]
["SD03-1 ",40040,"备留","提示信息 "]
["SD03-1 ",40050,"备留","提示信息 "]
["SD03-1 ",40060,"备留","提示信息 "]
["SD03-1 ",40070,"备留","提示信息 "]
["SD03-1 ",40080,"备留","提示信息 "]
["SD03-1 ",40090,"备留","提示信息 "]
["SD03-1 ",40100,"备留","提示信息 "]
["SD03-1 ",40110,"备留","提示信息 "]
["SD03-1 ",50001,"液压油泵加热器保护","故障 "]
["SD03-1 ",50002,"液压油泵马达保护","故障 "]
["SD03-1 ",50010,"液压泵反馈时间超限","故障 "]
["SD03-1 ",50020,"液压油油位超限","故障 "]
["SD03-1 ",50025,"液压油温度超限","故障 "]
["SD03-1 ",50030,"液压风轮制动压力故障","故障 "]
["SD03-1 ",50035,"液压系统主压力过低","故障 "]
["SD03-1 ",50036,"液压系统主压力过高","故障 "]
["SD03-1 ",50038,"液压过滤器入口压力故障","故障 "]
["SD03-1 ",50039,"液压过滤器出口压力故障","故障 "]
["SD03-1 ",50040,"备留","提示信息 "]
["SD03-1 ",50041,"备留","提示信息 "]
["SD03-1 ",50042,"备留","提示信息 "]
["SD03-1 ",50051,"备留","提示信息 "]
["SD03-1 ",50052,"备留","提示信息 "]
["SD03-1 ",50060,"备留","提示信息 "]
["SD03-1 ",50061,"备留","提示信息 "]
["SD03-1 ",50062,"备留","提示信息 "]
["SD03-1 ",50063,"备留","提示信息 "]
["SD03-1 ",50064,"备留","提示信息 "]
["SD03-1 ",50065,"备留","提示信息 "]
["SD03-1 ",50066,"备留","提示信息 "]
["SD03-1 ",50067,"备留","提示信息 "]
["SD03-1 ",50068,"备留","提示信息 "]
["SD03-1 ",50069,"备留","提示信息 "]
["SD03-1 ",60001,"偏航位置错误","故障 "]
["SD03-1 ",60002,"左偏航限位开关动作","故障 "]
["SD03-1 ",60003,"右偏航限位开关动作","故障 "]
["SD03-1 ",60004,"自动解缆","提示信息 "]
["SD03-1 ",60005,"手动偏航","提示信息 "]
["SD03-1 ",60006,"偏航齿轮润滑","告警信息 "]
["SD03-1 ",60010,"偏航速度过低","故障 "]
["SD03-1 ",60100,"偏航马达总保护","故障 "]
["SD03-1 ",60101,"偏航马达保护1","故障 "]
["SD03-1 ",60102,"偏航马达保护2","故障 "]
["SD03-1 ",60103,"偏航马达保护3","故障 "]
["SD03-1 ",60104,"偏航马达保护4","故障 "]
["SD03-1 ",60201,"偏航制动保护","故障 "]
["SD03-1 ",60300,"偏航软启动器故障","告警信息 "]
["SD03-1 ",60301,"偏航软启动器斜率错误","故障 "]
["SD03-1 ",60605,"偏航轴承润滑油油位低","告警信息 "]
["SD03-1 ",60606,"偏航轴承润滑故障","告警信息 "]
["SD03-1 ",60801,"偏航齿轮润滑油油位低","告警信息 "]
["SD03-1 ",60802,"偏航齿轮润滑故障","告警信息 "]
["SD03-1 ",60901,"备留","提示信息 "]
["SD03-1 ",60902,"备留","提示信息 "]
["SD03-1 ",60903,"备留","提示信息 "]
["SD03-1 ",60910,"备留","提示信息 "]
["SD03-1 ",60911,"备留","提示信息 "]
["SD03-1 ",60912,"备留","提示信息 "]
["SD03-1 ",60913,"备留","提示信息 "]
["SD03-1 ",60914,"备留","提示信息 "]
["SD03-1 ",60915,"备留","提示信息 "]
["SD03-1 ",60916,"备留","提示信息 "]
["SD03-1 ",60917,"备留","提示信息 "]
["SD03-1 ",60918,"备留","提示信息 "]
["SD03-1 ",60919,"备留","提示信息 "]
["SD03-1 ",60920,"备留","提示信息 "]
["SD03-1 ",60921,"备留","提示信息 "]
["SD03-1 ",60922,"备留","提示信息 "]
["SD03-1 ",70011,"发电机绕组u1温度超限","故障 "]
["SD03-1 ",70013,"发电机绕组v1温度超限","故障 "]
["SD03-1 ",70015,"发电机绕组w1温度超限","故障 "]
["SD03-1 ",70017,"发电机u1相绕组温度报警","告警信息 "]
["SD03-1 ",70018,"发电机v1相绕组温度报警","告警信息 "]
["SD03-1 ",70019,"发电机w1相绕组温度报警","告警信息 "]
["SD03-1 ",70021,"发电机前轴承温度超限","故障 "]
["SD03-1 ",70022,"发电机后轴承温度超限","故障 "]
["SD03-1 ",70025,"发电机前轴承温度报警","告警信息 "]
["SD03-1 ",70026,"发电机后轴承温度报警","告警信息 "]
["SD03-1 ",70036,"发电机冷却水温度超限","故障 "]
["SD03-1 ",70037,"备留","提示信息 "]
["SD03-1 ",70056,"发电机加热器1保护","故障 "]
["SD03-1 ",70057,"发电机加热器2保护","故障 "]
["SD03-1 ",70059,"发电机冷却水风扇保护","故障 "]
["SD03-1 ",70061,"发电机冷却水泵保护","故障 "]
["SD03-1 ",70062,"发电机注油泵油位报警","告警信息 "]
["SD03-1 ",70063,"发电机滑环和鼓风机加热器保护","故障 "]
["SD03-1 ",70064,"发电机冷却水风扇加热器保护","故障 "]
["SD03-1 ",70065,"发电机冷却水压力故障","故障 "]
["SD03-1 ",70070,"发电机电刷故障","故障 "]
["SD03-1 ",70091,"发电机滑环温度超限","故障 "]
["SD03-1 ",70101,"发电机进风口温度超限","故障 "]
["SD03-1 ",70102,"发电机出风口温度超限","故障 "]
["SD03-1 ",70103,"发电机停机加热器","告警信息 "]
["SD03-1 ",70201,"发电机定子温度和机舱温度过低","故障 "]
["SD03-1 ",70202,"发电机非轴伸端碳刷故障","故障 "]
["SD03-1 ",70203,"备留","提示信息 "]
["SD03-1 ",70204,"备留","提示信息 "]
["SD03-1 ",70205,"备留","提示信息 "]
["SD03-1 ",70301,"备留","提示信息 "]
["SD03-1 ",70302,"备留","提示信息 "]
["SD03-1 ",70303,"备留","提示信息 "]
["SD03-1 ",70304,"备留","提示信息 "]
["SD03-1 ",70305,"备留","提示信息 "]
["SD03-1 ",70306,"备留","提示信息 "]
["SD03-1 ",70307,"备留","提示信息 "]
["SD03-1 ",70308,"备留","提示信息 "]
["SD03-1 ",70309,"备留","提示信息 "]
["SD03-1 ",70310,"备留","提示信息 "]
["SD03-1 ",70311,"备留","提示信息 "]
["SD03-1 ",70312,"备留","提示信息 "]
["SD03-1 ",70313,"备留","提示信息 "]
["SD03-1 ",70314,"备留","提示信息 "]
["SD03-1 ",70315,"备留","提示信息 "]
["SD03-1 ",80001,"齿轮箱低速轴温度超限","故障 "]
["SD03-1 ",80002,"齿轮箱高速轴温度超限","故障 "]
["SD03-1 ",80012,"齿轮箱油温超限","故障 "]
["SD03-1 ",80014,"齿轮箱入口油温超限","故障 "]
["SD03-1 ",80020,"齿轮箱冷却水温超限","故障 "]
["SD03-1 ",80023,"齿轮箱冷却水压力异常","故障 "]
["SD03-1 ",80030,"齿轮箱油位过低","故障 "]
["SD03-1 ",80040,"齿轮箱润滑油压力异常","故障 "]
["SD03-1 ",80050,"齿轮箱过滤器油压力异常","故障 "]
["SD03-1 ",80071,"齿轮箱润滑油加热器保护","故障 "]
["SD03-1 ",80072,"齿轮箱润滑油泵马达保护","故障 "]
["SD03-1 ",80073,"齿轮箱润滑油泵加热器保护","故障 "]
["SD03-1 ",80075,"齿轮箱冷却水风扇保护","故障 "]
["SD03-1 ",80080,"齿轮箱冷却水泵保护","故障 "]
["SD03-1 ",80081,"齿轮箱冷却水泵加热器保护","故障 "]
["SD03-1 ",80091,"齿轮箱冷却水风扇加热器保护","故障 "]
["SD03-1 ",80092,"齿轮箱接油盘Pump油位报警","告警信息 "]
["SD03-1 ",80101,"齿轮箱中间轴转子侧温度超限","告警信息 "]
["SD03-1 ",80102,"齿轮箱中间轴发机电侧温度超限","告警信息 "]
["SD03-1 ",80104,"齿轮箱旁路过滤油泵保护","故障 "]
["SD03-1 ",80105,"备留","提示信息 "]
["SD03-1 ",80201,"备留","提示信息 "]
["SD03-1 ",80202,"备留","提示信息 "]
["SD03-1 ",80203,"备留","提示信息 "]
["SD03-1 ",80204,"备留","提示信息 "]
["SD03-1 ",80301,"备留","提示信息 "]
["SD03-1 ",80302,"备留","提示信息 "]
["SD03-1 ",80303,"备留","提示信息 "]
["SD03-1 ",80304,"备留","提示信息 "]
["SD03-1 ",80305,"备留","提示信息 "]
["SD03-1 ",80306,"备留","提示信息 "]
["SD03-1 ",80307,"备留","提示信息 "]
["SD03-1 ",80308,"备留","提示信息 "]
["SD03-1 ",80309,"备留","提示信息 "]
["SD03-1 ",80310,"备留","提示信息 "]
["SD03-1 ",80311,"备留","提示信息 "]
["SD03-1 ",80312,"备留","提示信息 "]
["SD03-1 ",80313,"备留","提示信息 "]
["SD03-1 ",80314,"备留","提示信息 "]
["SD03-1 ",80315,"备留","提示信息 "]
["SD03-1 ",90001,"发电机高温降容或齿轮箱低温降容","告警信息 "]
["SD03-1 ",90002,"变流器降容","告警信息 "]
["SD03-1 ",90011,"备留","提示信息 "]
["SD03-1 ",90012,"SCADA限功率","提示信息 "]
["SD03-1 ",90021,"备留","提示信息 "]
["SD03-1 ",90022,"备留","提示信息 "]
["SD03-1 ",90023,"备留","提示信息 "]
["SD03-1 ",90031,"备留","提示信息 "]
["SD03-1 ",90032,"备留","提示信息 "]
["SD03-1 ",90033,"备留","提示信息 "]
["SD03-1 ",100111,"电网A相电压高于上限值","故障 "]
["SD03-1 ",100112,"电网B相电压高于上限值","故障 "]
["SD03-1 ",100113,"电网C相电压高于上限值","故障 "]
["SD03-1 ",100121,"电网A相电压低于下限值","故障 "]
["SD03-1 ",100122,"电网B相电压低于下限值","故障 "]
["SD03-1 ",100123,"电网C相电压低于下限值","故障 "]
["SD03-1 ",100130,"电网电压不对称","故障 "]
["SD03-1 ",100211,"电网A相电流高于上限值","故障 "]
["SD03-1 ",100212,"电网B相电流高于上限值","故障 "]
["SD03-1 ",100220,"电网电流不对称","故障 "]
["SD03-1 ",100311,"电网频率高于上限值","故障 "]
["SD03-1 ",100321,"电网频率低于下限值","故障 "]
["SD03-1 ",100410,"电网实时有功功率超限","故障 "]
["SD03-1 ",100411,"电网30s平均有功功率超限","故障 "]
["SD03-1 ",100412,"电网10m平均有功功率超限","故障 "]
["SD03-1 ",100420,"电网有功功率超值超限","故障 "]
["SD03-1 ",100510,"电网无功功率超限","故障 "]
["SD03-1 ",100511,"低电压穿越","告警信息 "]
["SD03-1 ",100512,"备留","提示信息 "]
["SD03-1 ",100601,"备留","提示信息 "]
["SD03-1 ",100602,"备留","提示信息 "]
["SD03-1 ",100701,"电网线电压L1低于下限值","故障 "]
["SD03-1 ",100702,"电网线电压L2低于下限值","故障 "]
["SD03-1 ",100703,"电网线电压L3低于下限值","故障 "]
["SD03-1 ",100801,"备留","提示信息 "]
["SD03-1 ",100802,"备留","提示信息 "]
["SD03-1 ",100803,"备留","提示信息 "]
["SD03-1 ",100804,"备留","提示信息 "]
["SD03-1 ",100805,"备留","提示信息 "]
["SD03-1 ",100806,"备留","提示信息 "]
["SD03-1 ",100807,"备留","提示信息 "]
["SD03-1 ",100808,"备留","提示信息 "]
["SD03-1 ",100809,"备留","提示信息 "]
["SD03-1 ",100810,"备留","提示信息 "]
["SD03-1 ",110101,"塔底柜子温度超限","故障 "]
["SD03-1 ",110102,"机舱柜子温度超限","故障 "]
["SD03-1 ",110105,"备留","提示信息 "]
["SD03-1 ",110106,"备留","提示信息 "]
["SD03-1 ",110107,"备留","提示信息 "]
["SD03-1 ",110108,"备留","提示信息 "]
["SD03-1 ",110109,"备留","提示信息 "]
["SD03-1 ",110110,"备留","提示信息 "]
["SD03-1 ",110111,"备留","提示信息 "]
["SD03-1 ",110112,"备留","提示信息 "]
["SD03-1 ",120001,"塔底柜子温度控制开关保护","故障 "]
["SD03-1 ",120002,"机舱柜子温度控制开关保护","故障 "]
["SD03-1 ",120010,"备留","提示信息 "]
["SD03-1 ",120011,"备留","提示信息 "]
["SD03-1 ",120021,"备留","提示信息 "]
["SD03-1 ",120031,"备留","提示信息 "]
["SD03-1 ",120032,"备留","提示信息 "]
["SD03-1 ",120033,"备留","提示信息 "]
["SD03-1 ",120034,"备留","提示信息 "]
["SD03-1 ",120035,"备留","提示信息 "]
["SD03-1 ",130101,"塔底控制柜UPS电池故障","告警信息 "]
["SD03-1 ",130102,"机舱控制柜UPS电池故障","告警信息 "]
["SD03-1 ",130201,"塔底控制柜UPS供电异常","故障 "]
["SD03-1 ",130202,"机舱控制柜UPS供电异常","故障 "]
["SD03-1 ",130301,"备留","提示信息 "]
["SD03-1 ",130302,"备留","提示信息 "]
["SD03-1 ",130303,"备留","提示信息 "]
["SD03-1 ",130311,"备留","提示信息 "]
["SD03-1 ",130312,"备留","提示信息 "]
["SD03-1 ",130313,"备留","提示信息 "]
["SD03-1 ",130321,"备留","提示信息 "]
["SD03-1 ",130322,"备留","提示信息 "]
["SD03-1 ",130323,"备留","提示信息 "]
["SD03-1 ",130324,"备留","提示信息 "]
["SD03-1 ",130325,"备留","提示信息 "]
["SD03-1 ",160001,"塔底400VAC供电保护","故障 "]
["SD03-1 ",160025,"机舱控制柜24VDC供电异常","故障 "]
["SD03-1 ",160026,"机舱控制柜外部传感器24VDC供电异常","故障 "]
["SD03-1 ",160061,"变桨400VAC供电保护","故障 "]
["SD03-1 ",160062,"变桨230V供电保护","告警信息 "]
["SD03-1 ",160071,"备留","提示信息 "]
["SD03-1 ",160072,"备留","提示信息 "]
["SD03-1 ",160081,"备留","提示信息 "]
["SD03-1 ",160082,"备留","提示信息 "]
["SD03-1 ",160083,"备留","提示信息 "]
["SD03-1 ",160091,"备留","提示信息 "]
["SD03-1 ",160092,"备留","提示信息 "]
["SD03-1 ",160093,"备留","提示信息 "]
["SD03-1 ",160094,"备留","提示信息 "]
["SD03-1 ",160095,"备留","提示信息 "]
["SD03-1 ",160096,"备留","提示信息 "]
["SD03-1 ",160097,"备留","提示信息 "]
["SD03-1 ",160098,"备留","提示信息 "]
["SD03-1 ",160099,"备留","提示信息 "]
["SD03-1 ",160100,"备留","提示信息 "]
["SD03-1 ",170030,"风向与机舱偏差超限","故障 "]
["SD03-1 ",170041,"风速计1故障","告警信息 "]
["SD03-1 ",170042,"风速计2故障","告警信息 "]
["SD03-1 ",170043,"风速计故障","故障 "]
["SD03-1 ",170051,"风向标1故障1(120s延时)","告警信息 "]
["SD03-1 ",170052,"风向标2故障1(120s延时)","告警信息 "]
["SD03-1 ",170053,"火灾烟雾报警","故障 "]
["SD03-1 ",170056,"风向标1故障2(150s延时)","故障 "]
["SD03-1 ",170057,"风向标2故障2(150s延时)","故障 "]
["SD03-1 ",170058,"风向标故障","故障 "]
["SD03-1 ",170101,"桨叶位置判断暴风","故障 "]
["SD03-1 ",170102,"暴风","告警信息 "]
["SD03-1 ",170201,"风力不足1","告警信息 "]
["SD03-1 ",170202,"风力不足2","告警信息 "]
["SD03-1 ",170203,"风力不足3","告警信息 "]
["SD03-1 ",170301,"塔底烟雾报警","告警信息 "]
["SD03-1 ",170302,"备留","提示信息 "]
["SD03-1 ",170303,"备留","提示信息 "]
["SD03-1 ",170401,"备留","提示信息 "]
["SD03-1 ",170402,"备留","提示信息 "]
["SD03-1 ",170501,"机舱消防系统预报警","告警信息 "]
["SD03-1 ",170502,"机舱消防系统主报警","告警信息 "]
["SD03-1 ",170503,"机舱消防系统故障","故障 "]
["SD03-1 ",170504,"备留","提示信息 "]
["SD03-1 ",170505,"备留","提示信息 "]
["SD03-1 ",170601,"备留","提示信息 "]
["SD03-1 ",170602,"备留","提示信息 "]
["SD03-1 ",170603,"备留","提示信息 "]
["SD03-1 ",170604,"备留","提示信息 "]
["SD03-1 ",170605,"备留","提示信息 "]
["SD03-1 ",180001,"塔底控制柜熔断器断开","故障 "]
["SD03-1 ",180002,"备留","提示信息 "]
["SD03-1 ",180005,"塔底400V熔断反馈","告警信息 "]
["SD03-1 ",180006,"备留","提示信息 "]
["SD03-1 ",180009,"备留","提示信息 "]
["SD03-1 ",180010,"备留","提示信息 "]
["SD03-1 ",180011,"备留","提示信息 "]
["SD03-1 ",180012,"备留","提示信息 "]
["SD03-1 ",180013,"备留","提示信息 "]
["SD03-1 ",180014,"备留","提示信息 "]
["SD03-1 ",190001,"塔底避雷器保护动作","故障 "]
["SD03-1 ",190002,"机舱避雷器保护动作","故障 "]
["SD03-1 ",190011,"发电机定子避雷器保护动作","故障 "]
["SD03-1 ",190012,"发电机转子避雷器保护动作","故障 "]
["SD03-1 ",190031,"箱变避雷器保护动作","故障 "]
["SD03-1 ",190041,"备留","提示信息 "]
["SD03-1 ",190042,"备留","提示信息 "]
["SD03-1 ",190051,"备留","提示信息 "]
["SD03-1 ",190052,"备留","提示信息 "]
["SD03-1 ",190060,"备留","提示信息 "]
["SD03-1 ",190070,"备留","提示信息 "]
["SD03-1 ",190071,"备留","提示信息 "]
["SD03-1 ",190072,"备留","提示信息 "]
["SD03-1 ",190073,"备留","提示信息 "]
["SD03-1 ",190074,"备留","提示信息 "]
["SD03-1 ",200001,"写InitRun.txt文件出错","故障 "]
["SD03-1 ",200002,"写StatusList.txt文件出错","故障 "]
["SD03-1 ",200021,"写initRun.txt文件出错","故障 "]
["SD03-1 ",200022,"恢复默认参数出错","故障 "]
["SD03-1 ",200023,"备留","提示信息 "]
["SD03-1 ",200051,"备留","提示信息 "]
["SD03-1 ",200052,"备留","提示信息 "]
["SD03-1 ",200057,"备留","提示信息 "]
["SD03-1 ",200058,"备留","提示信息 "]
["SD03-1 ",200061,"备留","提示信息 "]
["SD03-1 ",200062,"备留","提示信息 "]
["SD03-1 ",200065,"备留","提示信息 "]
["SD03-1 ",200066,"备留","提示信息 "]
["SD03-1 ",200071,"备留","提示信息 "]
["SD03-1 ",200072,"备留","提示信息 "]
["SD03-1 ",220001,"停机超时1(25s)","故障 "]
["SD03-1 ",220002,"停机超时2(90s)","故障 "]
["SD03-1 ",220011,"紧急停机超时(10s)","故障 "]
["SD03-1 ",220021,"SCADA复位按钮故障","提示信息 "]
["SD03-1 ",220022,"备留","提示信息 "]
["SD03-1 ",220031,"备留","提示信息 "]
["SD03-1 ",220032,"备留","提示信息 "]
["SD03-1 ",220041,"备留","提示信息 "]
["SD03-1 ",220042,"备留","提示信息 "]
["SD03-1 ",220043,"备留","提示信息 "]
["SD03-1 ",220051,"备留","提示信息 "]
["SD03-1 ",220052,"备留","提示信息 "]
["SD03-1 ",220053,"备留","提示信息 "]
["SD03-1 ",220054,"备留","提示信息 "]
["SD03-1 ",220055,"备留","提示信息 "]
["SD03-1 ",230001,"电网重复故障","故障 "]
["SD03-1 ",230011,"温度重复故障","故障 "]
["SD03-1 ",230021,"液压重复故障","故障 "]
["SD03-1 ",230031,"变桨系统重复故障","故障 "]
["SD03-1 ",230091,"其它重复故障","故障 "]
["SD03-1 ",230092,"备留","提示信息 "]
["SD03-1 ",230095,"备留","提示信息 "]
["SD03-1 ",230096,"备留","提示信息 "]
["SD03-1 ",230101,"备留","提示信息 "]
["SD03-1 ",230102,"备留","提示信息 "]
["SD03-1 ",230110,"备留","提示信息 "]
["SD03-1 ",230111,"备留","提示信息 "]
["SD03-1 ",230112,"备留","提示信息 "]
["SD03-1 ",230113,"备留","提示信息 "]
["SD03-1 ",230114,"备留","提示信息 "]
["SD03-1 ",250101,"CPU占用率高(超过70%)","故障 "]
["SD03-1 ",250102,"CPU占用率非常高(超过86%)","故障 "]
["SD03-1 ",250103,"CP1486电池低","告警信息 "]
["SD03-1 ",250104,"备留","提示信息 "]
["SD03-1 ",250105,"备留","提示信息 "]
["SD03-1 ",250106,"备留","提示信息 "]
["SD03-1 ",250107,"备留","提示信息 "]
["SD03-1 ",250108,"备留","提示信息 "]
["SD03-1 ",250109,"备留","提示信息 "]
["SD03-1 ",250110,"备留","提示信息 "]
["SD03-1 ",260005,"机舱结冰传感器正常","故障 "]
["SD03-1 ",260007,"机舱结冰传感器报警","故障 "]
["SD03-1 ",260010,"备留","提示信息 "]
["SD03-1 ",260011,"备留","提示信息 "]
["SD03-1 ",260012,"备留","提示信息 "]
["SD03-1 ",260013,"备留","提示信息 "]
["SD03-1 ",260014,"备留","提示信息 "]
["SD03-1 ",260015,"备留","提示信息 "]
["SD03-1 ",260016,"备留","提示信息 "]
["SD03-1 ",260017,"备留","提示信息 "]
["SD03-1 ",270005,"机舱冷却风扇保护","故障 "]
["SD03-1 ",270010,"机舱外温度低","故障 "]
["SD03-1 ",270011,"机舱温度超限","故障 "]
["SD03-1 ",270021,"备留","提示信息 "]
["SD03-1 ",270022,"备留","提示信息 "]
["SD03-1 ",270030,"备留","提示信息 "]
["SD03-1 ",270031,"备留","提示信息 "]
["SD03-1 ",270032,"备留","提示信息 "]
["SD03-1 ",270033,"备留","提示信息 "]
["SD03-1 ",270034,"备留","提示信息 "]
["SD03-1 ",280005,"风轮位置超限","故障 "]
["SD03-1 ",280007,"备留","提示信息 "]
["SD03-1 ",280008,"备留","提示信息 "]
["SD03-1 ",280010,"备留","提示信息 "]
["SD03-1 ",280011,"备留","提示信息 "]
["SD03-1 ",280021,"备留","提示信息 "]
["SD03-1 ",280022,"备留","提示信息 "]
["SD03-1 ",280023,"备留","提示信息 "]
["SD03-1 ",280024,"备留","提示信息 "]
["SD03-1 ",280025,"备留","提示信息 "]
["SD03-1 ",290005,"主轴承齿轮箱侧温度超限","故障 "]
["SD03-1 ",290007,"主轴承风轮侧温度超限","故障 "]
["SD03-1 ",290050,"主轴承润滑油油位低","告警信息 "]
["SD03-1 ",290060,"主轴承润滑故障(分油器堵塞)","告警信息 "]
["SD03-1 ",290070,"电气滑环加热器保护","故障 "]
["SD03-1 ",290072,"备留","提示信息 "]
["SD03-1 ",290073,"备留","提示信息 "]
["SD03-1 ",290076,"备留","提示信息 "]
["SD03-1 ",290077,"备留","提示信息 "]
["SD03-1 ",290078,"备留","提示信息 "]
["SD03-1 ",290079,"备留","提示信息 "]
["SD03-1 ",290080,"备留","提示信息 "]
["SD03-1 ",290081,"备留","提示信息 "]
["SD03-1 ",290082,"备留","提示信息 "]
["SD03-1 ",290083,"备留","提示信息 "]
["SD03-1 ",300101,"桨叶1电容柜隔离开关断开","故障 "]
["SD03-1 ",300102,"桨叶2电容柜隔离开关断开","故障 "]
["SD03-1 ",300103,"桨叶3电容柜隔离开关断开","故障 "]
["SD03-1 ",300111,"变桨系统轴1电容柜过电压","故障 "]
["SD03-1 ",300112,"变桨系统轴2电容柜过电压","故障 "]
["SD03-1 ",300113,"变桨系统轴3电容柜过电压","故障 "]
["SD03-1 ",300114,"变桨系统轴1电容柜欠电压","故障 "]
["SD03-1 ",300115,"变桨系统轴2电容柜欠电压","故障 "]
["SD03-1 ",300116,"变桨系统轴3电容柜欠电压","故障 "]
["SD03-1 ",300121,"轴1充电器输出断路器断开","故障 "]
["SD03-1 ",300122,"轴2充电器输出断路器断开","故障 "]
["SD03-1 ",300123,"轴3充电器输出断路器断开","故障 "]
["SD03-1 ",300124,"轴1电容柜容量衰减","故障 "]
["SD03-1 ",300125,"轴2电容柜容量衰减","故障 "]
["SD03-1 ",300126,"轴3电容柜容量衰减","故障 "]
["SD03-1 ",300131,"轴1充电器故障继电器断开","故障 "]
["SD03-1 ",300132,"轴2充电器故障继电器断开","故障 "]
["SD03-1 ",300133,"轴3充电器故障继电器断开","故障 "]
["SD03-1 ",300141,"变桨系统电容柜1温度超限","故障 "]
["SD03-1 ",300142,"变桨系统电容柜2温度超限","故障 "]
["SD03-1 ",300143,"变桨系统电容柜3温度超限","故障 "]
["SD03-1 ",300150,"变桨电池运行信号","故障 "]
["SD03-1 ",300201,"变流器profitbus通讯超时","故障 "]
["SD03-1 ",300311,"变桨系统轴1驱动器故障","故障 "]
["SD03-1 ",300312,"变桨系统轴2驱动器故障","故障 "]
["SD03-1 ",300313,"变桨系统轴3驱动器故障","故障 "]
["SD03-1 ",300321,"变桨系统轴1直流母线侧断路器断开","故障 "]
["SD03-1 ",300322,"'变桨系统轴2直流母线侧断路器断开","故障 "]
["SD03-1 ",300323,"变桨系统轴3直流母线侧断路器断开","故障 "]
["SD03-1 ",300331,"变桨系统轴1抱闸电源模块断路器断开","故障 "]
["SD03-1 ",300332,"变桨系统轴2抱闸电源模块断路器断开","故障 "]
["SD03-1 ",300333,"变桨系统轴3抱闸电源模块断路器断开","故障 "]
["SD03-1 ",300334,"轴1电机刹车电源断路器断开","故障 "]
["SD03-1 ",300335,"轴2电机刹车电源断路器断开","故障 "]
["SD03-1 ",300336,"轴3电机刹车电源断路器断开","故障 "]
["SD03-1 ",300341,"变桨系统轴1电机未上电","故障 "]
["SD03-1 ",300342,"变桨系统轴2电机未上电","故障 "]
["SD03-1 ",300343,"变桨系统轴3电机未上电","故障 "]
["SD03-1 ",300347,"变桨系统轴1DC400V熔断丝断开","故障 "]
["SD03-1 ",300348,"变桨系统轴2DC400V熔断丝断开","故障 "]
["SD03-1 ",300349,"变桨系统轴3DC400V熔断丝断开","故障 "]
["SD03-1 ",300401,"轴1加热器供电断路器跳闸","故障 "]
["SD03-1 ",300402,"轴2加热器供电断路器跳闸","故障 "]
["SD03-1 ",300403,"轴3加热器供电断路器跳闸","故障 "]
["SD03-1 ",300511,"变桨系统轴1电机温度超限","故障 "]
["SD03-1 ",300512,"变桨系统轴2电机温度超限","故障 "]
["SD03-1 ",300513,"变桨系统轴3电机温度超限","故障 "]
["SD03-1 ",300611,"变桨系统轴1限位开关触发","故障 "]
["SD03-1 ",300612,"变桨系统轴2限位开关触发","故障 "]
["SD03-1 ",300613,"变桨系统轴3限位开关触发","故障 "]
["SD03-1 ",300621,"变桨系统轴1的91°限位开关触发","故障 "]
["SD03-1 ",300622,"变桨系统轴2的91°限位开关触发","故障 "]
["SD03-1 ",300623,"变桨系统轴3的91°限位开关触发","故障 "]
["SD03-1 ",300631,"变桨系统轴1的96°限位开关触发","故障 "]
["SD03-1 ",300632,"变桨系统轴2的96°限位开关触发","故障 "]
["SD03-1 ",300633,"变桨系统轴3的96°限位开关触发","故障 "]
["SD03-1 ",300641,"轴1的2个编码器角度偏差超限","故障 "]
["SD03-1 ",300642,"轴2的2个编码器角度偏差超限","故障 "]
["SD03-1 ",300643,"轴3的2个编码器角度偏差超限","故障 "]
["SD03-1 ",300670,"轴123桨距角两两偏差超限","故障 "]
["SD03-1 ",300681,"轴1实际桨距角与设定值偏差超限","故障 "]
["SD03-1 ",300682,"轴2实际桨距角与设定值偏差超限","故障 "]
["SD03-1 ",300683,"轴3实际桨距角与设定值偏差超限","故障 "]
["SD03-1 ",300684,"轴1实际桨距角与设定值偏差超限报警","告警信息 "]
["SD03-1 ",300685,"轴2实际桨距角与设定值偏差超限报警","告警信息 "]
["SD03-1 ",300686,"轴3实际桨距角与设定值偏差超限报警","告警信息 "]
["SD03-1 ",300691,"桨叶轴承润滑出错","告警信息 "]
["SD03-1 ",300692,"桨叶齿轮润滑出错","告警信息 "]
["SD03-1 ",300705,"变桨系统手动维护模式","故障 "]
["SD03-1 ",300708,"变桨紧停1","故障 "]
["SD03-1 ",300709,"变桨紧停2","故障 "]
["SD03-1 ",300711,"变桨系统轴柜1温度超限","故障 "]
["SD03-1 ",300712,"变桨系统轴柜2温度超限","故障 "]
["SD03-1 ",300713,"变桨系统轴柜3温度超限","故障 "]
["SD03-1 ",300720,"变桨系统轮毂温度超限","故障 "]
["SD03-1 ",300901,"变桨系统轴1安全运行模式","故障 "]
["SD03-1 ",300902,"变桨系统轴2安全运行模式","故障 "]
["SD03-1 ",300903,"变桨系统轴3安全运行模式","故障 "]
["SD03-1 ",300904,"变桨系统轴1驱动器Level1故障","故障 "]
["SD03-1 ",300905,"变桨系统轴2驱动器Level1故障","故障 "]
["SD03-1 ",300906,"变桨系统轴3驱动器Level1故障","故障 "]
["SD03-1 ",300907,"桨叶轴承润滑油位低","告警信息 "]
["SD03-1 ",300908,"桨叶齿轮润滑油位低","告警信息 "]
["SD03-1 ",300909,"变桨充电电池故障","故障 "]
["SD03-1 ",300910,"三个轴柜加热器供电断开","故障 "]
["SD03-1 ",300911,"变桨96°旁路开关激活","故障 "]
["SD03-1 ",300912,"备留","提示信息 "]
["SD03-1 ",300951,"变桨系统轴1未准备运行","故障 "]
["SD03-1 ",300952,"变桨系统轴2未准备运行","故障 "]
["SD03-1 ",300953,"变桨系统轴3未准备运行","故障 "]
["SD03-1 ",300954,"变桨系统轴1通讯故障","故障 "]
["SD03-1 ",300955,"变桨系统轴2通讯故障","故障 "]
["SD03-1 ",300956,"变桨系统轴3通讯故障","故障 "]
["SD03-1 ",300957,"变桨系统与主控之间通讯故障","故障 "]
["SD03-1 ",300958,"变桨系统轴1驱动器Level2故障","故障 "]
["SD03-1 ",300959,"变桨系统轴2驱动器Level2故障","故障 "]
["SD03-1 ",300960,"变桨系统轴3驱动器Level2故障","故障 "]
["SD03-1 ",300961,"变桨系统轴1驱动器超速","故障 "]
["SD03-1 ",300962,"变桨系统轴2驱动器超速","故障 "]
["SD03-1 ",300963,"变桨系统轴3驱动器超速","故障 "]
["SD03-1 ",300964,"变桨系统400V交流电故障","故障 "]
["SD03-1 ",300965,"变桨系统外部输出电压错误","故障 "]
["SD03-1 ",300966,"变桨系统熔断器故障","故障 "]
["SD03-1 ",300967,"变桨系统24V电源故障","故障 "]
["SD03-1 ",300968,"变桨系统油泵DC24V供电OK","故障 "]
["SD03-1 ",300969,"变桨轴1实际驱动器故障","故障 "]
["SD03-1 ",300970,"变桨轴2实际驱动器故障","故障 "]
["SD03-1 ",300971,"变桨轴3实际驱动器故障","故障 "]
["SD03-1 ",300972,"备留","提示信息 "]
["SD03-1 ",300973,"备留","提示信息 "]
["SD03-1 ",300974,"备留","提示信息 "]
["SD03-1 ",300975,"备留","提示信息 "]
["SD03-1 ",300976,"备留","提示信息 "]
["SD03-1 ",300981,"变桨控制器Pcu紧停","告警信息 "]
["SD03-1 ",300982,"变桨控制器Tcu紧停","告警信息 "]
["SD03-1 ",300983,"变桨控制器Tcu正常停机","告警信息 "]
["SD03-1 ",300984,"变桨控制器Tcu报警","告警信息 "]
["SD03-1 ",300985,"变桨系统故障","故障 "]
["SD03-1 ",300986,"备留","提示信息 "]
["SD03-1 ",300987,"备留","提示信息 "]
["SD03-1 ",300991,"备留","提示信息 "]
["SD03-1 ",300992,"备留","提示信息 "]
["SD03-1 ",300993,"备留","提示信息 "]
["SD03-1 ",300994,"备留","提示信息 "]
["SD03-1 ",300995,"备留","提示信息 "]
["SD03-1 ",300996,"备留","提示信息 "]
["SD03-1 ",300997,"备留","提示信息 "]
["SD03-1 ",300998,"备留","提示信息 "]
["SD03-1 ",300999,"备留","提示信息 "]
["SD03-1 ",301000,"备留","提示信息 "]
["SD03-1 ",301101,"备留","提示信息 "]
["SD03-1 ",301102,"备留","提示信息 "]
["SD03-1 ",301103,"备留","提示信息 "]
["SD03-1 ",301104,"备留","提示信息 "]
["SD03-1 ",301105,"备留","提示信息 "]
["SD03-1 ",301106,"备留","提示信息 "]
["SD03-1 ",301107,"备留","提示信息 "]
["SD03-1 ",301108,"备留","提示信息 "]
["SD03-1 ",301109,"备留","提示信息 "]
["SD03-1 ",301110,"备留","提示信息 "]
["SD03-1 ",301201,"备留","提示信息 "]
["SD03-1 ",301202,"备留","提示信息 "]
["SD03-1 ",301203,"备留","提示信息 "]
["SD03-1 ",301204,"备留","提示信息 "]
["SD03-1 ",301205,"备留","提示信息 "]
["SD03-1 ",301206,"备留","提示信息 "]
["SD03-1 ",301207,"备留","提示信息 "]
["SD03-1 ",301208,"备留","提示信息 "]
["SD03-1 ",301209,"备留","提示信息 "]
["SD03-1 ",301210,"备留","提示信息 "]
["SD03-1 ",301301,"备留","提示信息 "]
["SD03-1 ",301302,"备留","提示信息 "]
["SD03-1 ",301303,"备留","提示信息 "]
["SD03-1 ",301304,"备留","提示信息 "]
["SD03-1 ",301305,"备留","提示信息 "]
["SD03-1 ",301306,"备留","提示信息 "]
["SD03-1 ",301307,"备留","提示信息 "]
["SD03-1 ",301308,"备留","提示信息 "]
["SD03-1 ",301309,"备留","提示信息 "]
["SD03-1 ",301310,"备留","提示信息 "]
["SD03-1 ",301401,"ACDC电源故障","故障 "]
["SD03-1 ",301402,"驱动器DCDC电源故障","故障 "]
["SD03-1 ",301403,"PLC DCDC电源故障","故障 "]
["SD03-1 ",301404,"轴1 96度限位故障","故障 "]
["SD03-1 ",301405,"轴2 96度限位故障","故障 "]
["SD03-1 ",301406,"轴3 96度限位故障","故障 "]
["SD03-1 ",301407,"变桨与主控profibus通讯故障","故障 "]
["SD03-1 ",301408,"电网电压跌落故障","故障 "]
["SD03-1 ",301409,"轴柜主电未上故障","故障 "]
["SD03-1 ",301410,"轴柜电容柜连接故障","故障 "]
["SD03-1 ",301501,"桨叶不同步故障","故障 "]
["SD03-1 ",301502,"避雷器故障","故障 "]
["SD03-1 ",301503,"同轴编码器不同步","故障 "]
["SD03-1 ",301504,"电容模块过压","故障 "]
["SD03-1 ",301505,"电容模块过温","故障 "]
["SD03-1 ",301506,"DC24V供电故障","故障 "]
["SD03-1 ",301507,"PLC模块故障","故障 "]
["SD03-1 ",301508,"P1驱动器故障","故障 "]
["SD03-1 ",301509,"P2驱动器故障","故障 "]
["SD03-1 ",301510,"P3驱动器故障","故障 "]
["SD03-1 ",301601,"安全链断开","故障 "]
["SD03-1 ",301602,"变桨系统Canopen通讯故障","故障 "]
["SD03-1 ",301603,"CPU电池电量低","故障 "]
["SD03-1 ",301604,"编码器读数故障","故障 "]
["SD03-1 ",301605,"轴1抱闸接触器故障","故障 "]
["SD03-1 ",301606,"轴2抱闸接触器故障","故障 "]
["SD03-1 ",301607,"轴3抱闸接触器故障","故障 "]
["SD03-1 ",301608,"备留","提示信息 "]
["SD03-1 ",301609,"备留","提示信息 "]
["SD03-1 ",301610,"备留","提示信息 "]
["SD03-1 ",301701,"备留","提示信息 "]
["SD03-1 ",301702,"备留","提示信息 "]
["SD03-1 ",301703,"备留","提示信息 "]
["SD03-1 ",301704,"备留","提示信息 "]
["SD03-1 ",301705,"备留","提示信息 "]
["SD03-1 ",301706,"备留","提示信息 "]
["SD03-1 ",301707,"备留","提示信息 "]
["SD03-1 ",301708,"备留","提示信息 "]
["SD03-1 ",301709,"备留","提示信息 "]
["SD03-1 ",301710,"备留","提示信息 "]
["SD03-1 ",301801,"备留","提示信息 "]
["SD03-1 ",301802,"备留","提示信息 "]
["SD03-1 ",301803,"备留","提示信息 "]
["SD03-1 ",301804,"备留","提示信息 "]
["SD03-1 ",301805,"备留","提示信息 "]
["SD03-1 ",301806,"备留","提示信息 "]
["SD03-1 ",301807,"备留","提示信息 "]
["SD03-1 ",301808,"备留","提示信息 "]
["SD03-1 ",301809,"备留","提示信息 "]
["SD03-1 ",301810,"备留","提示信息 "]
["SD03-1 ",320000,"变压器超温开关动作","故障 "]
["SD03-1 ",320001,"变压器温度超限","故障 "]
["SD03-1 ",320002,"变压器轻瓦斯报警","告警信息 "]
["SD03-1 ",320003,"变压器重瓦斯故障","告警信息 "]
["SD03-1 ",320004,"高压负荷开关断开","告警信息 "]
["SD03-1 ",320005,"高压侧熔断器熔断","告警信息 "]
["SD03-1 ",320006,"箱变门开启","告警信息 "]
["SD03-1 ",320007,"低压侧断路器断开","告警信息 "]
["SD03-1 ",320008,"箱变超温报警","告警信息 "]
["SD03-1 ",320009,"箱变压力释放","告警信息 "]
["SD03-1 ",320010,"箱变故障信号'","告警信息 "]
["SD03-1 ",320011,"箱变油位低","告警信息 "]
["SD03-1 ",320012,"备留","提示信息 "]
["SD03-1 ",320013,"备留","提示信息 "]
["SD03-1 ",320014,"备留","提示信息 "]
["SD03-1 ",320015,"备留","提示信息 "]
["SD03-1 ",320016,"备留","提示信息 "]
["SD03-1 ",320017,"备留","提示信息 "]
["SD03-1 ",320018,"备留","提示信息 "]
["SD03-1 ",320019,"备留","提示信息 "]
["SD03-1 ",320020,"备留","提示信息 "]
["SD03-1 ",320021,"备留","提示信息 "]
["SD03-1 ",320022,"备留","提示信息 "]
["SD03-1 ",320023,"备留","提示信息 "]
["SD03-1 ",320024,"备留","提示信息 "]
["SD03-1 ",340000,"备留","提示信息 "]
["SD03-1 ",340001,"备留","提示信息 "]
["SD03-1 ",340002,"备留","提示信息 "]
["SD03-1 ",340003,"备留","提示信息 "]
["SD03-1 ",340004,"备留","提示信息 "]
["SD03-1 ",340005,"备留","提示信息 "]
["SD03-1 ",340006,"备留","提示信息 "]
["SD03-1 ",340007,"备留","提示信息 "]
["SD03-1 ",340008,"备留","提示信息 "]
["SD03-1 ",340009,"备留","提示信息 "]
["SD03-1 ",340010,"备留","提示信息 "]
["SD03-1 ",340011,"备留","提示信息 "]
["SD03-1 ",340012,"备留","提示信息 "]
["SD03-1 ",340013,"备留","提示信息 "]
["SD03-1 ",340014,"备留","提示信息 "]
["SD03-1 ",350005,"塔底出风口风扇保护","故障 "]
["SD03-1 ",350006,"塔底进风口风扇保护","故障 "]
["SD03-1 ",350007,"备留","提示信息 "]
["SD03-1 ",350008,"备留","提示信息 "]
["SD03-1 ",350009,"备留","提示信息 "]
["SD03-1 ",350011,"塔底温度超限","故障 "]
["SD03-1 ",350012,"备留","提示信息 "]
["SD03-1 ",350013,"备留","提示信息 "]
["SD03-1 ",350014,"备留","提示信息 "]
["SD03-1 ",350015,"备留","提示信息 "]
["SD03-1 ",350016,"备留","提示信息 "]
["SD03-1 ",350017,"备留","提示信息 "]
["SD03-1 ",350018,"备留","提示信息 "]
["SD03-1 ",350019,"备留","提示信息 "]
["SD03-1 ",350020,"备留","提示信息 "]
["SD03-1 ",650001,"航灯保护","故障 "]
["SD03-1 ",650003,"备留","提示信息 "]
["SD03-1 ",650004,"备留","提示信息 "]
["SD03-1 ",650005,"备留","提示信息 "]
["SD03-1 ",650006,"备留","提示信息 "]
["SD03-1 ",650007,"备留","提示信息 "]
["SD03-1 ",650008,"备留","提示信息 "]
["SD03-1 ",650009,"备留","提示信息 "]
["SD03-1 ",650010,"备留","提示信息 "]
["SD03-1 ",650011,"备留","提示信息 "]
["SD03-1 ",700002,"风轮转速比较出错","故障 "]
["SD03-1 ",700003,"风轮转速超速1","故障 "]
["SD03-1 ",700004,"风轮转速超速2","故障 "]
["SD03-1 ",700005,"发电机侧编码器测得超速","故障 "]
["SD03-1 ",700007,"备留","提示信息 "]
["SD03-1 ",700008,"备留","提示信息 "]
["SD03-1 ",700010,"备留","提示信息 "]
["SD03-1 ",700011,"低速轴SSI编码器测速故障","告警信息 "]
["SD03-1 ",700012,"低速轴过速模块测速故障","告警信息 "]
["SD03-1 ",700013,"发电机转速测速故障","告警信息 "]
["SD03-1 ",700014,"备留","提示信息 "]
["SD03-1 ",700015,"备留","提示信息 "]
["SD03-1 ",700016,"备留","提示信息 "]
["SD03-1 ",700017,"备留","提示信息 "]
["SD03-1 ",700018,"备留","提示信息 "]
["SD03-1 ",800001,"塔底紧停开关触发","提示信息 "]
["SD03-1 ",800002,"机舱紧停开关触发","提示信息 "]
["SD03-1 ",800003,"机舱远程紧停开关触发","提示信息 "]
["SD03-1 ",800004,"塔底主电源供电故障","故障 "]
["SD03-1 ",800011,"风轮超速1紧停","故障 "]
["SD03-1 ",800012,"风轮超速2紧停","故障 "]
["SD03-1 ",800015,"机舱振动开关动作","故障 "]
["SD03-1 ",800017,"偏航扭缆限位开关动作","故障 "]
["SD03-1 ",800020,"变桨系统紧停动作","故障 "]
["SD03-1 ",800030,"变频器紧停","故障 "]
["SD03-1 ",800031,"变频器并网开关故障","故障 "]
["SD03-1 ",800070,"安全系统紧停","故障 "]
["SD03-1 ",800071,"备留","提示信息 "]
["SD03-1 ",800075,"备留","提示信息 "]
["SD03-1 ",800077,"备留","提示信息 "]
["SD03-1 ",800081,"备留","提示信息 "]
["SD03-1 ",800082,"备留","提示信息 "]
["SD03-1 ",800083,"备留","提示信息 "]
["SD03-1 ",800091,"备留","提示信息 "]
["SD03-1 ",800092,"备留","提示信息 "]
["SD03-1 ",800101,"备留","提示信息 "]
["SD03-1 ",800102,"备留","提示信息 "]
["SD03-1 ",800103,"备留","提示信息 "]
["SD03-1 ",800104,"备留","提示信息 "]
["SD03-1 ",800105,"备留","提示信息 "]
["SD03-1 ",800106,"备留","提示信息 "]
["SD03-1 ",800107,"备留","提示信息 "]
["SD03-1 ",800108,"备留","提示信息 "]
["SD03-1 ",800109,"备留","提示信息 "]
["SD03-1 ",800110,"备留","提示信息 "]
["SD03-1 ",800111,"备留","提示信息 "]
["SD03-1 ",800112,"备留","提示信息 "]
["SD03-1 ",800113,"备留","提示信息 "]
["SD03-1 ",800114,"备留","提示信息 "]
["SD03-1 ",800115,"备留","提示信息 "]
["SD03-1 ",900101,"塔底DI9371-01模块故障","故障 "]
["SD03-1 ",900102,"塔底DI9371-02模块故障","故障 "]
["SD03-1 ",900111,"塔底AT4222-01模块故障","故障 "]
["SD03-1 ",900121,"备留","提示信息 "]
["SD03-1 ",900131,"塔底CM0985模块故障","故障 "]
["SD03-1 ",900141,"塔底DO9322-01模块故障","故障 "]
["SD03-1 ",900142,"塔底DO9322-02模块故障","故障 "]
["SD03-1 ",900151,"塔底SI4100-01模块故障","故障 "]
["SD03-1 ",900152,"塔底SI4100-02模块故障","故障 "]
["SD03-1 ",900153,"塔底SO2110-01模块故障","故障 "]
["SD03-1 ",900154,"塔底安全逻辑模块故障","故障 "]
["SD03-1 ",900161,"塔底总线控制器模块故障","故障 "]
["SD03-1 ",900171,"塔底电源PS9400-01模块故障","故障 "]
["SD03-1 ",900201,"机舱DI9371-01模块故障","故障 "]
["SD03-1 ",900202,"机舱DI9371-02模块故障","故障 "]
["SD03-1 ",900203,"机舱DI9371-03模块故障","故障 "]
["SD03-1 ",900204,"机舱DI9371-04模块故障","故障 "]
["SD03-1 ",900205,"机舱DI9371-05模块故障","故障 "]
["SD03-1 ",900206,"机舱DI9371-06模块故障","故障 "]
["SD03-1 ",900207,"机舱DI9371-07模块故障","故障 "]
["SD03-1 ",900211,"备留","提示信息 "]
["SD03-1 ",900212,"备留","提示信息 "]
["SD03-1 ",900221,"机舱DO9322-01模块故障","故障 "]
["SD03-1 ",900222,"机舱DO9322-02模块故障","故障 "]
["SD03-1 ",900223,"机舱DO9322-03模块故障","故障 "]
["SD03-1 ",900224,"机舱DO9322-04模块故障","故障 "]
["SD03-1 ",900231,"机舱SI4100-01模块故障","故障 "]
["SD03-1 ",900232,"机舱SI4100-02模块故障","故障 "]
["SD03-1 ",900233,"机舱SO4110-01模块故障","故障 "]
["SD03-1 ",900241,"机舱AI4622-01模块故障","故障 "]
["SD03-1 ",900242,"机舱AI4622-02模块故障","故障 "]
["SD03-1 ",900243,"机舱AI4622-03模块故障","故障 "]
["SD03-1 ",900244,"备留","提示信息 "]
["SD03-1 ",900251,"机舱DC1198-01模块故障","故障 "]
["SD03-1 ",900252,"机舱DC1198-02模块故障","故障 "]
["SD03-1 ",900261,"机舱AT4222-01模块故障","故障 "]
["SD03-1 ",900262,"机舱AT4222-02模块故障","故障 "]
["SD03-1 ",900263,"机舱AT4222-03模块故障","故障 "]
["SD03-1 ",900264,"机舱AT4222-04模块故障","故障 "]
["SD03-1 ",900265,"机舱AT4222-05模块故障","故障 "]
["SD03-1 ",900266,"CP1483模块故障","故障 "]
["SD03-1 ",900271,"机舱总线控制器模块故障","故障 "]
["SD03-1 ",900281,"机舱电源PS9400-02模块故障","故障 "]
["SD03-1 ",900286,"机舱电源PS3300-01模块故障","故障 "]
["SD03-1 ",900301,"轴柜3总线控制器模块故障","故障 "]
["SD03-1 ",900302,"机舱BC1083电源PS9400模块故障","故障 "]
["SD03-1 ",900303,"轴柜3DI9371-1模块故障","故障 "]
["SD03-1 ",900304,"轴柜3DI9371-2模块故障","故障 "]
["SD03-1 ",900305,"轴柜2DI9371-1模块故障","故障 "]
["SD03-1 ",900310,"轴柜2DI9371-2模块故障","故障 "]
["SD03-1 ",900401,"轴柜1DI9371-1模块故障","故障 "]
["SD03-1 ",900402,"轴柜1DI9371-2模块故障","故障 "]
["SD03-1 ",900403,"轴柜3DO9322模块故障","故障 "]
["SD03-1 ",900404,"轴柜2DO9322模块故障","故障 "]
["SD03-1 ",900405,"轴柜1DO9322模块故障","故障 "]
["SD03-1 ",900406,"轴柜3AT4222模块故障","故障 "]
["SD03-1 ",900407,"轴柜2AT4222模块故障","故障 "]
["SD03-1 ",900408,"轴柜1AT4222模块故障","故障 "]
["SD03-1 ",900409,"轴柜3BT9100模块故障","故障 "]
["SD03-1 ",900410,"轴柜2BT9100模块故障","故障 "]
["SD03-1 ",900501,"轴柜2BR9300模块故障","故障 "]
["SD03-1 ",900502,"轴柜1BR9300模块故障","故障 "]
["SD03-1 ",900503,"驱动器1故障","故障 "]
["SD03-1 ",900504,"驱动器2故障","故障 "]
["SD03-1 ",900505,"驱动器3故障","故障 "]
["SD03-1 ",900506,"轮毂BC0043远程IO模块故障","故障 "]
["SD03-1 ",900507,"备留","提示信息 "]
["SD03-1 ",900508,"备留","提示信息 "]
["SD03-1 ",900509,"备留","提示信息 "]
["SD03-1 ",900510,"备留","提示信息 "]
["SD03-1 ",910000,"塔底停止按钮激活","提示信息 "]
["SD03-1 ",910001,"塔底远程停止激活","提示信息 "]
["SD03-1 ",910002,"机舱停止按钮激活","提示信息 "]
["SD03-1 ",910006,"SCADA停止按钮激活","提示信息 "]
["SD03-1 ",910007,"画面停止按钮激活","提示信息 "]
["SD03-1 ",910008,"塔底紧停开关激活","提示信息 "]
["SD03-1 ",910010,"机舱紧停开关激活","提示信息 "]
["SD03-1 ",910011,"机舱远程紧停开关激活","提示信息 "]
["SD03-1 ",910012,"塔底复位按钮故障","提示信息 "]
["SD03-1 ",910013,"机舱复位按钮故障","提示信息 "]
["SD03-1 ",910021,"备留","提示信息 "]
["SD03-1 ",910022,"备留","提示信息 "]
["SD03-1 ",910023,"备留","提示信息 "]
["SD03-1 ",910024,"备留","提示信息 "]
["SD03-1 ",910025,"备留","提示信息 "]
["SD03-1 ",910026,"备留","提示信息 "]
["SD03-1 ",910027,"备留","提示信息 "]
["SD03-1 ",910028,"备留","提示信息 "]
["SD03-1 ",910029,"备留","提示信息 "]
["SD03-1 ",910030,"备留","提示信息 "]
["SD03-1 ",910031,"备留","提示信息 "]
["SD03-1 ",910032,"备留","提示信息 "]
["SD03-1 ",910033,"备留","提示信息 "]
["SD03-1 ",910034,"备留","提示信息 "]
["SD03-1 ",910035,"备留","提示信息 "]
["HZ15 ",-5,"通讯恢复","提示信息 "]
["HZ15 ",-4,"通讯中断","告警信息 "]
["HZ15 ",-3,"恢复连接","提示信息 "]
["HZ15 ",-2,"无连接","告警信息 "]
["HZ15 ",-1,"初始化","提示信息 "]
["HZ15 ",0,"系统正常","提示信息 "]
["HZ15 ",100,"存储器分配故障（WTC系统故障）","故障 "]
["HZ15 ",101,"事件表满（WTC系统故障）","故障 "]
["HZ15 ",102,"事件日志复位（WTC系统故障）","故障 "]
["HZ15 ",103,"无效处理（WTC系统故障）","故障 "]
["HZ15 ",104,"无效OP-bit（WTC系统故障）","故障 "]
["HZ15 ",105,"安装错误（WTC系统故障）","故障 "]
["HZ15 ",106,"事件日志写溢出（WTC系统故障）","故障 "]
["HZ15 ",107,"写权限已给出（WTC系统故障）","故障 "]
["HZ15 ",108,"未找到名称（WTC系统故障）","故障 "]
["HZ15 ",109,"命令已使用（WTC系统故障）","故障 "]
["HZ15 ",110,"无效参数（WTC系统故障）","故障 "]
["HZ15 ",111,"定时器已使用但未启动（WTC系统故障）","故障 "]
["HZ15 ",112,"I/O配置故障（WTC系统故障）","故障 "]
["HZ15 ",113,"链接列表故障（WTC系统故障）","故障 "]
["HZ15 ",114,"未知数据类型（WTC系统故障）","故障 "]
["HZ15 ",115,"得出未知空指针（WTC系统故障）","故障 "]
["HZ15 ",116,"无效CDI索引（WTC系统故障）","故障 "]
["HZ15 ",117,"事件日志混乱（WTC系统故障）","故障 "]
["HZ15 ",118,"签名故障（WTC系统故障）","故障 "]
["HZ15 ",119,"文件不存在警告","告警信息 "]
["HZ15 ",120,"Nv类型变化（WTC系统故障）","故障 "]
["HZ15 ",121,"XML文件故障（WTC系统故障）","故障 "]
["HZ15 ",122,"字符串太长（WTC系统故障）","故障 "]
["HZ15 ",123,"默认状态开关终止（WTC系统故障）","故障 "]
["HZ15 ",124,"错误的数据类型（WTC系统故障）","故障 "]
["HZ15 ",125,"事件被禁止警告","告警信息 "]
["HZ15 ",126,"系统启动错误","故障 "]
["HZ15 ",127,"变量被手动控制警告","告警信息 "]
["HZ15 ",128,"许可密钥无效（WTC系统故障）","故障 "]
["HZ15 ",129,"NV_RAM与制造厂商不匹配（WTC系统故障）","故障 "]
["HZ15 ",130,"应用周期超限（WTC系统故障）","故障 "]
["HZ15 ",131,"变量已经被手动些信息","提示信息 "]
["HZ15 ",132,"重启信息","提示信息 "]
["HZ15 ",133,"不能创建Nv文件","故障 "]
["HZ15 ",134,"以太网错误（WTC系统故障）","故障 "]
["HZ15 ",135,"NV-RAMerror（WTC系统错误）","故障 "]
["HZ15 ",136,"Applicationwatchdog引起重启（WTC系统错误）","故障 "]
["HZ15 ",137,"SEESF应用程序命令丢失（WTC系统错误）","故障 "]
["HZ15 ",138,"虚拟模块存在信息","提示信息 "]
["HZ15 ",139,"CanKK正在重启","故障 "]
["HZ15 ",140,"远程服务模式使能警告","告警信息 "]
["HZ15 ",141,"CAT通讯警告","告警信息 "]
["HZ15 ",142,"错误风机类型（WTC系统错误）","故障 "]
["HZ15 ",143,"NVfile不能备份NV文件警告","告警信息 "]
["HZ15 ",145,"操作系统相关错误（WTC系统错误）","故障 "]
["HZ15 ",1000,"齿轮箱油温度过高故障（油温开关）","故障 "]
["HZ15 ",1001,"齿轮箱油池测量温度过低故障","故障 "]
["HZ15 ",1002,"齿轮箱油池测量温度超温故障","故障 "]
["HZ15 ",1003,"齿轮箱油池温度低警告","告警信息 "]
["HZ15 ",1004,"齿轮箱油池温度高警告","告警信息 "]
["HZ15 ",1005,"齿轮箱油泵电机过载故障","故障 "]
["HZ15 ",1007,"齿轮箱油出口压力过低故障","故障 "]
["HZ15 ",1008,"齿轮箱出口低压力警告","告警信息 "]
["HZ15 ",1009,"齿轮箱油位过低故障","故障 "]
["HZ15 ",1010,"齿轮箱油入口测量温度过低故障","故障 "]
["HZ15 ",1011,"齿轮箱油入口测量温度过高故障","故障 "]
["HZ15 ",1012,"齿轮箱入口油温低警告","告警信息 "]
["HZ15 ",1013,"齿轮箱入口油温高警告","告警信息 "]
["HZ15 ",1014,"齿轮箱油加热器过载故障","故障 "]
["HZ15 ",1015,"齿轮箱油过滤差压过高警告","告警信息 "]
["HZ15 ",1016,"齿轮箱油差压过高故障","故障 "]
["HZ15 ",1017,"齿轮箱高油压差警告","告警信息 "]
["HZ15 ",1019,"齿轮箱油旁路过滤压力警告","告警信息 "]
["HZ15 ",1020,"齿轮箱油泵电机待机加热过载故障","故障 "]
["HZ15 ",1021,"齿轮箱冷却风扇过载故障","故障 "]
["HZ15 ",1022,"齿轮箱冷却水温度过低故障","故障 "]
["HZ15 ",1023,"齿轮箱冷却水温度过高故障","故障 "]
["HZ15 ",1024,"齿轮箱冷却水温低警告","告警信息 "]
["HZ15 ",1025,"齿轮箱冷却水温高警告","告警信息 "]
["HZ15 ",1026,"齿轮箱冷却水泵过载故障","故障 "]
["HZ15 ",1027,"齿轮箱冷却水压力开关故障","故障 "]
["HZ15 ",1028,"齿轮箱旁路过滤泵过载故障","故障 "]
["HZ15 ",1030,"齿轮箱低速侧轴承近端温度过高故障","故障 "]
["HZ15 ",1033,"齿轮箱高速轴承温度1警告","告警信息 "]
["HZ15 ",1034,"齿轮箱高速侧轴承近端温度过高故障","故障 "]
["HZ15 ",1035,"齿轮箱高速轴承温度2警告","告警信息 "]
["HZ15 ",1036,"齿轮箱高速侧轴承前端温度过高故障","故障 "]
["HZ15 ",2000,"偏航极限开关触发故障","故障 "]
["HZ15 ",2001,"偏航解缆信息","提示信息 "]
["HZ15 ",2002,"偏航润滑系统故障","故障 "]
["HZ15 ",2004,"1#偏航电机过载故障","故障 "]
["HZ15 ",2005,"2#偏航电机过载故障","故障 "]
["HZ15 ",2006,"3#偏航电机过载故障","故障 "]
["HZ15 ",2007,"4#偏航电机过载故障","故障 "]
["HZ15 ",2011,"偏航软启故障","故障 "]
["HZ15 ",2012,"偏航风向失调超过最大故障","故障 "]
["HZ15 ",2030,"偏航电机单次动作时间达到极限故障","故障 "]
["HZ15 ",2037,"偏航条件解缆激活","提示信息 "]
["HZ15 ",2038,"偏航无条件解缆激活","提示信息 "]
["HZ15 ",2045,"偏航机舱未移动故障","故障 "]
["HZ15 ",2046,"偏航速度过低故障","故障 "]
["HZ15 ",2047,"偏航润滑油位低故障","故障 "]
["HZ15 ",2049,"电缆缠绕预置解缆位置没有设置警告","告警信息 "]
["HZ15 ",2050,"机舱位置没有校正警告","告警信息 "]
["HZ15 ",2054,"偏航电机电磁刹车过载故障","故障 "]
["HZ15 ",3000,"前轴温度高警告","告警信息 "]
["HZ15 ",3001,"后轴温度高警告","告警信息 "]
["HZ15 ",3002,"主轴承前端温度过高故障","故障 "]
["HZ15 ",3003,"主轴承近端温度过高故障","故障 "]
["HZ15 ",4000,"变桨位置不同步故障","故障 "]
["HZ15 ",4001,"变桨400V电源过载故障","故障 "]
["HZ15 ",4002,"变桨1#叶片编码器不一致故障","故障 "]
["HZ15 ",4003,"变桨2#叶片编码器不一致故障","故障 "]
["HZ15 ",4004,"变桨3#叶片编码器不一致故障","故障 "]
["HZ15 ",4006,"变桨1#叶片手动操作激活","提示信息 "]
["HZ15 ",4007,"变桨2#叶片手动操作激活","提示信息 "]
["HZ15 ",4008,"变桨3#叶片手动操作激活","提示信息 "]
["HZ15 ",4011,"变桨1#叶片电机温度过高故障","故障 "]
["HZ15 ",4012,"变桨2#叶片电机温度过高故障","故障 "]
["HZ15 ",4013,"变桨3#叶片电机温度过高故障","故障 "]
["HZ15 ",4014,"变桨1#叶片柜温度过高故障","故障 "]
["HZ15 ",4015,"变桨2#叶片柜温度过高故障","故障 "]
["HZ15 ",4016,"变桨3#叶片柜温度过高故障","故障 "]
["HZ15 ",4017,"变桨中控柜温度过高故障","故障 "]
["HZ15 ",4018,"轮毂温度过高故障","故障 "]
["HZ15 ",4019,"变桨1#叶片电池温度过高故障","故障 "]
["HZ15 ",4020,"变桨2#叶片电池温度过高故障","故障 "]
["HZ15 ",4021,"变桨3#叶片电池温度过高故障","故障 "]
["HZ15 ",4022,"变桨1#叶片充电电流过大故障","故障 "]
["HZ15 ",4023,"变桨1#叶片充电电流过低故障","故障 "]
["HZ15 ",4024,"变桨1#叶片电池空载电压跌落故障","故障 "]
["HZ15 ",4025,"变桨2#叶片电池空载电压跌落故障","故障 "]
["HZ15 ",4026,"变桨3#叶片电池空载电压跌落故障","故障 "]
["HZ15 ",4028,"变桨2#叶片充电电流过大故障","故障 "]
["HZ15 ",4029,"变桨2#叶片充电电流过低故障","故障 "]
["HZ15 ",4030,"变桨3#叶片充电电流过大故障","故障 "]
["HZ15 ",4031,"变桨3#叶片充电电流过低故障","故障 "]
["HZ15 ",4032,"变桨系统检测1#叶片PMM散热器温度过高故障","故障 "]
["HZ15 ",4033,"变桨系统检测2#叶片PMM散热器温度过高故障","故障 "]
["HZ15 ",4034,"变桨系统检测3#叶片PMM散热器温度过高故障","故障 "]
["HZ15 ",4035,"变桨系统检测1#叶片电机温度过高故障","故障 "]
["HZ15 ",4036,"变桨系统检测2#叶片电机温度过高故障","故障 "]
["HZ15 ",4037,"变桨系统检测3#叶片电机温度过高故障","故障 "]
["HZ15 ",4038,"变桨系统检测雷电保护故障","故障 "]
["HZ15 ",4039,"变桨系统检测1#叶片PMC警告","告警信息 "]
["HZ15 ",4040,"变桨系统检测2#叶片PMC警告","告警信息 "]
["HZ15 ",4041,"变桨系统检测3#叶片PMC警告","告警信息 "]
["HZ15 ",4042,"变桨系统检测1#叶片编码器故障","故障 "]
["HZ15 ",4043,"变桨系统检测1#叶片电池温度过高故障","故障 "]
["HZ15 ",4044,"变桨系统检测2#叶片电池温度过高故障","故障 "]
["HZ15 ",4045,"变桨系统检测3#叶片电池温度过高故障","故障 "]
["HZ15 ",4046,"变桨系统检测1#叶片温度传感器故障","故障 "]
["HZ15 ",4047,"变桨系统检测2#叶片温度传感器故障","故障 "]
["HZ15 ",4048,"变桨系统检测3#叶片温度传感器故障","故障 "]
["HZ15 ",4050,"1#叶片变桨没有心跳故障","故障 "]
["HZ15 ",4051,"2#叶片变桨没有心跳故障","故障 "]
["HZ15 ",4052,"3#叶片变桨没有心跳故障","故障 "]
["HZ15 ",4053,"1#叶片变桨限位开关1位置校正故障","故障 "]
["HZ15 ",4054,"2#叶片变桨限位开关1位置校正故障","故障 "]
["HZ15 ",4055,"3#叶片变桨限位开关1位置校正故障","故障 "]
["HZ15 ",4056,"变桨系统检测2#叶片编码器故障","故障 "]
["HZ15 ",4057,"变桨1#叶片无效的PMC硬件版本故障","故障 "]
["HZ15 ",4058,"变桨2#叶片无效的PMC硬件版本故障","故障 "]
["HZ15 ",4059,"变桨3#叶片无效的PMC硬件版本故障","故障 "]
["HZ15 ",4060,"变桨1#叶片无效的PMC软件版本故障","故障 "]
["HZ15 ",4061,"变桨2#叶片无效的PMC软件版本故障","故障 "]
["HZ15 ",4062,"变桨3#叶片无效的PMC软件版本故障","故障 "]
["HZ15 ",4063,"变桨1#叶片无效的PMM硬件版本故障","故障 "]
["HZ15 ",4064,"变桨2#叶片无效的PMM硬件版本故障","故障 "]
["HZ15 ",4065,"变桨3#叶片无效的PMM硬件版本故障","故障 "]
["HZ15 ",4066,"变桨1#叶片无效的PMM软件版本故障","故障 "]
["HZ15 ",4067,"变桨2#叶片无效的PMM软件版本故障","故障 "]
["HZ15 ",4068,"变桨3#叶片无效的PMM软件版本故障","故障 "]
["HZ15 ",4070,"变桨系统检测3#叶片编码器故障","故障 "]
["HZ15 ",4071,"变桨1#叶片报告PMC故障","故障 "]
["HZ15 ",4072,"变桨2#叶片报告PMC故障","故障 "]
["HZ15 ",4073,"变桨3#叶片报告PMC故障","故障 "]
["HZ15 ",4074,"变桨1#叶片报告PMM故障","故障 "]
["HZ15 ",4075,"变桨2#叶片报告PMM故障","故障 "]
["HZ15 ",4076,"变桨3#叶片报告PMM故障","故障 "]
["HZ15 ",4082,"变桨系统传感器测试失败故障","故障 "]
["HZ15 ",4083,"变桨系统检测1#叶片PMC散热器温度过高故障","故障 "]
["HZ15 ",4084,"变桨系统检测2#叶片PMC散热器温度过高故障","故障 "]
["HZ15 ",4085,"变桨系统检测3#叶片PMC散热器温度过高故障","故障 "]
["HZ15 ",4086,"变桨1#叶片电池健康状态太低故障","故障 "]
["HZ15 ",4087,"变桨2#叶片电池健康状态太低故障","故障 "]
["HZ15 ",4088,"变桨3#叶片电池健康状态太低故障","故障 "]
["HZ15 ",4089,"变桨1#叶片电池充电太低故障","故障 "]
["HZ15 ",4090,"变桨2#叶片电池充电太低故障","故障 "]
["HZ15 ",4091,"变桨3#叶片电池充电太低故障","故障 "]
["HZ15 ",4092,"变桨1#叶片PMM散热器温度过高故障","故障 "]
["HZ15 ",4093,"变桨2#叶片PMM散热器温度过高故障","故障 "]
["HZ15 ",4094,"变桨3#叶片PMM散热器温度过高故障","故障 "]
["HZ15 ",4095,"变桨系统检测1#叶片PMM警告","告警信息 "]
["HZ15 ",4096,"变桨系统检测2#叶片PMM警告","告警信息 "]
["HZ15 ",4097,"变桨系统检测3#叶片PMM警告","告警信息 "]
["HZ15 ",4098,"变桨1#叶片PMC散热器温度过高故障","故障 "]
["HZ15 ",4099,"变桨2#叶片PMC散热器温度过高故障","故障 "]
["HZ15 ",4100,"变桨3#叶片PMC散热器温度过高故障","故障 "]
["HZ15 ",4103,"变桨系统检测1#叶片400VAC供电失效信息","提示信息 "]
["HZ15 ",4104,"#叶片400VAC供电失效信息","提示信息 "]
["HZ15 ",4105,"变桨系统检测3#叶片400VAC供电失效信息","提示信息 "]
["HZ15 ",4106,"变桨1#叶片400Vac电源失效过久故障","故障 "]
["HZ15 ",4107,"变桨2#叶片400Vac电源失效过久故障","故障 "]
["HZ15 ",4108,"变桨3#叶片400Vac电源失效过久故障","故障 "]
["HZ15 ",4109,"变桨1#叶片追踪故障","故障 "]
["HZ15 ",4110,"变桨2#叶片追踪故障","故障 "]
["HZ15 ",4111,"变桨3#叶片追踪故障","故障 "]
["HZ15 ",4112,"变桨系统检测 1#叶片 400VAC供电故障信息","提示信息 "]
["HZ15 ",4113,"变桨系统检测 2#叶片 400VAC供电故障信息","提示信息 "]
["HZ15 ",4114,"变桨系统检测 3#叶片 400VAC供电故障信息","提示信息 "]
["HZ15 ",4115,"变桨1#叶片自检速度过低故障","故障 "]
["HZ15 ",4116,"变桨2#叶片自检速度过低故障","故障 "]
["HZ15 ",4117,"变桨3#叶片自检速度过低故障","故障 "]
["HZ15 ",4118,"变桨1#叶片电池负载电压跌落故障","故障 "]
["HZ15 ",4119,"变桨2#叶片电池负载电压跌落故障","故障 "]
["HZ15 ",4120,"变桨3#叶片电池负载电压跌落故障","故障 "]
["HZ15 ",4121,"1#叶片变桨限位开关2位置校正故障","故障 "]
["HZ15 ",4122,"2#叶片变桨限位开关2位置校正故障","故障 "]
["HZ15 ",4123,"3#叶片变桨限位开关2位置校正故障","故障 "]
["HZ15 ",4124,"变桨1#叶片电池测试电压跌落故障","故障 "]
["HZ15 ",4125,"变桨2#叶片电池测试电压跌落故障","故障 "]
["HZ15 ",4126,"变桨3#叶片电池测试电压跌落故障","故障 "]
["HZ15 ",4127,"变桨1#电池测试间隔时间超过故障","故障 "]
["HZ15 ",4128,"变桨2#电池测试间隔时间超过故障","故障 "]
["HZ15 ",4129,"变桨3#电池测试间隔时间超过故障","故障 "]
["HZ15 ",4130,"变桨1#叶片限位开关2激活故障","故障 "]
["HZ15 ",4131,"变桨2#叶片限位开关2激活故障","故障 "]
["HZ15 ",4132,"变桨3#叶片限位开关2激活故障","故障 "]
["HZ15 ",4133,"变桨1#叶片电机电流超限故障","故障 "]
["HZ15 ",4134,"变桨2#叶片电机电流超限故障","故障 "]
["HZ15 ",4135,"变桨3#叶片电机电流超限故障","故障 "]
["HZ15 ",4136,"变桨1#叶片限位开关失效故障（SW1或SW2在小于88度被触发）","故障 "]
["HZ15 ",4137,"变桨2#叶片限位开关失效故障（SW1或SW2在小于88度被触发）","故障 "]
["HZ15 ",4138,"变桨3#叶片限位开关失效故障（SW1或SW2在小于88度被触发）","故障 "]
["HZ15 ",4139,"变桨SDO读通讯故障","故障 "]
["HZ15 ",4140,"变桨1#叶片外部24V电源失效故障","故障 "]
["HZ15 ",4141,"变桨2#叶片外部24V电源失效故障","故障 "]
["HZ15 ",4142,"变桨3#叶片外部24V电源失效故障","故障 "]
["HZ15 ",4143,"变桨SDO写通讯故障","故障 "]
["HZ15 ",4144,"变桨1#叶片内部24V电源失效故障","故障 "]
["HZ15 ",4145,"变桨2#叶片内部24V电源失效故障","故障 "]
["HZ15 ",4146,"变桨3#叶片内部24V电源失效故障","故障 "]
["HZ15 ",4147,"变桨1#叶片24V电源故障","故障 "]
["HZ15 ",4148,"变桨2#叶片24V电源故障","故障 "]
["HZ15 ",4149,"变桨3#叶片24V电源故障","故障 "]
["HZ15 ",4150,"变桨SDO读通讯超时故障","故障 "]
["HZ15 ",4151,"变桨SDO写通讯超时故障","故障 "]
["HZ15 ",4152,"变桨1#叶片控制过程故障（PMC快速停机后没有到达91度开关位置）","故障 "]
["HZ15 ",4153,"变桨2#叶片控制过程故障（PMC快速停机后没有到达91度开关位置）","故障 "]
["HZ15 ",4154,"变桨3#叶片控制过程故障（PMC快速停机后没有到达91度开关位置）","故障 "]
["HZ15 ",4155,"变桨外部24V电源电压过高故障","故障 "]
["HZ15 ",4158,"变桨1#叶片紧急停机激活故障","故障 "]
["HZ15 ",4159,"变桨2#叶片紧急停机激活故障","故障 "]
["HZ15 ",4160,"变桨3#叶片紧急停机激活故障","故障 "]
["HZ15 ",4161,"变桨1#叶片变桨限位开关未校正警告","告警信息 "]
["HZ15 ",4162,"变桨2#叶片变桨限位开关未校正警告","告警信息 "]
["HZ15 ",4166,"变桨1#叶片PMM通讯故障","故障 "]
["HZ15 ",4167,"变桨2#叶片PMM通讯故障","故障 "]
["HZ15 ",4168,"变桨3#叶片PMM通讯故障","故障 "]
["HZ15 ",4169,"变桨1#叶片PMC通讯故障","故障 "]
["HZ15 ",4170,"变桨2#叶片PMC通讯故障","故障 "]
["HZ15 ",4171,"变桨3#叶片PMC通讯故障","故障 "]
["HZ15 ",4172,"变桨1#叶片400VAC过压警告","告警信息 "]
["HZ15 ",4173,"变桨2#叶片400VAC过压警告","告警信息 "]
["HZ15 ",4174,"变桨3#叶片400VAC过压警告","告警信息 "]
["HZ15 ",4175,"变桨1#叶片400VAC缺相故障","故障 "]
["HZ15 ",4176,"变桨2#叶片400VAC缺相故障","故障 "]
["HZ15 ",4177,"变桨3#叶片400VAC缺相故障","故障 "]
["HZ15 ",4178,"变桨系统检测1#叶片追踪故障","故障 "]
["HZ15 ",4179,"变桨系统检测2#叶片追踪故障","故障 "]
["HZ15 ",4180,"变桨系统检测3#叶片追踪故障","故障 "]
["HZ15 ",4185,"变桨1#叶片无效PMC参数故障","故障 "]
["HZ15 ",4186,"变桨2#叶片无效PMC参数故障","故障 "]
["HZ15 ",4187,"变桨3#叶片无效PMC参数故障","故障 "]
["HZ15 ",4188,"变桨1#叶片无效PMM参数故障","故障 "]
["HZ15 ",4189,"变桨2#叶片无效PMM参数故障","故障 "]
["HZ15 ",4190,"变桨3#叶片无效PMM参数故障","故障 "]
["HZ15 ",4195,"变桨润滑系统故障","故障 "]
["HZ15 ",4196,"变桨润滑泵1油位低故障","故障 "]
["HZ15 ",4197,"变桨润滑泵2系统故障","故障 "]
["HZ15 ",4198,"变桨润滑最大循环时间超时警告","告警信息 "]
["HZ15 ",5000,"发电机轴承润滑油位低故障","故障 "]
["HZ15 ",5004,"发电机冷却水入口温度高警告","告警信息 "]
["HZ15 ",5005,"发电机冷却水入口温度低警告","告警信息 "]
["HZ15 ",5006,"发电机冷却水入口温度过高故障","故障 "]
["HZ15 ",5007,"发电机冷却水入口温度过低故障","故障 "]
["HZ15 ",5008,"发电机冷却水出口温度高警告","告警信息 "]
["HZ15 ",5009,"发电机冷却水出口温度低警告","告警信息 "]
["HZ15 ",5010,"发电机冷却水出口温度过高故障","故障 "]
["HZ15 ",5011,"发电机冷却液出口温度低故障","故障 "]
["HZ15 ",5012,"发电机冷却液压力低故障","故障 "]
["HZ15 ",5013,"发电机冷却水泵过载故障","故障 "]
["HZ15 ",5014,"发电机空冷温度高警告","告警信息 "]
["HZ15 ",5015,"发电机冷却空气温度过高故障","故障 "]
["HZ15 ",5016,"发电机冷却风扇1过载故障","故障 "]
["HZ15 ",5017,"发电机冷却风扇2过载故障","故障 "]
["HZ15 ",5018,"发电机DE轴承超温故障","故障 "]
["HZ15 ",5019,"发电机DE端轴承温度警告","告警信息 "]
["HZ15 ",5021,"发电机加热过载故障","故障 "]
["HZ15 ",5023,"发电机系统电动机加热过载故障","故障 "]
["HZ15 ",5024,"发电机NDE轴承超温故障","故障 "]
["HZ15 ",5025,"发电机NDE端轴承温度警告","告警信息 "]
["HZ15 ",5026,"发电机过压保护激活故障","故障 "]
["HZ15 ",5027,"发电机滑环故障","故障 "]
["HZ15 ",5028,"发电机滑环冷却风扇过载故障","故障 "]
["HZ15 ",5029,"发电机滑环超温故障","故障 "]
["HZ15 ",5030,"发电机滑环温度警告","告警信息 "]
["HZ15 ",5031,"发电机绕组U1超温故障","故障 "]
["HZ15 ",5032,"发电机绕组U1温度警告","告警信息 "]
["HZ15 ",5033,"发电机绕组U2超温故障","故障 "]
["HZ15 ",5034,"发电机绕组U2温度警告","告警信息 "]
["HZ15 ",5035,"发电机绕组V1超温故障","故障 "]
["HZ15 ",5036,"发电机绕组V1温度警告","告警信息 "]
["HZ15 ",5037,"发电机绕组V2超温故障","故障 "]
["HZ15 ",5038,"发电机绕组V2温度警告","告警信息 "]
["HZ15 ",5039,"发电机绕组W1超温故障","故障 "]
["HZ15 ",5040,"发电机绕组W1温度警告","告警信息 "]
["HZ15 ",5041,"发电机绕组W2超温故障","故障 "]
["HZ15 ",5042,"发电机绕组W2温度警告","告警信息 "]
["HZ15 ",5051,"发电机配置无效故障","故障 "]
["HZ15 ",6000,"UPS电池容量低故障","故障 "]
["HZ15 ",6001,"UPS旁路故障","故障 "]
["HZ15 ",6002,"UPS供电警告","告警信息 "]
["HZ15 ",6003,"UPS关断故障","故障 "]
["HZ15 ",6004,"UPS系统配置无效故障","故障 "]
["HZ15 ",8000,"中压断路器分闸故障","故障 "]
["HZ15 ",8002,"箱变超温故障","故障 "]
["HZ15 ",8003,"箱变温度高警告","告警信息 "]
["HZ15 ",8004,"箱变压力开关故障","故障 "]
["HZ15 ",8005,"箱变高压测断路器故障","故障 "]
["HZ15 ",8006,"箱变温度警告","告警信息 "]
["HZ15 ",10000,"远程手动停机","提示信息 "]
["HZ15 ",10001,"本地手动停机","提示信息 "]
["HZ15 ",11001,"变频器定子接触器故障","故障 "]
["HZ15 ",11002,"变频器转子接触器失效故障","故障 "]
["HZ15 ",11003,"变频器未准备好有加热要求警告","告警信息 "]
["HZ15 ",11004,"变频器柜加热过载故障","故障 "]
["HZ15 ",11005,"变频器有功功率超限故障","故障 "]
["HZ15 ",11006,"变频器配置无效故障","故障 "]
["HZ15 ",11007,"变频器电流限制警告","告警信息 "]
["HZ15 ",11008,"变频器柜通风过载故障","故障 "]
["HZ15 ",11009,"变频器Crowbar激活信息","提示信息 "]
["HZ15 ",11010,"变频器转子熔断器失效故障","故障 "]
["HZ15 ",11011,"发电机机械转速过高故障","故障 "]
["HZ15 ",11012,"LVRT激活故障","故障 "]
["HZ15 ",11013,"变频器控制过程故障（网侧/机侧启动/停止）","故障 "]
["HZ15 ",11014,"变频器Heartbeat信号失效故障","故障 "]
["HZ15 ",11015,"变频器警告","告警信息 "]
["HZ15 ",11016,"变频器非严重故障","故障 "]
["HZ15 ",11017,"变频器严重故障","故障 "]
["HZ15 ",11018,"变频器紧急停机故障","故障 "]
["HZ15 ",11020,"变频器IGBT散热器超温故障","故障 "]
["HZ15 ",11021,"变频器散热器温度警告","告警信息 "]
["HZ15 ",11022,"变频器通讯故障","故障 "]
["HZ15 ",11023,"变频器直流母线欠压故障","故障 "]
["HZ15 ",11024,"变频器直流母线过压故障","故障 "]
["HZ15 ",11025,"变频器发电机侧A类故障-外部停机命令","故障 "]
["HZ15 ",11026,"变频器发电机侧A类故障-24V短路","故障 "]
["HZ15 ",11027,"变频器发电机侧A类故障-编码器故障","故障 "]
["HZ15 ",11028,"变频器发电机侧A类故障-Crowbar激活时间过长","故障 "]
["HZ15 ",11029,"变频器发电机侧A类故障-bit4（备用）","提示信息 "]
["HZ15 ",11030,"变频器发电机侧A类故障-Crowbar误触发","故障 "]
["HZ15 ",11031,"变频器发电机侧A类故障-栅极驱动回路故障","故障 "]
["HZ15 ",11032,"变频器发电机侧A类故障-转子过流","故障 "]
["HZ15 ",11033,"变频器发电机侧A类故障-转子短路","故障 "]
["HZ15 ",11034,"变频器发电机侧A类故障-IGBTUce故障","故障 "]
["HZ15 ",11035,"变频器发电机侧A类故障-停机定子电流下降过慢","故障 "]
["HZ15 ",11036,"变频器发电机侧A类故障-接地故障","故障 "]
["HZ15 ",11037,"变频器发电机侧A类故障-直流母线过压","故障 "]
["HZ15 ",11038,"变频器发电机侧A类故障-网侧反馈故障","故障 "]
["HZ15 ",11039,"变频器发电机侧A类故障-主断路器故障","故障 "]
["HZ15 ",11040,"变频器发电机侧A类故障-转子多次过流","故障 "]
["HZ15 ",11041,"变频器发电机侧B类故障-温度传感器（NTC）故障","故障 "]
["HZ15 ",11042,"变频器发电机侧B类故障-散热器超温","故障 "]
["HZ15 ",11043,"变频器发电机侧B类故障-bit2（备用）","提示信息 "]
["HZ15 ",11044,"变频器发电机侧B类故障-bit3（备用）","提示信息 "]
["HZ15 ",11045,"变频器发电机侧B类故障-bit4（备用）","提示信息 "]
["HZ15 ",11046,"变频器发电机侧B类故障-速度超出运行范围","故障 "]
["HZ15 ",11047,"变频器发电机侧B类故障-网侧变流器启停故障","故障 "]
["HZ15 ",11048,"变频器发电机侧B类故障-外部CAN总线故障","故障 "]
["HZ15 ",11049,"变频器发电机侧B类故障-bit8（备用）","提示信息 "]
["HZ15 ",11050,"变频器发电机侧B类故障-同步故障","故障 "]
["HZ15 ",11051,"变频器发电机侧B类故障-断路器跳闸","故障 "]
["HZ15 ",11052,"变频器发电机侧B类故障-散热器温度过低","故障 "]
["HZ15 ",11053,"变频器发电机侧B类故障-CAN通讯故障","故障 "]
["HZ15 ",11054,"变频器发电机侧B类故障-电网故障","故障 "]
["HZ15 ",11055,"变频器发电机侧B类故障-bit14（备用）","提示信息 "]
["HZ15 ",11056,"变频器发电机侧B类故障-bit15（备用）","提示信息 "]
["HZ15 ",11057,"变频器网侧A类故障-外部故障","故障 "]
["HZ15 ",11058,"变频器网侧A类故障-24V短路","故障 "]
["HZ15 ",11059,"变频器网侧A类故障-bit2（备用）","提示信息 "]
["HZ15 ",11060,"变频器网侧A类故障-bit3（备用）","提示信息 "]
["HZ15 ",11061,"变频器网侧A类故障-放电故障","故障 "]
["HZ15 ",11062,"变频器网侧A类故障-直流母线过压","故障 "]
["HZ15 ",11063,"变频器网侧A类故障-栅极驱动回路故障","故障 "]
["HZ15 ",11064,"变频器网侧A类故障-IGBTUce开关故障","故障 "]
["HZ15 ",11065,"变频器网侧A类故障-短路","故障 "]
["HZ15 ",11066,"变频器网侧A类故障-IGBTUce故障","故障 "]
["HZ15 ",11067,"变频器网侧A类故障-网侧接触器故障","故障 "]
["HZ15 ",11068,"变频器网侧A类故障-Chopper开/关故障","故障 "]
["HZ15 ",11069,"变频器网侧A类故障-bit12（备用）","提示信息 "]
["HZ15 ",11070,"变频器网侧A类故障-bit13（备用）","提示信息 "]
["HZ15 ",11071,"变频器网侧A类故障-bit14（备用）","提示信息 "]
["HZ15 ",11072,"变频器网侧A类故障-bit15（备用）","提示信息 "]
["HZ15 ",11073,"变频器网侧B类故障-温度传感器（NTC）故障","故障 "]
["HZ15 ",11075,"变频器网侧B类故障-电网频率故障","故障 "]
["HZ15 ",11076,"变频器网侧B类故障-直流电压欠压","故障 "]
["HZ15 ",11077,"变频器网侧B类故障-CAN通讯故障","故障 "]
["HZ15 ",11078,"变频器网侧B类故障-网侧滤波器故障","故障 "]
["HZ15 ",11079,"变频器网侧B类故障-bit5（备用）","提示信息 "]
["HZ15 ",11080,"变频器网侧B类故障-散热器超温故障","故障 "]
["HZ15 ",11081,"变频器网侧B类故障-bit7（备用）","提示信息 "]
["HZ15 ",11082,"变频器网侧B类故障-bit8（备用）","提示信息 "]
["HZ15 ",11083,"变频器网侧B类故障-过流","故障 "]
["HZ15 ",11084,"变频器网侧B类故障-接地故障","故障 "]
["HZ15 ",11085,"变频器网侧B类故障-bit11（备用）","提示信息 "]
["HZ15 ",11086,"变频器网侧B类故障-充电故障","故障 "]
["HZ15 ",11087,"变频器网侧B类故障-bit13（备用）","提示信息 "]
["HZ15 ",11088,"变频器网侧B类故障-电网故障","故障 "]
["HZ15 ",11089,"变频器网侧B类故障-bit15（备用）","提示信息 "]
["HZ15 ",11090,"变频器LVRT错误警告","告警信息 "]
["HZ15 ",11092,"变频器通信重新初始化警告","告警信息 "]
["HZ15 ",11094,"变频器转矩追踪故障","故障 "]
["HZ15 ",11095,"变频器转矩追踪警告","告警信息 "]
["HZ15 ",11098,"变频器LVRT激活警告","告警信息 "]
["HZ15 ",11099,"变频器电网频率无效配置故障","故障 "]
["HZ15 ",11108,"变频器机侧A类故障2-定子接触器闭合故障","故障 "]
["HZ15 ",12000,"液压油超温高故障（油温开关）","故障 "]
["HZ15 ",12004,"液压油位低故障","故障 "]
["HZ15 ",12005,"液压电机过载故障","故障 "]
["HZ15 ",12009,"液压泵运行时间超限故障","故障 "]
["HZ15 ",12012,"液压系统高压力过低故障","故障 "]
["HZ15 ",12013,"液压系统低压力过低故障","故障 "]
["HZ15 ",12014,"液压系统油压过高故障","故障 "]
["HZ15 ",12016,"液压系统液压油加热过载故障","故障 "]
["HZ15 ",13000,"紧急停机按钮激活故障","提示信息 "]
["HZ15 ",13001,"安全控制器激活故障","故障 "]
["HZ15 ",13002,"G-传感器1振动开关超限故障","故障 "]
["HZ15 ",13004,"安全控制器故障","故障 "]
["HZ15 ",13005,"机舱瞬时振动值超限故障","故障 "]
["HZ15 ",13006,"转子超速故障","故障 "]
["HZ15 ",13007,"发电机超速故障","故障 "]
["HZ15 ",13008,"转子极端超速故障","故障 "]
["HZ15 ",13009,"发电机极端超速故障","故障 "]
["HZ15 ",13010,"速度传感器故障","故障 "]
["HZ15 ",13011,"安全控制检测速度传感器警告","告警信息 "]
["HZ15 ",13012,"安全链故障","故障 "]
["HZ15 ",13013,"安全控制器无效版本故障","故障 "]
["HZ15 ",13015,"转子反向超速警告","告警信息 "]
["HZ15 ",13016,"发电机反向超速警告","告警信息 "]
["HZ15 ",13017,"机舱振动10分钟平均值超限故障","故障 "]
["HZ15 ",13018,"安全控制器无效厂家","故障 "]
["HZ15 ",13020,"安全控制器版本验证正在进行信息","提示信息 "]
["HZ15 ",13021,"安全控制器版本读出故障","故障 "]
["HZ15 ",13022,"没有转子速度被选择故障","故障 "]
["HZ15 ",13023,"无效的紧急电路被选择故障","故障 "]
["HZ15 ",13024,"没有转子反转速度被选择故障","故障 "]
["HZ15 ",13025,"安全控制器版本信息验证完成信息","提示信息 "]
["HZ15 ",14001,"转子刹车液压力低故障","故障 "]
["HZ15 ",14002,"转子刹车盘预磨损警告","告警信息 "]
["HZ15 ",14003,"转子刹车盘磨损故障","故障 "]
["HZ15 ",14004,"转子刹车超时故障","故障 "]
["HZ15 ",14006,"转子刹车压力开关反馈故障","故障 "]
["HZ15 ",15002,"A10控制柜左侧温度低警告","告警信息 "]
["HZ15 ",15003,"A10控制柜左侧温度高警告","告警信息 "]
["HZ15 ",15004,"A10控制柜右侧温度低警告","告警信息 "]
["HZ15 ",15005,"A10控制柜右侧温度高警告","告警信息 "]
["HZ15 ",15006,"A11控制柜温度低警告","告警信息 "]
["HZ15 ",15007,"A11控制柜温度高警告","告警信息 "]
["HZ15 ",15008,"A20控制柜温度1低警告","告警信息 "]
["HZ15 ",15009,"A20控制柜温度1高警告","告警信息 "]
["HZ15 ",15010,"A20控制柜温度2低警告","告警信息 "]
["HZ15 ",15011,"A20控制柜温度2高警告","告警信息 "]
["HZ15 ",15012,"A30控制柜温度低警告","告警信息 "]
["HZ15 ",15013,"A30控制柜温度高警告","告警信息 "]
["HZ15 ",15020,"A10左柜温度低故障","故障 "]
["HZ15 ",15021,"A10左柜超温故障","故障 "]
["HZ15 ",15022,"A10右柜温度低故障","故障 "]
["HZ15 ",15023,"A10右柜超温故障","故障 "]
["HZ15 ",15024,"A11控制柜温度过低故障","故障 "]
["HZ15 ",15025,"A11柜超温故障","故障 "]
["HZ15 ",15026,"A20温度1温度低故障","故障 "]
["HZ15 ",15027,"A20柜温度1超温故障","故障 "]
["HZ15 ",15028,"A20温度2温度低故障","故障 "]
["HZ15 ",15029,"A20柜温度2超温故障","故障 "]
["HZ15 ",15030,"A30柜温度低故障","故障 "]
["HZ15 ",15031,"A30柜超温故障","故障 "]
["HZ15 ",15036,"A10烟雾检测动作","故障 "]
["HZ15 ",15037,"A11烟雾检测动作","故障 "]
["HZ15 ",15038,"A20烟雾检测动作","故障 "]
["HZ15 ",15039,"A30烟雾检测动作","故障 "]
["HZ15 ",15051,"电网模块CAN通讯故障","故障 "]
["HZ15 ",15052,"G-传感器1CAN通讯故障","故障 "]
["HZ15 ",15054,"I/O硬件故障","故障 "]
["HZ15 ",16001,"风机停机维护","提示信息 "]
["HZ15 ",16003,"转子维护超速故障","故障 "]
["HZ15 ",16004,"维护用户等级低","故障 "]
["HZ15 ",16005,"因风速过高维护不允许","故障 "]
["HZ15 ",16006,"变桨系统维护激活","提示信息 "]
["HZ15 ",16007,"服务停止顺序不成功故障","故障 "]
["HZ15 ",17000,"气象站配置无效故障","故障 "]
["HZ15 ",17002,"环境温度高故障","提示信息 "]
["HZ15 ",17003,"环境温度低故障","提示信息 "]
["HZ15 ",17004,"风速1s平均值超限","提示信息 "]
["HZ15 ",17005,"风速30s平均值超限","提示信息 "]
["HZ15 ",17006,"风速600s平均值超限","提示信息 "]
["HZ15 ",17008,"本地选择的气象站1故障","故障 "]
["HZ15 ",17009,"本地选择的气象站2故障","故障 "]
["HZ15 ",17010,"气象站1警告","告警信息 "]
["HZ15 ",17011,"气象站2警告","告警信息 "]
["HZ15 ",17012,"气象站1手动选择警告","告警信息 "]
["HZ15 ",17013,"气象站2手动选择警告","告警信息 "]
["HZ15 ",17014,"远程选择的气象站1故障","故障 "]
["HZ15 ",17015,"远程选择的气象站2故障","故障 "]
["HZ15 ",18000,"辅助供电断路器断开故障","故障 "]
["HZ15 ",18001,"辅助供电断路器故障","故障 "]
["HZ15 ",18002,"电网U相辅助电压过高故障","故障 "]
["HZ15 ",18003,"电网V相辅助电压过高故障","故障 "]
["HZ15 ",18004,"电网W相辅助电压过高故障","故障 "]
["HZ15 ",18005,"MCB储能完成警告","告警信息 "]
["HZ15 ",18006,"低压侧主断路器断开警告","告警信息 "]
["HZ15 ",18007,"变频器主断路器触发故障","故障 "]
["HZ15 ",18008,"低压断路器失效故障","故障 "]
["HZ15 ",18009,"低压主断路器切出故障","故障 "]
["HZ15 ",18010,"低压主断路器周期测试故障","故障 "]
["HZ15 ",19000,"转子刹车投入测试故障","故障 "]
["HZ15 ",19001,"变桨系统测试故障","故障 "]
["HZ15 ",19002,"转子刹车释放测试故障","故障 "]
["HZ15 ",19003,"机组启动故障","故障 "]
["HZ15 ",19004,"发电机切入","告警信息 "]
["HZ15 ",19005,"发电机切出","告警信息 "]
["HZ15 ",19006,"机组停机自检","提示信息 "]
["HZ15 ",19007,"停机顺序不成功故障","故障 "]
["HZ15 ",19008,"停机空转刹车未投入故障","故障 "]
["HZ15 ",19009,"停止闲置刹车未释放","故障 "]
["HZ15 ",19010,"风向失调警告","告警信息 "]
["HZ15 ",19011,"发电机机械转速低警告","告警信息 "]
["HZ15 ",19012,"安全链测试失败故障","故障 "]
["HZ15 ",20000,"机舱温度低警告","告警信息 "]
["HZ15 ",20001,"机舱温度高警告","告警信息 "]
["HZ15 ",20002,"机舱温度低故障","故障 "]
["HZ15 ",20003,"机舱超温故障","故障 "]
["HZ15 ",20004,"机舱前端温度低警告","告警信息 "]
["HZ15 ",20005,"机舱前端温度高警告","告警信息 "]
["HZ15 ",20006,"机舱前端温度低故障","故障 "]
["HZ15 ",20007,"机舱前端超温故障","故障 "]
["HZ15 ",20008,"机舱冷却风扇1过载故障","故障 "]
["HZ15 ",20009,"机舱冷却风扇2过载故障","故障 "]
["HZ15 ",20010,"机舱温度过高警告","告警信息 "]
["HZ15 ",20011,"机舱前端温度过高警告","告警信息 "]
["HZ15 ",21000,"电网监视U相电压过低故障","故障 "]
["HZ15 ",21001,"电网U相电压过高故障","故障 "]
["HZ15 ",21002,"电网监视V相电压过低故障","故障 "]
["HZ15 ",21003,"电网V相电压过高故障","故障 "]
["HZ15 ",21004,"电网监视W相电压过低故障","故障 "]
["HZ15 ",21005,"电网W相电压过高故障","故障 "]
["HZ15 ",21006,"电网监视u相过流故障","故障 "]
["HZ15 ",21007,"电网监视v相过流故障","故障 "]
["HZ15 ",21008,"电网监视w相过流故障","故障 "]
["HZ15 ",21009,"电网监视频率过低故障","故障 "]
["HZ15 ",21010,"电网监视频率过高故障","故障 "]
["HZ15 ",21011,"电网监视电压不平衡故障","故障 "]
["HZ15 ",21012,"电网检测电流相序差太高警告","告警信息 "]
["HZ15 ",21013,"电网相序错误","故障 "]
["HZ15 ",21014,"电网检测额定电流差太高警告","告警信息 "]
["HZ15 ",21015,"电网故障告知SCADA（电压、频率故障）","故障 "]
["HZ15 ",21016,"电网U相电压严重过高故障","故障 "]
["HZ15 ",21017,"电网V相辅助电压严重过高故障","故障 "]
["HZ15 ",21018,"电网W相辅助电压严重过高故障","故障 "]
["HZ15 ",21019,"电网检测谐波高警告","告警信息 "]
["HZ15 ",24000,"功率/速度控制SVI通讯连接故障","故障 "]
["HZ15 ",24001,"功率/速度控制SVI通讯地址故障","故障 "]
["HZ15 ",24002,"功率/速度控制SVI通讯故障","故障 "]
["HZ15 ",24003,"停机为变桨系统轴承润滑","故障 "]
["HZ15 ",24004,"功率/速度控制扭矩参考波动超限","故障 "]
["HZ15 ",24005,"功率速度控制器滤波器参数设置无效警告","告警信息 "]
["HZ15 ",24006,"功率/速度控制无用参数配置","故障 "]
["HZ15 ",24007,"发电机功率曲线低于下限故障","故障 "]
["HZ15 ",24008,"发电机功率曲线超过上限警告","告警信息 "]
["HZ15 ",24009,"发电机功率波动过大故障","故障 "]
["HZ15 ",24010,"发电机功率输出超极限故障","故障 "]
["HZ15 ",24011,"发电机速度波动过大故障","故障 "]
["HZ15 ",28000,"塔基温度低警告","告警信息 "]
["HZ15 ",28001,"塔基温度高警告","告警信息 "]
["HZ15 ",28002,"塔基温度过低故障","故障 "]
["HZ15 ",28003,"塔基温度过高故障","故障 "]
["HZ15 ",30000,"期间执行器停止运行警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",-5,"通讯恢复","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",-4,"通讯中断","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",-3,"风机通讯恢复","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",-2,"风机通讯中断","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",101001,"占位SC","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105001,"1号桨出现角度传感器故障警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105002,"安全位置信号触发时桨叶角度不在合理范围内","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105003,"变桨系统状态反馈错误","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105004,"1号桨叶从91度限位脱开失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105005,"2号桨叶从91度限位脱开失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105006,"3号桨叶从91度限位脱开失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105009,"1号桨的95度限位开关被撞开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105010,"1号桨电池电压过高或过低","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105011,"1号桨的91度限位开关被撞开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105012,"1号桨的变桨电机温度过高","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105013,"1号电池柜航空插头没有插好","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105014,"1号桨PM直流母线电压低","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105015,"变桨处于空转模式","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105016,"1号桨没有跟随位置设定值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105017,"1号桨的出现警报","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105018,"1号桨故障，触发电池驱动回桨警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105019,"某一桨叶电容电压过高","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105020,"某一桨叶电容电压过低警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105021,"2号桨出现角度传感器故障警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105022,"某一桨叶电容中间点电压警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105023,"某一桨叶电容箱温度过高","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105024,"某一个SSI传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105025,"华电变桨没有收到来自主控的EFC信号","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105026,"某一SSI编码器状态故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105027,"桨叶1Teached操作未完成","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105028,"某一个桨叶驱动器内部温度过高","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105029,"2号桨的95度限位开关被撞开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105030,"2号桨电池电压过高或过低","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105031,"2号桨的91度限位开关被撞开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105032,"2号桨的变桨电机温度过高","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105033,"2号电池柜航空插头没有插好","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105034,"2号桨PM直流母线电压低","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105035,"变桨系统某一桨叶处于强制手动模式","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105036,"2号桨没有跟随位置设定值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105037,"2号桨的出现警报","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105038,"2号桨故障，触发电池驱动回桨警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105039,"某一变桨电容充电器异常警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105040,"变桨系统轴控柜温度过低","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105041,"3号桨出现角度传感器故障警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105043,"某一桨叶电机电流过大","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105044,"某一桨叶变桨超速警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105045,"某一变桨电机堵转","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105046,"某一变桨电机堵转且超温","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105047,"某一桨叶桨矩角过小","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105048,"某一桨叶桨矩角过大","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105049,"3号桨的95度限位开关被撞开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105050,"3号桨电池电压过高或过低","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105051,"3号桨的91度限位开关被撞开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105052,"3号桨的变桨电机温度过高","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105053,"3号电池柜航空插头没有插好","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105054,"3号桨PM直流母线电压低","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105055,"某一个变桨伺服驱动器处于故障状态","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105056,"3号桨没有跟随位置设定值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105057,"3号桨的出现警报","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105058,"3号桨故障，触发电池驱动回桨警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105059,"某一桨叶3度位置传感器故障警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105060,"某一桨叶90度位置传感器故障警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105061,"变桨系统24V电源故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105062,"变桨系统电池充电回路故障警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105063,"1号，2号和3号桨都撞开91度限位开关","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105064,"变桨系统处在紧急模式","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105065,"桨叶2Teached操作未完成","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105066,"桨叶3Teached操作未完成","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105069,"变桨系统发生2级故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105071,"变桨系统轴控柜温度过高告警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105072,"两桨叶间的角度差大于设定值(相差1度持续10秒)","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105073,"MOOG变桨两桨叶间角度差相差2度警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105074,"两桨叶间的角度差大于设定值(相差1度持续10秒)故障多次出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105075,"MOOG变桨两桨叶间角度差相差2度重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105076,"变桨系统出现警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105077,"变桨系统400V电网存在故障警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105100,"1号，2号或3号桨报告预充电电阻过温","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105103,"变桨系统轴控柜温度过高","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105104,"变桨系统与PM的CAN通讯故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105107,"变桨系统处于维护模式","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105108,"变桨轴控柜温度信号异常","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105109,"变桨系统暖机模式","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105110,"变桨系统暖机超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105111,"1号桨的95度限位开关被撞开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105112,"2号桨的95度限位开关被撞开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105113,"3号桨的95度限位开关被撞开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105114,"1号桨的变桨电机温度过高","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105115,"2号桨的变桨电机温度过高","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105116,"3号桨的变桨电机温度过高","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105117,"天仁变桨系统处在紧急模式","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105118,"变桨系统400V电网存在故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105119,"天仁变桨系统轴控柜温度过高","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105120,"主控制器与天仁变桨系统Profibus通讯中断警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105121,"变桨系统与驱动器CAN通讯故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105122,"1号桨没有跟随位置设定值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105123,"2号桨没有跟随位置设定值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105124,"3号桨没有跟随位置设定值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105125,"天仁变桨两桨叶间角度差相差2度警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105126,"变桨系统处于维护模式","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105127,"桨叶1抱闸继电器4K1故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105128,"1，2或3号桨电池回桨电压降达到报警值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105129,"1,2或3号桨电池回桨电压降达到故障值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105130,"风机处于桨叶自检模式","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105131,"变速率回桨15s桨叶未到安全位置","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105132,"变桨超级电容充电超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105134,"变桨上电初始化失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105135,"变桨400V供电建立超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105150,"与MOOG变桨系统Profibus通讯亚健康","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105151,"与MOOG变桨系统Profibus通讯亚健康重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105152,"主控制器与MOOG变桨系统Profibus通讯自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105153,"1号桨出现角度传感器故障自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105154,"1号桨出现角度传感器故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105155,"2号桨出现角度传感器故障自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105156,"2号桨出现角度传感器故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105157,"3号桨出现角度传感器故障自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105158,"3号桨出现角度传感器故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105159,"变桨系统电池充电回路故障自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105160,"变桨系统电池充电回路故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105161,"1或2或3号桨6F6空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105162,"变桨系统400V电网故障自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105163,"变桨系统400V电网故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105164,"1号桨故障，触发电池驱动回桨自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105165,"1号桨故障，触发电池驱动回桨重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105166,"2号桨故障，触发电池驱动回桨自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105167,"2号桨故障，触发电池驱动回桨重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105168,"3号桨故障，触发电池驱动回桨自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105169,"3号桨故障，触发电池驱动回桨重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105170,"与天仁变桨系统Profibus通讯亚健康","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105171,"与天仁变桨系统Profibus通讯亚健康重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105172,"主控制器与天仁变桨系统Profibus通讯自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105173,"主控制器与天仁变桨系统Profibus通讯故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105174,"天仁变桨安全位置信号没有反馈","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105175,"某一桨叶变桨超速自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105176,"某一桨叶变桨超速重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105177,"某一桨叶电容中间点电压自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105178,"某一桨叶电容中间点电压警告重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105179,"某一变桨电容充电器异常自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105180,"某一变桨电容充电器异常重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105181,"某一桨叶电容电压过低自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105182,"某一桨叶电容电压过低重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105183,"天仁变桨系统EFC信号被强制","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105184,"主控没有收到来自天仁变桨的EFC反馈信号","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105185,"天仁变桨两桨叶间角度差相差2度自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105186,"天仁变桨两桨叶间角度差相差2度重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105201,"MOOG变桨没有收到来自主控的EFC信号","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105202,"MOOG变桨系统EFC信号被强制","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105203,"主控没有收到来自MOOG变桨的EFC反馈信号","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105204,"主控没有收到变桨EFC反馈信号自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105205,"主控没有收到变桨EFC反馈信号重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105206,"某一桨叶3度位置传感器故障自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105207,"某一桨叶3度位置传感器故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105208,"某一桨叶90度位置传感器故障自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105209,"某一桨叶90度位置传感器故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105221,"MOOG变桨两桨叶间角度差相差2度自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105230,"桨叶1变桨齿轮箱变比参数设置错误","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105231,"桨叶2变桨齿轮箱变比参数设置错误","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105232,"桨叶3变桨齿轮箱变比参数设置错误","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105233,"桨叶1备用抱闸继电器已动作,检查更换4K1","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105234,"请及时更换桨叶1抱闸继电器4K1","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105235,"桨叶2备用抱闸继电器已动作,注意检查更换","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105236,"请及时更换桨叶2抱闸继电器","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105237,"桨叶3备用抱闸继电器已动作,注意检查更换","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105238,"请及时更换桨叶3抱闸继电器","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105239,"桨叶1变速率回桨过程中电容电压过低","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105240,"桨叶2变速率回桨过程中电容电压过低","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105241,"桨叶3变速率回桨过程中电容电压过低","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105242,"桨叶1备用抱闸继电器动作过于频繁，需更换4k1","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105243,"桨叶2备用抱闸继电器动作过于频繁，需更换4k1","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105244,"桨叶3备用抱闸继电器动作过于频繁，需更换4k1","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105245,"桨叶2抱闸继电器4K1故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105246,"桨叶3抱闸继电器4K1故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105247,"在单次打泵过程中检测到变桨自润滑泵堵塞","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105248,"变桨自润滑泵堵塞报警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105249,"变桨自润滑泵油位低","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105250,"变桨自润滑泵油位低报警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105251,"变桨自润滑系统1个月时间内未打脂","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105252,"变桨自润滑泵电机启动","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105253,"变桨自润滑电机手动控制使能","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105254,"变桨自润滑电机强制控制使能","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105255,"变桨自润滑泵电机保护空开跳开","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105256,"变桨自润滑系统柱塞误动作","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",105257,"变桨自润滑系统柱塞误动作警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",106001,"主控制器没有收到来自变桨系统的EFC确认信号警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",201001,"机舱柜柜门急停按钮被拍下触发了紧急停机","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",201003,"PCH的振动过大继电器断开导致安全链断开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",201004,"过速继电器断开导致安全链断开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",201005,"无湍流或未在偏航状态时PCH的SSD开关断开导致安全链断开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",201006,"无湍流或未在偏航状态时PCH测得的SSD震动值高于设定值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",201007,"机舱人员安全链或机器安全链没有反馈信号","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",201009,"变桨系统的400V主接触器未闭合","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",201010,"刹车等级小于100时PCH振动过大导致安全链断开自恢复","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",201011,"未发电时PCH振动过大导致安全链断开","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",201101,"机舱柜安全链复位按钮被按下对安全链进行复位","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202001,"机舱柜恒温器测得温度超出范围","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202003,"机舱柜24V 电池更换警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202004,"塔底温控回路空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202005,"机舱温控回路空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202006,"机舱柜24V UPS处于电池模式","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202007,"偏航电机加热器保护空开跳开","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202008,"控制柜防雷器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202011,"机舱柜温度高于最大上限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202012,"机舱柜温度低于最小下限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202015,"机舱人工安全链或机舱机器安全链的24V电源开路","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202016,"塔底风扇供电保护跳开","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202017,"发电机滑环室风扇供电保护跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202018,"机舱柜中变桨系统400V电源保护空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202020,"机舱柜690V电源熔断器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202021,"机舱柜400V电源熔断器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202023,"机舱柜中偏航电机保护空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202026,"机舱柜中电气滑环加热器保护空开跳开","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202027,"机舱柜中齿轮箱的油泵电机保护空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202029,"机舱柜中齿轮箱冷却风扇保护空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202031,"机舱柜中齿轮箱油池加热器保护空开跳开","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202033,"机舱柜加热器或风扇230V保护空开跳开","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202036,"机舱柜中发电机冷却风扇保护空开跳开","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202037,"发电机散热器异常","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202038,"机舱柜中发电机空间加热器保护空开跳开","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202039,"机舱柜中开关电源保护空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202040,"机舱柜中航空障碍灯230V保护空开跳开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202041,"机舱柜中液压站的液压泵保护空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202042,"机舱柜中齿轮箱冷却风扇电机加热器或齿轮箱油泵电机加热器保护空开跳开","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202043,"机舱柜中齿轮箱油管加热器保护开关跳开","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202046,"偏航系统1号电机热保护继电器触发","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202047,"偏航系统2号电机热保护继电器触发","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202048,"偏航系统3号电机热保护继电器触发","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202049,"偏航系统4号电机热保护继电器触发","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202050,"偏航系统5号电机热保护继电器触发","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202052,"测量机舱柜温度的PT100传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202053,"测量机舱温度的PT100传感器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202054,"测量齿轮箱油池油温的PT100传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202055,"测量齿轮箱入口油温的PT100传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202058,"测量驱动端轴承温度的PT100传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202059,"测量非驱动端轴承温度的PT100传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202060,"主轴轴承座温度传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202061,"测量齿轮箱驱动端的中间轴温度的PT100传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202062,"测量齿轮箱非驱动端的中间轴温度的PT100传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202064,"齿轮箱过滤器入口压力传感器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202065,"齿轮箱入口压力传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202067,"测量发电机定子U相绕组温度的PT100传感器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202069,"测量发电机定子V相绕组温度的PT100传感器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202071,"测量发电机定子W相绕组温度的PT100传感器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202073,"测量发电机驱动端轴承温度的PT100传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202074,"测量发电机非驱动端轴承温度的PT100传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202075,"发电机单相定子PT100传感器故障超过限定时间未检修","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202076,"至少两相发电机定子PT100传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202077,"测量舱外环境温度的PT100传感器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202078,"机舱柜中偏航电机抱闸的保护空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202088,"偏航系统位置传感器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202089,"机械式风向标故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202090,"测量液压站蓄压罐压力的压力传感器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202091,"机械式风速仪故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202100,"机械刹车1号阀设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202101,"发电机冷却风扇设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202103,"发电机空间加热器设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202104,"齿轮箱油泵加热器设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202105,"齿轮箱冷却风扇低速设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202106,"齿轮箱油泵低速设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202107,"齿轮箱油泵高速设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202108,"齿轮箱油池加热器设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202109,"液压站的液压泵设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202110,"偏航系统电机加热器设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202111,"风速仪和风向标的加热器设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202112,"齿轮箱冷却风扇高速设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202113,"齿轮箱冷却风扇加热器设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202114,"偏航系统设定顺时针偏航","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202115,"偏航系统设定逆时针偏航","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202116,"偏航系统电机抱闸设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202117,"机械刹车2号阀设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202118,"机械刹车3号阀设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202119,"机械刹车4号阀设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202120,"机舱柜加热器设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202125,"变桨系统96度限位开关的旁路信号设定发出","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202128,"机舱柜中发电机水冷系统保护空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202129,"机舱柜中24V UPS处于充电模式","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202130,"齿轮箱精滤器设定运行","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202132,"齿轮箱精滤器热继跳开","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202133,"发电机滑环室测温PT100传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202135,"24V机械安全负载供电空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202136,"24V人工安全负载供电空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202137,"机舱控制柜风扇打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202138,"恒温器湿度报警","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202139,"24V柜外IO供电空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202140,"24V柜内IO供电空开跳开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202141,"机舱PT100和舱外PT100失效","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202142,"机舱柜恒温器测得温度超出范围警报","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202151,"主轴承润滑系统油位过低","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202152,"主轴承润滑MCB跳开","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202153,"主轴承润滑系统启动","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202154,"主轴承润滑系统未运行时间过长","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202155,"主轴润滑泵开启手动模式","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202156,"主轴承润滑系统泵柱塞误启动","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202157,"主轴承润滑系统泵柱塞误启动警告","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202158,"主轴承润滑系统电机阻塞警告","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202159,"主轴承润滑系统电机阻塞重复出现","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",202160,"主轴润滑泵开启强制模式","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",203001,"机舱温度高于过高设定值","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",203002,"机舱温度低于过低设定值","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",203003,"机舱温度高于最大上限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",203004,"机舱温度低于最小下限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",203005,"机舱温度高于过高设定值或机舱温度低于过低设定值故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",203006,"机舱温度低于最小下限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204002,"风机低速端转速高于2级超速门限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204004,"发电机转速高于2级超速门限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204006,"低速端转速与变频器测得发电机转速不匹配","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204007,"低速端旋转方向错误","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204008,"低速端转速与主控测得发电机转速不匹配","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204009,"低速端1号传感器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204010,"低速端2号传感器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204012,"过速继电器和低速端转速不匹配","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204014,"风轮锁被锁定","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204016,"无湍流时风轮转速高于3级超速门限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204017,"无湍流时发电机转速高于3级超速门限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204018,"塔架水平合方向的加速度高于1级振动门限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204019,"塔架水平合方向的加速度高于2级振动门限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204020,"塔架水平方向越1级振动门限值重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204021,"塔架前后方向的加速度高于1级振动门限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204022,"塔架前后方向的加速度高于2级振动门限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204023,"塔架前后方向越1级振动门限值重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204024,"塔架水平合方向的加速度超限","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204025,"塔架前后方向的加速度超限","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204026,"主轴的轴承座温度高于过高设定值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204027,"主轴的轴承座温度低于过低设定值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204028,"主轴的轴承座温度高于上限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204029,"主轴的轴承座温度低于下限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204030,"主轴的轴承座温度高于过高设定值或低于过低设定值故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204038,"PLC重启时发电机转速高于上限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204039,"主控系统测得的发电机转速与从变频器读得的不匹配","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204042,"桨叶振动过高警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204043,"桨叶振动超限停机","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204046,"存在湍流时风轮3级过速频出","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204047,"存在湍流时发电机3级过速频出","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204050,"机舱X方向瞬时加速度越1级门限","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204051,"机舱X方向瞬时加速度越1级门限频出","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204052,"机舱X方向瞬时加速度越2级门限","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204053,"机舱X方向瞬时加速度越2级门限频出","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204054,"偏航时机舱X方向瞬时加速度越1级门限","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204055,"偏航时机舱X方向瞬时加速度越1级门限频出","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204056,"偏航时机舱X方向瞬时加速度越2级门限","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204057,"偏航时机舱X方向瞬时加速度越2级门限频出","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204058,"机舱Y方向瞬时加速度越1级门限","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204059,"机舱Y方向瞬时加速度越1级门限频出","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204060,"机舱Y方向瞬时加速度越2级门限","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204061,"机舱Y方向瞬时加速度越2级门限频出","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204062,"偏航时机舱Y方向瞬时加速度越1级门限","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204063,"偏航时机舱Y方向瞬时加速度越1级门限频出","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204064,"偏航时机舱Y方向瞬时加速度越2级门限","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204065,"偏航时机舱Y方向瞬时加速度越2级门限频出","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204066,"机舱Z方向瞬时加速度越1级门限","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204067,"机舱Z方向瞬时加速度越1级门限频出","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204068,"机舱Z方向瞬时加速度越2级门限","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204069,"机舱Z方向瞬时加速度越2级门限频出","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204070,"偏航时机舱Z方向瞬时加速度越1级门限","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204071,"偏航时机舱Z方向瞬时加速度越1级门限频出","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204072,"偏航时机舱Z方向瞬时加速度越2级门限","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204073,"偏航时机舱Z方向瞬时加速度越2级门限频出","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204101,"风轮锁解锁","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204102,"发电机转速小于切出电网转速","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204103,"低速端两个PDM转速不匹配","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204104,"低速端转速与变频器测得发电机转速不匹配重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204105,"低速端转速与变频器测得发电机转速不匹配复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204106,"过速继电器和低速端转速不匹配重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204107,"过速继电器和低速端转速不匹配复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204108,"高速端空载转动","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204109,"存在湍流时低速端3级过速","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204110,"存在湍流时发电机3级过速","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",204111,"高湍流限转速","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205001,"齿轮箱过滤器阻塞警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205003,"齿轮箱过滤器阻塞故障，要求停机","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205005,"齿轮箱油池油位故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205008,"齿轮箱入口油压高于上限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205009,"齿轮箱油入口压力低于下限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205011,"轴承温度和油池温度相差过大","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205015,"齿轮箱油池温度高于过高设定值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205016,"齿轮箱油池温度低于过低设定值","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205017,"齿轮箱油池温度高于上限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205018,"齿轮箱油池温度低于下限值","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205019,"齿轮箱入口油温高于过高设定值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205020,"齿轮箱入口油温低于过低设定值","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205021,"齿轮箱入口油温高于上限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205022,"齿轮箱入口油温低于下限值","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205028,"齿轮箱驱动端轴承温度高于过高设定值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205029,"齿轮箱驱动端轴承温度低于过低设定值","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205030,"齿轮箱驱动端轴承温度高于上限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205031,"齿轮箱驱动端轴承温度低于下限值","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205033,"齿轮箱非驱动端轴承温度高于过高设定值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205034,"齿轮箱非驱动端轴承温度低于过低设定值","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205035,"齿轮箱非驱动端轴承温度高于上限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205036,"齿轮箱非驱动端轴承温度低于下限值","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205038,"齿轮箱中速轴驱动端温度过高告警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205039,"齿轮箱中速轴驱动端温度高于最大设定值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205041,"齿轮箱中速轴非驱动端温度过高告警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205042,"齿轮箱中速轴非驱动端温度高于最大设定值","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205043,"齿轮箱过滤器的油温过高","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205044,"齿轮箱过滤器压力过大","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205045,"齿轮箱精滤器堵塞","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205046,"齿轮箱过滤器入口压力高于上限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205047,"齿轮箱过滤器入口压力低于下限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205048,"齿轮箱油池温度限功率开启","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205049,"齿轮箱颗粒过多报警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205050,"齿轮箱颗粒过多故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205051,"齿轮箱颗粒计数器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",205100,"齿轮箱过滤器不监测阻塞情况","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",207002,"机械刹车刹车盘磨损警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",207003,"机械刹车刹车盘磨损故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",207005,"机械刹车释放失灵","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",208001,"发电机10分钟平均功率高于上限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",208002,"发电机30秒平均功率高于上限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",208003,"发电机1秒平均功率高于上限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",208004,"发电机10分钟平均功率高于上限值故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",208006,"发电机碳刷磨损警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",208012,"发电机定子两相绕组温差大于设定值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",208030,"发电机非驱动端轴承温度高于过高设定值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",208108,"发电机水冷系统故障模式","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",208135,"发电机水冷系统压力建立，达到加热器启动条件","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",210002,"偏航系统逆时针2级限位开关被撞开","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",210010,"偏航系统电机运行时间过长","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",210133,"偏航电机1热继保护传感器失效","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",210154,"偏航系统2#过温保护传感器失效","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",210161,"偏航撞二级限位保护","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",210186,"偏航制动PETP上摩擦片润滑泵闭锁时间太长","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",211095,"阵风造成PCH测得的SSD震动值高于设定值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",211122,"风机处于并网动作中","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",212002,"机舱发出风机进入检修或变桨检修命令","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",212102,"机舱或塔底发出快速启动命令","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",215007,"预留报警4（刹车等级100）","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",215028,"预留报警1（亚健康）","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",301004,"变频柜上的急停按钮被拍下触发了紧急停机","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",302036,"塔底24V UPS电池充电模式","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",302227,"声光报警器开启","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",304020,"电网频率高于上限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",304336,"电网电压过高故障重复出现","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",304345,"变频器内部限功率","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",304369,"CMS齿轮箱行星级加速度2总震值超过报警阈值1","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305033,"变频器水冷系统过压","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305040,"变频器水冷系统维护模式","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305062,"变频器水冷泵出口入口压差太低","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305141,"变频器外部故障保护","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305166,"变频器定子接触器断开超时","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305187,"变频器定子接触器状态反馈错误复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305196,"变频器Chopper过载复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305219,"变频器编码器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305240,"变频器未在转速运行范围","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305247,"变频器CAN Bus故障重复故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305271,"变频器网侧接触器动作超时复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305294,"断路器异常断开或闭合","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305319,"变频器网侧接地故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305340,"变频器网侧驱动故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305347,"变频器环境温度过低故障复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305368,"变频器机侧功率模块温差过大复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305389,"变频器主控通讯接口接收PDO数据超时复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305396,"变频器转子电流没有反馈","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305421,"网侧接触器或网侧滤波异常断开或闭合重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305465,"变频器网侧短路自恢复失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305514,"禾望变频器事件记录存储失败复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305535,"禾望变频器网侧模块IGBT过流复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305542,"禾望变频器同步失败","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305563,"禾望变频器定子过流","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305584,"禾望变频器电网频率异常","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305591,"禾望变频器转子相序反重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305612,"禾望变频器主断路器脱扣重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305637,"禾望变频器主动Crowbar动作次数超限复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305658,"禾望变频器机侧防雷器故障复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305679,"禾望变频器网侧电感过热复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305686,"禾望变频器变流器停机超时","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305712,"变频器电抗器过温复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305740,"变频器非法操作复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305743,"变频器功率单元过温复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305764,"变频器控制器过温复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305789,"变频器系统警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",305813,"变频器底层系统调度异常","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",306009,"PLC主任务执行时间高于其执行周期","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",306017,"主控制器与MOOG变桨系统Profibus通讯故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",306042,"CF卡中的Celogger_data超限","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",306068,"机舱EtherCAT Frame0数据帧出错","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",306071,"机舱BK1250状态异常","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",306134,"参数设定超限故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",306205,"塔底IO板输出配置无效","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",306226,"机舱IO板2固件失效","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",306247,"机舱IO板1CanOpen通讯CRC校验错误","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",306254,"机舱IO板1CanOpen通讯主站侧中断","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",308102,"远程发出风机快速启动指令","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",309114,"升速过程中处于共振区时间过长","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",309117,"桨叶2电池自检超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",402018,"3号桨叶超级电容电压过高故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",402046,"主控先断开了EFC信号","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",402074,"1号桨叶开始自主回桨","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",402081,"3号桨叶400V电源故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",402102,"1号轴控柜温度传感器断线故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",402128,"HVRT level1 报警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",403015,"KEB3号桨叶动器内部存在警告信息","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",403018,"KEB3号桨叶驱动器风扇报警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",403039,"KEB3号轴电机温度过高故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",403064,"KEB3号桨叶后备电源电压过低故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",403085,"KEB3号桨叶接近开关位置检测故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",403092,"KEB1号桨叶驱动器报出内部故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",403113,"KEB3号轴柜F1跳闸故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",403134,"KEB1号桨叶轴控柜温度传感器断线报警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",403159,"KEB变桨1号桨叶PLC手动重启使能","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",403165,"KEB变桨1号桨叶PLC处于重启状态","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",403192,"KEB1号桨叶驱动器温度传感器断线报警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",406036,"发电机高澜水冷系统三通阀全闭","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",415011,"桨叶3峰-峰值过高警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.6335 ",415018,"主控系统读得的叶片PCH震动值长时间不刷新","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",105005,"2号桨叶从91度限位脱开失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",105028,"某一个桨叶驱动器内部温度过高","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",105054,"3号桨PM直流母线电压低","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",105057,"3号桨的出现警报","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",105111,"1号桨的95度限位开关被撞开","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",105132,"变桨超级电容充电超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",105168,"3号桨故障，触发电池驱动回桨自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",105175,"某一桨叶变桨超速自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",105221,"MOOG变桨两桨叶间角度差相差2度自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",105250,"变桨自润滑泵油位低报警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",202008,"控制柜防雷器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",202015,"机舱人工安全链或机舱机器安全链的24V电源开路","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",202052,"测量机舱柜温度的PT100传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",202089,"机械式风向标故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",202119,"机械刹车4号阀设定打开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",202133,"发电机滑环室测温PT100传感器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",203003,"机舱温度高于最大上限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",204028,"主轴的轴承座温度高于上限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",204062,"偏航时机舱Y方向瞬时加速度越1级门限","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",204065,"偏航时机舱Y方向瞬时加速度越2级门限频出","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",205011,"轴承温度和油池温度相差过大","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",205043,"齿轮箱过滤器的油温过高","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",208012,"发电机定子两相绕组温差大于设定值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",208019,"发电机定子V相绕组温度高于上限值","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",208040,"发电机30秒平均功率高于上限值故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",208113,"发电机水冷系统散热器过载","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",208136,"发电机水冷加热器加热时间过长","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",208139,"高速轴转速信号的1s均方差过高","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",210019,"偏航系统1号电机PTC测温电阻触发","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",210134,"偏航电机2热继保护传感器失效","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",210155,"偏航系统3#过温保护传感器失效","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",210162,"偏航电机6热继保护传感器失效","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",210187,"偏航制动PETP上摩擦片润滑泵远程启动","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",211100,"检测到出现阵风","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",211123,"风机处于并网模式","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",211126,"风机处于自检2","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",213005,"独立变桨控制系统标定故障","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",215008,"预留报警1（刹车等级51）","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",215015,"预留报警3（刹车等级199）","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",301005,"塔底机器安全链没有反馈信号","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",302034,"塔底24V 电池更换警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",303004,"塔底温度低于下限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",304020,"电网频率高于上限值","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",304100,"箱变油温过高告警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",304345,"变频器内部限功率","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",304369,"CMS齿轮箱行星级加速度2总震值超过报警阈值1","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305003,"变频器机侧未及时响应启动指令","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305040,"变频器水冷系统维护模式","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305062,"变频器水冷泵出口入口压差太低","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305145,"变频器机侧过流","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305166,"变频器定子接触器断开超时","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305173,"变频器主断路器断开重复故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305196,"变频器Chopper过载复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305219,"变频器编码器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305226,"变频器机侧驱动故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305247,"变频器CAN Bus故障重复故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305271,"变频器网侧接触器动作超时复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305298,"断路器保护性跳闸重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305319,"变频器网侧接地故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305326,"变频器定子接地故障复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305347,"变频器环境温度过低故障复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305368,"变频器机侧功率模块温差过大复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305375,"变频器低风速短接开关断开超时","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305396,"变频器转子电流没有反馈","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305421,"网侧接触器或网侧滤波异常断开或闭合重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305465,"变频器网侧短路自恢复失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305514,"禾望变频器事件记录存储失败复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305521,"禾望变频器主控通讯错误","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305542,"禾望变频器同步失败","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305563,"禾望变频器定子过流","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305570,"禾望变频器母线软件过压重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305591,"禾望变频器转子相序反重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305616,"禾望变频器主断路器状态错误复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305637,"禾望变频器主动Crowbar动作次数超限复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305658,"禾望变频器机侧防雷器故障复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305665,"禾望变频器紧急停机","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305686,"禾望变频器变流器停机超时","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305712,"变频器电抗器过温复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305719,"变频器定子电压异常复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305743,"变频器功率单元过温复位失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305768,"变频器驱动故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305789,"变频器系统警告","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305813,"变频器底层系统调度异常","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",305821,"变频器定子接触器故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",306017,"主控制器与MOOG变桨系统Profibus通讯故障重复出现","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",306042,"CF卡中的Celogger_data超限","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",306049,"Celogger模块临时文件过多","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",306071,"机舱BK1250状态异常","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",306140,"风机处于齿轮箱监测状态","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",306205,"塔底IO板输出配置无效","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",306226,"机舱IO板2固件失效","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",306233,"机舱IO板2看门狗配置无效","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",306254,"机舱IO板1CanOpen通讯主站侧中断","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",309001,"风机正常运行","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",309008,"Scada发出手动控制风机指令","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",309117,"桨叶2电池自检超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",402022,"1号轴控柜温度过低故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",402046,"主控先断开了EFC信号","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",402074,"1号桨叶开始自主回桨","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",402081,"3号桨叶400V电源故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",402102,"1号轴控柜温度传感器断线故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",402132,"1号桨叶角度检查偏差过大报警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",402136,"变桨系统后备电源自检模式","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",403018,"KEB3号桨叶驱动器风扇报警","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",403043,"KEB400V浪涌保护器故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",403064,"KEB3号桨叶后备电源电压过低故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",403071,"KEB2号桨叶后备电源充电故障","告警信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",403092,"KEB1号桨叶驱动器报出内部故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",403113,"KEB3号轴柜F1跳闸故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",403138,"主控制器与变桨系统Profibus通讯自恢复超时","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",403141,"变桨EFC信号被强制故障","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",403165,"KEB变桨1号桨叶PLC处于重启状态","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",403196,"KEB变桨2号桨叶电容自检失败","故障 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",406036,"发电机高澜水冷系统三通阀全闭","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",409004,"超声波风速仪加热器MCB跳开","提示信息 "]
["PLC_ALL_Config_2016r2.rc5.powermodified.6536 ",415018,"主控系统读得的叶片PCH震动值长时间不刷新","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",-3,"恢复连接","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",105025,"华电变桨没有收到来自主控的EFC信号","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",105028,"某一个桨叶驱动器内部温度过高","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",105050,"3号桨电池电压过高或过低","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",105100,"1号，2号或3号桨报告预充电电阻过温","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",105125,"天仁变桨两桨叶间角度差相差2度警告","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",105132,"变桨超级电容充电超时","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",105167,"2号桨故障，触发电池驱动回桨重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",105202,"MOOG变桨系统EFC信号被强制","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",105246,"桨叶3抱闸继电器4K1故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",105249,"变桨自润滑泵油位低","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",202004,"塔底温控回路空开跳开","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",202038,"机舱柜中发电机空间加热器保护空开跳开","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",202065,"齿轮箱入口压力传感器故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",202076,"至少两相发电机定子PT100传感器故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",202111,"风速仪和风向标的加热器设定打开","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",202140,"24V柜内IO供电空开跳开","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",204010,"低速端2号传感器故障","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",204016,"无湍流时风轮转速高于3级超速门限值","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",204054,"偏航时机舱X方向瞬时加速度越1级门限","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",204101,"风轮锁解锁","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",205019,"齿轮箱入口油温高于过高设定值","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",205031,"齿轮箱驱动端轴承温度低于下限值","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",205055,"行星轮后轴承2温度高故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",208014,"发电机定子U相绕组温度低于过低设定值","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",208039,"发电机冷却系统入口或出口温度高于过高设定值或低于过低设定值故障重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",208042,"发电机10分钟平均功率高于上限值限功率","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",208117,"发电机水冷主循环泵电加热器三通阀MCB故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",208138,"发电机滑环室温度过高停机","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",210010,"偏航系统电机运行时间过长","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",210021,"偏航系统3号电机PTC测温电阻触发","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",210136,"偏航电机4热继保护传感器失效","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",210161,"偏航撞二级限位保护","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",210186,"偏航制动PETP上摩擦片润滑泵闭锁时间太长","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",210189,"偏航制动PETP上摩擦片润滑泵手动模式","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",211031,"当前采用机械式气象站","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",211115,"偏航或湍流情况下PCH测得的SSD震动值高于设定值","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",211137,"切换到双模-低速模式超时","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",212003,"远程发出手工偏航命令","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",214003,"主控跟PCH通讯的从站节点状态异常","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",215022,"预留报警5（保护性停机）","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",302001,"塔底柜恒温器测得温度超出范围","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",302006,"塔底柜防雷器故障","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",302127,"塔底温度PT100失效风扇强制开启","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",304003,"电网电压L2相超出上限值","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",304107,"35KV负荷开关分位","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",304110,"10KV负荷开关分位","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",304335,"电网电压正序分量过低故障重复出现","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",304364,"CMS齿轮箱输入端加速度1总震值超过报警阈值2","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305010,"变频器多种警告故障重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305028,"变频器过压保护被触发","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305053,"变频器水冷泵出口压力低（二级门限）","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305131,"变频器报告低风速模式并网成功","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305158,"变频器网侧滤波回路故障","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305161,"变频器网侧对地短路","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305182,"变频器定子接触器闭合情况下闭合主断路器","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305211,"控制板间通讯故障重复故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305220,"变频器编码器故障重复故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305234,"变频器断路器储能故障重复故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305259,"变频器控制板间通讯故障重复故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305285,"变频器定子接触器闭合超时复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305310,"变频器低风速短接开关断开重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305313,"变频器同步过程闭合定子接触器超时重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305334,"变频器定子CT故障重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305359,"变频器机侧功率模块温度过低复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305380,"变频器断开定子开关超时复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305387,"变频器主控通讯接口接收PDO数据超时","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305408,"变频器安全链断开复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305452,"变频器网侧驱动故障重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305505,"禾望变频器EEPROM参数回默认值复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305508,"禾望变频器CAN通讯故障复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305529,"禾望变频器驱动板连接错误复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305554,"禾望变频器网侧模块软件过流","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305575,"禾望变频器电网线电压过压","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305582,"禾望变频器定子电压异常重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305603,"禾望变频器主接触器状态异常重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305624,"禾望变频器Crowbar测试失败重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305649,"禾望变频器主滤波器断开复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305652,"禾望变频器主输入防雷器故障复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305677,"禾望变频器网侧电感过热","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305703,"变频器Chopper 故障复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305724,"变频器断路器故障重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305734,"变频器测得发电机转速异常复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305755,"变频器功率套件加热超时复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305776,"变频器散热风扇过温复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305801,"变频器判定低风速模式下未正常进入转速运行范围","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305804,"变频器低风速模式下机侧未及时响应启动指令重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",305833,"风机AVC：FaultReport错误","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",306022,"将参数保存到PLC的CF卡的xml文件时失败","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",306046,"CF卡中的CMS超限","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",306053,"读取Golden参数文件异常警告","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",306075,"机舱EL6751状态异常","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",306140,"风机处于齿轮箱监测状态","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",306209,"塔底IO板看门狗配置无效","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",306212,"机舱IO板1同步故障","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",306237,"塔底IO板CanOpen通讯CRC校验错误","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",306258,"塔底自研IO模块1状态异常","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",309001,"风机正常运行","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",309012,"100号刹车模式时间过长","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",309121,"PLC WinCE操作系统Load过高","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402026,"变桨系统发出报警信息","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402053,"1号超级电容自检报警","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402056,"1号超级电容自检故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402085,"3号轴控柜内1F2失效故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402106,"2号后备电源柜温度传感器断线低故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402132,"1号桨叶角度检查偏差过大报警","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402141,"穆格PCS3 桨叶1两编码器角度差值超限","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402162,"穆格PCS3变桨系统处于紧急模式","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402187,"穆格PCS3变桨3号桨叶91度限位触发位置故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402208,"穆格PCS3 桨叶1开始自主回桨","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402211,"穆格PCS3变桨系统LVRT故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402236,"穆格PCS3 桨叶1电机温度传感器断线故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402257,"穆格PCS3 桨叶1手动Bypass91度限位开关使能","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402278,"穆格PCS3 桨叶1变桨电机I2T超限警告","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",402285,"穆格PCS3 桨叶2驱动器I2T超限警告","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",403005,"KEB2号桨叶95度限位撞开","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",403030,"KEB3号轴驱动器内部温度过高报警","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",403051,"KEB2号桨叶后备电源电压过高报警","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",403054,"KEB2号桨叶直流母线熔丝断开报警","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",403079,"KEB3号电机堵转故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",403100,"KEB3号桨叶电机超速故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",403107,"KEB变桨LVRT故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",403128,"KEB1号桨叶轴控柜温度过高故障","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",403149,"变桨两桨叶间角度差相差超过一级门限重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",403180,"KEB变桨1号桨叶后备电源手动放电使能","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",403204,"KEB变桨1号桨叶反馈电容自检报警","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",403207,"KEB变桨EFC信号自检超时","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",411100,"箱变主绕组温度高亚健康报警","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",415014,"桨叶1一阶频谱强度异常危险警告","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",415021,"激光测量数据过小警告","提示信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",416007,"RunUp启动性能检测到叶片气动性能警告","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",429025,"后主轴承径向振动超限报警5","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",429050,"齿轮箱低速级径向振动超限报警5","故障 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",429071,"齿轮箱高速级电机侧轴向振动超限报警1","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",429078,"发电机驱动端径向振动超限报警3","告警信息 "]
["PLC_ALL_Config_2017r1.sp2.7801 ",517011,"偏航故障触发特殊回桨模式","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",105005,"2号桨叶从91度限位脱开失败","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",105014,"1号桨PM直流母线电压低","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",105035,"变桨系统某一桨叶处于强制手动模式","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",105057,"3号桨的出现警报","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",105111,"1号桨的95度限位开关被撞开","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",105132,"变桨超级电容充电超时","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",105154,"1号桨出现角度传感器故障重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",105175,"某一桨叶变桨超速自恢复超时","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",105221,"MOOG变桨两桨叶间角度差相差2度自恢复超时","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",105236,"请及时更换桨叶2抱闸继电器","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",105257,"变桨自润滑系统柱塞误动作警告","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",202008,"控制柜防雷器故障","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",202048,"偏航系统3号电机热保护继电器触发","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",202077,"测量舱外环境温度的PT100传感器故障","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",202093,"风速仪故障重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",202119,"机械刹车4号阀设定打开","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",202156,"主轴承润滑系统泵柱塞误启动","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",203003,"机舱温度高于最大上限值","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",204024,"塔架水平合方向的加速度超限","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",204062,"偏航时机舱Y方向瞬时加速度越1级门限","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",204109,"存在湍流时低速端3级过速","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",205033,"齿轮箱非驱动端轴承温度高于过高设定值","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",205042,"齿轮箱中速轴非驱动端温度高于最大设定值","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",207002,"机械刹车刹车盘磨损警告","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",208022,"发电机定子W相绕组温度低于过低设定值","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",208029,"发电机驱动端轴承温度低于下限值","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",208057,"发电机润滑泵柱塞规定时间内不动作重复出现故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",208125,"发电机水冷泵出口压力高（二级门限）","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",209010,"液压泵开启过于频繁警告","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",210022,"偏航系统4号电机PTC测温电阻触发","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",210107,"偏航系统开始自润滑","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",210144,"偏航2#电机热继保护触发","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",210169,"偏航滑移速率过快重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",210172,"偏航自润滑误动作","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",211021,"叶片结冰或性能下降导致功率曲线异常","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",211110,"SC02_11_115重复出现或复位失败或SC02_11_116复位失败","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",211132,"风速波动过大转速无法稳定","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",213007,"限制发电机转速降噪","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",213014,"扇区控制下限制功率","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",215013,"预留报警1（刹车等级199）","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",301007,"远程发出复位安全链命令","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",301010,"变频器过功率触发安全链断开","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",302109,"控制柜暖机模式","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",303007,"塔底温度过高过低故障重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",304021,"电网频率低于下限值","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",304119,"变压器油面温度高限功率","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",304330,"电网电压正序分量偏低","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",304355,"扇区管理限功率","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305004,"变频器机侧未及时响应启动指令重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305007,"变频器网侧无响应","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305044,"变频器水冷泵入口温度传感器故障","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305104,"变频器报告断路器断开","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305149,"变频器未准备就绪即启动重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305156,"变频器网侧UCE短路","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305177,"变频器主断路器断开延迟故障重复故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305194,"变频器Chopper过载","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305226,"变频器机侧驱动故障","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305229,"变频器脱网超时","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305250,"变频器同步超时重复故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305280,"变频器机侧报直流母线过压重复故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305301,"变频器网侧接触器闭合超时重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305308,"变频器低风速短接开关操作超时复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305329,"变频器网侧过流复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305350,"变频器环境温度过高故障复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305375,"变频器低风速短接开关断开超时","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305378,"变频器断开定子开关超时","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305399,"变频器定子电压反馈错误","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305428,"变频器网侧无响应自恢复失败","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305468,"变频器网侧对地短路重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305503,"禾望变频器EEPROM参数回默认值","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305524,"禾望变频器热线连接错误","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305545,"禾望变频器预充电超时","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305570,"禾望变频器母线软件过压重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305573,"禾望变频器母线欠压重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305598,"禾望变频器预充电接触器状态错误复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305619,"禾望变频器Crowbar触发复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305640,"禾望变频器电机超速复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305647,"禾望变频器主滤波器断开","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305668,"禾望变频器主控电网保护开关断开","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305689,"禾望变频器预留故障","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305719,"变频器定子电压异常复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305722,"变频器动力电缆接线接错复位失败","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305750,"变频器过流故障","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305771,"变频熔丝断开","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305792,"变频器烟雾报警","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305799,"变频器状态监测异常重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",305824,"变频器断路器故障跳闸","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",306016,"主控制器与MOOG变桨系统Profibus通讯中断警告","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",306041,"CF卡中的Celogger_data过多警告","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",306044,"CF卡中的ResetOperationLog超限","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",306070,"EtherCAT系统异常","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",306133,"参数设定超限报警","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",306200,"塔底IO板同步故障","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",306207,"塔底IO板分布时钟同步周期错误","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",306228,"机舱IO板2输入配置无效","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",306253,"机舱IO板1CanOpen通讯NMT状态机出错","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",308006,"操作员停机","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",308104,"风机接收到复位安全链指令","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",309116,"桨叶1电池自检超时","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402017,"2号桨叶超级电容电压过高故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402041,"3号变桨电机温度过高故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402051,"2号超级电容需要维护","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402076,"3号桨叶开始自主回桨","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402101,"3号后备电源柜温度过低故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402127,"轮毂温度过低报警","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402130,"HVRT 故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402157,"穆格PCS3两桨叶间角度差相差超过二级门限重复出现","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402178,"穆格PCS3 桨叶3直流母线电压异常","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402185,"穆格PCS3变桨1号桨叶91度限位触发位置故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402206,"穆格PCS3 反馈变桨与主控制器通讯故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402227,"穆格PCS3 桨叶1轴控柜温度传感器断线故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402252,"穆格PCS3变桨主接口模块AC/DC转换异常","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402273,"穆格PCS3 桨叶2编码器重置","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402276,"穆格PCS3 桨叶2后备电源模块电压不平衡故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",402301,"MOOG 特殊回桨使能硬线回路异常","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",403021,"KEB3号轴散热器风扇报警","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",403028,"KEB1号轴驱动器内部温度过高报警","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",403049,"KEB3号轴400V电源缺相故障","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",403070,"KEB1号桨叶后备电源充电故障自恢复失败","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",403095,"KEB1号桨叶电机编码器故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",403116,"KEB1号桨叶后备电源柜温度过高故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",403119,"KEB1号桨叶后备电源柜温度过高报警","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",403144,"主控制器没有收到EFC反馈信号警告","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",403168,"KEB1号桨叶PLC重启超时","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",403178,"KEB变桨2号桨叶P6与电网隔离","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",403202,"KEB变桨2号桨叶自检电容电压故障","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",408140,"变频器水冷系统三通阀全闭","提示信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",415010,"桨叶3振动峰值过高危险警告","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",429012,"前主轴承径向振动超限报警2","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",429019,"前主轴承轴向振动超限报警4","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",429040,"齿轮箱第一行星级径向振动超限报警5","故障 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",429061,"齿轮箱高速级风轮侧径向振动超限报警1","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",429068,"齿轮箱高速级电机侧径向振动超限报警3","告警信息 "]
["PLC_ALL_Config_2017r1.sp1.7393 ",429089,"发电机非驱动端径向振动超限报警4","告警信息 "]
["PLC_ALL_Config_8220 ",-5,"恢复连接","提示信息 "]
["PLC_ALL_Config_8220 ",202010,"机舱控制柜温度过低警告","提示信息 "]
["PLC_ALL_Config_8220 ",202043,"机舱柜中齿轮箱油管加热器保护开关跳开","告警信息 "]
["PLC_ALL_Config_8220 ",202053,"机舱温度测量PT100传感器故障","告警信息 "]
["PLC_ALL_Config_8220 ",202090,"液压站储能罐压力传感器故障","告警信息 "]
["PLC_ALL_Config_8220 ",202114,"偏航系统设定顺时针偏航","提示信息 "]
["PLC_ALL_Config_8220 ",202132,"齿轮箱精滤器保护空开跳开","提示信息 "]
["PLC_ALL_Config_8220 ",204004,"发电机转速高于1级超速门限值","告警信息 "]
["PLC_ALL_Config_8220 ",204052,"机舱X方向瞬时加速度越2级门限","告警信息 "]
["PLC_ALL_Config_8220 ",204073,"偏航时机舱Z方向瞬时加速度越2级门限频出","故障 "]
["PLC_ALL_Config_8220 ",205019,"齿轮箱入口油池温度过高警告","告警信息 "]
["PLC_ALL_Config_8220 ",205039,"齿轮箱中间级驱动端轴承温度过高故障","故障 "]
["PLC_ALL_Config_8220 ",207001,"液压泵电机过载","告警信息 "]
["PLC_ALL_Config_8220 ",208020,"发电机定子V相绕组温度过低故障","告警信息 "]
["PLC_ALL_Config_8220 ",208028,"发电机驱动端轴承温度过高故障","故障 "]
["PLC_ALL_Config_8220 ",209003,"液压系统刹车回路压力低于下限值故障","告警信息 "]
["PLC_ALL_Config_8220 ",210018,"偏航系统的机舱位置发生偏移","告警信息 "]
["PLC_ALL_Config_8220 ",210135,"偏航电机3热继保护传感器失效","故障 "]
["PLC_ALL_Config_8220 ",210156,"偏航系统4号过温保护传感器失效","故障 "]
["PLC_ALL_Config_8220 ",210165,"偏航系统6号电机温度保护触发异常","故障 "]
["PLC_ALL_Config_8220 ",211019,"舱外环境温度过低故障","告警信息 "]
["PLC_ALL_Config_8220 ",211119,"桨角积分判定风速过大","提示信息 "]
["PLC_ALL_Config_8220 ",211131,"风向标数据不刷新重复出现","故障 "]
["PLC_ALL_Config_8220 ",215001,"远景自研CMS运行故障","提示信息 "]
["PLC_ALL_Config_8220 ",215026,"预留报警4（重复出现）","故障 "]
["PLC_ALL_Config_8220 ",302025,"塔底控制柜温度过低警告","告警信息 "]
["PLC_ALL_Config_8220 ",302139,"塔底除湿机内部风扇启动","提示信息 "]
["PLC_ALL_Config_8220 ",302146,"塔底除湿机通讯故障","告警信息 "]
["PLC_ALL_Config_8220 ",302168,"机舱除湿机除湿机构空开跳开","告警信息 "]
["PLC_ALL_Config_8220 ",303004,"塔底温度过低故障","告警信息 "]
["PLC_ALL_Config_8220 ",303102,"电缆温度过高限超发","提示信息 "]
["PLC_ALL_Config_8220 ",304102,"箱变油位过低告警","告警信息 "]
["PLC_ALL_Config_8220 ",304365,"CMS齿轮箱输入端加速度2总震值超过报警阈值1","告警信息 "]
["PLC_ALL_Config_8220 ",305081,"变频器报告电网电压超出运行范围","告警信息 "]
["PLC_ALL_Config_8220 ",305145,"变频器机侧过流","告警信息 "]
["PLC_ALL_Config_8220 ",305152,"变频器定子侧过电流重复出现","故障 "]
["PLC_ALL_Config_8220 ",305178,"变频器主断路器断开延迟故障复位失败","故障 "]
["PLC_ALL_Config_8220 ",305205,"变频器NPR NTC 故障重复故障","故障 "]
["PLC_ALL_Config_8220 ",305210,"控制板间通讯故障","告警信息 "]
["PLC_ALL_Config_8220 ",305231,"变频器脱网超时复位失败","故障 "]
["PLC_ALL_Config_8220 ",305256,"变频器散热片温度过低重复故障","故障 "]
["PLC_ALL_Config_8220 ",305282,"变频器机侧散热片过热重复故障","故障 "]
["PLC_ALL_Config_8220 ",305289,"变频器风扇过温重复出现","故障 "]
["PLC_ALL_Config_8220 ",305313,"变频器同步过程闭合定子接触器超时重复出现","故障 "]
["PLC_ALL_Config_8220 ",305337,"变频器DCchopper驱动故障重复出现","故障 "]
["PLC_ALL_Config_8220 ",305362,"变频器机侧功率模块温度过低复位失败","故障 "]
["PLC_ALL_Config_8220 ",305371,"变频器电机速度过高复位失败","故障 "]
["PLC_ALL_Config_8220 ",305395,"变频器定子电压没有反馈复位失败","故障 "]
["PLC_ALL_Config_8220 ",305424,"变频器网侧预充电故障复位失败","故障 "]
["PLC_ALL_Config_8220 ",305466,"变频器网侧过流重复出现","故障 "]
["PLC_ALL_Config_8220 ",305501,"禾望变频器RAM自检失败重复出现","故障 "]
["PLC_ALL_Config_8220 ",305522,"禾望变频器主控通讯错误重复出现","故障 "]
["PLC_ALL_Config_8220 ",305543,"禾望变频器同步失败重复出现","故障 "]
["PLC_ALL_Config_8220 ",305568,"禾望变频器母线硬件过压复位失败","故障 "]
["PLC_ALL_Config_8220 ",305574,"禾望变频器母线欠压复位失败","故障 "]
["PLC_ALL_Config_8220 ",305591,"禾望变频器转子相序反重复出现","故障 "]
["PLC_ALL_Config_8220 ",305616,"禾望变频器主断路器状态错误复位失败","故障 "]
["PLC_ALL_Config_8220 ",305637,"禾望变频器主动Crowbar动作次数超限复位失败","故障 "]
["PLC_ALL_Config_8220 ",305644,"禾望变频器主路熔丝断开","告警信息 "]
["PLC_ALL_Config_8220 ",305665,"禾望变频器紧急停机","告警信息 "]
["PLC_ALL_Config_8220 ",305686,"禾望变频器变流器停机超时","告警信息 "]
["PLC_ALL_Config_8220 ",305716,"变频器电源故障复位失败","故障 "]
["PLC_ALL_Config_8220 ",305719,"变频器定子电压异常复位失败","故障 "]
["PLC_ALL_Config_8220 ",305747,"变频器柜内温度过高","告警信息 "]
["PLC_ALL_Config_8220 ",305768,"变频器驱动故障","告警信息 "]
["PLC_ALL_Config_8220 ",305789,"变频器系统警告","告警信息 "]
["PLC_ALL_Config_8220 ",305796,"变频器直流母线异常重复出现","故障 "]
["PLC_ALL_Config_8220 ",305821,"变频器定子接触器故障","告警信息 "]
["PLC_ALL_Config_8220 ",306012,"PLC-Task2任务执行超时","提示信息 "]
["PLC_ALL_Config_8220 ",306067,"机舱EtherCAT系统异常","提示信息 "]
["PLC_ALL_Config_8220 ",306071,"机舱BK1250状态异常","提示信息 "]
["PLC_ALL_Config_8220 ",306260,"机舱自研IO模块1状态异常","提示信息 "]
["PLC_ALL_Config_8220 ",309008,"远程命令进入手动模式","提示信息 "]
["PLC_ALL_Config_8220 ",401009,"安全链G传感器1错误","故障 "]
["PLC_ALL_Config_8220 ",401023,"安全控制器测得低速端编码器故障","故障 "]
["PLC_ALL_Config_8220 ",403018,"KEB3号桨叶驱动器风扇报警","告警信息 "]
["PLC_ALL_Config_8220 ",403039,"KEB3号轴电机温度过高故障","故障 "]
["PLC_ALL_Config_8220 ",403064,"KEB3号桨叶后备电源电压过低故障","故障 "]
["PLC_ALL_Config_8220 ",403067,"KEB3号桨叶后备电源充电回路故障","故障 "]
["PLC_ALL_Config_8220 ",403092,"KEB1号桨叶驱动器报出内部故障","故障 "]
["PLC_ALL_Config_8220 ",403113,"KEB3号轴柜F1跳闸故障","故障 "]
["PLC_ALL_Config_8220 ",403134,"KEB1号桨叶轴控柜温度传感器断线报警","告警信息 "]
["PLC_ALL_Config_8220 ",403156,"KEB变桨处于维护模式","提示信息 "]
["PLC_ALL_Config_8220 ",403195,"KEB变桨1号桨叶电容自检失败","故障 "]
["PLC_ALL_Config_8220 ",404018,"传动链联轴器打滑","告警信息 "]
["PLC_ALL_Config_8220 ",404046,"低速端转速RMS过高警告","故障 "]
["PLC_ALL_Config_8220 ",404052,"高速端两个PDM转速不匹配","告警信息 "]
["PLC_ALL_Config_8220 ",405027,"齿轮箱高速轴(GSGS)温度高警告","告警信息 "]
["PLC_ALL_Config_8220 ",405051,"齿轮箱右扭力臂位置传感器损坏","告警信息 "]
["PLC_ALL_Config_8220 ",406043,"发电机润滑泵控制进入手动模式","提示信息 "]
["PLC_ALL_Config_8220 ",408004,"冷却系统循环泵2高速电机启动","提示信息 "]
["PLC_ALL_Config_8220 ",408025,"水冷循环泵1空开跳开","告警信息 "]
["PLC_ALL_Config_8220 ",408110,"塔底控制柜底部湿度传感器故障","告警信息 "]
["PLC_ALL_Config_8220 ",408131,"塔底水冷进水口PT100故障","告警信息 "]
["PLC_ALL_Config_8220 ",408134,"塔底水冷塔内冷却器入口PT100故障","告警信息 "]
["PLC_ALL_Config_8220 ",408162,"塔底冷却系统水冷泵启动","提示信息 "]
["PLC_ALL_Config_8220 ",408183,"塔底冷却系统水冷泵1手动模式开启","提示信息 "]
["PLC_ALL_Config_8220 ",408210,"塔底水冷控制柜风扇进入手动模式","提示信息 "]
["PLC_ALL_Config_8220 ",408213,"塔底水冷控制柜加热器进入手动模式","提示信息 "]
["PLC_ALL_Config_8220 ",408234,"变频器水冷系统风扇2MCB断开","告警信息 "]
["PLC_ALL_Config_8220 ",408259,"变频器水冷系统风扇1防雷触发","告警信息 "]
["PLC_ALL_Config_8220 ",408285,"塔底风冷系统手动控制模式开启","提示信息 "]
["PLC_ALL_Config_8220 ",408288,"塔底水冷风扇加热带空开跳开","提示信息 "]
["PLC_ALL_Config_8220 ",409028,"机舱加热器空开跳开","告警信息 "]
["PLC_ALL_Config_8220 ",409118,"机械式风向标故障","告警信息 "]
["PLC_ALL_Config_8220 ",411014,"开关设备正在打开","提示信息 "]
["PLC_ALL_Config_8220 ",411032,"高压室内温度PT100故障","告警信息 "]
["PLC_ALL_Config_8220 ",411100,"箱变主绕组温度高亚健康报警","告警信息 "]
["PLC_ALL_Config_8220 ",412105,"ABB变频器充电回路故障","告警信息 "]
["PLC_ALL_Config_8220 ",412128,"ABB变频器网侧模块故障","告警信息 "]
["PLC_ALL_Config_8220 ",412131,"ABB变频器网侧控制器程序故障","告警信息 "]
["PLC_ALL_Config_8220 ",412178,"ABB变频器机械刹车故障重复出现","故障 "]
["PLC_ALL_Config_8220 ",412214,"ABB变频器网侧IGBT故障重复出现","故障 "]
["PLC_ALL_Config_8220 ",413012,"塔底690V防雷器触发","告警信息 "]
["PLC_ALL_Config_8220 ",413015,"机舱400V防雷器触发","告警信息 "]
["PLC_ALL_Config_8220 ",413036,"风机尚有问题禁止离开","提示信息 "]
["PLC_ALL_Config_8220 ",413065,"塔底温度过低警告重复出现","故障 "]
["PLC_ALL_Config_8220 ",415018,"主控系统读得的叶片PCH震动值长时间不刷新","故障 "]
["PLC_ALL_Config_8220 ",415025,"倾角传感器检测激光测量系统位置松动","提示信息 "]
["PLC_ALL_Config_8220 ",421017,"机舱EK1501通讯故障","提示信息 "]
["PLC_ALL_Config_8220 ",421061,"EtherCAT通讯环网重组警告","告警信息 "]
["PLC_ALL_Config_8220 ",429021,"后主轴承径向振动超限报警1","告警信息 "]
["PLC_ALL_Config_8220 ",429024,"后主轴承径向振动超限报警4","告警信息 "]
["PLC_ALL_Config_8220 ",429045,"齿轮箱第二行星级径向振动超限报警5","故障 "]
["PLC_ALL_Config_8220 ",429070,"齿轮箱高速级电机侧径向振动超限报警5","故障 "]
["PLC_ALL_Config_8220 ",429091,"远景自研CMS预警系统通道1报警1","提示信息 "]
["PLC_ALL_Config_8220 ",429098,"远景自研CMS预警系统通道4报警2","告警信息 "]
["PLC_ALL_Config_8220 ",429119,"远景自研CMS预警系统通道15报警1","提示信息 "]
["PLC_ALL_Config_8220 ",516001,"200#刹车测试","提示信息 "]
["PLC_ALL_Config_8220 ",520008,"偏航时SSD开关断开重复出现","故障 "]
["PLC_ALL_Config_8220 ",520011,"BP大于100时SSD开关断开重复出现","故障 "]
["PLC_ALL_Config_8220 ",601013,"SC1主控制器与变桨系统通讯故障自恢复超时","故障 "]
["PLC_ALL_Config_8220 ",601042,"变桨系统1号桨叶电机温度异常上升","提示信息 "]
["PLC_ALL_Config_8220 ",601065,"MOOG交流1号桨叶两编码器角度差值超限自恢复超时","故障 "]
["PLC_ALL_Config_8220 ",601072,"MOOG交流1号轴控柜内接触器3Q1的吸合次数超过了设计寿命报警","提示信息 "]
["PLC_ALL_Config_8220 ",601093,"MOOG交流1号桨叶24V电源故障","告警信息 "]
["PLC_ALL_Config_8220 ",601114,"MOOG交流2号轴控柜温度过低","故障 "]
["PLC_ALL_Config_8220 ",601139,"MOOG交流3号后备电源柜温度传感器断线故障","故障 "]
["PLC_ALL_Config_8220 ",601142,"MOOG交流系统轮毂温度传感器断线故障","故障 "]
["PLC_ALL_Config_8220 ",601168,"MOOG交流2号桨叶91度限位开关被撞开","提示信息 "]
["PLC_ALL_Config_8220 ",601189,"MOOG交流变桨系统编码器重置使能","提示信息 "]
["PLC_ALL_Config_8220 ",601210,"华电天仁2号桨叶电容充电器异常重复出现","故障 "]
["PLC_ALL_Config_8220 ",601217,"华电天仁3号桨叶后备电源电压过低","告警信息 "]
["PLC_ALL_Config_8220 ",601238,"华电天仁3号桨叶变桨超速-自复位失败","故障 "]
["PLC_ALL_Config_8220 ",601259,"华电天仁3号桨叶变桨电机堵转","故障 "]
["PLC_ALL_Config_8220 ",601284,"华电天仁1号桨叶400V电网存在故障","故障 "]
["PLC_ALL_Config_8220 ",601287,"华电天仁1号桨叶电机电流过大","故障 "]
["PLC_ALL_Config_8220 ",601312,"华电天仁2号桨叶后备电源柜温度过高","故障 "]
["PLC_ALL_Config_8220 ",601333,"华电天仁2号桨叶变桨齿轮箱变比参数设置错误","故障 "]
["PLC_ALL_Config_8220 ",601378,"KEB3号桨叶91度限位撞开","提示信息 "]
["PLC_ALL_Config_8220 ",601503,"KEB变桨3号桨叶齿轮箱变比校验异常","告警信息 "]
["PLC_ALL_Config_8220 ",601551,"KEB2号桨叶电机抱闸打开","提示信息 "]
["PLC_ALL_Config_8220 ",601576,"KEB1号桨叶91°限位开关位置偏差报警","故障 "]
["PLC_ALL_Config_8220 ",601597,"KEB3号电机刹车断线故障","故障 "]
["PLC_ALL_Config_8220 ",601600,"KEB3号电机动力线断线故障","故障 "]
["PLC_ALL_Config_8220 ",601625,"KEB3号桨叶后备电源充电故障自恢复失败","故障 "]
["PLC_ALL_Config_8220 ",601655,"变桨400V电源故障回桨","告警信息 "]
["PLC_ALL_Config_8220 ",601676,"SSB3号轴控柜内接触器3Q1的吸合次数超过了设计寿命报警","提示信息 "]
["PLC_ALL_Config_8220 ",601683,"SSB系统400V进线主接触器2Q1的吸合次数超过了设计寿命报警","提示信息 "]
["PLC_ALL_Config_8220 ",601704,"主控发出了SSB变桨系统应急模式命令","提示信息 "]
["PLC_ALL_Config_8220 ",601729,"SSB3号变桨电机温度过低","故障 "]
["PLC_ALL_Config_8220 ",601750,"SSB3号桨叶超级电容需要维护","提示信息 "]
["PLC_ALL_Config_8220 ",601753,"SSB3号桨叶后备电源内阻过大报警","告警信息 "]
["PLC_ALL_Config_8220 ",601778,"SSB2号桨叶驱动器出现通讯故障","故障 "]
["PLC_ALL_Config_8220 ",601799,"SSB 变桨处于特殊模式，响应特殊位置回桨走桨","提示信息 "]
["PLC_ALL_Config_8220 ",601821,"SSB3号轴控柜内1F1跳开故障故障","故障 "]
["PLC_ALL_Config_8220 ",601828,"SSB2号桨叶后备电源电压过高故障故障","故障 "]
["PLC_ALL_Config_8220 ",601849,"变桨安全位置与主控设置不匹配","故障 "]
["PLC_ALL_Config_8220 ",604074,"主轴承润滑系统工作时检测打泵脉冲超时","提示信息 "]
["PLC_ALL_Config_8220 ",606087,"发电机出风阀空开跳开","故障 "]
["PLC_ALL_Config_8220 ",606090,"发电机出风阀控制进入手动模式","提示信息 "]
["PLC_ALL_Config_8220 ",610005,"偏航接触器不正常报警","告警信息 "]
["PLC_ALL_Config_8220 ",612311,"等待变频器网侧就绪超时","故障 "]
["PLC_ALL_Config_8220 ",612845,"ABB变频器网侧模块风扇故障自恢复失败","故障 "]
["PLC_ALL_Config_8220 ",612866,"ABB变频器网侧主回路连接异常自恢复失败","故障 "]
["PLC_ALL_Config_8220 ",619001,"停机自复位中","提示信息 "]
["PLC_ALL_Config_8220 ",621052,"V柜断路器合闸","提示信息 "]
["PLC_ALL_Config_8220 ",621073,"C2柜负荷开关控制合闸","提示信息 "]
["PLC_ALL_Config_8220 ",621107,"开关柜V柜断开主断路器强制模式","提示信息 "]
["PLC_ALL_Config_8220 ",1005003,"齿轮箱变速风冷风扇强制启动","提示信息 "]
["PLC_ALL_Config_8220 ",1010003,"偏航系统7号电机PTC测温电阻触发","告警信息 "]
["PLC_ALL_Config_8220 ",1010010,"8#偏航电机空开跳开","故障 "]
["PLC_ALL_Config_8220 ",1012013,"变频器故障","告警信息 "]
["PLC_ALL_Config_8220 ",1021005,"动力电缆温度高停机","故障 "]
["PLC_ALL_Config_8220 ",1025025,"独立变桨控制传感器4故障超时","故障 "]
["SSD24 ",10103,"机舱左右加速度二级超限","故障 "]
["SSD24 ",10110,"机组1P过大","告警信息 "]
["SSD24 ",20021,"并网时能量不足","故障 "]
["SSD24 ",30102,"变流器内部通迅故障","故障 "]
["SSD24 ",30111,"变流器网侧C相过流","故障 "]
["SSD24 ",30136,"变流器机侧模块接地或电流不平衡","故障 "]
["SSD24 ",30202,"备留","提示信息 "]
["SSD24 ",30610,"备留","提示信息 "]
["SSD24 ",30901,"备留","提示信息 "]
["SSD24 ",30908,"备留","提示信息 "]
["SSD24 ",50020,"液压油油位低","故障 "]
["SSD24 ",50069,"备留","提示信息 "]
["SSD24 ",60010,"偏航速度过低","故障 "]
["SSD24 ",60915,"偏航电机3断路器故障","故障 "]
["SSD24 ",70017,"发电机u1相绕组温度报警","告警信息 "]
["SSD24 ",70203,"发电机滑环风扇保护故障","告警信息 "]
["SSD24 ",80014,"齿轮箱入口油温超限","故障 "]
["SSD24 ",80072,"齿轮箱润滑油泵马达保护","故障 "]
["SSD24 ",80307,"备留","提示信息 "]
["SSD24 ",100113,"电网C相电压高于上限值","故障 "]
["SSD24 ",100213,"电网C相电流高于上限值","故障 "]
["SSD24 ",100806,"备留","提示信息 "]
["SSD24 ",130101,"塔底控制柜UPS电池故障","告警信息 "]
["SSD24 ",160072,"备留","提示信息 "]
["SSD24 ",170051,"风向标1故障1(120s延时)","告警信息 "]
["SSD24 ",170058,"风向标故障","故障 "]
["SSD24 ",170605,"机舱主控柜消防喷放反馈","故障 "]
["SSD24 ",190070,"备留","提示信息 "]
["SSD24 ",200010,"读写StatusCodeXML错误","告警信息 "]
["SSD24 ",220021,"SCADA复位按钮故障","故障 "]
["SSD24 ",230113,"备留","提示信息 "]
["SSD24 ",260017,"备留","提示信息 "]
["SSD24 ",290005,"主轴承润滑间隔时间过长报警","告警信息 "]
["SSD24 ",290076,"偏航轴承润滑间隔时间过长","告警信息 "]
["SSD24 ",300125,"变桨轴2 DC-DC开关电源故障","故障 "]
["SSD24 ",300336,"变桨轴3后备电源未充满","故障 "]
["SSD24 ",300401,"轴1冷却风扇及加热器断路器断开","故障 "]
["SSD24 ",300683,"轴3实际桨距角与设定值偏差超限","故障 "]
["SSD24 ",300951,"变桨轴1电容模块过压","故障 "]
["SSD24 ",300972,"变桨控制器初始化参数故障","故障 "]
["SSD24 ",301000,"备留","提示信息 "]
["SSD24 ",301107,"变桨中央接口模块DC/DC控制器A3故障","故障 "]
["SSD24 ",301308,"备留","提示信息 "]
["SSD24 ",301603,"备留","提示信息 "]
["SSD24 ",301606,"备留","提示信息 "]
["SSD24 ",320001,"变压器温度超限","故障 "]
["SSD24 ",350005,"塔底出风口风扇保护","故障 "]
["SSD24 ",650008,"备留","提示信息 "]
["SSD24 ",800003,"机舱远程紧停开关触发","提示信息 "]
["SSD24 ",800030,"变频器紧停","故障 "]
["SSD24 ",900201,"机舱DI9371-01模块故障","故障 "]
["SSD24 ",900264,"机舱AT4222-04模块故障","故障 "]
["SSD24 ",900271,"机舱总线控制器模块故障","故障 "]
["SSD24 ",900503,"驱动器1故障","告警信息 "]
["SSD24 ",990204,"低桨叶角功率超限","故障 "]
["SGW53 ",2,"机舱位移超限","故障 "]
["SGW53 ",11,"低压电气柜温度高","故障 "]
["SGW53 ",33,"(33)电网电压极高故障","故障 "]
["SGW53 ",54,"woodward 电能值警告","告警信息 "]
["SGW53 ",79,"(79)水冷UPS故障","故障 "]
["SGW53 ",82,"变流器熔断器反馈丢失","故障 "]
["SGW53 ",105,"10 号子站电源故障","故障 "]
["SGW53 ",132,"风速转速不匹配故障","故障 "]
["SGW53 ",160,"1 号变桨软件不匹配","故障 "]
["SGW53 ",167,"2 号安全链 OK 变桨内丢失","故障 "]
["SGW53 ",188,"2 号变桨电机温度低","故障 "]
["SGW53 ",209,"2 号减速比选择错误","故障 "]
["SGW53 ",234,"3#变桨内部通讯中断","故障 "]
["SGW53 ",237,"3#变桨设定和实际角度偏差大","故障 "]
["SGW53 ",258,"3#变桨备电电容电压低","故障 "]
["SGW53 ",283,"2#变桨电机刹车电流大时间长","故障 "]
["SGW53 ",304,"3#变桨电机电流过大","故障 "]
["SGW53 ",311,"1 号变桨速度超限","故障 "]
["SGW53 ",337,"3#变频器 PLC 激活故障","故障 "]
["SGW53 ",358,"3#变桨过压警告","故障 "]
["SGW53 ",383,"1#变桨直流回路供电断故障","故障 "]
["SGW53 ",386,"1#变桨 91°限位开关触发故障","故障 "]
["SGW53 ",411,"变桨运行模式故障","故障 "]
["SGW53 ",501,"触发反馈丢失","故障 "]
["SGW53 ",522,"斩波升压 IGBT3 温度高","故障 "]
["SGW53 ",529,"直流电流高","故障 "]
["SGW53 ",550,"3#变桨散热器风扇警告","告警信息 "]
["SGW53 ",571,"3#变桨电容极性故障","故障 "]
["SGW53 ",596,"1#变桨预充电故障","故障 "]
["SGW53 ",599,"1#变桨总线急停","故障 "]
["SGW53 ",624,"2#变桨 SACB 故障","故障 "]
["SGW53 ",645,"3#变桨散热片过温","故障 "]
["SGW54 ",4,"停机及停机过程加速度超限","告警信息 "]
["SGW54 ",11,"低压电气柜温度高","告警信息 "]
["SGW54 ",32,"发电机绕组温升高","故障 "]
["SGW54 ",57,"转速比较2","故障 "]
["SGW54 ",78,"机舱控制柜UPS进入电池模式","告警信息 "]
["SGW54 ",81,"机舱熔断器反馈丢失","故障 "]
["SGW54 ",108,"水冷子站电源异常","故障 "]
["SGW54 ",131,"风向标工作异常","故障 "]
["SGW54 ",158,"2#变桨最小角度超限","故障 "]
["SGW54 ",165,"2#变桨发电位置传感器异常","故障 "]
["SGW54 ",186,"3#变桨电机温度高","故障 "]
["SGW54 ",211,"1#变桨电容高电压高","故障 "]
["SGW54 ",232,"1#变桨内部通讯中断","故障 "]
["SGW54 ",235,"1#变桨设定和实际角度偏差大","故障 "]
["SGW54 ",260,"2#变桨91°限位开关触发","故障 "]
["SGW54 ",281,"变桨24VDC UPS故障","故障 "]
["SGW54 ",302,"1#变桨电机电流过大","故障 "]
["SGW54 ",309,"2#主副编码器位置偏差大","故障 "]
["SGW54 ",335,"1#变频器PLC激活异常","故障 "]
["SGW54 ",360,"2#变桨欠压","故障 "]
["SGW54 ",381,"2#变桨230VAC和400VAC供电断开","故障 "]
["SGW54 ",384,"2#变桨直流回路供电断开","故障 "]
["SGW54 ",409,"3#变桨主副旋编位置偏差大","故障 "]
["SGW54 ",496,"变流器反馈丢失","故障 "]
["SGW54 ",503,"IGBT_ok丢失","故障 "]
["SGW54 ",524,"制动IGBT温度高","故障 "]
["SGW54 ",545,"1#变桨内部风扇异常","故障 "]
["SGW54 ",570,"2#变桨电容极性错误","故障 "]
["SGW54 ",591,"2#变桨位置比较偏差大","故障 "]
["SGW54 ",594,"2#变桨内部总线异常","故障 "]
["SGW54 ",619,"3#变桨电机温度高","故障 "]
["SGW54 ",640,"1#变桨电容电压低","故障 "]
["SGW54 ",647,"2#变桨电机温度高","故障 "]
["SGW54 ",673,"机侧L3b_IGBT温度高","故障 "]
["SGW54 ",700,"变流器现场总线异常","故障 "]
["SGW54 ",725,"变流器准备信号异常","故障 "]
["SGW54 ",746,"箱变水冷循环泵出口压力超高","故障 "]
["SGW54 ",749,"箱变水冷水冷流量低","故障 "]
["SGW54 ",779,"发电机定子温度变化率异常","告警信息 "]
["SGW54 ",800,"OverSpeed1转速异常","告警信息 "]
["SGW54 ",808,"雷达测风异常","故障 "]
["SGW54 ",882,"变流器机侧IGBT9_L2A过流","故障 "]
["SGW54 ",903,"变流器机侧IGBT10_L3A过温","故障 "]
["SGW54 ",943,"变流器母线电压过高(硬件)","故障 "]
["SGW54 ",980,"变流控制器故障10","故障 "]
["SGW54 ",992,"变流器电网电压高(硬件)","故障 "]
["SGW54 ",1014,"变流器低电压穿越超时","故障 "]
["SHZ22 ",119,"NV文件不存在警告","告警信息 "]
["SHZ22 ",126,"系统启动错误（WTC系统错误）","故障 "]
["SHZ22 ",149,"IO关联警告","告警信息 "]
["SHZ22 ",1020,"齿轮箱出口油压高故障","故障 "]
["SHZ22 ",2025,"机舱集中润滑油位低警告","告警信息 "]
["SHZ22 ",3007,"主轴后轴承温度2高警告","告警信息 "]
["SHZ22 ",4003,"1#叶片变桨没有心跳故障","故障 "]
["SHZ22 ",4024,"变桨3#叶片机舱维护模式激活故障","故障 "]
["SHZ22 ",4045,"变桨3桨叶角度过大故障","故障 "]
["SHZ22 ",4052,"变桨1#LVRT超时故障","故障 "]
["SHZ22 ",4073,"变桨2后备电源过压故障","故障 "]
["SHZ22 ",4098,"变桨叶片3MPC输出错误","故障 "]
["SHZ22 ",4119,"变桨叶片3刹车电阻过载故障","故障 "]
["SHZ22 ",4140,"变桨2控制柜超温警告","告警信息 "]
["SHZ22 ",4147,"变桨3电机超温警告","告警信息 "]
["SHZ22 ",4168,"变桨3#叶片电容当前容量低警告","告警信息 "]
["SHZ22 ",5011,"发电机绕组U2温度警告","告警信息 "]
["SHZ22 ",5018,"发电机滑环超温故障","故障 "]
["SHZ22 ",11012,"变流器LVRT激活","故障 "]
["SHZ22 ",11037,"变流器有功AI给定异常警告","告警信息 "]
["SHZ22 ",12011,"转子刹车未释放故障 ","故障 "]
["SHZ22 ",13015,"机舱振动10分钟平均值超限故障","故障 "]
["SHZ22 ",15000,"塔基690V防雷保护故障","故障 "]
["SHZ22 ",16005,"风速太高禁止维护警告","告警信息 "]
["SHZ22 ",19007,"停机顺序不成功故障","故障 "]
["SHZ22 ",20003,"机舱温度高故障","故障 "]
["SHZ22 ",21017,"电网V相辅助电压严重过高故障","故障 "]
["SHZ22 ",28004,"塔基自动消防故障","故障 "]
["SGW59 ",16,"预留","提示信息 "]
["SGW59 ",37,"电网电压不平衡","故障 "]
["SGW59 ",44,"预留","提示信息 "]
["SGW59 ",65,"发电机温度比较偏差大","故障 "]
["SGW59 ",90,"塔底急停按钮动作","提示信息 "]
["SGW59 ",93,"振动开关动作","提示信息 "]
["SGW59 ",114,"润滑加脂子站熔断器异常","故障 "]
["SGW59 ",139,"预留","提示信息 "]
["SGW59 ",160,"预留","提示信息 "]
["SGW59 ",181,"1#变桨旋编电池电压低","故障 "]
["SGW59 ",188,"2#变桨电机温度低","故障 "]
["SGW59 ",209,"预留","提示信息 "]
["SGW59 ",234,"预留","提示信息 "]
["SGW59 ",237,"1#变桨防雷模块异常","故障 "]
["SGW59 ",258,"预留","提示信息 "]
["SGW59 ",283,"水冷加热器异常","故障 "]
["SGW59 ",304,"变流器调制后rdy_ref丢失","故障 "]
["SGW59 ",325,"预留","提示信息 "]
["SGW59 ",332,"预留","提示信息 "]
["SGW59 ",353,"预留","提示信息 "]
["SGW59 ",378,"预留","提示信息 "]
["SGW59 ",381,"预留","提示信息 "]
["SGW59 ",402,"风向标1异常","故障 "]
["SGW59 ",427,"机舱加速度变化率异常","故障 "]
["SGW59 ",453,"(453)发电机前轴承温度1变化率异常","故障 "]
["SGW59 ",460,"(460)发电机后轴承外圈温度变化率异常","故障 "]
["SGW59 ",534,"(534)箱变水冷循环泵出口温度低","故障 "]
["SGW59 ",555,"(555)箱变油温传感器异常","故障 "]
["SGW59 ",762,"(762)过速继电器检测发电机过速","故障 "]
["SGW59 ",767,"(767)发电机后轴承内外圈温差大","故障 "]
["SGW59 ",1001,"1U1_软件直流过压","故障 "]
["SGW59 ",1026,"2U1_A相软件过流","故障 "]
["SGW59 ",1047,"1U2_STACK2_C相软件过流","故障 "]
["SGW59 ",1054,"2U1_STACK1_A相软件过流","故障 "]
["SGW59 ",1075,"2U1_频率高","故障 "]
["SGW59 ",1096,"1U1_STACK1硬件直流过压","故障 "]
["SGW59 ",1121,"1U2_STACK2硬件过流","故障 "]
["SGW59 ",1124,"1U4_STACK1硬件过流","故障 "]
["SGW59 ",1149,"1U1_直流熔断器1异常","故障 "]
["SGW59 ",1170,"2U2_直流熔断器2异常","故障 "]
["SGW59 ",1191,"1U3_C相驱动异常","故障 "]
["SGW59 ",1198,"2U2_B相驱动异常","故障 "]
["SGW59 ",1219,"1U3_STACK1_C相驱动异常","故障 "]
["SGW59 ",1240,"2U3_STACK2_C相驱动异常","故障 "]
["SGW59 ",1265,"1U4_IGBT软件过温","故障 "]
["SGW59 ",1268,"2U3_IGBT软件过温","故障 "]
["SGW59 ",1293,"1U4_STACK2_IGBT软件过温","故障 "]
["SGW59 ",1314,"1U3_IGBT13_过温","故障 "]
["SGW59 ",1335,"2U4_取能板异常","故障 "]
["SGW59 ",1342,"1U2_断路器断开","故障 "]
["SGW59 ",1363,"1U4_制动回路异常","故障 "]
["SGW59 ",1384,"2U1_相序错误","故障 "]
["SGW59 ",1409,"2U1_CAN网络通讯异常","故障 "]
["SGW59 ",1412,"2U4_CAN网络通讯异常","故障 "]
["SGW59 ",1437,"2U4_Sport1_通讯异常","故障 "]
["SGW59 ",1458,"2U1_驱动控制器光纤通讯异常","故障 "]
["SGW59 ",1479,"R-Safe启动异常","故障 "]
["SGW59 ",1486,"(1486)2U2直流母线电压瞬时值超限","故障 "]
["SGW59 ",1507,"1U1_频率低","故障 "]
["SGW59 ",1532,"2U4_STACK1_IGBT软件过温","故障 "]
["SGW59 ",1553,"1U2_IGBT8温度高","故障 "]
["SGW59 ",1556,"1U3_IGBT11温度高","故障 "]
["SGW59 ",1581,"2U3_频率高","故障 "]
["SGW59 ",1602,"2U3_STACK1_过载","故障 "]
["SGW59 ",1623,"2U1_STACK1/STACK2不均流","故障 "]
["SGW59 ",1630,"1#柜电抗器过温","故障 "]
["SGW59 ",1651,"开关柜1环境温度高","故障 "]
["SGW59 ",1676,"正常停机预留_18","提示信息 "]
["SGW59 ",1697,"预留","提示信息 "]
["SGW59 ",1700,"预留","提示信息 "]
["SGW59 ",1725,"1U2_版本校验错误","故障 "]
["SGW59 ",1746,"(1746)1U2机侧过压过流模块状态异常","故障 "]
["SGW59 ",1771,"2U1电网频率低异常提示","故障 "]
["SGW59 ",1774,"1U2 STACK1三相电流不平衡异常提示","故障 "]
["SGW59 ",1795,"2U1_IGBT软件温度低","故障 "]
["SGW59 ",1820,"1U2_STACK2_三相电流不平衡","故障 "]
["SGW59 ",1841,"1U3_STACK2_过载","故障 "]
["SGW59 ",1844,"2U1_STACK2_过载","故障 "]
["SGW59 ",1869,"Rsafe_预留9","提示信息 "]
["SGW59 ",1890,"(1890)指令异常","故障 "]
["SGW59 ",1921,"(1921)2U1_网侧电压谐波高","故障 "]
["SGW59 ",1924,"(1924)2U3_发电机转速波动异常","故障 "]
["SGW59 ",2708,"(2708)转速异常震荡","故障 "]
["SGW59 ",2733,"(2733)1#变桨柜温度变化率异常","故障 "]
["SGW59 ",3016,"预留报警","提示信息 "]
["SGW59 ",3019,"预留报警","提示信息 "]
["SGW59 ",3044,"预留报警","提示信息 "]
["SGW59 ",3065,"发电机温度比较偏差大报警","告警信息 "]
["SGW59 ",3090,"塔底急停按钮动作报警","告警信息 "]
["SGW59 ",3093,"振动开关动作报警","告警信息 "]
["SGW59 ",3114,"润滑加脂子站熔断器异常报警","告警信息 "]
["SGW59 ",3139,"预留报警","提示信息 "]
["SGW59 ",3160,"预留报警","提示信息 "]
["SGW59 ",3167,"2#变桨外部安全链信号异常报警","告警信息 "]
["SGW59 ",3188,"2#变桨电机温度低报警","告警信息 "]
["SGW59 ",3209,"预留报警","提示信息 "]
["SGW59 ",3234,"预留报警","提示信息 "]
["SGW59 ",3237,"1#变桨防雷模块异常报警","告警信息 "]
["SGW59 ",3258,"预留报警","提示信息 "]
["SGW59 ",3283,"水冷加热器异常报警","告警信息 "]
["SGW59 ",3304,"变流器调制后rdy_ref丢失报警","告警信息 "]
["SGW59 ",3311,"变流器柜体温度高报警","告警信息 "]
["SGW59 ",3332,"预留报警","提示信息 "]
["SGW59 ",3353,"预留报警","提示信息 "]
["SGW59 ",3378,"预留报警","提示信息 "]
["SGW59 ",3381,"预留报警","提示信息 "]
["SGW59 ",3402,"风向标1异常报警","告警信息 "]
["SGW59 ",3418,"水冷出阀温度变化率异常报警","告警信息 "]
["SGW59 ",3452,"(452)发电机定子温度变化率异常报警","告警信息 "]
["SGW59 ",3459,"(459)发电机后轴承内圈温度变化率异常报警","告警信息 "]
["SGW59 ",3533,"(533)箱变水冷循环泵出口温度高报警","告警信息 "]
["SGW59 ",3554,"(554)箱变水冷压力传感器比较异常报警","告警信息 "]
["SGW59 ",3761,"(761)轮毂散热风扇工作异常报警","告警信息 "]
["SGW59 ",3766,"(766)发电机前轴承内外圈温差大报警","告警信息 "]
["SGW59 ",4004,"1U4_软件直流过压报警","告警信息 "]
["SGW59 ",4025,"1U3_C相软件过流报警","告警信息 "]
["SGW59 ",4046,"1U2_STACK2_B相软件过流报警","告警信息 "]
["SGW59 ",4053,"1U3_STACK2_C相软件过流报警","告警信息 "]
["SGW59 ",4074,"1U1_频率高报警","告警信息 "]
["SGW59 ",4095,"2U4_硬件直流过压报警","告警信息 "]
["SGW59 ",4120,"1U2_STACK1硬件过流报警","告警信息 "]
["SGW59 ",4123,"1U3_STACK2硬件过流报警","告警信息 "]
["SGW59 ",4148,"2U1_交流熔断器异常报警","告警信息 "]
["SGW59 ",4169,"2U2_直流熔断器1异常报警","告警信息 "]
["SGW59 ",4190,"1U3_B相驱动异常报警","告警信息 "]
["SGW59 ",4197,"2U2_A相驱动异常报警","告警信息 "]
["SGW59 ",4218,"1U3_STACK1_B相驱动异常报警","告警信息 "]
["SGW59 ",4243,"1U1_GBT3_驱动异常报警","告警信息 "]
["SGW59 ",4264,"1U3_IGBT软件过温报警","告警信息 "]
["SGW59 ",4267,"2U2_IGBT软件过温报警","告警信息 "]
["SGW59 ",4292,"1U4_STACK1_IGBT软件过温报警","告警信息 "]
["SGW59 ",4313,"1U3_IGBT12_过温报警","告警信息 "]
["SGW59 ",4334,"2U3_取能板异常报警","告警信息 "]
["SGW59 ",4341,"1U2_断路器闭合报警","告警信息 "]
["SGW59 ",4362,"2U4_制动超时报警","告警信息 "]
["SGW59 ",4387,"1U3_相序错误报警","告警信息 "]
["SGW59 ",4408,"1U4_CAN网络通讯异常报警","告警信息 "]
["SGW59 ",4411,"2U3_CAN网络通讯异常报警","告警信息 "]
["SGW59 ",4436,"2U3_Sport1_通讯异常报警","告警信息 "]
["SGW59 ",4457,"1U4_驱动控制器光纤通讯异常报警","告警信息 "]
["SGW59 ",4478,"主控急停触发报警","告警信息 "]
["SGW59 ",4485,"(1485)2U1直流母线电压瞬时值超限报警","告警信息 "]
["SGW59 ",4506,"2U1_频率高报警","告警信息 "]
["SGW59 ",4531,"2U3_STACK2_IGBT软件过温报警","告警信息 "]
["SGW59 ",4552,"1U4_IGBT7温度高报警","告警信息 "]
["SGW59 ",4555,"1U2_IGBT10温度高报警","告警信息 "]
["SGW59 ",4580,"2U2_频率高报警","告警信息 "]
["SGW59 ",4601,"2U3_过载报警","告警信息 "]
["SGW59 ",4608,"1U2_三相电流不平衡报警","告警信息 "]
["SGW59 ",4629,"无功功率比较报警","告警信息 "]
["SGW59 ",4650,"功率柜2环境温度高报警","告警信息 "]
["SGW59 ",4675,"正常停机预留_17报警","提示信息 "]
["SGW59 ",4696,"预留报警","提示信息 "]
["SGW59 ",4699,"预留报警","提示信息 "]
["SGW59 ",4724,"1U1_版本校验错误报警","告警信息 "]
["SGW59 ",4745,"(1745)2U3机侧断路器反馈异常报警","告警信息 "]
["SGW59 ",4752,"警示预留_13报警","提示信息 "]
["SGW59 ",4773,"1U2 三相电流不平衡异常提示报警","告警信息 "]
["SGW59 ",4794,"1U4_IGBT软件温度低报警","告警信息 "]
["SGW59 ",4819,"1U2_STACK1_三相电流不平衡报警","告警信息 "]
["SGW59 ",4840,"1U3_STACK1_过载报警","告警信息 "]
["SGW59 ",4847,"2U2_STACK2_过载报警","告警信息 "]
["SGW59 ",4868,"Rsafe_预留8报警","提示信息 "]
["SGW59 ",4889,"(1889)主柜运行模式错误报警","告警信息 "]
["SGW59 ",4896,"(1896)1U4参数错误报警","告警信息 "]
["SGW59 ",4923,"(1923)1U3_发电机转速波动异常报警","告警信息 "]
["SGW59 ",5707,"(2707)叶轮平面模态异常振动报警","告警信息 "]
["SGW59 ",5732,"(2732)发电机散热风道温度变化率异常报警","告警信息 "]
["SGW32 ",13,"偏航齿轮加脂油路堵塞","故障 "]
["SGW32 ",20,"建压时间长","故障 "]
["SGW32 ",41,"电网频率低","故障 "]
["SGW32 ",62,"维护状态发电机转速超限","故障 "]
["SGW32 ",69,"发电机主轴润滑分配器堵塞","故障 "]
["SGW32 ",90,"塔底急停按钮动作","提示信息 "]
["SGW32 ",111,"机舱子站熔断器异常","故障 "]
["SGW32 ",136,"预留","提示信息 "]
["SGW32 ",157,"1#变桨最小角度超限","故障 "]
["SGW32 ",164,"2#变桨发电位置传感器异常","故障 "]
["SGW32 ",185,"2#变桨电机温度高","故障 "]
["SGW32 ",206,"2#变桨逆变器温度低","故障 "]
["SGW32 ",213,"3#变桨电容电压高(国产)","故障 "]
["SGW32 ",234,"预留","提示信息 "]
["SGW32 ",259,"预留","提示信息 "]
["SGW32 ",280,"预留","提示信息 "]
["SGW32 ",301,"变流器调制前rdy_run丢失","故障 "]
["SGW32 ",308,"网侧电抗器1温度高","故障 "]
["SGW32 ",329,"预留","提示信息 "]
["SGW32 ",350,"预留","提示信息 "]
["SGW32 ",357,"预留","提示信息 "]
["SGW32 ",378,"预留","提示信息 "]
["SGW32 ",403,"风向标2异常","故障 "]
["SGW32 ",424,"机舱控制柜温度变化率异常","故障 "]
["SGW32 ",446,"塔架频率偏低","故障 "]
["SGW32 ",743,"(743)载荷测量单元通讯异常","故障 "]
["SGW32 ",1010,"1U2_软件直流欠压","故障 "]
["SGW32 ",1031,"2U2_C相软件过流","故障 "]
["SGW32 ",1038,"1U1_STACK1_C相软件过流","故障 "]
["SGW32 ",1059,"2U1_STACK2_C相软件过流","故障 "]
["SGW32 ",1084,"网侧功率低1","故障 "]
["SGW32 ",1105,"2U1_STACK2硬件直流过压","故障 "]
["SGW32 ",1126,"2U1_STACK1硬件过流","故障 "]
["SGW32 ",1133,"2U4_STACK2硬件过流","故障 "]
["SGW32 ",1154,"1U2_直流熔断器2异常","故障 "]
["SGW32 ",1179,"2U4_直流熔断器3异常","故障 "]
["SGW32 ",1182,"2U1_滤波电容熔断器异常","故障 "]
["SGW32 ",1203,"2U4_驱动1异常","故障 "]
["SGW32 ",1228,"2U1_STACK2_C相驱动异常","故障 "]
["SGW32 ",1249,"1U2_ IGBT9_驱动异常","故障 "]
["SGW32 ",1270,"1U1_STACK1_IGBT硬件过温","故障 "]
["SGW32 ",1277,"1U4_STACK2_IGBT硬件过温","故障 "]
["SGW32 ",1298,"2U3_STACK1_IGBT软件过温","故障 "]
["SGW32 ",1323,"1#柜24V开关电源1保护","故障 "]
["SGW32 ",1326,"2#柜24V开关电源2保护","故障 "]
["SGW32 ",1347,"2U3_断路器闭合","故障 "]
["SGW32 ",1372,"1U2_STACK1_Sum","故障 "]
["SGW32 ",1393,"1U3_零序电流保护","故障 "]
["SGW32 ",1400,"1U2_缺相","故障 "]
["SGW32 ",1421,"2U4_FPGA通讯校验错误","故障 "]
["SGW32 ",1442,"2U1_以太网通讯异常","故障 "]
["SGW32 ",1467,"1U4_安全链反馈异常","故障 "]
["SGW32 ",1470,"2U3_安全链反馈异常","故障 "]
["SGW32 ",1491,"(1491)电网电压高超时故障1","故障 "]
["SGW32 ",1516,"2U1_电压不平衡","故障 "]
["SGW32 ",1537,"1U2_STACK2_IGBT软件温度低","故障 "]
["SGW32 ",1544,"2U3_STACK1_IGBT软件温度低","故障 "]
["SGW32 ",1565,"2U3_膜电容过温","故障 "]
["SGW32 ",1586,"1U1_过载","故障 "]
["SGW32 ",1611,"1U3_三相电流不平衡","故障 "]
["SGW32 ",1614,"2U2_三相电流不平衡","故障 "]
["SGW32 ",1635,"2#整流柜环境温度高","故障 "]
["SGW32 ",1660,"(1660)网侧功率B相模块温度异常","故障 "]
["SGW32 ",1681,"1U1电网电压低","故障 "]
["SGW32 ",1688,"2U1电网电压低","故障 "]
["SGW32 ",1709,"逆变柜除湿器反馈异常","故障 "]
["SGW32 ",1730,"2U3_版本校验错误","故障 "]
["SGW32 ",1755,"警示预留_16","提示信息 "]
["SGW32 ",1758,"警示预留_19","提示信息 "]
["SGW32 ",1783,"2U2 STACK2三相电流不平衡异常提示","故障 "]
["SGW32 ",1804,"1U3_STACK2_IGBT软件低温","故障 "]
["SGW32 ",1825,"2U1_STACK1_三相电流不平衡","故障 "]
["SGW32 ",1832,"2U3_STACK2_三相电流不平衡","故障 "]
["SGW32 ",1852,"1U2_STACK1/STACK2不均流","故障 "]
["SGW32 ",1873,"降功率运行_预留3","提示信息 "]
["SGW32 ",3018,"偏航方向异常警告","告警信息 "]
["SGW32 ",3021,"液压泵无反馈警告","告警信息 "]
["SGW32 ",3046,"变流器功率与上网功率不匹配警告","告警信息 "]
["SGW32 ",3067,"发电机主轴加脂油位低警告","告警信息 "]
["SGW32 ",3088,"变流安全链触发警告","告警信息 "]
["SGW32 ",3095,"变桨安全链触发警告","告警信息 "]
["SGW32 ",3116,"预留","提示信息 "]
["SGW32 ",3137,"预留","提示信息 "]
["SGW32 ",3162,"预留","提示信息 "]
["SGW32 ",3165,"3#变桨发电位置传感器异常警告","告警信息 "]
["SGW32 ",3190,"1#变桨电容温度高警告","告警信息 "]
["SGW32 ",3211,"1#变桨电容电压高(国产)警告","告警信息 "]
["SGW32 ",3232,"3#变桨心跳信号丢失警告","告警信息 "]
["SGW32 ",3239,"3#变桨防雷模块异常警告","告警信息 "]
["SGW32 ",3260,"水冷散热器风扇异常个数超限警告","告警信息 "]
["SGW32 ",3285,"预留","提示信息 "]
["SGW32 ",3306,"电机1侧逆变器温度高警告","告警信息 "]
["SGW32 ",3309,"网侧电抗器2温度高警告","告警信息 "]
["SGW32 ",3334,"预留","提示信息 "]
["SGW32 ",3355,"预留","提示信息 "]
["SGW32 ",3376,"预留","提示信息 "]
["SGW32 ",3383,"预留","提示信息 "]
["SGW32 ",3404,"凸轮与接近开关偏航位置差值大警告","告警信息 "]
["SGW32 ",3429,"机舱温度与环境温度反接警告","告警信息 "]
["SGW32 ",3741,"（3741)叶轮方位角测量异常警告","故障 "]
["SGW32 ",3744,"(3744)雷达硬件异常警告","告警信息 "]
["SGW32 ",4015,"2U3_软件直流欠压警告","告警信息 "]
["SGW32 ",4036,"1U1_STACK1_A相软件过流警告","告警信息 "]
["SGW32 ",4043,"1U2_STACK1_B相软件过流警告","告警信息 "]
["SGW32 ",4064,"2U2_STACK2_B相软件过流警告","告警信息 "]
["SGW32 ",4085,"1U1_三相电压不平衡警告","告警信息 "]
["SGW32 ",4110,"2U4_STACK1硬件直流过压警告","告警信息 "]
["SGW32 ",4131,"2U3_STACK2硬件过流警告","告警信息 "]
["SGW32 ",4134,"1U1_IGBT1硬件过流警告","告警信息 "]
["SGW32 ",4159,"1U3_直流熔断器3异常警告","告警信息 "]
["SGW32 ",4180,"2U4_直流熔断器4异常警告","告警信息 "]
["SGW32 ",4187,"1U2_B相驱动异常警告","告警信息 "]
["SGW32 ",4208,"1U1_STACK2_A相驱动异常警告","告警信息 "]
["SGW32 ",4229,"2U2_STACK1_A相驱动异常警告","告警信息 "]
["SGW32 ",4254,"1U1_IGBT硬件过温警告","告警信息 "]
["SGW32 ",4275,"1U3_STACK2_IGBT硬件过温警告","告警信息 "]
["SGW32 ",4278,"2U1_STACK1_IGBT硬件过温警告","告警信息 "]
["SGW32 ",4303,"1U1_IGBT2_过温警告","告警信息 "]
["SGW32 ",4324,"1#柜24V开关电源2保护警告","告警信息 "]
["SGW32 ",4331,"1U3_取能板异常警告","告警信息 "]
["SGW32 ",4352,"1#柜预充电超时警告","告警信息 "]
["SGW32 ",4373,"1U3_STACK1_Sum警告","告警信息 "]
["SGW32 ",4398,"2U3_电压高警告","告警信息 "]
["SGW32 ",4419,"2U2_FPGA通讯校验错误警告","告警信息 "]
["SGW32 ",4426,"2U1_Sport0_通讯异常警告","告警信息 "]
["SGW32 ",4447,"1U2_DSP/FPGA通讯异常警告","告警信息 "]
["SGW32 ",4468,"2U1_安全链反馈异常警告","告警信息 "]
["SGW32 ",4475,"2U2_转矩异常警告","告警信息 "]
["SGW32 ",4496,"急停预留_16警告","提示信息 "]
["SGW32 ",4517,"电网异常警告","告警信息 "]
["SGW32 ",4542,"2U2_STACK1_IGBT软件温度低警告","告警信息 "]
["SGW32 ",4563,"2U1_膜电容过温警告","告警信息 "]
["SGW32 ",4570,"1U4_均流电抗器过温警告","告警信息 "]
["SGW32 ",4591,"2U1_STACK2_过载警告","告警信息 "]
["SGW32 ",4612,"1U3_STACK1_三相电流不平衡警告","告警信息 "]
["SGW32 ",4619,"2U3_STACK2_三相电流不平衡警告","告警信息 "]
["SGW32 ",4640,"IGBT柜1环境温度高警告","告警信息 "]
["SGW32 ",4665,"(4665)从柜TCC_产品配置错误警告","告警信息 "]
["SGW32 ",4686,"1U1电压不平衡警告","告警信息 "]
["SGW32 ",4707,"逆变柜离心风机反馈异常警告","告警信息 "]
["SGW32 ",4714,"IGBT柜2除湿器反馈异常警告","告警信息 "]
["SGW32 ",4735,"1U4_产品配置错误警告","告警信息 "]
["SGW32 ",4756,"警示预留_17警告","提示信息 "]
["SGW32 ",4763,"1U1电网电压高异常提示警告","告警信息 "]
["SGW32 ",4784,"2U2 STACK1与STACK2不均流异常提示警告","告警信息 "]
["SGW32 ",4809,"2U2_STACK1_IGBT软件低温警告","告警信息 "]
["SGW32 ",4830,"2U3_三相电流不平衡警告","告警信息 "]
["SGW32 ",4851,"1U1_STACK1/STACK2不均流警告","告警信息 "]
["SGW32 ",4858,"1U3频率高警告","告警信息 "]
["SGW32 ",4879,"降功率运行_预留9警告","提示信息 "]
["SYD11 ",1564,"振动模块2#通道1过振动报警","故障 "]
["SYD11 ",1577,"振动模块通道1超限","故障 "]
["SYD11 ",5013,"安全链复位按钮失效","故障 "]
["SYD11 ",5201,"舱外温度过低","故障 "]
["SYD11 ",5323,"30s平均风速1超限","提示信息 "]
["SYD11 ",5416,"桨叶2限位开关触发误报","故障 "]
["SYD11 ",5423,"桨叶3备用限位开关触发误报","故障 "]
["SYD11 ",5462,"桨叶10.5s平均桨距角超限","故障 "]
["SYD11 ",5490,"变桨2电机电流大","故障 "]
["SYD11 ",5493,"桨叶2400伏异常","故障 "]
["SYD11 ",5520,"偏航信号有误","故障 "]
["SYD11 ",5622,"齿轮箱润滑油进口油压告警","告警信息 "]
["SYD11 ",5722,"发电机润滑泵断路器跳闸","故障 "]
["SYD11 ",5906,"变流器低电压穿越禁止","告警信息 "]
["SYD11 ",5927,"转矩不匹配告警","告警信息 "]
["SYD11 ",5951,"变流器网侧过频","故障 "]
["SYD11 ",5976,"变流器主断路器反馈故障","故障 "]
["SYD11 ",5979,"变流器crowbar触发告警","告警信息 "]
["SYD11 ",6403,"系统初始化等待超时待机","故障 "]
["SYD11 ",6428,"等待发电机脱网超时待机","故障 "]
["SYD11 ",6511,"消防预警","告警信息 "]
["SYD11 ",7031,"电网电流不对称","故障 "]
["SYD11 ",15402,"桨叶1电容欠压","故障 "]
["SYD11 ",15433,"桨叶2桨叶位置值过小","故障 "]
["SYD11 ",15606,"桨叶1位置过大故障","故障 "]
["SYD11 ",15609,"桨叶1编码器卡件故障","故障 "]
["SYD11 ",15710,"桨叶2变桨电机超速","故障 "]
["SYD11 ",15817,"桨叶3超级电容模组中间点电压故障","故障 "]
["SYD11 ",40183,"模块1.2正常运行时间未发送","故障 "]
["SYD11 ",40200,"模块1.4故障","故障 "]
["SYD11 ",40511,"模块3.3状态故障","故障 "]
["SYD11 ",64016,"未知原因关机(OS)","故障 "]
["SSD41 ",10002,"机舱振动瞬时值超限","故障 "]
["SSD41 ",10021,"备留","提示信息 "]
["SSD41 ",10111,"机舱前后加速度传感器测量偏差过大","故障 "]
["SSD41 ",20038,"备留","提示信息 "]
["SSD41 ",30110,"变流器网侧B相过流","故障 "]
["SSD41 ",30117,"变流器硬件监测链路故障2","故障 "]
["SSD41 ",30144,"变流器未准备好","告警信息 "]
["SSD41 ",30301,"备留","提示信息 "]
["SSD41 ",30706,"备留","提示信息 "]
["SSD41 ",30709,"备留","提示信息 "]
["SSD41 ",31004,"备留","提示信息 "]
["SSD41 ",50039,"液压过滤器出口压力故障","故障 "]
["SSD41 ",60006,"偏航齿轮润滑不足","告警信息 "]
["SSD41 ",60201,"偏航制动保护","故障 "]
["SSD41 ",60921,"偏航电机9断路器故障","故障 "]
["SSD41 ",70026,"发电机后轴承温度报警","告警信息 "]
["SSD41 ",70304,"备留","提示信息 "]
["SSD41 ",70307,"备留","提示信息 "]
["SSD41 ",80092,"齿轮箱接油盘Pump油位报警","告警信息 "]
["SSD41 ",80313,"备留","提示信息 "]
["SSD41 ",100212,"电网B相电流高于上限值","故障 "]
["SSD41 ",100412,"电网10m平均有功功率超限","故障 "]
["SSD41 ",110102,"机舱柜子温度超限","故障 "]
["SSD41 ",130201,"塔底控制柜UPS供电异常","故障 "]
["SSD41 ",160001,"塔底400VAC供电保护","故障 "]
["SSD41 ",160095,"高压负荷开关分位","告警信息 "]
["SSD41 ",170202,"风力不足2","提示信息 "]
["SSD41 ",180002,"备留","提示信息 "]
["SSD41 ",200001,"写InitRun.txt文件出错","故障 "]
["SSD41 ",200021,"写StatusCounttxt文件出错","故障 "]
["SSD41 ",220042,"备留","提示信息 "]
["SSD41 ",250104,"备留","提示信息 "]
["SSD41 ",270022,"备留","提示信息 "]
["SSD41 ",270032,"备留","提示信息 "]
["SSD41 ",290081,"主轴单次润滑时间过长","告警信息 "]
["SSD41 ",300141,"变桨轴1后备电源柜温度超限","故障 "]
["SSD41 ",300348,"变桨轴2直流母线侧熔断器断开","故障 "]
["SSD41 ",300513,"变桨轴3电机温度超限","故障 "]
["SSD41 ",300692,"桨叶齿轮润滑出错","告警信息 "]
["SSD41 ",300956,"变桨轴3电容模块过温","故障 "]
["SSD41 ",300981,"变桨系统轴1预送电电抗器过温","故障 "]
["SSD41 ",300984,"变桨系统轴1驱动器内部风扇故障","故障 "]
["SSD41 ",301202,"PLC DI模块2故障","故障 "]
["SSD41 ",301403,"变桨齿轮周润滑次数不足","告警信息 "]
["SSD41 ",301604,"备留","提示信息 "]
["SSD41 ",301701,"备留","提示信息 "]
["SSD41 ",320006,"备留","提示信息 "]
["SSD41 ",350011,"塔底温度超限","故障 "]
["SSD41 ",700003,"风轮转速超速1","故障 "]
["SSD41 ",700007,"发电机漏水报警","告警信息 "]
["SSD41 ",800083,"SD1207超速紧停","故障 "]
["SSD41 ",900206,"机舱DI9371-06模块故障","故障 "]
["SSD41 ",900286,"机舱电源PS3300-01模块故障","故障 "]
["SSD41 ",900303,"轴柜3DI9371-1模块故障","告警信息 "]
["SSD41 ",900508,"机舱IF1061-1模块2故障","故障 "]
["SSD41 ",990209,"轴2实际桨距角与设定值偏差超限","故障 "]
["SGW33 ",7,"机舱控制柜温度高","故障 "]
["SGW33 ",10,"机舱温度低","故障 "]
["SGW33 ",35,"电网电压高","故障 "]
["SGW33 ",56,"转速比较1","故障 "]
["SGW33 ",81,"机舱熔断器反馈丢失","故障 "]
["SGW33 ",84,"叶轮锁定销未退出","故障 "]
["SGW33 ",105,"预留","提示信息 "]
["SGW33 ",130,"风速仪工作异常","故障 "]
["SGW33 ",151,"机舱除湿机工作异常","故障 "]
["SGW33 ",158,"2#变桨最小角度超限","故障 "]
["SGW33 ",179,"2#变桨安全位置传感器异常","故障 "]
["SGW33 ",200,"2#变桨柜体温度低","故障 "]
["SGW33 ",225,"2#变桨电容电压不平衡","故障 "]
["SGW33 ",228,"2#变桨故障字非零","故障 "]
["SGW33 ",249,"电能表检测到高电压穿越","故障 "]
["SGW33 ",274,"水冷进出阀温度比较超限","故障 "]
["SGW33 ",295,"变流器准备未完成","故障 "]
["SGW33 ",302,"变流器调制后rdy_on丢失","故障 "]
["SGW33 ",323,"机舱控制柜UPS电池电量低","故障 "]
["SGW33 ",344,"预留","提示信息 "]
["SGW33 ",369,"预留","提示信息 "]
["SGW33 ",372,"预留","提示信息 "]
["SGW33 ",393,"预留","提示信息 "]
["SGW33 ",418,"水冷出阀温度变化率异常","故障 "]
["SGW33 ",440,"电网频率超高","故障 "]
["SGW33 ",591,"主轴润滑时间短","故障 "]
["SGW33 ",1004,"1U4_软件直流过压","故障 "]
["SGW33 ",1025,"1U3_C相软件过流","故障 "]
["SGW33 ",1050,"1U3_STACK1_C相软件过流","故障 "]
["SGW33 ",1053,"1U3_STACK2_C相软件过流","故障 "]
["SGW33 ",1078,"1U1_电压高","故障 "]
["SGW33 ",1099,"1U2_STACK2硬件直流过压","故障 "]
["SGW33 ",1120,"1U2_STACK1硬件过流","故障 "]
["SGW33 ",1127,"2U1_STACK2硬件过流","故障 "]
["SGW33 ",1148,"2U1_交流熔断器异常","故障 "]
["SGW33 ",1169,"2U2_直流熔断器1异常","故障 "]
["SGW33 ",1194,"2U1_A相驱动异常","故障 "]
["SGW33 ",1197,"2U2_A相驱动异常","故障 "]
["SGW33 ",1222,"1U3_STACK2_C相驱动异常","故障 "]
["SGW33 ",1243,"1U1_GBT3_驱动异常","故障 "]
["SGW33 ",1264,"1U3_IGBT软件过温","故障 "]
["SGW33 ",1271,"1U1_STACK2_IGBT硬件过温","故障 "]
["SGW33 ",1292,"1U4_STACK1_IGBT软件过温","故障 "]
["SGW33 ",1317,"1U3_CPU12V电源异常","故障 "]
["SGW33 ",1338,"1U1_断路器断开","故障 "]
["SGW33 ",1341,"1U2_断路器闭合","故障 "]
["SGW33 ",1366,"1U2_Sum","故障 "]
["SGW33 ",1387,"1U3_相序错误","故障 "]
["SGW33 ",1408,"1U4_CAN网络通讯异常","故障 "]
["SGW33 ",1415,"1U2_FPGA通讯校验错误","故障 "]
["SGW33 ",1436,"2U3_Sport1_通讯异常","故障 "]
["SGW33 ",1461,"2U4_驱动控制器光纤通讯异常","故障 "]
["SGW33 ",1482,"(1482)1U2直流母线电压瞬时值超限","故障 "]
["SGW33 ",1485,"急停预留_5","提示信息 "]
["SGW33 ",1510,"1U1_STACK1_三相电流不平衡","故障 "]
["SGW33 ",1531,"2U3_STACK2_IGBT软件过温","故障 "]
["SGW33 ",1552,"1U4_IGBT7温度高","故障 "]
["SGW33 ",1559,"1U1_膜电容过温","故障 "]
["SGW33 ",1580,"2U2_频率高","故障 "]
["SGW33 ",1605,"2U2_三相电压不平衡","故障 "]
["SGW33 ",1626,"有功功率比较","故障 "]
["SGW33 ",1629,"无功功率比较","故障 "]
["SGW33 ",1654,"2#网侧电抗器过温","故障 "]
["SGW33 ",1675,"正常停机预留_17","提示信息 "]
["SGW33 ",1682,"1U1电网电压高","故障 "]
["SGW33 ",1703,"1#防雷熔断器异常","故障 "]
["SGW33 ",1724,"1U1_版本校验错误","故障 "]
["SGW33 ",1749,"警示预留_10","提示信息 "]
["SGW33 ",1770,"2U1三相电压不平衡异常提示","故障 "]
["SGW33 ",1773,"1U2 三相电流不平衡异常提示","故障 "]
["SGW33 ",1798,"2U4_IGBT软件温度低","故障 "]
["SGW33 ",1819,"1U2_STACK1_三相电流不平衡","故障 "]
["SGW33 ",1826,"2U1_STACK2_三相电流不平衡","故障 "]
["SGW33 ",1847,"2U2_STACK2_过载","故障 "]
["SGW33 ",1868,"Rsafe_预留8","提示信息 "]
["SGW33 ",3009,"机舱温度高警告","告警信息 "]
["SGW33 ",3030,"液压站压力低警告","告警信息 "]
["SGW33 ",3033,"液压系统维护刹车反馈异常警告","告警信息 "]
["SGW33 ",3058,"转速比较3警告","告警信息 "]
["SGW33 ",3079,"变压器温度高警告","告警信息 "]
["SGW33 ",3086,"预留","提示信息 "]
["SGW33 ",3107,"机舱子站电源异常警告","告警信息 "]
["SGW33 ",3128,"禁止叶轮锁定释放警告","告警信息 "]
["SGW33 ",3153,"预留","提示信息 "]
["SGW33 ",3174,"3#变桨逆变器OK信号丢失警告","告警信息 "]
["SGW33 ",3181,"1#变桨旋编电池电压低警告","告警信息 "]
["SGW33 ",3202,"1#变桨逆变器温度高警告","告警信息 "]
["SGW33 ",3223,"3#变桨电容电压低警告","告警信息 "]
["SGW33 ",3230,"1#变桨心跳信号丢失警告","告警信息 "]
["SGW33 ",3251,"预留","提示信息 "]
["SGW33 ",3272,"出阀压力低警告","告警信息 "]
["SGW33 ",3297,"变流器未调制警告","告警信息 "]
["SGW33 ",3318,"CPU资源不足1警告","告警信息 "]
["SGW33 ",3325,"预留","提示信息 "]
["SGW33 ",3346,"预留","提示信息 "]
["SGW33 ",3367,"预留","提示信息 "]
["SGW33 ",3374,"预留","提示信息 "]
["SGW33 ",3395,"预留","提示信息 "]
["SGW33 ",3420,"水冷加热器异常警告","告警信息 "]
["SGW33 ",3442,"(3442)电网频率极高警告","告警信息 "]
["SGW33 ",3754,"（3754)除冰系统状态异常警告","故障 "]
["SGW33 ",4003,"1U3_软件直流过压警告","告警信息 "]
["SGW33 ",4026,"2U1_A相软件过流警告","告警信息 "]
["SGW33 ",4047,"1U2_STACK2_C相软件过流警告","告警信息 "]
["SGW33 ",4054,"2U1_STACK1_A相软件过流警告","告警信息 "]
["SGW33 ",4075,"2U1_频率高警告","告警信息 "]
["SGW33 ",4100,"1U3_STACK1硬件直流过压警告","告警信息 "]
["SGW33 ",4121,"1U2_STACK2硬件过流警告","告警信息 "]
["SGW33 ",4142,"1U2_IGBT9硬件过流警告","告警信息 "]
["SGW33 ",4149,"1U1_直流熔断器1异常警告","告警信息 "]
["SGW33 ",4170,"2U2_直流熔断器2异常警告","告警信息 "]
["SGW33 ",4191,"1U3_C相驱动异常警告","告警信息 "]
["SGW33 ",4198,"2U2_B相驱动异常警告","告警信息 "]
["SGW33 ",4219,"1U3_STACK1_C相驱动异常警告","告警信息 "]
["SGW33 ",4244,"1U1_IGBT4_驱动异常警告","告警信息 "]
["SGW33 ",4265,"1U4_IGBT软件过温警告","告警信息 "]
["SGW33 ",4286,"1U1_STACK1_IGBT软件过温警告","告警信息 "]
["SGW33 ",4293,"1U4_STACK2_IGBT软件过温警告","告警信息 "]
["SGW33 ",4314,"1U3_IGBT13_过温警告","告警信息 "]
["SGW33 ",4339,"2U1_断路器闭合警告","告警信息 "]
["SGW33 ",4342,"1U2_断路器断开警告","告警信息 "]
["SGW33 ",4363,"1U4_制动回路异常警告","告警信息 "]
["SGW33 ",4388,"2U3_相序错误警告","告警信息 "]
["SGW33 ",4409,"2U1_CAN网络通讯异常警告","告警信息 "]
["SGW33 ",4430,"1U1_Sport1_通讯异常警告","告警信息 "]
["SGW33 ",4437,"2U4_Sport1_通讯异常警告","告警信息 "]
["SGW33 ",4458,"2U1_驱动控制器光纤通讯异常警告","告警信息 "]
["SGW33 ",4483,"(4483)1U3直流母线电压瞬时值超限警告","告警信息 "]
["SGW33 ",4486,"急停预留_6警告","提示信息 "]
["SGW33 ",4507,"1U1_频率低警告","告警信息 "]
["SGW33 ",4532,"2U4_STACK1_IGBT软件过温警告","告警信息 "]
["SGW33 ",4553,"1U2_IGBT8温度高警告","告警信息 "]
["SGW33 ",4560,"1U2_膜电容过温警告","告警信息 "]
["SGW33 ",4581,"2U3_频率高警告","告警信息 "]
["SGW33 ",4602,"2U3_STACK1_过载警告","告警信息 "]
["SGW33 ",4627,"直流电压比较警告","告警信息 "]
["SGW33 ",4630,"1#柜电抗器过温警告","告警信息 "]
["SGW33 ",4651,"开关柜1环境温度高警告","告警信息 "]
["SGW33 ",4676,"正常停机预留_18警告","提示信息 "]
["SGW33 ",4697,"预留警告","提示信息 "]
["SGW33 ",4704,"2#防雷熔断器异常警告","告警信息 "]
["SGW33 ",4725,"1U2_版本校验错误警告","告警信息 "]
["SGW33 ",4746,"警示预留_7警告","提示信息 "]
["SGW33 ",4771,"2U1电网频率低异常提示警告","告警信息 "]
["SGW33 ",4774,"1U2 STACK1三相电流不平衡异常提示警告","告警信息 "]
["SGW33 ",4795,"2U1_IGBT软件温度低警告","告警信息 "]
["SGW33 ",4820,"1U2_STACK2_三相电流不平衡警告","告警信息 "]
["SGW33 ",4841,"1U3_STACK2_过载警告","告警信息 "]
["SGW33 ",4848,"2U3_过载警告","告警信息 "]
["SGW33 ",4869,"Rsafe_预留9警告","提示信息 "]
["SGW34 ",7,"机舱控制柜温度高","故障 "]
["SGW34 ",32,"预留","提示信息 "]
["SGW34 ",35,"电网电压高","故障 "]
["SGW34 ",60,"发电机过速1","故障 "]
["SGW34 ",81,"机舱熔断器反馈丢失","故障 "]
["SGW34 ",102,"叶片主轴润滑分配器堵塞","故障 "]
["SGW34 ",109,"预留","提示信息 "]
["SGW34 ",130,"风速仪工作异常","故障 "]
["SGW34 ",151,"机舱除湿机工作异常","故障 "]
["SGW34 ",176,"2#变桨充电器反馈丢失","故障 "]
["SGW34 ",179,"2#变桨安全位置传感器异常","故障 "]
["SGW34 ",204,"3#变桨逆变器温度高","故障 "]
["SGW34 ",225,"2#变桨电容电压不平衡","故障 "]
["SGW34 ",246,"预留","提示信息 "]
["SGW34 ",253,"预留","提示信息 "]
["SGW34 ",274,"水冷进出阀温度比较超限","故障 "]
["SGW34 ",295,"变流器准备未完成","故障 "]
["SGW34 ",320,"偏航速度超限","故障 "]
["SGW34 ",323,"机舱控制柜UPS电池电量低","故障 "]
["SGW34 ",348,"预留","提示信息 "]
["SGW34 ",369,"预留","提示信息 "]
["SGW34 ",390,"水冷进阀静压异常","故障 "]
["SGW34 ",397,"预留","提示信息 "]
["SGW34 ",418,"水冷出阀温度变化率异常","故障 "]
["SGW34 ",444,"电网电压极高","故障 "]
["SGW34 ",469,"发电机定子温度传感器异常","故障 "]
["SGW34 ",472,"发电机后轴承温度1传感器异常","故障 "]
["SGW34 ",550,"箱变水冷出泵压力传感器异常","故障 "]
["SGW34 ",748,"(748)叶片d轴载荷超限","故障 "]
["SGW34 ",777,"小风软件过速","故障 "]
["SGW34 ",784,"控制策略判断叶片1变桨速率跟随误差","故障 "]
["SGW34 ",1017,"1U1_A相软件过流","故障 "]
["SGW34 ",1042,"1U2_STACK1_A相软件过流","故障 "]
["SGW34 ",1063,"2U2_STACK2_A相软件过流","故障 "]
["SGW34 ",1066,"2U3_STACK1_A相软件过流","故障 "]
["SGW34 ",1091,"2U2_硬件直流过压","故障 "]
["SGW34 ",1112,"1U1_硬件过流","故障 "]
["SGW34 ",1119,"1U1_STACK2硬件过流","故障 "]
["SGW34 ",1140,"1U4_IGBT7硬件过流","故障 "]
["SGW34 ",1161,"1U4_直流熔断器1异常","故障 "]
["SGW34 ",1186,"1U2_A相驱动异常","故障 "]
["SGW34 ",1207,"1U1_STACK1_C相驱动异常","故障 "]
["SGW34 ",1210,"1U1_STACK2_C相驱动异常","故障 "]
["SGW34 ",1235,"2U3_STACK1_A相驱动异常","故障 "]
["SGW34 ",1256,"1U3_IGBT硬件过温","故障 "]
["SGW34 ",1263,"1U2_IGBT软件过温","故障 "]
["SGW34 ",1284,"2U4_STACK1_IGBT硬件过温","故障 "]
["SGW34 ",1305,"1U1_IGBT4_过温","故障 "]
["SGW34 ",1330,"1U2_取能板异常","故障 "]
["SGW34 ",1351,"1#柜预充电失败","故障 "]
["SGW34 ",1354,"2#柜预充电超时","故障 "]
["SGW34 ",1379,"1U3_STACK2_Sum","故障 "]
["SGW34 ",1400,"1U2_缺相","故障 "]
["SGW34 ",1407,"1U3_CAN网络通讯异常","故障 "]
["SGW34 ",1428,"2U3_Sport0_通讯异常","故障 "]
["SGW34 ",1449,"1U4_DSP/FPGA通讯异常","故障 "]
["SGW34 ",1474,"1U2_转矩异常","故障 "]
["SGW34 ",1495,"(1495)电网电压高超时故障5","故障 "]
["SGW34 ",1502,"2U1_电压高","故障 "]
["SGW34 ",1523,"1U3_STACK2_IGBT软件过温","故障 "]
["SGW34 ",1544,"2U3_STACK1_IGBT软件温度低","故障 "]
["SGW34 ",1551,"1U1_IGBT6温度高","故障 "]
["SGW34 ",1572,"2U2_均流电抗器过温","故障 "]
["SGW34 ",1593,"1U2_STACK1_过载","故障 "]
["SGW34 ",1618,"2U3_STACK1_三相电流不平衡","故障 "]
["SGW34 ",1639,"2#柜环境温度低","故障 "]
["SGW34 ",1646,"柜内环境温度低","故障 "]
["SGW34 ",1667,"正常停机预留_9","提示信息 "]
["SGW34 ",1688,"2U1电网电压低","故障 "]
["SGW34 ",1695,"预留","提示信息 "]
["SGW34 ",1716,"功率柜1离心风机反馈异常","故障 "]
["SGW34 ",1737,"2U2_产品配置错误","故障 "]
["SGW34 ",1762,"2U1频率高异常提示","故障 "]
["SGW34 ",1783,"2U2 STACK2三相电流不平衡异常提示","故障 "]
["SGW34 ",1790,"2#柜环境控制器通讯异常","故障 "]
["SGW34 ",1811,"2U3_STACK1_IGBT软件低温","故障 "]
["SGW34 ",1832,"2U3_STACK2_三相电流不平衡","故障 "]
["SGW34 ",1839,"1U3_过载","故障 "]
["SGW34 ",1860,"2U3频率高","故障 "]
["SGW34 ",1885,"1#柜滤波电容B相过流","故障 "]
["SGW34 ",1912,"1U3电流控制异常故障","故障 "]
["SGW34 ",1933,"2U3_W相温度不均衡警告","故障 "]
["SGW34 ",2703,"发电机散热风道温度高","故障 "]
["SGW34 ",2724,"2#变桨柜温度异常升高","故障 "]
["SGW34 ",2736,"变流柜温度变化率异常","故障 "]
["SGW34 ",3014,"偏航轴承加脂油路堵塞警告","告警信息 "]
["SGW34 ",3035,"电网电压高警告","告警信息 "]
["SGW34 ",3060,"发电机过速1警告","告警信息 "]
["SGW34 ",3081,"机舱熔断器反馈丢失警告","告警信息 "]
["SGW34 ",3102,"叶片主轴润滑分配器堵塞警告","告警信息 "]
["SGW34 ",3109,"预留","提示信息 "]
["SGW34 ",3130,"风速仪工作异常警告","告警信息 "]
["SGW34 ",3155,"预留","提示信息 "]
["SGW34 ",3158,"2#变桨最小角度超限警告","告警信息 "]
["SGW34 ",3179,"2#变桨安全位置传感器异常警告","告警信息 "]
["SGW34 ",3204,"3#变桨逆变器温度高警告","告警信息 "]
["SGW34 ",3225,"2#变桨电容电压不平衡警告","告警信息 "]
["SGW34 ",3246,"预留","提示信息 "]
["SGW34 ",3253,"预留","提示信息 "]
["SGW34 ",3274,"水冷进出阀温度比较超限警告","告警信息 "]
["SGW34 ",3299,"变流器启动环境条件不满足警告","告警信息 "]
["SGW34 ",3302,"变流器调制后rdy_on丢失警告","告警信息 "]
["SGW34 ",3323,"机舱控制柜UPS电池电量低警告","告警信息 "]
["SGW34 ",3348,"预留","提示信息 "]
["SGW34 ",3369,"预留","提示信息 "]
["SGW34 ",3390,"水冷进阀静压异常警告","告警信息 "]
["SGW34 ",3397,"预留","提示信息 "]
["SGW34 ",3418,"水冷出阀温度变化率异常警告","告警信息 "]
["SGW34 ",3444,"(3444)电网电压极高警告","告警信息 "]
["SGW34 ",3447,"警告","提示信息 "]
["SGW34 ",3468,"机舱环境温度传感器异常警告","告警信息 "]
["SGW34 ",3546,"箱变系统传感器异常警告","告警信息 "]
["SGW34 ",3743,"（3743)载荷测量单元通讯异常警告","故障 "]
["SGW34 ",3751,"（3751)叶片q轴IPC变桨较高警告","故障 "]
["SGW34 ",3779,"叶片2变桨跟随误差警告","告警信息 "]
["SGW34 ",4012,"1U4_软件直流欠压警告","告警信息 "]
["SGW34 ",4037,"1U1_STACK1_B相软件过流警告","告警信息 "]
["SGW34 ",4040,"1U1_STACK2_B相软件过流警告","告警信息 "]
["SGW34 ",4061,"2U2_STACK1_B相软件过流警告","告警信息 "]
["SGW34 ",4086,"2U1_三相电压不平衡警告","告警信息 "]
["SGW34 ",4107,"2U2_STACK2硬件直流过压警告","告警信息 "]
["SGW34 ",4114,"1U3_硬件过流警告","告警信息 "]
["SGW34 ",4135,"1U1_IGBT2硬件过流警告","告警信息 "]
["SGW34 ",4156,"1U2_直流熔断器4异常警告","告警信息 "]
["SGW34 ",4181,"1U1_滤波电容熔断器异常警告","告警信息 "]
["SGW34 ",4184,"1U1_B相驱动异常警告","告警信息 "]
["SGW34 ",4209,"1U1_STACK2_B相驱动异常警告","告警信息 "]
["SGW34 ",4230,"2U2_STACK1_B相驱动异常警告","告警信息 "]
["SGW34 ",4251,"1U3_ IGBT11_驱动异常警告","告警信息 "]
["SGW34 ",4258,"2U1_IGBT硬件过温警告","告警信息 "]
["SGW34 ",4279,"2U1_STACK2_IGBT硬件过温警告","告警信息 "]
["SGW34 ",4300,"2U4_STACK1_IGBT软件过温警告","告警信息 "]
["SGW34 ",4325,"2#柜24V开关电源1保护警告","告警信息 "]
["SGW34 ",4328,"24V开关电源2保护警告","告警信息 "]
["SGW34 ",4353,"2#柜预充电失败警告","告警信息 "]
["SGW34 ",4374,"2U1_STACK1_Sum警告","告警信息 "]
["SGW34 ",4395,"1U2_电压高警告","告警信息 "]
["SGW34 ",4402,"2U1_缺相警告","告警信息 "]
["SGW34 ",4423,"1U2_Sport0_通讯异常警告","告警信息 "]
["SGW34 ",4444,"2U3_以太网通讯异常警告","告警信息 "]
["SGW34 ",4469,"2U2_安全链反馈异常警告","告警信息 "]
["SGW34 ",4472,"1#柜PLC_安全链反馈异常警告","告警信息 "]
["SGW34 ",4497,"急停预留_17警告","提示信息 "]
["SGW34 ",4518,"1U1_STACK1_IGBT软件过温警告","告警信息 "]
["SGW34 ",4539,"1U3_STACK2_IGBT软件温度低警告","告警信息 "]
["SGW34 ",4546,"1U1_IGBT1温度高警告","告警信息 "]
["SGW34 ",4567,"1U1_均流电抗器过温警告","告警信息 "]
["SGW34 ",4592,"1U2_过载警告","告警信息 "]
["SGW34 ",4613,"1U3_STACK2_三相电流不平衡警告","告警信息 "]
["SGW34 ",4616,"2U2_STACK2_三相电流不平衡警告","告警信息 "]
["SGW34 ",4641,"IGBT柜2环境温度高警告","告警信息 "]
["SGW34 ",4662,"(4662)TCC_版本校验错误警告","告警信息 "]
["SGW34 ",4683,"1U1输出功率低警告","告警信息 "]
["SGW34 ",4690,"2U1输出功率低警告","告警信息 "]
["SGW34 ",4711,"IGBT柜2离心风机反馈异常警告","告警信息 "]
["SGW34 ",4736,"2U1_产品配置错误警告","告警信息 "]
["SGW34 ",4757,"警示预留_18警告","提示信息 "]
["SGW34 ",4760,"预留警告","提示信息 "]
["SGW34 ",4785,"2U3 三相电流不平衡异常提示警告","告警信息 "]
["SGW34 ",4806,"1U4_STACK2_IGBT软件低温警告","告警信息 "]
["SGW34 ",4827,"2U2_三相电流不平衡警告","告警信息 "]
["SGW34 ",4834,"1U1_STACK1_过载警告","告警信息 "]
["SGW34 ",4855,"2U2_STACK1/STACK2不均流警告","告警信息 "]
["SGW34 ",4880,"降功率运行_预留10警告","提示信息 "]
["SGW34 ",4901,"1U1_母线电压控制异常警告","告警信息 "]
["SGW34 ",4904,"警告","提示信息 "]
["SGW34 ",4929,"1U3_V相温度不均衡警告警告","告警信息 "]
["SGW34 ",5713,"偏航轴承长时间未润滑警告","告警信息 "]
["SGW34 ",5771,"架空净空传感器异常警告","告警信息 "]
["SGW35 ",1,"(1)机舱加速度超限","故障 "]
["SGW35 ",22,"(22)液压系统油位低","故障 "]
["SGW35 ",47,"(47)预留","提示信息 "]
["SGW35 ",68,"(68)发电机主轴润滑分配器堵塞","故障 "]
["SGW35 ",71,"(71)发电机轴承温度高","故障 "]
["SGW35 ",96,"(96)叶轮锁定","提示信息 "]
["SGW35 ",117,"(117)机舱子站总线异常","故障 "]
["SGW35 ",142,"(142)初始化未完成","故障 "]
["SGW35 ",145,"(145)停机过程转速异常2","故障 "]
["SGW35 ",166,"(166)1#变桨外部安全链信号异常","故障 "]
["SGW35 ",191,"(191)2#变桨电容温度高","故障 "]
["SGW35 ",212,"(212)2#变桨电容电压高(国产)","故障 "]
["SGW35 ",219,"(219)2#变桨速度超限","故障 "]
["SGW35 ",240,"(240)发电机冷却低速运行反馈丢失","故障 "]
["SGW35 ",261,"(261)1#水冷风扇反馈状态异常","故障 "]
["SGW35 ",286,"(286)预留","提示信息 "]
["SGW35 ",289,"(289)预留","提示信息 "]
["SGW35 ",310,"(310)制动单元温度高","故障 "]
["SGW35 ",335,"预留","提示信息 "]
["SGW35 ",356,"预留","提示信息 "]
["SGW35 ",363,"预留","提示信息 "]
["SGW35 ",384,"预留","提示信息 "]
["SGW35 ",405,"(405)停机及停机过程加速度超限","故障 "]
["SGW35 ",430,"(430)发电机温度传感器（1-12）失效","故障 "]
["SGW35 ",433,"(433)发电机轴承温升高","故障 "]
["SGW35 ",458,"(458)发电机前轴承外圈温度变化率异常","故障 "]
["SGW35 ",536,"(536)箱变水冷循环泵入口压力低","故障 "]
["SGW35 ",557,"(557)变压器油温高","故障 "]
["SGW35 ",740,"(740)叶轮方位传感器转速比较异常","故障 "]
["SGW35 ",766,"(766)发电机前轴承内外圈温差大","故障 "]
["SGW35 ",788,"(788)控制策略报发电机N4过速","故障 "]
["SGW35 ",1006,"(1006)2U2_软件直流过压","故障 "]
["SGW35 ",1009,"(1009)1U1_软件直流欠压","故障 "]
["SGW35 ",1034,"(1034)2U3_C相软件过流","故障 "]
["SGW35 ",1055,"(1055)2U1_STACK1_B相软件过流","故障 "]
["SGW35 ",1076,"(1076)1U1_频率低","故障 "]
["SGW35 ",1083,"(1083)2U1_电压峰值超限","故障 "]
["SGW35 ",1104,"(1104)2U1_STACK1硬件直流过压","故障 "]
["SGW35 ",1125,"(1125)1U4_STACK2硬件过流","故障 "]
["SGW35 ",1150,"(1150)1U1_直流熔断器2异常","故障 "]
["SGW35 ",1153,"(1153)1U2_直流熔断器1异常","故障 "]
["SGW35 ",1178,"(1178)2U4_直流熔断器2异常","故障 "]
["SGW35 ",1199,"(1199)2U2_C相驱动异常","故障 "]
["SGW35 ",1220,"(1220)1U3_STACK2_A相驱动异常","故障 "]
["SGW35 ",1227,"(1227)2U1_STACK2_B相驱动异常","故障 "]
["SGW35 ",1248,"(1248)1U2_ IGBT8_驱动异常","故障 "]
["SGW35 ",1269,"(1269)2U4_IGBT软件过温","故障 "]
["SGW35 ",1294,"(1294)2U1_STACK1_IGBT软件过温","故障 "]
["SGW35 ",1297,"(1297)2U2_STACK2_IGBT软件过温","故障 "]
["SGW35 ",1316,"(1316)1U2_CPU12V电源异常","故障 "]
["SGW35 ",1342,"(1342)1U2_断路器断开","故障 "]
["SGW35 ",1363,"(1363)1U4_制动回路异常","故障 "]
["SGW35 ",1370,"(1370)2U3_Sum","故障 "]
["SGW35 ",1391,"(1391)1U2_零序电流保护","故障 "]
["SGW35 ",1416,"(1416)1U3_FPGA通讯校验错误","故障 "]
["SGW35 ",1437,"(1437)2U4_Sport1_通讯异常","故障 "]
["SGW35 ",1440,"(1440)1U3_以太网通讯异常","故障 "]
["SGW35 ",1465,"(1465)1U2_安全链反馈异常","故障 "]
["SGW35 ",1486,"(1486)2U2直流母线电压瞬时值超限","故障 "]
["SGW35 ",1507,"(1507)1U1_频率低","故障 "]
["SGW35 ",1514,"(1514)2U1_STACK2_三相电流不平衡","故障 "]
["SGW35 ",1535,"(1535)1U1_STACK2_IGBT软件温度低","故障 "]
["SGW35 ",1560,"(1560)1U2_膜电容过温","故障 "]
["SGW35 ",1581,"(1581)2U3_频率高","故障 "]
["SGW35 ",1584,"(1584)2U2_频率低","故障 "]
["SGW35 ",1609,"(1609)1U2_STACK1_三相电流不平衡","故障 "]
["SGW35 ",1630,"(1630)1#柜电抗器过温","故障 "]
["SGW35 ",1637,"(1637)2#柜湿度高","故障 "]
["SGW35 ",1658,"(1658)2#滤波电容过温","故障 "]
["SGW35 ",1679,"(1679)2U4_软件过流","故障 "]
["SGW35 ",1704,"(1704)2#防雷熔断器异常","故障 "]
["SGW35 ",1725,"(1725)1U2_版本校验错误","故障 "]
["SGW35 ",1728,"(1728)2U1_版本校验错误","故障 "]
["SGW35 ",1753,"(1753)主柜运行反馈错误","故障 "]
["SGW35 ",1774,"(1774)1U2 STACK1三相电流不平衡异常提示","故障 "]
["SGW35 ",1781,"(1781)2U2 三相电流不平衡异常提示","故障 "]
["SGW35 ",1802,"(1802)1U2_STACK2_IGBT软件低温","故障 "]
["SGW35 ",1823,"(1823)1U3_STACK2_三相电流不平衡","故障 "]
["SGW35 ",1848,"(1848)2U3_过载","故障 "]
["SGW35 ",1869,"(1869)1U3_STACK1_U相温度不均衡错误","故障 "]
["SGW35 ",1872,"(1872)2#柜控制器24V蓄电池异常保护","故障 "]
["SGW35 ",1897,"(1897)TCC_DSP参数错误","故障 "]
["SGW35 ",1921,"(1921)2U1_网侧电压谐波高","故障 "]
["SGW35 ",1928,"(1928)1U3_U相温度不均衡警告","故障 "]
["SGW35 ",2005,"(2005)网侧硬件持续过流保护","故障 "]
["SGW35 ",2027,"(2027)网侧FLASH参数校验错误","故障 "]
["SGW35 ",2066,"(2066)机侧V相峰值过流","故障 "]
["SGW35 ",2088,"(2088)机侧并柜电流不平衡保护","故障 "]
["SGW35 ",2096,"(2096)机侧窄脉冲","故障 "]
["SGW35 ",2132,"(2132)撬棒触发超次数","故障 "]
["SGW35 ",2214,"(2214)网侧模块2C相硬件过流","故障 "]
["SGW35 ",2221,"(2221)网侧A相滤波电容过流","故障 "]
["SGW35 ",2242,"(2242)chopper过载","故障 "]
["SGW35 ",2263,"(2263)网侧模块2A相过流","故障 "]
["SGW35 ",2288,"(2288)水温过温","故障 "]
["SGW35 ",2421,"(2421)网侧检测板类型和发波拓扑不匹配","故障 "]
["SGW35 ",2428,"(2428)网侧2组IGBT过流","故障 "]
["SGW35 ",2449,"(2449)电网二级过压","故障 "]
["SGW35 ",2470,"(2470)母线运行欠压","故障 "]
["SGW35 ",2477,"(2477)主断路器闭合失败","故障 "]
["SGW35 ",2498,"(2498)机侧功率单元网侧滤波电容不均流","故障 "]
["SGW35 ",2523,"(2523)定子B有效值过流","故障 "]
["SGW35 ",2555,"(2555)水冷柜状态错误","故障 "]
["SGW35 ",2598,"(2598)定子相间电流不平衡","故障 "]
["SGW35 ",2707,"(2707)叶轮平面模态异常振动","故障 "]
["SGW35 ",2728,"(2728)1#变桨柜温度传感器异常","故障 "]
["SGW35 ",2784,"(2784)1#变桨备电系统预防性更换","故障 "]
["SGW35 ",2791,"(2791)启机过程中风速转速不匹配保护","故障 "]
["SGW35 ",3018,"(3018)偏航方向异常警告","告警信息 "]
["SGW35 ",3043,"(3043)有功功率低警告","告警信息 "]
["SGW35 ",3064,"(3064)警告","告警信息 "]
["SGW35 ",3085,"(3085)偏航过程中加速度超限警告","告警信息 "]
["SGW35 ",3092,"(3092)安全链过速警告","告警信息 "]
["SGW35 ",3113,"(3113)轮毂测控子站电源异常警告","告警信息 "]
["SGW35 ",3134,"(3134)风速功率偏差大警告","告警信息 "]
["SGW35 ",3141,"(3141)发电机绝缘低警告","告警信息 "]
["SGW35 ",3162,"(3162)预留警告","提示信息 "]
["SGW35 ",3187,"(3187)1#变桨电机温度低警告","告警信息 "]
["SGW35 ",3208,"(3208)预留警告","提示信息 "]
["SGW35 ",3229,"(3229)3#变桨故障字非零警告","告警信息 "]
["SGW35 ",3236,"(3236)预留警告","提示信息 "]
["SGW35 ",3257,"(3257)预留警告","提示信息 "]
["SGW35 ",3282,"(3282)水冷循环泵异常警告","告警信息 "]
["SGW35 ",3285,"(3285)预留警告","提示信息 "]
["SGW35 ",3306,"(3306)电机1侧逆变器温度高警告","告警信息 "]
["SGW35 ",3331,"(3331)警告","告警信息 "]
["SGW35 ",3352,"(3352)警告","告警信息 "]
["SGW35 ",3373,"(3373)警告","告警信息 "]
["SGW35 ",3380,"(3380)警告","告警信息 "]
["SGW35 ",3401,"(3401)2#风速仪工作异常警告","告警信息 "]
["SGW35 ",3426,"(3426)变压器绕组温度变化率异常警告","告警信息 "]
["SGW35 ",3429,"(3429)机舱温度与环境温度反接警告","告警信息 "]
["SGW35 ",3450,"(3450)警告","告警信息 "]
["SGW35 ",3475,"(3475)发电机前轴承外圈温度传感器异常警告","告警信息 "]
["SGW35 ",3496,"(3496)警告","告警信息 "]
["SGW35 ",3517,"(3517)警告","告警信息 "]
["SGW35 ",3524,"(3524)警告","告警信息 "]
["SGW35 ",3545,"(3545)箱变水冷子站总线异常警告","告警信息 "]
["SGW35 ",3570,"(3570)警告","告警信息 "]
["SGW35 ",3573,"(3573)警告","告警信息 "]
["SGW35 ",3594,"(3594)警告","告警信息 "]
["SGW35 ",3619,"(3619)警告","告警信息 "]
["SGW35 ",3640,"(3640)警告","告警信息 "]
["SGW35 ",3647,"(3647)警告","告警信息 "]
["SGW35 ",3668,"(3668)警告","告警信息 "]
["SGW35 ",3689,"(3689)警告","告警信息 "]
["SGW35 ",3714,"(3714)警告","告警信息 "]
["SGW35 ",3717,"(3717)警告","告警信息 "]
["SGW35 ",3738,"(3738)警告","告警信息 "]
["SGW35 ",3763,"(3763)过速继电器异常警告","告警信息 "]
["SGW35 ",3784,"(3784)控制策略判断叶片1变桨速率跟随误差警告","告警信息 "]
["SGW35 ",3791,"(3791)机舱加速度有效值偏差大","告警信息 "]
["SGW35 ",3812,"(3812)警告","告警信息 "]
["SGW35 ",3833,"(3833)警告","告警信息 "]
["SGW35 ",3858,"(3858)警告","告警信息 "]
["SGW35 ",3861,"(3861)警告","告警信息 "]
["SGW35 ",3886,"(3886)警告","告警信息 "]
["SGW35 ",3907,"(3907)警告","告警信息 "]
["SGW35 ",3928,"(3928)警告","告警信息 "]
["SGW35 ",3935,"(3935)警告","告警信息 "]
["SGW35 ",3956,"(3956)警告","告警信息 "]
["SGW35 ",3977,"(3977)警告","告警信息 "]
["SGW35 ",4002,"(4002)1U2_软件直流过压警告","告警信息 "]
["SGW35 ",4005,"(4005)2U1_软件直流过压警告","告警信息 "]
["SGW35 ",4030,"(4030)2U2_B相软件过流警告","告警信息 "]
["SGW35 ",4051,"(4051)1U3_STACK2_A相软件过流警告","告警信息 "]
["SGW35 ",4072,"(4072)低穿超时警告","告警信息 "]
["SGW35 ",4079,"(4079)2U1_电压高警告","告警信息 "]
["SGW35 ",4100,"(4100)1U3_STACK1硬件直流过压警告","告警信息 "]
["SGW35 ",4121,"(4121)1U2_STACK2硬件过流警告","告警信息 "]
["SGW35 ",4146,"(4146)1U3_IGBT13硬件过流警告","告警信息 "]
["SGW35 ",4149,"(4149)1U1_直流熔断器1异常警告","告警信息 "]
["SGW35 ",4174,"(4174)2U3_直流熔断器2异常警告","告警信息 "]
["SGW35 ",4195,"(4195)2U1_B相驱动异常警告","告警信息 "]
["SGW35 ",4216,"(4216)1U2_STACK2_C相驱动异常警告","告警信息 "]
["SGW35 ",4223,"(4223)2U1_STACK1_A相驱动异常警告","告警信息 "]
["SGW35 ",4244,"(4244)1U1_IGBT4_驱动异常警告","告警信息 "]
["SGW35 ",4269,"(4269)2U4_IGBT软件过温警告","告警信息 "]
["SGW35 ",4290,"(4290)1U3_STACK1_IGBT软件过温警告","告警信息 "]
["SGW35 ",4293,"(4293)1U4_STACK2_IGBT软件过温警告","告警信息 "]
["SGW35 ",4318,"(4318)1U4_CPU12V电源异常警告","告警信息 "]
["SGW35 ",4339,"(4339)2U1_断路器闭合警告","告警信息 "]
["SGW35 ",4348,"(4348)2U3_断路器断开警告","告警信息 "]
["SGW35 ",4366,"(4366)1U2_Sum警告","告警信息 "]
["SGW35 ",4387,"(4387)1U3_相序错误警告","告警信息 "]
["SGW35 ",4412,"(4412)2U4_CAN网络通讯异常警告","告警信息 "]
["SGW35 ",4433,"(4433)1U4_Sport1_通讯异常警告","告警信息 "]
["SGW35 ",4436,"(4436)2U3_Sport1_通讯异常警告","告警信息 "]
["SGW35 ",4461,"(4461)2U4_驱动控制器光纤通讯异常警告","告警信息 "]
["SGW35 ",4482,"(4482)1U2直流母线电压瞬时值超限警告","告警信息 "]
["SGW35 ",4489,"(4489)1#柜直流母线电压比较警告","告警信息 "]
["SGW35 ",4510,"(4510)1U1_STACK1_三相电流不平衡警告","告警信息 "]
["SGW35 ",4531,"(4531)2U3_STACK2_IGBT软件过温警告","告警信息 "]
["SGW35 ",4556,"(4556)1U3_IGBT11温度高警告","告警信息 "]
["SGW35 ",4577,"(4577)直流放电回路异常警告","告警信息 "]
["SGW35 ",4580,"(4580)2U2_频率高警告","告警信息 "]
["SGW35 ",4605,"(4605)2U2_三相电压不平衡警告","告警信息 "]
["SGW35 ",4626,"(4626)有功功率比较警告","告警信息 "]
["SGW35 ",4633,"(4633)2#柜电抗器过温警告","告警信息 "]
["SGW35 ",4654,"(4654)2#网侧电抗器过温警告","告警信息 "]
["SGW35 ",4675,"(4675)2#机侧电压异常警告","告警信息 "]
["SGW35 ",4700,"(4700)主柜预充电模式反馈错误警告","告警信息 "]
["SGW35 ",4721,"(4721)功率柜1除湿器反馈异常警告","告警信息 "]
["SGW35 ",4724,"(4724)1U1_版本校验错误警告","告警信息 "]
["SGW35 ",4749,"(4749)2U3机侧过压过流模块状态异常警告","告警信息 "]
["SGW35 ",4770,"(4770)2U1三相电压不平衡异常提示警告","告警信息 "]
["SGW35 ",4777,"(4777)1U3 三相电流不平衡异常提示警告","告警信息 "]
["SGW35 ",4798,"(4798)2U4_IGBT软件温度低警告","告警信息 "]
["SGW35 ",4819,"(4819)1U2_STACK1_三相电流不平衡警告","告警信息 "]
["SGW35 ",4844,"(4844)2U1_STACK2_过载警告","告警信息 "]
["SGW35 ",4865,"(4865)1U1_STACK2_C相温度不均衡错误警告","告警信息 "]
["SGW35 ",4872,"(4872)2#柜控制器24V蓄电池异常保护警告","告警信息 "]
["SGW35 ",4893,"(4893)1U1参数错误警告","告警信息 "]
["SGW35 ",4914,"(4914)1U1_电流控制异常故障警告","告警信息 "]
["SGW35 ",4921,"(4921)2U1_网侧电压谐波高警告","告警信息 "]
["SGW35 ",4942,"(4942)功率柜2叠排过温错误警告","告警信息 "]
["SGW35 ",4963,"(4963)警告","告警信息 "]
["SGW35 ",4988,"(4988)警告","告警信息 "]
["SGW35 ",5009,"(5009)警告","告警信息 "]
["SGW35 ",5016,"(5016)警告","告警信息 "]
["SGW35 ",5037,"(5037)警告","告警信息 "]
["SGW35 ",5058,"(5058)警告","告警信息 "]
["SGW35 ",5065,"(5065)警告","告警信息 "]
["SGW35 ",5086,"(5086)警告","告警信息 "]
["SGW35 ",5107,"(5107)警告","告警信息 "]
["SGW35 ",5132,"(5132)警告","告警信息 "]
["SGW35 ",5153,"(5153)警告","告警信息 "]
["SGW35 ",5160,"(5160)警告","告警信息 "]
["SGW35 ",5181,"(5181)警告","告警信息 "]
["SGW35 ",5202,"(5202)警告","告警信息 "]
["SGW35 ",5209,"(5209)警告","告警信息 "]
["SGW35 ",5230,"(5230)警告","告警信息 "]
["SGW35 ",5255,"(5255)警告","告警信息 "]
["SGW35 ",5276,"(5276)警告","告警信息 "]
["SGW35 ",5297,"(5297)警告","告警信息 "]
["SGW35 ",5304,"(5304)警告","告警信息 "]
["SGW35 ",5325,"(5325)警告","告警信息 "]
["SGW35 ",5346,"(5346)警告","告警信息 "]
["SGW35 ",5353,"(5353)警告","告警信息 "]
["SGW35 ",5374,"(5374)警告","告警信息 "]
["SGW35 ",5399,"(5399)警告","告警信息 "]
["SGW35 ",5420,"(5420)警告","告警信息 "]
["SGW35 ",5441,"(5441)警告","告警信息 "]
["SGW35 ",5448,"(5448)警告","告警信息 "]
["SGW35 ",5469,"(5469)警告","告警信息 "]
["SGW35 ",5494,"(5494)警告","告警信息 "]
["SGW35 ",5497,"(5497)警告","告警信息 "]
["SGW35 ",5518,"(5518)警告","告警信息 "]
["SGW35 ",5543,"(5543)警告","告警信息 "]
["SGW35 ",5564,"(5564)警告","告警信息 "]
["SGW35 ",5585,"(5585)警告","告警信息 "]
["SGW35 ",5592,"(5592)警告","告警信息 "]
["SGW35 ",5613,"(5613)警告","告警信息 "]
["SGW35 ",5638,"(5638)警告","告警信息 "]
["SGW35 ",5641,"(5641)警告","告警信息 "]
["SGW35 ",5662,"(5662)警告","告警信息 "]
["SGW35 ",5687,"(5687)警告","告警信息 "]
["SGW35 ",5708,"(5708)转速异常震荡警告","告警信息 "]
["SGW35 ",5729,"(5729)2#变桨柜温度传感器异常警告","告警信息 "]
["SGW35 ",5736,"(5736)变流柜温度变化率异常警告","告警信息 "]
["SGW35 ",5792,"(5792)无有功功率需求时有功功率异常警告","告警信息 "]
["SGW38 ",22,"(22)液压系统油位低","故障 "]
["SGW38 ",25,"(25)偏航方向异常","故障 "]
["SGW38 ",46,"(46)变流器功率与上网功率不匹配","故障 "]
["SGW38 ",71,"(71)变压器温度高","故障 "]
["SGW38 ",92,"(92)安全链过速","故障 "]
["SGW38 ",99,"(99)变桨安全链2触发","故障 "]
["SGW38 ",120,"(120)1#变桨子站总线异常","故障 "]
["SGW38 ",141,"(141)发电机绝缘低","故障 "]
["SGW38 ",166,"(166)1#变桨内部安全链","故障 "]
["SGW38 ",169,"(169)1#变桨限位开关触发","告警信息 "]
["SGW38 ",190,"(190)1#变桨电容温度高","故障 "]
["SGW38 ",215,"(215)2#变桨速度比较偏差大","故障 "]
["SGW38 ",236,"(236)2#变桨设定和实际角度偏差大","故障 "]
["SGW38 ",243,"(243)3#变桨位置超限","故障 "]
["SGW38 ",264,"(264)3#变桨极限位置限位开关触发","故障 "]
["SGW38 ",285,"(285)1#变桨电机电流大时间长","故障 "]
["SGW38 ",310,"(310)3#主副编码器位置偏差大","故障 "]
["SGW38 ",313,"(313)3#变桨速度超限","故障 "]
["SGW38 ",334,"(334)3#变桨变频器警告位激活","故障 "]
["SGW38 ",359,"(359)1#变桨欠压","故障 "]
["SGW38 ",380,"(380)1#变桨230VAC和400VAC供电断开","故障 "]
["SGW38 ",387,"(387)2#变桨限位开关触发","故障 "]
["SGW38 ",408,"(408)2#变桨主副旋编位置偏差大","故障 "]
["SGW38 ",429,"(429)进阀压力超低","故障 "]
["SGW38 ",454,"(454)变流器机侧2未调制","故障 "]
["SGW38 ",457,"(457)变流器未调制","故障 "]
["SGW38 ",482,"(421)IGBT风扇1运行异常","故障 "]
["SGW38 ",503,"(442)IGBT_ok丢失","故障 "]
["SGW38 ",524,"(463)制动IGBT温度高","故障 "]
["SGW38 ",531,"(470)斩波升压直流电压高","故障 "]
["SGW38 ",552,"(491)2#变桨直流保险断开","故障 "]
["SGW38 ",573,"(512)2#变桨电容模块过压","故障 "]
["SGW38 ",598,"(537)3#变桨预充电异常","故障 "]
["SGW38 ",601,"(540)3#变桨总线急停","故障 "]
["SGW38 ",626,"(565)1#变桨速度超限","故障 "]
["SGW38 ",647,"(586)2#变桨电机温度高","故障 "]
["SGW38 ",668,"(607)机侧L1b_IGBT温度高","故障 "]
["SGW38 ",675,"预留","提示信息 "]
["SGW38 ",696,"(635)网侧变流器硬件更换","故障 "]
["SGW38 ",721,"(660)变流器柜温超限","故障 "]
["SGW38 ",742,"(681)箱变水冷循环泵工作异常","故障 "]
["SGW38 ",745,"(684)箱变水冷循环泵出口温度低","故障 "]
["SGW38 ",770,"(709)塔底converter UPS电池电量低","故障 "]
["SGW38 ",791,"(730)2#变桨轴承裂纹","故障 "]
["SGW38 ",812,"(751)叶片q轴IPC变桨较高","故障 "]
["SGW38 ",819,"(758)叶片d轴IPC变桨较高","故障 "]
["SGW38 ",840,"预留","提示信息 "]
["SGW38 ",865,"(804)变流器机侧空开断开失败","故障 "]
["SGW38 ",886,"(825)变流器机侧IGBT13_L3B过流","故障 "]
["SGW38 ",889,"预留","提示信息 "]
["SGW38 ",914,"(853)变流器网侧IGBT4_L1B模块故障","故障 "]
["SGW38 ",935,"(874)变流器制动电阻阻值异常","故障 "]
["SGW38 ",956,"预留","提示信息 "]
["SGW38 ",963,"(902)变流器机侧控制失败","故障 "]
["SGW38 ",981,"(920)变流控制器故障11","故障 "]
["SGW38 ",1008,"(947)变流器网侧机侧程序版本不匹配  ","故障 "]
["SGW38 ",3009,"(3009)机舱温度高警告","告警信息 "]
["SGW38 ",3012,"(3012)低压电气柜温度低警告","告警信息 "]
["SGW38 ",3037,"(3037)电网电压不平衡警告","告警信息 "]
["SGW38 ",3058,"(3058)转速比较3警告","告警信息 "]
["SGW38 ",3083,"(3083)水冷系统熔断器反馈丢失警告","告警信息 "]
["SGW38 ",3086,"(3086)机舱柜空调故障反馈丢失警告","告警信息 "]
["SGW38 ",3109,"(3109)变流子站熔断器异常警告","告警信息 "]
["SGW38 ",3136,"(3136)航空灯故障位触发警告","告警信息 "]
["SGW38 ",3163,"(3163)1#变桨发电位置传感器异常警告","告警信息 "]
["SGW38 ",3166,"(3166)1#变桨内部安全链警告","告警信息 "]
["SGW38 ",3191,"(3191)2#变桨电容温度高警告","告警信息 "]
["SGW38 ",3212,"(3212)2#变桨电容高电压高警告","告警信息 "]
["SGW38 ",3237,"(3237)3#变桨设定和实际角度偏差大警告","告警信息 "]
["SGW38 ",3240,"(3240)3#变桨驱动器通讯不正常警告","告警信息 "]
["SGW38 ",3261,"(3261)3#变桨安全位置限位开关触发警告","告警信息 "]
["SGW38 ",3286,"(3286)2#变桨电机电流大时间长警告","告警信息 "]
["SGW38 ",3307,"(3307)3#变桨电机温度高警告","告警信息 "]
["SGW38 ",3314,"(3314)变桨位置比较偏差大警告","告警信息 "]
["SGW38 ",3340,"(3340)3#变桨旋转编码器异常警告","告警信息 "]
["SGW38 ",3361,"(3361)3#变桨欠压警告","告警信息 "]
["SGW38 ",3386,"(3386)1#变桨限位开关触发警告","告警信息 "]
["SGW38 ",3389,"(3389)1#变桨电容直流回路异常警告","告警信息 "]
["SGW38 ",3410,"(3410)变桨3个主旋编位置偏差大警告","告警信息 "]
["SGW38 ",3440,"(3440)水冷流量低警告","告警信息 "]
["SGW38 ",3461,"(3461)变流器调制前rdy_run丢失警告","告警信息 "]
["SGW38 ",3468,"(3468)变流器电机1侧控制器温度高警告","告警信息 "]
["SGW38 ",3491,"(3430)风道加热接触器反馈与指令不一致警告","告警信息 "]
["SGW38 ",3512,"(3451)变流器直流电压高警告","告警信息 "]
["SGW38 ",3537,"(3476)整流二极管温度低警告","告警信息 "]
["SGW38 ",3540,"(3479)塔底主空开检测温度高警告","告警信息 "]
["SGW38 ",3561,"(3500)2#变桨电机电缆异常警告","告警信息 "]
["SGW38 ",3586,"(3525)3#变桨变频器硬件异常警告","告警信息 "]
["SGW38 ",3607,"(3546)3#变桨400V掉电警告","告警信息 "]
["SGW38 ",3614,"(3553)1#变桨散热器温度异常警告","告警信息 "]
["SGW38 ",3635,"(3574)1#变桨安全位置限位开关触发警告","告警信息 "]
["SGW38 ",3664,"(3603)变流器故障触发警告","告警信息 "]
["SGW38 ",3696,"(3635)网侧变流器硬件更换警告","告警信息 "]
["SGW38 ",3699,"(3638)变流器外部异常警告","告警信息 "]
["SGW38 ",3724,"(3663)变流器机侧异常警告","告警信息 "]
["SGW38 ",3770,"(3709)塔底converter UPS电池电量低警告","告警信息 "]
["SGW38 ",3791,"(3730)2#变桨轴承裂纹警告","告警信息 "]
["SGW38 ",3798,"(3737)3#叶片主轴润滑分配器堵塞警告","告警信息 "]
["SGW38 ",3821,"(3760)LUST变桨位置比较偏差大警告","告警信息 "]
["SGW38 ",3885,"(3824)变流器机侧IGBT12_L2B过流警告","告警信息 "]
["SGW38 ",3925,"(3864)变流器机侧IGBT12_L2B模块故障警告","告警信息 "]
["SGW38 ",3932,"(3871)变流器制动IGBT过流(硬件)警告","告警信息 "]
["SGW38 ",3979,"(3918)变流控制器故障9警告","告警信息 "]
["SGW38 ",4008,"(3947)变流器网侧机侧程序版本不匹配 警告","告警信息 "]
["SANY ",32,"塔底柜温度高报警","告警信息 "]
["SANY ",102,"相电压跌落","故障 "]
["SANY ",237,"机舱外温度高停机","告警信息 "]
["SANY ",505,"发电机驱动端轴承温度高停机重复故障","故障 "]
["SANY ",683,"发电机滑环加热器保护开关跳闸","告警信息 "]
["SANY ",707,"顺时针偏航反馈故障停机","故障 "]
["SANY ",935,"发电机风扇2保护开关跳闸","故障 "]
["SANY ",1329,"齿轮箱油加热器保护开关跳闸","故障 "]
["SANY ",1448,"变流器Crowbar故障","故障 "]
["SANY ",1455,"变流器转子接地故障","故障 "]
["SANY ",1476,"变流器电网电压不平衡故障","故障 "]
["SANY ",1503,"定子电压过压","故障 "]
["SANY ",1533,"振动传感器X向振动大于设定值3","故障 "]
["SANY ",1536,"振动传感器Y向振动大于设定值3","故障 "]
["SANY ",1911,"轴2驱动器故障","故障 "]
["SANY ",2070,"400V变压器输入端保护开关跳闸","故障 "]
["SANY ",2451,"能量管理平台停机","告警信息 "]
["SANY ",2468,"市电230V供电异常","告警信息 "]
["SANY ",2639,"轴2 91度限位开关故障","故障 "]
["SANY ",2745,"变流器网侧CPLD故障","故障 "]
["SANY ",2766,"变流器网侧电网故障超时","故障 "]
["SANY ",2769,"变流器机侧直流母线欠压","故障 "]
["SANY ",2794,"变流器机侧相位同步超时","故障 "]
["SANY ",2815,"变流器网侧电抗过温","故障 "]
["SANY ",2822,"变流器辅助电源失压","故障 "]
["SANY ",2843,"变流器塔基风扇故障","故障 "]
["SANY ",2864,"变流器转子防雷告警","告警信息 "]
["SANY ",3201,"变流器电网欠压","故障 "]
["SANY ",3222,"变流器网侧电感过热","故障 "]
["SANY ",3225,"变流器机侧其他故障","故障 "]
["SANY ",3349,"变流器双馈定子电流零序故障","故障 "]
["SANY ",3561,"变桨轴191度限位动作","故障 "]
["SANY ",3568,"变桨轴1心跳反馈异常","故障 "]
["SANY ",3589,"变桨轴3控制器故障","故障 "]
["SANY ",3620,"变桨轴3驱动器24VDC输出电源故障","告警信息 "]
["SANY ",3648,"变桨轴2电机温度高停机","故障 "]
["SANY ",3669,"变桨轴1限位开关A位置角度偏差故障","故障 "]
["SANY ",3672,"变桨轴1限位开关B位置角度偏差故障","故障 "]
["SANY ",3702,"变桨主电源供电>120%过压报警","告警信息 "]
["SANY ",3726,"变桨控制器与客户柜扩展模块通讯故障","故障 "]
["SANY ",3733,"变桨接口模块轴1DC/DC转换单元故障","故障 "]
["SANY ",3820,"算法程序执行超时","故障 "]
["SANY ",3931,"轴2限位开关B激活","告警信息 "]
["SANY ",3956,"轴2电机编码器故障","故障 "]
["SANY ",3977,"轴1桨叶编码器故障","告警信息 "]
["SANY ",3984,"轴1电机与桨叶编码器间超差","故障 "]
["SANY ",4108,"变桨轴1散热板过热报警","故障 "]
["SANY ",4129,"变桨轴1功率模块型号更换","故障 "]
["SANY ",4136,"变桨轴1电机过温提前报警","故障 "]
["SANY ",4157,"变桨轴1电容柜温度过高","故障 "]
["SANY ",4178,"变桨轴1恒速过电流","故障 "]
["SANY ",4204,"变桨轴2直流母排欠压","故障 "]
["SANY ",4225,"变桨轴2C6软件开关拨向右边","故障 "]
["SANY ",4232,"变桨轴2编码器B故障","故障 "]
["SANY ",4253,"变桨轴2电机制动器开路","故障 "]
["SANY ",4274,"变桨轴2驱动器无授权","故障 "]
["SANY ",4281,"变桨轴2恒速过电压","故障 "]
["SANY ",4303,"变桨轴3直流母排过压","故障 "]
["SANY ",4328,"变桨轴3功率模块更换","故障 "]
["SANY ",4349,"变桨轴3超级电容容量检测失败","故障 "]
["SANY ",4370,"变桨轴3直流母排过压提前报警","故障 "]
["SANY ",4377,"变桨轴3减速过电流","故障 "]
["SANY ",4398,"变桨轴3速度偏差过大","故障 "]
["SANY ",4468,"变桨轴3电机抱闸故障","故障 "]
["SANY ",4475,"变桨轴3程序版本不匹配","故障 "]
["SANY ",4518,"轴一超级电容开关断开","故障 "]
["SANY ",4543,"轴二变桨内部安全链断开","故障 "]
["SANY ",4564,"轴二充电器过压","故障 "]
["SANY ",4585,"轴三桨叶位置未校准","故障 "]
["SANY ",4592,"轴三电网掉电","故障 "]
["SANY ",4613,"轴三驱动器I类故障触发","故障 "]
["SYD12 ",130,"电网相角不平衡1","故障 "]
["SYD12 ",1556,"振动模块 1#通道 1 过振 动报警","故障 "]
["SYD12 ",5001,"硬件看门狗触发安全链","故障 "]
["SYD12 ",5113,"电网故障停机","告警信息 "]
["SYD12 ",5302,"平均风速大于切出风速","告警信息 "]
["SYD12 ",5350,"桨叶 2 驱动器外部温度 低","告警信息 "]
["SYD12 ",5403,"桨叶1 和2 的桨距角差值 过大","故障 "]
["SYD12 ",5466,"桨叶 2 最小变桨速度超 限","故障 "]
["SYD12 ",5513,"偏航时间过长","故障 "]
["SYD12 ",5516,"应急偏航动作","故障 "]
["SYD12 ",5617,"齿轮箱高速轴前端轴承 温度高","故障 "]
["SYD12 ",5720,"发电机轴承温度高告警","告警信息 "]
["SYD12 ",5858,"偏航润滑故障","故障 "]
["SYD12 ",5903,"变流器同步失败频繁","故障 "]
["SYD12 ",5904,"机组正常待机","告警信息 "]
["SYD12 ",5905,"变流器通讯故障","故障 "]
["SYD12 ",5906,"变流器低电压穿越禁止","告警信息 "]
["SYD12 ",5920,"机组发电机过转速","故障 "]
["SYD12 ",5921,"机组过功率","故障 "]
["SYD12 ",5922,"小风正常停机","告警信息 "]
["SYD12 ",5923,"启动时发电机过转速","故障 "]
["SYD12 ",5924,"小风机组功率低","告警信息 "]
["SYD12 ",5925,"待机时发电机过转速","故障 "]
["SYD12 ",5926,"手动测试时发电机过转 速","提示信息 "]
["SYD12 ",5927,"转矩不匹配告警","告警信息 "]
["SYD12 ",5928,"运行时高、低速轴转速不匹配","故障 "]
["SYD12 ",5929,"高、低速轴转速不匹配","故障 "]
["SYD12 ",5930,"高速轴转速不匹配","故障 "]
["SYD12 ",5931,"发电机转速变化过快","故障 "]
["SYD12 ",5932,"发电机转速不变化","故障 "]
["SYD12 ",5933,"机组风轮过转速","故障 "]
["SYD12 ",5934,"齿箱低温空转过转速","故障 "]
["SYD12 ",5938,"转矩不匹配频繁","故障 "]
["SYD12 ",5939,"低电压检测不同步告警","告警信息 "]
["SYD12 ",5941,"变流器异常","故障 "]
["SYD12 ",5942,"变流器crowbar 触发告警1","告警信息 "]
["SYD12 ",5943,"变流器告警","告警信息 "]
["SYD12 ",5944,"变流器转矩减载","告警信息 "]
["SYD12 ",5945,"变流器本地控制","告警信息 "]
["SYD12 ",5946,"变流器低电压穿越","告警信息 "]
["SYD12 ",5947,"变流器主断路器故障","故障 "]
["SYD12 ",5948,"变流器内部通讯错误","故障 "]
["SYD12 ",5949,"变流器网侧线电压过压","故障 "]
["SYD12 ",5950,"变流器网侧线电压欠压","故障 "]
["SYD12 ",5951,"变流器网侧过频","故障 "]
["SYD12 ",5952,"变流器网侧欠频","故障 "]
["SYD12 ",5953,"变流器直流母线过压","故障 "]
["SYD12 ",5954,"变流器直流母线欠压","故障 "]
["SYD12 ",5955,"变流器定子过流","故障 "]
["SYD12 ",5956,"变流器转子过流","故障 "]
["SYD12 ",5957,"变流器网侧过流","故障 "]
["SYD12 ",5958,"变流器转子侧过温","故障 "]
["SYD12 ",5959,"变流器网侧过温","故障 "]
["SYD12 ",5960,"变流器监测到机组过转 速","故障 "]
["SYD12 ",5961,"变流器监测到机组欠速","故障 "]
["SYD12 ",5962,"变流器转子侧接地故障","故障 "]
["SYD12 ",5963,"变流器网侧接地故障","故障 "]
["SYD12 ",5964,"变流器与主控通讯失败","故障 "]
["SYD12 ",5965,"变流器接口模块通讯故 障","故障 "]
["SYD12 ",5966,"变流器网侧转子侧通讯 故障","故障 "]
["SYD12 ",5967,"变流器编码器故障","故障 "]
["SYD12 ",5968,"变流器电压和电流测量 单元板故障","故障 "]
["SYD12 ",5969,"变流器转子侧门极驱动 故障","故障 "]
["SYD12 ",5970,"变流器系统故障","故障 "]
["SYD12 ",5971,"变流器转子侧模块启动 故障","故障 "]
["SYD12 ",5972,"变流器网侧模块启动故 障","故障 "]
["SYD12 ",5973,"变流器网侧充电故障","故障 "]
["SYD12 ",5974,"变流器滤波器温度故障","故障 "]
["SYD12 ",5975,"变流器主断路器准备故 障","故障 "]
["SYD12 ",5976,"变流器主断路器反馈故 障","故障 "]
["SYD12 ",5977,"变流器转子侧其它故障","故障 "]
["SYD12 ",5978,"变流器网侧其它故障","故障 "]
["SYD12 ",5979,"变流器crowbar 触发告警","故障 "]
["SYD12 ",5980,"变流器急停触发","故障 "]
["SYD12 ",5981,"变流器网侧模块过温告 警","告警信息 "]
["SYD12 ",5982,"变流器转子侧模块过温 告警","告警信息 "]
["SYD12 ",5983,"变流器转速高告警","告警信息 "]
["SYD12 ",5984,"变流器监听打开告警","告警信息 "]
["SYD12 ",5985,"变流器加热启动","告警信息 "]
["SYD12 ",5986,"变流器柜内过湿告警","告警信息 "]
["SYD12 ",5987,"变流器网侧模块本地控 制告警","告警信息 "]
["SYD12 ",5988,"变流器网侧模块禁止启 动告警","告警信息 "]
["SYD12 ",5989,"变流器 UPS 电量低","告警信息 "]
["SYD12 ",5998,"变流器功率柜过温","故障 "]
["SYD12 ",6005,"变流器高电压穿越","告警信息 "]
["SYD12 ",6018,"变流器并网状态不匹配","故障 "]
["SYD12 ",6101,"能量管理平台通讯故障","告警信息 "]
["SYD12 ",6401,"系统初始化超时","故障 "]
["SYD12 ",6402,"系统初始化变桨待机请 求超时","故障 "]
["SYD12 ",6403,"系统初始化等待超时","故障 "]
["SYD12 ",6404,"系统待机超时","告警信息 "]
["SYD12 ",6405,"等待齿轮箱运转超时","告警信息 "]
["SYD12 ",6406,"等待变流器进入待机状 态超时","故障 "]
["SYD12 ",6407,"等待变桨系统正常工作 超时","故障 "]
["SYD12 ",6408,"启动超时","故障 "]
["SYD12 ",6409,"小风启动变桨超时","故障 "]
["SYD12 ",6410,"大风启动变桨超时","故障 "]
["SYD12 ",6411,"启机等风超时","告警信息 "]
["SYD12 ",6412,"等待同步超时","故障 "]
["SYD12 ",6413,"同步进行中超时","故障 "]
["SYD12 ",6414,"并网进行中超时","故障 "]
["SYD12 ",6415,"并网调整超时","故障 "]
["SYD12 ",6416,"转速&转矩爬升超时","故障 "]
["SYD12 ",6417,"转速爬升超时","故障 "]
["SYD12 ",6418,"转矩二次爬升初始化超 时","故障 "]
["SYD12 ",6419,"转矩爬升超时","故障 "]
["SYD12 ",6420,"转速&转矩下调超时","故障 "]
["SYD12 ",6421,"转矩下调超时","故障 "]
["SYD12 ",6422,"等待发电机转速降到脱 网转速超时","故障 "]
["SYD12 ",6423,"等待发电机脱网超时1","故障 "]
["SYD12 ",6424,"正常停机顺桨超时","故障 "]
["SYD12 ",6425,"快速停机正常超时","故障 "]
["SYD12 ",6426,"快速停机顺桨超时","故障 "]
["SYD12 ",6427,"等待发电机功率降到脱网功率超时1","故障 "]
["SYD12 ",6428,"等待发电机脱网超时2","故障 "]
["SYD12 ",6429,"电网故障停机顺桨超时","故障 "]
["SYD12 ",6430,"变距电池停机顺桨超时","故障 "]
["SYD12 ",6431,"等待发电机功率降到脱 网最大功率超时","故障 "]
["SYD12 ",6432,"等待发电机脱网超时","故障 "]
["SYD12 ",6433,"紧急停机切断看门狗超 时","告警信息 "]
["SYD12 ",6434,"变流器 Lvrt 等待电压恢 复超时","故障 "]
["SYD12 ",6436,"变流器 Lvrt 退出等待超 时","故障 "]
["SYD12 ",6438,"等待发电机功率降到脱 网功率超时","故障 "]
["SYD12 ",6460,"备用电源测试结束进入 超时","故障 "]
["SYD12 ",6470,"齿箱空转等待油温正常 超时","故障 "]
["SYD12 ",6498,"紧急顺桨命令自检失败","故障 "]
["SYD12 ",6499,"EFC 自检测试超时","故障 "]
["SYD12 ",6501,"HMI 手动停机","提示信息 "]
["SYD12 ",6502,"发电机浪涌保护故障","故障 "]
["SYD12 ",6503,"配电浪涌保护反馈超限","故障 "]
["SYD12 ",6504,"风轮锁紧销未退出","故障 "]
["SYD12 ",6505,"机舱手动正常停机","提示信息 "]
["SYD12 ",6506,"机舱防雷故障","故障 "]
["SYD12 ",6507,"UPS 逆变故障","故障 "]
["SYD12 ",6508,"UPS 保护关机","故障 "]
["SYD12 ",6509,"消防系统灭火","故障 "]
["SYD12 ",6511,"消防告警信号","告警信息 "]
["SYD12 ",6518,"风轮不平衡告警","告警信息 "]
["SYD12 ",6601,"禁止标定计算告警","告警信息 "]
["SYD12 ",6602,"调试模式启用告警","告警信息 "]
["SYD12 ",6603,"测试模式待机","故障 "]
["SYD12 ",7019,"电网电压相角偏移告警1","告警信息 "]
["SYD12 ",7020,"电网频率高1","故障 "]
["SYD12 ",7021,"电网频率低1","故障 "]
["SYD12 ",7022,"电网电流不对称1","故障 "]
["SYD12 ",7023,"电网电压高1","故障 "]
["SYD12 ",7024,"电网电压跌落","故障 "]
["SYD12 ",7025,"电网电压相角偏移告警","告警信息 "]
["SYD12 ",7026,"电网电压高","故障 "]
["SYD12 ",7027,"电网电压低","故障 "]
["SYD12 ",7028,"电网频率高","故障 "]
["SYD12 ",7029,"电网频率低","故障 "]
["SYD12 ",7030,"电网相角不平衡","故障 "]
["SYD12 ",7031,"电网电流不对称","故障 "]
["SYD12 ",7200,"电池测试告警","告警信息 "]
["SYD12 ",7201,"桨叶 1 第一次电池测试 故障","告警信息 "]
["SYD12 ",7204,"桨叶 2 第一次电池测试 故障","告警信息 "]
["SYD12 ",7207,"桨叶 3 第一次电池测试 故障","告警信息 "]
["SYD12 ",7210,"备用电源测试失败","故障 "]
["SYD12 ",7211,"桨叶 1 电池测试到零位 故障","告警信息 "]
["SYD12 ",7212,"桨叶 2 电池测试到零位 故障","告警信息 "]
["SYD12 ",7213,"桨叶 3 电池测试到零位 故障","告警信息 "]
["SYD12 ",7215,"电池测试运行","告警信息 "]
["SYD12 ",7300,"塔筒门打开告警","告警信息 "]
["SYD12 ",7513,"振动模块较长时间通讯 故障","故障 "]
["SYD12 ",7523,"振动模块通讯重复故障","故障 "]
["SYD12 ",8041,"机舱求救按钮触发","故障 "]
["SYD12 ",15401,"桨叶 1 电容过压","故障 "]
["SYD12 ",15402,"桨叶 1 电容欠压","故障 "]
["SYD12 ",15403,"桨叶 1 电容温度高","故障 "]
["SYD12 ",15404,"桨叶 1 驱动器温度高","故障 "]
["SYD12 ",15405,"桨叶 1 轴柜温度高","故障 "]
["SYD12 ",15406,"桨叶 1 轴柜温度低","故障 "]
["SYD12 ",15407,"桨叶 1 电机温度高","故障 "]
["SYD12 ",15408,"桨叶 1 电机过流","故障 "]
["SYD12 ",15409,"桨叶 1 编码器卡件故障","故障 "]
["SYD12 ",15411,"桨叶 1 电源管理模块故 障","故障 "]
["SYD12 ",15416,"桨叶 1 桨叶位置值过小","故障 "]
["SYD12 ",15417,"桨叶 1 桨叶位置值过大","故障 "]
["SYD12 ",15418,"桨叶 2 电容过压","故障 "]
["SYD12 ",15419,"桨叶 2 电容欠压","故障 "]
["SYD12 ",15420,"桨叶 2 电容温度高","故障 "]
["SYD12 ",15421,"桨叶 2 驱动器温度高","故障 "]
["SYD12 ",15422,"桨叶 2 轴柜温度高","故障 "]
["SYD12 ",15423,"桨叶 2 轴柜温度低","故障 "]
["SYD12 ",15424,"桨叶 2 电机温度高","故障 "]
["SYD12 ",15425,"桨叶 2 电机过流","故障 "]
["SYD12 ",15426,"桨叶 2 编码器卡件故障1","故障 "]
["SYD12 ",15428,"桨叶 2 电源管理模块故障","故障 "]
["SYD12 ",15433,"桨叶 2 桨叶位置值过小","故障 "]
["SYD12 ",15434,"桨叶 2 桨叶位置值过大","故障 "]
["SYD12 ",15435,"桨叶 3 电容过压","故障 "]
["SYD12 ",15436,"桨叶 3 电容欠压","故障 "]
["SYD12 ",15437,"桨叶 3 电容温度高","故障 "]
["SYD12 ",15438,"桨叶 3 驱动器温度高","故障 "]
["SYD12 ",15439,"桨叶 3 轴柜温度高","故障 "]
["SYD12 ",15440,"桨叶 3 轴柜温度低","故障 "]
["SYD12 ",15441,"桨叶 3 电机温度高","故障 "]
["SYD12 ",15442,"桨叶 3 电机过流","故障 "]
["SYD12 ",15443,"桨叶 3 编码器卡件故障1","故障 "]
["SYD12 ",15445,"桨叶 3 电源管理模块故 障","故障 "]
["SYD12 ",15450,"桨叶 3 桨叶位置值过小","故障 "]
["SYD12 ",15451,"桨叶 3 桨叶位置值过大","故障 "]
["SYD12 ",15452,"桨叶 2 驱动器告警码触 发","故障 "]
["SYD12 ",15453,"桨叶 3 驱动器告警码触 发","故障 "]
["SYD12 ",15454,"桨叶 1 驱动器告警码触 发","故障 "]
["SYD12 ",15455,"桨叶 1 电机制动器继电 器故障","故障 "]
["SYD12 ",15456,"桨叶 2 电机制动器继电 器故障","故障 "]
["SYD12 ",15457,"桨叶 3 电机制动器继电 器故障","故障 "]
["SYD12 ",15600,"桨叶 1 伺服CAN 通讯错 误","故障 "]
["SYD12 ",15601,"桨叶 1 主电源故障","故障 "]
["SYD12 ",15603,"桨叶 1 位置标定错误","故障 "]
["SYD12 ",15604,"桨叶 1 紧急顺桨模式","故障 "]
["SYD12 ",15605,"桨叶 1 位置过小故障","故障 "]
["SYD12 ",15606,"桨叶 1 位置过大故障","故障 "]
["SYD12 ",15607,"桨叶 1 90 度传感器故障","故障 "]
["SYD12 ",15608,"桨叶 1 3 度传感器故障","故障 "]
["SYD12 ",15609,"桨叶 1  编码器卡件故障","故障 "]
["SYD12 ",15610,"桨叶 1 变桨电机超速","故障 "]
["SYD12 ",15611,"桨叶 1 安全链故障","故障 "]
["SYD12 ",15614,"桨叶 1 变桨电机堵转故 障","故障 "]
["SYD12 ",15615,"桨叶 1 驱动器温度过高","故障 "]
["SYD12 ",15616,"桨叶 1 轴柜温度过高","故障 "]
["SYD12 ",15617,"桨叶 1 超级电容模组中间点电压故障","故障 "]
["SYD12 ",15618,"桨叶 1 变桨电机过温且 堵转故障","故障 "]
["SYD12 ",15619,"桨叶 1 手动操作允许","故障 "]
["SYD12 ",15620,"桨叶 1 手动运行","故障 "]
["SYD12 ",15622,"桨叶 1 限位开关触发","故障 "]
["SYD12 ",15623,"桨叶 1 变桨电机温度过 高","故障 "]
["SYD12 ",15700,"桨叶 2 伺服CAN 通讯错 误","故障 "]
["SYD12 ",15701,"桨叶 2 主电源 400V 故障","故障 "]
["SYD12 ",15703,"桨叶 2 位置标定错误","故障 "]
["SYD12 ",15704,"桨叶 2 紧急顺桨模式","故障 "]
["SYD12 ",15705,"桨叶 2 位置过小故障","故障 "]
["SYD12 ",15706,"桨叶 2 位置过大故障","故障 "]
["SYD12 ",15707,"桨叶 2 90 度传感器故障","故障 "]
["SYD12 ",15708,"桨叶 2 3 度传感器故障","故障 "]
["SYD12 ",15709,"桨叶 2 编码器卡件故障","故障 "]
["SYD12 ",15710,"桨叶 2 变桨电机超速","故障 "]
["SYD12 ",15711,"桨叶 2 安全链故障","故障 "]
["SYD12 ",15714,"桨叶 2 变桨电机堵转故 障","故障 "]
["SYD12 ",15715,"桨叶 2 驱动器温度过高","故障 "]
["SYD12 ",15716,"桨叶 2 轴柜温度过高","故障 "]
["SYD12 ",15717,"桨叶 2 超级电容模组中 间点电压故障","故障 "]
["SYD12 ",15718,"桨叶 2 变桨电机过温且 堵转故障","故障 "]
["SYD12 ",15719,"桨叶 2 手动操作允许","故障 "]
["SYD12 ",15720,"桨叶 2 手动运行","故障 "]
["SYD12 ",15721,"桨叶 2 限位开关触动触 发","故障 "]
["SYD12 ",15723,"桨叶 2 变桨电机温度过 高","故障 "]
["SYD12 ",15800,"桨叶 3 伺服CAN 通讯错 误","故障 "]
["SYD12 ",15801,"桨叶 3 主电源 400V 超限","故障 "]
["SYD12 ",15803,"桨叶 3 位置标定错误","故障 "]
["SYD12 ",15804,"桨叶 3 紧急顺桨模式","故障 "]
["SYD12 ",15805,"桨叶 3 位置过小故障","故障 "]
["SYD12 ",15806,"桨叶 3 位置过大故障","故障 "]
["SYD12 ",15807,"桨叶 3 90 度传感器故障","故障 "]
["SYD12 ",15808,"桨叶 3 3 度传感器故障","故障 "]
["SYD12 ",15809,"桨叶 3 编码器卡件故障","故障 "]
["SYD12 ",15810,"桨叶 3 变桨电机超速","故障 "]
["SYD12 ",15811,"桨叶 3 安全链故障","故障 "]
["SYD12 ",15814,"桨叶 3 变桨电机堵转故 障","故障 "]
["SYD12 ",15815,"桨叶 3 驱动器温度过高","故障 "]
["SYD12 ",15816,"桨叶 3 轴柜温度过高","故障 "]
["SYD12 ",15817,"桨叶 3 超级电容模组中 间点电压故障","故障 "]
["SYD12 ",15818,"桨叶 3 变桨电机过温且 堵转故障","故障 "]
["SYD12 ",15819,"桨叶 3 手动操作允许","故障 "]
["SYD12 ",15820,"桨叶 3 手动运行","故障 "]
["SYD12 ",15821,"桨叶 3 限位开关触发","故障 "]
["SYD12 ",15822,"变桨系统初始化失败","故障 "]
["SYD12 ",15823,"桨叶 3 变桨电机温度过 高","故障 "]
["SYD12 ",15824,"变桨润滑故障","故障 "]
["SYD12 ",15825,"轴柜 1 4K1 继电器触发 次数告警","告警信息 "]
["SYD12 ",15826,"轴柜 2 4K1 继电器触发 次数告警","告警信息 "]
["SYD12 ",15827,"轴柜 3 4K1 继电器触发 次数告警","告警信息 "]
["SYD12 ",15828,"轴柜 1 4K8 继电器触发 次数告警","告警信息 "]
["SYD12 ",15829,"轴柜 2 4K8 继电器触发 次数告警","告警信息 "]
["SYD12 ",15830,"轴柜 3 4K8 继电器触发 次数告警","告警信息 "]
["SYD12 ",15834,"桨叶 1 主控侧变桨通讯 故障","故障 "]
["SYD12 ",15835,"桨叶 2 主控侧变桨通讯 故障","故障 "]
["SYD12 ",15836,"桨叶 3 主控侧变桨通讯 故障","故障 "]
["SYD12 ",15837,"变桨系统温度未到达","告警信息 "]
["SYD12 ",15838,"桨叶 1 变桨自学习未完 成","故障 "]
["SYD12 ",15839,"桨叶 2 变桨自学习未完 成","故障 "]
["SYD12 ",15840,"桨叶 3 变桨自学习未完 成","故障 "]
["SYD12 ",15851,"顺桨到位信号与桨距角 不匹配","故障 "]
["SYD12 ",16001,"轴 1 驱动器故障","故障 "]
["SYD12 ",16002,"轴 2 驱动器故障","故障 "]
["SYD12 ",16003,"轴 3 驱动器故障","故障 "]
["SYD12 ",16004,"轴 1CAN 通讯拨码错误","故障 "]
["SYD12 ",16005,"轴 2CAN 通讯拨码错误","故障 "]
["SYD12 ",16006,"轴 3CAN 通讯拨码错误","故障 "]
["SYD12 ",16007,"轴 1 电机过载提前告警 （OL1）","故障 "]
["SYD12 ",16008,"轴 2 电机过载提前告警 （OL1）","故障 "]
["SYD12 ",16009,"轴 3 电机过载提前告警 （OL1）","故障 "]
["SYD12 ",16010,"轴 1 电机过温","故障 "]
["SYD12 ",16011,"轴 2 电机过温","故障 "]
["SYD12 ",16012,"轴 3 电机过温","故障 "]
["SYD12 ",16013,"轴 1 驱动器散热板过温","故障 "]
["SYD12 ",16014,"轴 2 驱动器散热板过温","故障 "]
["SYD12 ",16015,"轴 3 驱动器散热板过温","故障 "]
["SYD12 ",16016,"轴 1 伺服内部过温","故障 "]
["SYD12 ",16017,"轴 2 伺服内部过温","故障 "]
["SYD12 ",16018,"轴 3 伺服内部过温","故障 "]
["SYD12 ",16019,"轴 1 伺服内部风扇故障","告警信息 "]
["SYD12 ",16020,"轴 2 伺服内部风扇故障","告警信息 "]
["SYD12 ",16021,"轴 3 伺服内部风扇故障","告警信息 "]
["SYD12 ",16022,"轴 1 伺服柜外风扇故障","告警信息 "]
["SYD12 ",16023,"轴 2 伺服柜外风扇故障","告警信息 "]
["SYD12 ",16024,"轴 3 伺服柜外风扇故障","告警信息 "]
["SYD12 ",16025,"轴 1 86°接近开关异常","告警信息 "]
["SYD12 ",16026,"轴 2 86°接近开关异常","告警信息 "]
["SYD12 ",16027,"轴 3 86°接近开关异常","告警信息 "]
["SYD12 ",16028,"轴 1 5°接近开关异常","告警信息 "]
["SYD12 ",16029,"轴 2 5°接近开关异常","告警信息 "]
["SYD12 ",16030,"轴 3 5°接近开关异常","告警信息 "]
["SYD12 ",16031,"轴 1 电容充电时间过长","告警信息 "]
["SYD12 ",16032,"轴 2 电容充电时间过长","告警信息 "]
["SYD12 ",16033,"轴 3 电容充电时间过长","告警信息 "]
["SYD12 ",16034,"轴 1 主电源掉电","故障 "]
["SYD12 ",16035,"轴 2 主电源掉电","故障 "]
["SYD12 ",16036,"轴 3 主电源掉电","故障 "]
["SYD12 ",16037,"轴 1 桨叶位置值过小","故障 "]
["SYD12 ",16038,"轴 2 桨叶位置值过小","故障 "]
["SYD12 ",16039,"轴 3 桨叶位置值过小","故障 "]
["SYD12 ",16040,"轴 1 桨叶位置值过大","故障 "]
["SYD12 ",16041,"轴 2 桨叶位置值过大","故障 "]
["SYD12 ",16042,"轴 3 桨叶位置值过大","故障 "]
["SYD12 ",16043,"轴 1 超级电容充电失效 或老化","故障 "]
["SYD12 ",16044,"轴 2 超级电容充电失效 或老化","故障 "]
["SYD12 ",16045,"轴 3 超级电容充电失效 或老化","故障 "]
["SYD12 ",16046,"轴 1 超级电容过压","故障 "]
["SYD12 ",16047,"轴 2 超级电容过压","故障 "]
["SYD12 ",16048,"轴 3 超级电容过压","故障 "]
["SYD12 ",16049,"轴 1 超级电容欠压","故障 "]
["SYD12 ",16050,"轴 2 超级电容欠压","故障 "]
["SYD12 ",16051,"轴 3 超级电容欠压","故障 "]
["SYD12 ",16052,"轴 1 超级电容容量检测 失败","告警信息 "]
["SYD12 ",16053,"轴 2 超级电容容量检测 失败","告警信息 "]
["SYD12 ",16054,"轴 3 超级电容容量检测 失败","告警信息 "]
["SYD12 ",16055,"轴 1 超级电容未连接","故障 "]
["SYD12 ",16056,"轴 2 超级电容未连接","故障 "]
["SYD12 ",16057,"轴 3 超级电容未连接","故障 "]
["SYD12 ",16058,"轴 1 超级电容容量低","告警信息 "]
["SYD12 ",16059,"轴 2 超级电容容量低","告警信息 "]
["SYD12 ",16060,"轴 3 超级电容容量低","告警信息 "]
["SYD12 ",16061,"轴 1 主电源接触器异常 （仅限轴 1）","故障 "]
["SYD12 ",16062,"轴 1 驱动器主电源缺相故障","故障 "]
["SYD12 ",16063,"轴 2 驱动器主电源缺相 故障","故障 "]
["SYD12 ",16064,"轴 3 驱动器主电源缺相 故障","故障 "]
["SYD12 ",16065,"轴 1 抱闸回路故障","故障 "]
["SYD12 ",16066,"轴 2 抱闸回路故障","故障 "]
["SYD12 ",16067,"轴 3 抱闸回路故障","故障 "]
["SYD12 ",16068,"轴 1 主控硬件安全链断 开（仅限轴 1）","告警信息 "]
["SYD12 ",16069,"轴 1 刹车制动力矩不足","故障 "]
["SYD12 ",16070,"轴 2 刹车制动力矩不足","故障 "]
["SYD12 ",16071,"轴 3 刹车制动力矩不足","故障 "]
["SYD12 ",16072,"轴 1 控制柜温度超限","告警信息 "]
["SYD12 ",16073,"轴 2 控制柜温度超限","告警信息 "]
["SYD12 ",16074,"轴 3 控制柜温度超限","告警信息 "]
["SYD12 ",16075,"轴 1 电容柜温度超限","告警信息 "]
["SYD12 ",16076,"轴 2 电容柜温度超限","告警信息 "]
["SYD12 ",16077,"轴 3 电容柜温度超限","告警信息 "]
["SYD12 ",16078,"轴 1 轮毂温度超限（仅限 轴 1）","告警信息 "]
["SYD12 ",16079,"轴 1 电机 KTY 接线异常","故障 "]
["SYD12 ",16080,"轴 2 电机 KTY 接线异常","故障 "]
["SYD12 ",16081,"轴 3 电机 KTY 接线异常","故障 "]
["SYD12 ",16082,"轴 1 驱动器与主控通信 故障","故障 "]
["SYD12 ",16083,"轴 2 驱动器与主控通信 故障","故障 "]
["SYD12 ",16084,"轴 3 驱动器与主控通信 故障","故障 "]
["SYD12 ",16085,"轴 1 驱动器内部通讯故 障","故障 "]
["SYD12 ",16086,"轴 2 驱动器内部通讯故 障","故障 "]
["SYD12 ",16087,"轴 3 驱动器内部通讯故 障","故障 "]
["SYD12 ",16088,"轴 1 变桨速度过快","故障 "]
["SYD12 ",16089,"轴 2 变桨速度过快","故障 "]
["SYD12 ",16090,"轴 3 变桨速度过快","故障 "]
["SYD12 ",16091,"轴 1 变桨电机堵转","故障 "]
["SYD12 ",16092,"轴 2 变桨电机堵转","故障 "]
["SYD12 ",16093,"轴 3 变桨电机堵转","故障 "]
["SYD12 ",16094,"轴 1 驱动器 400V 辅助触 点断开","告警信息 "]
["SYD12 ",16095,"轴 2 驱动器 400V 辅助触 点断开","告警信息 "]
["SYD12 ",16096,"轴 3 驱动器 400V 辅助触 点断开","告警信息 "]
["SYD12 ",16097,"轴 1 电机超温且堵转","故障 "]
["SYD12 ",16098,"轴 2 电机超温且堵转","故障 "]
["SYD12 ",16099,"轴 3 电机超温且堵转","故障 "]
["SYD12 ",16100,"轴 1 旋转变压器故障","故障 "]
["SYD12 ",16101,"轴 2 旋转变压器故障","故障 "]
["SYD12 ",16102,"轴 3 旋转变压器故障","故障 "]
["SYD12 ",16103,"轴 1 防雷模块动作（仅限 轴 1）","故障 "]
["SYD12 ",16104,"轴 1 超级电容禁止充电","告警信息 "]
["SYD12 ",16105,"轴 2 超级电容禁止充电","告警信息 "]
["SYD12 ",16106,"轴 3 超级电容禁止充电","告警信息 "]
["SYD12 ",16107,"轴 1 电机电缆开路","故障 "]
["SYD12 ",16108,"轴 2 电机电缆开路","故障 "]
["SYD12 ",16109,"轴 3 电机电缆开路","故障 "]
["SYD12 ",16110,"轴 1DO 输出过载","故障 "]
["SYD12 ",16111,"轴 2DO 输出过载","故障 "]
["SYD12 ",16112,"轴 3DO 输出过载","故障 "]
["SYD12 ",16113,"轴 1 直流母线过压","故障 "]
["SYD12 ",16114,"轴 2 直流母线过压","故障 "]
["SYD12 ",16115,"轴 3 直流母线过压","故障 "]
["SYD12 ",16116,"轴 1 系统安全链断开","故障 "]
["SYD12 ",16117,"轴 2 系统安全链断开","故障 "]
["SYD12 ",16118,"轴 3 系统安全链断开","故障 "]
["SYD12 ",16119,"轴 1 电容回路主开关断 开","故障 "]
["SYD12 ",16120,"轴 2 电容回路主开关断 开","故障 "]
["SYD12 ",16121,"轴 3 电容回路主开关断 开","故障 "]
["SYD12 ",16122,"轴 1 硬件使能信号误触 发","故障 "]
["SYD12 ",16123,"轴 2 硬件使能信号误触 发","故障 "]
["SYD12 ",16124,"轴 3 硬件使能信号误触 发","故障 "]
["SYD12 ",16125,"轴 1 电网过压","故障 "]
["SYD12 ",16126,"轴 2 电网过压","故障 "]
["SYD12 ",16127,"轴 3 电网过压","故障 "]
["SYD12 ",16128,"轴 1 相对湿度过大","告警信息 "]
["SYD12 ",16129,"轴 2 相对湿度过大","告警信息 "]
["SYD12 ",16130,"轴 3 相对湿度过大","告警信息 "]
["SYD12 ",16131,"轴 3 润滑油泵故障（仅限 轴 3）","告警信息 "]
["SYD12 ",16132,"轴 1 91 度限位开关触发","故障 "]
["SYD12 ",16133,"轴 2 91 度限位开关触发","故障 "]
["SYD12 ",16134,"轴 3 91 度限位开关触发","故障 "]
["SYD12 ",16135,"轴 1 95 度限位开关触发","故障 "]
["SYD12 ",16136,"轴 2 95 度限位开关触发","故障 "]
["SYD12 ",16137,"轴 3 95 度限位开关触发","故障 "]
["SYD12 ",16138,"轴 1 接近开关故障","故障 "]
["SYD12 ",16139,"轴 2 接近开关故障","故障 "]
["SYD12 ",16140,"轴 3 接近开关故障","故障 "]
["SYD12 ",16141,"轴 1 柜内加热器异常","告警信息 "]
["SYD12 ",16142,"轴 2 柜内加热器异常","告警信息 "]
["SYD12 ",16143,"轴 3 柜内加热器异常","告警信息 "]
["SYD12 ",16144,"轴 1 变桨初始化失败","故障 "]
["SYD12 ",16145,"轴 2 变桨初始化失败","故障 "]
["SYD12 ",16146,"轴 3 变桨初始化失败","故障 "]
["SYD12 ",16147,"变桨抗涡激模式激活","故障 "]
["SYD12 ",40170,"模块 1.1 故障","故障 "]
["SYD12 ",40171,"模块 1.1 状态故障","故障 "]
["SYD12 ",40172,"模块 1.1 温度高","故障 "]
["SYD12 ",40173,"模块1.1 正常运行时间未 发送","故障 "]
["SYD12 ",40174,"模块 1.1 虚拟","故障 "]
["SYD12 ",40180,"模块 1.2 故障","故障 "]
["SYD12 ",40181,"模块 1.2 状态故障","故障 "]
["SYD12 ",40182,"模块 1.2 温度高","故障 "]
["SYD12 ",40183,"模块1.2 正常运行时间未 发送","故障 "]
["SYD12 ",40184,"模块 1.2 虚拟","故障 "]
["SYD12 ",40190,"模块 1.3 故障","故障 "]
["SYD12 ",40191,"模块 1.3 状态故障","故障 "]
["SYD12 ",40192,"模块 1.3 温度高","故障 "]
["SYD12 ",40193,"模块1.3 正常运行时间未 发送","故障 "]
["SYD12 ",40194,"模块 1.3 虚拟","故障 "]
["SYD12 ",40200,"模块 1.4 故障","故障 "]
["SYD12 ",40201,"模块 1.4 状态故障","故障 "]
["SYD12 ",40202,"模块 1.4 温度高","故障 "]
["SYD12 ",40203,"模块1.4 正常运行时间未 发送","故障 "]
["SYD12 ",40204,"模块 1.4 虚拟","故障 "]
["SYD12 ",40330,"模块 2.1 故障","故障 "]
["SYD12 ",40331,"模块 2.1 状态故障","故障 "]
["SYD12 ",40332,"模块 2.1 温度高","故障 "]
["SYD12 ",40333,"模块2.1 正常运行时间未 发送","故障 "]
["SYD12 ",40334,"模块 2.1 虚拟","故障 "]
["SYD12 ",40490,"模块 3.1 故障","故障 "]
["SYD12 ",40491,"模块 3.1 状态故障","故障 "]
["SYD12 ",40492,"模块 3.1 温度高","故障 "]
["SYD12 ",40493,"模块3.1 正常运行时间未 发送","故障 "]
["SYD12 ",40494,"模块 3.1 虚拟","故障 "]
["SYD12 ",40500,"模块 3.2 故障","故障 "]
["SYD12 ",40501,"模块 3.2 状态故障","故障 "]
["SYD12 ",40502,"模块 3.2 温度高","故障 "]
["SYD12 ",40503,"模块3.2 正常运行时间未 发送","故障 "]
["SYD12 ",40504,"模块 3.2 虚拟","故障 "]
["SYD12 ",40510,"模块 3.3 故障","故障 "]
["SYD12 ",40511,"模块 3.3 状态故障","故障 "]
["SYD12 ",40512,"模块 3.3 温度高","故障 "]
["SYD12 ",40513,"模块3.3 正常运行时间未 发送","故障 "]
["SYD12 ",40514,"模块 3.3 虚拟","故障 "]
["SYD12 ",40650,"模块 4.1 故障","故障 "]
["SYD12 ",40651,"模块 4.1 状态故障","故障 "]
["SYD12 ",40652,"模块 4.1 温度高","故障 "]
["SYD12 ",40653,"模块4.1 正常运行时间未发送","故障 "]
["SYD12 ",40654,"模块 4.1 虚拟","故障 "]
["SYD12 ",41600,"软硬件不兼容告警","告警信息 "]
["SYD12 ",41601,"软硬件不兼容错误","故障 "]
["SYD12 ",64000,"主控制器温度过高","故障 "]
["SYD12 ",64001,"主控制器电源电压过低 (OS)","故障 "]
["SYD12 ",64002,"主控制器备用电源电压 过低(OS)","故障 "]
["SYD12 ",64003,"文件系统故障(OS)","故障 "]
["SYD12 ",64010,"系统启动中（OS）","故障 "]
["SYD12 ",64011,"手动重启(OS)","告警信息 "]
["SYD12 ",64012,"主控制器电源故障关机 (OS)","故障 "]
["SYD12 ",64013,"软件看门狗关机(OS)","故障 "]
["SYD12 ",64014,"硬件看门狗关机(OS)","故障 "]
["SYD12 ",64015,"主控制器电源上电或硬 件复位(OS)","告警信息 "]
["SYD12 ",64016,"未知原因关机(OS)","故障 "]
["SYD12 ",64017,"手动关机(OS)","告警信息 "]
["SYD12 ",64018,"关机(OS)","告警信息 "]
["SYD12 ",64019,"应用程序没有加载(OS)","故障 "]
["SYD12 ",64020,"主控制器安全链输出丢失(OS)","故障 "]
["SYD12 ",64021,"主控制器内部继电器 1 持续通(OS)","故障 "]
["SYD12 ",64022,"主控制器内部继电器 1 持续断(OS)","故障 "]
["SYD12 ",64023,"主控制器内部继电器 2 持续通(OS)","故障 "]
["SYD12 ",64024,"主控制器内部继电器 2 持续断(OS)","故障 "]
["SYD12 ",64025,"主控制器安全链输入丢 失(OS)","故障 "]
["SYD12 ",64026,"WP-Line 模块初始化故 障(OS)","故障 "]
["SYD12 ",64027,"WP-Line 模块配置故障 (OS)","故障 "]
["SYD12 ",64028,"WP-Line 配置调整(OS)","故障 "]
["SYD12 ",64029,"系统告警(OS)","告警信息 "]
["SYD12 ",64030,"系统故障(OS)","故障 "]
["SYD12 ",64031,"系统软件需要更新","告警信息 "]
["SYD12 ",64032,"请求系统重启(OS)","故障 "]
["SYD12 ",64033,"应用程序请求重启(OS)","故障 "]
["SYD12 ",64035,"IO 告警(OS)","故障 "]
["SYD12 ",64036,"看门狗超时(OS)","故障 "]
["SYD12 ",64037,"非正常关机(OS)","故障 "]
["SYD12 ",64038,"系统重复错误(OS)","故障 "]
["SYD12 ",70001,"高速制动器温度高","故障 "]
["SYD12 ",70002,"高速制动器温度过高","故障 "]