{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":9818,"n_cols":8,"rows_kept":9818,"cut":false,"hidden":false,"merged":[]}
["风场id","风场名称","标准机型","原始机型","风速","有功功率","描述","空气密度"]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",0,0,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",0.5,0,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",1,0,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",1.5,0,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",2,0,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",2.5,0,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",3,10,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",3.5,20.5,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",4,31,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",4.5,54.5,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",5,78,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",5.5,113,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",6,148,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",6.5,195.5,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",7,243,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",7.5,306,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",8,369,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",8.5,447,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",9,525,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",9.5,610,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",10,695,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",10.5,746,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",11,797,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",11.5,816.5,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",12,836,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",12.5,841.5,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",13,847,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",13.5,848,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",14,849,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",14.5,846.5,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",15,844,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",15.5,847,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",16,850,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",16.5,850,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",17,850,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",17.5,850,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",18,850,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",18.5,850,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",19,850,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",19.5,850,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",20,850,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",20.5,850,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",21,850,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",21.5,850,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","G58-850","G58",22,850,"吉林双辽歌美飒G58-850机型当地空气密度曲线",1.225]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",0,0,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",0.5,0,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",1,0,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",1.5,0,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",2,0,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",2.5,0,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",3,45,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",3.5,91,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",4,170,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",4.5,268,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",5,383,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",5.5,510,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",6,661,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",6.5,842,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",7,1048,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",7.5,1279,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",8,1465,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",8.5,1641,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",9,1773,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",9.5,1851,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",10,1942,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",10.5,1974,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",11,1997,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",11.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",12,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",12.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",13,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",13.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",14,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",14.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",15,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",15.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",16,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",16.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",17,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",17.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",18,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",18.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",19,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",19.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",20,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",20.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",21,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",21.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",22,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",22.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",23,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",23.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",24,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",24.5,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","MY2.0se-121","MY2.0se-121",25,2000,"广西马王MY2.0SE-121功率曲线",1.103]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",0,0,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",0.5,0,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",1,0,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",1.5,0,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",2,0,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",2.5,0,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",3,49,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",3.5,116,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",4,182,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",4.5,297,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",5,411,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",5.5,561,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",6,711,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",6.5,919,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",7,1126,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",7.5,1350,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",8,1574,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",8.5,1740,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",9,1905,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",9.5,1951,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",10,1997,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",10.5,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",11,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",11.5,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",12,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",12.5,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",13,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",13.5,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",14,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",14.5,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",15,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",15.5,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",16,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",16.5,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",17,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",17.5,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",18,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",18.5,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",19,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",19.5,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["JofPf4O2","河南博创风电场","MY2.0se-121","MY2.0se-121",20,2000,"河南博创风电场机型MY2.0se-121当地空气密度功率曲线",1.232]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",0,0,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",0.5,0,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",1,0,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",1.5,0,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",2,0,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",2.5,0,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",3,15,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",3.5,103,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",4,241,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",4.5,406,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",5,602,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",5.5,841,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",6,1106,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",6.5,1408,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",7,1757,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",7.5,2162,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",8,2622,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",8.5,3031,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",9,3379,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",9.5,3691,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",10,3963,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",10.5,4231,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",11,4496,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",11.5,4734,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",12,4939,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",12.5,5128,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",13,5288,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",13.5,5392,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",14,5449,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",14.5,5486,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",15,5500,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",15.5,5500,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",16,5500,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",16.5,5500,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",17,5500,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",17.5,5500,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",18,5500,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",18.5,5500,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",19,5500,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",19.5,5500,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["hKTaW7gl","四川则洛日风电场","DEW-G5500-183","DEW-G5500-183",20,5500,"四川则洛日风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",0,0,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",0.5,0,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",1,0,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",1.5,0,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",2,0,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",2.5,49,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",3,119,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",3.5,231,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",4,392,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",4.5,580,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",5,802,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",5.5,1068,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",6,1386,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",6.5,1763,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",7,2202,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",7.5,2707,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",8,3277,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",8.5,3767,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",9,3924,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",9.5,3975,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",10,3992,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",10.5,3996,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",11,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",11.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",12,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",12.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",13,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",13.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",14,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",14.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",15,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",15.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",16,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",16.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",17,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",17.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",18,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",18.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",19,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",19.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",20,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",20.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",21,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",21.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",22,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",22.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",23,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",23.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",24,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",24.5,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY4.0se-166","MY4.0se-166",25,4000,"云南金龙山风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",0,0,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",0.5,0,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",1,0,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",1.5,0,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",2,0,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",2.5,0,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",3,8,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",3.5,4,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",4,15,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",4.5,31,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",5,46,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",5.5,68,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",6,90,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",6.5,119,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",7,148,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",7.5,185,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",8,222,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",8.5,264,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",9,306,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",9.5,354,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",10,401,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",10.5,449,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",11,498,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",11.5,541,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",12,584,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",12.5,618,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",13,652,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",13.5,678,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",14,704,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",14.5,719,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",15,734,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",15.5,742,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",16,750,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",16.5,753,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",17,755,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",17.5,753,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",18,751,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",18.5,747,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",19,743,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",19.5,738,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",20,733,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",20.5,727,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",21,722,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",21.5,717,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",22,709,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",22.5,704,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",23,704,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",23.5,704,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",24,704,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",24.5,704,"图古风电场S48-750当地空气密度功率曲线",1.122]
["JzjvvD9l","内蒙图古风电场","S48-750","GW-48/0.75",25,704,"图古风电场S48-750当地空气密度功率曲线",1.122]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",3,65.31,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",3.5,155.48,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",4,245.65,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",4.5,400.54,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",5,555.43,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",5.5,750.37,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",6,945.3,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",6.5,1204.84,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",7,1464.38,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",7.5,1819.23,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",8,2174.08,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",8.5,2575.28,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",9,2976.47,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",9.5,3155.98,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",10,3335.49,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",10.5,3342.62,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",11,3349.76,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",11.5,3350.12,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",12,3350.49,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",12.5,3350.89,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",13,3351.3,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",13.5,3351.34,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",14,3351.38,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",14.5,3350.88,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",15,3350.38,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",15.5,3350.61,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",16,3350.84,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",16.5,3350.21,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",17,3349.63,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",17.5,3350.32,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",18,3350.29,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",18.5,3349.21,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",19,3348.14,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",19.5,3348.14,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["ph0YFc0H","江苏滨海风电场","GW140-3300","GW140/3300",20,3348.39,"海洋滨海金风GW140/3300机型当地空气密度曲线",1.21]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",0,0,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",0.5,0,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",1,0,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",1.5,0,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",2,0,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",2.5,0,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",3,24.75,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",3.5,49.75,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",4,83.5,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",4.5,124.5,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",5,170.25,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",5.5,235,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",6,307.75,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",6.5,393.25,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",7,492.75,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",7.5,605.25,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",8,729,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",8.5,859.25,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",9,988,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",9.5,1104.5,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",10,1209.5,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",10.5,1296.75,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",11,1354,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",11.5,1396.5,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",12,1428.5,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",12.5,1463.75,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",13,1483,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",13.5,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",14,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",14.5,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",15,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",15.5,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",16,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",16.5,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",17,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",17.5,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",18,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",18.5,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",19,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",19.5,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",20,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["S0reB7Dy","黑龙江双岭风电场","GW82-1500","GW82/1500",20.5,1500,"黑龙江双岭风电场GW82/1500机型当地空气密度曲线",1.122]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",0,0,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",0.5,0,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",1,0,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",1.5,0,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",2,0,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",2.5,0,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",3,47,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",3.5,100,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",4,156,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",4.5,224,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",5,309,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",5.5,410,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",6,530,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",6.5,669,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",7,825,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",7.5,990,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",8,1157,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",8.5,1325,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",9,1487,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",9.5,1635,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",10,1773,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",10.5,1878,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",11,1952,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",11.5,1990,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",12,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",12.5,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",13,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",13.5,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",14,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",14.5,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",15,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",15.5,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",16,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",16.5,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",17,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",17.5,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",18,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",18.5,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",19,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",19.5,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",20,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",20.5,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",21,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",21.5,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",22,2000,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",22.5,0,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",23,0,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",23.5,0,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",24,0,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",24.5,0,"河南荆山上海电气w2000N-111-80本地",1.129]
["LtlqU7z4","河南荆山风电场","W2000-111","w2000N-111-80",25,0,"河南荆山上海电气w2000N-111-80本地",1.129]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",0,0,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",0.5,0,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",1,0,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",1.5,0,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",2,0,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",2.5,0,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",3,25,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",3.5,44,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",4,71,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",4.5,106,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",5,148,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",5.5,199,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",6,259,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",6.5,331,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",7,414,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",7.5,509,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",8,617,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",8.5,737,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",9,858,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",9.5,967,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",10,1068,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",10.5,1166,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",11,1254,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",11.5,1323,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",12,1375,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",12.5,1415,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",13,1444,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",13.5,1462,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",14,1473,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",14.5,1481,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",15,1488,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",15.5,1495,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",16,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",16.5,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",17,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",17.5,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",18,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",18.5,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",19,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",19.5,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",20,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",20.5,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",21,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",21.5,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",22,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",22.5,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",23,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",23.5,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",24,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",24.5,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","GW82-1500","GW82-1500",25,1500,"山西利民金风科技GW82-1500风机功率曲线",1.027]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",0,0,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",0.5,0,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",1,0,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",1.5,0,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",2,0,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",2.5,0,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",3,0,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",3.5,25,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",4,78,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",4.5,147,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",5,270,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",5.5,422,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",6,601,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",6.5,816,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",7,1068,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",7.5,1370,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",8,1716,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",8.5,2044,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",9,2386,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",9.5,2596,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",10,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",10.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",11,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",11.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",12,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",12.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",13,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",13.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",14,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",14.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",15,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",15.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",16,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",16.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",17,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",17.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",18,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",18.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",19,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",19.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",20,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",20.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",21,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",21.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",22,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",22.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",23,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",23.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",24,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",24.5,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",25,2650,"安徽唐古风电场EN-141/2.65机型当地空气密度功率曲线",1.122]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",0,0,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",0.5,0,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",1,0,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",1.5,0,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",2,0,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",2.5,0,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",3,50,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",3.5,87.933449,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",4,144,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",4.5,207.856125,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",5,289,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",5.5,387.203921,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",6,506,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",6.5,645.532588,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",7,809,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",7.5,996.433937,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",8,1211,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",8.5,1433.908525,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",9,1680,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",9.5,1937.893311,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",10,2216,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",10.5,2502.894837,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",11,2806,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",11.5,2923.350218,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",12,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",12.5,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",13,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",13.5,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",14,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",14.5,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",15,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",15.5,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",16,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",16.5,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",17,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",17.5,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",18,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",18.5,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",19,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",19.5,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",20,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",20.5,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",21,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",21.5,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",22,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",22.5,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",23,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",23.5,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",24,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",24.5,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fWhUXelr","山西青龙山风电场","CCWE3000-122.HD","CCWE3000-122.HD",25,3000,"当地空气密度-山西青龙山风电场-CCWE3000-122.HD",1.014]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",0,0,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",0.5,0,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",1,0,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",1.5,0,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",2,0,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",2.5,60,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",3,123,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",3.5,178,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",4,282,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",4.5,408,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",5,564,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",5.5,748,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",6,981,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",6.5,1238,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",7,1556,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",7.5,1890,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",8,2268,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",8.5,2614,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",9,2854,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",9.5,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",10,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",10.5,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",11,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",11.5,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",12,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",12.5,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",13,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",13.5,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",14,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",14.5,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",15,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",15.5,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",16,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",16.5,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",17,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",17.5,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",18,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",18.5,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",19,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",19.5,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["fP4fGag9","内蒙宝日胡风电场","MY3.0se-145","MySE3.0-145",20,3000,"内蒙宝日胡风电场MySE3.0-145机型当地空气密度功率曲线",1.31]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",0,0,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",0.5,0,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",1,0,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",1.5,0,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",2,0,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",2.5,0,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",3,96,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",3.5,203,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",4,356,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",4.5,567,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",5,831,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",5.5,1147,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",6,1507,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",6.5,1924,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",7,2404,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",7.5,2957,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",8,3589,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",8.5,4305,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",9,4729,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",9.5,5082,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",10,5398,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",10.5,5691,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",11,5863,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",11.5,5987,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",12,6085,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",12.5,6144,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",13,6200,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",13.5,6229,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",14,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",14.5,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",15,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",15.5,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",16,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",16.5,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",17,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",17.5,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",18,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",18.5,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",19,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",19.5,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",20,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",20.5,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",21,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",21.5,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",22,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",22.5,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",23,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",23.5,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",24,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",24.5,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY6.25se-172","MY6.25se-172",25,6250,"云南舍得风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",0,0,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",0.5,0,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",1,0,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",1.5,0,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",2,0,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",2.5,0,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",3,19,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",3.5,44,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",4,79,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",4.5,120,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",5,163,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",5.5,227,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",6,285,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",6.5,363,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",7,454,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",7.5,571,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",8,685,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",8.5,811,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",9,952,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",9.5,1089,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",10,1234,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",10.5,1333,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",11,1415,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",11.5,1469,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",12,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",12.5,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",13,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",13.5,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",14,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",14.5,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",15,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",15.5,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",16,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",16.5,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",17,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",17.5,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",18,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",18.5,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",19,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",19.5,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",20,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",20.5,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",21,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",21.5,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",22,1500,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",22.5,0,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",23,0,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",23.5,0,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",24,0,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",24.5,0,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["1lBtf8vX","新疆鄂能风电场","GW82-1500","GW-82/1.5",25,0,"鄂能金风GW82-1500当地空气密度功率曲线",1.122]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",0,0,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",0.5,0,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",1,0,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",1.5,0,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",2,0,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",2.5,0,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",3,10,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",3.5,19,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",4,30,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",4.5,45,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",5,64,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",5.5,85,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",6,111,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",6.5,142,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",7,179,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",7.5,218,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",8,259,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",8.5,303,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",9,351,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",9.5,395,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",10,438,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",10.5,479,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",11,527,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",11.5,574,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",12,623,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",12.5,665,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",13,700,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",13.5,720,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",14,745,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",14.5,765,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",15,802,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",15.5,845,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",16,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",16.5,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",17,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",17.5,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",18,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",18.5,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",19,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",19.5,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",20,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",20.5,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",21,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",21.5,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",22,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",22.5,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",23,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",23.5,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",24,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",24.5,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["8p96xOyt","甘肃玉门风电场","V52-850","V52-850",25,850,"甘肃玉门维斯塔斯V52-850功率曲线",1.056]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",0,0,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",0.5,0,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",1,0,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",1.5,0,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",2,0,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",2.5,0,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",3,61.46,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",3.5,116.46,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",4,176.93,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",4.5,260.34,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",5,364.17,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",5.5,505.67,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",6,658.89,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",6.5,853.84,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",7,1065.12,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",7.5,1335.02,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",8,1625.51,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",8.5,1968.67,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",9,2282.46,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",9.5,2417.72,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",10,2512.62,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",10.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",11,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",11.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",12,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",12.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",13,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",13.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",14,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",14.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",15,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",15.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",16,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",16.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",17,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",17.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",18,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",18.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",19,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",19.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",20,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",20.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",21,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",21.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",22,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",22.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",23,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",23.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",24,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",24.5,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Pq6OPNMA","江西沙岭风电场","XE122-2500","XE122-2500",25,2515.18,"江西沙岭风电场XE122-2500机型当地空气密度功率曲线",1.049]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",0,0,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",0.5,0,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",1,0,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",1.5,0,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",2,0,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",2.5,0,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",3,84,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",3.5,233,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",4,447,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",4.5,691,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",5,972,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",5.5,1294,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",6,1680,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",6.5,2135,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",7,2667,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",7.5,3281,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",8,3981,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",8.5,4775,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",9,5650,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",9.5,6123,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",10,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",10.5,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",11,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",11.5,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",12,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",12.5,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",13,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",13.5,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",14,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",14.5,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",15,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",15.5,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",16,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",16.5,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",17,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",17.5,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",18,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",18.5,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",19,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",19.5,6250,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",20,6220,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",20.5,6016,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",21,5781,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",21.5,5547,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",22,5312,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",22.5,5078,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",23,4843,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",23.5,4609,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",24,4374,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",24.5,4140,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["Ne1QAzL9","吉林敖都风电场","EN182-6250","EN182-6250",25,3906,"吉林敖都风电场EN-182-6250机型标准空气密度曲线",1.239]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",0,0,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",0.5,0,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",1,0,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",1.5,0,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",2,0,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",2.5,0,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",3,30,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",3.5,53,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",4,84,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",4.5,124,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",5,173,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",5.5,231,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",6,301,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",6.5,384,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",7,481,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",7.5,591,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",8,714,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",8.5,845,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",9,978,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",9.5,1104,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",10,1215,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",10.5,1306,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",11,1375,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",11.5,1423,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",12,1456,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",12.5,1477,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",13,1489,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",13.5,1493,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",14,1495,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",14.5,1497,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",15,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",15.5,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",16,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",16.5,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",17,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",17.5,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",18,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",18.5,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",19,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",19.5,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",20,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",20.5,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",21,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",21.5,1500,"湖北华山观GW82-1500功率曲线",1.191]
["tXJhoQG5","湖北华山观风电场","GW82-1500","GW82-1500",22,1500,"湖北华山观GW82-1500功率曲线",1.191]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",0,0,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",0.5,0,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",1,0,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",1.5,0,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",2,0,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",2.5,0,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",3,1,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",3.5,30,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",4,50,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",4.5,100,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",5,150,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",5.5,200,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",6,280,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",6.5,400,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",7,500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",7.5,600,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",8,750,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",8.5,900,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",9,1050,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",9.5,1200,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",10,1350,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",10.5,1450,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",11,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",11.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",12,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",12.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",13,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",13.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",14,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",14.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",15,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",15.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",16,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",16.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",17,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",17.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",18,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",18.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",19,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",19.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",20,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",20.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",21,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",21.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",22,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",22.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",23,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",23.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",24,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",24.5,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["uMLQodz2","辽宁阜新风电场","SL1500-82","SL-82/1.5",25,1500,"后查台风电场SL-82/1.5当地空气密度功率曲线",1.224]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",0,0,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",0.5,0,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",1,0,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",1.5,0,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",2,0,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",2.5,0,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",3,63,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",3.5,153,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",4,266,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",4.5,402,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",5,559,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",5.5,746,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",6,970,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",6.5,1235,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",7,1542,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",7.5,1896,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",8,2293,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",8.5,2611,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",9,2638,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",9.5,2646,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",10,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",10.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",11,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",11.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",12,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",12.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",13,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",13.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",14,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",14.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",15,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",15.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",16,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",16.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",17,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",17.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",18,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",18.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",19,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",19.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",20,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",20.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",21,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",21.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",22,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",22.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",23,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",23.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",24,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",24.5,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["FKPhLnt6","江苏宝应风电场","EN141-2650","EN-141/2.65",25,2650,"江苏宝应风电场远景能源EN-141-2.65机型当地空气密度功率曲线",1.205]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",0,0,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",0.5,0,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",1,0,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",1.5,0,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",2,0,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",2.5,0,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",3,9,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",3.5,14,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",4,25,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",4.5,50,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",5,94,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",5.5,160,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",6,232,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",6.5,292,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",7,346,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",7.5,404,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",8,476,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",8.5,569,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",9,683,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",9.5,811,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",10,946,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",10.5,1086,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",11,1241,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",11.5,1416,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",12,1565,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",12.5,1650,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",13,1711,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",13.5,1807,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",14,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",14.5,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",15,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",15.5,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",16,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",16.5,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",17,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",17.5,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",18,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",18.5,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",19,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",19.5,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",20,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",20.5,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",21,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",21.5,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",22,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",22.5,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",23,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",23.5,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",24,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",24.5,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",25,2000,"京津冀骆驼沟湘电风能XE72-2000功率曲线",1.223]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",0,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",0.5,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",1,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",1.5,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",2,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",2.5,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",3,54.2,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",3.5,120.48,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",4,168.95,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",4.5,234.75,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",5,290.7,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",5.5,436.47,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",6,538.68,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",6.5,646.34,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",7,769.64,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",7.5,900.19,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",8,1029.81,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",8.5,1157.89,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",9,1273.45,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",9.5,1373.36,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",10,1458.17,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",10.5,1496.98,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",11,1502.42,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",11.5,1503.85,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",12,1503.64,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",12.5,1505.7,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",13,1504.74,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",13.5,1508.6,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",14,1508.11,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",14.5,1509.38,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",15,1507.99,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",15.5,1510.62,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",16,1508.13,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",16.5,1515,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",17,1515,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",17.5,1515,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",18,1515,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",18.5,1515,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",19,1515,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",19.5,1515,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",20,1515,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",20.5,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",21,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",21.5,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",22,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",22.5,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",23,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",23.5,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",24,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",24.5,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["h3pdAW7k","黑龙江虎峰岭风电场","SL1500-82","SL1500-82",25,0,"黑龙江虎峰岭SL1500/82机型当地空气密度曲线",1.181]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",0,0,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",0.5,0,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",1,0,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",1.5,0,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",2,0,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",2.5,0,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",3,24,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",3.5,51,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",4,81,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",4.5,130,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",5,185,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",5.5,265,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",6,360,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",6.5,450,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",7,570,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",7.5,710,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",8,850,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",8.5,985,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",9,1100,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",9.5,1220,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",10,1310,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",10.5,1400,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",11,1450,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",11.5,1470,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",12,1500,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",12.5,1510,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",13,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",13.5,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",14,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",14.5,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",15,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",15.5,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",16,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",16.5,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",17,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",17.5,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",18,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",18.5,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",19,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",19.5,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",20,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",20.5,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",21,1520,"塔林花风电场CCWE-1500-82二三期当地空气密度功率曲线",1.16]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",0,0,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",0.5,0,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",1,0,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",1.5,0,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",2,0,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",2.5,0,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",3,4,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",3.5,17,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",4,30,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",4.5,63,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",5,97,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",5.5,151,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",6,205,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",6.5,277,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",7,350,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",7.5,442,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",8,534,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",8.5,649,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",9,765,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",9.5,902,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",10,1040,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",10.5,1190,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",11,1340,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",11.5,1499,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",12,1632,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",12.5,1711,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",13,1763,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",13.5,1801,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",14,1842,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",14.5,1875,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",15,1899,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",15.5,1927,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",16,1951,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",16.5,1982,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",17,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",17.5,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",18,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",18.5,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",19,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",19.5,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",20,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",20.5,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",21,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",21.5,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",22,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",22.5,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",23,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",23.5,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",24,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",24.5,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["TcnIcTwf","内蒙卓资二号风电场","XE72-2000","XE72-2000",25,2000,"卓资二号风电场Z72-2000当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",0,0,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",0.5,0,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",1,0,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",1.5,0,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",2,0,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",2.5,0,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",3,7,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",3.5,21,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",4,49,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",4.5,91.5,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",5,134,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",5.5,198.5,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",6,263,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",6.5,348.4,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",7,433,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",7.5,544,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",8,655,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",8.5,784,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",9,913,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",9.5,1035,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",10,1158,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",10.5,1262,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",11,1367,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",11.5,1430,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",12,1493,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",12.5,1496,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",13,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",13.5,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",14,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",14.5,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",15,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",15.5,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",16,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",16.5,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",17,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",17.5,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",18,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",18.5,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",19,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",19.5,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",20,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",20.5,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",21,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",21.5,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",22,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",22.5,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",23,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",23.5,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",24,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",24.5,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["kaFpUUPs","辽宁十间房风电场","FD77-1500","FD-77/1.5B",25,1500,"十间房风电场FD-77/1.5B当地空气密度功率曲线",1.122]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",0,0,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",0.5,0,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",1,0,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",1.5,0,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",2,14.1,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",2.5,27.76,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",3,52.24,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",3.5,81.42,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",4,99.89,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",4.5,138.03,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",5,198.09,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",5.5,271.78,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",6,362.99,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",6.5,458.65,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",7,570.38,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",7.5,686.01,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",8,808.83,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",8.5,941.14,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",9,1067.7,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",9.5,1194.83,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",10,1302.4,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",10.5,1393.08,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",11,1453.52,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",11.5,1489.27,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",12,1506.29,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",12.5,1514.81,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",13,1520.47,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",13.5,1520.36,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",14,1521.36,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",14.5,1522.79,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",15,1522.61,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",15.5,1524.29,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",16,1524.42,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",16.5,1525.83,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",17,1525.97,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",17.5,1525.63,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",18,1525.3,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",18.5,1525.1,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",19,1523.57,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",19.5,1523,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",20,1523.83,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",20.5,1521.29,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",21,1523.77,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",21.5,1523.19,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["SNNSTwO0","新疆鄯善风电场","GW82-1500","GW82-1500",22,1524.92,"鄯善金风GW82-1500当地空气密度功率曲线",1.1]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",0,0,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",0.5,0,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",1,0,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",1.5,0,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",2,0,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",2.5,17,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",3,67,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",3.5,185,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",4,370,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",4.5,593.95,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",5,849,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",5.5,1141,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",6,1481,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",6.5,1883,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",7,2351,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",7.5,2892,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",8,3510,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",8.5,4210,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",9,4993,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",9.5,5749,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",10,6145,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",10.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",11,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",11.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",12,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",12.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",13,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",13.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",14,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",14.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",15,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",15.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",16,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",16.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",17,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",17.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",18,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",18.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",19,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",19.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",20,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",20.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",21,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",21.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",22,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",22.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",23,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",23.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",24,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",24.5,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["FmowTOzB","内蒙海勒斯风电场","EN182-6250","EN182-6250",25,6250,"内蒙海勒斯风储电站远景能源EN182-6250机型当地空气密度曲线",1.11]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",0,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",0.5,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",1,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",1.5,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",2,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",2.5,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",3,54.2,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",3.5,120.48,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",4,168.95,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",4.5,234.75,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",5,290.7,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",5.5,436.47,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",6,538.68,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",6.5,646.34,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",7,769.64,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",7.5,900.19,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",8,1029.81,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",8.5,1157.89,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",9,1273.45,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",9.5,1373.36,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",10,1458.17,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",10.5,1496.98,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",11,1502.42,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",11.5,1503.85,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",12,1503.64,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",12.5,1505.7,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",13,1504.74,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",13.5,1508.6,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",14,1508.11,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",14.5,1509.38,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",15,1507.99,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",15.5,1510.62,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",16,1508.13,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",16.5,1515,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",17,1515,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",17.5,1515,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",18,1515,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",18.5,1515,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",19,1508.12,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",19.5,1515,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",20,1515,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",20.5,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",21,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",21.5,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",22,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",22.5,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",23,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",23.5,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",24,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",24.5,0,"碾子山华锐SL150082本地",1.122]
["UvhcydNX","黑龙江碾子山风电场","SL1500-82","SL-82/1.5",25,0,"碾子山华锐SL150082本地",1.122]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",0,0,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",0.5,0,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",1,0,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",1.5,0,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",2,0,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",2.5,0,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",3,50,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",3.5,107,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",4,166,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",4.5,239,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",5,329,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",5.5,437,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",6,564,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",6.5,713,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",7,878,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",7.5,1054,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",8,1232,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",8.5,1413,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",9,1590,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",9.5,1765,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",10,1897,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",10.5,1960,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",11,1993,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",11.5,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",12,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",12.5,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",13,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",13.5,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",14,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",14.5,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",15,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",15.5,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",16,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",16.5,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",17,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",17.5,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",18,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",18.5,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",19,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",19.5,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",20,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",20.5,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",21,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",21.5,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",22,2000,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",22.5,0,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",23,0,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",23.5,0,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",24,0,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",24.5,0,"山东宝山W2000-111功率曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",25,0,"山东宝山W2000-111功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",0,0,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",0.5,0,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",1,0,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",1.5,0,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",2,0,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",2.5,0,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",3,4,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",3.5,37,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",4,72,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",4.5,116,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",5,163,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",5.5,225,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",6,298,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",6.5,385,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",7,484,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",7.5,609,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",8,750,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",8.5,899,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",9,1042,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",9.5,1214,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",10,1368,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",10.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",11,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",11.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",12,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",12.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",13,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",13.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",14,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",14.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",15,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",15.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",16,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",16.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",17,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",17.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",18,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",18.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",19,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",19.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",20,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",20.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",21,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",21.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",22,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",22.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",23,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",23.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",24,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",24.5,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["J1k1SKg7","内蒙唐兴风电场","SL1500-82","SL-82/1.5",25,1523,"唐兴风电场SL-821.5当地空气密度功率曲线",1.208]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",3,24,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",3.5,87,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",4,172,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",4.5,274,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",5,396,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",5.5,536,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",6,699,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",6.5,890,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",7,1113,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",7.5,1368,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",8,1659,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",8.5,1985,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",9,2331,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",9.5,2611,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",10,2636,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",10.5,2644,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",11,2649,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",11.5,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",12,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",12.5,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",13,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",13.5,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",14,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",14.5,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",15,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",15.5,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",16,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",16.5,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",17,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",17.5,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",18,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",18.5,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",19,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",19.5,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["epgp9nxH","青海番昌风电场","EN141-2650","EN-141/2.65",20,2650,"青海番昌风电场EN-141/2.65机型当地空气密度功率曲线",0.8861]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",0,0,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",0.5,0,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",1,0,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",1.5,0,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",2,0,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",2.5,0,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",3,96,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",3.5,203,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",4,356,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",4.5,567,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",5,831,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",5.5,1147,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",6,1507,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",6.5,1924,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",7,2404,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",7.5,2957,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",8,3589,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",8.5,4305,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",9,4729,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",9.5,5082,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",10,5398,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",10.5,5691,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",11,5863,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",11.5,5987,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",12,6085,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",12.5,6144,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",13,6200,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",13.5,6229,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",14,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",14.5,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",15,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",15.5,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",16,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",16.5,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",17,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",17.5,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",18,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",18.5,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",19,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",19.5,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",20,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",20.5,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",21,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",21.5,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",22,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",22.5,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",23,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",23.5,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",24,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",24.5,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["SPnODEpG","云南金龙山风电场","MY6.25se-172","MY6.25se-172",25,6250,"云南金龙山风电场明阳智能MY6.25se-172机型当地空气密度曲线",0.924]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",0,0,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",0.5,0,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",1,0,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",1.5,0,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",2,0,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",2.5,16,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",3,49,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",3.5,92,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",4,148,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",4.5,221,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",5,309,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",5.5,417,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",6,546,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",6.5,692,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",7,872,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",7.5,1074,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",8,1305,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",8.5,1551,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",9,1772,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",9.5,2036,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",10,2224,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",10.5,2348,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",11,2408,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",11.5,2459,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",12,2489,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",12.5,2494,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",13,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",13.5,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",14,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",14.5,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",15,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",15.5,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",16,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",16.5,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",17,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",17.5,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",18,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",18.5,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",19,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",19.5,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",20,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",20.5,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",21,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",21.5,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",22,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",22.5,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",23,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",23.5,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",24,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",24.5,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["qjb3GalE","青海朝晖风电场","MY2.0se-121","MY2.0-121",25,2500,"青海大柴旦明阳MY2.0se-121当地空气密度功率曲线",0.857]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",0,0,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",0.5,0,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",1,0,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",1.5,0,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",2,0,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",2.5,0,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",3,73.56,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",3.5,104.86,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",4,172.11,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",4.5,225,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",5,315.85,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",5.5,383.27,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",6,489.37,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",6.5,655.07,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",7,828.53,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",7.5,1024.04,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",8,1188.08,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",8.5,1417.51,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",9,1632.84,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",9.5,1829.85,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",10,2171.37,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",10.5,2335.47,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",11,2444.97,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",11.5,2500,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",12,2512.28,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",12.5,2526.43,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",13,2526.42,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",13.5,2538.46,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",14,2527.65,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",14.5,2529.05,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",15,2516.38,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",15.5,2512.2,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",16,2519.68,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",16.5,2512.06,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",17,2527.45,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",17.5,2521.04,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",18,2522.59,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",18.5,2530.73,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",19,2527,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",19.5,2522.4,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",20,2523.89,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",20.5,2566.5,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",21,2514,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",21.5,2526.67,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["vxtz7yZv","华银银子山风电场","XE122-2500","XE122-2500",22,2500,"银子山风电场XE122-2500当地空气密度曲线",1.122]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",0,0,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",0.5,0,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",1,0,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",1.5,0,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",2,0,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",2.5,26.5,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",3,86.5,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",3.5,166.75,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",4,266.5,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",4.5,388.33,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",5,533.67,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",5.5,711.42,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",6,922.67,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",6.5,1172.58,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",7,1447.33,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",7.5,1724.08,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",8,1972.83,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",8.5,2187.08,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",9,2346.83,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",9.5,2441.58,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",10,2487.42,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",10.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",11,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",11.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",12,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",12.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",13,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",13.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",14,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",14.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",15,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",15.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",16,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",16.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",17,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",17.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",18,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",18.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",19,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",19.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",20,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",20.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",21,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",21.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",22,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",22.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",23,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",23.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",24,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",24.5,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["MLDp7ohC","河南凯安风电场","GW140-2500","GW140-2500",25,2500,"河南凯安风电场GW140-2500机型当地空气密度曲线",1.21]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",0,0,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",0.5,0,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",1,0,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",1.5,0,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",2,0,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",2.5,0,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",3,68,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",3.5,99,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",4,131,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",4.5,182,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",5,243,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",5.5,327,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",6,436,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",6.5,552,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",7,704,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",7.5,801,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",8,1009,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",8.5,1176,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",9,1358,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",9.5,1498,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",10,1634,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",10.5,1863,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",11,1878,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",11.5,1939,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",12,1955,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",12.5,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",13,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",13.5,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",14,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",14.5,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",15,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",15.5,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",16,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",16.5,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",17,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",17.5,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",18,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",18.5,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",19,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",19.5,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",20,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",20.5,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",21,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",21.5,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",22,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",22.5,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",23,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",23.5,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",24,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",24.5,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","DF103-2000","DF2000-103",25,2050,"山西茨庙风电场东方电气 DF(JG)-2000-103机型当地空气密度曲线",1.129]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",0,0,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",0.5,0,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",1,0,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",1.5,0,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",2,0,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",2.5,0,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",3,4,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",3.5,17,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",4,30,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",4.5,63,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",5,97,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",5.5,151,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",6,205,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",6.5,277,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",7,350,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",7.5,442,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",8,534,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",8.5,649,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",9,765,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",9.5,902,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",10,1040,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",10.5,1190,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",11,1340,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",11.5,1499,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",12,1632,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",12.5,1711,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",13,1763,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",13.5,1801,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",14,1842,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",14.5,1875,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",15,1899,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",15.5,1927,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",16,1951,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",16.5,1982,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",17,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",17.5,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",18,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",18.5,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",19,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",19.5,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",20,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",20.5,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",21,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",21.5,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",22,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",22.5,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",23,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",23.5,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",24,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",24.5,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","XE72-2000","XE72-2000",25,2000,"红牧风电场Z72-2000当地空气密度功率曲线",1.122]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",0,0,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",0.5,0,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",1,0,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",1.5,0,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",2,0,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",2.5,73.05,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",3,133.03,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",3.5,263.12,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",4,426.57,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",4.5,625.88,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",5,857.93,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",5.5,1089.07,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",6,1340.47,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",6.5,1775.72,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",7,2051.81,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",7.5,2344.2,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",8,2696.6,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",8.5,4753.65,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",9,4941.51,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",9.5,5006.52,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",10,4937.85,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",10.5,5022.87,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",11,5052.77,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",11.5,5144.02,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",12,5144.03,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",12.5,5158.79,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",13,5156.67,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",13.5,5155.65,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",14,5154.64,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",14.5,5160.25,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",15,5160.79,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",15.5,5155.5,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",16,5168.86,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",16.5,5166.57,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",17,5000,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",17.5,5000,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",18,5000,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",18.5,5000,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",19,5000,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",19.5,5000,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",20,5000,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",20.5,4963,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",21,4815,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",21.5,4639,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",22,4467,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",22.5,4360,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",23,4203,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",23.5,4058,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",24,3939,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",24.5,3827,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",25,3729,"重庆兴顺风电场2期明阳MY5.0se-166当地空气密度功率曲线",1.019]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",0,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",0.5,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",1,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",1.5,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",2,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",2.5,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",3,31,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",3.5,55,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",4,87,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",4.5,125,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",5,171,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",5.5,228,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",6,296,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",6.5,372,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",7,464,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",7.5,568,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",8,677,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",8.5,784,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",9,913,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",9.5,1035.5,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",10,1158,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",10.5,1262.5,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",11,1367,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",11.5,1430,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",12,1493,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",12.5,1496.5,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",13,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",13.5,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",14,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",14.5,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",15,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",15.5,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",16,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",16.5,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",17,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",17.5,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",18,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",18.5,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",19,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",19.5,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",20,1500,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",20.5,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",21,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",21.5,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",22,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",22.5,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",23,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",23.5,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",24,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",24.5,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",25,0,"山东东营东方电气FD77-1500（艾尔姆叶片加装增功组件）标准空气密度功率曲线",1.232]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",0,0,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",0.5,0,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",1,0,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",1.5,0,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",2,0,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",2.5,0,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",3,97.46,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",3.5,142.03,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",4,211.29,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",4.5,280.36,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",5,360.76,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",5.5,469.53,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",6,595.89,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",6.5,749.28,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",7,907.45,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",7.5,1150.43,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",8,1362.08,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",8.5,1545.91,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",9,1754.41,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",9.5,1878.78,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",10,1945.5,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",10.5,1994.91,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",11,2036.75,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",11.5,2043.19,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",12,2040.74,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",12.5,2045.57,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",13,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",13.5,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",14,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",14.5,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",15,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",15.5,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",16,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",16.5,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",17,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",17.5,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",18,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",18.5,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",19,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",19.5,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",20,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",20.5,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",21,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",21.5,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",22,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",22.5,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",23,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",23.5,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",24,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",24.5,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["YhYo9zX9","江西太阳山风电场","MY2.0se-121","MY2.0-121",25,2048.3,"江西太阳山风电场明阳MY2.0-121机型当地空气密度功率曲线",1.1]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",0,0,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",0.5,0,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",1,0,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",1.5,0,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",2,0,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",2.5,0,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",3,11,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",3.5,23,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",4,34,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",4.5,73,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",5,112,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",5.5,163,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",6,213,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",6.5,285,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",7,356,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",7.5,452,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",8,547,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",8.5,668,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",9,789,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",9.5,928,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",10,1068,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",10.5,1219,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",11,1300,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",11.5,1358,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",12,1400,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",12.5,1453,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",13,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",13.5,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",14,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",14.5,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",15,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",15.5,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",16,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",16.5,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",17,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",17.5,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",18,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",18.5,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",19,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",19.5,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",20,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",20.5,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",21,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",21.5,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",22,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",22.5,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",23,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",23.5,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",24,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",24.5,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["sDLagJOE","辽宁太阳山风电场","SL1500-82","SL1500-82",25,1500,"辽宁太阳山风电场华锐SL1500-82当地空气密度功率曲线",1.225]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",0,0,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",0.5,0,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",1,0,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",1.5,0,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",2,0,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",2.5,47,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",3,107,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",3.5,197,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",4,322,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",4.5,494,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",5,728,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",5.5,1029,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",6,1358,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",6.5,1750,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",7,2218,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",7.5,2741,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",8,3238,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",8.5,3741,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",9,4211,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",9.5,4654,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",10,5143,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",10.5,5534,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",11,5824,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",11.5,6054,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",12,6135,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",12.5,6181,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",13,6213,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",13.5,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",14,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",14.5,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",15,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",15.5,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",16,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",16.5,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",17,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",17.5,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",18,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",18.5,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",19,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",19.5,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",20,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",20.5,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",21,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",21.5,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",22,6250,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",22.5,5625,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",23,5000,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",23.5,4375,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",24,3750,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",24.5,3125,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G6250-186","DEW-G6250-186",25,2500,"京津冀摇铃沟DEW-G6250-186机型当地空气密度曲线",1.028]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",0,0,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",0.5,0,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",1,0,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",1.5,0,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",2,0,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",2.5,0,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",3,0,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",3.5,38,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",4,53,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",4.5,83,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",5,124,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",5.5,173,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",6,235,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",6.5,309,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",7,396,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",7.5,494,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",8,603,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",8.5,718,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",9,837,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",9.5,957,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",10,1074,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",10.5,1186,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",11,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",11.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",12,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",12.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",13,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",13.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",14,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",14.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",15,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",15.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",16,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",16.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",17,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",17.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",18,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",18.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",19,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",19.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",20,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",20.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",21,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",21.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",22,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",22.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",23,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",23.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",24,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",24.5,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",25,1250,"大水菠萝风电场V80-2.0MW（24号）当地空气密度功率曲线",1]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",0,0,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",0.5,0,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",1,0,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",1.5,0,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",2,0,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",2.5,0,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",3,23,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",3.5,104,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",4,230,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",4.5,380,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",5,555,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",5.5,758,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",6,989,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",6.5,1261,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",7,1581,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",7.5,1950,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",8,2370,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",8.5,2831,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",9,3143,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",9.5,3227,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",10,3279,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",10.5,3297,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",11,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",11.5,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",12,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",12.5,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",13,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",13.5,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",14,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",14.5,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",15,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",15.5,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",16,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",16.5,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",17,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",17.5,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",18,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",18.5,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",19,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",19.5,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",20,3300,"内蒙图步盛风电场远景能源EN156-3300机型当地空气密度曲线",1.03]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",0,0,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",0.5,0,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",1,0,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",1.5,0,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",2,0,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",2.5,0,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",3,4.47,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",3.5,36.3,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",4,72.2,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",4.5,116,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",5,165,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",5.5,226,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",6,300,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",6.5,387,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",7,489,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",7.5,611,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",8,750,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",8.5,902,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",9,1064,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",9.5,1230,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",10,1396,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",10.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",11,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",11.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",12,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",12.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",13,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",13.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",14,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",14.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",15,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",15.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",16,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",16.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",17,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",17.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",18,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",18.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",19,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",19.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",20,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",20.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",21,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",21.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",22,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",22.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",23,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",23.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",24,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",24.5,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",25,1501,"驼山风电场SL-82/1.5当地空气密度功率曲线",1.04]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",0,0,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",0.5,0,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",1,0,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",1.5,0,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",2,0,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",2.5,0,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",3,0,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",3.5,29.18,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",4,31.11,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",4.5,85.54,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",5,131.75,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",5.5,169.93,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",6,209.19,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",6.5,259.67,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",7,328.41,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",7.5,417.8,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",8,525.7,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",8.5,646.51,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",9,772.61,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",9.5,895.86,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",10,1008.87,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",10.5,1105.96,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",11,1183.66,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",11.5,1240.86,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",12,1278.63,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",12.5,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",13,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",13.5,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",14,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",14.5,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",15,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",15.5,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",16,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",16.5,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",17,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",17.5,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",18,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",18.5,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",19,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",19.5,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",20,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",20.5,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",21,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",21.5,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",22,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",22.5,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",23,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",23.5,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",24,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",24.5,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",25,1300,"东山风电场V80-2000（83号）当地空气密度功率曲线",1.15]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0,0,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0.5,0,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1,0,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1.5,0,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2,0,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2.5,0,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3,12,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3.5,27,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4,47,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4.5,88,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5,138,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5.5,198,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6,266,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6.5,346,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7,434,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7.5,540,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8,654,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8.5,780,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9,923,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9.5,1059,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10,1205,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10.5,1327,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11,1453,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11.5,1487,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12.5,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13.5,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14.5,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15.5,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16.5,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17.5,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18.5,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19.5,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20.5,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21.5,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22.5,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23.5,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24.5,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["NGRkf3n3","新疆十三师风电场","CCWE1500-82.DF","CCWE-1500/82.DF",25,1500,"十三师华创CCWE-1500/82.DF当地空气密度功率曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",0,0,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",0.5,0,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",1,0,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",1.5,0,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",2,0,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",2.5,38,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",3,60,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",3.5,60,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",4,214,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",4.5,214,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",5,439,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",5.5,439,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",6,760,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",6.5,760,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",7,1190,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",7.5,1190,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",8,1740,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",8.5,1740,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",9,2260,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",9.5,2260,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",10,2480,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",10.5,2480,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",11,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",11.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",12,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",12.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",13,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",13.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",14,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",14.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",15,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",15.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",16,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",16.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",17,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",17.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",18,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",18.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",19,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",19.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",20,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",20.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",21,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",21.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",22,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",22.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",23,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",23.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",24,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",24.5,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",25,2500,"山东顾家东方电气FD77C当地空气密度曲线",1.122]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",0,0,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",0.5,0,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",1,0,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",1.5,0,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",2,0,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",2.5,15.5,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",3,31,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",3.5,128.5,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",4,226,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",4.5,392.5,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",5,559,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",5.5,808.5,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",6,1058,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",6.5,1402.5,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",7,1747,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",7.5,2192.5,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",8,2638,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",8.5,3178,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",9,3718,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",9.5,4311,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",10,4904,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",10.5,5463,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",11,6022,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",11.5,6378.5,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",12,6735,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",12.5,6848.5,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",13,6962,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",13.5,6979.5,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",14,6997,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",14.5,6998.5,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",15,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",15.5,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",16,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",16.5,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",17,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",17.5,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",18,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",18.5,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",19,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",19.5,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",20,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",20.5,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",21,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",21.5,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",22,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",22.5,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",23,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",23.5,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",24,7000,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",24.5,6965,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",25,6930,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",25.5,6860.5,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",26,6791,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",26.5,6312,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",27,5833,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",27.5,5250,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",28,4667,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",28.5,4083.5,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",29,3500,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",29.5,2916.5,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",30,2333,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",30.5,1750,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",31,1167,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",31.5,1167,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["SVLgVZfi","广东勒门海上风电场","SWT7000-154","SWT7000-154",32,1167,"广东勒门海上风电场SWT7000-154机型当地空气密度功率曲线",1.125]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",0,0,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",0.5,0,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",1,0,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",1.5,0,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",2,0,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",2.5,66,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",3,104.9,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",3.5,149.27,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",4,201.01,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",4.5,262.63,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",5,336.59,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",5.5,423.97,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",6,524.3,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",6.5,632.98,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",7,750.21,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",7.5,869.89,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",8,992.51,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",8.5,1110.67,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",9,1215.13,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",9.5,1304.66,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",10,1374.58,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",10.5,1426.37,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",11,1460.72,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",11.5,1500,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",12,1500,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",12.5,1500,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",13,1500,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",13.5,1500,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",14,1500,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",14.5,1500,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",15,1500,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",15.5,1500,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",16,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",16.5,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",17,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",17.5,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",18,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",18.5,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",19,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",19.5,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",20,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",20.5,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",21,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",21.5,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",22,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",22.5,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",23,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",23.5,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",24,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",24.5,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["kjqKo3PM","内蒙查干风电场","SL1500-82","SL-82/1.5",25,1520,"查干风电场SL-1500当地空气密度功率曲线",1.16]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",0,0,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",3,21.5,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",3.5,52.3,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",4,90.9,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",4.5,137.7,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",5,194.7,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",5.5,264,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",6,346.7,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",6.5,443.9,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",7,559.2,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",7.5,694.3,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",8,841.1,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",8.5,994.1,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",9,1167,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",9.5,1359.9,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",10,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",10.5,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",11,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",11.5,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",12,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",12.5,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",13,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",13.5,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",14,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",14.5,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",15,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",16,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",17,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",18,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",19,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",20,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",21,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",22,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",23,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",24,1500,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",25,0,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",26,0,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-86","UP-86/1.5",50,0,"山东安城联合动力UP1500-86当地空气密度功率曲线",1.223]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",0,0,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",0.5,0,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",1,0,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",1.5,0,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",2,0,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",2.5,0,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",3,1,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",3.5,24,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",4,47,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",4.5,86,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",5,136,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",5.5,201,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",6,265,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",6.5,349,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",7,430,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",7.5,545,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",8,658,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",8.5,796,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",9,911,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",9.5,1038,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",10,1160,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",10.5,1278,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",11,1370,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",11.5,1448,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",12,1498,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",12.5,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",13,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",13.5,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",14,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",14.5,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",15,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",15.5,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",16,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",16.5,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",17,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",17.5,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",18,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",18.5,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",19,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",19.5,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",20,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",20.5,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",21,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",21.5,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",22,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",22.5,1500,"河南清源东方电气FD77A本地",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD-77/1.5A",23,1500,"河南清源东方电气FD77A本地",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",0,0,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",0.5,0,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",1,0,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",1.5,0,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",2,0,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",2.5,0,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",3,13,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",3.5,51,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",4,107,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",4.5,175,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",5,253,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",5.5,346,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",6,454,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",6.5,584,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",7,738,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",7.5,912,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",8,1109,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",8.5,1321,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",9,1538,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",9.5,1734,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",10,1873,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",10.5,1951,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",11,1984,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",11.5,1995,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",12,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",12.5,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",13,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",13.5,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",14,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",14.5,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",15,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",15.5,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",16,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",16.5,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",17,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",17.5,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",18,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",18.5,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",19,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",19.5,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["WzJBVp2a","辽宁高桥风电场","V100-2000","V100-2MW",20,2000,"高桥风电场V100-2MW当地空气密度功率曲线",1.13]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",0,0,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",0.5,0,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",1,0,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",1.5,0,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",2,0,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",2.5,0,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",3,0,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",3.5,0,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",4,15.2,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",4.5,27.4,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",5,45.1,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",5.5,69.4,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",6,88,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",6.5,117,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",7,145.5,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",7.5,178.5,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",8,216.7,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",8.5,263.9,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",9,299.2,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",9.5,348.3,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",10,391.5,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",10.5,442,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",11,487.1,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",11.5,530.7,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",12,572.9,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",12.5,606.1,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",13,643.4,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",13.5,674.3,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",14,696.9,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",14.5,716.4,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",15,728.1,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",15.5,735.9,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",16,746.6,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",16.5,749.3,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",17,753.2,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",17.5,751,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",18,751,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",18.5,745.8,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",19,743.9,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",19.5,737,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",20,734.1,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",20.5,727.9,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",21,724,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",21.5,717.1,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",22,714.2,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",22.5,710.1,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",23,707.2,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",23.5,705,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",24,703,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",24.5,703,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","S48-750","GW-48/0.75",25,703,"大黑山风电场S48-750当地空气密度功率曲线",1.16]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",0,0,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",0.5,0,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",1,0,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",1.5,0,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",2,0,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",2.5,0,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",3,44,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",3.5,101,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",4,177,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",4.5,275,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",5,404,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",5.5,563,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",6,752,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",6.5,963,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",7,1211,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",7.5,1490,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",8,1804,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",8.5,2112,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",9,2411,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",9.5,2676,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",10,2844,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",10.5,2941,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",11,2978,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",11.5,2988,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",12,2995,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",12.5,2999,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",13,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",13.5,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",14,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",14.5,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",15,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",15.5,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",16,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",16.5,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",17,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",17.5,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",18,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",18.5,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",19,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",19.5,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",20,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",20.5,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",21,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",21.5,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",22,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",22.5,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",23,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",23.5,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",24,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",24.5,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["aBuq2wUD","陕西营盘风电场","MY3.0se-145","MySE3.0-145",25,3000,"陕西营盘风电场明阳MYSE145-3.0机型当地空气密度曲线",1.022]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",0,0,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",0.5,0,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",1,0,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",1.5,0,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",2,0,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",2.5,0,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",3,59.8,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",3.5,130.8,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",4,218.1,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",4.5,320.5,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",5,446.6,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",5.5,598.1,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",6,779.1,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",6.5,994.6,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",7,1248.7,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",7.5,1530.7,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",8,1823.4,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",8.5,2116,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",9,2351.4,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",9.5,2473.9,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",10,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",10.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",11,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",11.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",12,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",12.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",13,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",13.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",14,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",14.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",15,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",15.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",16,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",16.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",17,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",17.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",18,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",18.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",19,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",19.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",20,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",20.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",21,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",21.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",22,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",22.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",23,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",23.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",24,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",24.5,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["S1hWvMOE","桂冠马王风电场","W2500-135","W2500-135",25,2500,"广西马王风电场二期W2500-135机型当地空气密度功率曲线",1.103]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",0,0,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",0.5,0,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",1,0,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",1.5,0,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",2,0,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",2.5,0,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",3,21.5,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",3.5,52.3,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",4,90.9,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",4.5,137.7,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",5,194.7,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",5.5,264,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",6,346.7,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",6.5,443.9,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",7,559.2,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",7.5,694.1,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",8,841.1,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",8.5,994.6,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",9,1167,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",9.5,1358,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",10,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",10.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",11,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",11.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",12,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",12.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",13,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",13.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",14,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",14.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",15,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",15.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",16,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",16.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",17,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",17.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",18,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",18.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",19,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",19.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",20,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",20.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",21,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",21.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",22,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",22.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",23,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",23.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",24,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",24.5,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["XDn6awEJ","山东平阴风电场","UP1500-86","UP-86/1.5",25,1500,"山东平阴联合动力UP1500-86当地空气密度功率曲线",1.206]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",0,0,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",0.5,0,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",1,0,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",1.5,0,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",2,0,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",2.5,0,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",3,23,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",3.5,104,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",4,208,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",4.5,326,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",5,477,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",5.5,663,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",6,892,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",6.5,1173,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",7,1502,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",7.5,1808,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",8,2122,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",8.5,2437,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",9,2741,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",9.5,3017,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",10,3254,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",10.5,3396,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",11,3467,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",11.5,3539,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",12,3574,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",12.5,3585,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",13,3588,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",13.5,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",14,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",14.5,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",15,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",15.5,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",16,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",16.5,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",17,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",17.5,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",18,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",18.5,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",19,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",19.5,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["vqBw2lWx","青海和畅风电场","DEW-G3600-165","DEW-G3600-165",20,3600,"青海和畅风电场DEW-G3600-165机型当地空气密度功率曲线",0.82]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",0,0,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",0.5,0,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",1,0,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",1.5,0,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",2,0,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",2.5,0,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",3,36,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",3.5,88,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",4,152,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",4.5,228,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",5,321,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",5.5,432,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",6,551,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",6.5,715,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",7,902,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",7.5,1114,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",8,1344,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",8.5,1575,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",9,1792,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",9.5,1960,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",10,2088,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",10.5,2143,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",11,2171,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",11.5,2188,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",12,2197,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",12.5,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",13,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",13.5,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",14,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",14.5,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",15,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",15.5,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",16,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",16.5,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",17,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",17.5,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",18,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",18.5,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",19,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",19.5,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",20,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",20.5,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",21,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",21.5,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",22,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",22.5,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",23,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",23.5,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",24,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",24.5,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["k8DfllKP","辽宁茶家风电场","V110-2200","V110-2.2MW",25,2200,"辽宁茶家风电场V110-2.2MW机型当地空气密度功率曲线",1.191]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",0,0,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",0.5,0,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",1,0,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",1.5,0,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",2,0,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",2.5,0,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",3,22,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",3.5,113,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",4,264,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",4.5,468,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",5,730,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",5.5,1045,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",6,1407,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",6.5,1812,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",7,2264,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",7.5,2784,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",8,3379,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",8.5,4044,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",9,4709,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",9.5,5249,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",10,5603,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",10.5,5893,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",11,6065,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",11.5,6162,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",12,6217,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",12.5,6242,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",13,6249,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",13.5,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",14,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",14.5,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",15,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",15.5,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",16,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",16.5,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",17,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",17.5,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",18,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",18.5,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",19,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",19.5,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",20,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",20.5,6250,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",21,6190,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",21.5,6024,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",22,5771,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",22.5,5466,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",23,5145,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",23.5,4837,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",24,4548,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",24.5,4263,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["9yA9ainh","重庆和顺风电场","EN182-6250","EN182-6250",25,3963,"重庆和顺风电场远景能源EN182-6250机型当地空气密度曲线",1.04]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",0,0,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",0.5,0,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",1,0,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",1.5,0,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",2,0,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",2.5,0,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",3,0,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",3.5,55,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",4,136,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",4.5,235,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",5,352,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",5.5,485,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",6,644,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",6.5,832,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",7,1053,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",7.5,1307,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",8,1592,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",8.5,1888,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",9,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",9.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",10,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",10.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",11,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",11.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",12,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",12.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",13,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",13.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",14,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",14.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",15,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",15.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",16,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",16.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",17,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",17.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",18,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",18.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",19,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",19.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",20,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",20.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",21,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",21.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",22,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",22.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",23,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",23.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",24,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",24.5,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["z8Xo4tYG","桂冠龙头风电场","MY2.0se-121","MY2.0-121/85",25,2000,"广西龙头MY2.0-121/85功率曲线",1.178]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",0,0,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",0.5,0,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",1,0,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",1.5,0,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",2,0,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",2.5,49,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",3,111,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",3.5,206,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",4,340,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",4.5,527,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",5,783,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",5.5,1110,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",6,1469,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",6.5,1899,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",7,2397,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",7.5,2950,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",8,3449,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",8.5,3944,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",9,4402,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",9.5,4790,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",10,5244,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",10.5,5603,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",11,5870,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",11.5,6070,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",12,6148,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",12.5,6188,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",13,6223,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",13.5,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",14,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",14.5,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",15,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",15.5,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",16,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",16.5,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",17,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",17.5,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",18,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",18.5,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",19,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",19.5,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",20,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",20.5,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",21,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",21.5,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",22,6250,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",22.5,5625,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",23,5000,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",23.5,4375,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",24,3750,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",24.5,3125,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["GVjZ4b0y","京津冀府平风电场","DEW-G6250-186","DEW-G6250-186",25,2500,"京津冀府平东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",0,0,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",0.5,0,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",1,0,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",1.5,0,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",2,0,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",2.5,0,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",3,26.9,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",3.5,58.5,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",4,90.1,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",4.5,136.7,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",5,183.3,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",5.5,253.2,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",6,323.1,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",6.5,420.95,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",7,518.8,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",7.5,649.1,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",8,779.4,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",8.5,933.2,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",9,1087,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",9.5,1251,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",10,1415,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",10.5,1457.5,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",11,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",11.5,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",12,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",12.5,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",13,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",13.5,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",14,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",14.5,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",15,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",15.5,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",16,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",16.5,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",17,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",17.5,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",18,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",18.5,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",19,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",19.5,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",20,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",20.5,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",21,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",21.5,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["nanxOx8h","辽宁中三家风电场","GW82-1500","GW-82/1.5",22,1500,"中三家风电场GW-82/1.5当地空气密度功率曲线",1.19]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",0,0,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",0.5,0,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",1,0,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",1.5,0,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",2,0,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",2.5,73.05,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",3,133.03,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",3.5,263.12,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",4,426.57,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",4.5,625.88,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",5,857.93,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",5.5,1089.07,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",6,1340.47,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",6.5,1775.72,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",7,2051.81,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",7.5,2344.2,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",8,2696.6,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",8.5,4753.65,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",9,4941.51,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",9.5,5006.52,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",10,4937.85,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",10.5,5022.87,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",11,5052.77,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",11.5,5144.02,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",12,5144.03,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",12.5,5158.79,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",13,5156.67,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",13.5,5155.65,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",14,5154.64,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",14.5,5160.25,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",15,5160.79,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",15.5,5155.5,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",16,5168.86,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY5.0se-166","MY5.0se-166",16.5,5166.57,"重庆兴顺二期风电场明阳5.0当地空气密度功率曲线",1.019]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0,0,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0.5,0,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1,0,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1.5,0,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2,0,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2.5,0,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3,9,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3.5,36.9,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4,75,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4.5,123.7,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5,181,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5.5,245.7,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6,322,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6.5,413.8,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7,518,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7.5,631.9,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8,760,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8.5,907.6,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9,1075,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9.5,1252.8,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10,1399,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10.5,1476.3,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24.5,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",25,1500,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",25.5,0,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["gJR54ocT","山东金岭风电场","CCWE1500-82.DF","CCWE-1500/82.DF",26,0,"山东金岭华创CCWE-1500-82.DF机型当地空气密度曲线",1.212]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",0,0,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",0.5,0,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",1,0,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",1.5,0,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",2,0,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",2.5,0,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",3,71,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",3.5,135,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",4,202,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",4.5,266,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",5,306,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",5.5,407,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",6,526,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",6.5,665,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",7,822,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",7.5,998,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",8,1181,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",8.5,1376,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",9,1588,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",9.5,1778,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",10,1931,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",10.5,2034,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",11,2080,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",11.5,2086,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",12,2074,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",12.5,2076,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",13,2056,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",13.5,2056,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",14,2057,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",14.5,2056,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",15,2058,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",15.5,2057,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",16,2000,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",16.5,2000,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",17,2000,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",17.5,2000,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",18,2000,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",18.5,2000,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",19,2000,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",19.5,2000,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",20,2000,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",20.5,2000,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",21,2000,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",21.5,2000,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",22,2000,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",22.5,0,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",23,0,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",23.5,0,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",24,0,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",24.5,0,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000-111",25,0,"黑龙江东安二期上海电气W2000-111当地密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",0,0,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",0.5,0,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",1,0,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",1.5,0,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",2,0,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",2.5,0,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",3,54.3,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",3.5,120.8,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",4,202.5,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",4.5,298.7,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",5,417,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",5.5,559.4,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",6,728.8,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",6.5,930,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",7,1167.2,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",7.5,1430.6,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",8,1704.2,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",8.5,1983.9,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",9,2248.8,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",9.5,2412.2,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",10,2480.4,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",10.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",11,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",11.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",12,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",12.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",13,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",13.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",14,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",14.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",15,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",15.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",16,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",16.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",17,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",17.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",18,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",18.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",19,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",19.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",20,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",20.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",21,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",21.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",22,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",22.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",23,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",23.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",24,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",24.5,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["A1XCQkxB","陕西广洛风电场","W2500-135","W2500-135",25,2500,"陕西广洛风电场W2500-135机型当地空气密度曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",0,0,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",0.5,0,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",1,0,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",1.5,0,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",2,0,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",2.5,0,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",3,21,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",3.5,28,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",4,77,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",4.5,96,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",5,156,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",5.5,198,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",6,276,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",6.5,346,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",7,443,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",7.5,555,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",8,667,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",8.5,814,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",9,941,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",9.5,1095,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",10,1226,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",10.5,1353,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",11,1496,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",11.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",12,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",12.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",13,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",13.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",14,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",14.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",15,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",15.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",16,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",16.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",17,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",17.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",18,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",18.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",19,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",19.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",20,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",20.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",21,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",21.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",22,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",22.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",23,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",23.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",24,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",24.5,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["TlOUeROv","内蒙怀朔风电场","GW82-1500","GW82-1500",25,1500,"怀朔风电场GW82-1500当地空气密度功率曲线",1.122]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",0,0,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",0.5,0,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",1,0,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",1.5,0,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",2,0,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",2.5,0,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",3,11,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",3.5,37,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",4,48,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",4.5,127,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",5,148,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",5.5,251,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",6,278,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",6.5,387,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",7,467,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",7.5,577,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",8,713,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",8.5,872,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",9,1023,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",9.5,1237,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",10,1350,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",10.5,1401,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",11,1488,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",11.5,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",12,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",12.5,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",13,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",13.5,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",14,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",14.5,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",15,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",15.5,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",16,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",16.5,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",17,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",17.5,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",18,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",18.5,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",19,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",19.5,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-82","UP82-1500",20,1500,"陕西张家山联合动力UP82-1500功率曲线",1.0067]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",0,0,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",0.5,0,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",1,0,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",1.5,0,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",2,0,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",2.5,0,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",3,20,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",3.5,129,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",4,296,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",4.5,496,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",5,736,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",5.5,1032,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",6,1347,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",6.5,1724,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",7,2154,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",7.5,2642,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",8,3153,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",8.5,3593,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",9,4088,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",9.5,4516,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",10,4923,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",10.5,5173,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",11,5333,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",11.5,5399,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",12,5469,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",12.5,5487,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",13,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",13.5,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",14,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",14.5,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",15,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",15.5,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",16,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",16.5,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",17,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",17.5,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",18,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",18.5,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",19,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",19.5,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",20,5500,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",20.5,5150,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",21,4800,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",21.5,4450,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",22,4100,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",22.5,3750,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",23,3400,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",23.5,3050,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",24,2700,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",24.5,2350,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["8OubW7Gt","京津冀摇铃沟风电场","DEW-G5500-183","DEW-G5500-183",25,2000,"京津冀摇铃沟DEW-G5500-183型当地空气密度曲线",1.028]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",0,0,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",0.5,0,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",1,0,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",1.5,0,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",2,0,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",2.5,22,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",3,58.9,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",3.5,106.6,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",4,170,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",4.5,250.6,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",5,349.7,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",5.5,470.6,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",6,614,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",6.5,779.1,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",7,981.9,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",7.5,1210.2,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",8,1467.4,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",8.5,1732.8,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",9,1935.1,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",9.5,2204.5,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",10,2354.3,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",10.5,2432.4,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",11,2465,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",11.5,2494.1,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",12,2499.5,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",12.5,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",13,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",13.5,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",14,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",14.5,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",15,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",15.5,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",16,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",16.5,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",17,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",17.5,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",18,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",18.5,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",19,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",19.5,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",20,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",20.5,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",21,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",21.5,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",22,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",22.5,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",23,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",23.5,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",24,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",24.5,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["wazaFXsW","贵州白龙山风电场","DF131-2500","DF131-2500",25,2500,"贵州白龙山风电场东方电气FD131-2500机型当地空气密度功率曲线",0.947]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",0,0,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",0.5,0,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",1,0,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",1.5,0,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",2,0,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",2.5,0,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",3,31,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",3.5,77.6,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",4,137,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",4.5,208,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",5,292,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",5.5,394,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",6,501,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",6.5,650,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",7,822,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",7.5,1017,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",8,1235,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",8.5,1463,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",9,1690,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",9.5,1892,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",10,2043,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",10.5,2133,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",11,2176,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",11.5,2191,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",12,2198,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",12.5,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",13,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",13.5,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",14,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",14.5,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",15,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",15.5,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",16,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",16.5,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",17,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",17.5,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",18,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",18.5,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",19,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",19.5,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["AWBmBVjP","京津冀闪电河风电场","V110-2200","V110-2.2MW",20,2200,"京津冀闪电河二期风电场VESTAS-V110-2.2机型当地空气密度功率曲线",1.09]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",0,0,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",0.5,0,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",1,0,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",1.5,0,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",2,0,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",2.5,22.94,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",3,116.33,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",3.5,247.98,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",4,410.77,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",4.5,602.05,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",5,834.79,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",5.5,1119.77,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",6,1452.38,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",6.5,1837.36,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",7,2273.47,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",7.5,2749.61,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",8,3243.59,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",8.5,3733.45,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",9,4193.21,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",9.5,4611.81,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",10,4975.25,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",10.5,5270,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",11,5270,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",11.5,5270,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",12,5270,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",12.5,5270,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",13,5270,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",13.5,5270,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",14,5270,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",14.5,5270,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",15,5270,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",15.5,5270,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",16,5252.71,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",16.5,5219.73,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",17,5138.08,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",17.5,5002.57,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",18,4841.62,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",18.5,4653.76,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",19,4467.49,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",19.5,4279.94,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",20,4086.25,"京津冀西桥梁风电场金风科技GW191/5270机型DA当地空气密度功率曲线",1.06]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",0,0,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",0.5,0,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",1,0,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",1.5,0,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",2,0,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",2.5,0,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",3,22.2,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",3.5,38.34,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",4,62.56,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",4.5,107.39,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",5,160.57,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",5.5,223.16,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",6,297.24,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",6.5,384.4,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",7,485.05,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",7.5,598.21,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",8,721.59,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",8.5,851.99,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",9,985.6,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",9.5,1118.49,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",10,1246.95,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",10.5,1367.77,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",11,1478.47,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",11.5,1577.34,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",12,1663.51,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",12.5,1736.89,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",13,1798,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",13.5,1847.84,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",14,1887.73,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",14.5,1919.14,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",15,1944.08,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",15.5,1964.02,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",16,1979.8,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",16.5,1992.52,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",17,2001.97,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",17.5,2008.36,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",18,2012.22,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",18.5,2013.62,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",19,2014.2,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",19.5,2014.41,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",20,2014.92,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",20.5,2015.38,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",21,2015.81,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",21.5,2015.81,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",22,2015.81,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",22.5,2015.81,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",23,2015.9,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",23.5,2016.02,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",24,2016.05,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",24.5,2016.13,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",25,2016.22,"大水菠萝风电场V80-2.0MW（高低压穿越改造）当地空气密度功率曲线",1]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",0,0,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",0.5,0,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",1,0,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",1.5,0,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",2,0,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",2.5,23,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",3,79.5,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",3.5,154.75,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",4,248,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",4.5,360.5,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",5,496.25,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",5.5,662,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",6,859.5,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",6.5,1092,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",7,1358.5,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",7.5,1639,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",8,1902.75,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",8.5,2133.25,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",9,2309.25,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",9.5,2428,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",10,2481,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",10.5,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",11,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",11.5,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",12,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",12.5,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",13,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",13.5,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",14,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",14.5,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",15,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",15.5,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",16,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",16.5,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",17,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",17.5,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",18,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",18.5,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",19,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",19.5,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["yZf1JVkW","河南殷都风电场","GW140-2500","GW140/2500",20,2500,"河南殷都风电场GW140-2500机型当地空气密度曲线",1.25]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",0,0,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",0.5,0,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",1,0,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",1.5,0,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",2,0,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",2.5,0,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",3,20,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",3.5,53,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",4,85,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",4.5,139,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",5,192,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",5.5,269,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",6,346,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",6.5,440,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",7,534,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",7.5,652,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",8,769,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",8.5,907,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",9,1045,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",9.5,1170,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",10,1294,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",10.5,1376,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",11,1458,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",11.5,1480,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",12,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",12.5,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",13,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",13.5,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",14,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",14.5,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",15,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",15.5,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",16,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",16.5,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",17,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",17.5,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",18,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",18.5,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",19,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",19.5,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",20,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",20.5,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",21,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",21.5,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",22,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",22.5,1500,"河南鞍子山金风GW82/1500本地",1.132]
["xrvjxEe5","河南鞍子山风电场","GW82-1500","GW-82/1.5",23,1500,"河南鞍子山金风GW82/1500本地",1.132]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0,0,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0.5,0,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1,0,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1.5,0,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2,0,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2.5,0,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3,42,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3.5,67,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4,100,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4.5,142,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5,195,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5.5,258,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6,336,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6.5,427,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7,530,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7.5,656,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8,796,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8.5,954,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9,1134,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9.5,1240.5,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10,1397,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10.5,1476.1,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24.5,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["EmlMGcty","山东驿道风电场","CCWE1500-82.DF","CCWE-1500/82.DF",25,1500,"山东驿道华创CCWE-1500-82.DF机型当地空气密度曲线",1.211]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",0,0,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",0.5,0,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",1,0,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",1.5,0,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",2,0,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",2.5,53.9,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",3,85.94,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",3.5,124.78,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",4,171.2,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",4.5,226.44,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",5,292.91,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",5.5,379.44,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",6,458.18,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",6.5,554.79,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",7,661.5,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",7.5,777.9,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",8,897.42,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",8.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",9,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",9.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",10,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",10.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",11,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",11.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",12,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",12.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",13,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",13.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",14,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",14.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",15,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",15.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",16,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",16.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",17,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",17.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",18,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",18.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",19,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",19.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",20,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",20.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",21,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",21.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",22,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",22.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",23,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",23.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",24,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",24.5,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",25,1000,"达里风电场SL1500-82（33号）当地空气密度功率曲线",1.14]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",0,0,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",0.5,0,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",1,0,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",1.5,0,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",2,0,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",2.5,0,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",3,45,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",3.5,98,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",4,153,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",4.5,221,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",5,306,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",5.5,406,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",6,525,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",6.5,665,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",7,821,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",7.5,997,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",8,1180,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",8.5,1375,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",9,1588,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",9.5,1777,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",10,1896,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",10.5,1975,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",11,1998,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",11.5,1997,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",12,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",12.5,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",13,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",13.5,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",14,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",14.5,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",15,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",15.5,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",16,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",16.5,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",17,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",17.5,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",18,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",18.5,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",19,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",19.5,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",20,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",20.5,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",21,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",21.5,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",22,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",22.5,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",23,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",23.5,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",24,2000,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",24.5,0,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["nfKZcAEc","黑龙江东安风电场","W2000-111","W2000C-111-80",25,0,"黑龙江东安风电场W2000C-111-80机型当地空气密度曲线",1.122]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",0,0,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",0.5,0,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",1,0,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",1.5,0,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",2,0,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",2.5,0,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",3,48,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",3.5,111,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",4,193,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",4.5,300,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",5,430,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",5.5,589,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",6,780,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",6.5,998,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",7,1250,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",7.5,1540,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",8,1869,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",8.5,2237,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",9,2594,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",9.5,2913,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",10,3176,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",10.5,3340,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",11,3408,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",11.5,3440,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",12,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",12.5,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",13,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",13.5,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",14,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",14.5,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",15,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",15.5,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",16,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",16.5,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",17,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",17.5,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",18,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",18.5,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",19,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",19.5,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",20,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",20.5,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",21,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",21.5,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",22,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",22.5,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",23,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",23.5,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",24,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",24.5,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["ZCAfh48q","山西团龙沟风电场","W3450-146","W3450-146",25,3450,"山西团龙沟风电场W3450-146-90机型当地空气密度曲线",0.974]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",0,0,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",0.5,0,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",1,0,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",1.5,0,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",2,0,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",2.5,0,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",3,44,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",3.5,69,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",4,104,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",4.5,149,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",5,203,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",5.5,271,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",6,352,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",6.5,447,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",7,559,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",7.5,688,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",8,834,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",8.5,1001,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",9,1187,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",9.5,1297,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",10,1410,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",10.5,1433.09,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",11,1477.48,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",11.5,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",12,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",12.5,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",13,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",13.5,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",14,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",14.5,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",15,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",15.5,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",16,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",16.5,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",17,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",17.5,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",18,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",18.5,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",19,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",19.5,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",20,1500,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",20.5,0,"山东泽库SL1500/82（叶片加长）当地功率曲线",1.214]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",0,0,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",0.5,0,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",1,0,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",1.5,0,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",2,0,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",2.5,0,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",3,85.87,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",3.5,139.89,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",4,213.75,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",4.5,307.76,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",5,421.94,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",5.5,568.63,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",6,750.33,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",6.5,944.26,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",7,1162.32,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",7.5,1445.8,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",8,1732.76,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",8.5,2008.38,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",9,2283.94,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",9.5,2410.07,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",10,2458.44,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",10.5,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",11,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",11.5,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",12,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",12.5,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",13,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",13.5,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",14,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",14.5,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",15,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",15.5,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",16,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",16.5,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",17,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",17.5,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",18,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",18.5,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",19,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",19.5,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",20,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",20.5,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",21,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",21.5,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["oacUqLWX","四川赛果乐风电场","DF131-2500","DF131-2500",22,2500,"四川赛果乐东方电气DF131-2500当地空气密度功率曲线",1.243]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",0,0,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",0.5,0,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",1,0,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",1.5,0,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",2,0,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",2.5,0,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",3,43.9,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",3.5,93.2,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",4,144.7,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",4.5,208.5,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",5,287.7,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",5.5,381.6,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",6,492.7,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",6.5,622.6,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",7,767.1,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",7.5,920.5,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",8,1075.7,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",8.5,1226.3,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",9,1362.8,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",9.5,1501.4,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",10,1635.8,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",10.5,1749.7,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",11,1856.7,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",11.5,1929.3,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",12,1980.1,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",12.5,1998.7,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",13,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",13.5,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",14,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",14.5,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",15,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",15.5,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",16,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",16.5,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",17,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",17.5,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",18,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",18.5,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",19,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",19.5,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",20,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",20.5,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",21,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",21.5,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["vaqpKNMZ","江西乱罗嶂风电场","W2000-111","W2000-111",22,2000,"江西乱罗嶂风电场W2000-111机型当地空气密度功率曲线",1.044]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",0,0,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",0.5,0,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",1,0,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",1.5,0,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",2,0,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",2.5,0,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",3,0,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",3.5,0,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",4,21.9,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",4.5,40.2,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",5,57.8,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",5.5,82.5,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",6,107.1,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",6.5,139.6,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",7,174,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",7.5,206.7,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",8,260.6,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",8.5,306.5,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",9,364.3,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",9.5,420.9,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",10,474.9,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",10.5,540.4,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",11,593.4,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",11.5,641.2,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",12,693.2,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",12.5,734.7,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",13,764.1,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",13.5,796.1,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",14,811.8,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",14.5,837,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",15,846,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",15.5,849,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",16,849,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",16.5,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",17,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",17.5,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",18,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",18.5,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",19,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",19.5,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",20,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",20.5,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",21,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",21.5,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",22,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",22.5,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",23,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",23.5,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",24,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",24.5,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V52-850","VT-52/0.85",25,850,"大黑山风电场V52-850当地空气密度功率曲线",1.16]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",0,0,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",0.5,0,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",1,0,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",1.5,0,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",2,50,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",2.5,119,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",3,49,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",3.5,152,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",4,298,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",4.5,479,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",5,685,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",5.5,921,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",6,1198,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",6.5,1523,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",7,1902,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",7.5,2339,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",8,2836,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",8.5,3382,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",9,3909,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",9.5,4274,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",10,4404,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",10.5,4459,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",11,4485,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",11.5,4494,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",12,4499,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",12.5,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",13,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",13.5,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",14,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",14.5,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",15,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",15.5,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",16,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",16.5,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",17,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",17.5,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",18,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",18.5,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",19,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",19.5,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",20,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",20.5,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",21,4500,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",21.5,4404,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",22,4248,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",22.5,4091,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",23,3934,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",23.5,3776,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",24,3619,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",24.5,3461,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",25,3302,"内蒙图步盛当地空气密度EN171-4.5功率曲线",1.03]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",0,0,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",0.5,0,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",1,0,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",1.5,0,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",2,0,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",2.5,20,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",3,112,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",3.5,244,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",4,404,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",4.5,594,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",5,824,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",5.5,1104,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",6,1435,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",6.5,1810,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",7,2241,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",7.5,2710,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",8,3196,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",8.5,3670,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",9,4104,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",9.5,4505,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",10,4834,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",10.5,5076,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",11,5204,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",11.5,5251,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",12,5263,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",12.5,5270,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",13,5270,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",13.5,5270,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",14,5270,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",14.5,5270,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",15,5270,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",15.5,5270,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",16,5253,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",16.5,5220,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",17,5138,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",17.5,5003,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",18,4842,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",18.5,4654,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",19,4467,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",19.5,4280,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-5270","GWH191-5270",20,4086,"京津冀水泉风电场GWH191-5270机型当地空气密度曲线",1.065]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",0,0,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",0.5,0,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",1,0,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",1.5,0,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",2,0,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",2.5,0,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",3,0,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",3.5,55,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",4,135,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",4.5,234,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",5,350,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",5.5,483,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",6,641,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",6.5,829,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",7,1049,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",7.5,1302,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",8,1587,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",8.5,1864,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",9,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",9.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",10,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",10.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",11,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",11.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",12,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",12.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",13,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",13.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",14,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",14.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",15,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",15.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",16,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",16.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",17,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",17.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",18,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",18.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",19,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",19.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",20,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",20.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",21,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",21.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",22,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",22.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",23,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",23.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",24,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",24.5,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["rzWDBHug","桂冠恭城风电场","MY2.0se-121","MY2.0-121/85",25,2000,"广西恭城MY2.0-121/85功率曲线",1.174]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",0,0,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",0.5,0,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",1,0,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",1.5,0,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",2,0,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",2.5,30,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",3,71,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",3.5,127,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",4,198,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",4.5,292,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",5,408,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",5.5,545,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",6,715,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",6.5,903,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",7,1133,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",7.5,1396,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",8,1666,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",8.5,1933,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",9,2124,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",9.5,2322,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",10,2410,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",10.5,2442,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",11,2460,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",11.5,2480,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",12,2498,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",12.5,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",13,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",13.5,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",14,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",14.5,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",15,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",15.5,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",16,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",16.5,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",17,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",17.5,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",18,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",18.5,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",19,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",19.5,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["w1l9QntN","江西蜈蚣山风电场","DF131-2500","DF131-2500",20,2500,"江西蜈蚣山风电场东方电气DF131-2500机型当地空气密度功率曲线",1.242]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",0,0,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",0.5,0,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",1,0,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",1.5,0,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",2,0,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",2.5,0,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",3,79.32,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",3.5,142.48,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",4,221.18,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",4.5,310.47,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",5,425.84,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",5.5,558.22,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",6,711.59,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",6.5,883.94,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",7,1092.89,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",7.5,1296.8,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",8,1532.83,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",8.5,1794.91,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",9,2021.58,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",9.5,2253.72,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",10,2481.97,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",10.5,2697.85,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",11,2851.77,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",11.5,2950.51,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",12,2997.96,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",12.5,3027.64,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",13,3035.69,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",13.5,3041.17,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",14,3044.2,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",14.5,3046.8,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",15,3047.6,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",15.5,3047.84,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",16,3049.22,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",16.5,3048.43,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",17,3048.47,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",17.5,3048.69,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",18,3049.28,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",18.5,3049.36,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",19,3049.26,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",19.5,3049.68,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",20,3048.43,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",20.5,3048.42,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",21,3050.03,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",21.5,3050.03,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",22,3050.03,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",22.5,3050.03,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",23,3050.03,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",23.5,3050.03,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",24,3050.03,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",24.5,3050.03,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["Rzkrjrzc","新疆哈密风电场","SL3000-113","SL-113/3.0",25,3050.03,"哈密华锐SL3000/113当地空气密度功率曲线",1.1]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",0,0,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",0.5,0,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",1,0,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",1.5,0,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",2,0,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",2.5,0,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",3,39.4,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",3.5,87.2,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",4,140.4,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",4.5,206.2,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",5,286.1,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",5.5,383.3,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",6,498.4,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",6.5,634.4,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",7,790.2,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",7.5,952.4,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",8,1115.7,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",8.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",9,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",9.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",10,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",10.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",11,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",11.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",12,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",12.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",13,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",13.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",14,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",14.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",15,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",15.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",16,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",16.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",17,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",17.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",18,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",18.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",19,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",19.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",20,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",20.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",21,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",21.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",22,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",22.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",23,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",23.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",24,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",24.5,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",25,1250,"山西燕家村二期风电场W2000-111/80机型（64号）当地空气密度曲线",0.9939]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",0,0,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",0.5,0,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",1,0,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",1.5,0,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",2,0,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",2.5,0,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",3,42,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",3.5,85,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",4,148,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",4.5,230,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",5,336,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",5.5,453,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",6,595,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",6.5,763,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",7,956,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",7.5,1179,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",8,1433,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",8.5,1692,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",9,1858,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",9.5,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",10,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",10.5,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",11,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",11.5,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",12,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",12.5,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",13,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",13.5,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",14,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",14.5,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",15,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",15.5,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",16,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",16.5,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",17,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",17.5,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",18,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",18.5,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",19,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",19.5,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["1MleSFxP","宁夏同心风电场","MY2.0se-121","MY2.0-121",20,2000,"同心风电场明阳MY2.0-121机型当地空气密度曲线",1.122]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0,0,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0.5,0,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1,0,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1.5,0,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2,0,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2.5,0,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3,5,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3.5,21.3,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4,51,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4.5,96.3,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5,154,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5.5,220.7,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6,297,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6.5,384.7,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7,486,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7.5,602.6,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8,733,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8.5,876.7,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9,1041,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9.5,1224.3,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10,1381,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10.5,1468.7,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24.5,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",25,1500,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["jIH0tyAA","山东云山风电场","CCWE1500-82.DF","CCWE-1500/82.DF",26,0,"山东云山华创CCWE-1500/82.DF当地空气密度功率曲线",1.212]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",0,0,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",0.5,0,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",1,0,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",1.5,0,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",2,0,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",2.5,0,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",3,23,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",3.5,104,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",4,230,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",4.5,380,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",5,555,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",5.5,758,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",6,989,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",6.5,1261,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",7,1581,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",7.5,1950,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",8,2370,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",8.5,2831,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",9,3143,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",9.5,3227,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",10,3279,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",10.5,3297,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",11,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",11.5,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",12,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",12.5,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",13,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",13.5,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",14,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",14.5,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",15,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",15.5,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",16,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",16.5,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",17,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",17.5,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",18,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",18.5,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",19,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",19.5,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN156-3300","EN156-3300",20,3300,"内蒙图步盛EN-156-3.3当地空气密度功率曲线",1.03]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",0,0,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",0.5,0,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",1,0,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",1.5,0,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",2,22,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",2.5,51,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",3,103,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",3.5,173,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",4,259,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",4.5,376,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",5,511,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",5.5,673,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",6,883,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",6.5,1130,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",7,1380,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",7.5,1689,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",8,1968,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",8.5,2237,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",9,2418,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",9.5,2481,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",10,2496,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",10.5,2503,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",11,2506,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",11.5,2508,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",12,2511,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",12.5,2511,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",13,2516,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",13.5,2519,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",14,2517,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",14.5,2512,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",15,2505,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",15.5,2514,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",16,2514,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",16.5,2513,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",17,2517,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",17.5,2505,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",18,2514,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",18.5,2514,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",19,2513,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",19.5,2517,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["izkj6kya","河南雄风风电场","GW140-2500","GW140/2500",20,2513,"河南雄风风电场GW140-2500机型当地空气密度曲线",1.225]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",0,0,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",0.5,0,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",1,0,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",1.5,0,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",2,0,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",2.5,0,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",3,0,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",3.5,27,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",4,54,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",4.5,89,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",5,126,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",5.5,173,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",6,234,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",6.5,306,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",7,388,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",7.5,483,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",8,592,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",8.5,714,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",9,842,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",9.5,977,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",10,1114,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",10.5,1246,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",11,1371,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",11.5,1484,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",12,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",12.5,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",13,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",13.5,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",14,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",14.5,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",15,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",15.5,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",16,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",16.5,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",17,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",17.5,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",18,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",18.5,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",19,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",19.5,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",20,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",20.5,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",21,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",21.5,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",22,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",22.5,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",23,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",23.5,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",24,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",24.5,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["tlfzNWFi","云南朗目山风电场","UP1500-86","UP86-1500ⅢB",25,1500,"云南朗目山风电场UP86-1500IIIB机型当地空气密度功率曲线",0.93]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",0,0,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",0.5,0,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",1,0,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",1.5,0,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",2,0,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",2.5,33,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",3,99,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",3.5,197,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",4,337,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",4.5,502,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",5,694,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",5.5,925,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",6,1202,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",6.5,1528,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",7,1908,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",7.5,2345,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",8,2831,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",8.5,3346,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",9,3746,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",9.5,3927,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",10,3973,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",10.5,3984,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",11,3987,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",11.5,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",12,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",12.5,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",13,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",13.5,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",14,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",14.5,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",15,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",15.5,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",16,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",16.5,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",17,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",17.5,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",18,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",18.5,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",19,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",19.5,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",20,4000,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",20.5,3923,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",21,3720,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",21.5,3569,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",22,3454,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",22.5,3225,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",23,3058,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",23.5,2876,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",24,2792,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",24.5,2648,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["1aXLzGlg","京津冀梧桐沟风电场","MY4.0se-166","MY4.0se-166",25,2508,"京津冀梧桐沟风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.062]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",0,0,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",0.5,0,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",1,0,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",1.5,0,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",2,0,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",2.5,0,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",3,0,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",3.5,46.3,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",4,71.88,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",4.5,108.43,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",5,149.32,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",5.5,195.23,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",6,249.35,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",6.5,315.23,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",7,392.5,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",7.5,479.8,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",8,577.4,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",8.5,678.54,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",9,784.84,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",9.5,889.98,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",10,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",10.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",11,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",11.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",12,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",12.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",13,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",13.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",14,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",14.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",15,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",15.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",16,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",16.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",17,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",17.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",18,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",18.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",19,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",19.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",20,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",20.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",21,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",21.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",22,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",22.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",23,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",23.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",24,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",24.5,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL1500-82",25,1000,"达里风电场SL1500-82（66号）当地空气密度功率曲线",1.14]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",0,0,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",0.5,0,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",1,0,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",1.5,0,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",2,0,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",2.5,0,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",3,4,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",3.5,17,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",4,30,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",4.5,63,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",5,97,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",5.5,151,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",6,205,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",6.5,277,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",7,350,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",7.5,442,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",8,534,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",8.5,649,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",9,765,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",9.5,902,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",10,1040,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",10.5,1190,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",11,1340,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",11.5,1499,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",12,1632,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",12.5,1711,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",13,1763,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",13.5,1801,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",14,1842,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",14.5,1875,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",15,1899,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",15.5,1927,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",16,1951,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",16.5,1982,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",17,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",17.5,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",18,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",18.5,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",19,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",19.5,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",20,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",20.5,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",21,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",21.5,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",22,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",22.5,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",23,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",23.5,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",24,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",24.5,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["kBOyIRx7","内蒙卓资一号风电场","XE72-2000","XE72-2000",25,2000,"卓资一号风电场Z72-2000当地空气密度功率曲线",1.122]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",0,0,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",0.5,0,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",1,0,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",1.5,0,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",2,0,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",2.5,0,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",3,59.36,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",3.5,120.88,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",4,199.29,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",4.5,292.39,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",5,404.64,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",5.5,541.7,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",6,706.08,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",6.5,900.35,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",7,1126.88,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",7.5,1388.21,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",8,1686.8,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",8.5,2024.81,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",9,2383.55,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",9.5,2756.16,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",10,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",10.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",11,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",11.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",12,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",12.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",13,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",13.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",14,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",14.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",15,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",15.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",16,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",16.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",17,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",17.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",18,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",18.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",19,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",19.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",20,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",20.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",21,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",21.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",22,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",22.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",23,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",23.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",24,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",24.5,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["UvIjaTYC","宁夏青铜峡风电场","CCWE3000-122.HD","CCWE-3000/122.HD",25,3000,"青铜峡风电场华创CCWE-3000/122.HD机型当地空气密度曲线",1.062]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",0,0,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",0.5,0,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",1,0,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",1.5,0,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",2,0,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",2.5,98.32,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",3,132.39,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",3.5,188.15,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",4,263.34,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",4.5,356.36,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",5,478.08,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",5.5,639.05,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",6,840.8,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",6.5,1077.08,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",7,1348.83,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",7.5,1652.7,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",8,1987.07,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",8.5,2329.12,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",9,2663.64,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",9.5,2980.86,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",10,3230,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",10.5,3384.33,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",11,3450,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",11.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",12,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",12.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",13,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",13.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",14,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",14.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",15,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",15.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",16,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",16.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",17,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",17.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",18,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",18.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",19,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",19.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",20,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",20.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",21,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",21.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",22,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",22.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",23,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",23.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",24,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",24.5,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W3450-146","W3450-146",25,3490,"贵州革利风电场W3450-146机型当地空气密度曲线",1.021]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",0,0,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",0.5,0,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",1,0,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",1.5,0,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",2,0,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",2.5,0,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",3,1,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",3.5,20,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",4,47,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",4.5,80,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",5,127,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",5.5,190,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",6,280,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",6.5,350,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",7,411,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",7.5,512,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",8,622,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",8.5,762,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",9,867,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",9.5,987,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",10,1100,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",10.5,1200,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",11,1299,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",11.5,1359,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",12,1418,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",12.5,1440,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",13,1485,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",13.5,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",14,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",14.5,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",15,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",15.5,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",16,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",16.5,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",17,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",17.5,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",18,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",18.5,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",19,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",19.5,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",20,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",20.5,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",21,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",21.5,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",22,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",22.5,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",23,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",23.5,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",24,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",24.5,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["Ys0XlOCz","山东顾家风电场（桂冠）","FD77-1500","FD77C-1500",25,1500,"山东顾家东方电气FD77C标准空气密度曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",0,0,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",0.5,0,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",1,0,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",1.5,0,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",2,0,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",2.5,35,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",3,70,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",3.5,145.5,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",4,221,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",4.5,332.5,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",5,444,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",5.5,607,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",6,770,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",6.5,994,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",7,1218,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",7.5,1500.5,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",8,1783,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",8.5,2032,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",9,2281,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",9.5,2384,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",10,2487,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",10.5,2493.5,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",11,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",11.5,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",12,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",12.5,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",13,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",13.5,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",14,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",14.5,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",15,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",15.5,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",16,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",16.5,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",17,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",17.5,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",18,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",18.5,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",19,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",19.5,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["aw954E5H","陕西油房庄风电场","GW140-2500","GW140/2500",20,2500,"陕西油房庄金风GW140/2500功率曲线",1.122]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",0,0,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",0.5,0,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",1,0,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",1.5,0,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",2,0,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",2.5,85,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",3,120,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",3.5,194,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",4,254,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",4.5,352,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",5,470,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",5.5,608,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",6,736,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",6.5,998,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",7,1247,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",7.5,1460,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",8,1749,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",8.5,1977,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",9,2363,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",9.5,2517,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",10,2719,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",10.5,2944,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",11,2974,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",11.5,2978,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",12,2983,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",12.5,3009,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",13,3027,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",13.5,3025,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",14,3029,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",14.5,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",15,3028,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",15.5,3028,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",16,3028,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",16.5,3026,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",17,3027,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",17.5,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",18,3028,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",18.5,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",19,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",19.5,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",20,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",20.5,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",21,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",21.5,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",22,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",22.5,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",23,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",23.5,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",24,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",24.5,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["5vF7WkO3","河南睦风风电场","CCWE3000-122.HD","CCWE-3000/122.HD",25,3030,"河南睦风华创CCWE-3000/122.HD本地",1.17]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",0,0,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",0.5,0,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",1,0,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",1.5,0,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",2,0,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",2.5,0,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",3,96,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",3.5,203,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",4,356,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",4.5,567,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",5,831,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",5.5,1147,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",6,1507,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",6.5,1924,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",7,2404,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",7.5,2957,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",8,3589,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",8.5,4305,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",9,4729,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",9.5,5082,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",10,5398,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",10.5,5691,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",11,5863,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",11.5,5987,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",12,6085,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",12.5,6144,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",13,6200,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",13.5,6229,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",14,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",14.5,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",15,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",15.5,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",16,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",16.5,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",17,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",17.5,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",18,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",18.5,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",19,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",19.5,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",20,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",20.5,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",21,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",21.5,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",22,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",22.5,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",23,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",23.5,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",24,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",24.5,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY6.25se-172","MY6.25se-172",25,6250,"云南蜜蜂山MY6.25se-172当地空气密度功率曲线",0.924]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",0,0,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",0.5,0,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",1,0,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",1.5,0,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",2,0,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",2.5,0,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",3,0,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",3.5,0,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",4,26,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",4.5,44,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",5,63,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",5.5,89,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",6,118,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",6.5,153,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",7,196,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",7.5,240,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",8,296,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",8.5,351,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",9,420,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",9.5,474,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",10,544,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",10.5,595,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",11,661,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",11.5,702,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",12,762,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",12.5,796,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",13,831,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",13.5,838,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",14,844,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",14.5,846,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",15,848,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",15.5,849,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",16,849,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",16.5,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",17,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",17.5,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",18,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",18.5,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",19,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",19.5,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",20,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",20.5,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",21,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",21.5,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",22,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",22.5,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",23,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",23.5,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",24,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",24.5,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["d5btw15h","福建六鳌风电场","G52-850","GM-52/0.85",25,850,"福建六鳌风电场歌美飒GM52-850",1.15]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",0,0,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",0.5,0,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",1,0,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",1.5,0,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",2,0,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",2.5,0,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",3,4.48442,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",3.5,36.4744,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",4,72.4419,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",4.5,116.437,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",5,165.263,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",5.5,226.656,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",6,301.096,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",6.5,387.998,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",7,490.997,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",7.5,612.919,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",8,752.644,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",8.5,904.275,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",9,1068.01,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",9.5,1234.09,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",10,1400.23,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",10.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",11,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",11.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",12,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",12.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",13,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",13.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",14,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",14.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",15,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",15.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",16,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",16.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",17,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",17.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",18,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",18.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",19,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",19.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",20,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",20.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",21,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",21.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",22,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",22.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",23,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",23.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",24,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",24.5,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["0M6OwnLd","山东东平风电场","SL1500-82","SL-82/1.5",25,1500.61,"山东东平华锐SL1500/82当地空气密度功率曲线",1.229]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",0,0,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",0.5,0,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",1,0,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",1.5,0,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",2,0,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",2.5,22.94,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",3,116.33,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",3.5,247.98,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",4,410.77,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",4.5,602.05,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",5,834.79,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",5.5,1119.77,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",6,1452.38,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",6.5,1837.36,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",7,2273.47,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",7.5,2749.61,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",8,3243.59,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",8.5,3733.45,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",9,4193.21,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",9.5,4611.81,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",10,4975.25,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",10.5,5270,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",11,5270,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",11.5,5270,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",12,5270,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",12.5,5270,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",13,5270,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",13.5,5270,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",14,5270,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",14.5,5270,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",15,5270,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",15.5,5270,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",16,5252.71,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",16.5,5219.73,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",17,5138.08,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",17.5,5002.57,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",18,4841.62,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",18.5,4653.76,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",19,4467.49,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",19.5,4279.94,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","GWH191-5270","GWH191-5270",20,4086.25,"京津冀西桥梁风电场金风科技GW191/5270机型当地空气密度功率曲线",1.06]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",0,0,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",0.5,0,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",1,0,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",1.5,0,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",2,0,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",2.5,0,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",3,4.47,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",3.5,36.3,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",4,72.2,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",4.5,116,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",5,165,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",5.5,226,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",6,300,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",6.5,387,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",7,489,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",7.5,611,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",8,750,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",8.5,902,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",9,1064,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",9.5,1230,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",10,1396,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",10.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",11,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",11.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",12,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",12.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",13,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",13.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",14,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",14.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",15,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",15.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",16,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",16.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",17,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",17.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",18,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",18.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",19,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",19.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",20,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",20.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",21,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",21.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",22,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",22.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",23,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",23.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",24,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",24.5,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["OzMILmUP","辽宁海派风电场","SL1500-82","SL-82/1.5",25,1501,"东岗风电场SL-82/1.5当地空气密度功率曲线",1.04]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",0,0,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",0.5,0,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",1,0,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",1.5,0,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",2,0,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",2.5,1,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",3,20,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",3.5,39,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",4,73,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",4.5,107,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",5,158,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",5.5,209,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",6,276,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",6.5,345,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",7,433,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",7.5,522,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",8,632,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",8.5,741,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",9,842,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",9.5,955,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",10,1076,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",10.5,1191,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",11,1269,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",11.5,1318,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",12,1374,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",12.5,1416,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",13,1456,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",13.5,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",14,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",14.5,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",15,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",15.5,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",16,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",16.5,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",17,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",17.5,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",18,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",18.5,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",19,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",19.5,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",20,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",20.5,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",21,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",21.5,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",22,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",22.5,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",23,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",23.5,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",24,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",24.5,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["mAhz2hkB","内蒙红牧风电场","FD77-1500","FD77D-1500",25,1500,"红牧风电场FD77D-1500当地空气密度功率曲线",1.122]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",0,0,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",0.5,0,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",1,0,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",1.5,0,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",2,0,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",2.5,0,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",3,50,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",3.5,84,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",4,141,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",4.5,220,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",5,314,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",5.5,430,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",6,561,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",6.5,713,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",7,893,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",7.5,1082,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",8,1302,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",8.5,1491,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",9,1664,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",9.5,1785,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",10,1881,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",10.5,1935,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",11,1974,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",11.5,1980,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",12,1991,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",12.5,1998,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",13,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",13.5,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",14,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",14.5,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",15,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",15.5,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",16,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",16.5,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",17,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",17.5,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",18,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",18.5,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",19,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",19.5,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["uokqAQUW","四川漫天岭风电场","MY2.0se-121","MY2.0-121",20,2000,"四川漫天岭明阳MY2.0-121功率曲线",1.023]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",3,19,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",3.5,80,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",4,161,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",4.5,261,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",5,380,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",5.5,515,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",6,672,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",6.5,855,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",7,1068,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",7.5,1313,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",8,1591,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",8.5,1904,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",9,2255,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",9.5,2544,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",10,2629,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",10.5,2642,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",11,2648,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",11.5,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",12,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",12.5,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",13,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",13.5,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",14,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",14.5,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",15,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",15.5,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",16,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",16.5,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",17,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",17.5,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",18,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",18.5,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",19,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",19.5,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["dyumcWKP","青海枫岚风电场","EN141-2650","EN-141/2.65",20,2650,"青海枫岚风电场EN-141/2.65机型当地空气密度功率曲线",0.864]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",0,0,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",0.5,0,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",1,0,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",1.5,0,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",2,0,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",2.5,0,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",3,1,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",3.5,20,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",4,47,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",4.5,80,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",5,127,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",5.5,190,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",6,280,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",6.5,350,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",7,411,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",7.5,512,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",8,622,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",8.5,762,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",9,867,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",9.5,987,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",10,1100,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",10.5,1200,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",11,1299,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",11.5,1359,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",12,1418,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",12.5,1440,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",13,1485,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",13.5,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",14,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",14.5,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",15,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",15.5,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",16,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",16.5,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",17,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",17.5,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",18,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",18.5,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",19,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",19.5,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",20,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",20.5,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",21,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",21.5,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",22,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",22.5,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",23,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",23.5,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",24,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",24.5,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","FD77-1500","FD77C-1500",25,1500,"山东莱州FD77C当地空气密度功率曲线",1.122]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",0,0,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",1,0,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",2,0,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",3,0,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",3.2,17.2,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",3.4,34.4,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",3.6,51.6,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",3.8,68.8,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",4,86,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",4.2,106.8,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",4.4,127.6,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",4.6,148.4,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",4.8,169.2,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",5,190,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",5.2,220.8,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",5.4,251.6,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",5.6,282.4,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",5.8,313.2,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",6,344,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",6.2,387.2,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",6.4,430.4,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",6.6,473.6,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",6.8,516.8,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",7,560,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",7.2,617.4,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",7.4,674.8,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",7.6,732.2,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",7.8,789.6,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",8,847,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",8.2,917.2,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",8.4,987.4,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",8.6,1057.6,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",8.8,1127.8,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",9,1198,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",9.2,1282.6,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",9.4,1356.4,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",9.6,1426.6,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",9.8,1496.8,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",10,1567,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",10.2,1625.4,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",10.4,1683.8,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",10.6,1742.2,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",10.8,1800.6,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",11,1859,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",11.2,1882.6,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",11.4,1906.2,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",11.6,1929.8,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",11.8,1953.4,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",12,1977,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",12.2,1981.2,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",12.4,1985.4,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",12.6,1989.6,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",12.8,1993.8,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",13,1998,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",14,2000,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",15,2000,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["GjzgBgUB","内蒙扎罗木得风电场","V90-2000","VT-90/2.0",25,2000,"扎罗木得风电场V90-2000当地空气密度功率曲线",1.17]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",0,0,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",0.5,0,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",1,0,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",1.5,0,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",2,0,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",2.5,0,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",3,50,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",3.5,107,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",4,166,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",4.5,239,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",5,329,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",5.5,437,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",6,564,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",6.5,713,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",7,878,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",7.5,1054,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",8,1232,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",8.5,1413,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",9,1590,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",9.5,1765,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",10,1897,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",10.5,1960,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",11,1993,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",11.5,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",12,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",12.5,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",13,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",13.5,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",14,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",14.5,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",15,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",15.5,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",16,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",16.5,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",17,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",17.5,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",18,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",18.5,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",19,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",19.5,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",20,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",20.5,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",21,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",21.5,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",22,2000,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",22.5,0,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",23,0,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",23.5,0,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",24,0,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",24.5,0,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["eCvndqZW","山东宝山风电场","W2000-111","W2000-111",25,0,"山东宝山上气机型W2000-111当地空气密度曲线",1.208]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",0,0,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",0.5,0,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",1,0,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",1.5,0,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",2,0,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",2.5,0,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",3,7.55,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",3.5,27.64,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",4,60.38,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",4.5,91.53,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",5,138.63,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",5.5,212.52,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",6,255.82,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",6.5,352.1,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",7,422.11,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",7.5,520.67,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",8,648.32,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",8.5,824.66,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",9,917.51,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",9.5,1067.77,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",10,1210.2,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",10.5,1372.33,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",11,1487.4,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",11.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",12,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",12.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",13,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",13.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",14,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",14.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",15,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",15.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",16,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",16.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",17,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",17.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",18,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",18.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",19,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",19.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",20,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",20.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",21,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",21.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",22,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",22.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",23,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",23.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",24,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",24.5,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["7uHDyKUK","陕西张家山风电场","UP1500-86","UP1500-86",25,1500,"陕西张家山联合动力UP1500-86机型当地空气密度曲线",1.0067]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",0,0,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",0.5,0,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",1,0,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",1.5,0,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",2,0,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",2.5,0,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",3,108,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",3.5,205,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",4,324,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",4.5,462,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",5,632,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",5.5,842,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",6,1087,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",6.5,1379,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",7,1714,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",7.5,2073,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",8,2451,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",8.5,2842,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",9,3224,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",9.5,3396,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",10,3487,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",10.5,3523,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",11,3576,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",11.5,3592,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",12,3594,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",12.5,3596,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",13,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",13.5,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",14,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",14.5,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",15,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",15.5,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",16,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",16.5,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",17,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",17.5,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",18,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",18.5,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",19,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",19.5,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["ZTRCGwcz","甘肃喜集水风电场","DEW-G3600-165","DEW-G3600-165",20,3600,"甘肃喜集水风电场DEW-G3600-165机型当地空气密度功率曲线",1.122]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",0,0,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",0.5,0,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",1,0,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",1.5,0,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",2,0,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",2.5,12,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",3,90,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",3.5,228,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",4,406,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",4.5,614,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",5,859,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",5.5,1154,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",6,1501,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",6.5,1900,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",7,2349,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",7.5,2834,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",8,3329,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",8.5,3802,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",9,4219,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",9.5,4543,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",10,4754,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",10.5,4876,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",11,4954,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",11.5,4982,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",12,4998,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",12.5,5000,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",13,5000,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",13.5,5000,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",14,5000,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",14.5,5000,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",15,5000,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",15.5,5000,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",16,5000,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",16.5,5000,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",17,4864,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",17.5,4649,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",18,4413,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",18.5,4139,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",19,3865,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",19.5,3585,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["pBftJKeJ","重庆莲花山风电场","GW191-5000","GW191-5000",20,3349.33,"重庆莲花山金风GWH191-5.0机型当地空气密度功率曲线",1.075]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0,0,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0.5,0,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1,0,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1.5,0,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2,0,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2.5,0,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3,8,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3.5,32.3,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4,63,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4.5,101.4,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5,155,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5.5,229.1,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6,315,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6.5,404,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7,501,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7.5,613.4,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8,744,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8.5,894,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9,1061,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9.5,1235.4,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10,1381,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10.5,1465.8,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24.5,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",25,1500,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",25.5,0,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["tnjSaHgC","山东苏家风电场","CCWE1500-82.DF","CCWE-1500/82.DF",26,0,"山东苏家华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",0,0,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",0.5,0,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",1,0,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",1.5,0,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",2,0,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",2.5,0,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",3,0,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",3.5,2.48,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",4,28.38,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",4.5,56.1,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",5,86.62,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",5.5,124.94,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",6,164.36,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",6.5,212.71,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",7,270.24,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",7.5,337.79,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",8,414.81,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",8.5,501.8,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",9,602.52,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",9.5,715.46,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",10,840.48,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",10.5,967.59,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",11,1098.82,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",11.5,1230.8,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",12,1368.89,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",12.5,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",13,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",13.5,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",14,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",14.5,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",15,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",15.5,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",16,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",16.5,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",17,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",17.5,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",18,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",18.5,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",19,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",19.5,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",20,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",20.5,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",21,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",21.5,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",22,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",22.5,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",23,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",23.5,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",24,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",24.5,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["B57V8tus","内蒙达里风电场","SL1500-82","SL-82/1.5",25,1500.96,"达里风电场SL1500-82当地空气密度功率曲线",1.14]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",0,0,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",0.5,0,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",1,0,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",1.5,0,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",2,0,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",2.5,0,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",3,128.3,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",3.5,269.7,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",4,428.4,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",4.5,655.1,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",5,937.3,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",5.5,1295.6,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",6,1723.8,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",6.5,2182.8,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",7,2721.5,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",7.5,3291.2,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",8,3981.5,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",8.5,4731.2,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",9,5553.7,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",9.5,6341.1,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",10,7147,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",10.5,7927.7,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",11,8549.6,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",11.5,9074.3,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",12,9498.5,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",12.5,9715.4,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",13,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",13.5,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",14,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",14.5,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",15,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",15.5,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",16,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",16.5,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",17,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",17.5,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",18,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",18.5,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",19,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",19.5,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",20,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",20.5,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",21,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",21.5,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",22,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",22.5,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",23,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",23.5,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",24,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",24.5,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","DEW-D10000-185","DEW-D10000-185",25,10000,"福建显美风电场DEW-D10000-185当地空气密度功率曲线",1.197]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",0,0,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",0.5,0,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",1,0,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",1.5,0,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",2,0,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",2.5,0,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",3,1,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",3.5,23,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",4,50,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",4.5,94.5,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",5,136,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",5.5,201.5,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",6,266,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",6.5,351,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",7,438,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",7.5,548,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",8,661,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",8.5,788,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",9,918,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",9.5,1039.5,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",10,1161,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",10.5,1265.5,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",11,1370,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",11.5,1438,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",12,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",12.5,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",13,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",13.5,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",14,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",14.5,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",15,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",15.5,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",16,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",16.5,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",17,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",17.5,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",18,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",18.5,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",19,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",19.5,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77C-1500",20,1500,"山东东营东方电气FD77-1500当地空气密度功率曲线",1.232]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",0,0,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",0.5,0,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",1,0,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",1.5,0,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",2,0,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",2.5,0,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",3,0,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",3.5,0,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",4,20,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",4.5,35,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",5,56,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",5.5,78,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",6,105,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",6.5,135,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",7,171,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",7.5,211,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",8,258,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",8.5,307,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",9,362,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",9.5,416,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",10,475,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",10.5,532,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",11,589,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",11.5,640,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",12,689,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",12.5,729,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",13,763,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",13.5,789,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",14,807,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",14.5,823,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",15,829,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",15.5,838,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",16,838,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",16.5,844,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",17,841,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",17.5,849,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",18,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",18.5,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",19,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",19.5,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",20,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",20.5,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",21,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",21.5,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",22,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",22.5,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",23,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",23.5,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",24,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",24.5,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V52-850","VT-52/0.85",25,850,"扎鲁特扎一风电场V52-850当地空气密度功率曲线",1.162]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",0,0,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",0.5,0,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",1,0,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",1.5,0,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",2,0,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",2.5,0,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",3,0,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",3.5,0,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",4,6,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",4.5,41,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",5,102,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",5.5,158,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",6,218,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",6.5,313,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",7,384,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",7.5,506,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",8,598,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",8.5,762,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",9,871,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",9.5,1028,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",10,1179,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",10.5,1339,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",11,1489,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",11.5,1632,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",12,1739,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",12.5,1821,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",13,1864,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",13.5,1907,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",14,1931,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",14.5,1948,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",15,1960,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",15.5,1965,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",16,1969,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",16.5,1970,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",17,1985,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",17.5,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",18,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",18.5,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",19,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",19.5,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",20,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",20.5,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",21,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",21.5,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",22,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",22.5,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",23,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",23.5,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",24,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",24.5,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","VT-80/2.0",25,2000,"大水菠萝风电场V80-2.0MW当地空气密度功率曲线",1]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",0,0,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",0.5,0,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",1,0,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",1.5,0,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",2,0,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",2.5,33,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",3,100,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",3.5,197,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",4,338,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",4.5,503,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",5,696,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",5.5,927,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",6,1204,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",6.5,1531,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",7,1912,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",7.5,2349,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",8,2836,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",8.5,3351,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",9,3751,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",9.5,3929,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",10,3974,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",10.5,3985,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",11,3988,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",11.5,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",12,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",12.5,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",13,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",13.5,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",14,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",14.5,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",15,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",15.5,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",16,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",16.5,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",17,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",17.5,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",18,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",18.5,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",19,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",19.5,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",20,4000,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",20.5,3923,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",21,3720,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",21.5,3569,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",22,3454,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",22.5,3225,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",23,3058,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",23.5,2876,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",24,2792,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",24.5,2648,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["XlX3d9wp","重庆山水风电场","MY4.0se-166","MY4.0se-166",25,2508,"山水明阳MY4.0se-166当地空气密度功率曲线",1.03]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",0,0,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",0.5,0,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",1,0,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",1.5,0,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",2,0,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",2.5,0,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",3,42,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",3.5,69,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",4,117,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",4.5,183,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",5,262,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",5.5,360,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",6,470,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",6.5,599,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",7,753,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",7.5,915,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",8,1105,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",8.5,1283,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",9,1466,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",9.5,1642,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",10,1771,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",10.5,1880,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",11,1924,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",11.5,1950,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",12,1969,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",12.5,1992,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",13,1993,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",13.5,1997,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",14,1999,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",14.5,2000,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",15,2000,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",15.5,2000,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",16,2000,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",16.5,2000,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",17,2000,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",17.5,2000,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",18,1994,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",18.5,1983,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",19,1969,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",19.5,1951,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",20,1920,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",20.5,1876,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",21,1812,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",21.5,1758,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",22,1688,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",22.5,1614,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",23,1553,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",23.5,1515,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",24,1469,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",24.5,1428,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["Fmt5Dyir","青海辰旭风电场","DF131-2500","DF131-2500",25,1381,"青海辰旭东方电气DF131-2500kW当地空气密度功率曲线",0.897]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",0,0,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",0.5,0,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",1,0,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",1.5,0,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",2,0,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",2.5,0,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",3,0,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",3.5,51.02,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",4,85.18,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",4.5,129.21,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",5,182.54,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",5.5,247.74,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",6,325.41,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",6.5,417.04,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",7,522.19,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",7.5,641.86,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",8,773.31,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",8.5,912.02,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",9,1052.62,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",9.5,1196.57,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",10,1338.71,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",10.5,1481.03,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",11,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",11.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",12,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",12.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",13,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",13.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",14,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",14.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",15,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",15.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",16,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",16.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",17,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",17.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",18,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",18.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",19,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",19.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",20,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",20.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",21,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",21.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",22,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",22.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",23,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",23.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",24,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",24.5,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",25,1500,"大水菠萝风电场V80-2.0MW（50号）当地空气密度功率曲线",1]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",0,0,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",0.5,0,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",1,0,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",1.5,0,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",2,0,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",2.5,49,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",3,119,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",3.5,231,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",4,392,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",4.5,580,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",5,802,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",5.5,1068,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",6,1386,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",6.5,1763,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",7,2202,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",7.5,2707,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",8,3277,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",8.5,3767,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",9,3924,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",9.5,3975,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",10,3992,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",10.5,3996,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",11,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",11.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",12,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",12.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",13,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",13.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",14,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",14.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",15,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",15.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",16,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",16.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",17,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",17.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",18,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",18.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",19,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",19.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",20,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",20.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",21,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",21.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",22,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",22.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",23,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",23.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",24,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",24.5,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["B7zmXcOi","云南蜜蜂山风电场","MY4.0se-166","MY4.0se-166",25,4000,"云南蜜蜂山MY4.0se-166当地空气密度功率曲线",0.924]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",0,0,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",0.5,0,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",1,0,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",1.5,0,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",2,0,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",2.5,0,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",3,108,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",3.5,205,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",4,324,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",4.5,462,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",5,632,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",5.5,842,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",6,1087,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",6.5,1379,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",7,1714,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",7.5,2073,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",8,2451,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",8.5,2842,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",9,3224,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",9.5,3396,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",10,3487,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",10.5,3523,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",11,3576,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",11.5,3592,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",12,3594,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",12.5,3596,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",13,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",13.5,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",14,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",14.5,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",15,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",15.5,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",16,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",16.5,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",17,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",17.5,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",18,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",18.5,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",19,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",19.5,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["SQhGR4pK","甘肃乾丰风电场","DEW-G3600-165","DEW-G3600-165",20,3600,"甘肃乾丰前台子东方电气DEW-G3600-165机型当地空气密度功率曲线",1.019]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",0,0,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",0.5,0,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",1,0,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",1.5,0,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",2,0,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",2.5,11.554,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",3,66.602,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",3.5,132.197,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",4,227.412,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",4.5,348.578,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",5,505.645,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",5.5,698.478,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",6,924.531,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",6.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",7,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",7.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",8,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",8.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",9,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",9.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",10,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",10.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",11,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",11.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",12,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",12.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",13,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",13.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",14,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",14.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",15,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",15.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",16,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",16.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",17,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",17.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",18,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",18.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",19,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",19.5,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MY3.0se-145",20,1000,"内蒙学田地风电场MySE3.0-145/90（51号）机型当地空气密度曲线",1.103]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",0,0,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",0.5,0,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",1,0,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",1.5,0,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",2,0,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",2.5,0,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",3,51,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",3.5,90,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",4,140,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",4.5,190,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",5,285,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",5.5,364,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",6,472,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",6.5,601,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",7,729,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",7.5,879,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",8,1036,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",8.5,1195,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",9,1324,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",9.5,1497,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",10,1604,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",10.5,1730,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",11,1821,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",11.5,1886,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",12,1940,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",12.5,1973,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",13,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",13.5,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",14,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",14.5,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",15,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",15.5,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",16,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",16.5,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",17,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",17.5,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",18,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",18.5,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",19,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",19.5,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",20,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",20.5,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",21,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",21.5,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",22,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",22.5,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",23,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",23.5,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",24,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",24.5,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["3Q7evHuX","山西茨庙风电场","W2000-111","W2000-111",25,2000,"山西茨庙风电场上海电气W2000-111-80机型当地空气密度曲线",1.129]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",0,0,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",0.5,0,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",1,0,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",1.5,0,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",2,0,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",2.5,69,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",3,122,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",3.5,198,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",4,282,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",4.5,383,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",5,509,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",5.5,685,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",6,893,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",6.5,1171,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",7,1466,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",7.5,1769,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",8,2039,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",8.5,2309,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",9,2448,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",9.5,2497,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",10,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",10.5,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",11,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",11.5,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",12,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",12.5,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",13,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",13.5,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",14,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",14.5,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",15,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",15.5,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",16,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",16.5,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",17,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",17.5,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",18,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",18.5,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",19,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",19.5,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["hRfoM8LY","山东莱州风电场（桂冠）","GW140-2500","GW140/2500",20,2500,"山东莱州金风GW-2500机型当地空气密度曲线",1.122]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0,0,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0.5,0,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1,0,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1.5,0,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2,0,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2.5,0,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3,5,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3.5,21.7,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4,52,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4.5,97.8,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5,156,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5.5,223,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6,300,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6.5,389.1,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7,492,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7.5,609.7,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8,741,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8.5,886,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9,1053,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9.5,1240,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10,1397,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10.5,1477.9,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24.5,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",25,1500,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",25.5,0,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",26,0,"山东泽库华创CCWE-1500-82.DF机型当地空气密度曲线",1.214]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",0,0,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",0.5,0,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",1,0,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",1.5,0,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",2,0,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",2.5,0,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",3,49,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",3.5,152,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",4,298,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",4.5,479,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",5,685,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",5.5,921,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",6,1198,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",6.5,1523,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",7,1902,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",7.5,2339,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",8,2836,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",8.5,3382,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",9,3909,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",9.5,4274,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",10,4404,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",10.5,4459,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",11,4485,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",11.5,4494,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",12,4499,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",12.5,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",13,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",13.5,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",14,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",14.5,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",15,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",15.5,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",16,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",16.5,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",17,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",17.5,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",18,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",18.5,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",19,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",19.5,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",20,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",20.5,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",21,4500,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",21.5,4404,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",22,4248,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",22.5,4091,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",23,3934,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",23.5,3776,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",24,3619,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",24.5,3461,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","EN171-4500","EN171-4500",25,3302,"内蒙图步盛风电场远景能源EN171-4500机型当地空气密度曲线",1.03]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",0,0,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",0.5,0,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",1,0,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",1.5,0,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",2,0,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",2.5,0,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",3,117,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",3.5,267,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",4,437,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",4.5,604,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",5,813,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",5.5,1065,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",6,1363,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",6.5,1718,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",7,2108,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",7.5,2625,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",8,3135,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",8.5,3654,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",9,4191,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",9.5,4662,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",10,5090,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",10.5,5299,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",11,5388,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",11.5,5451,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",12,5484,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",12.5,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",13,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",13.5,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",14,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",14.5,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",15,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",15.5,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",16,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",16.5,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",17,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",17.5,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",18,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",18.5,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",19,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",19.5,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",20,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",20.5,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",21,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",21.5,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",22,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",22.5,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",23,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",23.5,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",24,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",24.5,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["qwx0AWl6","福建显美风电场","MY5.0se-155","MY5.0se-155",25,5500,"福建显美明阳智能MY5.0se-155机型当地空气密度功率曲线",1.197]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",0,0,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",0.5,0,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",1,0,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",1.5,0,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",2,0,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",2.5,0,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",3,9.25,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",3.5,14.336714,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",4,26.51,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",4.5,50.593286,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",5,91.41,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",5.5,151.185142,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",6,221.75,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",6.5,294.118645,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",7,366.43,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",7.5,439.612779,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",8,518.63,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",8.5,609.095241,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",9,715.19,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",9.5,839.550009,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",10,980.06,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",10.5,1133.925973,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",11,1300.39,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",11.5,1477.163598,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",12,1653.8,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",12.5,1816.105884,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",13,1943.06,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",13.5,1998.15,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",14,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",14.5,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",15,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",15.5,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",16,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",16.5,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",17,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",17.5,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",18,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",18.5,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",19,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",19.5,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",20,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",20.5,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",21,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",21.5,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",22,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",22.5,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",23,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",23.5,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",24,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",24.5,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["iD2zeJQE","京津冀骆驼沟风电场","XE72-2000","XE72-2000",25,2000,"京津冀骆驼沟二期湘电风能XE72-2000功率曲线",1.223]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",0,0,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",0.5,0,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",1,0,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",1.5,0,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",2,0,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",2.5,0,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",3,0,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",3.5,1,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",4,38,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",4.5,67.5,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",5,97,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",5.5,144,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",6,191,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",6.5,256.5,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",7,322,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",7.5,411,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",8,500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",8.5,612.5,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",9,725,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",9.5,856,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",10,987,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",10.5,1122.5,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",11,1258,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",11.5,1394,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",12,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",12.5,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",13,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",13.5,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",14,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",14.5,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",15,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",15.5,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",16,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",16.5,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",17,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",17.5,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",18,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",18.5,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",19,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",19.5,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",20,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",20.5,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",21,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",21.5,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",22,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",22.5,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",23,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",23.5,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",24,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",24.5,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["18RIzjHn","京津冀西桥梁风电场","FD77-1500","FD77D",25,1500,"京津冀西桥梁东汽FD77D风机功率曲线",1.06]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",0,0,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",0.5,0,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",1,0,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",1.5,0,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",2,0,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",2.5,0,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",3,27,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",3.5,59,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",4,91,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",4.5,138.5,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",5,186,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",5.5,256.5,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",6,327,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",6.5,426,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",7,525,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",7.5,657,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",8,789,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",8.5,944.5,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",9,1100,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",9.5,1266.5,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",10,1433,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",10.5,1466.5,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",11,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",11.5,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",12,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",12.5,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",13,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",13.5,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",14,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",14.5,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",15,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",15.5,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",16,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",16.5,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",17,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",17.5,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",18,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",18.5,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",19,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",19.5,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",20,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",20.5,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",21,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",21.5,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["lGPvQPjH","吉林双辽风电场","GW82-1500","GW-1500",22,1500,"吉林双辽金风82-1500机型当地空气密度曲线",1.225]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",0,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",0.5,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",1,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",1.5,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",2,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",2.5,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",3,51,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",3.5,112,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",4,198,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",4.5,307,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",5,449,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",5.5,624,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",6,832,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",6.5,1062,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",7,1332,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",7.5,1634,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",8,1970,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",8.5,2293,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",9,2594,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",9.5,2860,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",10,3024,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",10.5,3109,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",11,3155,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",11.5,3173,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",12,3187,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",12.5,3193,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",13,3199,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",13.5,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",14,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",14.5,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",15,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",15.5,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",16,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",16.5,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",17,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",17.5,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",18,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",18.5,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",19,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",19.5,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",20,3200,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",20.5,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",21,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",21.5,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",22,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",22.5,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",23,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",23.5,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",24,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",24.5,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["v67gM3S1","内蒙学田地风电场","MY3.0se-145","MySE3.0-145",25,0,"内蒙学田地风电场MySE3.0-14590机型当地空气密度曲线",1.103]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",0,0,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",0.5,0,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",1,0,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",1.5,0,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",2,0,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",2.5,2,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",3,53,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",3.5,115,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",4,202,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",4.5,313,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",5,457,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",5.5,635,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",6,846,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",6.5,1079,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",7,1353,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",7.5,1659,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",8,1999,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",8.5,2325,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",9,2625,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",9.5,2886,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",10,2950,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",10.5,3000,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",11,3000,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",11.5,3000,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",12,3000,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",12.5,3000,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",13,3000,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",13.5,3000,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",14,3000,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",14.5,3000,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",15,3000,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",15.5,3000,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["CEXvCYPY","内蒙达日罕风电场","MY3.0se-145","MySE3.0-145",16,3000,"内蒙达日罕风电场MySE3.0-145机型当地空气密度功率曲线",1.061]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",0,0,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",0.5,0,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",1,0,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",1.5,0,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",2,0,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",2.5,0,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",3,0,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",3.5,0,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",4,12.69,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",4.5,27.79,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",5,42.88,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",5.5,67.8,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",6,92.72,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",6.5,127.29,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",7,161.86,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",7.5,204.26,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",8,246.66,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",8.5,293.51,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",9,340.35,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",9.5,387.48,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",10,434.61,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",10.5,478,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",11,521.4,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",11.5,558,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",12,594,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",12.5,621,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",13,648,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",13.5,665,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",14,682,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",14.5,689,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",15,695,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",15.5,693,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",16,693,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",16.5,685,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",17,680,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",17.5,671,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",18,664,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",18.5,660,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",19,656,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",19.5,658,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",20,661,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",20.5,672,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",21,683,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",21.5,701,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",22,715,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",22.5,729,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",23,744,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",23.5,750,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",24,754,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",24.5,752,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["TefEHata","内蒙那仁风电场","S48-750","GW-48/0.75",25,748,"那仁风电场S48-750当地空气密度功率曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",0,0,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",0.5,0,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",1,0,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",1.5,20,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",2,26,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",2.5,50,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",3,97,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",3.5,170,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",4,267,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",4.5,391,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",5,551,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",5.5,745,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",6,973,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",6.5,1240,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",7,1524,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",7.5,1746,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",8,2051,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",8.5,2243,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",9,2377,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",9.5,2455,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",10,2487,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",10.5,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",11,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",11.5,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",12,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",12.5,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",13,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",13.5,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",14,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",14.5,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",15,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",15.5,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",16,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",16.5,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",17,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",17.5,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",18,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",18.5,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",19,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",19.5,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",20,2500,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",20.5,2404,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",21,2311,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",21.5,2215,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",22,2122,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",22.5,2026,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",23,1929,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",23.5,1839,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",24,1746,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",24.5,1651,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",25,1559,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",25.5,1465,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",26,1368,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",26.5,1277,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",27,1181,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",27.5,1089,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",28,1000,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",28.5,0,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["S8gOoMyU","宁夏新庄集风电场","DF131-2500","DF131-2500",29,0,"新庄集风电场东汽DF131-2500机型当地空气密度曲线",1.122]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",0,0,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",0.5,0,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",1,0,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",1.5,0,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",2,0,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",2.5,0,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",3,22,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",3.5,50,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",4,82,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",4.5,122,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",5,183,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",5.5,258,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",6,340,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",6.5,440,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",7,544,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",7.5,654,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",8,790,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",8.5,910,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",9,1020,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",9.5,1140,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",10,1260,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",10.5,1362,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",11,1440,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",11.5,1470,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",12,1490,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",12.5,1500,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",13,1510,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",13.5,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",14,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",14.5,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",15,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",15.5,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",16,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",16.5,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",17,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",17.5,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",18,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",18.5,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",19,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",19.5,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",20,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",20.5,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["Twr2SPNt","内蒙塔林花风电场","CCWE1500-82.DF","CCWE1500-82.DF",21,1520,"塔林花风电场CCWE-1500-82四期当地空气密度功率曲线",1.16]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0,0,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0.5,0,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1,0,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1.5,0,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2,0,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2.5,0,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3,5,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3.5,21.7,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4,52,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4.5,97.8,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5,156,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5.5,223,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6,300,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6.5,389.1,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7,492,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7.5,609.7,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8,741,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8.5,886,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9,1053,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9.5,1240,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10,1397,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10.5,1477.9,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24.5,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",25,1500,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",25.5,0,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["olgHrLiO","山东泽库风电场","CCWE1500-82.DF","CCWE-1500/82.DF",26,0,"山东泽库CCWE-1500/82.DF功率曲线",1.214]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",0,0,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",0.5,0,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",1,0,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",1.5,0,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",2,0,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",2.5,0,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",3,71,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",3.5,152,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",4,257,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",4.5,382,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",5,535,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",5.5,723,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",6,949,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",6.5,1207,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",7,1510,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",7.5,1857,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",8,2246,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",8.5,2648,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",9,3017,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",9.5,3287,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",10,3458,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",10.5,3579,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",11,3665,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",11.5,3768,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",12,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",12.5,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",13,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",13.5,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",14,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",14.5,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",15,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",15.5,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",16,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",16.5,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",17,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",17.5,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",18,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",18.5,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",19,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",19.5,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["RxWasih5","山西君辉风电场","DEW-D3800-148","DEW-D3800-148",20,3800,"山西君辉风电场DEW-D3800-148机型当地空气密度曲线",1.081]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",0,0,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",0.5,0,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",1,0,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",1.5,0,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",2,0,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",2.5,0,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",3,25.67,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",3.5,49.54,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",4,77.98,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",4.5,122.05,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",5,173.7,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",5.5,233.51,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",6,315.95,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",6.5,407.58,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",7,524.04,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",7.5,644.96,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",8,790.23,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",8.5,931.95,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",9,1093.06,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",9.5,1266.03,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",10,1421.13,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",10.5,1553.46,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",11,1662.83,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",11.5,1761.86,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",12,1844.69,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",12.5,1923.05,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",13,1975.65,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",13.5,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",14,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",14.5,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",15,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",15.5,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",16,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",16.5,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",17,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",17.5,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",18,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",18.5,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",19,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",19.5,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",20,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",20.5,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",21,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",21.5,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",22,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",22.5,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",23,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",23.5,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",24,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",24.5,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["vyKpQlcD","贵州大风坪风电场","W2000-111","W2000-111",25,2000,"贵州大风坪风电场上海电气W2000-111机型当地空气密度曲线",1.023]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",0,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",0.5,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",1,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",1.5,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",2,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",2.5,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",3,40,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",3.5,67,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",4,100,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",4.5,142,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",5,194,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",5.5,258,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",6,335,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",6.5,427,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",7,533,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",7.5,656,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",8,795,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",8.5,955,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",9,1100,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",9.5,1229,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",10,1339,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",10.5,1423,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",11,1472,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",11.5,1495,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",12,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",12.5,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",13,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",13.5,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",14,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",14.5,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",15,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",15.5,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",16,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",16.5,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",17,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",17.5,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",18,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",18.5,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",19,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",19.5,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",20,1500,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",20.5,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",21,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",21.5,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",22,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",22.5,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",23,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",23.5,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",24,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",24.5,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",25,0,"山东东营东方电气FD77-1500（叶片加长）当地空气密度功率曲线",1.232]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",0,0,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",0.5,0,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",1,0,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",1.5,0,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",2,0,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",2.5,0,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",3,0,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",3.5,0,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",4,21.9,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",4.5,42.1,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",5,57.8,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",5.5,79.6,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",6,107.1,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",6.5,140.6,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",7,174,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",7.5,213.6,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",8,260.6,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",8.5,305.5,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",9,364.3,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",9.5,420.9,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",10,474.9,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",10.5,545.3,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",11,593.4,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",11.5,654,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",12,693.2,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",12.5,737.6,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",13,764.1,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",13.5,793.2,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",14,811.8,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",14.5,835.9,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",15,846,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",15.5,847,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",16,849,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",16.5,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",17,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",17.5,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",18,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",18.5,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",19,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",19.5,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",20,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",20.5,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",21,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",21.5,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",22,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",22.5,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",23,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",23.5,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",24,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",24.5,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["LqRDXfA7","内蒙塞罕坝风电场","V52-850","VT-52/0.85",25,850,"赛罕坝风电场V52-850当地空气密度功率曲线",1.16]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",0,0,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",0.5,0,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",1,0,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",1.5,0,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",2,0,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",2.5,15.7196,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",3,35.570052,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",3.5,61.265484,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",4,89.20665,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",4.5,133.579377,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",5,193.970271,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",5.5,260.685,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",6,364.4992,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",6.5,477.483479,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",7,592.43555,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",7.5,713.817252,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",8,861.8076,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",8.5,1013.208812,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",9,1125.153802,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",9.5,1252.34235,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",10,1332.204,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",10.5,1398.0672,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",11,1442.6325,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",11.5,1489.88,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",12,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",12.5,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",13,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",13.5,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",14,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",14.5,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",15,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",15.5,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",16,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",16.5,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",17,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",17.5,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",18,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",18.5,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",19,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",19.5,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",20,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",20.5,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",21,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",21.5,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",22,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",22.5,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",23,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",23.5,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",24,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",24.5,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["kA8QcZ7s","甘肃景泰风电场","SL1500-82","SL1500-82",25,1500,"甘肃景泰华锐SL1500-82当地空气密度功率曲线",1.002]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",0,0,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",0.5,0,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",1,0,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",1.5,0,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",2,0,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",2.5,38.75,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",3,117.31,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",3.5,238.71,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",4,405.39,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",4.5,619,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",5,888.22,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",5.5,1209.4,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",6,1590.84,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",6.5,2022.62,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",7,2525.77,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",7.5,3074.28,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",8,3622.12,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",8.5,4075.36,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",9,4441.65,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",9.5,4708.87,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",10,4874.43,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",10.5,4952.7,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",11,4988.58,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",11.5,5000,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",12,5000,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",12.5,5000,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",13,5000,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",13.5,5000,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",14,5000,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",14.5,5000,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",15,5000,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",15.5,5000,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",16,5000,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",16.5,4997.22,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",17,4821.02,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",17.5,4608.82,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",18,4381.79,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",18.5,4112.38,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",19,3848.17,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",19.5,3578.31,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["685wYKee","山西白玉山风电场","GW191-5000","GW191-5000",20,3362.53,"山西白玉山风电场GW191-5000当地功率曲线",1.225]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",0,0,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",0.5,0,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",1,0,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",1.5,0,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",2,0,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",2.5,0,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",3,11,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",3.5,18,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",4,30,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",4.5,65,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",5,110,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",5.5,194,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",6,289,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",6.5,351,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",7,430,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",7.5,503,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",8,594,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",8.5,713,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",9,850,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",9.5,1004,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",10,1178,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",10.5,1351,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",11,1545,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",11.5,1687,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",12,1851,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",12.5,1884,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",13,1936,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",13.5,1958,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",14,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",14.5,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",15,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",15.5,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",16,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",16.5,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",17,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",17.5,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",18,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",18.5,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",19,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",19.5,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",20,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",20.5,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",21,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",21.5,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",22,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",22.5,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",23,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",23.5,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",24,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",24.5,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["d5btw15h","福建六鳌风电场","XE72-2000","XE72-2000",25,2000,"福建六鳌风电场湘电XE-2000当地空气密度",1.15]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",0,0,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",0.5,0,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",1,0,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",1.5,0,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",2,0,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",2.5,76.77,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",3,151.77,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",3.4,245.83,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",4,403.97,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",4.5,584.6,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",5.1,903.78,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",5.5,1062.18,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",6,1403.4,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",6.5,1692.26,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",7.1,2028.25,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",7.5,2301.27,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",8,2679.89,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",8.5,3129.82,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",9,3703.09,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",9.5,3862.22,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",10,3867.33,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",10.5,3940.78,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",11,4003.12,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",11.5,4064.35,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",12,4064.93,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",12.5,4070.78,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",13,4066.23,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",13.5,4069.43,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",14,4071.24,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",14.5,4069.19,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",15,4070.66,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",15.5,4069.16,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",16,4071.17,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",16.5,4070.05,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",17,4070.15,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",17.5,4070.56,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",18,4071.03,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",19,4068.51,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",19.5,4069.14,"重庆兴顺风电场2期明阳MY4.0se-166当地空气密度功率曲线",1.019]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",0,0,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",0.5,0,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",1,0,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",1.5,0,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",2,0,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",2.5,0,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",3,0,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",3.5,0,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",4,90.6,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",4.5,136,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",5,194,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",5.5,268.5,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",6,345.6,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",6.5,464.9,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",7,557.3,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",7.5,696.4,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",8,838.4,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",8.5,1021.2,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",9,1163.1,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",9.5,1402,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",10,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",10.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",11,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",11.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",12,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",12.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",13,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",13.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",14,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",14.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",15,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",15.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",16,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",16.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",17,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",17.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",18,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",18.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",19,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",19.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",20,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",20.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",21,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",21.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",22,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",22.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",23,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",23.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",24,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",24.5,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["fB9guiq0","内蒙如德风电场","UP1500-86","UP-86/1.5",25,1500,"如德风电场UP86-1500当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",0,0,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",0.5,0,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",1,0,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",1.5,0,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",2,0,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",2.5,69,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",3,103,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",3.5,149,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",4,178,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",4.5,247,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",5,320,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",5.5,418,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",6,524,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",6.5,643,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",7,803,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",7.5,921,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",8,1080,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",8.5,1215,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",9,1300,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",9.5,1355,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",10,1413,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",10.5,1455,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",11,1500,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",11.5,1500,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",12,1500,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",12.5,1500,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",13,1500,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",13.5,1500,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",14,1500,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",14.5,1500,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",15,1500,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",15.5,1500,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",16,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",16.5,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",17,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",17.5,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",18,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",18.5,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",19,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",19.5,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",20,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",20.5,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",21,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",21.5,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",22,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",22.5,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",23,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",23.5,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",24,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",24.5,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["cd6WYLw0","内蒙道德风电场","SL1500-82","SL-82/1.5",25,1520,"道德风电场SL1500-82当地空气密度功率曲线",1.15]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",0,0,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",0.5,0,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",1,0,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",1.5,0,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",2,0,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",2.5,0,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",3,0,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",3.5,0,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",4,20,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",4.5,35,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",5,57,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",5.5,78,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",6,106,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",6.5,137,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",7,173,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",7.5,214,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",8,260,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",8.5,310,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",9,365,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",9.5,420,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",10,480,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",10.5,537,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",11,595,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",11.5,646,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",12,696,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",12.5,736,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",13,770,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",13.5,797,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",14,815,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",14.5,831,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",15,837,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",15.5,846,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",16,846,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",16.5,849,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",17,849,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",17.5,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",18,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",18.5,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",19,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",19.5,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",20,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",20.5,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",21,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",21.5,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",22,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",22.5,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",23,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",23.5,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",24,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",24.5,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["0JLh05br","内蒙大西山风电场","V52-850","V52-850",25,850,"内蒙大西山维斯塔斯V52-850当地空气密度功率曲线",1.06]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",0,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",0.5,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",1,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",1.5,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",2,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",2.5,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",3,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",3.5,37,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",4,58,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",4.5,87,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",5,125,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",5.5,171,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",6,228,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",6.5,296,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",7,376,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",7.5,470,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",8,578,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",8.5,702,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",9,842,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",9.5,999,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",10,1154,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",10.5,1230,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",11,1300,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",11.5,1345,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",12,1430,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",12.5,1493,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",13,1496.5,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",13.5,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",14,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",14.5,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",15,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",15.5,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",16,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",16.5,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",17,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",17.5,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",18,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",18.5,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",19,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",19.5,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",20,1500,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",20.5,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",21,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",21.5,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",22,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",22.5,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",23,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",23.5,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",24,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",24.5,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["lOvTtdZJ","山东东营风电场","FD77-1500","FD77-1500",25,0,"山东东营东方电气FD77-1500（加装增功组当地件）空气密度功率曲线",1.232]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",0,0,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",0.5,0,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",1,0,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",1.5,0,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",2,0,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",2.5,0,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",3,3.4695,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",3.5,25.2068,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",4,57.1046,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",4.5,91.4872,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",5,133.786,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",5.5,178.848,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",6,239.113,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",6.5,310.317,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",7,392.394,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",7.5,488.845,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",8,601.32,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",8.5,730.243,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",9,866.755,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",9.5,1006.78,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",10,1147.58,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",10.5,1281.81,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",11,1405.76,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",11.5,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",12,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",12.5,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",13,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",13.5,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",14,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",14.5,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",15,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",15.5,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",16,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",16.5,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",17,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",17.5,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",18,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",18.5,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",19,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",19.5,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["KUSMbt7f","山西凌云口风电场","SL1500-82","SL1500/82",20,1500.61,"山西凌云口华锐科技SL1500/82风机公功率曲线",1.007]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",0,0,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",0.5,0,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",1,0,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",1.5,0,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",2,0,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",2.5,76,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",3,112,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",3.5,189,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",4,276,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",4.5,383,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",5,537,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",5.5,720,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",6,974,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",6.5,1202,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",7,1502,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",7.5,1829,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",8,2200,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",8.5,2592,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",9,2959,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",9.5,3319,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",10,3431,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",10.5,3467,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",11,3475,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",11.5,3478,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",12,3479,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",12.5,3482,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",13,3486,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",13.5,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",14,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",14.5,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",15,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",15.5,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",16,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",16.5,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",17,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",17.5,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",18,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",18.5,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",19,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",19.5,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",20,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",20.5,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",21,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",21.5,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",22,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",22.5,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",23,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",23.5,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",24,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",24.5,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","W3450-146","W3450-146",25,3487,"山西圣水塘三期风电场W3450-146机型当地空气密度曲线",1.031]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",0,0,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",0.5,0,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",1,0,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",1.5,0,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",2,0,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",2.5,0,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",3,32,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",3.5,102,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",4,193,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",4.5,303,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",5,431,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",5.5,579,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",6,752,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",6.5,957,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",7,1199,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",7.5,1475,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",8,1790,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",8.5,2142,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",9,2464,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",9.5,2623,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",10,2641,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",10.5,2647,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",11,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",11.5,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",12,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",12.5,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",13,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",13.5,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",14,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",14.5,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",15,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",15.5,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",16,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",16.5,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",17,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",17.5,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",18,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",18.5,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",19,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",19.5,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["rQQ0AxFG","青海存志风电场","EN141-2650","EN-141/2.65",20,2650,"青海存志风电场EN-141/2.65机型当地空气密度功率曲线",0.95]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",0,0,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",0.5,0,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",1,0,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",1.5,0,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",2,0,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",2.5,0,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",3,74.5,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",3.5,121.3,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",4,190.9,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",4.5,278.1,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",5,393.96,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",5.5,537.8,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",6,699.7,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",6.5,907.2,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",7,1143.2,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",7.5,1396.2,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",8,1608,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",8.5,1855.7,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",9,1935.4,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",9.5,1999.3,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",10,2007.8,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",10.5,2007.53,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",11,2005.5,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",11.5,2008.5,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",12,2008.7,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",12.5,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",13,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",13.5,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",14,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",14.5,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",15,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",15.5,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",16,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",16.5,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",17,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",17.5,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",18,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",18.5,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",19,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",19.5,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",20,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",20.5,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",21,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",21.5,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",22,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",22.5,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",23,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",23.5,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",24,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",24.5,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["GPwpiRQ3","山西圣水塘风电场","MY2.0se-121","MY2.0-121",25,2009,"山西圣水塘二期风电场MYse2.0-121机型当地空气密度曲线",1.031]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",0,0,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",0.5,0,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",1,0,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",1.5,0,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",2,0,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",2.5,0,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",3,10,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",3.5,21,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",4,33,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",4.5,62,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",5,86,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",5.5,125,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",6,160,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",6.5,208,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",7,262,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",7.5,335,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",8,398,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",8.5,470,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",9,568,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",9.5,638,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",10,732,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",10.5,792,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",11,833,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",11.5,845,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",12,847,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",12.5,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",13,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",13.5,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",14,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",14.5,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",15,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",15.5,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",16,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",16.5,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",17,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",17.5,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",18,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",18.5,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",19,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",19.5,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",20,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",20.5,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",21,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",21.5,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",22,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",22.5,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",23,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",23.5,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",24,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",24.5,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["uhX1ueLn","内蒙兴牧风电场","V52-850","VT-52/0.85",25,850,"兴牧风电场V60-850当地空气密度功率曲线",1.22]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",0,0,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",0.5,0,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",1,0,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",1.5,0,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",2,0,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",2.5,18.8,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",3,72.6,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",3.5,143.4,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",4,230,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",4.5,334.6,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",5,461.2,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",5.5,616.6,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",6,798.8,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",6.5,1013.8,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",7,1264,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",7.5,1545.6,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",8,1843.2,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",8.5,2116.4,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",9,2319.8,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",9.5,2451.2,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",10,2493.6,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",10.5,2499.8,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",11,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",11.5,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",12,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",12.5,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",13,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",13.5,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",14,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",14.5,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",15,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",15.5,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",16,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",16.5,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",17,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",17.5,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",18,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",18.5,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",19,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",19.5,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",20,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",20.5,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",21,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",21.5,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",22,2500,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",22.5,2000,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",23,2000,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",23.5,2000,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",24,2000,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",24.5,2000,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["7V2xSuma","新疆老君庙风电场","GW140-2500","GW140/2500",25,2000,"新疆老君庙风电场GW140/2.5机型当地空气密度功率曲线",1.1]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",0,0,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",0.5,0,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",1,0,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",1.5,0,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",2,0,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",2.5,19.8,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",3,53.397,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",3.5,88.4654,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",4,135.12553,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",4.5,207.27168,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",5,305.20232,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",5.5,400.6335,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",6,493.710525,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",6.5,605.9745,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",7,719.747571,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",7.5,863.058105,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",8,978.28965,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",8.5,1080.368352,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",9,1173.856593,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",9.5,1285.145158,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",10,1367.313242,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",10.5,1448.315579,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",11,1474.6248,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",11.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",12,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",12.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",13,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",13.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",14,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",14.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",15,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",15.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",16,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",16.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",17,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",17.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",18,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",18.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",19,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",19.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",20,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",20.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",21,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",21.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",22,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",22.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",23,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",23.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",24,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",24.5,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["PnAS8DhB","甘肃昌西一风电场","SL1500-82","SL1500-82",25,1500,"甘肃昌西一SL1500-BHM-华锐-V14.513当地空气密度功率曲线",1.062]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0,0,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0.5,0,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1,0,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1.5,0,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2,0,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2.5,0,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3,13.53,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3.5,35,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4,65.16,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4.5,101.2,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5,154.6,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5.5,218,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6,293.33,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6.5,375,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7,476.66,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7.5,587,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8,728.05,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8.5,869,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9,1013.62,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9.5,1170,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10,1284.1,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10.5,1388,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11,1419.2,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11.5,1479,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12,1470.83,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12.5,1470.83,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13,1484.12,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13.5,1484.12,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14,1486.83,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14.5,1486.83,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15,1486.53,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15.5,1486.53,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16,1482.95,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16.5,1482.95,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17,1478.81,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17.5,1478.81,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18,1476.17,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18.5,1476.17,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19,1468.4,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19.5,1468.4,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20,1461.49,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20.5,1461.49,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21,1457.28,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21.5,1457.28,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22,1453.13,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22.5,1456.62,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23,1456.62,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23.5,1481.63,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24,1481.63,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24.5,1494.55,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["jEFLXLqf","新疆哈巴河风电场","CCWE1500-82.DF","CCWE-1500/82.DF",25,1494.55,"哈巴河华创ccwe-1500/82当地空气密度功率曲线",1.121]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",0,0,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",0.5,0,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",1,0,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",1.5,0,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",2,0,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",2.5,24.4,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",3,77.8,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",3.5,149.2,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",4,239.6,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",4.5,349.4,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",5,480.6,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",5.5,640.4,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",6,831,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",6.5,1057.6,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",7,1303.8,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",7.5,1563.2,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",8,1800.4,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",8.5,2012,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",9,2190.2,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",9.5,2331,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",10,2442.2,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",10.5,2480.6,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",11,2492.4,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",11.5,2498.4,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",12,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",12.5,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",13,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",13.5,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",14,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",14.5,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",15,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",15.5,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",16,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",16.5,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",17,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",17.5,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",18,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",18.5,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",19,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",19.5,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",20,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",20.5,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",21,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",21.5,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",22,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",22.5,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["8vr7SXec","河南瑞源风电场","GW140-2500","GW140/2500",23,2500,"河南瑞源风电场GW140-2500机型当地空气密度功率曲线",1.22]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",0,0,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",0.5,0,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",1,0,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",1.5,0,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",2,0,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",2.5,49,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",3,119,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",3.5,231,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",4,392,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",4.5,580,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",5,802,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",5.5,1068,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",6,1386,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",6.5,1763,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",7,2202,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",7.5,2707,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",8,3277,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",8.5,3767,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",9,3924,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",9.5,3975,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",10,3992,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",10.5,3996,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",11,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",11.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",12,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",12.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",13,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",13.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",14,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",14.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",15,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",15.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",16,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",16.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",17,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",17.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",18,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",18.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",19,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",19.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",20,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",20.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",21,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",21.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",22,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",22.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",23,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",23.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",24,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",24.5,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY4.0se-166","MY4.0se-166",25,4000,"云南舍得风电场明阳智能MY4.0se-166机型当地空气密度曲线",0.924]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",0,0,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",0.5,0,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",1,0,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",1.5,0,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",2,0,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",2.5,0,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",3,38,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",3.5,153,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",4,302,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",4.5,473,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",5,681,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",5.5,914,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",6,1191,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",6.5,1522,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",7,1909,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",7.5,2354,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",8,2840,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",8.5,3154,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",9,3237,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",9.5,3286,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",10,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",10.5,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",11,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",11.5,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",12,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",12.5,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",13,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",13.5,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",14,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",14.5,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",15,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",15.5,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",16,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",16.5,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",17,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",17.5,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",18,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",18.5,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",19,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",19.5,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["Ki2UOEF8","吉林胜利风电场","EN156-3300","EN156-3300",20,3300,"胜利风场EN-156/3.3机型当地空气密度曲线",1.242]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",0,0,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",0.5,0,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",1,0,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",1.5,0,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",2,0,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",2.5,0,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",3,1,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",3.5,21,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",4,43,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",4.5,81,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",5,119,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",5.5,178,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",6,236,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",6.5,300,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",7,381,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",7.5,477,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",8,592,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",8.5,705,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",9,831,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",9.5,961,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",10,1072,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",10.5,1186,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",11,1286,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",11.5,1365,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",12,1440,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",12.5,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",13,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",13.5,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",14,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",14.5,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",15,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",15.5,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",16,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",16.5,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",17,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",17.5,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",18,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",18.5,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",19,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",19.5,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",20,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",20.5,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",21,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",21.5,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",22,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",22.5,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["VVy33PxA","河南清源风电场","FD77-1500","FD77-1500",23,1500,"河南清源东方电气FD77-1500当地空气密度功率曲线",1.13]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",0,0,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",0.5,0,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",1,0,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",1.5,0,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",2,0,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",2.5,0,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",3,0,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",3.5,0,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",4,22,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",4.5,40,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",5,59,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",5.5,90,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",6,110,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",6.5,150,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",7,181,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",7.5,222,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",8,271,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",8.5,331,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",9,380,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",9.5,445,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",10,498,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",10.5,563,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",11,615,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",11.5,670,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",12,713,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",12.5,753,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",13,782,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",13.5,808,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",14,821,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",14.5,837,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",15,840,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",15.5,846,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",16,847,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",16.5,849,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",17,849,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",17.5,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",18,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",18.5,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",19,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",19.5,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",20,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",20.5,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",21,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",21.5,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",22,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",22.5,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",23,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",23.5,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",24,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",24.5,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V52-850","VT-52/0.85",25,850,"东山风电场V52-850当地空气密度功率曲线",1.15]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",0,0,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",0.5,0,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",1,0,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",1.5,0,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",2,0,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",2.5,16,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",3,49,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",3.5,92,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",4,148,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",4.5,221,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",5,309,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",5.5,417,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",6,546,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",6.5,692,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",7,872,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",7.5,1074,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",8,1305,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",8.5,1551,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",9,1772,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",9.5,2036,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",10,2224,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",10.5,2348,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",11,2408,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",11.5,2459,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",12,2489,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",12.5,2494,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",13,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",13.5,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",14,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",14.5,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",15,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",15.5,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",16,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",16.5,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",17,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",17.5,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",18,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",18.5,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",19,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",19.5,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["qjb3GalE","青海朝晖风电场","DF131-2500","DF131-2500",20,2500,"青海朝晖DF131-2500当地密度曲线",0.857]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",0,0,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",0.5,0,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",1,0,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",1.5,0,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",2,0,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",2.5,0,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",3,105,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",3.5,264,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",4,476,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",4.5,683,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",5,943,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",5.5,1257,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",6,1630,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",6.5,2073,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",7,2577,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",7.5,3152,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",8,3723,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",8.5,4135,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",9,4409,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",9.5,4610,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",10,4737,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",10.5,4840,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",11,4902,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",11.5,4950,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",12,4969,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",12.5,4988,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",13,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",13.5,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",14,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",14.5,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",15,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",15.5,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",16,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",16.5,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",17,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",17.5,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",18,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",18.5,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",19,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",19.5,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",20,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",20.5,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",21,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",21.5,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",22,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",22.5,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",23,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",23.5,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",24,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",24.5,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["suCL3QzI","云南舍得风电场","MY5.0se-166","MY5.0se-166",25,5000,"云南舍得风电场明阳智能MY5.0se-166机型当地空气密度曲线",0.924]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",0,0,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",0.5,0,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",1,0,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",1.5,0,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",2,0,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",2.5,0,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",3,4.46627,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",3.5,36.2793,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",4,72.1655,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",4.5,115.988,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",5,164.675,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",5.5,225.812,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",6,300.021,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",6.5,386.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",7,489.326,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",7.5,611.499,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",8,749.966,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",8.5,901.227,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",9,1064.34,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",9.5,1230.09,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",10,1395.97,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",10.5,1498.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",11,1499.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",11.5,1500.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",12,1500.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",12.5,1500.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",13,1500.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",13.5,1500.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",14,1500.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",14.5,1500.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",15,1500.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",15.5,1500.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",16,1500.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",16.5,1500.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","SL1500-82","SL1500-82",17,1500.61,"扎鲁特北沙拉风电场SL1500（叶片加长）当地空气密度功率曲线",1.162]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",0,0,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",0.5,0,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",1,0,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",1.5,0,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",2,0,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",2.5,0,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",3,0,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",3.5,32.71,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",4,52.34,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",4.5,75.4,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",5,107.8,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",5.5,152.88,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",6,212.27,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",6.5,286.29,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",7,374.25,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",7.5,474.49,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",8,584.57,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",8.5,701.32,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",9,821.08,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",9.5,939.86,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",10,1053.64,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",10.5,1158.63,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",11,1251.56,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",11.5,1329.92,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",12,1392.19,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",12.5,1437.89,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",13,1467.7,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",13.5,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",14,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",14.5,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",15,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",15.5,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",16,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",16.5,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",17,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",17.5,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",18,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",18.5,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",19,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",19.5,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",20,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",20.5,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",21,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",21.5,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",22,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",22.5,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",23,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",23.5,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",24,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",24.5,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",25,1500,"东山风电场V80-2000（133号）当地空气密度功率曲线",1.15]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",0,0,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",0.5,0,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",1,0,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",1.5,0,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",2,0,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",2.5,20,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",3,80,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",3.5,173,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",4,297,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",4.5,456,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",5,655,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",5.5,897,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",6,1179,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",6.5,1509,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",7,1897,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",7.5,2344,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",8,2843,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",8.5,3353,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",9,3858,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",9.5,4357,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",10,4650,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",10.5,4850,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",11,5015,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",11.5,5080,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",12,5150,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",12.5,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",13,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",13.5,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",14,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",14.5,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",15,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",15.5,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",16,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",16.5,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",17,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",17.5,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",18,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",18.5,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",19,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",19.5,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",20,5200,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",20.5,4930,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",21,4660,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",21.5,4390,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",22,4120,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",22.5,3850,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",23,3580,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",23.5,3310,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",24,3040,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",24.5,2770,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["nTMWNLRl","辽宁南岛风电场","MY5.2se-166","MY5.2se-166",25,2500,"上海南岛风电场明阳MY5.2se-166本地功率曲线",1.233]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",0,0,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",0.5,0,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",1,0,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",1.5,0,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",2,0,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",2.5,0,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",3,0,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",3.5,27,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",4,54,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",4.5,94,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",5,134,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",5.5,197,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",6,260,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",6.5,345,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",7,431,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",7.5,553,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",8,676,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",8.5,811,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",9,947,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",9.5,1090,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",10,1234,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",10.5,1351,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",11,1468,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",11.5,1606,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",12,1744,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",12.5,1812,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",13,1880,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",13.5,1911,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",14,1942,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",14.5,1960,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",15,1979,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",15.5,1985,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",16,1990,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",16.5,1994,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",17,1998,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",17.5,1999,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",18,1999,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",18.5,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",19,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",19.5,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",20,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",20.5,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",21,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",21.5,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",22,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",22.5,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",23,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",23.5,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",24,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",24.5,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["YgDkeKwF","内蒙扎鲁特风电场","V80-2000","VT-80/2.0",25,2000,"扎鲁特阿勒坦风电场V80-2000当地空气密度功率曲线",1.162]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",0,0,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",0.5,0,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",1,0,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",1.5,0,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",2,0,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",2.5,0,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",3,21.59,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",3.5,39.21,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",4,73.72,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",4.5,122.54,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",5,187.24,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",5.5,270.28,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",6,373.15,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",6.5,495.51,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",7,634.99,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",7.5,787.47,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",8,947.63,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",8.5,1109.5,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",9,1267.16,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",9.5,1415.2,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",10,1549.23,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",10.5,1666.05,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",11,1763.86,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",11.5,1842.22,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",12,1901.87,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",12.5,1944.6,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",13,1972.91,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",13.5,1989.69,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",14,1998,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",14.5,2000.69,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",15,2000.69,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",15.5,2000.69,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",16,2000.69,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",16.5,2000.69,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",17,2000.69,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",17.5,2000.88,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",18,2001.08,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",18.5,2002.73,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",19,2003.61,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",19.5,2003.61,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",20,2003.61,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",20.5,2003.61,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",21,2003.61,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",21.5,2003.61,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",22,2003.61,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",22.5,2003.61,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",23,2003.61,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",23.5,2003.61,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",24,2003.61,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",24.5,2003.61,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V90-2000","V90-2000",25,2003.61,"大水菠萝风电场V90-2.0MW标准空气密度功率曲线",1]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0,0,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",0.5,0,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1,0,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",1.5,0,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2,0,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",2.5,0,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3,25,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",3.5,44,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4,71,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",4.5,106,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5,148,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",5.5,199,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6,259,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",6.5,331,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7,414,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",7.5,509,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8,617,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",8.5,737,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9,858,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",9.5,967,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10,1068,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",10.5,1166,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11,1254,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",11.5,1323,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12,1375,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",12.5,1415,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13,1444,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",13.5,1462,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14,1473,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",14.5,1481,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15,1488,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",15.5,1495,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",16.5,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",17.5,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",18.5,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",19.5,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",20.5,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",21.5,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",22.5,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",23.5,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",24.5,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["xcuYzoUe","山西利民风电场","CCWE1500-82.DF","CCWE-1500/82.DF",25,1500,"山西利民华创风能CCWE-1500/82.DF风机功率曲线",1.027]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",0,0,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",0.5,0,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",1,0,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",1.5,0,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",2,0,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",2.5,14,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",3,101,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",3.5,233,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",4,392,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",4.5,577,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",5,796,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",5.5,1065,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",6,1390,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",6.5,1764,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",7,2196,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",7.5,2675,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",8,3184,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",8.5,3724,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",9,4272,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",9.5,4814,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",10,5335,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",10.5,5804,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",11,6194,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",11.5,6442,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",12,6591,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",12.5,6670,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",13,6689,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",13.5,6694,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",14,6700,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",14.5,6700,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",15,6700,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",15.5,6700,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",16,6678,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",16.5,6636,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",17,6532,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",17.5,6360,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",18,6155,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",18.5,5917,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",19,5680,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",19.5,5441,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",20,5195,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",20.5,4945,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",21,4694,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",21.5,4447,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",22,4208,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",22.5,3979,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",23,3766,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",23.5,3571,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["5vgxg6Ai","京津冀水泉风电场","GWH191-6700","GWH191-6700",24,3399,"京津冀水泉金风GWH191-6700机型当地空气密度曲线",1.065]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",0,0,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",0.5,0,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",1,0,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",1.5,0,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",2,0,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",2.5,0,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",3,15,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",3.5,103,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",4,240,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",4.5,405,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",5,601,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",5.5,840,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",6,1103,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",6.5,1402,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",7,1753,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",7.5,2155,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",8,2598,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",8.5,3029,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",9,3376,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",9.5,3688,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",10,3956,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",10.5,4225,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",11,4493,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",11.5,4730,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",12,4935,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",12.5,5122,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",13,5285,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",13.5,5386,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",14,5449,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",14.5,5487,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",15,5500,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",15.5,5500,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",16,5500,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",16.5,5500,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",17,5500,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",17.5,5500,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",18,5500,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",18.5,5500,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",19,5500,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",19.5,5500,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["HkCtndpL","四川马洪风电场","DEW-G5500-183","DEW-G5500-183",20,5500,"四川马洪风电场东方电气DEW-G5500-183机型当地空气密度曲线",0.847]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",0,0,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",0.5,0,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",1,0,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",1.5,0,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",2,0,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",2.5,26,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",3,86,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",3.5,167,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",4,266,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",4.5,388,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",5,535,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",5.5,712,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",6,924,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",6.5,1174,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",7,1454,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",7.5,1741,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",8,1998,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",8.5,2218,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",9,2374,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",9.5,2460,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",10,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",10.5,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",11,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",11.5,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",12,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",12.5,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",13,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",13.5,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",14,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",14.5,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",15,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",15.5,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",16,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",16.5,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",17,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",17.5,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",18,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",18.5,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",19,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",19.5,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["VZdTu9L6","江苏大丰风电场","GW140-2500","GW140/2500",20,2500,"江苏大丰二期风电场金风科技GW140-2500机型当地空气密度功率曲线",1.2187]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",0,0,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",0.5,0,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",1,0,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",1.5,0,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",2,0,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",2.5,48,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",3,108,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",3.5,199,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",4,324,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",4.5,498,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",5,733,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",5.5,1036,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",6,1366,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",6.5,1761,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",7,2230,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",7.5,2756,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",8,3256,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",8.5,3762,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",9,4235,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",9.5,4680,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",10,5169,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",10.5,5556,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",11,5838,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",11.5,6062,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",12,6140,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",12.5,6184,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",13,6218,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",13.5,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",14,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",14.5,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",15,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",15.5,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",16,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",16.5,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",17,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",17.5,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",18,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",18.5,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",19,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",19.5,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",20,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",20.5,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",21,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",21.5,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",22,6250,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",22.5,5625,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",23,5000,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",23.5,4375,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",24,3750,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",24.5,3125,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G6250-186","DEW-G6250-186",25,2500,"京津冀石门东方电气DEW-G6250-186机型当地空气密度曲线",1.028]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",0,0,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",0.5,0,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",1,0,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",1.5,0,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",2,0,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",2.5,0,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",3,0,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",3.5,35,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",4,55,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",4.5,75,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",5,105,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",5.5,140,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",6,180,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",6.5,230,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",7,290,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",7.5,360,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",8,440,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",8.5,520,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",9,620,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",9.5,730,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",10,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",10.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",11,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",11.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",12,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",12.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",13,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",13.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",14,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",14.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",15,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",15.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",16,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",16.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",17,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",17.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",18,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",18.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",19,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",19.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",20,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",20.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",21,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",21.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",22,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",22.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",23,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",23.5,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["OqU7Tj53","吉林洮南风电场","G58-850","G58",24,850,"吉林洮南歌美飒G58-850机型当地空气密度曲线",1.245]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",0,0,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",0.5,0,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",1,0,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",1.5,0,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",2,0,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",2.5,17,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",3,49,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",3.5,92,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",4,148,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",4.5,220,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",5,307,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",5.5,415,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",6,543,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",6.5,688,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",7,867,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",7.5,1068,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",8,1298,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",8.5,1543,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",9,1764,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",9.5,2027,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",10,2216,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",10.5,2343,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",11,2405,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",11.5,2458,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",12,2489,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",12.5,2493,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",13,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",13.5,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",14,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",14.5,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",15,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",15.5,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",16,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",16.5,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",17,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",17.5,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",18,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",18.5,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",19,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",19.5,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["fHTOT3N1","青海奋进风电场","DF131-2500","DF131-2500",20,2500,"青海都兰东方电气DF131-2500kW当地空气密度功率曲线",0.8935]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",0,0,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",0.5,0,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",1,0,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",1.5,0,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",2,0,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",2.5,0,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",3,41,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",3.5,82,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",4,143,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",4.5,223,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",5,325,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",5.5,438,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",6,575,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",6.5,738,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",7,925,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",7.5,1141,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",8,1386,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",8.5,1637,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",9,1888,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",9.5,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",10,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",10.5,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",11,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",11.5,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",12,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",12.5,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",13,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",13.5,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",14,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",14.5,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",15,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",15.5,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",16,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",16.5,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",17,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",17.5,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",18,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",18.5,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",19,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",19.5,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["l7rOHE9I","山西西寨风电场","MY2.0se-121","MY2.0se-121",20,2000,"山西西寨MY2.0se-121功率曲线",1.0427]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",0,0,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",0.5,0,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",1,0,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",1.5,0,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",2,0,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",2.5,0,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",3,0,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",3.5,38.05,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",4,53.14,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",4.5,82.85,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",5,123.6,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",5.5,173.41,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",6,235.23,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",6.5,309.31,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",7,395.99,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",7.5,494.43,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",8,602.71,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",8.5,718.1,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",9,837.39,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",9.5,957.23,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",10,1074.47,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",10.5,1186.33,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",11,1290.64,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",11.5,1385.85,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",12,1471.1,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",12.5,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",13,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",13.5,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",14,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",14.5,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",15,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",15.5,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",16,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",16.5,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",17,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",17.5,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",18,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",18.5,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",19,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",19.5,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",20,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",20.5,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",21,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",21.5,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",22,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",22.5,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",23,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",23.5,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",24,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",24.5,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["uS3brhLG","内蒙大水菠萝风电场","V80-2000","V80-2000",25,1500,"大水菠萝风电场V80-2.0MW（25号）当地空气密度功率曲线",1]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",0,0,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",0.5,0,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",1,0,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",1.5,0,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",2,0,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",2.5,0,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",3,56,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",3.5,78,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",4,101,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",4.5,143,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",5,196,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",5.5,260,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",6,324,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",6.5,430,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",7,530,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",7.5,626,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",8,768,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",8.5,886,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",9,1031,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",9.5,1207,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",10,1364,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",10.5,1429,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",11,1466,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",11.5,1493,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",12,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",12.5,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",13,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",13.5,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",14,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",14.5,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",15,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",15.5,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",16,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",16.5,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",17,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",17.5,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",18,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",18.5,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",19,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",19.5,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",20,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",20.5,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",21,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",21.5,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",22,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",22.5,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",23,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",23.5,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",24,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",24.5,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["DVDyAmkL","宁夏太阳山风电场","UP1500-86","UP-86/1.5",25,1500,"太阳山风电场联合动力UP86-1500机型当地空气密度曲线",1.09]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",0,0,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",0.5,0,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",1,0,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",1.5,0,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",2,0,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",2.5,0,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",3,0,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",3.5,31.04,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",4,39.19,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",4.5,84.08,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",5,124.29,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",5.5,160.61,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",6,200.12,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",6.5,250.68,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",7,317.84,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",7.5,403.63,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",8,506.52,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",8.5,622.06,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",9,743.98,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",9.5,865.22,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",10,979.06,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",10.5,1079.83,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",11,1163.57,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",11.5,1228.2,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",12,1273.58,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",12.5,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",13,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",13.5,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",14,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",14.5,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",15,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",15.5,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",16,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",16.5,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",17,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",17.5,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",18,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",18.5,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",19,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",19.5,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",20,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",20.5,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",21,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",21.5,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",22,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",22.5,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",23,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",23.5,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",24,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",24.5,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","V80-2000",25,1300,"东山风电场V80-2000（108号）当地空气密度功率曲线",1.15]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",0,0,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",0.5,0,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",1,0,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",1.5,0,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",2,0,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",2.5,76.77,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",3,151.77,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",3.4,245.83,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",4,403.97,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",4.5,584.6,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",5.1,903.78,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",5.5,1062.18,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",6,1403.4,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",6.5,1692.26,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",7.1,2028.25,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",7.5,2301.27,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",8,2679.89,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",8.5,3129.82,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",9,3703.09,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",9.5,3862.22,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",10,3867.33,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",10.5,3940.78,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",11,4003.12,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",11.5,4064.35,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",12,4064.93,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",12.5,4070.78,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",13,4066.23,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",13.5,4069.43,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",14,4071.24,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",14.5,4069.19,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",15,4070.66,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",15.5,4069.16,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",16,4071.17,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",16.5,4070.05,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",17,4070.15,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",17.5,4070.56,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",18,4071.03,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",19,4068.51,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["BbYik4Jc","重庆兴顺二期风电场","MY4.0se-166","MY4.0se-166",19.5,4069.14,"重庆兴顺二期风电场明阳4.0当地空气密度功率曲线",1.019]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",0,0,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",3,17,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",3.5,43.6,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",4,78.6,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",4.5,122.5,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",5,175.8,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",5.5,239.3,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",6,314.5,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",6.5,403.1,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",7,506.5,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",7.5,624.9,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",8,753.4,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",8.5,889.8,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",9,1047.9,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",9.5,1231.6,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",10,1389.3,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",10.5,1472.5,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",11,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",11.5,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",12,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",12.5,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",13,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",13.5,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",14,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",14.5,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",15,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",16,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",17,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",18,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",19,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",20,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",21,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",22,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",23,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",24,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",25,1500,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",26,0,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["wgaRPXTs","山东安城风电场","UP1500-82","UP-82/1.5",50,0,"山东安城联合动力UP1500-82当地空气密度功率曲线",1.223]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",0,0,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",0.5,0,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",1,0,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",1.5,0,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",2,0,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",2.5,0,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",3,21.92,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",3.5,44.58,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",4,82.62,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",4.5,128.52,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",5,183.28,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",5.5,251.15,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",6,336.29,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",6.5,441.04,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",7,565.24,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",7.5,706.23,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",8,859.41,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",8.5,1018.86,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",9,1178.21,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",9.5,1331.26,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",10,1472.64,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",10.5,1598.2,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",11,1705.23,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",11.5,1792.59,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",12,1860.53,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",12.5,1910.53,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",13,1945.01,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",13.5,1966.92,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",14,1979.56,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",14.5,1986.61,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",15,1990.54,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",15.5,1992.52,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",16,1993.69,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",16.5,1994.79,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",17,1997.13,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",17.5,2000.07,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",18,2002.6,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",18.5,2004.04,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",19,2005.16,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",19.5,2005.93,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",20,2006.46,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",20.5,2006.88,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",21,2007.04,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",21.5,2007.1,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",22,2007.1,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",22.5,2007.1,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",23,2007.17,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",23.5,2007.25,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",24,2007.65,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",24.5,2007.97,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V90-2000","V90-2000",25,2009.3,"东山风电场V90-2000当地空气密度功率曲线",1.15]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",0,0,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",0.5,0,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",1,0,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",1.5,0,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",2,0,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",2.5,0,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",3,42,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",3.5,66.6,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",4,100,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",4.5,141,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",5,194,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",5.5,258,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",6,335,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",6.5,426,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",7,533,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",7.5,655,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",8,795,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",8.5,954,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",9,1081.514167,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",9.5,1204.122083,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",10,1309.82875,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",10.5,1392.461667,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",11,1445.492917,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",11.5,1475.045833,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",12,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",12.5,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",13,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",13.5,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",14,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",14.5,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",15,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",15.5,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",16,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",16.5,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",17,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",17.5,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",18,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",18.5,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",19,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",19.5,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500-82",20,1500,"山东泽库SL1500/82（增功组件）当地功率曲线",1.214]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",0,0,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",1,0,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",2,0,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",3,39.6,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",4,154.4,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",5,314.1,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",6,544.4,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",7,857.9,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",8,1271.1,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",9,1580.8,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",10,1908.9,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",11,1995,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",12,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",13,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",14,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",15,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",16,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",17,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",18,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",19,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",20,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",21,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",22,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",23,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",24,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["3XBmdeqd","山西燕家村风电场","W2000-111","W2000-111",25,2000,"山西燕家村二期风电场W2000-111/80机型当地空气密度曲线",0.9939]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",0,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",0.5,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",1,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",1.5,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",2,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",2.5,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",3,54.2,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",3.5,120.48,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",4,168.95,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",4.5,234.75,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",5,290.7,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",5.5,436.47,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",6,538.68,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",6.5,646.34,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",7,769.64,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",7.5,900.19,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",8,1029.81,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",8.5,1157.89,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",9,1273.45,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",9.5,1373.36,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",10,1458.17,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",10.5,1496.98,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",11,1502.42,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",11.5,1503.85,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",12,1503.64,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",12.5,1505.7,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",13,1504.74,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",13.5,1508.6,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",14,1508.11,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",14.5,1509.38,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",15,1507.99,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",15.5,1510.62,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",16,1508.13,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",16.5,1515,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",17,1515,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",17.5,1515,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",18,1515,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",18.5,1515,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",19,1508.12,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",19.5,1515,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",20,1515,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",20.5,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",21,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",21.5,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",22,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",22.5,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",23,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",23.5,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",24,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",24.5,0,"桦川华锐SL150082本地",1.1277]
["6AfecpKP","黑龙江桦川风电场","SL1500-82","SL-82/1.5",25,0,"桦川华锐SL150082本地",1.1277]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",0,0,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",0.5,0,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",1,0,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",1.5,0,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",2,0,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",2.5,0,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",3,21,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",3.5,132,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",4,304,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",4.5,514,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",5,769,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",5.5,1088,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",6,1424,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",6.5,1827,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",7,2288,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",7.5,2799,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",8,3308,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",8.5,3734,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",9,4209,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",9.5,4616,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",10,4957,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",10.5,5199,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",11,5339,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",11.5,5405,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",12,5470,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",12.5,5488,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",13,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",13.5,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",14,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",14.5,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",15,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",15.5,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",16,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",16.5,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",17,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",17.5,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",18,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",18.5,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",19,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",19.5,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",20,5500,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",20.5,5150,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",21,4800,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",21.5,4450,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",22,4100,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",22.5,3750,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",23,3400,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",23.5,3050,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",24,2700,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",24.5,2350,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["xl7TQMZ0","京津冀石门风电场","DEW-G5500-183","DEW-G5500-183",25,2000,"京津冀石门东方电气DEW-G5500-183机型当地空气密度曲线",1.028]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",0,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",0.5,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",1,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",1.5,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",2,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",2.5,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",3,38,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",3.5,153,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",4,302,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",4.5,473,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",5,681,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",5.5,914,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",6,1191,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",6.5,1522,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",7,1909,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",7.5,2354,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",8,2840,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",8.5,3154,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",9,3237,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",9.5,3286,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",10,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",10.5,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",11,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",11.5,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",12,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",12.5,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",13,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",13.5,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",14,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",14.5,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",15,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",15.5,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",16,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",16.5,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",17,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",17.5,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",18,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",18.5,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",19,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",19.5,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",20,3300,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",20.5,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",21,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",21.5,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",22,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",22.5,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",23,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",23.5,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",24,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",24.5,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["eIHhxLIU","内蒙绿源风电场","EN156-3300","EN156-3300",25,0,"内蒙绿源EN156-3300当地密度曲线",1.242]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",0,0,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",0.5,0,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",1,0,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",1.5,0,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",2,0,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",2.5,0,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",3,10.68,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",3.5,25.19,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",4,42.59,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",4.5,59.58,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",5,78.68,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",5.5,104.16,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",6,139.61,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",6.5,186.8,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",7,245.45,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",7.5,313.36,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",8,387.09,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",8.5,462.49,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",9,535.4,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",9.5,602.19,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",10,660.1,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",10.5,707.48,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",11,743.86,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",11.5,769.82,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",12,786.81,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",12.5,796.87,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",13,802.44,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",13.5,805.45,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",14,808.27,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",14.5,812.45,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",15,818.32,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",15.5,825.84,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",16,834.28,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",16.5,843.83,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",17,852.66,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",17.5,859.54,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",18,863.49,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",18.5,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",19,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",19.5,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",20,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",20.5,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",21,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",21.5,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",22,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",22.5,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",23,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",23.5,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",24,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",24.5,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["zVrHBiQU","内蒙大黑山风电场","V60-850","V60-850",25,864.17,"大黑山风电场V60-850当地空气密度功率曲线",1.16]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",0,0,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",0.5,0,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",1,0,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",1.5,0,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",2,0,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",2.5,30,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",3,95,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",3.5,188,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",4,322,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",4.5,477,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",5,664,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",5.5,888,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",6,1159,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",6.5,1475,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",7,1840,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",7.5,2252,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",8,2655,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",8.5,3013,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",9,3244,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",9.5,3407,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",10,3557,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",10.5,3705,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",11,3853,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",11.5,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",12,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",12.5,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",13,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",13.5,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",14,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",14.5,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",15,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",15.5,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",16,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",16.5,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",17,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",17.5,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",18,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",18.5,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",19,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",19.5,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",20,4000,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",20.5,3801,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",21,3602,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",21.5,3404,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",22,3205,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",22.5,3006,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",23,2807,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",23.5,2608,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",24,2410,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",24.5,2211,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",25,2012,"内蒙图步盛风电场明阳智能MY4.0se-166机型当地空气密度曲线",1.03]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",0,0,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",0.5,0,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",1,0,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",1.5,0,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",2,0,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",2.5,0,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",3,21.3,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",3.5,51.9,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",4,90.3,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",4.5,136.8,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",5,193.5,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",5.5,262.5,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",6,344.7,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",6.5,441.3,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",7,555.9,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",7.5,690.3,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",8,836.3,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",8.5,988.1,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",9,1160.3,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",9.5,1354.5,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",10,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",10.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",11,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",11.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",12,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",12.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",13,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",13.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",14,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",14.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",15,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",15.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",16,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",16.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",17,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",17.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",18,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",18.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",19,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",19.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",20,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",20.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",21,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",21.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",22,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",22.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",23,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",23.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",24,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",24.5,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["RnlbplmA","山东花园风电场","UP1500-86","UP-86/1.5",25,1500,"山东花园联合动力UP1500-86当地空气密度功率曲线",1.221]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",0,0,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",0.5,0,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",1,0,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",1.5,0,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",2,0,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",2.5,55.01,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",3,78.06,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",3.5,128.51,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",4,198.52,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",4.5,291.08,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",5,410.58,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",5.5,557.29,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",6,734.13,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",6.5,942.38,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",7,1182.14,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",7.5,1423.28,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",8,1658.29,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",8.5,1892.86,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",9,2127.63,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",9.5,2276.05,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",10,2382.05,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",10.5,2452.08,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",11,2482.87,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",11.5,2500,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",12,2506.27,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",12.5,2515.79,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",13,2517.36,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",13.5,2518.57,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",14,2520.61,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",14.5,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",15,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",15.5,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",16,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",16.5,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",17,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",17.5,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",18,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",18.5,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",19,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",19.5,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",20,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",20.5,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",21,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",21.5,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",22,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",22.5,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",23,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",23.5,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",24,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",24.5,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["qEmbqmJ6","贵州革利风电场","W2500-135","W2500-135",25,2525,"贵州革利风电场W2500-135机型当地空气密度曲线",1.021]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",0,0,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",0.5,0,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",1,0,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",1.5,0,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",2,50,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",2.5,119,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",3,231,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",3.5,391,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",4,576,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",4.5,798,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",5,1067,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",5.5,1386,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",6,1761,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",6.5,2181,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",7,2622,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",7.5,3034,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",8,3330,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",8.5,3533,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",9,3669,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",9.5,3771,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",10,3849,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",10.5,3926,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",11,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",11.5,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",12,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",12.5,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",13,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",13.5,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",14,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",14.5,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",15,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",15.5,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",16,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",16.5,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",17,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",17.5,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",18,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",18.5,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",19,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",19.5,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",20,4000,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",20.5,3801,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",21,3602,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",21.5,3404,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",22,3205,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",22.5,3006,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",23,2807,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",23.5,2608,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",24,2410,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",24.5,2211,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["Vu9OU8OQ","内蒙图步盛风电场","MY4.0se-166","MY4.0se-166",25,2012,"内蒙图步盛MYSE-4.0-166当地空气密度功率曲线",1.03]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",0,0,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",0.5,0,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",1,0,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",1.5,0,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",2,0,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",2.5,0,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",3,0,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",3.5,25,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",4,78,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",4.5,147,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",5,270,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",5.5,422,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",6,601,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",6.5,816,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",7,1068,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",7.5,1370,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",8,1716,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",8.5,2044,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",9,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",9.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",10,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",10.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",11,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",11.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",12,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",12.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",13,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",13.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",14,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",14.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",15,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",15.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",16,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",16.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",17,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",17.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",18,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",18.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",19,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",19.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",20,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",20.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",21,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",21.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",22,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",22.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",23,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",23.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",24,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",24.5,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["rAbnXQWA","安徽唐古风电场","EN141-2650","EN-141/2.65",25,2300,"安徽唐古风电场EN-141/2.65机型降功率2.3MW当地空气密度曲线",1.122]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",0,0,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",0.5,0,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",1,0,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",1.5,0,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",2,0,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",2.5,0,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",3,0,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",3.5,0,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",4,57,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",4.5,102,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",5,138,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",5.5,215,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",6,253,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",6.5,330,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",7,416,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",7.5,513,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",8,631,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",8.5,793,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",9,896,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",9.5,1035,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",10,1193,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",10.5,1362,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",11,1490,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",11.5,1656,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",12,1761,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",12.5,1860,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",13,1928,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",13.5,1982,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",14,1985,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",14.5,1997,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",15,1998,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",15.5,1998,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",16,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",16.5,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",17,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",17.5,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",18,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",18.5,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",19,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",19.5,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",20,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",20.5,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",21,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",21.5,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",22,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",22.5,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",23,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",23.5,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",24,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",24.5,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["3Jyq67jd","内蒙东山风电场","V80-2000","VT-80/2.0",25,2000,"东山风电场V80-2000当地空气密度功率曲线",1.15]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",0,0,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",0.5,0,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",1,0,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",1.5,0,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",2,0,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",2.5,4.47,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",3,35.5,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",3.5,72.16,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",4,114.3,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",4.5,164.67,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",5,226.3,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",5.5,300.02,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",6,386.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",6.5,489.3,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",7,611.2,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",7.5,749.9,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",8,902.3,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",8.5,1064.3,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",9,1227.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",9.5,1395.9,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",10,1455.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",10.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",11,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",11.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",12,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",12.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",13,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",13.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",14,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",14.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",15,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",15.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",16,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",16.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",17,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",17.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",18,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",18.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",19,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",19.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",20,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",20.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",21,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",21.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",22,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",22.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",23,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",23.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",24,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",24.5,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",25,1500.6,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",25.5,0,"山东泽库SL1500/82功率曲线",1.214]
["olgHrLiO","山东泽库风电场","SL1500-82","SL1500/82",26,0,"山东泽库SL1500/82功率曲线",1.214]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",0,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",0.5,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",1,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",1.5,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",2,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",2.5,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",3,54.2,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",3.5,120.48,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",4,168.95,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",4.5,234.75,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",5,290.7,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",5.5,436.47,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",6,538.68,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",6.5,646.34,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",7,769.64,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",7.5,900.19,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",8,1029.81,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",8.5,1157.89,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",9,1273.45,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",9.5,1373.36,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",10,1458.17,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",10.5,1496.98,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",11,1502.42,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",11.5,1503.85,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",12,1503.64,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",12.5,1505.7,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",13,1504.74,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",13.5,1508.6,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",14,1508.11,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",14.5,1509.38,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",15,1507.99,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",15.5,1510.62,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",16,1508.13,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",16.5,1515,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",17,1515,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",17.5,1515,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",18,1515,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",18.5,1515,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",19,1508.12,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",19.5,1515,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",20,1515,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",20.5,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",21,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",21.5,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",22,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",22.5,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",23,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",23.5,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",24,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",24.5,0,"太平华锐SL150082本地",1.122]
["PNKFows2","黑龙江太平风电场","SL1500-82","SL1500/82",25,0,"太平华锐SL150082本地",1.122]